{"text_format":"1","workbook":"xlsx","n_sheets":12,"sheets":["Documentation","Configuration","Import data","Arkusz1","Regions","Article translations","Region translations","Possible values","DATA","RÓŻNICE","BRYŁY FOTO","Zmiany Dawid Głód"],"not_rendered":{"charts":0,"images":5,"macros":1,"external_links":0,"defined_names":15,"comments":0,"pivot_tables":0},"unopened":[],"bounds":{"document_bytes":16777216,"sheet_cells":100000,"rows_first":2000,"rows_last":500,"rows_between":2000,"halvings":0,"cell_chars":16384,"cell_head_chars":4096},"cells_cut":0,"cells_raw":0,"read":"whole","date_system":"1900"}

{"sheet":"Documentation","index":0,"n_rows":139,"n_cols":4,"rows_kept":139,"cut":false,"hidden":false,"merged":[[10,0,10,2],[125,0,125,2],[3,0,3,2],[138,0,138,3]]}
["Description of data sheets and fields in this document"]
[]
["Field name","Unit","Description","Remark "]
["1. Sheet CONFIGURATION - Set global parameters for the import routine"]
["DIAL Manufacturer name",null,"Manufacturer identification name, given by DIAL"]
["Unit of lengths",null,"1: Meter; 2:Feet"]
["ProductPictureRelativePath",null,"The relative directory path to your product pictures, starting from this file"]
["AdditionalFileRelativePath",null,"The relative directory path to your additional files, starting from this file"]
["PhotometryFileRelativePath",null,"The relative directory path to your photometry files, starting from this file"]
["Separator",null,"The separator to import more than one element"]
["2. Sheet IMPORT DATA - Define your products"]
["InternalIdentifier",null,"Persistent ID of this article in your system. (The same article always must have the same ID over time)"]
["ArticleNumber",null,"Article number or order number"]
["ArticleName",null,"Short name of this luminaire"]
["DescriptionText",null,"Long description text"]
["Group1Name",null,"Short name for product family (can be named individually as you like). ","One or more values can be entered using the separator defined in the configuration."]
["Group2Name",null,"Short name for product assortment (can be named individually as you like). ","One or more values can be entered using the separator defined in the configuration."]
["ProductTypeId",null,"1: Indoor luminaire; 2: Outdoor luminaire, 3: Interior and Exterior Luminaire"]
["MountingTypeId",null,"ID describing the mounting type of the luminaire (please refer to page \"Possible values\")"]
["DefaultDistance","[unit of length]","How far shall the luminaire be positioned into the reference surface? Example: A luminaire, which is recessed 20cm into the ceiling has a DefaultDistance of -0.2. A pendant luminaire, with a pendant length of 40cm would have a DefaultDistance of 0.4."]
["MountingHeight","[unit of length]","Position in Z for wall luminaires when positioned in plane view."]
["AdditionalMountingType",null,"Alternative mounting types. This type is a textural descripting value and is not used by DIALux (please refer to page \"Possible values\") Several values can be entered comma separated."]
["InstallationDetailHasRim",null,"Set to 1 if the installation has a rim. Otherwise enter 0."]
["InstallationDetailHasEdge",null,"Set to 1 if the installation has an edge. Otherwise enter 0."]
["InstallationLength","[unit of length]","The length which is required for installation of the luminaire"]
["InstallationWidth","[unit of length]","The width which is required for installation of the luminaire"]
["InstallationRecessedDepth","[unit of length]","The depth which is required for installation of the luminaire"]
["InstallationDiameter","[unit of length]","For a round installation surface please enter here a diameter. InstallationWidth and InstallationLength does not have to be entered in this case. "]
["MaximalPointLoad","kg","Maximal point load in kg"]
["ProductPictureFileName",null,"File name of the product picture without path. The path to the picture folder has to be set in the configuration page. Please do not use CMYK coded JPEG images."]
["DcLightDistributionId",null,"Search criteria for a luminaire: Light distribution. ","One or more values can be entered using the separator defined in the configuration."]
["DcAdjustabilityId",null,"Search criteria for a luminaire: Adjustability. ","One or more values can be entered using the separator defined in the configuration."]
["DcShapeId",null,"Search criteria for a luminaire: Shape (please refer to page \"Possible values\")"]
["DcMountingPlaceId",null,"Search criteria for a luminaire: Mounting place (please refer to page \"Possible values\")"]
["DcMountingTypeId",null,"Search criteria for a luminaire: Mounting type. ","One or more values can be entered using the separator defined in the configuration."]
["DcControllabilityId",null,"Search criteria for a luminaire: Controllability. ","One or more values can be entered using the separator defined in the configuration."]
["DcProtectionId",null,"Search criteria for a luminaire: IP (please refer to page \"Possible values\")"]
["Labelling",null,"Labels of the luminaire (please refer to page \"Possible values\"). The label will be entered as textural value. Several values can be entered comma separated, e.g. GS,CE"]
["Safety",null,"Safety attributes of the luminaire (please refer to page \"Possible values\"). The attributes will be entered as textural values. Several values can be entered comma separated."]
["IKCode",null,"IK code of the luminaire (please refer to page \"Possible values\")"]
["ApplianceClass",null,"Appliance class of the luminaire (please refer to page \"Possible values\")"]
["ExplosionZone",null,"Explosion zone of the luminaire (please refer to page \"Possible values\")"]
["Shape3dId",null,"ID describing the shape of the luminaire (please refer to page \"Possible values\")","Can be read from Eulumdat, IESNA or model file"]
["CaseSizeX","[unit of length]","Ceiling and floor luminaires: Usually the shorter side (width) of the luminaire\nWall luminaires: The depth of the luminaire, directed to the mounting wall.","Can be read from Eulumdat, IESNA or model file"]
["CaseSizeY","[unit of length]","Ceiling and floor luminaires: Usually the longer side (length) of the luminaire\nWall luminaires: The horizontal dimension along the wall.","Can be read from Eulumdat, IESNA or model file"]
["CaseSizeZ","[unit of length]","Ceiling and floor luminaires: The height of the luminaire case\nWall luminaires: The vertical dimension along the wall.","Can be read from Eulumdat, IESNA or model file"]
["LuminaireLength","[unit of length]","Total length of the luminaire. While attribute CaseSize only describes one luminaire part the size for luminaires which are using m4d models and have more than one luminaire part can be different. "]
["LuminaireWidth","[unit of length]","Total width of the luminaire. While attribute CaseSize only describes one luminaire part the size for luminaires which are using m4d models and have more than one luminaire part can be different. "]
["LuminaireHeight","[unit of length]","Total height of the luminaire. While attribute CaseSize only describes one luminaire part the size for luminaires which are using m4d models and have more than one luminaire part can be different. "]
["LuminaireDiameter","[unit of length]","Total diameter of the luminaire. While attribute CaseSize only describes one luminaire part the size for luminaires which are using m4d models and have more than one luminaire part can be different. "]
["ModelFileName",null,"M3d file name, starting from the import document file. The path to the M3d folder has to be set in the configuration page. Only simple Models can be imported (Models with more than one data item or with more than one light emitting  object will not be imported)"]
["Accessory",null,"Possible accessories (please refer to page \"Possible values\"). One or more values can be entered comma separated, e.g. Color filter, UV protection filter"]
["AdjustabilityTiltDegrees",null,"The angle of the luminaire if it is tiltable"]
["PhotometryFileName",null,"Photometric file name, starting from the import document file. (e.g. LDT, IES, … file). The path to the photometric folder has to be set in the configuration page."]
["IsAbsolutPhotometry",null,"Set to 1 if the photometry file contains absolute measured photometric data. Usually used with LEDs based luminaires where the luminaire and LEDs can't be separated and measured on their own. Please see http://www.dial.de/DIAL/en/light/download.html?tx_drblob_pi1[downloadUid]=22 for EULUMDAT and the ANSI/IESNA LM-63-02 specification for IES for further information.","Can be read from Eulumdat or IESNA file"]
["LumDistTypeId",null,"ID describing the basic photometric behaviour of this luminaire (please refer to page \"Possible values\")","Can be read from Eulumdat or IESNA file"]
["Shape2dId",null,"ID describing the shape of the light emitting output (please refer to page \"Possible values\")","Can be read from Eulumdat or IESNA file"]
["LeoLength","[unit of length]","Longer side of the LEO (Size in Y).","Can be read from Eulumdat, IESNA file or model file"]
["LeoWidth","[unit of length]","Shorter side of the LEO (Size in X for ceiling/floor luminaires, size in Z for wall luminaires).","Can be read from Eulumdat, IESNA file or model file"]
["LeoPositionRelativeToCase",null,"Definition of the leo position and rotation."]
["HeightC0","[unit of length]","Height of light emitting surface in C0 plane","Can be read from Eulumdat or IESNA file"]
["HeightC90","[unit of length]","Height of light emitting surface in C90 plane","Can be read from Eulumdat or IESNA file"]
["HeightC180","[unit of length]","Height of light emitting surface in C180 plane","Can be read from Eulumdat or IESNA file"]
["HeightC270","[unit of length]","Height of light emitting surface in C270 plane","Can be read from Eulumdat or IESNA file"]
["RotatePhotometryForMountingType",null,"Set to 1 if the luminaire was not measured in it's mounting position. As an example, wall luminaires are often measured in ceiling mounting position. If set to one, the photometry will be rotated 90° for wall mounted luminaires and 180° for floor luminaires."]
["LdcRotationAroundG0","°","Set between 0° and 360°. Usually, only IES files for street luminaires have to be rotated by 90°, otherwise the default should be 0°"]
["LampName",null,"Short name of the lamp used in this luminaire."]
["LampTypeId",null,"Type of the used lamp, e.g. fluorescent lamp, induction lamp, LED (please refer to page \"Possible values\")"]
["NumberOfLamps",null,"Number of lamps in this luminaire","Can be read from Eulumdat or IESNA file"]
["SocketName",null,"Standardized socket designation (e.g. \"E27\", \"G8.5\")"]
["LampFlux","lm","Lamp flux of the lamp, used in this luminaire.","Can be read from Eulumdat or IESNA file"]
["LampLoad","W","Power of the single lamp used in this luminaire.","Can be read from Eulumdat or IESNA file"]
["SpectrumID",null,"Spectrum to be used for calculation in DIALux. (please refer to page \"Possible values\" for some default spectrums you can use)","Will be overwritten by SpectrumFileName"]
["SpectrumFileName",null,"An individual spectrum file"]
["ColorTemperature","K","Correlating Color temperature of the lamp.","Can be read from spectrum"]
["ColorRenderingIndex",null,"Color Rendering Index, an integer between -44 and 100","Can be read from spectrum"]
["ILCOS",null,"ILCOS-L of this lamp."]
["TotalSystemPower","W","Nominal power of the luminaire, including complete lamp load and ballast loss.","Can be read from Eulumdat or IESNA file"]
["EMBLF",null,"Emergency Ballast Lumen Factor from 0 to 1 (100%)","0.8 means 80%"]
["EmergencyPhotometryFileName",null,"Photometric file name, starting from the import document file. (e.g. LDT, IES, … file). The path to the photometric folder has to be set in the configuration page."]
["EmergencyIsAbsolutPhotometry",null,"Set to 1 if the photometry file contains absolute measured photometric data. Usually used with LEDs based luminaires where the luminaire and LEDs can't be separated and measured on their own. Please see http://www.dial.de/DIAL/en/light/download.html?tx_drblob_pi1[downloadUid]=22 for EULUMDAT and the ANSI/IESNA LM-63-02 specification for IES for further information.","Can be read from Eulumdat or IESNA file"]
["EmergencyLumDistTypeId",null,"ID describing the basic photometric behaviour of this luminaire (please refer to page \"Possible values\")","Can be read from Eulumdat or IESNA file"]
["EmergencyShape2dId",null,"ID describing the shape of the light emitting output (please refer to page \"Possible values\")","Can be read from Eulumdat or IESNA file"]
["EmergencyLeoLength","[unit of length]","Longer side of the Emergency LEO (Size in Y).","Can be read from Eulumdat, IESNA file or model file"]
["EmergencyLeoWidth","[unit of length]","Shorter side of the Emergency LEO (Size in X for ceiling/floor luminaires, size in Z for wall luminaires).","Can be read from Eulumdat, IESNA file or model file"]
["EmergencyLeoPositionRelativeToCase",null,"Definition of the leo position and rotation."]
["EmergencyHeightC0","[unit of length]","Height of light emitting surface in C0 plane","Can be read from Eulumdat or IESNA file"]
["EmergencyHeightC90","[unit of length]","Height of light emitting surface in C90 plane","Can be read from Eulumdat or IESNA file"]
["EmergencyHeightC180","[unit of length]","Height of light emitting surface in C180 plane","Can be read from Eulumdat or IESNA file"]
["EmergencyHeightC270","[unit of length]","Height of light emitting surface in C270 plane","Can be read from Eulumdat or IESNA file"]
["EmergencyRotatePhotometryForMountingType",null,"Set to 1 if the luminaire was not measured in it's mounting position. As an example, wall luminaires are often measured in ceiling mounting position. If set to one, the photometry will be rotated 90° for wall mounted luminaires and 180° for floor luminaires."]
["EmergencyLdcRotationAroundG0","°","Set between 0° and 360°. Usually, only IES files for street luminaires have to be rotated by 90°, otherwise the default should be 0°"]
["EmergencyLampName",null,"Short name of the lamp used in this luminaire."]
["EmergencyLampTypeId",null,"Type of the used lamp, e.g. fluorescent lamp, induction lamp, LED (please refer to page \"Possible values\")"]
["EmergencyNumberOfLamps",null,"Number of lamps in this luminaire","Can be read from Eulumdat or IESNA file"]
["EmergencySocketName",null,"Standardized socket designation (e.g. \"E27\", \"G8.5\")"]
["EmergencyLampFlux","lm","Lamp flux of the lamp, used in this luminaire.","Can be read from Eulumdat or IESNA file"]
["EmergencyLampLoad","W","Power of the single lamp used in this luminaire.","Can be read from Eulumdat or IESNA file"]
["EmergencySpectrumID",null,"Spectrum to be used for calculation in DIALux. (please refer to page \"Possible values\" for some default spectrums you can use)","Will be overwritten by SpectrumFileName"]
["EmergencySpectrumFileName",null,"An individual spectrum file"]
["EmergencyColorTemperature","K","Correlating Color temperature of the lamp.","Can be read from spectrum"]
["EmergencyColorRenderingIndex",null,"Color Rendering Index, an integer between -44 and 100","Can be read from spectrum"]
["EmergencyILCOS",null,"ILCOS-L of this lamp."]
["EmergencyTotalSystemPower","W","Nominal power of the luminaire, including complete lamp load and ballast loss.","Can be read from Eulumdat or IESNA file"]
["EmergencyEMBLF",null,"Emergency Ballast Lumen Factor from 0 to 1 (100%)","0.8 means 80%"]
["AmbientTemperatureMin","°C","The lower range of the ambient temperature"]
["AmbientTemperatureMax","°C","The higher range of the ambient temperature"]
["MaximalSurfaceTemperature","°C","The maximum surface temperature"]
["Application",null,"Possible application (please refer to page \"Possible values\"). One or more values can be entered comma separated, e.g. Kitchens,Bathrooms,Living and dining rooms and bedrooms,Children´s rooms"]
["BallastType",null,"The ballast type of the luminaire. Please refer to page \"Possible values\"). One or more values can be entered comma separated, e.g. "]
["Controller",null,"The controller of the luminaire (please refer to page \"Possible values\"). One or more values can be entered comma separated. E.g. DALI,DMX"]
["IntegratedSensor",null,"Attributes describing an integrated sensor (please refer to page \"Possible values\"). One or more values can be entered comma separated"]
["LightDeflection",null,"Describing optic or light deflection components (please refer to page \"Possible values\"). One or more values can be entered comma separated, e.g. Reflector with louver: bright,Reflector with louver: matt,Reflector with louver: white"]
["SaturatedLightColor",null,"IDs describing the saturated light colors (please refer to page \"Possible values\"). One or more values can be entered comma separated. E.g. green, red, yellow"]
["SystemTypeAndVoltage","V","The system type and voltage of the luminaire. One or more values can be entered comma separated, e.g. AC230,DC12. Please prefix the voltage with the voltage type (AC or DC). "]
["IntegratedSwitch",null,"Attributes describing an integrated switch (please refer to page \"Possible values\"). One or more values can be entered comma separated"]
["IsWireForwardCapable",null,"Set to 1 for luminaires which are suitable for feed-through wiring."]
["IsGlareBap1000Compliant",null,"Glare prevention for luminaires which are having a BAP value below 1000 cd/m^2. Please enter 1 if the luminaire fulfils this condition. "]
["IsGlareUgr19Compliant",null,"Glare prevention for luminaires which are having an UGR value below 19.Please enter 1 if the luminaire fulfils this condition. "]
["Impression",null,"The impression of the luminaire (please refer to page \"Possible values\")"]
["ImpressionSurface",null,"The impression of the surface (please refer to page \"Possible values\"). One or more values can be entered comma separated, e.g. Bronze, Chrome"]
["Color",null,"The color of the luminaire case (please refer to page \"Possible values\"). One or more values can be entered comma separated, e.g. White,Black "]
["DesignerName",null,"Name of the designer"]
["DesignerOriginCountry",null,"Country name of the designers origin country  (please refer to page \"Possible values\"). "]
[]
["3. Sheet article translations - Translate your article texts into different languages"]
["ArticleReplicationID",null,"Same ID as in \"Import data\". You can define multiple rows for one ArticleReplicationID with different LanguageIDs to enter translations in multiple languages."]
["LanguageID",null,"Numeric ID of the language. For valid entries, please refer to page \"Possible values\"."]
["ArticleNumber",null,"Article number, translated into language {LanguageID}"]
["ArticleName",null,"Article name, translated into language {LanguageID}"]
["DescriptionText",null,"Article description, translated into language {LanguageID}"]
["AdvertisementText",null,"Article advertisment text, translated into language {LanguageID}"]
["FamilyName",null,"Family name, translated into language {LanguageID}."]
["AssortmentName",null,"Assortment name, translated into language {LanguageID}"]
["LampName",null,"Lamp name, translated into language {LanguageID}"]
[]
[]
["Handling of optional values:"]
["It is possible that the Excel Import reads some information from Eulumdat, IESNA or m3d files. To ensure that the value is read automatically please note that the field has to be empty.\nThe values can be found in the table column \"Remark\"."]

{"sheet":"Configuration","index":1,"n_rows":13,"n_cols":4,"rows_kept":13,"cut":false,"hidden":false,"merged":[]}
["Set global parameters for the import routine"]
[]
["Parameter","Value","Usage","Internal Identifier"]
["DIAL Manufacturer name","Manuf. name (OPK)","Your manufacturer identification name, given by DIAL. Change before first use","ManufacturerName"]
["DIAL Schema ID","STANDARD:2","Id of the excel file schema, given by DIAL.","SchemaID"]
["Unit of lengths",1,"1: Meter, 2:Feet","UnitOfLength"]
["ProductPictureRelativePath","picture","The relative directory path to your product pictures, starting from this file","PictureRelativePath"]
["AdditionalFileRelativePath","files","The relative directory path to your additional files, starting from this file","AdditionalFileRelativePath"]
["PhotometryFileRelativePath","photometry","The relative directory path to your photometry files, starting from this file","PhotometryRelativePath"]
["M3dFileRelativePath","m3d","The relative directory path to your m3d files, starting from this file","M3dRelativePath"]
["Update behaviour",1,"1: Replace, 2: Skip … luminares with existing ArticleReplicationID","UpdateType"]
["Region update behaviour",2,"1: Replace, 2: Skip … existing Regions","RegionUpdateType"]
["Separator",",","The separator to import more than one element","Separator"]

{"sheet":"Import data","index":2,"n_rows":747,"n_cols":122,"rows_kept":747,"cut":false,"hidden":false,"merged":[[0,0,0,6],[2,64,2,75],[3,1,3,4],[3,6,3,7],[3,9,3,12],[3,35,3,37],[3,45,3,46],[3,48,3,51],[3,52,3,55],[3,58,3,68],[2,40,2,49],[3,22,3,33],[3,14,3,20],[2,0,2,39],[2,51,2,63],[0,35,0,37],[3,114,3,115],[2,117,2,121],[3,97,3,98],[2,103,2,106],[3,101,3,102],[3,104,3,105],[3,109,3,110],[2,107,2,116],[2,90,2,102],[3,95,3,96],[3,84,3,94],[0,18,0,20],[1,18,1,20],[2,77,2,89],[3,38,3,41],[3,69,3,70],[3,56,3,57],[3,71,3,72],[3,74,3,77],[3,78,3,81],[3,82,3,83]]}
["Define geometric and photometric product data and English texts (for translations please use \"Article translations\" worksheet).",null,null,null,null,null,null,"Mandatory fields which have to be entered",null,null,null,null,null,null,null,null,"Optional data e.g. for LUMsearch",null,"WYMAGANE DO RĘCZNEGO UZUPEŁNIENIA",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"uzupełnianie ręczene gdy zmieniamy osie",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"uzupełnianie ręczene gdy zmieniamy osie"]
["While entering decimal numbers please keep in mind the configurated unit of length.",null,null,null,null,null,null,"Optional data which will be read from photometric file if the fied is empty",null,null,null,"RĘCZNIE WYMAGANE",null,null,null,null,null,null,"L, Y, AZ",null,null,null,null,null,"RĘCZNIE WYMAGANE",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"RĘCZNIE WYMAGANE",null,null,null,null,"Obrót fotometri względem osi montażu = 1"]
["A R T I C L E ",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"L U M I N A I R E    C A S E",null,null,null,null,null,null,null,null,null,null,"P H O T O M E T R Y",null,null,null,null,null,null,null,null,null,null,null,null,"E Q U I P M E N T ",null,null,null,null,null,null,null,null,null,null,null,null,"E M E R G E N C Y - P H O T O M E T R Y",null,null,null,null,null,null,null,null,null,null,null,null,"E M E R G E N C Y - E Q U I P M E N T ",null,null,null,null,null,null,null,null,null,null,null,null,"APPLICATION",null,null,null,"ELECTRIC",null,null,null,null,null,null,null,null,null,"DESIGN"]
["Identifier","Description",null,null,null,"Sort number","Groups",null,null,"Type",null,null,null,null,"Installation details",null,null,null,null,null,null,"Picture","Design criteria",null,null,null,null,null,null,null,null,null,null,null,"Shape","Size",null,null,"Total dimensions",null,null,null,"Model","Accessory","Adjustability","Photometric file",null,"Light distribution","Light Emitting Object geometry",null,null,null,"C-Heights",null,null,null,"Rotation",null,"Lamp description",null,null,null,null,null,null,null,null,null,null,"Equipment",null,"Photometric file",null,"Light distribution","Light Emitting Object geometry",null,null,null,"C-Heights",null,null,null,"Rotation",null,"Lamp description",null,null,null,null,null,null,null,null,null,null,"Equipment",null,"AmbientTemperature",null,"SurfaceTemperature","Application","Control Gear",null,"Sensor","Optic",null,"System voltage","SwitchIntegration","WireForwardCapability","GlareProtection",null,"Impression","Impression of surface","Color of housing","Designer"]
[]
["InternalIdentifier","ArticleNumber","ArticleName","EAN","DescriptionText","ArticleSortNo","Group1Name","Group2Name","Regions","ProductTypeId","MountingTypeId","DefaultDistance","MountingHeight","AdditionalMountingType","InstallationDetailHasRim","InstallationDetailHasEdge","InstallationLength","InstallationWidth","InstallationRecessedDepth","InstallationDiameter","MaximalPointLoad","ProductPictureFileName","DcLightDistributionId","DcAdjustabilityId","DcShapeId","DcMountingPlaceId","DcMountingTypeId","DcControllabilityId","DcProtectionId","Labelling","Safety","IKCode","ApplianceClass","ExplosionZone","Shape3DID","CaseSizeX","CaseSizeY","CaseSizeZ","LuminaireLength","LuminaireWidth","LuminaireHeight","LuminaireDiameter","ModelFileName","Accessory","AdjustabilityTiltDegrees","PhotometryFileName","IsAbsolutePhotometry","LumDistTypeId","Shape2dId","LeoLength","LeoWidth","LeoPositionRelativeToCase","HeightC0","HeightC90","HeightC180","HeightC270","RotatePhotometryForMountingType","LdcRotationAroundG0","LampName","LampTypeId","NumberOfLamps","SocketName","LampFlux","LampLoad","SpectrumId","SpectrumFileName","ColorTemperature","ColorRenderingIndex","ILCOS","TotalSystemPower","EMBLF","EmergencyPhotometryFileName","EmergencyIsAbsolutePhotometry","EmergencyLumDistTypeID","EmergencyShape2DID","EmergencyLeoLength","EmergencyLeoWidth","EmergencyLeoPositionRelativeToCase","EmergencyHeightC0","EmergencyHeightC90","EmergencyHeightC180","EmergencyHeightC270","EmergencyRotatePhotometryForMountingType","EmergencyLdcRotationAroundG0","EmergencyLampName","EmergencyLampTypeId","EmergencyNumberOfLamps","EmergencySocketName","EmergencyLampFlux","EmergencyLampLoad","EmergencySpectrumId","EmergencySpectrumFileName","EmergencyColorTemperature","EmergencyColorRenderingIndex","EmergencyILCOS","EmergencyTotalSystemPower","EmergencyEMBLF","AmbientTemperatureMin","AmbientTemperatureMax","MaximalSurfaceTemperature","Application","BallastType","Controller","IntegratedSensor","LightDeflection","SaturatedLightColor","SystemTypeAndVoltage","IntegratedSwitch","IsWireForwardCapable","IsGlareBap1000Compliant","IsGlareUgr19Compliant","Impression","ImpressionSurface","Color","DesignerName","DesignerOriginCountry"]
["1157",{"$f":"INDEX(DB,MATCH($A7,ID,0),2)","v":"1157XX0009"},{"$f":"INDEX(DB,MATCH($A7,ID,0),3)","v":"KOSTER DOUBLE HEAD POLE-TOP 2XLED 3960LM 3000K ON/OFF"},null,{"$f":"IF(INDEX(DB,MATCH($A7,ID,0),35)=0,\"\",INDEX(DB,MATCH($A7,ID,0),35))","v":"Top-mounted luminaire, designed to be mounted on a lighting pole with a Ø50mm mounting shaft"},null,{"$f":"IF(INDEX(DB,MATCH($A7,ID,0),4)=0,\"\",INDEX(DB,MATCH($A7,ID,0),4))","v":"Koster"},{"$f":"IF(INDEX(DB,MATCH($A7,ID,0),5)=0,\"\",INDEX(DB,MATCH($A7,ID,0),5))","v":"Post,Head"},"Europe, Africa, Asia, Australia and Oceania, North America, South America",2,{"$f":"IFERROR(INDEX(TYPMONT,MATCH((INDEX(DB,MATCH($A7,ID,0),31)),ID_RODZ,0),3),\"\")","v":512},4,{"$f":"IF(K7=4,2.5,IF(K7=64,0.5,0))","v":0},{"$f":"IFERROR(IF(INDEX(TYPMONT,MATCH((INDEX(DB,MATCH($A7,ID,0),31)),ID_RODZ,0),6)=0,\"\",INDEX(TYPMONT,MATCH((INDEX(DB,MATCH($A7,ID,0),31)),ID_RODZ,0),6)),\"\")","v":""},null,null,null,null,null,null,null,{"$f":"IF(INDEX(DB,MATCH($A7,ID,0),57)=0,\"\",INDEX(DB,MATCH($A7,ID,0),57))","v":"1157XX0009.png"},{"$f":"IF((IFERROR(INDEX(BRYLA_FOTO,MATCH(INDEX(DB,MATCH($A7,ID,0),62),ID_BRYLAFOTO,0),6),\"\"))<>0,IFERROR(INDEX(BRYLA_FOTO,MATCH(INDEX(DB,MATCH($A7,ID,0),62),ID_BRYLAFOTO,0),6),\"\"),\"\")","v":3},{"$f":"IF(INDEX(DB,MATCH($A7,ID,0),61)=0,\"\",INDEX(DB,MATCH($A7,ID,0),61))","v":1},2,{"$f":"IFERROR(INDEX(TYPMONT,MATCH((INDEX(DB,MATCH($A7,ID,0),31)),ID_RODZ,0),1),\"\")","v":5},{"$f":"IFERROR(INDEX(TYPMONT,MATCH((INDEX(DB,MATCH($A7,ID,0),31)),ID_RODZ,0),2),\"\")","v":9},{"$f":"IF(INDEX(DB,MATCH($A7,ID,0),59)=0,\"\",INDEX(DB,MATCH($A7,ID,0),59))","v":4},{"$f":"IFERROR(IF(INDEX(DB,MATCH($A7,ID,0),19)=0,\"\",INDEX(DB,MATCH($A7,ID,0),19)+1),\"\")","v":66},{"$f":"IF(INDEX(DB,MATCH($A7,ID,0),27)=0,\"\",INDEX(DB,MATCH($A7,ID,0),27))","v":"CE"},{"$f":"IFERROR(IF(FIND(\"RENA\",$C7)>0,\"Vehicle resistant\",\"\"),\"\")","v":""},{"$f":"IF(INDEX(DB,MATCH($A7,ID,0),20)=0,\"\",INDEX(DB,MATCH($A7,ID,0),20))","v":"IK10"},{"$f":"IF(INDEX(DB,MATCH($A7,ID,0),21)=0,\"\",INDEX(DB,MATCH($A7,ID,0),21))","v":"Class I"},null,null,null,null,null,{"$f":"INDEX(DB,MATCH($A7,ID,0),24)","v":0.82},{"$f":"INDEX(DB,MATCH($A7,ID,0),25)","v":0.24},{"$f":"INDEX(DB,MATCH($A7,ID,0),26)","v":0.22},null,null,null,null,{"$f":"IF(INDEX(DB,MATCH($A7,ID,0),58)=0,\"\",INDEX(DB,MATCH($A7,ID,0),58))","v":"1157XX0009.ldt"},{"$f":"IF($BJ7=\"\",1,0)","v":1},null,null,null,null,0,null,null,null,null,null,null,"LED",16,null,{"$f":"IF(INDEX(DB,MATCH($A7,ID,0),60)=0,\"\",INDEX(DB,MATCH($A7,ID,0),60))","v":""},null,null,{"$f":"IF($BO7=4000,24,23)","v":23},null,{"$f":"IF(INDEX(DB,MATCH($A7,ID,0),22)=0,\"\",INDEX(DB,MATCH($A7,ID,0),22))","v":3000},{"$f":"IF(INDEX(DB,MATCH($A7,ID,0),53)=0,\"\",INDEX(DB,MATCH($A7,ID,0),53))","v":80},null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,{"$f":"IF(INDEX(DB,MATCH($A7,ID,0),29)=0,\"\",INDEX(DB,MATCH($A7,ID,0),29))","v":""},{"$f":"IF(INDEX(DB,MATCH($A7,ID,0),28)=0,\"\",INDEX(DB,MATCH($A7,ID,0),28))","v":""},null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"Poland"]
["1370","1370XX0010","MANDAL WALL 2XLED GU10 530LM UP25D & DOWN25D 2700K DIM.",null,"Wall-mounted luminaire with modern design. For lighting private areas and public spaces.",null,{"$f":"IF(INDEX(DB,MATCH($A8,ID,0),4)=0,\"\",INDEX(DB,MATCH($A8,ID,0),4))","v":"Mandal"},"Wall","Europe, Africa, Asia, Australia and Oceania, North America, South America",2,4,0,{"$f":"IF(K8=4,2.5,IF(K8=64,0.5,0))","v":2.5},"",null,null,null,null,null,null,null,"1370XX0010.jpg",2,1,1,2,2,1,45,"CE",{"$f":"IFERROR(IF(FIND(\"RENA\",$C8)>0,\"Vehicle resistant\",\"\"),\"\")","v":""},"IK08","Class I",null,null,null,null,null,0.09,0.12,0.18,null,null,null,null,"1370XX0010.ldt",{"$f":"IF($BJ8=\"\",1,0)","v":0},null,null,null,null,1,null,null,null,null,null,null,"LED",16,null,"GU10",null,null,{"$f":"IF($BO8=4000,24,23)","v":23},null,2700,97,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"","",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"Poland"]
["1440","1440XX0010","ALTA BOLLARD 85CM E27",null,"Bollard luminaire of stable and durable construction. For lighting private areas and public spaces.",null,"Alta,Wood","Bollard","Europe, Africa, Asia, Australia and Oceania, North America, South America",2,2,0.7,0,"",null,null,null,null,null,null,null,"1440XX0010.jpg",7.3,1,1,3,6,4,66,"CE","","IK10","Class II",null,null,null,null,null,0.15,0.15,0.85,null,null,null,null,"1440XX0010.ldt",0,null,null,null,null,1,null,null,null,null,null,null,"LED",16,null,"E27",null,null,23,null,"",80,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"","",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"Poland"]
["1550","1550XX0016","RENA IN-GROUND LED GU10 375LM 36D 3000K DIM.",null,"An orientation luminaire that can be driven on by vehicles with pneumatic tires. Luminaires should not be used on traffic lanes where they would be exposed to horizontal weight load as a result of sudden braking, acceleration, and change of direction. The light direction angle can be adjusted, up to a maximum of 10 degrees",null,"Rena","Recessed","Europe, Africa, Asia, Australia and Oceania, North America, South America",2,128,-0.127,0,"",null,null,null,null,null,null,null,"1550XX0016.jpg",2,3,1,3,1,1,69,"CE","Vehicle resistant","IK09","Class I",null,null,null,null,null,0,0,0,null,null,null,null,"1550XX0016.ldt",0,null,null,null,null,2,null,null,null,null,1,null,"LED",16,null,"GU10",null,null,23,null,3000,90,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"","",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"Poland"]
["1580","1580XX0017","LILLEHAMMER WALL 2XLED 1008LM UP & DOWN 4º/60º 3000K DIM.",null,"Luminaire with a wide range of applications, among others for lighting: wall surfaces, facades and other architectural concepts",null,"Lillehammer","Wall","Europe, Africa, Asia, Australia and Oceania, North America, South America",2,4,0,2.5,"",null,null,null,null,null,null,null,"1580XX0017.jpg",10,1,2,2,2,1,66,"CE","","IK08","Class I",null,null,null,null,null,0.18,0.11,0.08,null,null,null,null,"1580XX0017.ldt",1,null,null,null,null,1,null,null,null,null,null,null,"LED",16,null,"",null,null,23,null,3000,80,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"","",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"Poland"]
["1631","1631XX0011","RENA IN-GROUND LED GU10 375LM 3000K DIM.",null,"An orientation luminaire on which vehicles with pneumatic tires can drive. The luminaires should not be used on roads, where they would be exposed to horizontal loads as a result of sudden braking, acceleration and changes in driving direction.",null,"Rena","Recessed","Europe, Africa, Asia, Australia and Oceania, North America, South America",2,128,-0.127,0,"",null,null,null,null,null,null,null,"1631XX0011.jpg",4,3,1,3,1,1,69,"CE","Vehicle resistant","IK10","Class I",null,null,null,null,null,0,0,0,null,null,null,null,"1631XX0011.ldt",0,null,null,null,null,2,null,null,null,null,1,null,"LED",16,null,"GU10",null,null,23,null,3000,90,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"","",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"Poland"]
["1733","1733XX0010","NARVIK II BOLLARD LED 2058LM 4000K DIM.",null,"A bollard luminaire with a stable and durable structure. For lighting private and public areas",null,"Narvik","Bollard","Europe, Africa, Asia, Australia and Oceania, North America, South America",2,2,0.7,0,"",null,null,null,null,null,null,null,"1733XX0010.png",4,1,1,3,6,1,66,"CE","","IK10","Class II",null,null,null,null,null,0.24,0.24,0.95,null,null,null,null,"1733XX0010.ldt",1,null,null,null,null,1,null,null,null,null,null,null,"LED",16,null,"",null,null,24,null,4000,80,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"","",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"Poland"]
["1734","1734XX0010","NARVIK II BOLLARD LED 2058LM 4000K DIM.",null,"A bollard luminaire with a stable and durable structure. For lighting private and public areas",null,"Narvik","Bollard","Europe, Africa, Asia, Australia and Oceania, North America, South America",2,2,0.7,0,"",null,null,null,null,null,null,null,"1734XX0010.png",4,1,1,3,6,1,66,"CE","","IK10","Class II",null,null,null,null,null,0.24,0.24,0.95,null,null,null,null,"1734XX0010.ldt",1,null,null,null,null,1,null,null,null,null,null,null,"LED",16,null,"",null,null,24,null,4000,80,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"","",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"Poland"]
["2401","2401XX0010","HELLVIK BOLLARD 55CM LED 978LM 4000K DIM.",null,"A luminaire with a contemporary design. For lighting gardens, private areas and other architectural concepts.",null,"Hellvik","Bollard","Europe, Africa, Asia, Australia and Oceania, North America, South America",2,2,0.55000000000000004,0,"",null,null,null,null,null,null,null,"2401XX0010.png",7.9,1,2,3,6,1,66,"CE","","IK08","Class II",null,null,null,null,null,0.42,0.11,0.55000000000000004,null,null,null,null,"2401XX0010.ldt",1,null,null,null,null,0,null,null,null,null,null,null,"LED",16,null,"",null,null,24,null,4000,80,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"","",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"Poland"]
["240A","240XX0111","OSLO CEILING-CHAIN E27",null,"Scandinavian design luminaire with chain suspension. For lighting gardens, terraces and other architectural concepts.",null,"Oslo","Ceiling","Europe, Africa, Asia, Australia and Oceania, North America, South America",2,16,0.7,0,"",null,null,null,null,null,null,null,"240XX0111.jpg",9,1,1,1,4,4,56,"CE","","IK07","Class II",null,null,null,null,null,0.28000000000000003,0.28000000000000003,0.86,null,null,null,null,"240XX0111.ldt",0,null,null,null,null,1,null,null,null,null,null,null,"LED",16,null,"E27",null,null,23,null,"",80,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"","",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"Poland"]
["5001","5001XX0016","NICE POLE-TOP LED 3092LM 4000K ON/OFF",null,"Top-mounted luminaire designed for mounting on a lighting pole with a Ø60mm mounting shaft",null,"Nice","Post,Head","Europe, Africa, Asia, Australia and Oceania, North America, South America",2,512,3.84,0,"",null,null,null,null,null,null,null,"5001XX0016.jpg",9,1,1,5,9,4,66,"CE","","","Class I",null,null,null,null,null,0.7,0.55000000000000004,0.55000000000000004,null,null,null,null,"5001XX0016.ldt",1,null,null,null,null,0,null,null,null,null,null,null,"LED",16,null,"",null,null,24,null,4000,80,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"","",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"Poland"]
["5132","5132XX0009","HAMMERFEST POLE-TOP LED 4503LM 4000K DALI2",null,"Luminaire mounted on a telescopic lighting pole with a diameter Ø60mm. Other components need to be ordered separately",null,"Hammerfest","Post,Head","Europe, Africa, Asia, Australia and Oceania, North America, South America",2,512,4,0,"",null,null,null,null,null,null,null,"5132XX0009.jpg",7,1,1,5,9,3,66,"CE","","IK07","Class I",null,null,null,null,null,0.76,0.55000000000000004,0.55000000000000004,null,null,null,null,"5132XX0009.ldt",1,null,null,null,null,0,null,null,null,null,null,null,"LED",16,null,"",null,null,24,null,4000,80,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"DALI","",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"Poland"]
["541","541XX0014","BORNHOLM CEILING/WALL LED 1059LM 3000K DIM.",null,"A ceiling-type luminaire with a modern design",null,"Bornholm","Wall,Ceiling","Europe, Africa, Asia, Australia and Oceania, North America, South America",2,4,0,2.5,"Ceiling mounted",null,null,null,null,null,null,null,"541XX0014.jpg",8,1,1,2,2,1,66,"CE","","IK10","Class I",null,null,null,null,null,0,0,0,null,null,null,null,"541XX0014.ldt",1,null,null,null,null,4,null,null,null,null,1,null,"LED",16,null,"",null,null,23,null,3000,80,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"","",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"Poland"]
["576","576XX0309","VISBY POLE-TOP 2XLED 4900LM 3000K",null,"A mounted luminaire designed to be mounted on a lighting pole with a Ø60mm mounting shaft",null,"Visby","Post,Head","Europe, Africa, Asia, Australia and Oceania, North America, South America",2,512,3.85,0,"",null,null,null,null,null,null,null,"576XX0309.jpg",9,1,1,5,9,4,66,"CE","","IK05","Class I",null,null,null,null,null,0,0,0,null,null,null,null,"576XX0309.ldt",1,null,null,null,null,1,null,null,null,null,null,null,"LED",16,null,"",null,null,23,null,3000,80,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"","",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"Poland"]
["6153","6153XX0010","BORG PRO POLE-TOP LED 7218LM VSM 3000K DALI2",null,"Luminaire designed to be mounted on a lighting pole with a mounting shaft Ø60mm",null,"Borg","Post,Head","Europe, Africa, Asia, Australia and Oceania, North America, South America",2,512,4,0,"",null,null,null,null,null,null,null,"6153XX0010.png",4,1,1,5,9,3,66,"CE","","IK08","Class I",null,null,null,null,null,0.15,0.51,0.51,null,null,null,null,"6153XX0010.ldt",1,null,null,null,null,0,null,null,null,null,null,null,"LED",16,null,"",null,null,23,null,3000,80,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"DALI","",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"Poland"]
["6402","6402XX0009","LYSFJORD WALL 2XLED 4144LM UP60º & DOWN4º 3000K DALI2",null,"A luminaire with a wide range of applications, including lighting: wall surfaces, facades and other architectural concepts.",null,"Lysfjord","Wall","Europe, Africa, Asia, Australia and Oceania, North America, South America",2,4,0.2,2.5,"",null,null,null,null,null,null,null,"6402XX0009.png",10,1,1,2,2,3,66,"CE","","IK08","Class I",null,null,null,null,null,0.43,0.15,0.2,null,null,null,null,"6402XX0009.ldt",1,null,null,null,null,1,null,null,null,null,null,null,"LED",16,null,"",null,null,23,null,3000,80,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"DALI","",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"Poland"]
["6473","6473XX0009","MOSS LED 439LM 36D 3000K DIM.",null,"For illuminating gardens, private areas and other architectural concepts. Possibility to adjust the direction of light also in the vertical plane.",null,"Moss,Move","Spot,Ground","Europe, Africa, Asia, Australia and Oceania, North America, South America",2,2,1,0,"",null,null,null,null,null,null,null,"6473XX0009.png",2,4,1,3,7,1,66,"CE","","","Class I",null,null,null,null,null,0,0,0,null,null,null,null,"6473XX0009.ldt",1,null,null,null,null,2,null,null,null,null,1,null,"LED",16,null,"",null,null,23,null,3000,80,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"","",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"Poland"]
["6706","6706XX0309",{"$f":"INDEX(DB,MATCH($A24,ID,0),3)","v":"MOSS FLOODLIGHT-BOX LED 438LM 36D 3000K DIM."},null,"For lighting gardens, private areas and other architectural concepts. Possibility to adjust the lighting direction also in the vertical plane.",null,"Moss,Arm","Spot,Wall","Europe, Africa, Asia, Australia and Oceania, North America, South America",2,2,0.6,0,"",null,null,null,null,null,null,null,"6706XX0309.png",2,4,1,3,6.7,1,66,"CE","","","Class I",null,null,null,null,null,0,0,0,null,null,null,null,"6706XX0309.ldt",1,null,null,null,null,2,null,null,null,null,null,null,"LED",16,null,"",null,null,23,null,3000,80,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"","",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"Poland"]
["544","544XX0009","BORNHOLM CEILING/WALL LED 1080LM 3000K MD",null,"A ceiling type luminaire with a modern design",null,"Bornholm","Wall","Europe, Africa, Asia, Australia and Oceania, North America, South America",2,4,0,2.5,"Ceiling mounted",null,null,null,null,null,null,null,"544XX0009.jpg",8,1,1,2,2,3,66,"CE","","","Class I",null,null,null,null,null,0.28999999999999998,0.28999999999999998,0.09,null,null,null,null,"544XX0009.ldt",1,null,null,null,null,4,null,null,null,null,1,null,"LED",16,null,"",null,null,23,null,3000,80,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"","Daylight sensor,Motion sensor",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"Poland"]
["1000","1000XX0009","TRYSIL 263CM 4XLED 3976LM DOWN 3000K DIM.",null,"Luminaire with a contemporary design. For lighting gardens, private areas, and other architectural concepts",null,"Trysil","Post","Europe, Africa, Asia, Australia and Oceania, North America, South America",2,256,2.63,{"$f":"IF(K26=4,2.5,IF(K26=64,0.5,0))","v":0},"",null,null,null,null,null,null,null,"1000XX0009.png",7,1,2,5,8,1,66,"CE","","IK10","Class I",null,null,null,null,null,1.18,0.24,2.63,null,null,null,null,"1000XX0009.ldt",1,null,null,null,null,0,null,null,null,null,null,null,"LED",16,null,"",null,null,23,null,3000,80,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"","",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"Poland"]
["1001","1001XX0009","TRYSIL 263CM 4XLED 4168LM DOWN 4000K DIM.",null,"Luminaire with a contemporary design. For lighting gardens, private areas, and other architectural concepts",null,"Trysil","Post","Europe, Africa, Asia, Australia and Oceania, North America, South America",2,256,2.63,0,"",null,null,null,null,null,null,null,"1001XX0009.png",7,1,2,5,8,1,66,"CE","","IK10","",null,null,null,null,null,1.18,0.24,2.63,null,null,null,null,"1001XX0009.ldt",1,null,null,null,null,0,null,null,null,null,null,null,"LED",16,null,"",null,null,24,null,4000,80,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"","",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"Poland"]
["1002","1002XX0009","TRYSIL 263CM 4XLED 6256LM DOWN 3000K DALI",null,"Luminaire with a contemporary design. For lighting gardens, private areas, and other architectural concepts",null,"Trysil","Post","Europe, Africa, Asia, Australia and Oceania, North America, South America",2,256,2.63,0,"",null,null,null,null,null,null,null,"1002XX0009.png",7,1,2,5,8,3,66,"CE","","IK10","Class I",null,null,null,null,null,1.18,0.24,2.63,null,null,null,null,"1002XX0009.ldt",1,null,null,null,null,0,null,null,null,null,null,null,"LED",16,null,"",null,null,23,null,3000,80,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"DALI","",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"Poland"]
["1003","1003XX0009","TRYSIL 263CM 4XLED 6648LM DOWN 4000K DALI",null,"Luminaire with a contemporary design. For lighting gardens, private areas, and other architectural concepts",null,"Trysil","Post","Europe, Africa, Asia, Australia and Oceania, North America, South America",2,256,2.63,0,"",null,null,null,null,null,null,null,"1003XX0009.png",7,1,2,5,8,3,66,"CE","","IK10","",null,null,null,null,null,1.18,0.24,2.63,null,null,null,null,"1003XX0009.ldt",1,null,null,null,null,0,null,null,null,null,null,null,"LED",16,null,"",null,null,24,null,4000,80,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"DALI","",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"Poland"]
["1006","1006XX0009","TRYSIL 263CM 2XLED 2317LM VSM 3000K DALI2",null,"Luminaire with a contemporary design. For lighting gardens, private areas, and other architectural concepts",null,"Trysil","Pole","Europe, Africa, Asia, Australia and Oceania, North America, South America",2,256,2.63,0,"",null,null,null,null,null,null,null,"1006XX0009.png",4,1,2,5,8,3,66,"CE","","IK10","Class I",null,null,null,null,null,1.18,0.24,2.63,null,null,null,null,"1006XX0009.ldt",1,null,null,null,null,0,null,null,null,null,null,null,"LED",16,null,"",null,null,23,null,3000,70,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"DALI","",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"Poland"]
["1007","1007XX0009","TRYSIL 263CM 2XLED 2509LM VSM 4000K DALI2",null,"Luminaire with a contemporary design. For lighting gardens, private areas, and other architectural concepts",null,"Trysil","Pole","Europe, Africa, Asia, Australia and Oceania, North America, South America",2,256,2.63,0,"",null,null,null,null,null,null,null,"1007XX0009.png",4,1,2,5,8,3,66,"CE","","","Class I",null,null,null,null,null,1.18,0.24,2.63,null,null,null,null,"1007XX0009.ldt",1,null,null,null,null,0,null,null,null,null,null,null,"LED",16,null,"",null,null,24,null,4000,70,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"DALI","",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"Poland"]
["1010","1010XX0009","TRYSIL 263CM 2XLED 2317LM SCL 3000K DALI2",null,"Luminaire with a contemporary design. For lighting gardens, private areas, and other architectural concepts",null,"Trysil","Pole","Europe, Africa, Asia, Australia and Oceania, North America, South America",2,256,2.63,0,"",null,null,null,null,null,null,null,"1010XX0009.png",6,1,2,5,8,3,66,"CE","","IK10","Class I",null,null,null,null,null,1.18,0.24,2.63,null,null,null,null,"1010XX0009.ldt",1,null,null,null,null,0,null,null,null,null,null,null,"LED",16,null,"",null,null,23,null,3000,70,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"DALI","",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"Poland"]
["1011","1011XX0009","TRYSIL 263CM 2XLED 2509LM SCL 4000K DALI2",null,"Luminaire with a contemporary design. For lighting gardens, private areas, and other architectural concepts",null,"Trysil","Pole","Europe, Africa, Asia, Australia and Oceania, North America, South America",2,256,2.63,0,"",null,null,null,null,null,null,null,"1011XX0009.png",6,1,2,5,8,3,66,"CE","","IK10","Class I",null,null,null,null,null,1.18,0.24,2.63,null,null,null,null,"1011XX0009.ldt",1,null,null,null,null,0,null,null,null,null,null,null,"LED",16,null,"",null,null,24,null,4000,70,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"DALI","",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"Poland"]
["1012","1012XX0009","TRYSIL 300CM 4XLED 5496LM 3000K DIM.",null,"For lighting private areas and other architectural concepts",null,"Trysil","Post","Europe, Africa, Asia, Australia and Oceania, North America, South America",2,256,3,0,"",null,null,null,null,null,null,null,"1012XX0009.png",7,1,2,5,8,1,66,"CE","","IK10","Class I",null,null,null,null,null,1.18,0.24,3,null,null,null,null,"1012XX0009.ldt",1,null,null,null,null,0,null,null,null,null,null,null,"LED",16,null,"",null,null,23,null,3000,80,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"","",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"Poland"]
["1013","1013XX0009","TRYSIL 300CM 4XLED 5840LM 4000K DIM.",null,"For lighting private areas and other architectural concepts",null,"Trysil","Post","Europe, Africa, Asia, Australia and Oceania, North America, South America",2,256,3,0,"",null,null,null,null,null,null,null,"1013XX0009.png",7,1,2,5,8,1,66,"CE","","IK10","Class I",null,null,null,null,null,1.18,0.24,3,null,null,null,null,"1013XX0009.ldt",1,null,null,null,null,0,null,null,null,null,null,null,"LED",16,null,"",null,null,24,null,4000,80,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"","",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"Poland"]
["1024","1024XX0009","TRYSIL 350CM 4XLED 5496LM 3000K DIM.",null,"For lighting private areas and other architectural concepts",null,"Trysil","Post","Europe, Africa, Asia, Australia and Oceania, North America, South America",2,256,3.5,0,"",null,null,null,null,null,null,null,"1024XX0009.png",7,1,2,5,8,1,66,"CE","","IK10","Class I",null,null,null,null,null,1.18,0.24,3.5,null,null,null,null,"1024XX0009.ldt",1,null,null,null,null,0,null,null,null,null,null,null,"LED",16,null,"",null,null,23,null,3000,80,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"","",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"Poland"]
["1025","1025XX0009","TRYSIL 350CM 4XLED 5840LM 4000K DIM.",null,"For lighting private areas and other architectural concepts",null,"Trysil","Post","Europe, Africa, Asia, Australia and Oceania, North America, South America",2,256,3.5,0,"",null,null,null,null,null,null,null,"1025XX0009.png",7,1,2,5,8,1,66,"CE","","IK10","Class I",null,null,null,null,null,1.18,0.24,3.5,null,null,null,null,"1025XX0009.ldt",1,null,null,null,null,0,null,null,null,null,null,null,"LED",16,null,"",null,null,24,null,4000,80,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"","",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"Poland"]
["1036","1036XX0009","TRYSIL 400CM 4XLED 5496LM DOWN 3000K DIM.",null,"For lighting private areas and other architectural concepts",null,"Trysil","Post","Europe, Africa, Asia, Australia and Oceania, North America, South America",2,256,4,0,"",null,null,null,null,null,null,null,"1036XX0009.png",7,1,2,5,8,1,66,"CE","","IK10","Class I",null,null,null,null,null,1.18,0.24,4,null,null,null,null,"1036XX0009.ldt",1,null,null,null,null,0,null,null,null,null,null,null,"LED",16,null,"",null,null,23,null,3000,80,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"","",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"Poland"]
["1037","1037XX0009","TRYSIL 400CM 4XLED 5840LM 4000K DIM.",null,"For lighting private areas and other architectural concepts",null,"Trysil","Post","Europe, Africa, Asia, Australia and Oceania, North America, South America",2,256,4,0,"",null,null,null,null,null,null,null,"1037XX0009.png",7,1,2,5,8,1,66,"CE","","IK10","Class I",null,null,null,null,null,1.18,0.24,4,null,null,null,null,"1037XX0009.ldt",1,null,null,null,null,0,null,null,null,null,null,null,"LED",16,null,"",null,null,24,null,4000,80,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"","",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"Poland"]
["1038","1038XX0009","TRYSIL 400CM 4XLED 6256LM DOWN 3000K DALI",null,"Luminaire with a contemporary design. For lighting gardens, private areas and other architectural concepts",null,"Trysil","Post","Europe, Africa, Asia, Australia and Oceania, North America, South America",2,256,4,0,"",null,null,null,null,null,null,null,"1038XX0009.png",7,1,2,5,8,3,66,"CE","","IK10","Class I",null,null,null,null,null,1.18,0.24,4,null,null,null,null,"1038XX0009.ldt",1,null,null,null,null,0,null,null,null,null,null,null,"LED",16,null,"",null,null,23,null,3000,80,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"DALI","",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"Poland"]
["1039","1039XX0009","TRYSIL 400CM 4XLED 6648LM DOWN 4000K DALI",null,"Luminaire with a contemporary design. For lighting gardens, private areas and other architectural concepts",null,"Trysil","Post","Europe, Africa, Asia, Australia and Oceania, North America, South America",2,256,4,0,"",null,null,null,null,null,null,null,"1039XX0009.png",7,1,2,5,8,3,66,"CE","","IK10","Class I",null,null,null,null,null,1.18,0.24,4,null,null,null,null,"1039XX0009.ldt",1,null,null,null,null,0,null,null,null,null,null,null,"LED",16,null,"",null,null,24,null,4000,80,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"DALI","",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"Poland"]
["1042","1042XX0009","TRYSIL 400CM 2XLED 3382LM VSM 3000K DALI2",null,"Luminaire with a contemporary design. For lighting gardens, private areas and other architectural concepts",null,"Trysil","Pole","Europe, Africa, Asia, Australia and Oceania, North America, South America",2,256,4,0,"",null,null,null,null,null,null,null,"1042XX0009.png",4,1,2,5,8,3,66,"CE","","IK10","Class I",null,null,null,null,null,1.18,0.24,4,null,null,null,null,"1042XX0009.ldt",1,null,null,null,null,0,null,null,null,null,null,null,"LED",16,null,"",null,null,23,null,3000,70,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"DALI","",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"Poland"]
["1043","1043XX0009","TRYSIL 400CM 2XLED 3663LM VSM 4000K DALI2",null,"Luminaire with a contemporary design. For lighting gardens, private areas and other architectural concepts",null,"Trysil","Pole","Europe, Africa, Asia, Australia and Oceania, North America, South America",2,256,4,0,"",null,null,null,null,null,null,null,"1043XX0009.png",4,1,2,5,8,3,66,"CE","","IK10","Class I",null,null,null,null,null,1.18,0.24,4,null,null,null,null,"1043XX0009.ldt",1,null,null,null,null,0,null,null,null,null,null,null,"LED",16,null,"",null,null,24,null,4000,70,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"DALI","",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"Poland"]
["1046","1046XX0009","TRYSIL 400CM 2XLED 3382LM SCL 3000K DALI2",null,"Luminaire with a contemporary design. For lighting gardens, private areas and other architectural concepts",null,"Trysil","Pole","Europe, Africa, Asia, Australia and Oceania, North America, South America",2,256,4,0,"",null,null,null,null,null,null,null,"1046XX0009.png",6,1,2,5,8,3,66,"CE","","IK10","Class I",null,null,null,null,null,1.18,0.24,4,null,null,null,null,"1046XX0009.ldt",1,null,null,null,null,0,null,null,null,null,null,null,"LED",16,null,"",null,null,23,null,3000,70,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"DALI","",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"Poland"]
["1047","1047XX0009","TRYSIL 400CM 2XLED 3663LM SCL 4000K DALI2",null,"Luminaire with a contemporary design. For lighting gardens, private areas and other architectural concepts",null,"Trysil","Pole","Europe, Africa, Asia, Australia and Oceania, North America, South America",2,256,4,0,"",null,null,null,null,null,null,null,"1047XX0009.png",6,1,2,5,8,3,66,"CE","","IK10","Class I",null,null,null,null,null,1.18,0.24,4,null,null,null,null,"1047XX0009.ldt",1,null,null,null,null,0,null,null,null,null,null,null,"LED",16,null,"",null,null,24,null,4000,70,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"DALI","",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"Poland"]
["1048","1048XX0009","TRYSIL 263CM 2XLED 1988LM 3000K DIM.",null,"For lighting private areas and other architectural concepts",null,"Trysil","Post,Post complete","Europe, Africa, Asia, Australia and Oceania, North America, South America",2,256,2.63,0,"",null,null,null,null,null,null,null,"1048XX0009.png",3,1,2,5,8,1,66,"CE","","IK10","Class I",null,null,null,null,null,0.71,0.24,2.63,null,null,null,null,"1048XX0009.ldt",1,null,null,null,null,0,null,null,null,null,null,null,"LED",16,null,"",null,null,23,null,3000,80,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"","",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"Poland"]
["1049","1049XX0009","TRYSIL 263CM 2XLED 2084LM 4000K DIM.",null,"For lighting private areas and other architectural concepts",null,"Trysil","Post,Post complete","Europe, Africa, Asia, Australia and Oceania, North America, South America",2,256,2.63,0,"",null,null,null,null,null,null,null,"1049XX0009.png",3,1,2,5,8,1,66,"CE","","IK10","Class I",null,null,null,null,null,0.71,0.24,2.63,null,null,null,null,"1049XX0009.ldt",1,null,null,null,null,0,null,null,null,null,null,null,"LED",16,null,"",null,null,24,null,4000,80,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"","",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"Poland"]
["1054","1054XX0009","TRYSIL 263CM LED 1158LM VSM 3000K DALI2",null,"Luminaire with a contemporary design For lighting gardens, private areas and other architectural concepts",null,"Trysil","Pole","Europe, Africa, Asia, Australia and Oceania, North America, South America",2,256,2.63,0,"",null,null,null,null,null,null,null,"1054XX0009.png",4,1,2,5,8,3,66,"CE","","IK10","Class I",null,null,null,null,null,0.71,0.24,2.63,null,null,null,null,"1054XX0009.ldt",1,null,null,null,null,0,null,null,null,null,null,null,"LED",16,null,"",null,null,23,null,3000,70,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"DALI","",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"Poland"]
["1055","1055XX0009","TRYSIL 263CM LED 1254LM VSM 4000K DALI2",null,"Luminaire with a contemporary design For lighting gardens, private areas and other architectural concepts",null,"Trysil","Pole","Europe, Africa, Asia, Australia and Oceania, North America, South America",2,256,2.63,0,"",null,null,null,null,null,null,null,"1055XX0009.png",4,1,2,5,8,3,66,"CE","","IK10","Class I",null,null,null,null,null,0.71,0.24,2.63,null,null,null,null,"1055XX0009.ldt",1,null,null,null,null,0,null,null,null,null,null,null,"LED",16,null,"",null,null,24,null,4000,70,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"DALI","",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"Poland"]
["1058","1058XX0009","TRYSIL 263CM LED 11585LM SCL 3000K DALI2",null,"Luminaire with a contemporary design For lighting gardens, private areas and other architectural concepts",null,"Trysil","Pole","Europe, Africa, Asia, Australia and Oceania, North America, South America",2,256,2.63,0,"",null,null,null,null,null,null,null,"1058XX0009.png",6,1,2,5,8,3,66,"CE","","IK10","Class I",null,null,null,null,null,0.71,0.24,2.63,null,null,null,null,"1058XX0009.ldt",1,null,null,null,null,0,null,null,null,null,null,null,"LED",16,null,"",null,null,23,null,3000,70,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"DALI","",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"Poland"]
["1059","1059XX0009","TRYSIL 263CM LED 1254LM SCL 4000K DALI2",null,"Luminaire with a contemporary design For lighting gardens, private areas and other architectural concepts",null,"Trysil","Pole","Europe, Africa, Asia, Australia and Oceania, North America, South America",2,256,2.63,0,"",null,null,null,null,null,null,null,"1059XX0009.png",6,1,2,5,8,3,66,"CE","","","Class I",null,null,null,null,null,0.71,0.24,2.63,null,null,null,null,"1059XX0009.ldt",1,null,null,null,null,0,null,null,null,null,null,null,"LED",16,null,"",null,null,24,null,4000,70,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"DALI","",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"Poland"]
["1060","1060XX0009","TRYSIL 300CM 2XLED 2748LM DOWN 3000K DIM.",null,"For lighting private areas and other architectural concepts",null,"Trysil","Post","Europe, Africa, Asia, Australia and Oceania, North America, South America",2,256,3,0,"",null,null,null,null,null,null,null,"1060XX0009.png",7,1,2,5,8,1,66,"CE","","IK10","Class I",null,null,null,null,null,0.71,0.24,3,null,null,null,null,"1060XX0009.ldt",1,null,null,null,null,0,null,null,null,null,null,null,"LED",16,null,"",null,null,23,null,3000,80,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"","",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"Poland"]
["1061","1061XX0009","TRYSIL 300CM 2XLED 2920LM DOWN 4000K DIM.",null,"For lighting private areas and other architectural concepts",null,"Trysil","Post","Europe, Africa, Asia, Australia and Oceania, North America, South America",2,{"$f":"IFERROR(INDEX(TYPMONT,MATCH((INDEX(DB,MATCH($A53,ID,0),31)),ID_RODZ,0),3),\"\")","v":256},3,0,"",null,null,null,null,null,null,null,"1061XX0009.png",7,1,2,5,8,1,66,"CE","","IK10","Class I",null,null,null,null,null,0.71,0.24,3,null,null,null,null,"1061XX0009.ldt",1,null,null,null,null,0,null,null,null,null,null,null,"LED",16,null,"",null,null,24,null,4000,80,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"","",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"Poland"]
["1072","1072XX0009","TRYSIL 350CM 2XLED 2748LM DOWN 3000K DIM.",null,"For lighting private areas and other architectural concepts",null,"Trysil","Post","Europe, Africa, Asia, Australia and Oceania, North America, South America",2,256,3.5,0,"",null,null,null,null,null,null,null,"1072XX0009.png",7,1,2,5,8,1,66,"CE","","IK10","Class I",null,null,null,null,null,0.71,0.24,3.5,null,null,null,null,"1072XX0009.ldt",1,null,null,null,null,0,null,null,null,null,null,null,"LED",16,null,"",null,null,23,null,3000,80,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"","",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"Poland"]
["1073","1073XX0009","TRYSIL 350CM 2XLED 2920LM DOWN 4000K DIM.",null,"For lighting private areas and other architectural concepts",null,"Trysil","Post","Europe, Africa, Asia, Australia and Oceania, North America, South America",2,256,3.5,0,"",null,null,null,null,null,null,null,"1073XX0009.png",7,1,2,5,8,1,66,"CE","","IK10","Class I",null,null,null,null,null,0.71,0.24,3.5,null,null,null,null,"1073XX0009.ldt",1,null,null,null,null,0,null,null,null,null,null,null,"LED",16,null,"",null,null,24,null,4000,80,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"","",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"Poland"]
["1084","1084XX0009","TRYSIL 400CM 2XLED 2748LM DOWN 3000K DIM.",null,"For lighting gardens, private areas and other architectural concepts",null,"Trysil","Post","Europe, Africa, Asia, Australia and Oceania, North America, South America",2,256,4,0,"",null,null,null,null,null,null,null,"1084XX0009.png",7,1,2,5,8,1,66,"CE","","IK10","Class I",null,null,null,null,null,0.71,0.24,4,null,null,null,null,"1084XX0009.ldt",1,null,null,null,null,0,null,null,null,null,null,null,"LED",16,null,"",null,null,23,null,3000,80,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"","",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"Poland"]
["1085","1085XX0009","TRYSIL 400CM 2XLED 2920LM DOWN 4000K DIM.",null,"For lighting gardens, private areas and other architectural concepts",null,"Trysil","Post","Europe, Africa, Asia, Australia and Oceania, North America, South America",2,256,4,0,"",null,null,null,null,null,null,null,"1085XX0009.png",7,1,2,5,8,1,66,"CE","","IK10","Class I",null,null,null,null,null,0.71,0.24,4,null,null,null,null,"1085XX0009.ldt",1,null,null,null,null,0,null,null,null,null,null,null,"LED",16,null,"",null,null,24,null,4000,80,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"","",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"Poland"]
["1090","1090XX0009","TRYSIL 400CM LED 1691LM VSM 3000K DALI2",null,"Luminaire with a contemporary design For lighting gardens, private areas and other architectural concepts",null,"Trysil","Pole","Europe, Africa, Asia, Australia and Oceania, North America, South America",2,256,4,0,"",null,null,null,null,null,null,null,"1090XX0009.png",4,1,2,5,8,3,66,"CE","","IK10","Class I",null,null,null,null,null,0.71,0.24,4,null,null,null,null,"1090XX0009.ldt",1,null,null,null,null,0,null,null,null,null,null,null,"LED",16,null,"",null,null,23,null,3000,70,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"DALI","",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"Poland"]
["1091","1091XX0009","TRYSIL 400CM LED 1831LM VSM 4000K DALI2",null,"Luminaire with a contemporary design For lighting gardens, private areas and other architectural concepts",null,"Trysil","Pole","Europe, Africa, Asia, Australia and Oceania, North America, South America",2,256,4,0,"",null,null,null,null,null,null,null,"1091XX0009.png",4,1,2,5,8,3,66,"CE","","IK10","Class I",null,null,null,null,null,0.71,0.24,4,null,null,null,null,"1091XX0009.ldt",1,null,null,null,null,0,null,null,null,null,null,null,"LED",16,null,"",null,null,24,null,4000,70,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"DALI","",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"Poland"]
["1094","1094XX0009","TRYSIL 400CM LED 1691LM SCL 3000K DALI2",null,"Luminaire with a contemporary design For lighting gardens, private areas and other architectural concepts",null,"Trysil","Pole","Europe, Africa, Asia, Australia and Oceania, North America, South America",2,256,4,0,"",null,null,null,null,null,null,null,"1094XX0009.png",6,1,2,5,8,3,66,"CE","","IK10","Class I",null,null,null,null,null,0.71,0.24,4,null,null,null,null,"1094XX0009.ldt",1,null,null,null,null,0,null,null,null,null,null,null,"LED",16,null,"",null,null,23,null,3000,70,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"DALI","",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"Poland"]
["1095","1095XX0009","TRYSIL 400CM LED 1831LM SCL 4000K DALI2",null,"Luminaire with a contemporary design For lighting gardens, private areas and other architectural concepts",null,"Trysil","Pole","Europe, Africa, Asia, Australia and Oceania, North America, South America",2,256,4,0,"",null,null,null,null,null,null,null,"1095XX0009.png",6,1,2,5,8,3,66,"CE","","IK10","Class I",null,null,null,null,null,0.71,0.24,4,null,null,null,null,"1095XX0009.ldt",1,null,null,null,null,0,null,null,null,null,null,null,"LED",16,null,"",null,null,24,null,4000,70,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"DALI","",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"Poland"]
["1096","1096XX0009","TRYSIL BOLLARD 85CM 2XLED 1010LM 3000K DIM.",null,"Luminaire with a contemporary design For lighting gardens, private areas and other architectural concepts",null,"Trysil","Bollard","Europe, Africa, Asia, Australia and Oceania, North America, South America",2,2,0.8,0,"",null,null,null,null,null,null,null,"1096XX0009.png",7,1,2,3,6,1,66,"CE","","IK10","",null,null,null,null,null,0.34,0.11,0.85,null,null,null,null,"1096XX0009.ldt",1,null,null,null,null,0,null,null,null,null,null,null,"LED",16,null,"",null,null,23,null,3000,80,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"","",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"Poland"]
["1097","1097XX0009","TRYSIL BOLLARD 85CM 2XLED 1069LM 4000K DIM.",null,"Luminaire with a contemporary design For lighting gardens, private areas and other architectural concepts",null,"Trysil","Bollard","Europe, Africa, Asia, Australia and Oceania, North America, South America",2,2,0.8,0,"",null,null,null,null,null,null,null,"1097XX0009.png",7,1,2,3,6,1,66,"CE","","IK10","",null,null,null,null,null,0.34,0.11,0.85,null,null,null,null,"1097XX0009.ldt",1,null,null,null,null,0,null,null,null,null,null,null,"LED",16,null,"",null,null,24,null,4000,80,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"","",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"Poland"]
["1100","1100XX0009","TRYSIL BOLLARD 85CM LED 828LM VSM 3000K DIM.",null,"Luminaire with a contemporary design For lighting gardens, private areas and other architectural concepts",null,"Trysil","Bollard","Europe, Africa, Asia, Australia and Oceania, North America, South America",2,2,0.8,0,"",null,null,null,null,null,null,null,"1100XX0009.png",4,1,2,3,6,1,66,"CE","","IK08","Class I",null,null,null,null,null,0.34,0.11,0.85,null,null,null,null,"1100XX0009.ldt",1,null,null,null,null,0,null,null,null,null,null,null,"LED",16,null,"",null,null,23,null,3000,80,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"","",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"Poland"]
["1101","1101XX0009","TRYSIL BOLLARD 85CM LED 828LM VSM 4000K DIM.",null,"Luminaire with a contemporary design For lighting gardens, private areas and other architectural concepts",null,"Trysil","Bollard","Europe, Africa, Asia, Australia and Oceania, North America, South America",2,2,0.8,0,"",null,null,null,null,null,null,null,"1101XX0009.png",4,1,2,3,6,1,66,"CE","","IK08","Class I",null,null,null,null,null,0.34,0.11,0.85,null,null,null,null,"1101XX0009.ldt",1,null,null,null,null,0,null,null,null,null,null,null,"LED",16,null,"",null,null,24,null,4000,80,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"","",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"Poland"]
["1102","1102XX0009","TRYSIL BOLLARD 85CM LED 828LM VSM 3000K DALI2",null,"Luminaire with a contemporary design For lighting gardens, private areas and other architectural concepts",null,"Trysil","Bollard","Europe, Africa, Asia, Australia and Oceania, North America, South America",2,2,0.8,0,"",null,null,null,null,null,null,null,"1102XX0009.png",4,1,2,3,6,3,66,"CE","","IK08","Class I",null,null,null,null,null,0.34,0.11,0.85,null,null,null,null,"1102XX0009.ldt",1,null,null,null,null,0,null,null,null,null,null,null,"LED",16,null,"",null,null,23,null,3000,80,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"DALI","",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"Poland"]
["1103","1103XX0009","TRYSIL BOLLARD 85CM LED 828LM VSM 4000K DALI2",null,"Luminaire with a contemporary design For lighting gardens, private areas and other architectural concepts",null,"Trysil","Bollard","Europe, Africa, Asia, Australia and Oceania, North America, South America",2,2,0.8,0,"",null,null,null,null,null,null,null,"1103XX0009.png",4,1,2,3,6,3,66,"CE","","IK08","Class I",null,null,null,null,null,0.34,0.11,0.85,null,null,null,null,"1103XX0009.ldt",1,null,null,null,null,0,null,null,null,null,null,null,"LED",16,null,"",null,null,24,null,4000,80,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"DALI","",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"Poland"]
["1104","1104XX0009","TRYSIL BOLLARD 85CM LED 828LM SCL 3000K DIM.",null,"Luminaire with a contemporary design For lighting gardens, private areas and other architectural concepts",null,"Trysil","Bollard","Europe, Africa, Asia, Australia and Oceania, North America, South America",2,2,0.8,0,"",null,null,null,null,null,null,null,"1104XX0009.png",6,1,2,3,6,1,66,"CE","","IK08","Class I",null,null,null,null,null,0.34,0.11,0.85,null,null,null,null,"1104XX0009.ldt",1,null,null,null,null,0,null,null,null,null,null,null,"LED",16,null,"",null,null,23,null,3000,80,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"","",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"Poland"]
["1105","1105XX0009","TRYSIL BOLLARD 85CM LED 828LM SCL 4000K DIM.",null,"Luminaire with a contemporary design For lighting gardens, private areas and other architectural concepts",null,"Trysil","Bollard","Europe, Africa, Asia, Australia and Oceania, North America, South America",2,2,0.8,0,"",null,null,null,null,null,null,null,"1105XX0009.png",6,1,2,3,6,1,66,"CE","","IK08","Class I",null,null,null,null,null,0.34,0.11,0.85,null,null,null,null,"1105XX0009.ldt",1,null,null,null,null,0,null,null,null,null,null,null,"LED",16,null,"",null,null,24,null,4000,80,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"","",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"Poland"]
["1106","1106XX0009","TRYSIL BOLLARD 85CM LED 828LM SCL 3000K DALI2",null,"Luminaire with a contemporary design For lighting gardens, private areas and other architectural concepts",null,"Trysil","Bollard","Europe, Africa, Asia, Australia and Oceania, North America, South America",2,2,0.8,0,"",null,null,null,null,null,null,null,"1106XX0009.png",6,1,2,3,6,3,66,"CE","","IK08","Class I",null,null,null,null,null,0.34,0.11,0.85,null,null,null,null,"1106XX0009.ldt",1,null,null,null,null,0,null,null,null,null,null,null,"LED",16,null,"",null,null,23,null,3000,80,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"DALI","",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"Poland"]
["1107",{"$f":"INDEX(DB,MATCH($A71,ID,0),2)","v":"1107XX0009"},{"$f":"INDEX(DB,MATCH($A71,ID,0),3)","v":"TRYSIL BOLLARD 85CM LED 828LM SCL 4000K DALI2"},null,{"$f":"IF(INDEX(DB,MATCH($A71,ID,0),35)=0,\"\",INDEX(DB,MATCH($A71,ID,0),35))","v":"Luminaire with a contemporary design For lighting gardens, private areas and other architectural concepts"},null,"Trysil",{"$f":"IF(INDEX(DB,MATCH($A71,ID,0),5)=0,\"\",INDEX(DB,MATCH($A71,ID,0),5))","v":"Bollard"},"Europe, Africa, Asia, Australia and Oceania, North America, South America",2,{"$f":"IFERROR(INDEX(TYPMONT,MATCH((INDEX(DB,MATCH($A71,ID,0),31)),ID_RODZ,0),3),\"\")","v":2},0.8,0,{"$f":"IFERROR(IF(INDEX(TYPMONT,MATCH((INDEX(DB,MATCH($A71,ID,0),31)),ID_RODZ,0),6)=0,\"\",INDEX(TYPMONT,MATCH((INDEX(DB,MATCH($A71,ID,0),31)),ID_RODZ,0),6)),\"\")","v":""},null,null,null,null,null,null,null,{"$f":"IF(INDEX(DB,MATCH($A71,ID,0),57)=0,\"\",INDEX(DB,MATCH($A71,ID,0),57))","v":"1107XX0009.png"},{"$f":"IF((IFERROR(INDEX(BRYLA_FOTO,MATCH(INDEX(DB,MATCH($A71,ID,0),62),ID_BRYLAFOTO,0),6),\"\"))<>0,IFERROR(INDEX(BRYLA_FOTO,MATCH(INDEX(DB,MATCH($A71,ID,0),62),ID_BRYLAFOTO,0),6),\"\"),\"\")","v":6},{"$f":"IF(INDEX(DB,MATCH($A71,ID,0),61)=0,\"\",INDEX(DB,MATCH($A71,ID,0),61))","v":1},2,{"$f":"IFERROR(INDEX(TYPMONT,MATCH((INDEX(DB,MATCH($A71,ID,0),31)),ID_RODZ,0),1),\"\")","v":3},{"$f":"IFERROR(INDEX(TYPMONT,MATCH((INDEX(DB,MATCH($A71,ID,0),31)),ID_RODZ,0),2),\"\")","v":6},{"$f":"IF(INDEX(DB,MATCH($A71,ID,0),59)=0,\"\",INDEX(DB,MATCH($A71,ID,0),59))","v":3},{"$f":"IFERROR(IF(INDEX(DB,MATCH($A71,ID,0),19)=0,\"\",INDEX(DB,MATCH($A71,ID,0),19)+1),\"\")","v":66},{"$f":"IF(INDEX(DB,MATCH($A71,ID,0),27)=0,\"\",INDEX(DB,MATCH($A71,ID,0),27))","v":"CE"},"",{"$f":"IF(INDEX(DB,MATCH($A71,ID,0),20)=0,\"\",INDEX(DB,MATCH($A71,ID,0),20))","v":"IK08"},{"$f":"IF(INDEX(DB,MATCH($A71,ID,0),21)=0,\"\",INDEX(DB,MATCH($A71,ID,0),21))","v":"Class I"},null,null,null,null,null,{"$f":"INDEX(DB,MATCH($A71,ID,0),24)","v":0.34},{"$f":"INDEX(DB,MATCH($A71,ID,0),25)","v":0.11},{"$f":"INDEX(DB,MATCH($A71,ID,0),26)","v":0.85},null,null,null,null,{"$f":"IF(INDEX(DB,MATCH($A71,ID,0),58)=0,\"\",INDEX(DB,MATCH($A71,ID,0),58))","v":"1107XX0009.ldt"},1,null,null,null,null,0,null,null,null,null,null,null,"LED",16,null,{"$f":"IF(INDEX(DB,MATCH($A71,ID,0),60)=0,\"\",INDEX(DB,MATCH($A71,ID,0),60))","v":""},null,null,24,null,{"$f":"IF(INDEX(DB,MATCH($A71,ID,0),22)=0,\"\",INDEX(DB,MATCH($A71,ID,0),22))","v":4000},{"$f":"IF(INDEX(DB,MATCH($A71,ID,0),53)=0,\"\",INDEX(DB,MATCH($A71,ID,0),53))","v":80},null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,{"$f":"IF(INDEX(DB,MATCH($A71,ID,0),29)=0,\"\",INDEX(DB,MATCH($A71,ID,0),29))","v":"DALI"},{"$f":"IF(INDEX(DB,MATCH($A71,ID,0),28)=0,\"\",INDEX(DB,MATCH($A71,ID,0),28))","v":""},null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"Poland"]
["1108","1108XX0009","TRYSIL BOLLARD 85CM LED 1080LM 3000K ON/OFF",null,"Luminaire with a contemporary design. For lighting gardens and other private and public areas",null,{"$f":"IF(INDEX(DB,MATCH($A72,ID,0),4)=0,\"\",INDEX(DB,MATCH($A72,ID,0),4))","v":"Trysil"},"Bollard","Europe, Africa, Asia, Australia and Oceania, North America, South America",2,2,0.8,0,"",null,null,null,null,null,null,null,"1108XX0009.png",7,1,2,3,6,4,66,"CE",{"$f":"IFERROR(IF(FIND(\"RENA\",$C72)>0,\"Vehicle resistant\",\"\"),\"\")","v":""},"IK08","Class I",null,null,null,null,null,0.34,0.11,0.85,null,null,null,null,"1108XX0009.ldt",{"$f":"IF($BJ72=\"\",1,0)","v":1},null,null,null,null,0,null,null,null,null,null,null,"LED",16,null,"",null,null,{"$f":"IF($BO72=4000,24,23)","v":23},null,3000,80,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"","",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"Poland"]
["1109","1109XX0009","TRYSIL BOLLARD 85CM LED 1150LM 4000K ON/OFF",null,"Luminaire with a contemporary design For lighting gardens and other private and public areas",null,"Trysil","Bollard","Europe, Africa, Asia, Australia and Oceania, North America, South America",2,2,0.8,0,"",null,null,null,null,null,null,null,"1109XX0009.png",7,1,2,3,6,4,66,"CE","","IK08","Class I",null,null,null,null,null,0.34,0.11,0.85,null,null,null,null,"1109XX0009.ldt",1,null,null,null,null,0,null,null,null,null,null,null,"LED",16,null,"",null,null,24,null,4000,80,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"","",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"Poland"]
["1159","1159XX0009","KOSTER DOUBLE HEAD POLE-TOP 2XLED 4100LM 4000K ON/OFF",null,"Top-mounted luminaire, designed to be mounted on a lighting pole with a Ø50mm mounting shaft",null,"Koster","Post,Head","Europe, Africa, Asia, Australia and Oceania, North America, South America",2,512,4,0,"",null,null,null,null,null,null,null,"1159XX0009.png",3,1,2,5,9,4,66,"CE","","IK10","Class I",null,null,null,null,null,0.82,0.24,0.22,null,null,null,null,"1159XX0009.ldt",1,null,null,null,null,0,null,null,null,null,null,null,"LED",16,null,"",null,null,24,null,4000,80,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"","",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"Poland"]
["1165","1165XX0009","KOSTER DOUBLE HEAD POLE-TOP 4XLED 5200LM VSM 3000K DIM. TRIAC",null,"Top-mounted luminaire, designed to be mounted on a lighting pole with a Ø50mm mounting shaft",null,"Koster","Post","Europe, Africa, Asia, Australia and Oceania, North America, South America",2,512,4,0,"",null,null,null,null,null,null,null,"1165XX0009.png",4,1,2,5,9,1,66,"CE","","IK10","Class II",null,null,null,null,null,0.82,0.24,0.22,null,null,null,null,"1165XX0009.ldt",1,null,null,null,null,0,null,null,null,null,null,null,"LED",16,null,"",null,null,23,null,3000,70,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"","",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"Poland"]
["1167","1167XX0009","KOSTER DOUBLE HEAD POLE-TOP 4XLED 5480LM VSM 4000K DIM. TRIAC",null,"Top-mounted luminaire, designed to be mounted on a lighting pole with a Ø60mm mounting shaft",null,"Koster","Post,Head","Europe, Africa, Asia, Australia and Oceania, North America, South America",2,512,4,0,"",null,null,null,null,null,null,null,"1167XX0009.png",4,1,2,5,9,1,66,"CE","","IK10","Class II",null,null,null,null,null,0.82,0.24,0.22,null,null,null,null,"1167XX0009.ldt",1,null,null,null,null,0,null,null,null,null,null,null,"LED",16,null,"",null,null,24,null,4000,70,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"","",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"Poland"]
["1173","1173XX0009","KOSTER DOUBLE HEAD POLE-TOP 4XLED 5200LM VSM 3000K DALI2",null,"Top-mounted luminaire, designed to be mounted on a lighting pole with a Ø60mm mounting shaft",null,"Koster","Post,Head","Europe, Africa, Asia, Australia and Oceania, North America, South America",2,512,4,0,"",null,null,null,null,null,null,null,"1173XX0009.png",4,1,2,5,9,3,66,"CE","","IK10","Class I",null,null,null,null,null,0.82,0.24,0.22,null,null,null,null,"1173XX0009.ldt",1,null,null,null,null,0,null,null,null,null,null,null,"LED",16,null,"",null,null,23,null,3000,70,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"DALI","",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"Poland"]
["1175","1175XX0009","KOSTER DOUBLE HEAD POLE-TOP 4XLED 5480LM VSM 4000K DALI2",null,"Top-mounted luminaire, designed to be mounted on a lighting pole with a Ø60mm mounting shaft",null,"Koster","Post,Head","Europe, Africa, Asia, Australia and Oceania, North America, South America",2,512,4,0,"",null,null,null,null,null,null,null,"1175XX0009.png",4,1,2,5,9,3,66,"CE","","IK10","Class I",null,null,null,null,null,0.82,0.24,0.22,null,null,null,null,"1175XX0009.ldt",1,null,null,null,null,0,null,null,null,null,null,null,"LED",16,null,"",null,null,24,null,4000,70,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"DALI","",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"Poland"]
["1179","1179XX0009","KOSTER DOUBLE HEAD POLE-TOP 2XLED 3960LM 3000K ON/OFF",null,"Top-mounted luminaire, designed to be mounted on a lighting pole with a Ø60mm mounting shaft",null,"Koster","Post,Head","Europe, Africa, Asia, Australia and Oceania, North America, South America",2,512,4,0,"",null,null,null,null,null,null,null,"1179XX0009.png",3,1,2,5,9,4,66,"CE","","IK10","Class I",null,null,null,null,null,0.82,0.24,0.22,null,null,null,null,"1179XX0009.ldt",1,null,null,null,null,0,null,null,null,null,null,null,"LED",16,null,"",null,null,23,null,3000,80,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"","",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"Poland"]
["1181","1181XX0009","KOSTER DOUBLE HEAD POLE-TOP 2XLED 4100LM 4000K ON/OFF",null,"Top-mounted luminaire, designed to be mounted on a lighting pole with a Ø60mm mounting shaft",null,"Koster","Post,Head","Europe, Africa, Asia, Australia and Oceania, North America, South America",2,512,4,0,"",null,null,null,null,null,null,null,"1181XX0009.png",3,1,2,5,9,4,66,"CE","","IK10","Class I",null,null,null,null,null,0.82,0.24,0.22,null,null,null,null,"1181XX0009.ldt",1,null,null,null,null,0,null,null,null,null,null,null,"LED",16,null,"",null,null,24,null,4000,80,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"","",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"Poland"]
["1187","1187XX0009","KOSTER DOUBLE HEAD POLE-TOP 4XLED 5200LM VSM 3000K DIM. TRIAC",null,"Top-mounted luminaire, designed to be mounted on a lighting pole with a Ø60mm mounting shaft",null,"Koster","Post,Head","Europe, Africa, Asia, Australia and Oceania, North America, South America",2,512,4,0,"",null,null,null,null,null,null,null,"1187XX0009.png",4,1,2,5,9,1,66,"CE","","IK10","Class II",null,null,null,null,null,0.82,0.24,0.22,null,null,null,null,"1187XX0009.ldt",1,null,null,null,null,0,null,null,null,null,null,null,"LED",16,null,"",null,null,23,null,3000,70,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"","",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"Poland"]
["1189","1189XX0009","KOSTER DOUBLE HEAD POLE-TOP 4XLED 5480LM VSM 4000K DIM. TRIAC",null,"Top-mounted luminaire, designed to be mounted on a lighting pole with a Ø60mm mounting shaft",null,"Koster","Post,Head","Europe, Africa, Asia, Australia and Oceania, North America, South America",2,512,4,0,"",null,null,null,null,null,null,null,"1189XX0009.png",4,1,2,5,9,1,66,"CE","","IK10","Class II",null,null,null,null,null,0.82,0.24,0.22,null,null,null,null,"1189XX0009.ldt",1,null,null,null,null,0,null,null,null,null,null,null,"LED",16,null,"",null,null,24,null,4000,80,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"","",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"Poland"]
["1195","1195XX0009","KOSTER DOUBLE HEAD POLE-TOP 4XLED 5200LM VSM 3000K DALI2",null,"Top-mounted luminaire, designed to be mounted on a lighting pole with a Ø60mm mounting shaft",null,"Koster","Post,Head","Europe, Africa, Asia, Australia and Oceania, North America, South America",2,512,4,0,"",null,null,null,null,null,null,null,"1195XX0009.png",4,1,2,5,9,3,66,"CE","","IK10","Class I",null,null,null,null,null,0.82,0.24,0.22,null,null,null,null,"1195XX0009.ldt",1,null,null,null,null,0,null,null,null,null,null,null,"LED",16,null,"",null,null,23,null,3000,70,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"DALI","",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"Poland"]
["1197","1197XX0009","KOSTER DOUBLE HEAD POLE-TOP 4XLED 5480LM VSM 4000K DALI2",null,"Top-mounted luminaire, designed to be mounted on a lighting pole with a Ø60mm mounting shaft",null,"Koster","Post,Head","Europe, Africa, Asia, Australia and Oceania, North America, South America",2,512,4,0,"",null,null,null,null,null,null,null,"1197XX0009.png",4,1,2,5,9,3,66,"CE","","IK10","Class I",null,null,null,null,null,0.82,0.24,0.22,null,null,null,null,"1197XX0009.ldt",1,null,null,null,null,0,null,null,null,null,null,null,"LED",16,null,"",null,null,24,null,4000,70,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"DALI","",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"Poland"]
["120","120XX0011","VASA WALL E27 UP-DOWN",null,"A luminaire with a wide range of applications, among others for lighting: wall and facade surfaces and other architectural concepts",null,"Vasa","Wall","Europe, Africa, Asia, Australia and Oceania, North America, South America",2,4,0,2.5,"",null,null,null,null,null,null,null,"120XX0011.jpg",8,1,5,2,2,4,66,"CE","","IK08","Class I",null,null,null,null,null,0.31,0.12,0.16,null,null,null,null,"120XX0011.ldt",0,null,null,null,null,1,null,null,null,null,null,null,"LED",16,null,"E27",null,null,23,null,"",80,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"","",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"Poland"]
["1240","1240XX0013","STAVANGER BOLLARD 95CM LED 1179LM 3000K DIM.",null,"Bollard luminaire of stable and durable construction For lighting private areas and public spaces",null,"Stavanger","Bollard","Europe, Africa, Asia, Australia and Oceania, North America, South America",2,2,0.9,0,"",null,null,null,null,null,null,null,"1240XX0013.jpg",9,1,1,3,6,1,66,"CE","","IK10","Class I",null,null,null,null,null,0.2,0.2,0.95,null,null,null,null,"1240XX0013.ldt",1,null,null,null,null,0,null,null,null,null,null,null,"LED",16,null,"",null,null,23,null,3000,80,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"","",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"Poland"]
["1244","1244XX0013","STAVANGER BOLLARD 50CM LED 1179LM 3000K DIM.",null,"Bollard luminaire of stable and durable construction. For lighting private areas and public spaces",null,"Stavanger","Bollard","Europe, Africa, Asia, Australia and Oceania, North America, South America",2,2,0.45,0,"",null,null,null,null,null,null,null,"1244XX0013.jpg",9,1,1,3,6,1,66,"CE","","IK10","Class I",null,null,null,null,null,0.2,0.2,0.5,null,null,null,null,"1244XX0013.ldt",1,null,null,null,null,0,null,null,null,null,null,null,"LED",16,null,"",null,null,23,null,3000,80,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"","",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"Poland"]
["1247","1247XX0013","STAVANGER BOLLARD 28CM LED 854LM 3000K DIM.",null,"Bollard luminaire of stable and durable construction. For lighting private areas and public spaces",null,"Stavanger","Bollard","Europe, Africa, Asia, Australia and Oceania, North America, South America",2,2,0.23,0,"",null,null,null,null,null,null,null,"1247XX0013.jpg",9,1,1,3,6,1,66,"CE","","IK10","Class I",null,null,null,null,null,0.2,0.2,0.28000000000000003,null,null,null,null,"1247XX0013.ldt",1,null,null,null,null,0,null,null,null,null,null,null,"LED",16,null,"",null,null,23,null,3000,80,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"","",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"Poland"]
["1260","1260XX0013","STOCKHOLM BOLLARD 49CM LED 1059LM 3000K DIM.",null,"A bollard luminaire with a stable and durable structure For lighting private areas and other architectural concepts",null,"Stockholm","Bollard","Europe, Africa, Asia, Australia and Oceania, North America, South America",2,2,0.32,{"$f":"IF(K89=4,2.5,IF(K89=64,0.5,0))","v":0},"",null,null,null,null,null,null,null,"1260XX0013.jpg",7,1,1,3,6,1,66,"CE","","IK10","Class II",null,null,null,null,null,0,0,0,null,null,null,null,"1260XX0013.ldt",1,null,null,null,null,1,null,null,null,null,null,null,"LED",16,null,"",null,null,23,null,3000,80,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"","",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"Poland"]
["1261","1261XX0009","GLODE BOLLARD 65CM LED 7479LM T4-B 3000K DALI2",null,"A luminaire with a modern design. For lighting buildings and other architectural concepts",null,"Glode","Bollard","Europe, Africa, Asia, Australia and Oceania, North America, South America",2,2,0.41,0,"",null,null,null,null,null,null,null,"1261XX0009.png",5,1,2,3,6,3,66,"CE","","IK10","Class I",null,null,null,null,null,0.65,0.24,0.12,null,null,null,null,"1261XX0009.ldt",1,null,null,null,null,1,null,null,null,null,null,null,"LED",16,null,"",null,null,23,null,3000,80,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"DALI","",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"Poland"]
["1262","1262XX0009","GLODE BOLLARD 65CM LED 8099LM T4-B 4000K DALI2",null,"A luminaire with a modern design. For lighting buildings and other architectural concepts",null,"Glode","Bollard","Europe, Africa, Asia, Australia and Oceania, North America, South America",2,2,0.41,0,"",null,null,null,null,null,null,null,"1262XX0009.png",5,1,2,3,6,3,66,"CE","","IK10","Class I",null,null,null,null,null,0.65,0.24,0.12,null,null,null,null,"1262XX0009.ldt",1,null,null,null,null,1,null,null,null,null,null,null,"LED",16,null,"",null,null,24,null,4000,80,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"DALI","",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"Poland"]
["1263","1263XX0009","GLODE BOLLARD 40CM LED 7479LM T4-B 3000K DALI2",null,"A luminaire with a modern design. For lighting buildings and other architectural concepts",null,"Glode","Bollard","Europe, Africa, Asia, Australia and Oceania, North America, South America",2,2,0.16,0,"",null,null,null,null,null,null,null,"1263XX0009.png",5,1,2,3,6,3,66,"CE","","IK10","Class I",null,null,null,null,null,0.4,0.24,0.12,null,null,null,null,"1263XX0009.ldt",1,null,null,null,null,1,null,null,null,null,null,null,"LED",16,null,"",null,null,23,null,3000,80,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"DALI","",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"Poland"]
["1264","1264XX0009","GLODE BOLLARD 40CM LED 8099LM T4-B 4000K DALI2",null,"A luminaire with a modern design. For lighting buildings and other architectural concepts",null,"Glode","Bollard","Europe, Africa, Asia, Australia and Oceania, North America, South America",2,2,0.16,0,"",null,null,null,null,null,null,null,"1264XX0009.png",5,1,2,3,6,3,66,"CE","","IK10","Class I",null,null,null,null,null,0.4,0.24,0.12,null,null,null,null,"1264XX0009.ldt",1,null,null,null,null,1,null,null,null,null,null,null,"LED",16,null,"",null,null,24,null,4000,80,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"DALI","",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"Poland"]
["1265","1265XX0013","STOCKHOLM BOLLARD 85CM LED 1059LM 3000K DIM.",null,"A bollard luminaire with a stable and durable structure. For lighting gardens, private areas, and other architectural structures",null,"Stockholm","Bollard","Europe, Africa, Asia, Australia and Oceania, North America, South America",2,2,0.68,0,"",null,null,null,null,null,null,null,"1265XX0013.jpg",7,1,1,3,6,1,66,"CE","","IK10","Class II",null,null,null,null,null,0,0,0,null,null,null,null,"1265XX0013.ldt",1,null,null,null,null,1,null,null,null,null,null,null,"LED",16,null,"",null,null,23,null,3000,80,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"","",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"Poland"]
["1268","1268XX0010","STOCKHOLM BOLLARD 28CM LED 1150LM 3000K DIM.",null,"Bollard luminaire of stable and durable construction. For lighting private areas and public spaces.",null,"Stockholm","Bollard","Europe, Africa, Asia, Australia and Oceania, North America, South America",2,2,0.11,0,"",null,null,null,null,null,null,null,"1268XX0010.jpg",7,1,1,3,6,1,66,"CE","","IK10","Class I",null,null,null,null,null,0,0,0,null,null,null,null,"1268XX0010.ldt",1,null,null,null,null,1,null,null,null,null,null,null,"LED",16,null,"",null,null,23,null,3000,80,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"","",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"Poland"]
["1269","1269XX0010","STOCKHOLM BOLLARD 28CM LED E27 806LM 2700K DIM.",null,"Bollard luminaire of stable and durable construction. For lighting private areas and public spaces.",null,"Stockholm","Bollard","Europe, Africa, Asia, Australia and Oceania, North America, South America",2,2,0.11,0,"",null,null,null,null,null,null,null,"1269XX0010.jpg",7,1,1,3,6,1,66,"CE","","IK10","Class II",null,null,null,null,null,0.16,0.16,0.28000000000000003,null,null,null,null,"1269XX0010.ldt",0,null,null,null,null,1,null,null,null,null,null,null,"LED",16,null,"E27",null,null,23,null,2700,80,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"","",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"Poland"]
["127","127XX0012","VASA WALL LED E27 806LM UP-DOWN 2700K DIM.",null,"Luminaire with a wide range of applications for example for illumination of walls and facade surfaces or any other architectural concepts.",null,"Vasa","Wall","Europe, Africa, Asia, Australia and Oceania, North America, South America",2,4,0,2.5,"",null,null,null,null,null,null,null,"127XX0012.jpg",8,1,5,2,2,1,66,"CE","","IK08","Class I",null,null,null,null,null,0.31,0.12,0.16,null,null,null,null,"127XX0012.ldt",0,null,null,null,null,1,null,null,null,null,null,null,"LED",16,null,"E27",null,null,23,null,2700,80,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"","",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"Poland"]
["1280","1280XX0014","EGERSUND BOLLARD 108CM LED 2617LM 3000K DIM.",null,"Luminaire with a contemporary design. For lighting gardens and other private and public areas",null,"Egersund","Bollard","Europe, Africa, Asia, Australia and Oceania, North America, South America",2,2,1.04,0,"",null,null,null,null,null,null,null,"1280XX0014.jpg",3,1,1,3,6,1,66,"CE","","IK08","Class II",null,null,null,null,null,0.2,0.2,1.08,null,null,null,null,"1280XX0014.ldt",1,null,null,null,null,0,null,null,null,null,null,null,"LED",16,null,"",null,null,23,null,3000,80,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"","",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"Poland"]
["1281","1281XX0009","GLODE BOLLARD 65CM LED 7479LM T4-B 3000K ON/OFF",null,"A luminaire with a modern design. For lighting buildings and other architectural concepts",null,"Glode","Bollard","Europe, Africa, Asia, Australia and Oceania, North America, South America",2,{"$f":"IFERROR(INDEX(TYPMONT,MATCH((INDEX(DB,MATCH($A99,ID,0),31)),ID_RODZ,0),3),\"\")","v":2},0.41,0,"",null,null,null,null,null,null,null,"1281XX0009.png",5,1,2,3,6,4,66,"CE","","IK10","Class I",null,null,null,null,null,0.65,0.24,0.12,null,null,null,null,"1281XX0009.ldt",1,null,null,null,null,1,null,null,null,null,null,null,"LED",16,null,"",null,null,23,null,3000,80,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"","",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"Poland"]
["1282","1282XX0009","GLODE BOLLARD 65CM LED 8099LM T4-B 4000K ON/OFF",null,"A luminaire with a modern design. For lighting buildings and other architectural concepts",null,"Glode","Bollard","Europe, Africa, Asia, Australia and Oceania, North America, South America",2,2,0.41,0,"",null,null,null,null,null,null,null,"1282XX0009.png",5,1,2,3,6,4,66,"CE","","IK10","Class I",null,null,null,null,null,0.65,0.24,0.12,null,null,null,null,"1282XX0009.ldt",1,null,null,null,null,1,null,null,null,null,null,null,"LED",16,null,"",null,null,24,null,4000,80,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"","",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"Poland"]
["1283","1283XX0009","GLODE BOLLARD 40CM LED 7479LM T4-B 3000K ON/OFF",null,"A luminaire with a modern design. For lighting buildings and other architectural concepts",null,"Glode","Bollard","Europe, Africa, Asia, Australia and Oceania, North America, South America",2,2,0.16,0,"",null,null,null,null,null,null,null,"1283XX0009.png",5,1,2,3,6,4,66,"CE","","IK10","Class I",null,null,null,null,null,0.4,0.24,0.12,null,null,null,null,"1283XX0009.ldt",1,null,null,null,null,1,null,null,null,null,null,null,"LED",16,null,"",null,null,23,null,3000,80,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"","",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"Poland"]
["1284","1284XX0009","GLODE BOLLARD 40CM LED 8099LM T4-B 4000K ON/OFF",null,"A luminaire with a modern design. For lighting buildings and other architectural concepts",null,"Glode","Bollard","Europe, Africa, Asia, Australia and Oceania, North America, South America",2,2,0.16,0,"",null,null,null,null,null,null,null,"1284XX0009.png",5,1,2,3,6,4,66,"CE","","IK10","Class I",null,null,null,null,null,0.4,0.24,0.12,null,null,null,null,"1284XX0009.ldt",1,null,null,null,null,1,null,null,null,null,null,null,"LED",16,null,"",null,null,24,null,4000,80,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"","",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"Poland"]
["128","128XX0014","VASA WALL 2XLED 1128LM UP-DOWN 3000K DIM.",null,"Luminaire with a wide range of applications for example for illumination of walls and facade surfaces or any other architectural concepts",null,"Vasa","Wall","Europe, Africa, Asia, Australia and Oceania, North America, South America",2,4,0,2.5,"",null,null,null,null,null,null,null,"128XX0014.jpg",8,1,5,2,2,1,66,"CE","","IK08","Class I",null,null,null,null,null,0.31,0.12,0.16,null,null,null,null,"128XX0014.ldt",1,null,null,null,null,1,null,null,null,null,null,null,"LED",16,null,"",null,null,23,null,3000,80,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"","",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"Poland"]
["1290","1290XX0014","EGERSUND MINI BOLLARD 85CM LED 1370LM 3000K DIM.",null,"Luminaire with contemporary design, for lighting gardens and other private and public areas",null,"Egersund Mini","Bollard","Europe, Africa, Asia, Australia and Oceania, North America, South America",2,2,0.69,0,"",null,null,null,null,null,null,null,"1290XX0014.jpg",3,1,1,3,6,1,66,"CE","","IK08","Class II",null,null,null,null,null,0,0,0,null,null,null,null,"1290XX0014.ldt",1,null,null,null,null,1,null,null,null,null,null,null,"LED",16,null,"",null,null,23,null,3000,80,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"","",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"Poland"]
["1291","1291XX0013","EGERSUND MINI BOLLARD 49CM LED 1370LM 3000K DIM.",null,"Luminaire with contemporary design, for lighting gardens and other private and public areas",null,"Egersund Mini","Bollard","Europe, Africa, Asia, Australia and Oceania, North America, South America",2,2,0.33,0,"",null,null,null,null,null,null,null,"1291XX0013.jpg",3,1,1,3,6,1,66,"CE","","IK08","Class II",null,null,null,null,null,0,0,0,null,null,null,null,"1291XX0013.ldt",1,null,null,null,null,1,null,null,null,null,null,null,"LED",16,null,"",null,null,23,null,3000,80,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"","",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"Poland"]
["1300","1300XX0014","ASKER BIG WALL 2XLED 1128LM UP-DOWN 3000K DIM.",null,"Luminaire with a wide range of applications, for illumination of walls and facade surfaces or any other architectural concepts",null,"Asker,Big","Wall","Europe, Africa, Asia, Australia and Oceania, North America, South America",2,4,0,2.5,"",null,null,null,null,null,null,null,"1300XX0014.jpg",8,1,2,2,2,1,66,"CE","","IK08","Class I",null,null,null,null,null,0.3,0.12,0.12,null,null,null,null,"1300XX0014.ldt",1,null,null,null,null,1,null,null,null,null,null,null,"LED",16,null,"",null,null,23,null,3000,80,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"","",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"Poland"]
["1302","1302XX0013","ASKER BIG WALL LED 653LM DOWN 3000K DIM.",null,"A luminaire with a wide range of applications, for illuminating wall and facade surfaces as well as other architectural concepts",null,"Asker,Big","Wall","Europe, Africa, Asia, Australia and Oceania, North America, South America",2,4,0,2.5,"",null,null,null,null,null,null,null,"1302XX0013.jpg",7,1,2,2,2,1,66,"CE","","IK08","Class I",null,null,null,null,null,0,0,0,null,null,null,null,"1302XX0013.ldt",1,null,null,null,null,0,null,null,null,null,null,null,"LED",16,null,"",null,null,23,null,3000,80,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"","",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"Poland"]
["1303","1303XX0010","ASKER BIG WALL E27 UP-DOWN",null,"Luminaire with a wide range of applications for example for illumination of walls and facade surfaces or any other architectural concepts.",null,"Asker,Big","Wall","Europe, Africa, Asia, Australia and Oceania, North America, South America",2,4,0,2.5,"",null,null,null,null,null,null,null,"1303XX0010.jpg",8,1,2,2,2,4,66,"CE","","IK08","Class I",null,null,null,null,null,0.3,0.12,0.12,null,null,null,null,"1303XX0010.ldt",0,null,null,null,null,1,null,null,null,null,null,null,"LED",16,null,"E27",null,null,23,null,"",80,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"","",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"Poland"]
["1305","1305XX0010","ASKER BIG WALL E27 DOWN",null,"Luminaire with a wide range of applications for example for illumination of walls and facade surfaces or any other architectural concepts.",null,"Asker,Big","Wall","Europe, Africa, Asia, Australia and Oceania, North America, South America",2,4,0,2.5,"",null,null,null,null,null,null,null,"1305XX0010.jpg",7,1,2,2,2,4,66,"CE","","IK08","Class I",null,null,null,null,null,0,0,0,null,null,null,null,"1305XX0010.ldt",0,null,null,null,null,0,null,null,null,null,null,null,"LED",16,null,"E27",null,null,23,null,"",80,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"","",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"Poland"]
["1306","1306XX0010","ASKER BIG PRO WALL 4XLED 2043LM UP-DOWN 3000K DIM.",null,"A luminaire with a wide range of applications, including lighting of wall surfaces, facades and other architectural concepts",null,"Asker,Big","Wall","Europe, Africa, Asia, Australia and Oceania, North America, South America",2,4,0,2.5,"",null,null,null,null,null,null,null,"1306XX0010.jpg",8,1,2,2,2,1,66,"CE","","IK08","Class I",null,null,null,null,null,0,0,0,null,null,null,null,"1306XX0010.ldt",1,null,null,null,null,1,null,null,null,null,null,null,"LED",16,null,"",null,null,23,null,3000,80,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"","",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"Poland"]
["1308","1308XX0012","ASKER BIG WALL 2XLED 1122LM DOWN 3000K DIM.",null,"A luminaire with a wide range of applications, for illuminating wall, facade surfaces and other architectural concepts",null,"Asker,Big","Wall","Europe, Africa, Asia, Australia and Oceania, North America, South America",2,4,0,2.5,"",null,null,null,null,null,null,null,"1308XX0012.jpg",7,1,2,2,2,1,66,"CE","","IK08","Class I",null,null,null,null,null,0.3,0.12,0.12,null,null,null,null,"1308XX0012.ldt",1,null,null,null,null,0,null,null,null,null,null,null,"LED",16,null,"",null,null,23,null,3000,80,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"","",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"Poland"]
["1310","1310XX0009","ASKER BOLLARD 55CM LED 1080LM 3000K ON/OFF",null,"Luminaire with contemporary design. For lighting private areas and other architectural concepts",null,"Asker","Bollard","Europe, Africa, Asia, Australia and Oceania, North America, South America",2,2,0.5,0,"",null,null,null,null,null,null,null,"1310XX0009.jpg",7,1,2,3,6,4,66,"CE","","IK10","Class I",null,null,null,null,null,0.56999999999999995,0.23,0.14000000000000001,null,null,null,null,"1310XX0009.ldt",1,null,null,null,null,0,null,null,null,null,null,null,"LED",16,null,"",null,null,23,null,3000,80,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"","",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"Poland"]
["1311","1311XX0012","ASKER BOLLARD 85CM LED 1080LM 3000K ON/OFF",null,"Luminaire with a contemporary design. For lighting gardens, private areas and other architectural applications",null,"Asker","Bollard","Europe, Africa, Asia, Australia and Oceania, North America, South America",2,2,0.8,0,"",null,null,null,null,null,null,null,"1311XX0012.jpg",7,1,2,3,6,4,66,"CE","","IK10","Class I",null,null,null,null,null,0.85,0.2,0.11,null,null,null,null,"1311XX0012.ldt",1,null,null,null,null,0,null,null,null,null,null,null,"LED",16,null,"",null,null,23,null,3000,80,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"","",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"Poland"]
["1312","1312XX0013","ASKER BOLLARD 2XLED 1190LM 3000K DALI2",null,"A fixture with a contemporary design. For lighting gardens, private areas and other architectural concepts.",null,"Asker","Bollard","Europe, Africa, Asia, Australia and Oceania, North America, South America",2,2,0.8,0,"",null,null,null,null,null,null,null,"1312XX0013.jpg",7,1,2,3,6,3,66,"CE","","IK10","Class I",null,null,null,null,null,0.85,0.2,0.11,null,null,null,null,"1312XX0013.ldt",1,null,null,null,null,0,null,null,null,null,null,null,"LED",16,null,"",null,null,23,null,3000,80,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"DALI","",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"Poland"]
["1314","1314XX0011","ASKER PRO BOLLARD 85CM LED 828LM SCL 3000K DIM. TE",null,"A luminaire with a contemporary design. For lighting gardens and other private areas.",null,"Asker","Bollard","Europe, Africa, Asia, Australia and Oceania, North America, South America",2,2,0.8,0,"",null,null,null,null,null,null,null,"1314XX0011.jpg",6,1,2,3,6,1,66,"CE","","IK08","Class I",null,null,null,null,null,0,0,0,null,null,null,null,"1314XX0011.ldt",1,null,null,null,null,0,null,null,null,null,null,null,"LED",16,null,"",null,null,23,null,3000,80,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"","",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"Poland"]
["1315","1315XX0011","ASKER PRO BOLLARD 85CM LED 828LM SCL 3000K DALI2",null,"A luminaire with a contemporary design. For lighting gardens and other private areas.",null,"Asker","Bollard","Europe, Africa, Asia, Australia and Oceania, North America, South America",2,2,0.8,0,"",null,null,null,null,null,null,null,"1315XX0011.jpg",6,1,2,3,6,3,66,"CE","","IK08","Class I",null,null,null,null,null,0,0,0,null,null,null,null,"1315XX0011.ldt",1,null,null,null,null,0,null,null,null,null,null,null,"LED",16,null,"",null,null,23,null,3000,80,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"DALI","",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"Poland"]
["1316","1316XX0011","ASKER PRO BOLLARD 85CM LED 828LM VSM 3000K DIM. TE",null,"A luminaire with a contemporary design. For lighting gardens and other private areas.",null,"Asker","Bollard","Europe, Africa, Asia, Australia and Oceania, North America, South America",2,2,0.8,0,"",null,null,null,null,null,null,null,"1316XX0011.jpg",4,1,2,3,6,1,66,"CE","","IK08","Class I",null,null,null,null,null,0,0,0,null,null,null,null,"1316XX0011.ldt",1,null,null,null,null,0,null,null,null,null,null,null,"LED",16,null,"",null,null,23,null,3000,80,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"","",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"Poland"]
["1317","1317XX0011","ASKER PRO BOLLARD 85CM LED 828LM VSM 3000K DALI2",null,"A luminaire with a contemporary design. For lighting gardens and other private areas.",null,"Asker","Bollard","Europe, Africa, Asia, Australia and Oceania, North America, South America",2,2,0.8,0,"",null,null,null,null,null,null,null,"1317XX0011.jpg",4,1,2,3,6,3,66,"CE","","IK08","Class I",null,null,null,null,null,0,0,0,null,null,null,null,"1317XX0011.ldt",1,null,null,null,null,0,null,null,null,null,null,null,"LED",16,null,"",null,null,23,null,3000,80,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"DALI","",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"Poland"]
["1318","1318XX0011","ASKER PRO BOLLARD 85CM LED 828LM SCL 4000K DIM. TE",null,"A luminaire with a contemporary design. For lighting gardens and other private areas.",null,"Asker","Bollard","Europe, Africa, Asia, Australia and Oceania, North America, South America",2,2,0.8,0,"",null,null,null,null,null,null,null,"1318XX0011.jpg",6,1,2,3,6,1,66,"CE","","IK08","Class I",null,null,null,null,null,0.2,0.11,0.85,null,null,null,null,"1318XX0011.ldt",1,null,null,null,null,0,null,null,null,null,null,null,"LED",16,null,"",null,null,24,null,4000,80,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"","",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"Poland"]
["1319","1319XX0011","ASKER PRO BOLLARD 85CM LED 828LM SCL 4000K DALI2",null,"A luminaire with a contemporary design. For lighting gardens and other private areas.",null,"Asker","Bollard","Europe, Africa, Asia, Australia and Oceania, North America, South America",2,2,0.8,0,"",null,null,null,null,null,null,null,"1319XX0011.jpg",6,1,2,3,6,3,66,"CE","","IK08","Class I",null,null,null,null,null,0,0,0,null,null,null,null,"1319XX0011.ldt",1,null,null,null,null,0,null,null,null,null,null,null,"LED",16,null,"",null,null,24,null,4000,80,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"DALI","",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"Poland"]
["1320","1320XX0011","ASKER PRO BOLLARD 85CM LED 856LM VSM 4000K DIM. TE",null,"A luminaire with a contemporary design. For lighting gardens and other private areas.",null,"Asker","Bollard","Europe, Africa, Asia, Australia and Oceania, North America, South America",2,2,0.8,0,"",null,null,null,null,null,null,null,"1320XX0011.jpg",4,1,2,3,6,1,66,"CE","","IK08","Class I",null,null,null,null,null,0.85,0.2,0.11,null,null,null,null,"1320XX0011.ldt",1,null,null,null,null,0,null,null,null,null,null,null,"LED",16,null,"",null,null,24,null,4000,80,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"","",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"Poland"]
["1321","1321XX0012","OPPLAND BOLLARD LED 984LM 3000K DIM.",null,"A bollard luminaire with a stable and durable construction. For lighting private areas and other architectural concepts",null,"Oppland","Bollard","Europe, Africa, Asia, Australia and Oceania, North America, South America",2,2,0.8,0,"",null,null,null,null,null,null,null,"1321XX0012.jpg",7,1,1,3,6,1,66,"CE","","IK09","Class II",null,null,null,null,null,0.85,0.12,0.12,null,null,null,null,"1321XX0012.ldt",1,null,null,null,null,0,null,null,null,null,null,null,"LED",16,null,"",null,null,23,null,3000,80,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"","",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"Poland"]
["1322","1322XX0011","ASKER PRO BOLLARD 85CM LED 828LM VSM 4000K DALI2",null,"A luminaire with a contemporary design. For lighting gardens and other private areas.",null,"Asker","Bollard","Europe, Africa, Asia, Australia and Oceania, North America, South America",2,2,0.8,0,"",null,null,null,null,null,null,null,"1322XX0011.jpg",4,1,2,3,6,3,66,"CE","","IK08","Class I",null,null,null,null,null,0,0,0,null,null,null,null,"1322XX0011.ldt",1,null,null,null,null,0,null,null,null,null,null,null,"LED",16,null,"",null,null,24,null,4000,80,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"DALI","",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"Poland"]
["1324","1324XX0009","OPPLAND BOLLARD LED 984LM 3000K DALI2",null,"A bollard luminaire with a stable and durable construction For lighting private and public areas",null,"Oppland","Bollard","Europe, Africa, Asia, Australia and Oceania, North America, South America",2,2,0.8,0,"",null,null,null,null,null,null,null,"1324XX0009.jpg",7,1,1,3,6,3,66,"CE","","IK09","Class I",null,null,null,null,null,0.85,0.12,0.12,null,null,null,null,"1324XX0009.ldt",1,null,null,null,null,0,null,null,null,null,null,null,"LED",16,null,"",null,null,23,null,3000,80,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"DALI","",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"Poland"]
["1330","1330XX0009","HITRA WALL LED 1080LM 3000K ON/OFF",null,"Modern design luminaire. For lighting private areas and public spaces.",null,"Hitra","Wall","Europe, Africa, Asia, Australia and Oceania, North America, South America",2,4,0,2.5,"",null,null,null,null,null,null,null,"1330XX0009.jpg",7,1,2,2,2,4,66,"CE","","IK06","Class I",null,null,null,null,null,0.2,0.15,0.06,null,null,null,null,"1330XX0009.ldt",1,null,null,null,null,0,null,null,null,null,null,null,"LED",16,null,"",null,null,23,null,3000,80,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"","",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"Poland"]
["1331","1331XX0009","HITRA WALL LED 1950LM 3000K ON/OFF",null,"Modern design luminaire. For lighting private areas and public spaces.",null,"Hitra","Wall","Europe, Africa, Asia, Australia and Oceania, North America, South America",2,4,0,2.5,"",null,null,null,null,null,null,null,"1331XX0009.jpg",7,1,2,2,2,4,66,"CE","","IK08","Class I",null,null,null,null,null,0,0,0,null,null,null,null,"1331XX0009.ldt",1,null,null,null,null,0,null,null,null,null,null,null,"LED",16,null,"",null,null,23,null,3000,80,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"","",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"Poland"]
["1336","1336XX0009","ASKER BOLLARD 55CM LED 1080LM 3000K ON/OFF MD",null,"Luminaire with a contemporary design. For lighting private areas and other architectural concepts",null,"Asker","Bollard","Europe, Africa, Asia, Australia and Oceania, North America, South America",2,2,0.5,0,"",null,null,null,null,null,null,null,"1336XX0009.png",7,1,2,3,6,3,66,"CE","","","Class I",null,null,null,null,null,0.55000000000000004,0.2,0.11,null,null,null,null,"1336XX0009.ldt",1,null,null,null,null,0,null,null,null,null,null,null,"LED",16,null,"",null,null,23,null,3000,80,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"","Daylight sensor,Motion sensor",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"Poland"]
["1337","1337XX0009","ASKER BOLLARD 55CM LED 1150LM 4000K ON/OFF MD",null,"Luminaire with a contemporary design. For lighting private areas and other architectural concepts",null,"Asker","Bollard","Europe, Africa, Asia, Australia and Oceania, North America, South America",2,2,0.5,0,"",null,null,null,null,null,null,null,"1337XX0009.png",7,1,2,3,6,3,66,"CE","","","Class I",null,null,null,null,null,0.55000000000000004,0.2,0.11,null,null,null,null,"1337XX0009.ldt",1,null,null,null,null,0,null,null,null,null,null,null,"LED",16,null,"",null,null,24,null,4000,80,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"","Daylight sensor,Motion sensor",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"Poland"]
["1338","1338XX0009","ASKER BOLLARD 85CM LED 1080LM 3000K ON/OFF MD",null,"Luminaire with a contemporary design. For lighting private areas and other architectural concepts",null,"Asker","Bollard","Europe, Africa, Asia, Australia and Oceania, North America, South America",2,2,0.8,0,"",null,null,null,null,null,null,null,"1338XX0009.png",7,1,2,3,6,3,66,"CE","","","Class I",null,null,null,null,null,0.85,0.2,0.11,null,null,null,null,"1338XX0009.ldt",1,null,null,null,null,0,null,null,null,null,null,null,"LED",16,null,"",null,null,23,null,3000,80,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"","Daylight sensor,Motion sensor",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"Poland"]
["1339","1339XX0009","ASKER BOLLARD 85CM LED 1150LM 4000K ON/OFF MD",null,"Luminaire with a contemporary design. For lighting private areas and other architectural concepts",null,"Asker","Bollard","Europe, Africa, Asia, Australia and Oceania, North America, South America",2,2,0.8,0,"",null,null,null,null,null,null,null,"1339XX0009.png",7,1,2,3,6,3,66,"CE","","","Class I",null,null,null,null,null,0.85,0.2,0.11,null,null,null,null,"1339XX0009.ldt",1,null,null,null,null,0,null,null,null,null,null,null,"LED",16,null,"",null,null,24,null,4000,80,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"","Daylight sensor,Motion sensor",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"Poland"]
["1340","1340XX0011","NAMSOS MINI WALL-RECESSED LED 439LM 3000K DIM.",null,"The luminaire is adapted to illuminate stairs, steps, staircases, passageways, ceilings, and for the implementation of other architectural concepts",null,"Namsos,Mini","Recessed","Europe, Africa, Asia, Australia and Oceania, North America, South America",2,64,0,0.5,"",null,null,null,null,null,null,null,"1340XX0011.jpg",7,1,2,2,1,1,66,"CE","","IK10","Class I",null,null,null,null,null,0,0,0,null,null,null,null,"1340XX0011.ldt",1,null,null,null,null,4,null,null,null,null,null,null,"LED",16,null,"",null,null,23,null,3000,80,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"","",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"Poland"]
["1341","1341XX0010","NAMSOS MINI WALL LED 439LM 3000K DIM.",null,"Luminaire designed to illuminate stairs, steps, staircases, communication routes, ceiling illumination, and many other architectural applications",null,"Namsos,Mini","Wall","Europe, Africa, Asia, Australia and Oceania, North America, South America",2,4,0,0.5,"",null,null,null,null,null,null,null,"1341XX0010.jpg",7,1,2,2,2,1,66,"CE","","IK09","Class I",null,null,null,null,null,0,0,0,null,null,null,null,"1341XX0010.ldt",1,null,null,null,null,4,null,null,null,null,null,null,"LED",16,null,"",null,null,23,null,3000,80,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"","",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"Poland"]
["1346","1346XX0009","HALMSTAD BOLLARD 49CM LED 1059LM 4000K DIM. TE",null,"A bollard luminaire with a stable and durable structure For lighting private areas and other architectural concepts",null,"Halmstad","Bollard","Europe, Africa, Asia, Australia and Oceania, North America, South America",2,2,0.34,0,"",null,null,null,null,null,null,null,"1346XX0009.jpg",7,1,2,3,6,1,66,"CE","","IK10","Class II",null,null,null,null,null,0.12,0.12,0.49,null,null,null,null,"1346XX0009.ldt",1,null,null,null,null,1,null,null,null,null,null,null,"LED",16,null,"",null,null,24,null,4000,80,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"","",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"Poland"]
["1347","1347XX0009",{"$f":"INDEX(DB,MATCH($A134,ID,0),3)","v":"HALMSTAD BOLLARD 49CM LED 1121LM 4000K DIM."},null,"A bollard luminaire with a stable and durable structure For lighting private areas and other architectural concepts",null,"Halmstad,Wood",{"$f":"IF(INDEX(DB,MATCH($A134,ID,0),5)=0,\"\",INDEX(DB,MATCH($A134,ID,0),5))","v":"Bollard"},"Europe, Africa, Asia, Australia and Oceania, North America, South America",2,{"$f":"IFERROR(INDEX(TYPMONT,MATCH((INDEX(DB,MATCH($A134,ID,0),31)),ID_RODZ,0),3),\"\")","v":2},0.34,0,{"$f":"IFERROR(IF(INDEX(TYPMONT,MATCH((INDEX(DB,MATCH($A134,ID,0),31)),ID_RODZ,0),6)=0,\"\",INDEX(TYPMONT,MATCH((INDEX(DB,MATCH($A134,ID,0),31)),ID_RODZ,0),6)),\"\")","v":""},null,null,null,null,null,null,null,{"$f":"IF(INDEX(DB,MATCH($A134,ID,0),57)=0,\"\",INDEX(DB,MATCH($A134,ID,0),57))","v":"1347XX0009.png"},7,{"$f":"IF(INDEX(DB,MATCH($A134,ID,0),61)=0,\"\",INDEX(DB,MATCH($A134,ID,0),61))","v":1},2,{"$f":"IFERROR(INDEX(TYPMONT,MATCH((INDEX(DB,MATCH($A134,ID,0),31)),ID_RODZ,0),1),\"\")","v":3},{"$f":"IFERROR(INDEX(TYPMONT,MATCH((INDEX(DB,MATCH($A134,ID,0),31)),ID_RODZ,0),2),\"\")","v":6},{"$f":"IF(INDEX(DB,MATCH($A134,ID,0),59)=0,\"\",INDEX(DB,MATCH($A134,ID,0),59))","v":1},{"$f":"IFERROR(IF(INDEX(DB,MATCH($A134,ID,0),19)=0,\"\",INDEX(DB,MATCH($A134,ID,0),19)+1),\"\")","v":66},{"$f":"IF(INDEX(DB,MATCH($A134,ID,0),27)=0,\"\",INDEX(DB,MATCH($A134,ID,0),27))","v":"CE"},"",{"$f":"IF(INDEX(DB,MATCH($A134,ID,0),20)=0,\"\",INDEX(DB,MATCH($A134,ID,0),20))","v":"IK10"},{"$f":"IF(INDEX(DB,MATCH($A134,ID,0),21)=0,\"\",INDEX(DB,MATCH($A134,ID,0),21))","v":"Class II"},null,null,null,null,null,0.12,0.12,0.49,null,null,null,null,{"$f":"IF(INDEX(DB,MATCH($A134,ID,0),58)=0,\"\",INDEX(DB,MATCH($A134,ID,0),58))","v":"1347XX0009.ldt"},1,null,null,null,null,1,null,null,null,null,null,null,"LED",16,null,{"$f":"IF(INDEX(DB,MATCH($A134,ID,0),60)=0,\"\",INDEX(DB,MATCH($A134,ID,0),60))","v":""},null,null,24,null,{"$f":"IF(INDEX(DB,MATCH($A134,ID,0),22)=0,\"\",INDEX(DB,MATCH($A134,ID,0),22))","v":4000},{"$f":"IF(INDEX(DB,MATCH($A134,ID,0),53)=0,\"\",INDEX(DB,MATCH($A134,ID,0),53))","v":80},null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,{"$f":"IF(INDEX(DB,MATCH($A134,ID,0),29)=0,\"\",INDEX(DB,MATCH($A134,ID,0),29))","v":""},{"$f":"IF(INDEX(DB,MATCH($A134,ID,0),28)=0,\"\",INDEX(DB,MATCH($A134,ID,0),28))","v":""},null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"Poland"]
["1350",{"$f":"INDEX(DB,MATCH($A135,ID,0),2)","v":"1350XX0009"},"HALMSTAD BOLLARD 85CM LED 1121LM 4000K DIM.",null,{"$f":"IF(INDEX(DB,MATCH($A135,ID,0),35)=0,\"\",INDEX(DB,MATCH($A135,ID,0),35))","v":"A bollard luminaire with a stable and durable structure For lighting private areas and other architectural concepts"},null,{"$f":"IF(INDEX(DB,MATCH($A135,ID,0),4)=0,\"\",INDEX(DB,MATCH($A135,ID,0),4))","v":"Halmstad,Wood"},"Bollard","Europe, Africa, Asia, Australia and Oceania, North America, South America",2,2,0.7,0,"",null,null,null,null,null,null,null,"1350XX0009.png",{"$f":"IF((IFERROR(INDEX(BRYLA_FOTO,MATCH(INDEX(DB,MATCH($A135,ID,0),62),ID_BRYLAFOTO,0),6),\"\"))<>0,IFERROR(INDEX(BRYLA_FOTO,MATCH(INDEX(DB,MATCH($A135,ID,0),62),ID_BRYLAFOTO,0),6),\"\"),\"\")","v":7},1,2,3,6,1,66,"CE",{"$f":"IFERROR(IF(FIND(\"RENA\",$C135)>0,\"Vehicle resistant\",\"\"),\"\")","v":""},"IK10","Class II",null,null,null,null,null,{"$f":"INDEX(DB,MATCH($A135,ID,0),24)","v":0.12},{"$f":"INDEX(DB,MATCH($A135,ID,0),25)","v":0.12},{"$f":"INDEX(DB,MATCH($A135,ID,0),26)","v":0.85},null,null,null,null,"1350XX0009.ldt",1,null,null,null,null,1,null,null,null,null,null,null,"LED",16,null,"",null,null,{"$f":"IF($BO135=4000,24,23)","v":24},null,4000,80,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"","",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"Poland"]
["1353","1353XX0009","HALMSTAD BOLLARD 49CM LED 1121LM 4000K DIM.",null,"A bollard luminaire with a stable and durable structure For lighting private areas and other architectural concepts",null,"Halmstad,Wood","Bollard","Europe, Africa, Asia, Australia and Oceania, North America, South America",2,2,0.34,0,"",null,null,null,null,null,null,null,"1353XX0009.png",7,1,2,3,6,1,66,"CE","","IK10","Class II",null,null,null,null,null,0.12,0.12,0.49,null,null,null,null,"1353XX0009.ldt",{"$f":"IF($BJ136=\"\",1,0)","v":1},null,null,null,null,1,null,null,null,null,null,null,"LED",16,null,"",null,null,24,null,4000,80,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"","",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"Poland"]
["1356","1356XX0009","HALMSTAD BOLLARD 85CM LED 1121LM 4000K DIM.",null,"A bollard luminaire with a stable and durable structure For lighting private areas and other architectural concepts",null,"Halmstad,Wood","Bollard","Europe, Africa, Asia, Australia and Oceania, North America, South America",2,2,0.34,0,"",null,null,null,null,null,null,null,"1356XX0009.png",7,1,2,3,6,1,66,"CE","","","Class II",null,null,null,null,null,0.12,0.12,0.85,null,null,null,null,"1356XX0009.ldt",1,null,null,null,null,1,null,null,null,null,null,null,"LED",16,null,"",null,null,24,null,4000,80,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"","",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"Poland"]
["1360","1360XX0011","ASKER POLE LIGHT LUMINAIRES POLE 216CM 2XLED 1988LM 3000K DIM.",null,"For lighting private areas and other architectural concepts",null,"Asker","Post,Post complete","Europe, Africa, Asia, Australia and Oceania, North America, South America",2,512,2.16,0,"",null,null,null,null,null,null,null,"1360XX0011.jpg",3,1,2,5,9,1,66,"CE","","","Class I",null,null,null,null,null,0,0,0,null,null,null,null,"1360XX0011.ldt",1,null,null,null,null,0,null,null,null,null,null,null,"LED",16,null,"",null,null,23,null,3000,80,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"","",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"Poland"]
["1361","1361XX0009","ASKER POLE PRO LIGHT LUMINAIRES POLE 216CM LED 1099LM VSM 3000K ON/OFF",null,"Luminaire for lighting private areas, public spaces, and other architectural concepts",null,"Asker","Post,Post complete","Europe, Africa, Asia, Australia and Oceania, North America, South America",2,512,2.16,0,"",null,null,null,null,null,null,null,"1361XX0009.jpg",4,1,2,5,9,4,66,"CE","","IK08","Class I",null,null,null,null,null,0.11,2.16,0.39,null,null,null,null,"1361XX0009.ldt",1,null,null,null,null,0,null,null,null,null,null,null,"LED",16,null,"",null,null,23,null,3000,70,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"","",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"Poland"]
["1362","1362XX0009","ASKER POLE PRO LIGHT LUMINAIRES POLE 216CM LED 1158LM VSM 3000K DALI2",null,"For lighting private areas, parks, and other architectural concepts",null,"Asker","Post,Post complete","Europe, Africa, Asia, Australia and Oceania, North America, South America",2,512,2.16,0,"",null,null,null,null,null,null,null,"1362XX0009.jpg",4,1,2,5,9,3,66,"CE","","IK08","Class I",null,null,null,null,null,0.11,0.39,2.16,null,null,null,null,"1362XX0009.ldt",1,null,null,null,null,0,null,null,null,null,null,null,"LED",16,null,"",null,null,23,null,3000,70,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"DALI","",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"Poland"]
["1363","1363XX0011","ASKER POLE LIGHT LUMINAIRES POLE 2XLED 1988LM 3000K DIM.",null,"For lighting private areas and other architectural concepts",null,"Asker","Post,Post complete","Europe, Africa, Asia, Australia and Oceania, North America, South America",2,512,2.36,0,"",null,null,null,null,null,null,null,"1363XX0011.jpg",3,1,2,5,9,1,66,"CE","","","Class I",null,null,null,null,null,0,0,0,null,null,null,null,"1363XX0011.ldt",1,null,null,null,null,0,null,null,null,null,null,null,"LED",16,null,"",null,null,23,null,3000,80,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"","",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"Poland"]
["1364","1364XX0009","ASKER POLE PRO LIGHT LUMINAIRES POLE 236CM LED 1099LM VSM 3000K ON/OFF",null,"Luminaire for lighting private areas, public spaces, and other architectural concepts",null,"Asker","Post,Post complete","Europe, Africa, Asia, Australia and Oceania, North America, South America",2,512,2.36,0,"",null,null,null,null,null,null,null,"1364XX0009.jpg",4,1,2,5,9,4,66,"CE","","IK08","Class I",null,null,null,null,null,0.24,2.36,0.39,null,null,null,null,"1364XX0009.ldt",1,null,null,null,null,0,null,null,null,null,null,null,"LED",16,null,"",null,null,23,null,3000,70,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"","",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"Poland"]
["1365","1365XX0009","ASKER POLE PRO LIGHT LUMINAIRES POLE 236CM LED 1158LM VSM 3000K DALI2",null,"Luminaire for lighting private areas, public spaces, and other architectural concepts",null,"Asker","Post,Post complete","Europe, Africa, Asia, Australia and Oceania, North America, South America",2,512,2.36,0,"",null,null,null,null,null,null,null,"1365XX0009.jpg",4,1,2,5,9,3,66,"CE","","IK06","Class I",null,null,null,null,null,0.39,0.11,2.36,null,null,null,null,"1365XX0009.ldt",1,null,null,null,null,0,null,null,null,null,null,null,"LED",16,null,"",null,null,23,null,3000,70,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"DALI","",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"Poland"]
["1366","1366XX0009","ASKER POLE PRO LIGHT LUMINAIRES POLE 216CM LED 1099LM T2-L 3000K ON/OFF",null,"Luminaire for lighting private areas, public spaces, and other architectural concepts",null,"Asker","Post,Post complete","Europe, Africa, Asia, Australia and Oceania, North America, South America",2,512,2.36,0,"",null,null,null,null,null,null,null,"1366XX0009.jpg",6,1,2,5,9,4,66,"CE","","IK08","Class I",null,null,null,null,null,2.16,0.11,0.39,null,null,null,null,"1366XX0009.ldt",1,null,null,null,null,0,null,null,null,null,null,null,"LED",16,null,"",null,null,23,null,3000,70,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"","",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"Poland"]
["1367","1367XX0009","ASKER POLE PRO LIGHT LUMINAIRES POLE 236CM LED 1099LM T2-L 3000K ON/OFF",null,"Luminaire for lighting private areas, public spaces, and other architectural concepts",null,"Asker","Post,Post complete","Europe, Africa, Asia, Australia and Oceania, North America, South America",2,512,2.36,0,"",null,null,null,null,null,null,null,"1367XX0009.jpg",6,1,2,5,9,4,66,"CE","","IK06","Class I",null,null,null,null,null,2.36,0.11,0.39,null,null,null,null,"1367XX0009.ldt",1,null,null,null,null,0,null,null,null,null,null,null,"LED",16,null,"",null,null,23,null,3000,70,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"","",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"Poland"]
["1368","1368XX0009","ASKER POLE PRO LIGHT LUMINAIRES POLE 216CM LED 1158LM T2-L 3000K DALI2",null,"For lighting private areas, parks, and other architectural concepts",null,"Asker","Post,Post complete","Europe, Africa, Asia, Australia and Oceania, North America, South America",2,512,2.36,0,"",null,null,null,null,null,null,null,"1368XX0009.jpg",6,1,2,5,9,3,66,"CE","","IK08","Class I",null,null,null,null,null,3.9,0.24,2.16,null,null,null,null,"1368XX0009.ldt",1,null,null,null,null,0,null,null,null,null,null,null,"LED",16,null,"",null,null,23,null,3000,70,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"DALI","",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"Poland"]
["1369","1369XX0009","ASKER POLE PRO LIGHT LUMINAIRES POLE 236CM LED 1158LM T2-L 3000K DALI2",null,"Luminaire for lighting private areas, public spaces, and other architectural concepts",null,"Asker","Post,Post complete","Europe, Africa, Asia, Australia and Oceania, North America, South America",2,512,2.36,0,"",null,null,null,null,null,null,null,"1369XX0009.jpg",6,1,2,5,9,3,66,"CE","","IK06","Class I",null,null,null,null,null,0,0,0,null,null,null,null,"1369XX0009.ldt",1,null,null,null,null,0,null,null,null,null,null,null,"LED",16,null,"",null,null,23,null,3000,70,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"DALI","",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"Poland"]
["1371","1371XX0010","MANDAL WALL 2XLED GU10 UP25D & DOWN25D",null,"Wall-mounted luminaire with modern design. For lighting private areas and public spaces.",null,"Mandal","Wall","Europe, Africa, Asia, Australia and Oceania, North America, South America",2,4,0,2.5,"",null,null,null,null,null,null,null,"1371XX0010.jpg",2,1,1,2,2,4,45,"CE","","","Class I",null,null,null,null,null,0.09,0.12,0.18,null,null,null,null,"1371XX0010.ldt",0,null,null,null,null,1,null,null,null,null,null,null,"LED",16,null,"GU10",null,null,23,null,"",80,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"","",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"Poland"]
["1373","1373XX0010","MANDAL WALL LED GU10 265LM DOWN 25D 2700K DIM.",null,"Wall-mounted luminaire with modern design. For lighting private areas and public spaces.",null,"Mandal","Wall","Europe, Africa, Asia, Australia and Oceania, North America, South America",2,4,0,2.5,"",null,null,null,null,null,null,null,"1373XX0010.jpg",2,1,1,2,2,1,45,"CE","","IK08","Class I",null,null,null,null,null,0.12,0.09,0.1,null,null,null,null,"1373XX0010.ldt",0,null,null,null,null,0,null,null,null,null,null,null,"LED",16,null,"GU10",null,null,23,null,2700,97,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"","",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"Poland"]
["1374","1374XX0010","MANDAL WALL LED GU10 DOWN 25D",null,"Wall-mounted luminaire with modern design. For lighting private areas and public spaces.",null,"Mandal","Wall","Europe, Africa, Asia, Australia and Oceania, North America, South America",2,4,0,2.5,"",null,null,null,null,null,null,null,"1374XX0010.jpg",2,1,1,2,2,4,45,"CE","","IK08","Class I",null,null,null,null,null,0.09,0.12,0.1,null,null,null,null,"1374XX0010.ldt",0,null,null,null,null,0,null,null,null,null,null,null,"LED",16,null,"GU10",null,null,23,null,"",80,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"","",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"Poland"]
["1380","1380XX0010","LILLESAND BOLLARD 85CM E27",null,"Luminaire with a contemporary design For lighting gardens and other private and public areas",null,"Lillesand","Bollard","Europe, Africa, Asia, Australia and Oceania, North America, South America",2,2,0.74,0,"",null,null,null,null,null,null,null,"1380XX0010.jpg",3,1,1,3,6,4,56,"CE","","IK08","Class II",null,null,null,null,null,0.12,0.12,0.85,null,null,null,null,"1380XX0010.ldt",0,null,null,null,null,1,null,null,null,null,null,null,"LED",16,null,"E27",null,null,23,null,"",80,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"","",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"Poland"]
["1382","1382XX0010","LILLESAND BOLLARD 85CM LED E27 806LM 2700K DIM.",null,"Modern design luminaire. For lighting gardens, private areas and public spaces.",null,"Lillesand","Bollard","Europe, Africa, Asia, Australia and Oceania, North America, South America",2,2,0.74,{"$f":"IF(K152=4,2.5,IF(K152=64,0.5,0))","v":0},"",null,null,null,null,null,null,null,"1382XX0010.jpg",3,1,1,3,6,1,56,"CE","","IK08","Class II",null,null,null,null,null,0.12,0.12,0.85,null,null,null,null,"1382XX0010.ldt",0,null,null,null,null,1,null,null,null,null,null,null,"LED",16,null,"E27",null,null,23,null,2700,80,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"","",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"Poland"]
["1383","1383XX0009","LILLESAND BOLLARD 49CM LED E27",null,"A luminaire with a contemporary design. For lighting gardens and other private areas.",null,"Lillesand","Bollard","Europe, Africa, Asia, Australia and Oceania, North America, South America",2,2,0.38,0,"",null,null,null,null,null,null,null,"1383XX0009.jpg",3,1,1,3,6,4,56,"CE","","IK08","Class II",null,null,null,null,null,0.49,0.12,0.12,null,null,null,null,"1383XX0009.ldt",0,null,null,null,null,1,null,null,null,null,null,null,"LED",16,null,"E27",null,null,23,null,"",80,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"","",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"Poland"]
["1384","1384XX0009","LILLESAND BOLLARD 49CM LED E27 806LM 2700K DIM.",null,"Luminaire with a contemporary design. For lighting gardens, private areas, and for other architectural uses",null,"Lillesand","Bollard","Europe, Africa, Asia, Australia and Oceania, North America, South America",2,2,0.38,0,"",null,null,null,null,null,null,null,"1384XX0009.png",3,1,1,3,6,1,66,"CE","","IK08","Class II",null,null,null,null,null,0.12,0.12,0.49,null,null,null,null,"1384XX0009.ldt",0,null,null,null,null,1,null,null,null,null,null,null,"LED",16,null,"E27",null,null,23,null,2700,80,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"","",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"Poland"]
["1390","1390XX0011","SKI WALL-CONNECTORS LED 653LM DOWN 3000K DIM.",null,"Wall luminaire and 220 ... 240V electricity distributor. For lighting private areas and other applications",null,"Ski","Wall","Europe, Africa, Asia, Australia and Oceania, North America, South America",2,4,0,2.5,"",null,null,null,null,null,null,null,"1390XX0011.jpg",7,1,2,2,2,1,45,"CE","","IK09","Class I",null,null,null,null,null,0.2,0.14000000000000001,0.13,null,null,null,null,"1390XX0011.ldt",1,null,null,null,null,0,null,null,null,null,null,null,"LED",16,null,"",null,null,23,null,3000,80,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"","",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"Poland"]
["1392","1392XX0010","SKI WALL LED 653LM DOWN 3000K DIM.",null,"A luminaire with a wide range of applications, used for general and decorative lighting of wall surfaces, facades, and other architectural concepts",null,"Ski","Wall","Europe, Africa, Asia, Australia and Oceania, North America, South America",2,4,0,2.5,"",null,null,null,null,null,null,null,"1392XX0010.jpg",7,1,2,2,2,1,45,"CE","","IK09","Class I",null,null,null,null,null,0.2,0.14000000000000001,0.13,null,null,null,null,"1392XX0010.ldt",1,null,null,null,null,0,null,null,null,null,null,null,"LED",16,null,"",null,null,23,null,3000,80,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"","",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"Poland"]
["1400","1400XX0010","HALMSTAD BOLLARD 49CM E27",null,"Bollard luminaire of stable and durable construction For lighting private areas and public spaces",null,"Halmstad,Wood","Bollard","Europe, Africa, Asia, Australia and Oceania, North America, South America",2,2,0.36,0,"",null,null,null,null,null,null,null,"1400XX0010.jpg",7,1,2,3,6,4,66,"CE","","IK10","Class II",null,null,null,null,null,0.49,0.12,0.12,null,null,null,null,"1400XX0010.ldt",0,null,null,null,null,1,null,null,null,null,null,null,"LED",16,null,"E27",null,null,23,null,"",80,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"","",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"Poland"]
["1403","1403XX0010","HALMSTAD BOLLARD 49CM E27",null,"Bollard luminaire of stable and durable construction. For lighting private areas and public spaces.",null,"Halmstad","Bollard","Europe, Africa, Asia, Australia and Oceania, North America, South America",2,2,0.36,0,"",null,null,null,null,null,null,null,"1403XX0010.jpg",7,1,2,3,6,4,66,"CE","","IK10","Class II",null,null,null,null,null,0,0,0,null,null,null,null,"1403XX0010.ldt",0,null,null,null,null,1,null,null,null,null,null,null,"LED",16,null,"E27",null,null,23,null,"",80,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"","",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"Poland"]
["1407","1407XX0009","HALMSTAD BOLLARD 49CM LED 1059LM 3000K DIM.",null,"A bollard luminaire with a stable and durable structure For lighting private areas and other architectural concepts",null,"Halmstad,Wood","Bollard","Europe, Africa, Asia, Australia and Oceania, North America, South America",2,2,0.34,0,"",null,null,null,null,null,null,null,"1407XX0009.png",7,1,2,3,6,1,66,"CE","","IK10","Class II",null,null,null,null,null,0,0,0,null,null,null,null,"1407XX0009.ldt",1,null,null,null,null,1,null,null,null,null,null,null,"LED",16,null,"",null,null,23,null,3000,80,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"","",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"Poland"]
["1409","1409XX0009","HALMSTAD BOLLARD 49CM LED 1059LM 3000K DIM.",null,"A bollard luminaire with a stable and durable structure For lighting private areas and other architectural concepts",null,"Halmstad,Wood","Bollard","Europe, Africa, Asia, Australia and Oceania, North America, South America",2,2,0.34,0,"",null,null,null,null,null,null,null,"1409XX0009.png",7,1,2,3,6,1,66,"CE","","IK10","Class II",null,null,null,null,null,0,0,0,null,null,null,null,"1409XX0009.ldt",1,null,null,null,null,1,null,null,null,null,null,null,"LED",16,null,"",null,null,23,null,3000,80,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"","",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"Poland"]
["1410","1410XX0010","HALMSTAD BOLLARD 85CM E27",null,"Bollard luminaire of stable and durable construction For lighting private areas and public spaces",null,"Halmstad,Wood","Bollard","Europe, Africa, Asia, Australia and Oceania, North America, South America",2,2,0.72,0,"",null,null,null,null,null,null,null,"1410XX0010.jpg",7,1,2,3,6,4,66,"CE","","IK10","Class II",null,null,null,null,null,0,0,0,null,null,null,null,"1410XX0010.ldt",0,null,null,null,null,1,null,null,null,null,null,null,"LED",16,null,"E27",null,null,23,null,"",80,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"","",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"Poland"]
["1413","1413XX0010","HALMSTAD BOLLARD 85CM E27",null,"Bollard luminaire of stable and durable construction. For lighting private areas and public spaces.",null,"Halmstad","Bollard","Europe, Africa, Asia, Australia and Oceania, North America, South America",2,2,0.72,0,"",null,null,null,null,null,null,null,"1413XX0010.jpg",7,1,2,3,6,4,66,"CE","","IK10","Class II",null,null,null,null,null,0,0,0,null,null,null,null,"1413XX0010.ldt",0,null,null,null,null,1,null,null,null,null,null,null,"LED",16,null,"E27",null,null,23,null,"",80,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"","",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"Poland"]
["1417","1417XX0009","HALMSTAD BOLLARD 85CM LED 1059LM 3000K DIM.",null,"A bollard luminaire with a stable and durable structure For lighting private areas and other architectural concepts",null,"Halmstad,Wood","Bollard","Europe, Africa, Asia, Australia and Oceania, North America, South America",2,2,0.7,0,"",null,null,null,null,null,null,null,"1417XX0009.png",7,1,2,3,6,1,66,"CE","","","Class II",null,null,null,null,null,0,0,0,null,null,null,null,"1417XX0009.ldt",1,null,null,null,null,1,null,null,null,null,null,null,"LED",16,null,"",null,null,23,null,3000,80,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"","",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"Poland"]
["1419","1419XX0009","HALMSTAD BOLLARD 85CM LED 1059LM 3000K DIM.",null,"A bollard luminaire with a stable and durable structure For lighting private areas and other architectural concepts",null,"Halmstad,Wood","Bollard","Europe, Africa, Asia, Australia and Oceania, North America, South America",2,2,0.7,0,"",null,null,null,null,null,null,null,"1419XX0009.png",7,1,2,3,6,1,66,"CE","","","Class II",null,null,null,null,null,0,0,0,null,null,null,null,"1419XX0009.ldt",1,null,null,null,null,1,null,null,null,null,null,null,"LED",16,null,"",null,null,23,null,3000,80,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"","",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"Poland"]
["1420","1420XX0010","STOCKHOLM BOLLARD 85CM E27",null,"Bollard luminaire of stable and durable construction. For lighting private areas and public spaces.",null,"Stockholm,Wood","Bollard","Europe, Africa, Asia, Australia and Oceania, North America, South America",2,2,0.68,0,"",null,null,null,null,null,null,null,"1420XX0010.jpg",7,1,1,3,6,4,66,"CE","","IK10","Class II",null,null,null,null,null,0.17,0.17,0.85,null,null,null,null,"1420XX0010.ldt",0,null,null,null,null,1,null,null,null,null,null,null,"LED",16,null,"E27",null,null,23,null,"",80,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"","",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"Poland"]
["1423","1423XX0010","STOCKHOLM BOLLARD 85CM E27",null,"Bollard luminaire of stable and durable construction. For lighting private areas and public spaces.",null,"Stockholm,Wood","Bollard","Europe, Africa, Asia, Australia and Oceania, North America, South America",2,2,0.68,0,"",null,null,null,null,null,null,null,"1423XX0010.jpg",7,1,1,3,6,4,66,"CE","","IK10","Class II",null,null,null,null,null,0.17,0.17,0.85,null,null,null,null,"1423XX0010.ldt",0,null,null,null,null,1,null,null,null,null,null,null,"LED",16,null,"E27",null,null,23,null,"",80,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"","",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"Poland"]
["1426","1426XX0009","STOCKHOLM BOLLARD 85CM LED 1059LM 3000K DIM.",null,"A bollard luminaire with a stable and durable structure For lighting gardens, private areas, and other architectural applications",null,"Stockholm,Wood","Bollard","Europe, Africa, Asia, Australia and Oceania, North America, South America",2,2,0.68,0,"",null,null,null,null,null,null,null,"1426XX0009.png",7,1,1,3,6,1,66,"CE","","","Class II",null,null,null,null,null,0.17,0.17,0.85,null,null,null,null,"1426XX0009.ldt",1,null,null,null,null,1,null,null,null,null,null,null,"LED",16,null,"",null,null,23,null,3000,80,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"","",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"Poland"]
["1429","1429XX0009","STOCKHOLM BOLLARD 85CM LED 1059LM 3000K DIM.",null,"A bollard luminaire with a stable and durable structure For lighting gardens, private areas, and other architectural applications",null,"Stockholm,Wood","Bollard","Europe, Africa, Asia, Australia and Oceania, North America, South America",2,2,0.68,0,"",null,null,null,null,null,null,null,"1429XX0009.png",7,1,1,3,6,1,66,"CE","","","Class II",null,null,null,null,null,0.17,0.17,0.85,null,null,null,null,"1429XX0009.ldt",1,null,null,null,null,1,null,null,null,null,null,null,"LED",16,null,"",null,null,23,null,3000,80,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"","",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"Poland"]
["1430","1430XX0010","STOCKHOLM BOLLARD 49CM E27",null,"Bollard luminaire of stable and durable construction. For lighting private areas and public spaces.",null,"Stockholm,Wood","Bollard","Europe, Africa, Asia, Australia and Oceania, North America, South America",2,2,0.32,0,"",null,null,null,null,null,null,null,"1430XX0010.jpg",7,1,1,3,6,4,66,"CE","","IK10","Class II",null,null,null,null,null,0.17,0.17,0.49,null,null,null,null,"1430XX0010.ldt",0,null,null,null,null,1,null,null,null,null,null,null,"LED",16,null,"E27",null,null,23,null,"",80,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"","",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"Poland"]
["1433","1433XX0010","STOCKHOLM BOLLARD 49CM E27",null,"A bollard luminaire with a stable and durable structure. For lighting private areas and public areas",null,"Stockholm,Wood","Bollard","Europe, Africa, Asia, Australia and Oceania, North America, South America",2,2,0.32,0,"",null,null,null,null,null,null,null,"1433XX0010.jpg",9,1,1,3,6,4,66,"CE","","IK10","Class II",null,null,null,null,null,0.17,0.17,0.49,null,null,null,null,"1433XX0010.ldt",0,null,null,null,null,1,null,null,null,null,null,null,"LED",16,null,"E27",null,null,23,null,"",80,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"","",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"Poland"]
["1436","1436XX0009","STOCKHOLM BOLLARD 49CM LED 1059LM 3000K DIM.",null,"A bollard luminaire with a stable and durable structure For lighting gardens, private areas, parks, and other concepts architectural",null,"Stockholm,Wood","Bollard","Europe, Africa, Asia, Australia and Oceania, North America, South America",2,2,0.32,0,"",null,null,null,null,null,null,null,"1436XX0009.png",7,1,1,3,6,1,66,"CE","","","Class II",null,null,null,null,null,0.17,0.17,0.49,null,null,null,null,"1436XX0009.ldt",1,null,null,null,null,1,null,null,null,null,null,null,"LED",16,null,"",null,null,23,null,3000,80,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"","",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"Poland"]
["1439","1439XX0009","STOCKHOLM BOLLARD 49CM LED 1059LM 3000K DIM.",null,"A bollard luminaire with a stable and durable structure For lighting gardens, private areas, parks, and other concepts architectural",null,"Stockholm,Wood","Bollard","Europe, Africa, Asia, Australia and Oceania, North America, South America",2,2,0.32,0,"",null,null,null,null,null,null,null,"1439XX0009.png",7,1,1,3,6,1,66,"CE","","","Class II",null,null,null,null,null,0,0,0,null,null,null,null,"1439XX0009.ldt",1,null,null,null,null,1,null,null,null,null,null,null,"LED",16,null,"",null,null,23,null,3000,80,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"","",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"Poland"]
["1443","1443XX0010","ALTA BOLLARD 85CM E27",null,"Bollard luminaire of stable and durable construction. For lighting private areas and public spaces.",null,"Alta","Bollard","Europe, Africa, Asia, Australia and Oceania, North America, South America",2,2,0.7,0,"",null,null,null,null,null,null,null,"1443XX0010.jpg",7.3,1,1,3,6,4,66,"CE","","IK10","Class II",null,null,null,null,null,0.15,0.15,0.85,null,null,null,null,"1443XX0010.ldt",0,null,null,null,null,1,null,null,null,null,null,null,"LED",16,null,"E27",null,null,23,null,"",80,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"","",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"Poland"]
["1450","1450XX0010","ALTA BOLLARD 49CM E27",null,"Bollard luminaire of stable and durable construction. For lighting private areas and public spaces.",null,"Alta,Wood","Bollard","Europe, Africa, Asia, Australia and Oceania, North America, South America",2,2,0.34,0,"",null,null,null,null,null,null,null,"1450XX0010.jpg",7.3,1,1,3,6,4,66,"CE","","IK10","Class II",null,null,null,null,null,0.15,0.15,0.49,null,null,null,null,"1450XX0010.ldt",0,null,null,null,null,1,null,null,null,null,null,null,"LED",16,null,"E27",null,null,23,null,"",80,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"","",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"Poland"]
["1453","1453XX0010","ALTA BOLLARD 49CM E27",null,"Bollard luminaire of stable and durable construction. For lighting private areas and public spaces.",null,"Alta","Bollard","Europe, Africa, Asia, Australia and Oceania, North America, South America",2,2,0.34,0,"",null,null,null,null,null,null,null,"1453XX0010.jpg",7.3,1,1,3,6,4,66,"CE","","IK10","Class II",null,null,null,null,null,0.15,0.15,0.49,null,null,null,null,"1453XX0010.ldt",0,null,null,null,null,1,null,null,null,null,null,null,"LED",16,null,"E27",null,null,23,null,"",80,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"","",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"Poland"]
["1464","1464XX0012",{"$f":"INDEX(DB,MATCH($A176,ID,0),3)","v":"STOCKHOLM BOLLARD 85CM LED E27 806LM 2700K DIM."},null,"Bollard luminaire of stable and durable construction. For lighting private areas and public spaces.",null,"Stockholm","Bollard","Europe, Africa, Asia, Australia and Oceania, North America, South America",2,2,0.68,0,"",null,null,null,null,null,null,null,"1464XX0012.jpg",7,1,1,3,6,1,66,"CE","","IK10","Class II",null,null,null,null,null,0.17,0.17,0.85,null,null,null,null,"1464XX0012.ldt",0,null,null,null,null,1,null,null,null,null,null,null,"LED",16,null,"E27",null,null,23,null,2700,80,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"","",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"Poland"]
["1468","1468XX0009","ALTA BOLLARD 49CM LED 1121LM 4000K DIM.",null,"A bollard luminaire with a stable and durable structure For lighting private areas and other architectural concepts",null,"Alta","Bollard","Europe, Africa, Asia, Australia and Oceania, North America, South America",2,2,0.34,0,"",null,null,null,null,null,null,null,"1468XX0009.jpg",7.3,1,1,3,6,1,66,"CE","","","Class II",null,null,null,null,null,0,0,0,null,null,null,null,"1468XX0009.ldt",1,null,null,null,null,1,null,null,null,null,null,null,"LED",16,null,"",null,null,24,null,4000,80,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"","",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"Poland"]
["1469","1469XX0011","STOCKHOLM BOLLARD 49CM LED E27 806LM 2700K DIM.",null,"Bollard luminaire of stable and durable construction. For lighting private areas and public spaces.",null,"Stockholm","Bollard","Europe, Africa, Asia, Australia and Oceania, North America, South America",2,2,0.32,0,"",null,null,null,null,null,null,null,"1469XX0011.jpg",7,1,1,3,6,1,66,"CE","","IK10","Class II",null,null,null,null,null,0.17,0.17,0.49,null,null,null,null,"1469XX0011.ldt",0,null,null,null,null,1,null,null,null,null,null,null,"LED",16,null,"E27",null,null,23,null,2700,80,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"","",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"Poland"]
["1475","1475XX0012","ALTA BOLLARD 85CM LED E27 806LM 2700K DIM.",null,"Bollard luminaire of stable and durable construction. For lighting private areas and public spaces.",null,"Alta","Bollard","Europe, Africa, Asia, Australia and Oceania, North America, South America",2,2,0.7,0,"",null,null,null,null,null,null,null,"1475XX0012.jpg",7.3,1,1,3,6,1,66,"CE","","IK10","Class II",null,null,null,null,null,0.15,0.15,0.85,null,null,null,null,"1475XX0012.ldt",0,null,null,null,null,1,null,null,null,null,null,null,"LED",16,null,"E27",null,null,23,null,2700,80,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"","",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"Poland"]
["1476","1476XX0012","ALTA BOLLARD 49CM LED 1098LM 3000K DIM.",null,"A bollard luminaire with a stable and durable structure. For lighting private areas and public areas",null,"Alta","Bollard","Europe, Africa, Asia, Australia and Oceania, North America, South America",2,2,0.34,0,"",null,null,null,null,null,null,null,"1476XX0012.jpg",7.3,1,1,3,6,1,66,"CE","","","Class I",null,null,null,null,null,0,0,0,null,null,null,null,"1476XX0012.ldt",1,null,null,null,null,1,null,null,null,null,null,null,"LED",16,null,"",null,null,23,null,3000,80,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"","",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"Poland"]
["1477","1477XX0012","ALTA BOLLARD 49CM LED E27 806LM 2700K DIM.",null,"Bollard luminaire of stable and durable construction. For lighting private areas and public spaces.",null,"Alta","Bollard","Europe, Africa, Asia, Australia and Oceania, North America, South America",2,2,0.34,0,"",null,null,null,null,null,null,null,"1477XX0012.jpg",7.3,1,1,3,6,1,66,"CE","","IK10","Class II",null,null,null,null,null,0.15,0.15,0.49,null,null,null,null,"1477XX0012.ldt",0,null,null,null,null,1,null,null,null,null,null,null,"LED",16,null,"E27",null,null,23,null,2700,80,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"","",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"Poland"]
["1479","1479XX0012","ALTA BOLLARD 85CM LED 1098LM 3000K DIM.",null,"A bollard luminaire with a stable and durable structure. For lighting private areas and public areas",null,"Alta","Bollard","Europe, Africa, Asia, Australia and Oceania, North America, South America",2,2,0.7,0,"",null,null,null,null,null,null,null,"1479XX0012.jpg",7.3,1,1,3,6,1,66,"CE","","","Class I",null,null,null,null,null,0,0,0,null,null,null,null,"1479XX0012.ldt",1,null,null,null,null,1,null,null,null,null,null,null,"LED",16,null,"",null,null,23,null,3000,80,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"","",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"Poland"]
["1482","1482XX0013","HALMSTAD BOLLARD 85CM LED 1059LM 3000K DIM.",null,"A bollard luminaire with a stable and durable structure. For lighting private areas and other architectural concepts",null,"Halmstad","Bollard","Europe, Africa, Asia, Australia and Oceania, North America, South America",2,2,0.7,0,"",null,null,null,null,null,null,null,"1482XX0013.jpg",7,1,2,3,6,1,66,"CE","","IK10","Class II",null,null,null,null,null,0,0,0,null,null,null,null,"1482XX0013.ldt",1,null,null,null,null,1,null,null,null,null,null,null,"LED",16,null,"",null,null,23,null,3000,80,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"","",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"Poland"]
["1483","1483XX0012","HALMSTAD BOLLARD 85CM LED E27 806LM 2700K DIM.",null,"Bollard luminaire of stable and durable construction. For lighting private areas and public spaces.",null,"Halmstad","Bollard","Europe, Africa, Asia, Australia and Oceania, North America, South America",2,2,0.72,0,"",null,null,null,null,null,null,null,"1483XX0012.jpg",7,1,2,3,6,1,66,"CE","","IK10","Class II",null,null,null,null,null,0,0,0,null,null,null,null,"1483XX0012.ldt",0,null,null,null,null,1,null,null,null,null,null,null,"LED",16,null,"E27",null,null,23,null,2700,80,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"","",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"Poland"]
["1488","1488XX0012","HALMSTAD BOLLARD 49CM E27 806LM 2700K DIM.",null,"Bollard luminaire of stable and durable construction. For lighting private areas and public spaces.",null,"Halmstad","Bollard","Europe, Africa, Asia, Australia and Oceania, North America, South America",2,2,0.36,0,"",null,null,null,null,null,null,null,"1488XX0012.jpg",7,1,2,3,6,1,66,"CE","","IK10","Class II",null,null,null,null,null,0,0,0,null,null,null,null,"1488XX0012.ldt",0,null,null,null,null,1,null,null,null,null,null,null,"LED",16,null,"E27",null,null,23,null,2700,80,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"","",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"Poland"]
["1495","1495XX0013","PARIS WALL LED 653LM DOWN 3000K DIM.",null,"A luminaire with a classic and simple design for general use",null,"Paris","Wall","Europe, Africa, Asia, Australia and Oceania, North America, South America",2,4,0,2.5,"",null,null,null,null,null,null,null,"1495XX0013.jpg",7,1,5,2,2,1,44,"CE","","","Class I",null,null,null,null,null,0,0,0,null,null,null,null,"1495XX0013.ldt",1,null,null,null,null,0,null,null,null,null,null,null,"LED",16,null,"",null,null,23,null,3000,80,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"","",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"Poland"]
["1496","1496XX0013","PARIS WALL LED 653LM DOWN 3000K DIM.",null,"A luminaire with a classic and simple design for general use",null,"Paris,Big","Wall","Europe, Africa, Asia, Australia and Oceania, North America, South America",2,4,0,2.5,"",null,null,null,null,null,null,null,"1496XX0013.jpg",7,1,5,2,2,1,44,"CE","","","Class I",null,null,null,null,null,0,0,0,null,null,null,null,"1496XX0013.ldt",1,null,null,null,null,0,null,null,null,null,null,null,"LED",16,null,"",null,null,23,null,3000,80,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"","",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"Poland"]
["1510","1510XX0016","ASKER WALL LED 840LM UP-DOWN 3000K DIM.",null,"Luminaire with a wide range of applications for example for illumination of walls and facade surfaces or any other architectural concepts",null,"Asker","Wall","Europe, Africa, Asia, Australia and Oceania, North America, South America",2,4,0,2.5,"",null,null,null,null,null,null,null,"1510XX0016.jpg",8,1,2,2,2,1,66,"CE","","IK08","Class I",null,null,null,null,null,0,0,0,null,null,null,null,"1510XX0016.ldt",1,null,null,null,null,1,null,null,null,null,null,null,"LED",16,null,"",null,null,23,null,3000,80,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"","",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"Poland"]
["1511","1511XX0016","ASKER WALL LED 840LM DOWN 3000K DIM.",null,"A luminaire with a wide range of applications, including lighting wall surfaces, facades, and other architectural concepts",null,"Asker","Wall","Europe, Africa, Asia, Australia and Oceania, North America, South America",2,4,0,2.5,"",null,null,null,null,null,null,null,"1511XX0016.jpg",7,1,2,2,2,1,66,"CE","","IK08","Class I",null,null,null,null,null,0,0,0,null,null,null,null,"1511XX0016.ldt",1,null,null,null,null,0,null,null,null,null,null,null,"LED",16,null,"",null,null,23,null,3000,80,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"","",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"Poland"]
["1513","1513XX0013","ASKER WALL E27 UP-DOWN",null,"Luminaire with a wide range of applications for example for illumination of walls and facade surfaces or any other architectural concepts.",null,"Asker","Wall","Europe, Africa, Asia, Australia and Oceania, North America, South America",2,4,0,2.5,"",null,null,null,null,null,null,null,"1513XX0013.jpg",8,1,2,2,2,4,66,"CE","","IK08","Class I",null,null,null,null,null,0.22,0.11,0.08,null,null,null,null,"1513XX0013.ldt",0,null,null,null,null,1,null,null,null,null,null,null,"LED",16,null,"E27",null,null,23,null,"",80,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"","",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"Poland"]
["1514","1514XX0013","ASKER WALL E27",null,"Luminaire with a wide range of applications for example for illumination of walls and facade surfaces or any other architectural concepts.",null,"Asker","Wall","Europe, Africa, Asia, Australia and Oceania, North America, South America",2,4,0,2.5,"",null,null,null,null,null,null,null,"1514XX0013.jpg",3,1,2,2,2,4,66,"CE","","IK08","Class I",null,null,null,null,null,0.22,0.11,0.08,null,null,null,null,"1514XX0013.ldt",0,null,null,null,null,0,null,null,null,null,null,null,"LED",16,null,"E27",null,null,23,null,"",80,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"","",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"Poland"]
["1544","1544XX0014","GRIMSTAD WALL-RECESSED LED 653LM 3000K DIM.",null,"The luminaire is adapted to illuminate stairs, steps, staircases, pathways, and other places",null,"Grimstad","Recessed","Europe, Africa, Asia, Australia and Oceania, North America, South America",2,64,0,0.5,"",null,null,null,null,null,null,null,"1544XX0014.jpg",8,1,2,2,1,1,66,"CE","","IK08","Class I",null,null,null,null,null,0,0,0,null,null,null,null,"1544XX0014.ldt",1,null,null,null,null,4,null,null,null,null,1,null,"LED",16,null,"",null,null,23,null,3000,80,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"","",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"Poland"]
["1545","1545XX0012","GRIMSTAD WALL-RECESSED LED 981LM 3000K DIM.",null,"The luminaire is adapted to illuminate stairs, steps, staircases, communication pathways and other applications",null,"Grimstad","Recessed","Europe, Africa, Asia, Australia and Oceania, North America, South America",2,64,0,0.5,"",null,null,null,null,null,null,null,"1545XX0012.jpg",7,1,2,2,1,1,66,"CE","","IK09","Class I",null,null,null,null,null,0,0,0,null,null,null,null,"1545XX0012.ldt",1,null,null,null,null,4,null,null,null,null,null,null,"LED",16,null,"",null,null,23,null,3000,80,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"","",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"Poland"]
["1551","1551XX0016",{"$f":"INDEX(DB,MATCH($A194,ID,0),3)","v":"RENA IN-GROUND LED GU10 375LM 36D 3000K DIM."},null,"Indicative luminaire or as a spotlight on which you can ride with pneumatic tires. Luminaires should not be used on traffic lanes, where they would be exposed to horizontal weight due to sudden braking, acceleration, and reversing. Adjustable angle of the light max. up to 10 degrees",null,{"$f":"IF(INDEX(DB,MATCH($A194,ID,0),4)=0,\"\",INDEX(DB,MATCH($A194,ID,0),4))","v":"Rena"},{"$f":"IF(INDEX(DB,MATCH($A194,ID,0),5)=0,\"\",INDEX(DB,MATCH($A194,ID,0),5))","v":"Recessed"},"Europe, Africa, Asia, Australia and Oceania, North America, South America",2,{"$f":"IFERROR(INDEX(TYPMONT,MATCH((INDEX(DB,MATCH($A194,ID,0),31)),ID_RODZ,0),3),\"\")","v":128},-0.127,0,{"$f":"IFERROR(IF(INDEX(TYPMONT,MATCH((INDEX(DB,MATCH($A194,ID,0),31)),ID_RODZ,0),6)=0,\"\",INDEX(TYPMONT,MATCH((INDEX(DB,MATCH($A194,ID,0),31)),ID_RODZ,0),6)),\"\")","v":""},null,null,null,null,null,null,null,{"$f":"IF(INDEX(DB,MATCH($A194,ID,0),57)=0,\"\",INDEX(DB,MATCH($A194,ID,0),57))","v":"1551XX0016.jpg"},2,{"$f":"IF(INDEX(DB,MATCH($A194,ID,0),61)=0,\"\",INDEX(DB,MATCH($A194,ID,0),61))","v":3},2,{"$f":"IFERROR(INDEX(TYPMONT,MATCH((INDEX(DB,MATCH($A194,ID,0),31)),ID_RODZ,0),1),\"\")","v":3},{"$f":"IFERROR(INDEX(TYPMONT,MATCH((INDEX(DB,MATCH($A194,ID,0),31)),ID_RODZ,0),2),\"\")","v":1},{"$f":"IF(INDEX(DB,MATCH($A194,ID,0),59)=0,\"\",INDEX(DB,MATCH($A194,ID,0),59))","v":1},{"$f":"IFERROR(IF(INDEX(DB,MATCH($A194,ID,0),19)=0,\"\",INDEX(DB,MATCH($A194,ID,0),19)+1),\"\")","v":69},{"$f":"IF(INDEX(DB,MATCH($A194,ID,0),27)=0,\"\",INDEX(DB,MATCH($A194,ID,0),27))","v":"CE"},{"$f":"IFERROR(IF(FIND(\"RENA\",$C194)>0,\"Vehicle resistant\",\"\"),\"\")","v":"Vehicle resistant"},{"$f":"IF(INDEX(DB,MATCH($A194,ID,0),20)=0,\"\",INDEX(DB,MATCH($A194,ID,0),20))","v":"IK09"},{"$f":"IF(INDEX(DB,MATCH($A194,ID,0),21)=0,\"\",INDEX(DB,MATCH($A194,ID,0),21))","v":"Class I"},null,null,null,null,null,0.13,0.13,0.16,null,null,null,null,{"$f":"IF(INDEX(DB,MATCH($A194,ID,0),58)=0,\"\",INDEX(DB,MATCH($A194,ID,0),58))","v":"1551XX0016.ldt"},0,null,null,null,null,2,null,null,null,null,1,null,"LED",16,null,{"$f":"IF(INDEX(DB,MATCH($A194,ID,0),60)=0,\"\",INDEX(DB,MATCH($A194,ID,0),60))","v":"GU10"},null,null,{"$f":"IF($BO194=4000,24,23)","v":23},null,{"$f":"IF(INDEX(DB,MATCH($A194,ID,0),22)=0,\"\",INDEX(DB,MATCH($A194,ID,0),22))","v":3000},{"$f":"IF(INDEX(DB,MATCH($A194,ID,0),53)=0,\"\",INDEX(DB,MATCH($A194,ID,0),53))","v":90},null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,{"$f":"IF(INDEX(DB,MATCH($A194,ID,0),29)=0,\"\",INDEX(DB,MATCH($A194,ID,0),29))","v":""},{"$f":"IF(INDEX(DB,MATCH($A194,ID,0),28)=0,\"\",INDEX(DB,MATCH($A194,ID,0),28))","v":""},null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"Poland"]
["1552","1552XX0014","RENA IN-GROUND LED GU10",null,"An orientation luminaire that can be driven on by vehicles with pneumatic tires. Luminaires should not be used on traffic lanes where they would be exposed to horizontal weight load as a result of sudden braking, acceleration, and change of direction. The light direction angle can be adjusted, up to a maximum of 10 degrees",null,"Rena","Recessed","Europe, Africa, Asia, Australia and Oceania, North America, South America",2,128,-0.127,0,"",null,null,null,null,null,null,null,"1552XX0014.jpg",9,3,1,3,1,4,69,"CE","Vehicle resistant","IK09","Class I",null,null,null,null,null,0.13,0.13,0.17,null,null,null,null,"1552XX0014.ldt",0,null,null,null,null,2,null,null,null,null,1,null,"LED",16,null,"GU10",null,null,23,null,"",80,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"","",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"Poland"]
["1553","1553XX0014","RENA IN-GROUND LED GU10",null,"Indicative luminaire or as a spotlight on which you can ride with pneumatic tires. Luminaires should not be used on traffic lanes, where they would be exposed to horizontal weight due to sudden braking, acceleration, and reversing. Adjustable angle of the light maximum up to 10 degrees",null,"Rena","Recessed","Europe, Africa, Asia, Australia and Oceania, North America, South America",2,128,-0.127,0,"",null,null,null,null,null,null,null,"1553XX0014.jpg",9,3,2,3,1,4,69,"CE","Vehicle resistant","IK09","Class I",null,null,null,null,null,0.13,0.13,0.17,null,null,null,null,"1553XX0014.ldt",0,null,null,null,null,2,null,null,null,null,1,null,"LED",16,null,"GU10",null,null,23,null,"",80,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"","",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"Poland"]
["1554","1554XX0016","RENA IN-GROUND LED GU10 375LM 36D 3000K DIM.",null,"Indicative luminaire or as a spotlight on which you can ride with pneumatic tires. Luminaires should not be used on traffic lanes, where they would be exposed to horizontal weight due to sudden braking, acceleration, and reversing. Adjustable angle of the light max. up to 10 degrees",null,"Rena","Recessed","Europe, Africa, Asia, Australia and Oceania, North America, South America",2,128,-0.127,0,"",null,null,null,null,null,null,null,"1554XX0016.jpg",2,3,1,3,1,1,69,"CE","Vehicle resistant","IK09","Class I",null,null,null,null,null,0,0,0,null,null,null,null,"1554XX0016.ldt",0,null,null,null,null,2,null,null,null,null,1,null,"LED",16,null,"GU10",null,null,23,null,3000,90,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"","",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"Poland"]
["1555","1555XX0016","RENA IN-GROUND LED GU10 375LM 36D 3000K DIM.",null,"An orientation luminaire that can be driven on by vehicles with pneumatic tires. Luminaires should not be used on traffic lanes where they would be exposed to horizontal weight load as a result of sudden braking, acceleration, and change of direction. The light direction angle can be adjusted, up to a maximum of 10 degrees",null,"Rena","Recessed","Europe, Africa, Asia, Australia and Oceania, North America, South America",2,128,-0.127,0,"",null,null,null,null,null,null,null,"1555XX0016.jpg",2,3,2,3,1,1,69,"CE","Vehicle resistant","IK09","Class I",null,null,null,null,null,0,0,0,null,null,null,null,"1555XX0016.ldt",0,null,null,null,null,2,null,null,null,null,1,null,"LED",16,null,"GU10",null,null,23,null,3000,90,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"","",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"Poland"]
["1556",{"$f":"INDEX(DB,MATCH($A199,ID,0),2)","v":"1556XX0014"},"RENA IN-GROUND LED GU10 375LM",null,{"$f":"IF(INDEX(DB,MATCH($A199,ID,0),35)=0,\"\",INDEX(DB,MATCH($A199,ID,0),35))","v":"Indicative luminaire or as a spotlight on which you can ride with pneumatic tires. Luminaires should not be used on traffic lanes, where they would be exposed to horizontal weight due to sudden braking, acceleration, and reversing. Adjustable angle of the light maximum up to 10 degrees"},null,"Rena","Recessed","Europe, Africa, Asia, Australia and Oceania, North America, South America",2,128,-0.127,0,"",null,null,null,null,null,null,null,"1556XX0014.jpg",{"$f":"IF((IFERROR(INDEX(BRYLA_FOTO,MATCH(INDEX(DB,MATCH($A199,ID,0),62),ID_BRYLAFOTO,0),6),\"\"))<>0,IFERROR(INDEX(BRYLA_FOTO,MATCH(INDEX(DB,MATCH($A199,ID,0),62),ID_BRYLAFOTO,0),6),\"\"),\"\")","v":8},3,1,3,1,4,69,"CE","Vehicle resistant","IK09","Class I",null,null,null,null,null,{"$f":"INDEX(DB,MATCH($A199,ID,0),24)","v":0.13},{"$f":"INDEX(DB,MATCH($A199,ID,0),25)","v":0.13},{"$f":"INDEX(DB,MATCH($A199,ID,0),26)","v":0.17},null,null,null,null,"1556XX0014.ldt",0,null,null,null,null,2,null,null,null,null,1,null,"LED",16,null,"GU10",null,null,23,null,"",80,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"","",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"Poland"]
["1557","1557XX0014","RENA IN-GROUND LED GU10 375LM",null,"Indicative luminaire or as a spotlight on which you can ride with pneumatic tires. Luminaires should not be used on traffic lanes, where they would be exposed to horizontal weight due to sudden braking, acceleration, and reversing. Adjustable angle of the light maximum up to 10 degrees",null,"Rena","Recessed","Europe, Africa, Asia, Australia and Oceania, North America, South America",2,128,-0.127,0,"",null,null,null,null,null,null,null,"1557XX0014.jpg",8,3,2,3,1,4,69,"CE","Vehicle resistant","IK09","Class I",null,null,null,null,null,0.13,0.13,0.16,null,null,null,null,"1557XX0014.ldt",{"$f":"IF($BJ200=\"\",1,0)","v":0},null,null,null,null,2,null,null,null,null,1,null,"LED",16,null,"GU10",null,null,23,null,"",80,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"","",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"Poland"]
["1561","1561XX0010","ARENDAL MINI BOLLARD 64CM LED 439LM 3000K DIM.",null,"A luminaire with a modern design, which combines a decorative crystal lampshade with a durable and stable base.",null,"Arendal Mini","Bollard","Europe, Africa, Asia, Australia and Oceania, North America, South America",2,2,0.53,0,"",null,null,null,null,null,null,null,"1561XX0010.jpg",9,1,2,3,6,1,66,"CE","","IK08","Class II",null,null,null,null,null,0,0,0,null,null,null,null,"1561XX0010.ldt",1,null,null,null,null,1,null,null,null,null,null,null,"LED",16,null,"",null,null,23,null,3000,80,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"","",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"Poland"]
["1562","1562XX0010","ARENDAL MINI BOLLARD 64CM LED 466LM 4000K DIM.",null,"A luminaire with a modern design, which combines a decorative crystal lampshade with a durable and stable base.",null,"Arendal Mini","Bollard","Europe, Africa, Asia, Australia and Oceania, North America, South America",2,2,0.53,0,"",null,null,null,null,null,null,null,"1562XX0010.jpg",9,1,2,3,6,1,66,"CE","","IK08","Class II",null,null,null,null,null,0,0,0,null,null,null,null,"1562XX0010.ldt",1,null,null,null,null,1,null,null,null,null,null,null,"LED",16,null,"",null,null,24,null,4000,80,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"","",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"Poland"]
["1566","1566XX0010","ARENDAL MINI BOLLARD 37CM LED 439LM 3000K DIM.",null,"A luminaire with a modern design, in which a combination of a decorative crystal lampshade with a durable and stable structure of the luminaire.",null,"Arendal Mini","Bollard","Europe, Africa, Asia, Australia and Oceania, North America, South America",2,2,0.26,0,"",null,null,null,null,null,null,null,"1566XX0010.jpg",9,1,2,3,6,1,66,"CE","","IK08","Class II",null,null,null,null,null,0,0,0,null,null,null,null,"1566XX0010.ldt",1,null,null,null,null,1,null,null,null,null,null,null,"LED",16,null,"",null,null,23,null,3000,80,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"","",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"Poland"]
["1567","1567XX0009","ARENDAL MINI BOLLARD 37CM LED 466LM 4000K DIM.",null,"A luminaire with a modern design, combining a decorative crystal lampshade with a durable and stable luminaire base",null,"Arendal Mini","Bollard","Europe, Africa, Asia, Australia and Oceania, North America, South America",2,2,0.26,0,"",null,null,null,null,null,null,null,"1567XX0009.jpg",9,1,2,3,6,1,66,"CE","","IK08","Class II",null,null,null,null,null,0,0,0,null,null,null,null,"1567XX0009.ldt",1,null,null,null,null,1,null,null,null,null,null,null,"LED",16,null,"",null,null,24,null,4000,80,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"","",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"Poland"]
["1581","1581XX0016","LILLEHAMMER WALL 2XLED 1008LM UP60º & DOWN60º 3000K DIM.",null,"Luminaire with a wide range of applications, among others for lighting: wall surfaces, facades and other architectural concepts",null,"Lillehammer","Wall","Europe, Africa, Asia, Australia and Oceania, North America, South America",2,4,0,2.5,"",null,null,null,null,null,null,null,"1581XX0016.jpg",10,1,2,2,2,1,66,"CE","","IK08","Class I",null,null,null,null,null,0.18,0.11,0.08,null,null,null,null,"1581XX0016.ldt",1,null,null,null,null,1,null,null,null,null,null,null,"LED",16,null,"",null,null,23,null,3000,80,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"","",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"Poland"]
["1582","1582XX0016","LILLEHAMMER WALL LED 504LM DOWN60º 3000K DIM. TE",null,"A luminaire with a wide range of applications, including lighting wall surfaces, facades and other architectural concepts",null,"Lillehammer","Wall","Europe, Africa, Asia, Australia and Oceania, North America, South America",2,4,0,2.5,"",null,null,null,null,null,null,null,"1582XX0016.jpg",10,1,2,2,2,1,66,"CE","","IK08","Class I",null,null,null,null,null,0.18,0.11,0.08,null,null,null,null,"1582XX0016.ldt",1,null,null,null,null,0,null,null,null,null,null,null,"LED",16,null,"",null,null,23,null,3000,80,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"","",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"Poland"]
["1583","1583XX0017","LILLEHAMMER WALL 2XLED 1008LM UP4º & DOWN4º 3000K DIM.",null,"A luminaire with a wide range of applications, including lighting: wall surfaces, facades and other architectural concepts",null,"Lillehammer","Wall","Europe, Africa, Asia, Australia and Oceania, North America, South America",2,4,0,2.5,"",null,null,null,null,null,null,null,"1583XX0017.jpg",10,1,2,2,2,1,66,"CE","","IK08","Class I",null,null,null,null,null,0.18,0.11,0.08,null,null,null,null,"1583XX0017.ldt",1,null,null,null,null,1,null,null,null,null,null,null,"LED",16,null,"",null,null,23,null,3000,80,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"","",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"Poland"]
["1584","1584XX0017","LILLEHAMMER WALL LED 504LM DOWN 4º 3000K DIM.",null,"A luminaire with a wide range of applications, including lighting wall surfaces, facades and other architectural concepts",null,"Lillehammer","Wall","Europe, Africa, Asia, Australia and Oceania, North America, South America",2,4,0,2.5,"",null,null,null,null,null,null,null,"1584XX0017.jpg",10,1,2,2,2,1,66,"CE","","IK08","Class I",null,null,null,null,null,0.18,0.11,0.08,null,null,null,null,"1584XX0017.ldt",1,null,null,null,null,0,null,null,null,null,null,null,"LED",16,null,"",null,null,23,null,3000,80,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"","",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"Poland"]
["1585","1585XX0009","LILLEHAMMER WALL LED 504LM UP 4º 3000K DIM.",null,"A luminaire with a wide range of applications, including lighting wall surfaces, facades and other architectural concepts",null,"Lillehammer","Wall","Europe, Africa, Asia, Australia and Oceania, North America, South America",2,4,0,2.5,"",null,null,null,null,null,null,null,"1585XX0009.jpg",10,1,2,2,2,1,66,"CE","","IK08","Class I",null,null,null,null,null,0.18,0.11,0.08,null,null,null,null,"1585XX0009.ldt",1,null,null,null,null,2,null,null,null,null,null,null,"LED",16,null,"",null,null,23,null,3000,80,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"","",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"Poland"]
["1586","1586XX0010","LILLEHAMMER WALL LED 534LM UP 4º 4000K DIM.",null,"A luminaire with a wide range of applications, including lighting wall surfaces, facades and other architectural concepts",null,"Lillehammer","Wall","Europe, Africa, Asia, Australia and Oceania, North America, South America",2,4,0,2.5,"",null,null,null,null,null,null,null,"1586XX0010.jpg",10,1,2,2,2,1,66,"CE","","IK08","Class I",null,null,null,null,null,0.18,0.11,0.08,null,null,null,null,"1586XX0010.ldt",1,null,null,null,null,2,null,null,null,null,null,null,"LED",16,null,"",null,null,24,null,4000,80,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"","",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"Poland"]
["1587","1587XX0009","LILLEHAMMER WALL LED 504LM UP60º 3000K DIM.",null,"A luminaire with a wide range of applications, including lighting wall surfaces, facades and other architectural concepts",null,"Lillehammer","Wall","Europe, Africa, Asia, Australia and Oceania, North America, South America",2,4,0,{"$f":"IF(K211=4,2.5,IF(K211=64,0.5,0))","v":2.5},"",null,null,null,null,null,null,null,"1587XX0009.jpg",10,1,2,2,2,1,66,"CE","","IK08","Class I",null,null,null,null,null,0.18,0.11,0.08,null,null,null,null,"1587XX0009.ldt",1,null,null,null,null,2,null,null,null,null,null,null,"LED",16,null,"",null,null,23,null,3000,80,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"","",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"Poland"]
["1588","1588XX0009","LILLEHAMMER WALL LED 534LM UP60º 4000K DIM.",null,"A luminaire with a wide range of applications, including lighting wall surfaces, facades and other architectural concepts",null,"Lillehammer","Wall","Europe, Africa, Asia, Australia and Oceania, North America, South America",2,4,0,2.5,"",null,null,null,null,null,null,null,"1588XX0009.jpg",10,1,2,2,2,1,66,"CE","","IK08","Class I",null,null,null,null,null,0.18,0.11,0.08,null,null,null,null,"1588XX0009.ldt",1,null,null,null,null,2,null,null,null,null,null,null,"LED",16,null,"",null,null,24,null,4000,80,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"","",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"Poland"]
["1592","1592XX0012","SANDE FLOODLIGHT-BOX LED GU10 375LM 36D 3000K DIM.",null,"Reflector type luminaire for permanent mounting. For lighting gardens and other private areas and public spaces. Possibility to adjust the direction of light in the vertical plane.",null,"Sande,Stick","Spot,Ground","Europe, Africa, Asia, Australia and Oceania, North America, South America",2,2,0,0,"",null,null,null,null,null,null,null,"1592XX0012.jpg",2,4,1,3,6.7,1,66,"CE","","IK08","Class I",null,null,null,null,null,0,0,0,null,null,null,null,"1592XX0012.ldt",0,null,null,null,null,2,null,null,null,null,1,null,"LED",16,null,"GU10",null,null,23,null,3000,90,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"","",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"Poland"]
["1593","1593XX0015","SANDE FLOODLIGHT-EARTHSPIKE LED 854LM 40D 3000K DIM.",null,"Fixed and portable spotlight. For lighting private areas, parks, and other architectural concepts. Possibility to adjust the lighting direction vertically",null,"Sande,Stick","Spot,Ground","Europe, Africa, Asia, Australia and Oceania, North America, South America",2,2,0,0,"",null,null,null,null,null,null,null,"1593XX0015.jpg",2,4,1,3,7,1,66,"CE","","IK08","Class I",null,null,null,null,null,0.19,0.1,0.1,null,null,null,null,"1593XX0015.ldt",1,null,null,null,null,2,null,null,null,null,1,null,"LED",16,null,"",null,null,23,null,3000,90,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"","",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"Poland"]
["1594","1594XX0014","SANDE FLOODLIGHT-BOX LED 854LM 40D 3000K DIM.",null,"Spotlight for lighting private areas, parks, and other concepts architectural. The light direction can be adjusted vertically and horizontally",null,"Sande,Base","Spot,Ground/Wall","Europe, Africa, Asia, Australia and Oceania, North America, South America",2,2,0,0,"",null,null,null,null,null,null,null,"1594XX0014.jpg",2,4,1,3,6.7,1,66,"CE","","IK08","Class I",null,null,null,null,null,0.15,0.09,0.24,null,null,null,null,"1594XX0014.ldt",1,null,null,null,null,2,null,null,null,null,1,null,"LED",16,null,"",null,null,23,null,3000,80,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"","",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"Poland"]
["1598","1598XX0012","SANDE FLOODLIGHT-BOX LED GU10 375LM 36D 3000K DIM.",null,"Reflector type luminaire for permanent mounting. For lighting gardens and other private areas and public spaces. Possibility to adjust the direction of light in the vertical and horizontal plane.",null,"Sande,Base","Spot,Ground/Wall","Europe, Africa, Asia, Australia and Oceania, North America, South America",2,2,0,0,"",null,null,null,null,null,null,null,"1598XX0012.jpg",2,4,1,3,6.7,1,66,"CE","","IK08","Class I",null,null,null,null,null,0,0,0,null,null,null,null,"1598XX0012.ldt",0,null,null,null,null,2,null,null,null,null,1,null,"LED",16,null,"GU10",null,null,23,null,3000,90,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"","",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"Poland"]
["1600","1600XX0013","STOCKHOLM WALL LED 743LM 3000K DIM.",null,"Luminaire with Scandinavian design. For lighting gardens, private areas and other architectural concepts",null,"Stockholm,Połówka","Wall,Ceiling","Europe, Africa, Asia, Australia and Oceania, North America, South America",2,4,0,2.5,"",null,null,null,null,null,null,null,"1600XX0013.jpg",8,1,2,2,2,1,55,"CE","","IK10","Class I",null,null,null,null,null,0,0,0,null,null,null,null,"1600XX0013.ldt",1,null,null,null,null,3,null,null,null,null,null,null,"LED",16,null,"",null,null,23,null,3000,80,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"","",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"Poland"]
["160","160XX0010","PARIS SMALL WALL E27 DOWN",null,"A luminaire with a classic and simple design for general use",null,"Paris","Wall","Europe, Africa, Asia, Australia and Oceania, North America, South America",2,4,0,2.5,"",null,null,null,null,null,null,null,"160XX0010.jpg",7,1,5,2,2,4,44,"CE","","","Class I",null,null,null,null,null,0.23,0.14000000000000001,0.12,null,null,null,null,"160XX0010.ldt",0,null,null,null,null,0,null,null,null,null,null,null,"LED",16,null,"E27",null,null,23,null,"",80,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"","",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"Poland"]
["1620","1620XX0013","NORDKAPP WALL LED 1419LM 3000K DIM.",null,"A ceiling-type luminaire with a modern design. For lighting private areas and other architectural concepts",null,"Nordkapp","Wall,Ceiling","Europe, Africa, Asia, Australia and Oceania, North America, South America",2,4,0,2.5,"",null,null,null,null,null,null,null,"1620XX0013.jpg",8,1,2,2,2,1,66,"CE","","","Class I",null,null,null,null,null,0,0,0,null,null,null,null,"1620XX0013.ldt",1,null,null,null,null,0,null,null,null,null,null,null,"LED",16,null,"",null,null,23,null,3000,80,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"","",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"Poland"]
["1630","1630XX0012","RENA IN-GROUND LED GU10",null,"An orientation luminaire that can be driven on by vehicles with pneumatic tires. Luminaires should not be used on traffic lanes where they would be exposed to horizontal weight load as a result of sudden braking, acceleration, and change of direction",null,"Rena","Recessed","Europe, Africa, Asia, Australia and Oceania, North America, South America",2,128,-0.127,0,"",null,null,null,null,null,null,null,"1630XX0012.jpg",4,3,1,3,1,4,69,"CE","Vehicle resistant","IK10","Class I",null,null,null,null,null,0.13,0.13,0.18,null,null,null,null,"1630XX0012.ldt",0,null,null,null,null,2,null,null,null,null,null,null,"LED",16,null,"GU10",null,null,23,null,"",80,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"","",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"Poland"]
["1632","1632XX0012","RENA IN-GROUND LED GU10",null,"An orientation luminaire that can be driven on by vehicles with pneumatic tires. Luminaires should not be used on traffic lanes where they would be exposed to horizontal weight load as a result of sudden braking, acceleration, and change of direction",null,"Rena","Recessed","Europe, Africa, Asia, Australia and Oceania, North America, South America",2,128,-0.127,0,"",null,null,null,null,null,null,null,"1632XX0012.jpg",4,3,2,3,1,4,69,"CE","Vehicle resistant","IK10","Class I",null,null,null,null,null,0.13,0.13,0.18,null,null,null,null,"1632XX0012.ldt",0,null,null,null,null,2,null,null,null,null,null,null,"LED",16,null,"GU10",null,null,23,null,"",80,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"","",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"Poland"]
["1633","1633XX0011","RENA IN-GROUND LED GU10 375LM 3000K DIM.",null,"An orientation luminaire or as a reflector on which vehicles with pneumatic tires can be driven. Luminaires should not be used on standard road lanes, where they would be exposed to horizontal loads as a result of sudden braking, acceleration, and change of direction",null,"Rena","Recessed","Europe, Africa, Asia, Australia and Oceania, North America, South America",2,128,-0.127,0,"",null,null,null,null,null,null,null,"1633XX0011.jpg",4,3,2,3,1,1,69,"CE","Vehicle resistant","IK10","Class I",null,null,null,null,null,0,0,0,null,null,null,null,"1633XX0011.ldt",0,null,null,null,null,2,null,null,null,null,null,null,"LED",16,null,"GU10",null,null,23,null,3000,90,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"","",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"Poland"]
["163","163XX0010","PARIS WALL E27 DOWN",null,"Classic design luminaire with a wide range of applications for example for illumination of walls and facade surfaces or any other architectural concepts.",null,"Paris,Big","Wall","Europe, Africa, Asia, Australia and Oceania, North America, South America",2,4,0,2.5,"",null,null,null,null,null,null,null,"163XX0010.jpg",7,1,5,2,2,4,44,"CE","","","Class I",null,null,null,null,null,0.28000000000000003,0.16,0.14000000000000001,null,null,null,null,"163XX0010.ldt",0,null,null,null,null,0,null,null,null,null,null,null,"LED",16,null,"E27",null,null,23,null,"",80,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"","",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"Poland"]
["1640","1640XX0009","RENA IN-GROUND LED GU10 375LM 36D 3000K DIM.",null,"An orientation luminaire that can be driven on by vehicles with pneumatic tires. Luminaires should not be used on traffic lanes where they would be exposed to horizontal weight load as a result of sudden braking, acceleration, and change of direction. The light direction angle can be adjusted, up to a maximum of 10 degrees",null,"Rena","Recessed","Europe, Africa, Asia, Australia and Oceania, North America, South America",2,128,-0.127,0,"",null,null,null,null,null,null,null,"1640XX0009.jpg",2,3,1,3,1,1,69,"CE","Vehicle resistant","","Class I",null,null,null,null,null,0,0,0,null,null,null,null,"1640XX0009.ldt",0,null,null,null,null,2,null,null,null,null,1,null,"LED",16,null,"GU10",null,null,23,null,3000,90,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"","",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"Poland"]
["1641","1641XX0009","RENA IN-GROUND LED GU10 375LM 36D 3000K DIM.",null,"An orientation luminaire or as a reflector on which vehicles with pneumatic tires can be driven. Luminaires should not be used on road lanes where they would be exposed to horizontal loads as a result of sudden braking, acceleration, and direction changes. The angle of the lighting direction can be adjusted, up to a maximum of 10 degrees",null,"Rena","Recessed","Europe, Africa, Asia, Australia and Oceania, North America, South America",2,128,-0.127,0,"",null,null,null,null,null,null,null,"1641XX0009.jpg",2,3,1,3,1,1,69,"CE","Vehicle resistant","","Class I",null,null,null,null,null,0,0,0,null,null,null,null,"1641XX0009.ldt",0,null,null,null,null,2,null,null,null,null,1,null,"LED",16,null,"GU10",null,null,23,null,3000,90,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"","",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"Poland"]
["1642","1642XX0009","RENA IN-GROUND LED GU10",null,"An orientation luminaire or as a driveable reflector with pneumatic tires. Luminaires should not be used on road lanes where they would be exposed to horizontal loads as a result of sudden braking, acceleration, and direction changes. The angle of the lighting direction can be adjusted, up to a maximum of 10 degrees",null,"Rena","Recessed","Europe, Africa, Asia, Australia and Oceania, North America, South America",2,128,-0.127,0,"",null,null,null,null,null,null,null,"1642XX0009.jpg",9,3,1,3,1,4,69,"CE","Vehicle resistant","","Class I",null,null,null,null,null,0,0,0,null,null,null,null,"1642XX0009.ldt",0,null,null,null,null,2,null,null,null,null,1,null,"LED",16,null,"GU10",null,null,23,null,"",80,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"","",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"Poland"]
["1643","1643XX0009","RENA IN-GROUND LED GU10",null,"An orientation luminaire or as a driveable reflector with pneumatic tires. Luminaires should not be used on the road lanes where they would be exposed to horizontal loads as a result of sudden braking, acceleration, and direction changes. The angle of the lighting direction can be adjusted, up to a maximum of 10 degrees",null,"Rena","Recessed","Europe, Africa, Asia, Australia and Oceania, North America, South America",2,128,-0.127,0,"",null,null,null,null,null,null,null,"1643XX0009.jpg",9,3,2,3,1,4,69,"CE","Vehicle resistant","","Class I",null,null,null,null,null,0,0,0,null,null,null,null,"1643XX0009.ldt",0,null,null,null,null,2,null,null,null,null,1,null,"LED",16,null,"GU10",null,null,23,null,"",80,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"","",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"Poland"]
["1644","1644XX0009","RENA IN-GROUND LED GU10 375LM 36D 3000K DIM.",null,"An orientation luminaire or as a reflector on which vehicles with pneumatic tires can be driven. Luminaires should not be used on the road lanes where they would be exposed to horizontal loads as a result of sudden braking, acceleration, and direction changes. The angle of the lighting direction can be adjusted, up to a maximum of 10 degrees",null,"Rena","Recessed","Europe, Africa, Asia, Australia and Oceania, North America, South America",2,128,-0.127,0,"",null,null,null,null,null,null,null,"1644XX0009.jpg",2,3,1,3,1,1,69,"CE","Vehicle resistant","","Class I",null,null,null,null,null,0.13,0.13,0.28000000000000003,null,null,null,null,"1644XX0009.ldt",0,null,null,null,null,2,null,null,null,null,1,null,"LED",16,null,"GU10",null,null,23,null,3000,90,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"","",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"Poland"]
["1645","1645XX0009","RENA IN-GROUND LED GU10 375LM 36D 3000K DIM.",null,"An orientation luminaire or as a reflector on which vehicles with pneumatic tires can be driven. Luminaires should not be used on the road lanes where they would be exposed to horizontal loads as a result of sudden braking, acceleration, and direction changes. The angle of the lighting direction can be adjusted, up to a maximum of 10 degrees",null,"Rena","Recessed","Europe, Africa, Asia, Australia and Oceania, North America, South America",2,128,-0.127,0,"",null,null,null,null,null,null,null,"1645XX0009.jpg",2,3,2,3,1,1,69,"CE","Vehicle resistant","","Class I",null,null,null,null,null,0,0,0,null,null,null,null,"1645XX0009.ldt",0,null,null,null,null,2,null,null,null,null,1,null,"LED",16,null,"GU10",null,null,23,null,3000,90,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"","",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"Poland"]
["1646","1646XX0009","RENA IN-GROUND LED GU10",null,"An orientation luminaire or as a driveable reflector with pneumatic tires. Luminaires should not be used on the road lanes where they would be exposed to horizontal loads as a result of sudden braking, acceleration, and direction changes. The angle of the lighting direction can be adjusted, up to a maximum of 10 degrees",null,"Rena","Recessed","Europe, Africa, Asia, Australia and Oceania, North America, South America",2,128,-0.127,0,"",null,null,null,null,null,null,null,"1646XX0009.jpg",8,3,1,3,1,4,69,"CE","Vehicle resistant","","Class I",null,null,null,null,null,0,0,0,null,null,null,null,"1646XX0009.ldt",0,null,null,null,null,2,null,null,null,null,1,null,"LED",16,null,"GU10",null,null,23,null,"",80,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"","",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"Poland"]
["1647","1647XX0009","RENA IN-GROUND LED GU10",null,"An orientation luminaire or as a driveable reflector with pneumatic tires. Luminaires should not be used on the road lanes where they would be exposed to horizontal loads as a result of sudden braking, acceleration, and direction changes. The angle of the lighting direction can be adjusted, up to a maximum of 10 degrees",null,"Rena","Recessed","Europe, Africa, Asia, Australia and Oceania, North America, South America",2,128,-0.127,0,"",null,null,null,null,null,null,null,"1647XX0009.jpg",8,3,2,3,1,4,69,"CE","Vehicle resistant","","Class I",null,null,null,null,null,0,0,0,null,null,null,null,"1647XX0009.ldt",0,null,null,null,null,2,null,null,null,null,1,null,"LED",16,null,"GU10",null,null,23,null,"",80,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"","",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"Poland"]
["1650","1650XX0009","RENA IN-GROUND LED GU10",null,"An orientation luminaire on which vehicles with pneumatic tires can be driven. Luminaires should not be used on the road lanes, where they would be exposed to horizontal loads as a result of sudden braking, acceleration, and change of direction",null,"Rena","Recessed","Europe, Africa, Asia, Australia and Oceania, North America, South America",2,128,-0.127,0,"",null,null,null,null,null,null,null,"1650XX0009.jpg",4,3,1,3,1,4,69,"CE","Vehicle resistant","","Class I",null,null,null,null,null,0,0,0,null,null,null,null,"1650XX0009.ldt",0,null,null,null,null,2,null,null,null,null,null,null,"LED",16,null,"GU10",null,null,23,null,"",80,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"","",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"Poland"]
["1651","1651XX0009","RENA IN-GROUND LED GU10 375LM 3000K DIM.",null,"An orientation luminaire on which vehicles with pneumatic tires can be driven. Luminaires should not be used on the road lanes, where they would be exposed to horizontal loads as a result of sudden braking, acceleration, and change of direction",null,"Rena","Recessed","Europe, Africa, Asia, Australia and Oceania, North America, South America",2,128,-0.127,0,"",null,null,null,null,null,null,null,"1651XX0009.jpg",4,3,1,3,1,1,69,"CE","Vehicle resistant","","Class I",null,null,null,null,null,0,0,0,null,null,null,null,"1651XX0009.ldt",0,null,null,null,null,2,null,null,null,null,null,null,"LED",16,null,"GU10",null,null,23,null,3000,90,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"","",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"Poland"]
["1652","1652XX0009","RENA IN-GROUND LED GU10",null,"An orientation luminaire on which vehicles with pneumatic tires can be driven. Luminaires should not be used on the road lanes, where they would be exposed to horizontal loads as a result of sudden braking, acceleration, and change of direction",null,"Rena","Recessed","Europe, Africa, Asia, Australia and Oceania, North America, South America",2,128,-0.127,0,"",null,null,null,null,null,null,null,"1652XX0009.jpg",4,3,2,3,1,4,69,"CE","Vehicle resistant","","Class I",null,null,null,null,null,0,0,0,null,null,null,null,"1652XX0009.ldt",0,null,null,null,null,2,null,null,null,null,null,null,"LED",16,null,"GU10",null,null,23,null,"",80,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"","",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"Poland"]
["1653","1653XX0009","RENA IN-GROUND LED GU10 375LM 3000K DIM.",null,"An orientation luminaire on which vehicles with pneumatic tires can be driven. Luminaires should not be used on the road lanes, where they would be exposed to horizontal loads as a result of sudden braking, acceleration, and change of direction",null,"Rena","Recessed","Europe, Africa, Asia, Australia and Oceania, North America, South America",2,128,-0.127,0,"",null,null,null,null,null,null,null,"1653XX0009.jpg",4,3,2,3,1,1,69,"CE","Vehicle resistant","","Class I",null,null,null,null,null,0,0,0,null,null,null,null,"1653XX0009.ldt",0,null,null,null,null,2,null,null,null,null,null,null,"LED",16,null,"GU10",null,null,23,null,3000,90,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"","",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"Poland"]
["1700","1700XX0011","ASKER WALL LED 743LM UP-DOWN 3000K DIM.",null,"A luminaire with a wide range of applications, including lighting wall surfaces, facades and other architectural concepts",null,"Asker","Wall","Europe, Africa, Asia, Australia and Oceania, North America, South America",2,4,0,2.5,"",null,null,null,null,null,null,null,"1700XX0011.jpg",8,1,2,2,2,1,45,"CE","","IK08","Class I",null,null,null,null,null,0,0,0,null,null,null,null,"1700XX0011.ldt",1,null,null,null,null,1,null,null,null,null,null,null,"LED",16,null,"",null,null,23,null,3000,80,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"","",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"Poland"]
["1702","1702XX0010","ASKER WALL E27 UP-DOWN",null,"Luminaire with a wide range of applications for example for illumination of walls and facade surfaces or any other architectural concepts.",null,"Asker","Wall","Europe, Africa, Asia, Australia and Oceania, North America, South America",2,4,0,2.5,"",null,null,null,null,null,null,null,"1702XX0010.jpg",8,1,2,2,2,4,45,"CE","","","Class I",null,null,null,null,null,0.22,0.11,0.08,null,null,null,null,"1702XX0010.ldt",0,null,null,null,null,1,null,null,null,null,null,null,"LED",16,null,"E27",null,null,23,null,"",80,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"","",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"Poland"]
["1705","1705XX0011","ASKER WALL LED 840LM DOWN 3000K DIM.",null,"A luminaire with a wide range of applications, including lighting wall surfaces, facades, and other architectural concepts",null,"Asker","Wall","Europe, Africa, Asia, Australia and Oceania, North America, South America",2,4,0,2.5,"",null,null,null,null,null,null,null,"1705XX0011.jpg",7,1,2,2,2,1,45,"CE","","IK08","Class I",null,null,null,null,null,0,0,0,null,null,null,null,"1705XX0011.ldt",1,null,null,null,null,0,null,null,null,null,null,null,"LED",16,null,"",null,null,23,null,3000,80,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"","",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"Poland"]
["1707","1707XX0010","ASKER WALL E27 DOWN",null,"Luminaire with a wide range of applications for example for illumination of walls and facade surfaces or any other architectural concepts.",null,"Asker","Wall","Europe, Africa, Asia, Australia and Oceania, North America, South America",2,4,0,2.5,"",null,null,null,null,null,null,null,"1707XX0010.jpg",7,1,2,2,2,4,45,"CE","","IK08","Class I",null,null,null,null,null,0.22,0.11,0.08,null,null,null,null,"1707XX0010.ldt",0,null,null,null,null,0,null,null,null,null,null,null,"LED",16,null,"E27",null,null,23,null,"",80,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"","",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"Poland"]
["1710","1710XX0011","ASKER BIG WALL 2XLED 1128LM UP-DOWN 3000K DIM.",null,"Luminaire with a wide range of applications for example for illumination of walls and facade surfaces or any other architectural concepts",null,"Asker,Big","Wall","Europe, Africa, Asia, Australia and Oceania, North America, South America",2,4,0,2.5,"",null,null,null,null,null,null,null,"1710XX0011.jpg",8,1,2,2,2,1,45,"CE","","IK08","Class I",null,null,null,null,null,0,0,0,null,null,null,null,"1710XX0011.ldt",1,null,null,null,null,1,null,null,null,null,null,null,"LED",16,null,"",null,null,23,null,3000,80,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"","",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"Poland"]
["1712","1712XX0010","ASKER BIG WALL E27 UP-DOWN",null,"Luminaire with a wide range of applications for example for illumination of walls and facade surfaces or any other architectural concepts.",null,"Asker,Big","Wall","Europe, Africa, Asia, Australia and Oceania, North America, South America",2,4,0,2.5,"",null,null,null,null,null,null,null,"1712XX0010.jpg",8,1,2,2,2,4,45,"CE","","IK08","Class I",null,null,null,null,null,0,0,0,null,null,null,null,"1712XX0010.ldt",0,null,null,null,null,1,null,null,null,null,null,null,"LED",16,null,"E27",null,null,23,null,"",80,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"","",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"Poland"]
["1715","1715XX0011","ASKER BIG WALL LED 653LM DOWN 3000K DIM.",null,"A luminaire with a wide range of applications, for illuminating wall and facade surfaces as well as other architectural concepts",null,"Asker,Big","Wall","Europe, Africa, Asia, Australia and Oceania, North America, South America",2,4,0,2.5,"",null,null,null,null,null,null,null,"1715XX0011.jpg",7,1,2,2,2,1,45,"CE","","IK08","Class I",null,null,null,null,null,0,0,0,null,null,null,null,"1715XX0011.ldt",1,null,null,null,null,0,null,null,null,null,null,null,"LED",16,null,"",null,null,23,null,3000,80,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"","",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"Poland"]
["1717","1717XX0010","ASKER BIG WALL E27 DOWN",null,"Luminaire with a wide range of applications for example for illumination of walls and facade surfaces or any other architectural concepts.",null,"Asker,Big","Wall","Europe, Africa, Asia, Australia and Oceania, North America, South America",2,4,0,2.5,"",null,null,null,null,null,null,null,"1717XX0010.jpg",7,1,2,2,2,4,45,"CE","","IK08","Class I",null,null,null,null,null,0,0,0,null,null,null,null,"1717XX0010.ldt",0,null,null,null,null,0,null,null,null,null,null,null,"LED",16,null,"E27",null,null,23,null,"",80,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"","",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"Poland"]
["1720","1720XX0010","ASKER SMALL PRO WALL 2XLED 1128LM UP-DOWN 3000K DIM.",null,"A luminaire with a wide range of applications, including lighting wall surfaces, facades, and other architectural concepts",null,"Asker","Wall","Europe, Africa, Asia, Australia and Oceania, North America, South America",2,4,0,2.5,"",null,null,null,null,null,null,null,"1720XX0010.jpg",8,1,2,2,2,1,66,"CE","","IK08","Class I",null,null,null,null,null,0,0,0,null,null,null,null,"1720XX0010.ldt",1,null,null,null,null,1,null,null,null,null,null,null,"LED",16,null,"",null,null,23,null,3000,80,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"","",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"Poland"]
["1726","1726XX0010","ASKER SMALL PRO WALL LED 653LM DOWN 3000K DIM. TE",null,"A luminaire with a wide range of applications, including lighting wall surfaces, facades, and other architectural concepts",null,"Asker","Wall","Europe, Africa, Asia, Australia and Oceania, North America, South America",2,4,0,2.5,"",null,null,null,null,null,null,null,"1726XX0010.jpg",7,1,2,2,2,1,66,"CE","","IK08","Class I",null,null,null,null,null,0,0,0,null,null,null,null,"1726XX0010.ldt",1,null,null,null,null,0,null,null,null,null,null,null,"LED",16,null,"",null,null,23,null,3000,80,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"","",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"Poland"]
["1727","1727XX0009","ASKER SMALL PRO WALL LED 653LM DOWN 3000K DALI2",null,"A luminaire with a wide range of applications, including lighting wall surfaces, facades, and other architectural concepts",null,"Asker","Wall","Europe, Africa, Asia, Australia and Oceania, North America, South America",2,4,0,2.5,"",null,null,null,null,null,null,null,"1727XX0009.jpg",7,1,2,2,2,3,66,"CE","","","Class I",null,null,null,null,null,0.22,0.11,0.08,null,null,null,null,"1727XX0009.ldt",1,null,null,null,null,0,null,null,null,null,null,null,"LED",16,null,"",null,null,23,null,3000,80,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"DALI","",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"Poland"]
["1730","1730XX0009","SANDVIK WALL 2XLED GU10 UP-DOWN",null,"Classic design ceiling luminaire. For lighting private areas and public spaces.",null,"Sandvik","Wall","Europe, Africa, Asia, Australia and Oceania, North America, South America",2,4,0,2.5,"",null,null,null,null,null,null,null,"1730XX0009.jpg",8,1,2,2,2,4,66,"CE","","IK08","Class I",null,null,null,null,null,0,0,0,null,null,null,null,"1730XX0009.ldt",0,null,null,null,null,1,null,null,null,null,null,null,"LED",16,null,"GU10",null,null,23,null,"",80,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"","",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"Poland"]
["1731","1731XX0009","SANDVIK WALL 2XLED GU10 530LM UP-DOWN 2700K DIM.",null,"Classic design ceiling luminaire. For lighting private areas and public spaces.",null,"Sandvik","Wall","Europe, Africa, Asia, Australia and Oceania, North America, South America",2,4,0,2.5,"",null,null,null,null,null,null,null,"1731XX0009.jpg",8,1,2,2,2,1,66,"CE","","IK08","Class I",null,null,null,null,null,0,0,0,null,null,null,null,"1731XX0009.ldt",0,null,null,null,null,1,null,null,null,null,null,null,"LED",16,null,"GU10",null,null,23,null,2700,90,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"","",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"Poland"]
["1732","1732XX0009","SANDVIK WALL 2XLED 1512LM UP36D&DOWN36D 3000K DIM.",null,"Classic design ceiling luminaire. For lighting private areas and public spaces.",null,"Sandvik","Wall","Europe, Africa, Asia, Australia and Oceania, North America, South America",2,4,0,2.5,"",null,null,null,null,null,null,null,"1732XX0009.jpg",2,1,2,2,2,1,66,"CE","","IK08","Class I",null,null,null,null,null,0,0,0,null,null,null,null,"1732XX0009.ldt",1,null,null,null,null,1,null,null,null,null,null,null,"LED",16,null,"",null,null,23,null,3000,80,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"","",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"Poland"]
["1735","1735XX0010","NARVIK II BOLLARD LED 3017LM 3000K DALI2",null,"A bollard luminaire with a stable and durable structure. For lighting private and public areas",null,"Narvik","Bollard","Europe, Africa, Asia, Australia and Oceania, North America, South America",2,2,0.7,0,"",null,null,null,null,null,null,null,"1735XX0010.png",4,1,1,3,6,3,66,"CE","","IK10","Class II",null,null,null,null,null,0.24,0.24,0.95,null,null,null,null,"1735XX0010.ldt",1,null,null,null,null,0,null,null,null,null,null,null,"LED",16,null,"",null,null,23,null,3000,80,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"DALI","",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"Poland"]
["1736","1736XX0010","NARVIK II BOLLARD LED 3017LM 3000K DALI2",null,"A bollard luminaire with a stable and durable structure. For lighting private and public areas",null,"Narvik","Bollard","Europe, Africa, Asia, Australia and Oceania, North America, South America",2,2,0.7,0,"",null,null,null,null,null,null,null,"1736XX0010.png",4,1,1,3,6,3,66,"CE","","IK10","Class II",null,null,null,null,null,0.24,0.24,0.95,null,null,null,null,"1736XX0010.ldt",1,null,null,null,null,0,null,null,null,null,null,null,"LED",16,null,"",null,null,23,null,3000,80,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"DALI","",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"Poland"]
["1737","1737XX0010","NARVIK II BOLLARD LED 3200LM 4000K DALI2",null,"A bollard luminaire with a stable and durable structure. For lighting private and public areas",null,"Narvik","Bollard","Europe, Africa, Asia, Australia and Oceania, North America, South America",2,2,0.7,0,"",null,null,null,null,null,null,null,"1737XX0010.png",4,1,1,3,6,3,66,"CE","","IK10","Class II",null,null,null,null,null,0.24,0.24,0.95,null,null,null,null,"1737XX0010.ldt",1,null,null,null,null,0,null,null,null,null,null,null,"LED",16,null,"",null,null,24,null,4000,80,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"DALI","",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"Poland"]
["1738","1738XX0010",{"$f":"INDEX(DB,MATCH($A253,ID,0),3)","v":"NARVIK II BOLLARD LED 3200LM 4000K DALI2"},null,"A bollard luminaire with a stable and durable structure. For lighting private and public areas",null,"Narvik",{"$f":"IF(INDEX(DB,MATCH($A253,ID,0),5)=0,\"\",INDEX(DB,MATCH($A253,ID,0),5))","v":"Bollard"},"Europe, Africa, Asia, Australia and Oceania, North America, South America",2,{"$f":"IFERROR(INDEX(TYPMONT,MATCH((INDEX(DB,MATCH($A253,ID,0),31)),ID_RODZ,0),3),\"\")","v":2},0.7,0,{"$f":"IFERROR(IF(INDEX(TYPMONT,MATCH((INDEX(DB,MATCH($A253,ID,0),31)),ID_RODZ,0),6)=0,\"\",INDEX(TYPMONT,MATCH((INDEX(DB,MATCH($A253,ID,0),31)),ID_RODZ,0),6)),\"\")","v":""},null,null,null,null,null,null,null,{"$f":"IF(INDEX(DB,MATCH($A253,ID,0),57)=0,\"\",INDEX(DB,MATCH($A253,ID,0),57))","v":"1738XX0010.png"},4,{"$f":"IF(INDEX(DB,MATCH($A253,ID,0),61)=0,\"\",INDEX(DB,MATCH($A253,ID,0),61))","v":1},1,{"$f":"IFERROR(INDEX(TYPMONT,MATCH((INDEX(DB,MATCH($A253,ID,0),31)),ID_RODZ,0),1),\"\")","v":3},{"$f":"IFERROR(INDEX(TYPMONT,MATCH((INDEX(DB,MATCH($A253,ID,0),31)),ID_RODZ,0),2),\"\")","v":6},{"$f":"IF(INDEX(DB,MATCH($A253,ID,0),59)=0,\"\",INDEX(DB,MATCH($A253,ID,0),59))","v":3},{"$f":"IFERROR(IF(INDEX(DB,MATCH($A253,ID,0),19)=0,\"\",INDEX(DB,MATCH($A253,ID,0),19)+1),\"\")","v":66},{"$f":"IF(INDEX(DB,MATCH($A253,ID,0),27)=0,\"\",INDEX(DB,MATCH($A253,ID,0),27))","v":"CE"},"",{"$f":"IF(INDEX(DB,MATCH($A253,ID,0),20)=0,\"\",INDEX(DB,MATCH($A253,ID,0),20))","v":"IK10"},{"$f":"IF(INDEX(DB,MATCH($A253,ID,0),21)=0,\"\",INDEX(DB,MATCH($A253,ID,0),21))","v":"Class II"},null,null,null,null,null,0.24,0.24,0.95,null,null,null,null,{"$f":"IF(INDEX(DB,MATCH($A253,ID,0),58)=0,\"\",INDEX(DB,MATCH($A253,ID,0),58))","v":"1738XX0010.ldt"},1,null,null,null,null,0,null,null,null,null,null,null,"LED",16,null,{"$f":"IF(INDEX(DB,MATCH($A253,ID,0),60)=0,\"\",INDEX(DB,MATCH($A253,ID,0),60))","v":""},null,null,24,null,{"$f":"IF(INDEX(DB,MATCH($A253,ID,0),22)=0,\"\",INDEX(DB,MATCH($A253,ID,0),22))","v":4000},{"$f":"IF(INDEX(DB,MATCH($A253,ID,0),53)=0,\"\",INDEX(DB,MATCH($A253,ID,0),53))","v":80},null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,{"$f":"IF(INDEX(DB,MATCH($A253,ID,0),29)=0,\"\",INDEX(DB,MATCH($A253,ID,0),29))","v":"DALI"},{"$f":"IF(INDEX(DB,MATCH($A253,ID,0),28)=0,\"\",INDEX(DB,MATCH($A253,ID,0),28))","v":""},null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"Poland"]
["1740","1740XX0009","SANDVIK DOWN WALL LED GU10 DOWN 25D",null,"Classic design wall luminaire. For lighting private areas and public spaces",null,{"$f":"IF(INDEX(DB,MATCH($A254,ID,0),4)=0,\"\",INDEX(DB,MATCH($A254,ID,0),4))","v":"Sandvik"},"Wall","Europe, Africa, Asia, Australia and Oceania, North America, South America",2,4,0,2.5,"",null,null,null,null,null,null,null,"1740XX0009.jpg",2,1,2,2,2,4,66,"CE",{"$f":"IFERROR(IF(FIND(\"RENA\",$C254)>0,\"Vehicle resistant\",\"\"),\"\")","v":""},"IK08","Class I",null,null,null,null,null,0,0,0,null,null,null,null,"1740XX0009.ldt",0,null,null,null,null,0,null,null,null,null,null,null,"LED",16,null,"GU10",null,null,{"$f":"IF($BO254=4000,24,23)","v":23},null,"",80,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"","",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"Poland"]
["1741","1741XX0009","SANDVIK DOWN WALL LED GU10 265LM DOWN 25D 2700K DIM.",null,"Classic design ceiling luminaire. For lighting private areas and public spaces",null,"Sandvik","Wall","Europe, Africa, Asia, Australia and Oceania, North America, South America",2,4,0,2.5,"",null,null,null,null,null,null,null,"1741XX0009.jpg",2,1,2,2,2,1,66,"CE","","IK08","Class I",null,null,null,null,null,0,0,0,null,null,null,null,"1741XX0009.ldt",0,null,null,null,null,0,null,null,null,null,null,null,"LED",16,null,"GU10",null,null,23,null,2700,90,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"","",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"Poland"]
["1742","1742XX0009","SANDVIK DOWN WALL LED 756LM DOWN 36D 3000K DIM.",null,"Classic design wall luminaire. For lighting private areas and public spaces",null,"Sandvik","Wall","Europe, Africa, Asia, Australia and Oceania, North America, South America",2,4,0,2.5,"",null,null,null,null,null,null,null,"1742XX0009.jpg",2,1,2,2,2,1,66,"CE","","IK08","Class I",null,null,null,null,null,0,0,0,null,null,null,null,"1742XX0009.ldt",1,null,null,null,null,0,null,null,null,null,null,null,"LED",16,null,"",null,null,23,null,3000,80,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"","",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"Poland"]
["1751","1751XX0009","RENA IN-GROUND LED 466LM 4000K DIM.",null,"An orientation luminaire on which vehicles with pneumatic tires can be driven. Luminaires should not be used on the road lanes, where they would be exposed to horizontal loads as a result of sudden braking, acceleration, and change of direction",null,"Rena","Recessed","Europe, Africa, Asia, Australia and Oceania, North America, South America",2,128,-0.127,0,"",null,null,null,null,null,null,null,"1751XX0009.jpg",8,1,1,3,1,1,69,"CE","Vehicle resistant","IK09","Class I",null,null,null,null,null,0.13,0.13,0.17,null,null,null,null,"1751XX0009.ldt",1,null,null,null,null,2,null,null,null,null,1,null,"LED",16,null,"",null,null,24,null,4000,80,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"","",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"Poland"]
["1753","1753XX0009","RENA IN-GROUND LED 466LM 4000K DIM.",null,"An orientation luminaire on which vehicles with pneumatic tires can be driven. Luminaires should not be used on the road lanes, where they would be exposed to horizontal loads as a result of sudden braking, acceleration, and change of direction",null,"Rena","Recessed","Europe, Africa, Asia, Australia and Oceania, North America, South America",2,128,-0.127,0,"",null,null,null,null,null,null,null,"1753XX0009.jpg",8,1,2,3,1,1,69,"CE","Vehicle resistant","IK09","Class I",null,null,null,null,null,0.13,0.13,0.16,null,null,null,null,"1753XX0009.ldt",1,null,null,null,null,2,null,null,null,null,1,null,"LED",16,null,"",null,null,24,null,4000,80,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"","",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"Poland"]
["1754","1754XX0009","RENA IN-GROUND LED 880LM 3000K DIM.",null,"An orientation luminaire on which vehicles with pneumatic tires can be driven. Luminaires should not be used on the road lanes, where they would be exposed to horizontal loads as a result of sudden braking, acceleration, and change of direction",null,"Rena","Recessed","Europe, Africa, Asia, Australia and Oceania, North America, South America",2,128,-0.127,0,"",null,null,null,null,null,null,null,"1754XX0009.jpg",8,1,1,3,1,1,69,"CE","Vehicle resistant","IK09","Class I",null,null,null,null,null,0.13,0.13,0.17,null,null,null,null,"1754XX0009.ldt",1,null,null,null,null,2,null,null,null,null,1,null,"LED",16,null,"",null,null,23,null,3000,80,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"","",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"Poland"]
["1755","1755XX0009","RENA IN-GROUND LED 891LM 4000K DIM.",null,"An orientation luminaire on which vehicles with pneumatic tires can be driven. Luminaires should not be used on the road lanes, where they would be exposed to horizontal loads as a result of sudden braking, acceleration, and change of direction",null,"Rena","Recessed","Europe, Africa, Asia, Australia and Oceania, North America, South America",2,128,-0.127,0,"",null,null,null,null,null,null,null,"1755XX0009.jpg",8,1,1,3,1,1,69,"CE","Vehicle resistant","IK09","Class I",null,null,null,null,null,0.17,0.13,0.13,null,null,null,null,"1755XX0009.ldt",1,null,null,null,null,2,null,null,null,null,1,null,"LED",16,null,"",null,null,24,null,4000,80,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"","",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"Poland"]
["1756","1756XX0009","RENA IN-GROUND LED 880LM 3000K DIM.",null,"An orientation luminaire on which vehicles with pneumatic tires can be driven. Luminaires should not be used on the road lanes, where they would be exposed to horizontal loads as a result of sudden braking, acceleration, and change of direction",null,"Rena","Recessed","Europe, Africa, Asia, Australia and Oceania, North America, South America",2,128,-0.127,0,"",null,null,null,null,null,null,null,"1756XX0009.jpg",8,1,2,3,1,1,69,"CE","Vehicle resistant","IK09","Class I",null,null,null,null,null,0,0,0,null,null,null,null,"1756XX0009.ldt",1,null,null,null,null,2,null,null,null,null,1,null,"LED",16,null,"",null,null,23,null,3000,80,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"","",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"Poland"]
["1757","1757XX0009","RENA IN-GROUND LED 891LM 4000K DIM.",null,"An orientation luminaire on which vehicles with pneumatic tires can be driven. Luminaires should not be used on the road lanes, where they would be exposed to horizontal loads as a result of sudden braking, acceleration, and change of direction",null,"Rena","Recessed","Europe, Africa, Asia, Australia and Oceania, North America, South America",2,128,-0.127,0,"",null,null,null,null,null,null,null,"1757XX0009.jpg",8,1,2,3,1,1,69,"CE","Vehicle resistant","IK09","Class I",null,null,null,null,null,0,0,0,null,null,null,null,"1757XX0009.ldt",1,null,null,null,null,2,null,null,null,null,1,null,"LED",16,null,"",null,null,24,null,4000,80,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"","",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"Poland"]
["1760",{"$f":"INDEX(DB,MATCH($A263,ID,0),2)","v":"1760XX0009"},"RENA IN-GROUND LED 460LM 36D 3000K DIM. TRIAC",null,{"$f":"IF(INDEX(DB,MATCH($A263,ID,0),35)=0,\"\",INDEX(DB,MATCH($A263,ID,0),35))","v":"Indicative luminaire or as a spotlight on which you can ride with pneumatic tires. Luminaires should not be used on the road lanes, where they would be exposed to horizontal loads as a result of sudden braking, acceleration, and change of direction"},null,"Rena","Recessed","Europe, Africa, Asia, Australia and Oceania, North America, South America",2,128,-0.16,0,"",null,null,null,null,null,null,null,"1760XX0009.png",{"$f":"IF((IFERROR(INDEX(BRYLA_FOTO,MATCH(INDEX(DB,MATCH($A263,ID,0),62),ID_BRYLAFOTO,0),6),\"\"))<>0,IFERROR(INDEX(BRYLA_FOTO,MATCH(INDEX(DB,MATCH($A263,ID,0),62),ID_BRYLAFOTO,0),6),\"\"),\"\")","v":2},1,1,3,1,1,69,"CE","Vehicle resistant","IK09","Class I",null,null,null,null,null,{"$f":"INDEX(DB,MATCH($A263,ID,0),24)","v":0},{"$f":"INDEX(DB,MATCH($A263,ID,0),25)","v":0},{"$f":"INDEX(DB,MATCH($A263,ID,0),26)","v":0},null,null,null,null,"1760XX0009.ldt",1,null,null,null,null,2,null,null,null,null,null,null,"LED",16,null,"",null,null,23,null,3000,80,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"","",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"Poland"]
["1761","1761XX0009","RENA IN-GROUND LED 488LM 36D 4000K DIM. TRIAC",null,"Indicative luminaire or as a spotlight on which you can ride with pneumatic tires. Luminaires should not be used on the road lanes, where they would be exposed to horizontal loads as a result of sudden braking, acceleration, and change of direction",null,"Rena","Recessed","Europe, Africa, Asia, Australia and Oceania, North America, South America",2,128,-0.16,0,"",null,null,null,null,null,null,null,"1761XX0009.png",2,1,1,3,1,1,69,"CE","Vehicle resistant","","Class I",null,null,null,null,null,0,0,0,null,null,null,null,"1761XX0009.ldt",{"$f":"IF($BJ264=\"\",1,0)","v":1},null,null,null,null,2,null,null,null,null,null,null,"LED",16,null,"",null,null,24,null,4000,80,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"","",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"Poland"]
["1762","1762XX0009","RENA IN-GROUND LED 460LM 36D 3000K DIM.",null,"",null,"Rena","Recessed","Europe, Africa, Asia, Australia and Oceania, North America, South America",2,128,-0.16,0,"",null,null,null,null,null,null,null,"1762XX0009.png",2,1,2,3,1,1,69,"CE","Vehicle resistant","IK09","Class I",null,null,null,null,null,0.13,0.13,0.16,null,null,null,null,"1762XX0009.ldt",1,null,null,null,null,2,null,null,null,null,null,null,"LED",16,null,"",null,null,23,null,3000,80,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"","",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"Poland"]
["1763","1763XX0009","RENA IN-GROUND LED 488LM 36D 4000K DIM.",null,"Indicative luminaire or as a spotlight on which you can ride with pneumatic tires. Luminaires should not be used on the road lanes, where they would be exposed to horizontal loads as a result of sudden braking, acceleration, and change of direction",null,"Rena","Recessed","Europe, Africa, Asia, Australia and Oceania, North America, South America",2,128,-0.16,0,"",null,null,null,null,null,null,null,"1763XX0009.png",2,1,2,3,1,1,69,"CE","Vehicle resistant","","Class I",null,null,null,null,null,0.13,0.13,0.16,null,null,null,null,"1763XX0009.ldt",1,null,null,null,null,2,null,null,null,null,null,null,"LED",16,null,"",null,null,24,null,4000,80,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"","",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"Poland"]
["1764","1764XX0009","RENA IN-GROUND LED 880LM 36D 3000K DIM. TRIAC",null,"Indicative luminaire or as a spotlight on which you can ride with pneumatic tires. Luminaires should not be used on the road lanes, where they would be exposed to horizontal loads as a result of sudden braking, acceleration, and change of direction",null,"Rena","Recessed","Europe, Africa, Asia, Australia and Oceania, North America, South America",2,128,-0.16,0,"",null,null,null,null,null,null,null,"1764XX0009.png",2,1,1,3,1,1,69,"CE","Vehicle resistant","IK09","Class I",null,null,null,null,null,0,0,0,null,null,null,null,"1764XX0009.ldt",1,null,null,null,null,2,null,null,null,null,null,null,"LED",16,null,"",null,null,23,null,3000,80,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"","",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"Poland"]
["1765","1765XX0009","RENA IN-GROUND LED 933LM 36D 4000K DIM. TRIAC",null,"Indicative luminaire or as a spotlight on which you can ride with pneumatic tires. Luminaires should not be used on the road lanes, where they would be exposed to horizontal loads as a result of sudden braking, acceleration, and change of direction",null,"Rena","Recessed","Europe, Africa, Asia, Australia and Oceania, North America, South America",2,128,-0.16,0,"",null,null,null,null,null,null,null,"1765XX0009.png",2,1,1,3,1,1,69,"CE","Vehicle resistant","","Class I",null,null,null,null,null,0,0,0,null,null,null,null,"1765XX0009.ldt",1,null,null,null,null,2,null,null,null,null,null,null,"LED",16,null,"",null,null,24,null,4000,80,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"","",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"Poland"]
["1766","1766XX0009","RENA IN-GROUND LED 880LM 36D 3000K DIM.",null,"Indicative luminaire or as a spotlight on which you can ride with pneumatic tires. Luminaires should not be used on the road lanes, where they would be exposed to horizontal loads as a result of sudden braking, acceleration, and change of direction",null,"Rena","Recessed","Europe, Africa, Asia, Australia and Oceania, North America, South America",2,128,-0.16,0,"",null,null,null,null,null,null,null,"1766XX0009.png",2,1,2,3,1,1,69,"CE","Vehicle resistant","IK09","Class I",null,null,null,null,null,0.13,0.13,0.16,null,null,null,null,"1766XX0009.ldt",1,null,null,null,null,2,null,null,null,null,null,null,"LED",16,null,"",null,null,23,null,3000,80,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"","",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"Poland"]
["1767","1767XX0009","RENA IN-GROUND LED 933LM 36D 4000K DIM.",null,"Indicative luminaire or as a spotlight on which you can ride with pneumatic tires. Luminaires should not be used on the road lanes, where they would be exposed to horizontal loads as a result of sudden braking, acceleration, and change of direction",null,"Rena","Recessed","Europe, Africa, Asia, Australia and Oceania, North America, South America",2,128,-0.16,0,"",null,null,null,null,null,null,null,"1767XX0009.png",2,1,2,3,1,1,69,"CE","Vehicle resistant","","Class I",null,null,null,null,null,0.13,0.13,0.16,null,null,null,null,"1767XX0009.ldt",1,null,null,null,null,2,null,null,null,null,null,null,"LED",16,null,"",null,null,24,null,4000,80,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"","",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"Poland"]
["1769","1769XX0009","RENA IN-GROUND LED 488LM 4000K DIM.",null,"Indicative luminaire or as a spotlight on which you can ride with pneumatic tires. Luminaires should not be used on the road lanes, where they would be exposed to horizontal loads as a result of sudden braking, acceleration, and change of direction",null,"Rena","Recessed","Europe, Africa, Asia, Australia and Oceania, North America, South America",2,128,-0.127,0,"",null,null,null,null,null,null,null,"1769XX0009.jpg",4,1,1,3,1,1,69,"CE","Vehicle resistant","","Class I",null,null,null,null,null,0.13,0.13,0.18,null,null,null,null,"1769XX0009.ldt",1,null,null,null,null,2,null,null,null,null,1,null,"LED",16,null,"",null,null,24,null,4000,80,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"","",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"Poland"]
["1773","1773XX0009","RENA IN-GROUND LED 933LM 4000K DIM.",null,"Indicative luminaire or as a spotlight on which you can ride with pneumatic tires. Luminaires should not be used on the road lanes, where they would be exposed to horizontal loads as a result of sudden braking, acceleration, and change of direction",null,"Rena","Recessed","Europe, Africa, Asia, Australia and Oceania, North America, South America",2,128,-0.127,{"$f":"IF(K272=4,2.5,IF(K272=64,0.5,0))","v":0},"",null,null,null,null,null,null,null,"1773XX0009.jpg",4,1,1,3,1,1,69,"CE","Vehicle resistant","","Class I",null,null,null,null,null,0.13,0.13,0.18,null,null,null,null,"1773XX0009.ldt",1,null,null,null,null,2,null,null,null,null,1,null,"LED",16,null,"",null,null,24,null,4000,80,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"","",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"Poland"]
["1774","1774XX0009","RENA IN-GROUND LED 880LM 3000K DIM.",null,"Indicative luminaire or as a spotlight on which you can ride with pneumatic tires. Luminaires should not be used on the road lanes, where they would be exposed to horizontal loads as a result of sudden braking, acceleration, and change of direction",null,"Rena","Recessed","Europe, Africa, Asia, Australia and Oceania, North America, South America",2,128,-0.127,0,"",null,null,null,null,null,null,null,"1774XX0009.jpg",4,1,2,3,1,1,69,"CE","Vehicle resistant","","Class I",null,null,null,null,null,0.13,0.13,0.18,null,null,null,null,"1774XX0009.ldt",1,null,null,null,null,2,null,null,null,null,1,null,"LED",16,null,"",null,null,23,null,3000,80,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"","",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"Poland"]
["1814","1814XX0010","KOSTER PRO WALL-ARM 2XLED 2595LM VSM 3000K DIM.",null,"Wall lamp luminaire with a modern design Can be mounted on the corners of architectural structures",null,"Koster","Wall","Europe, Africa, Asia, Australia and Oceania, North America, South America",2,4,0.22,2.25,"",null,null,null,null,null,null,null,"1814XX0010.jpg",4,1,1,2,2,1,55,"CE","","","Class I",null,null,null,null,null,0.44,0.24,0.24,null,null,null,null,"1814XX0010.ldt",1,null,null,null,null,0,null,null,null,null,null,null,"LED",16,null,"",null,null,23,null,3000,70,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"","",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"Poland"]
["1815","1815XX0009","KOSTER PRO POLE-TOP LED 2035LM VSM 3000K ON/OFF",null,"Luminaire on a straight shoulder, intended for mounting on a lighting pole with a Ø50mm mounting shaft",null,"Koster","Post","Europe, Africa, Asia, Australia and Oceania, North America, South America",2,512,4,0,"",null,null,null,null,null,null,null,"1815XX0009.jpg",4,1,1,5,9,4,66,"CE","","","Class I",null,null,null,null,null,0,0,0,null,null,null,null,"1815XX0009.ldt",1,null,null,null,null,0,null,null,null,null,null,null,"LED",16,null,"",null,null,23,null,3000,70,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"","",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"Poland"]
["1816","1816XX0309","KOSTER PRO LIGHT LUMINAIRES POLE LED 2035LM VSM 3000K ON/OFF",null,"Luminaire with a classic design mounted on a telescopic pole with adjustable height 2360..3360mm, Pole equipped with a revision door",null,"Koster","Post,Post complete","Europe, Africa, Asia, Australia and Oceania, North America, South America",2,512,4,0,"",null,null,null,null,null,null,null,"1816XX0309.jpg",4,1,1,5,9,4,66,"CE","","","Class I",null,null,null,null,null,0,0,0,null,null,null,null,"1816XX0309.ldt",1,null,null,null,null,0,null,null,null,null,null,null,"LED",16,null,"",null,null,23,null,3000,70,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"","",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"Poland"]
["1817","1817XX0009","KOSTER PRO POLE-TOP LED 2035LM VSM 3000K ON/OFF",null,"Luminaire on a straight shoulder, intended for mounting on a lighting pole with a Ø60mm mounting shaft",null,"Koster","Post,Head","Europe, Africa, Asia, Australia and Oceania, North America, South America",2,512,4,0,"",null,null,null,null,null,null,null,"1817XX0009.jpg",4,1,1,5,9,4,66,"CE","","","Class I",null,null,null,null,null,0,0,0,null,null,null,null,"1817XX0009.ldt",1,null,null,null,null,0,null,null,null,null,null,null,"LED",16,null,"",null,null,23,null,3000,70,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"","",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"Poland"]
["1822","1822XX0009","KOSTER PRO WALL-ARM LED 2776LM VSM 3000K DALI2",null,"Wall lamp luminaire with a modern design, Can be mounted on the corners of architectural structures",null,"Koster","Wall","Europe, Africa, Asia, Australia and Oceania, North America, South America",2,4,0.22,2.25,"",null,null,null,null,null,null,null,"1822XX0009.jpg",4,1,1,2,2,3,46,"CE","","","Class I",null,null,null,null,null,0,0,0,null,null,null,null,"1822XX0009.ldt",1,null,null,null,null,0,null,null,null,null,null,null,"LED",16,null,"",null,null,23,null,3000,70,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"DALI","",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"Poland"]
["1823","1823XX0009","KOSTER PRO POLE-TOP LED 2776LM VSM 3000K DALI2",null,"Luminaire on a straight arm, intended for mounting on a pole with a Ø50mm mounting shaft",null,"Koster","Post,Head","Europe, Africa, Asia, Australia and Oceania, North America, South America",2,512,4,0,"",null,null,null,null,null,null,null,"1823XX0009.jpg",4,1,1,5,9,3,66,"CE","","","Class I",null,null,null,null,null,0,0,0,null,null,null,null,"1823XX0009.ldt",1,null,null,null,null,0,null,null,null,null,null,null,"LED",16,null,"",null,null,23,null,3000,70,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"DALI","",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"Poland"]
["1824","1824XX0309","KOSTER PRO LIGHT LUMINAIRES POLE LED 2776LM VSM 3000K DALI2",null,"Luminaire with a classic design mounted on a telescopic pole with adjustable height 2360..3360mm, Pole equipped with a revision door",null,"Koster","Post,Post complete","Europe, Africa, Asia, Australia and Oceania, North America, South America",2,512,4,0,"",null,null,null,null,null,null,null,"1824XX0309.jpg",4,1,1,5,9,3,66,"CE","","","Class I",null,null,null,null,null,0.45,0.24,0.24,null,null,null,null,"1824XX0309.ldt",1,null,null,null,null,0,null,null,null,null,null,null,"LED",16,null,"",null,null,23,null,3000,70,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"DALI","",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"Poland"]
["1825","1825XX0009","KOSTER PRO POLE-TOP LED 2776LM VSM 3000K DALI2",null,"Luminaire on a straight arm, intended for mounting on a pole with a Ø60mm mounting shaft",null,"Koster","Post,Head","Europe, Africa, Asia, Australia and Oceania, North America, South America",2,512,4,0,"",null,null,null,null,null,null,null,"1825XX0009.jpg",4,1,1,5,9,3,66,"CE","","","Class I",null,null,null,null,null,0,0,0,null,null,null,null,"1825XX0009.ldt",1,null,null,null,null,0,null,null,null,null,null,null,"LED",16,null,"",null,null,23,null,3000,70,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"DALI","",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"Poland"]
["1834","1834XX0010","KOSTER PRO WALL-ARM 2XLED 2801LM VSM 4000K DIM.",null,"Wall lamp luminaire with a modern design Can be mounted on the corners of architectural structures",null,"Koster","Wall","Europe, Africa, Asia, Australia and Oceania, North America, South America",2,4,0.22,2.25,"",null,null,null,null,null,null,null,"1834XX0010.jpg",4,1,1,2,2,1,46,"CE","","","Class I",null,null,null,null,null,0.44,0.24,0.24,null,null,null,null,"1834XX0010.ldt",1,null,null,null,null,0,null,null,null,null,null,null,"LED",16,null,"",null,null,24,null,4000,70,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"","",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"Poland"]
["1835","1835XX0009","KOSTER PRO POLE-TOP LED 2145LM VSM 4000K ON/OFF",null,"Classic design luminaire on a straight top arm. Intended for mounting on a pole with a Ø50mm mounting shaft",null,"Koster","Post","Europe, Africa, Asia, Australia and Oceania, North America, South America",2,512,4,0,"",null,null,null,null,null,null,null,"1835XX0009.jpg",4,1,1,5,9,4,66,"CE","","","Class I",null,null,null,null,null,0,0,0,null,null,null,null,"1835XX0009.ldt",1,null,null,null,null,0,null,null,null,null,null,null,"LED",16,null,"",null,null,24,null,4000,70,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"","",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"Poland"]
["1836","1836XX0309","KOSTER PRO LIGHT LUMINAIRES POLE LED 2145LM VSM 4000K ON/OFF",null,"Luminaire with a classic design mounted on a telescopic pole with adjustable height 2360..3360mm, Pole equipped with a revision door",null,"Koster","Post","Europe, Africa, Asia, Australia and Oceania, North America, South America",2,512,4,0,"",null,null,null,null,null,null,null,"1836XX0309.jpg",4,1,1,5,9,4,66,"CE","","","Class I",null,null,null,null,null,0,0,0,null,null,null,null,"1836XX0309.ldt",1,null,null,null,null,0,null,null,null,null,null,null,"LED",16,null,"",null,null,24,null,4000,70,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"","",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"Poland"]
["1837","1837XX0009","KOSTER PRO POLE-TOP LED 2145LM VSM 4000K ON/OFF",null,"Luminaire on a straight top arm, intended for mounting on a pole with a Ø60mm mounting shaft",null,"Koster","Post","Europe, Africa, Asia, Australia and Oceania, North America, South America",2,512,4,0,"",null,null,null,null,null,null,null,"1837XX0009.jpg",4,1,1,5,9,4,66,"CE","","","Class I",null,null,null,null,null,0,0,0,null,null,null,null,"1837XX0009.ldt",1,null,null,null,null,0,null,null,null,null,null,null,"LED",16,null,"",null,null,24,null,4000,70,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"","",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"Poland"]
["1842","1842XX0009","KOSTER PRO WALL-ARM LED 2927LM VSM 4000K DALI2",null,"Wall lamp luminaire with a modern design, Can be mounted on the corners of architectural structures",null,"Koster","Wall","Europe, Africa, Asia, Australia and Oceania, North America, South America",2,4,0.22,2.25,"",null,null,null,null,null,null,null,"1842XX0009.jpg",4,1,1,2,2,3,46,"CE","","","Class I",null,null,null,null,null,0,0,0,null,null,null,null,"1842XX0009.ldt",1,null,null,null,null,0,null,null,null,null,null,null,"LED",16,null,"",null,null,24,null,4000,70,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"DALI","",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"Poland"]
["1843","1843XX0009","KOSTER PRO POLE-TOP LED 2927LM VSM 4000K DALI2",null,"Luminaire on a straight arm with classic design. Mounted, intended for mounting on a lighting pole with a Ø50mm mounting base.",null,"Koster","Post","Europe, Africa, Asia, Australia and Oceania, North America, South America",2,512,4,0,"",null,null,null,null,null,null,null,"1843XX0009.jpg",4,1,1,5,9,3,66,"CE","","","Class I",null,null,null,null,null,0,0,0,null,null,null,null,"1843XX0009.ldt",1,null,null,null,null,0,null,null,null,null,null,null,"LED",16,null,"",null,null,24,null,4000,70,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"DALI","",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"Poland"]
["1844","1844XX0309","KOSTER PRO LIGHT LUMINAIRES POLE LED 2927LM VSM 4000K DALI2",null,"Luminaire with a classic design mounted on a telescopic pole with adjustable height 2360..3360mm, Pole equipped with a revision door",null,"Koster","Post","Europe, Africa, Asia, Australia and Oceania, North America, South America",2,512,4,0,"",null,null,null,null,null,null,null,"1844XX0309.jpg",4,1,1,5,9,3,66,"CE","","","Class I",null,null,null,null,null,0.45,0.24,0.24,null,null,null,null,"1844XX0309.ldt",1,null,null,null,null,0,null,null,null,null,null,null,"LED",16,null,"",null,null,24,null,4000,70,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"DALI","",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"Poland"]
["1845","1845XX0009","KOSTER PRO POLE-TOP LED 2927LM VSM 4000K DALI2",null,"Luminaire on a straight arm, intended for mounting on a pole with a Ø60mm mounting shaft",null,"Koster","Post","Europe, Africa, Asia, Australia and Oceania, North America, South America",2,512,4,0,"",null,null,null,null,null,null,null,"1845XX0009.jpg",4,1,1,5,9,3,66,"CE","","","Class I",null,null,null,null,null,0,0,0,null,null,null,null,"1845XX0009.ldt",1,null,null,null,null,0,null,null,null,null,null,null,"LED",16,null,"",null,null,24,null,4000,70,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"DALI","",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"Poland"]
["1850","1850XX0010","NARVIK II BOLLARD LED 3017LM 3000K ON/OFF",null,"A bollard luminaire with a stable and durable structure. For lighting private and public areas",null,"Narvik","Bollard","Europe, Africa, Asia, Australia and Oceania, North America, South America",2,2,0.7,0,"",null,null,null,null,null,null,null,"1850XX0010.png",4,1,1,3,6,4,66,"CE","","IK10","Class II",null,null,null,null,null,0.24,0.24,0.95,null,null,null,null,"1850XX0010.ldt",1,null,null,null,null,0,null,null,null,null,null,null,"LED",16,null,"",null,null,23,null,3000,80,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"","",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"Poland"]
["1851","1851XX0010","NARVIK II BOLLARD LED 3200LM 4000K ON/OFF",null,"A bollard luminaire with a stable and durable structure. For lighting private and public areas",null,"Narvik","Bollard","Europe, Africa, Asia, Australia and Oceania, North America, South America",2,2,0.7,0,"",null,null,null,null,null,null,null,"1851XX0010.png",4,1,1,3,6,4,66,"CE","","IK10","Class II",null,null,null,null,null,0.24,0.24,0.95,null,null,null,null,"1851XX0010.ldt",1,null,null,null,null,0,null,null,null,null,null,null,"LED",16,null,"",null,null,24,null,4000,80,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"","",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"Poland"]
["1852","1852XX0010","NARVIK II BOLLARD LED 3017LM 3000K ON/OFF",null,"A bollard luminaire with a stable and durable structure. For lighting private and public areas",null,"Narvik","Bollard","Europe, Africa, Asia, Australia and Oceania, North America, South America",2,2,0.7,0,"",null,null,null,null,null,null,null,"1852XX0010.png",4,1,1,3,6,4,66,"CE","","IK10","Class II",null,null,null,null,null,0.24,0.24,0.95,null,null,null,null,"1852XX0010.ldt",1,null,null,null,null,0,null,null,null,null,null,null,"LED",16,null,"",null,null,23,null,3000,80,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"","",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"Poland"]
["1853","1853XX0010","NARVIK II BOLLARD LED 3200LM 4000K ON/OFF",null,"A bollard luminaire with a stable and durable structure. For lighting private and public areas",null,"Narvik","Bollard","Europe, Africa, Asia, Australia and Oceania, North America, South America",2,2,0.7,0,"",null,null,null,null,null,null,null,"1853XX0010.png",4,1,1,3,6,4,66,"CE","","IK10","Class II",null,null,null,null,null,0.24,0.24,0.95,null,null,null,null,"1853XX0010.ldt",1,null,null,null,null,0,null,null,null,null,null,null,"LED",16,null,"",null,null,24,null,4000,80,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"","",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"Poland"]
["1874","1874XX0009","GENEVE WALL E27 UP-DOWN",null,"A luminaire with a wide range of applications, including lighting: wall surfaces, facades, and other architectural concepts.",null,"Geneva","Wall","Europe, Africa, Asia, Australia and Oceania, North America, South America",2,4,0,2.5,"",null,null,null,null,null,null,null,"1874XX0009.jpg",8,1,2,2,2,4,66,"CE","","IK08","Class I",null,null,null,null,null,0.31,0.21,0.95,null,null,null,null,"1874XX0009.ldt",0,null,null,null,null,1,null,null,null,null,null,null,"LED",16,null,"E27",null,null,23,null,"",80,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"","",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"Poland"]
["1879","1879XX0009","GENEVE WALL 2XLED 1128LM UP-DOWN 3000K DIM.",null,"A luminaire with a wide range of applications, including lighting: wall surfaces, facades, and other architectural concepts.",null,"Geneva","Wall","Europe, Africa, Asia, Australia and Oceania, North America, South America",2,4,0,2.5,"",null,null,null,null,null,null,null,"1879XX0009.jpg",8,1,2,2,2,1,66,"CE","","IK08","Class I",null,null,null,null,null,0.21,0.1,0.31,null,null,null,null,"1879XX0009.ldt",1,null,null,null,null,1,null,null,null,null,null,null,"LED",16,null,"",null,null,23,null,3000,80,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"","",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"Poland"]
["1880","1880XX0009","GENEVE WALL 2XLED 1196LM UP-DOWN 4000K DIM.",null,"A luminaire with a wide range of applications, including lighting: wall surfaces, facades, and other architectural concepts.",null,"Geneva","Wall","Europe, Africa, Asia, Australia and Oceania, North America, South America",2,4,0,2.5,"",null,null,null,null,null,null,null,"1880XX0009.jpg",8,1,2,2,2,1,66,"CE","","IK08","Class I",null,null,null,null,null,0,0,0,null,null,null,null,"1880XX0009.ldt",1,null,null,null,null,1,null,null,null,null,null,null,"LED",16,null,"",null,null,24,null,4000,80,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"","",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"Poland"]
["1901","1901XX0013","MOLDE BOLLARD 80CM LED 743LM 3000K DIM.",null,"Luminaire with contemporary design. For lighting private areas, parks, and other concepts architectural",null,"Molde","Bollard","Europe, Africa, Asia, Australia and Oceania, North America, South America",2,2,0.75,0,"",null,null,null,null,null,null,null,"1901XX0013.jpg",7,1,2,3,6,1,55,"CE","","IK07","Class I",null,null,null,null,null,0.8,0.16,0.11,null,null,null,null,"1901XX0013.ldt",1,null,null,null,null,0,null,null,null,null,null,null,"LED",16,null,"",null,null,23,null,3000,80,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"","",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"Poland"]
["1903","1903XX0009","MOLDE BOLLARD 50CM LED 743LM 3000K DIM.",null,"Luminaire with contemporary design. For lighting private areas, parks and other concepts architectural",null,"Molde","Bollard","Europe, Africa, Asia, Australia and Oceania, North America, South America",2,2,0.45,0,"",null,null,null,null,null,null,null,"1903XX0009.jpg",7,1,2,3,6,1,55,"CE","","","Class I",null,null,null,null,null,0.5,0.16,0.11,null,null,null,null,"1903XX0009.ldt",1,null,null,null,null,0,null,null,null,null,null,null,"LED",16,null,"",null,null,23,null,3000,80,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"","",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"Poland"]
["1904","1904XX0009","MOLDE BOLLARD 50CM LED 772LM 4000K DIM.",null,"Luminaire with contemporary design. For lighting private areas, parks and other concepts architectural",null,"Molde","Bollard","Europe, Africa, Asia, Australia and Oceania, North America, South America",2,2,0.45,0,"",null,null,null,null,null,null,null,"1904XX0009.jpg",7,1,2,3,6,1,55,"CE","","","Class I",null,null,null,null,null,0.5,0.16,0.11,null,null,null,null,"1904XX0009.ldt",1,null,null,null,null,0,null,null,null,null,null,null,"LED",16,null,"",null,null,24,null,4000,80,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"","",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"Poland"]
["1912","1912XX0012","KOSTER WALL-ARM LED 1950LM 3000K ON/OFF",null,"Classic type wall-mounted luminaire. Possibility to install on corners of architectural objects.",null,"Koster","Wall","Europe, Africa, Asia, Australia and Oceania, North America, South America",2,4,0.22,2.5,"",null,null,null,null,null,null,null,"1912XX0012.jpg",3,1,1,2,2,4,55,"CE","","IK10","Class I",null,null,null,null,null,0,0,0,null,null,null,null,"1912XX0012.ldt",1,null,null,null,null,0,null,null,null,null,null,null,"LED",16,null,"",null,null,23,null,3000,80,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"","",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"Poland"]
["1913","1913XX0011","KOSTER POLE-TOP LED 1950LM 3000K",null,"Classic design luminaire for mounting on a telescopic lighting pole with cap diameter Ø60mm.",null,"Koster","Post,Head","Europe, Africa, Asia, Australia and Oceania, North America, South America",2,512,4,0,"",null,null,null,null,null,null,null,"1913XX0011.jpg",3,1,1,5,9,4,55,"CE","","IK10","Class I",null,null,null,null,null,0,0,0,null,null,null,null,"1913XX0011.ldt",1,null,null,null,null,0,null,null,null,null,null,null,"LED",16,null,"",null,null,23,null,3000,80,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"","",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"Poland"]
["1914","1914XX0309","KOSTER POLE-TOP LED 1950LM 3000K",null,"Classic design luminaire, mounted on a telescopic lighting pole. Adjustable height 2360..3360mm.",null,"Koster","Post,Post complete","Europe, Africa, Asia, Australia and Oceania, North America, South America",2,512,4,0,"",null,null,null,null,null,null,null,"1914XX0309.jpg",3,1,1,5,9,4,55,"CE","","IK10","Class I",null,null,null,null,null,0,0,0,null,null,null,null,"1914XX0309.ldt",1,null,null,null,null,0,null,null,null,null,null,null,"LED",16,null,"",null,null,23,null,3000,80,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"","",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"Poland"]
["1915","1915XX0011","KOSTER POLE-TOP LED 1950LM 3000K",null,"Classic design luminaire for mounting on a telescopic lighting pole with cap diameter Ø50mm.",null,"Koster","Post,Head","Europe, Africa, Asia, Australia and Oceania, North America, South America",2,512,4,0,"",null,null,null,null,null,null,null,"1915XX0011.jpg",3,1,1,5,9,4,55,"CE","","IK10","Class I",null,null,null,null,null,0,0,0,null,null,null,null,"1915XX0011.ldt",1,null,null,null,null,0,null,null,null,null,null,null,"LED",16,null,"",null,null,23,null,3000,80,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"","",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"Poland"]
["1920","1920XX0010","VANSBRO WALL E27",null,"Scandinavian design wall-mounted luminaire. Possibility to install on corners of architectural objects.",null,"Vansbro","Wall","Europe, Africa, Asia, Australia and Oceania, North America, South America",2,4,0.3,2.5,"",null,null,null,null,null,null,null,"1920XX0010.jpg",7,1,1,2,2,4,56,"CE","","","Class II",null,null,null,null,null,0,0,0,null,null,null,null,"1920XX0010.ldt",0,null,null,null,null,0,null,null,null,null,null,null,"LED",16,null,"E27",null,null,23,null,"",80,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"","",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"Poland"]
["1921","1921XX0009","NAMSOS BOLLARD 95CM LED 1891LM 3000K DIM.",null,"Luminaire with a modern design. For lighting gardens and other private and public areas",null,"Namsos","Bollard","Europe, Africa, Asia, Australia and Oceania, North America, South America",2,2,0.71,0,"",null,null,null,null,null,null,null,"1921XX0009.jpg",7,1,2,3,6,1,66,"CE","","IK08","Class I",null,null,null,null,null,0.24,0.12,0.95,null,null,null,null,"1921XX0009.ldt",1,null,null,null,null,1,null,null,null,null,null,null,"LED",16,null,"",null,null,23,null,3000,80,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"","",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"Poland"]
["1922","1922XX0009","NAMSOS BOLLARD 95CM LED 2006LM 4000K DIM.",null,"Luminaire with a modern design. For lighting gardens and other private and public areas",null,"Namsos","Bollard","Europe, Africa, Asia, Australia and Oceania, North America, South America",2,2,0.71,0,"",null,null,null,null,null,null,null,"1922XX0009.jpg",7,1,2,3,6,1,66,"CE","","IK08","Class I",null,null,null,null,null,0.24,0.12,0.95,null,null,null,null,"1922XX0009.ldt",1,null,null,null,null,1,null,null,null,null,null,null,"LED",16,null,"",null,null,24,null,4000,80,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"","",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"Poland"]
["1923","1923XX0009","NAMSOS BOLLARD 65CM LED 1891LM 3000K DIM.",null,"Luminaire with a modern design. For lighting gardens and other private and public areas",null,"Namsos","Bollard","Europe, Africa, Asia, Australia and Oceania, North America, South America",2,2,0.41,0,"",null,null,null,null,null,null,null,"1923XX0009.jpg",7,1,2,3,6,1,66,"CE","","IK08","Class I",null,null,null,null,null,0.24,0.12,0.65,null,null,null,null,"1923XX0009.ldt",1,null,null,null,null,1,null,null,null,null,null,null,"LED",16,null,"",null,null,23,null,3000,80,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"","",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"Poland"]
["1924","1924XX0009","NAMSOS BOLLARD 65CM LED 2006LM 4000K DIM.",null,"Luminaire with a modern design. For lighting gardens and other private and public areas",null,"Namsos","Bollard","Europe, Africa, Asia, Australia and Oceania, North America, South America",2,2,0.41,0,"",null,null,null,null,null,null,null,"1924XX0009.jpg",7,1,2,3,6,1,66,"CE","","IK08","Class I",null,null,null,null,null,0.24,0.12,0.65,null,null,null,null,"1924XX0009.ldt",1,null,null,null,null,1,null,null,null,null,null,null,"LED",16,null,"",null,null,24,null,4000,80,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"","",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"Poland"]
["1929","1929XX0010","NAMSOS WALL-RECESSED LED 1891LM 3000K DIM. TRIAC",null,"The luminaire is adapted to illuminate stairs, steps, staircases, pathways, ceiling illumination and the implementation of other architectural concepts",null,"Namsos","Bollard","Europe, Africa, Asia, Australia and Oceania, North America, South America",2,64,0,0.5,"",null,null,null,null,null,null,null,"1929XX0010.jpg",7,1,2,2,1,1,66,"CE","","IK08","Class I",null,null,null,null,null,0.22,0.22,0.12,null,null,null,null,"1929XX0010.ldt",1,null,null,null,null,4,null,null,null,null,null,null,"LED",16,null,"",null,null,23,null,3000,80,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"","",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"Poland"]
["1930","1930XX0016","NAMSOS WALL-RECESSED LED 1176LM 3000K DIM.",null,"The luminaire is adapted to illuminate stairs, steps, staircases, pathways, ceiling lighting and implementation of other architectural concepts",null,"Namsos","Recessed","Europe, Africa, Asia, Australia and Oceania, North America, South America",2,64,0,0.5,"",null,null,null,null,null,null,null,"1930XX0016.jpg",7,1,2,2,1,1,66,"CE","","IK08","Class I",null,null,null,null,null,0.22,0.22,0.12,null,null,null,null,"1930XX0016.ldt",1,null,null,null,null,4,null,null,null,null,null,null,"LED",16,null,"",null,null,23,null,3000,80,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"","",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"Poland"]
["1931","1931XX0015","NAMSOS BOLLARD 95CM LED 1176LM 3000K DIM.",null,"Luminaire with a modern design. For lighting gardens and other private and public areas",null,"Namsos","Bollard","Europe, Africa, Asia, Australia and Oceania, North America, South America",2,2,0.71,0,"",null,null,null,null,null,null,null,"1931XX0015.jpg",7,1,2,3,6,1,66,"CE","","IK08","Class I",null,null,null,null,null,0.24,0.12,0.95,null,null,null,null,"1931XX0015.ldt",1,null,null,null,null,1,null,null,null,null,null,null,"LED",16,null,"",null,null,23,null,3000,80,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"","",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"Poland"]
["1932","1932XX0014","NAMSOS BOLLARD 65CM LED 1176LM 3000K DIM.",null,"Luminaire with a modern design. For lighting gardens and other private and public areas",null,"Namsos","Bollard","Europe, Africa, Asia, Australia and Oceania, North America, South America",2,2,0.41,0,"",null,null,null,null,null,null,null,"1932XX0014.jpg",7,1,2,3,6,1,66,"CE","","IK08","Class I",null,null,null,null,null,0.24,0.12,0.65,null,null,null,null,"1932XX0014.ldt",1,null,null,null,null,1,null,null,null,null,null,null,"LED",16,null,"",null,null,23,null,3000,80,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"","",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"Poland"]
["1933","1933XX0011","NAMSOS WALL-RECESSED LED 653LM 3000K DIM.",null,"The luminaire is adapted to illuminate stairs, steps, staircases, communication pathways and other applications",null,"Namsos,Galvanized","Recessed","Europe, Africa, Asia, Australia and Oceania, North America, South America",2,64,0,0.5,"",null,null,null,null,null,null,null,"1933XX0011.jpg",7,1,2,2,1,1,45,"CE","","IK10","Class I",null,null,null,null,null,0,0,0,null,null,null,null,"1933XX0011.ldt",1,null,null,null,null,4,null,null,null,null,null,null,"LED",16,null,"",null,null,23,null,3000,80,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"","",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"Poland"]
["1954","1954XX0D09","VOSS WALL LED 629LM DOWN 4º 3000K ON/OFF",null,"A luminaire with a wide range of applications, including lighting: wall and facade surfaces as well as other architectural concepts",null,"Voss","Wall","Europe, Africa, Asia, Australia and Oceania, North America, South America",2,4,0,2.5,"",null,null,null,null,null,null,null,"1954XX0D09.jpg",10,1,2,2,2,4,55,"CE","","IK06","Class I",null,null,null,null,null,0.18,0.16,0.27,null,null,null,null,"1954XX0D09.ldt",1,null,null,null,null,2,null,null,null,null,null,null,"LED",16,null,"",null,null,23,null,3000,80,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"","",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"Poland"]
["1955","1955XX0H10",{"$f":"INDEX(DB,MATCH($A315,ID,0),3)","v":"VOSS WALL 2XLED 1444LM UP62º 3000K DIM."},null,"A luminaire with a wide range of applications, for lighting: wall and facade surfaces and other architectural concepts",null,"Voss",{"$f":"IF(INDEX(DB,MATCH($A315,ID,0),5)=0,\"\",INDEX(DB,MATCH($A315,ID,0),5))","v":"Wall"},"Europe, Africa, Asia, Australia and Oceania, North America, South America",2,{"$f":"IFERROR(INDEX(TYPMONT,MATCH((INDEX(DB,MATCH($A315,ID,0),31)),ID_RODZ,0),3),\"\")","v":4},0,2.5,{"$f":"IFERROR(IF(INDEX(TYPMONT,MATCH((INDEX(DB,MATCH($A315,ID,0),31)),ID_RODZ,0),6)=0,\"\",INDEX(TYPMONT,MATCH((INDEX(DB,MATCH($A315,ID,0),31)),ID_RODZ,0),6)),\"\")","v":""},null,null,null,null,null,null,null,{"$f":"IF(INDEX(DB,MATCH($A315,ID,0),57)=0,\"\",INDEX(DB,MATCH($A315,ID,0),57))","v":"1955XX0H10.jpg"},10,{"$f":"IF(INDEX(DB,MATCH($A315,ID,0),61)=0,\"\",INDEX(DB,MATCH($A315,ID,0),61))","v":1},2,{"$f":"IFERROR(INDEX(TYPMONT,MATCH((INDEX(DB,MATCH($A315,ID,0),31)),ID_RODZ,0),1),\"\")","v":2},{"$f":"IFERROR(INDEX(TYPMONT,MATCH((INDEX(DB,MATCH($A315,ID,0),31)),ID_RODZ,0),2),\"\")","v":2},{"$f":"IF(INDEX(DB,MATCH($A315,ID,0),59)=0,\"\",INDEX(DB,MATCH($A315,ID,0),59))","v":1},{"$f":"IFERROR(IF(INDEX(DB,MATCH($A315,ID,0),19)=0,\"\",INDEX(DB,MATCH($A315,ID,0),19)+1),\"\")","v":55},{"$f":"IF(INDEX(DB,MATCH($A315,ID,0),27)=0,\"\",INDEX(DB,MATCH($A315,ID,0),27))","v":"CE"},"",{"$f":"IF(INDEX(DB,MATCH($A315,ID,0),20)=0,\"\",INDEX(DB,MATCH($A315,ID,0),20))","v":""},{"$f":"IF(INDEX(DB,MATCH($A315,ID,0),21)=0,\"\",INDEX(DB,MATCH($A315,ID,0),21))","v":"Class I"},null,null,null,null,null,0.18,0.16,0.27,null,null,null,null,{"$f":"IF(INDEX(DB,MATCH($A315,ID,0),58)=0,\"\",INDEX(DB,MATCH($A315,ID,0),58))","v":"1955XX0H10.ldt"},1,null,null,null,null,2,null,null,null,null,null,null,"LED",16,null,{"$f":"IF(INDEX(DB,MATCH($A315,ID,0),60)=0,\"\",INDEX(DB,MATCH($A315,ID,0),60))","v":""},null,null,23,null,{"$f":"IF(INDEX(DB,MATCH($A315,ID,0),22)=0,\"\",INDEX(DB,MATCH($A315,ID,0),22))","v":3000},{"$f":"IF(INDEX(DB,MATCH($A315,ID,0),53)=0,\"\",INDEX(DB,MATCH($A315,ID,0),53))","v":80},null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,{"$f":"IF(INDEX(DB,MATCH($A315,ID,0),29)=0,\"\",INDEX(DB,MATCH($A315,ID,0),29))","v":""},{"$f":"IF(INDEX(DB,MATCH($A315,ID,0),28)=0,\"\",INDEX(DB,MATCH($A315,ID,0),28))","v":""},null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"Poland"]
["1960","1960XX0009","LOFOTEN WALL E27",null,"A luminaire with a classic and simple design for general use, Perfect for lighting terraces, entrances, gazebos, and other architectural concepts",null,{"$f":"IF(INDEX(DB,MATCH($A316,ID,0),4)=0,\"\",INDEX(DB,MATCH($A316,ID,0),4))","v":"Lofoten"},"Wall","Europe, Africa, Asia, Australia and Oceania, North America, South America",2,4,0,2.5,"",null,null,null,null,null,null,null,"1960XX0009.jpg",9,1,2,2,2,4,45,"CE",{"$f":"IFERROR(IF(FIND(\"RENA\",$C316)>0,\"Vehicle resistant\",\"\"),\"\")","v":""},"","Class II",null,null,null,null,null,0,0,0,null,null,null,null,"1960XX0009.ldt",0,null,null,null,null,3,null,null,null,null,null,null,"LED",16,null,"E27",null,null,{"$f":"IF($BO316=4000,24,23)","v":23},null,"",80,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"","",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"Poland"]
["1963","1963XX0009","LOFOTEN UP WALL-ARM E27",null,"Luminaire with a classic and simple design for general use. Perfect for lighting terraces, entrances, gazebos and other architectural concepts. Possibility to mount the luminaire as a wall lamp directed upwards Possibility of mounting the luminaire on the corners",null,"Lofoten","Wall","Europe, Africa, Asia, Australia and Oceania, North America, South America",2,4,0.2,2.5,"",null,null,null,null,null,null,null,"1963XX0009.png",9,1,2,2,2,4,45,"CE","","","Class II",null,null,null,null,null,0,0,0,null,null,null,null,"1963XX0009.ldt",0,null,null,null,null,3,null,null,null,null,null,null,"LED",16,null,"E27",null,null,23,null,"",80,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"","",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"Poland"]
["1970","1970XX0009","MOLDE BOLLARD 80CM LED 743LM 3000K ON/OFF MD",null,"Luminaire with a contemporary design For lighting private areas, parks and other architectural concepts",null,"Molde","Bollard","Europe, Africa, Asia, Australia and Oceania, North America, South America",2,2,0.75,0,"",null,null,null,null,null,null,null,"1970XX0009.jpg",7,1,2,3,6,3,55,"CE","","","Class I",null,null,null,null,null,0.8,0.16,0.11,null,null,null,null,"1970XX0009.ldt",1,null,null,null,null,0,null,null,null,null,null,null,"LED",16,null,"",null,null,23,null,3000,80,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"","Daylight sensor,Motion sensor",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"Poland"]
["1971","1971XX0009","MOLDE BOLLARD 50CM LED 743LM 3000K ON/OFF MD",null,"Luminaire with a contemporary design For lighting private areas, parks and other architectural concepts",null,"Molde","Bollard","Europe, Africa, Asia, Australia and Oceania, North America, South America",2,2,0.45,0,"",null,null,null,null,null,null,null,"1971XX0009.jpg",7,1,2,3,6,3,55,"CE","","","Class I",null,null,null,null,null,0.16,0.11,0.5,null,null,null,null,"1971XX0009.ldt",1,null,null,null,null,0,null,null,null,null,null,null,"LED",16,null,"",null,null,23,null,3000,80,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"","Daylight sensor,Motion sensor",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"Poland"]
["1972","1972XX0009","MOLDE BOLLARD 80CM LED 772LM 4000K ON/OFF MD",null,"Luminaire with a contemporary design For lighting private areas, parks and other architectural concepts",null,"Molde","Bollard","Europe, Africa, Asia, Australia and Oceania, North America, South America",2,2,0.75,0,"",null,null,null,null,null,null,null,"1972XX0009.jpg",7,1,2,3,6,3,55,"CE","","","Class I",null,null,null,null,null,0.8,0.16,0.11,null,null,null,null,"1972XX0009.ldt",1,null,null,null,null,0,null,null,null,null,null,null,"LED",16,null,"",null,null,24,null,4000,80,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"","Daylight sensor,Motion sensor",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"Poland"]
["1973","1973XX0009","MOLDE BOLLARD 50CM LED 772LM 4000K ON/OFF MD",null,"Luminaire with a contemporary design For lighting private areas, parks and other architectural concepts",null,"Molde","Bollard","Europe, Africa, Asia, Australia and Oceania, North America, South America",2,2,0.45,0,"",null,null,null,null,null,null,null,"1973XX0009.jpg",7,1,2,3,6,3,55,"CE","","","Class I",null,null,null,null,null,0.16,0.11,0.5,null,null,null,null,"1973XX0009.ldt",1,null,null,null,null,0,null,null,null,null,null,null,"LED",16,null,"",null,null,24,null,4000,80,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"","Daylight sensor,Motion sensor",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"Poland"]
["2018","2018XX0010","STOCKHOLM POLE-TOP E27",null,"Luminaire with Scandinavian design, mounted on a telescopic lighting pole with a diameter of ø50 mm. For lighting gardens, parks and other architectural concepts.",null,"Stockholm","Pole","Europe, Africa, Asia, Australia and Oceania, North America, South America",2,512,4,0,"",null,null,null,null,null,null,null,"2018XX0010.jpg",7,1,1,5,9,4,55,"CE","","","Class II",null,null,null,null,null,0.92,0.35,0.45,null,null,null,null,"2018XX0010.ldt",0,null,null,null,null,1,null,null,null,null,null,null,"LED",16,null,"E27",null,null,23,null,"",80,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"","",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"Poland"]
["2026","2026XX0009","MOLDE WALL LED 743LM 3000K DIM.",null,"A luminaire with a contemporary design. For lighting private areas, parks and other concepts architectural",null,"Molde","Wall","Europe, Africa, Asia, Australia and Oceania, North America, South America",2,4,0,2.5,"",null,null,null,null,null,null,null,"2026XX0009.png",7,1,2,2,2,1,55,"CE","","IK07","Class I",null,null,null,null,null,0.3,0.23,0.11,null,null,null,null,"2026XX0009.ldt",1,null,null,null,null,0,null,null,null,null,null,null,"LED",16,null,"",null,null,23,null,3000,80,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"","",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"Poland"]
["2027","2027XX0009","MOLDE WALL LED 772LM 4000K DIM.",null,"A luminaire with a contemporary design. For lighting private areas, parks and other concepts architectural",null,"Molde","Wall","Europe, Africa, Asia, Australia and Oceania, North America, South America",2,4,0,2.5,"",null,null,null,null,null,null,null,"2027XX0009.png",7,1,2,2,2,1,55,"CE","","IK07","Class I",null,null,null,null,null,0.23,0.11,0.3,null,null,null,null,"2027XX0009.ldt",1,null,null,null,null,0,null,null,null,null,null,null,"LED",16,null,"",null,null,24,null,4000,80,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"","",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"Poland"]
["2028","2028XX0009","MOLDE WALL LED 743LM 3000K ON/OFF MD",null,"A luminaire with a contemporary design. For lighting private areas, parks and other concepts architectural",null,"Molde","Wall","Europe, Africa, Asia, Australia and Oceania, North America, South America",2,4,0,2.5,"",null,null,null,null,null,null,null,"2028XX0009.png",7,1,2,2,2,3,55,"CE","","IK07","Class I",null,null,null,null,null,0.3,0.23,0.11,null,null,null,null,"2028XX0009.ldt",1,null,null,null,null,0,null,null,null,null,null,null,"LED",16,null,"",null,null,23,null,3000,80,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"","Daylight sensor,Motion sensor",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"Poland"]
["2029","2029XX0009","MOLDE WALL LED 772LM 4000K ON/OFF MD",null,"A luminaire with a contemporary design. For lighting private areas, parks and other concepts architectural",null,"Molde","Wall","Europe, Africa, Asia, Australia and Oceania, North America, South America",2,4,0,2.5,"",null,null,null,null,null,null,null,"2029XX0009.png",7,1,2,2,2,3,55,"CE","","IK07","Class I",null,null,null,null,null,0.23,0.11,0.3,null,null,null,null,"2029XX0009.ldt",1,null,null,null,null,0,null,null,null,null,null,null,"LED",16,null,"",null,null,24,null,4000,80,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"","Daylight sensor,Motion sensor",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"Poland"]
["210",{"$f":"INDEX(DB,MATCH($A327,ID,0),2)","v":"210XX0010"},"HALMSTAD BOLLARD 26CM E27",null,{"$f":"IF(INDEX(DB,MATCH($A327,ID,0),35)=0,\"\",INDEX(DB,MATCH($A327,ID,0),35))","v":"Bollard luminaire of stable and durable construction For lighting private areas and public spaces"},null,"Halmstad","Bollard","Europe, Africa, Asia, Australia and Oceania, North America, South America",2,2,0.13,0,"",null,null,null,null,null,null,null,"210XX0010.jpg",{"$f":"IF((IFERROR(INDEX(BRYLA_FOTO,MATCH(INDEX(DB,MATCH($A327,ID,0),62),ID_BRYLAFOTO,0),6),\"\"))<>0,IFERROR(INDEX(BRYLA_FOTO,MATCH(INDEX(DB,MATCH($A327,ID,0),62),ID_BRYLAFOTO,0),6),\"\"),\"\")","v":7},1,2,3,6,4,66,"CE","","IK10","Class II",null,null,null,null,null,{"$f":"INDEX(DB,MATCH($A327,ID,0),24)","v":0.26},{"$f":"INDEX(DB,MATCH($A327,ID,0),25)","v":0.12},{"$f":"INDEX(DB,MATCH($A327,ID,0),26)","v":0.12},null,null,null,null,"210XX0010.ldt",0,null,null,null,null,1,null,null,null,null,null,null,"LED",16,null,"E27",null,null,23,null,"",80,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"","",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"Poland"]
["211","211XX0011","HALMSTAD BOLLARD 26CM LED 1098LM 3000K DIM. TRIAC",null,"Bollard luminaire of stable and durable construction. For lighting private areas and public spaces.",null,"Halmstad","Bollard","Europe, Africa, Asia, Australia and Oceania, North America, South America",2,2,0.13,0,"",null,null,null,null,null,null,null,"211XX0011.jpg",7,1,2,3,6,1,66,"CE","","IK10","Class I",null,null,null,null,null,0,0,0,null,null,null,null,"211XX0011.ldt",{"$f":"IF($BJ328=\"\",1,0)","v":1},null,null,null,null,1,null,null,null,null,null,null,"LED",16,null,"",null,null,23,null,3000,80,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"","",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"Poland"]
["2120","2120XX0010","NIDAROS CEILING 9CM LED 1051LM DOWN 24º 3000K DIM.",null,"A luminaire with a wide range of applications mounted on horizontal surfaces, including lighting: wall and facade surfaces, and other architectural concepts",null,"Nidaros","Ceiling","Europe, Africa, Asia, Australia and Oceania, North America, South America",2,1,2.8,0,"",null,null,null,null,null,null,null,"2120XX0010.png",2,1,1,1,2,1,66,"CE","","","Class I",null,null,null,null,null,0.09,0.12,0.12,null,null,null,null,"2120XX0010.ldt",1,null,null,null,null,0,null,null,null,null,null,null,"LED",16,null,"",null,null,23,null,3000,80,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"","",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"Poland"]
["2121","2121XX0010","NIDAROS CEILING 18CM LED 1051LM DOWN 24º 3000K DIM.",null,"A luminaire with a wide range of applications mounted on horizontal surfaces, including lighting: walls, facade surfaces and other architectural concepts.",null,"Nidaros","Ceiling","Europe, Africa, Asia, Australia and Oceania, North America, South America",2,1,2.8,0,"",null,null,null,null,null,null,null,"2121XX0010.png",2,1,1,1,2,1,66,"CE","","","Class I",null,null,null,null,null,0.18,0.12,0.12,null,null,null,null,"2121XX0010.ldt",1,null,null,null,null,0,null,null,null,null,null,null,"LED",16,null,"",null,null,23,null,3000,80,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"","",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"Poland"]
["2122","2122XX0010","NIDAROS CEILING 23CM LED 1051LM DOWN 24º 3000K DIM.",null,"A luminaire with a wide range of applications can be mounted on horizontal surfaces, including wall, facade surfaces, and other architectural concepts",null,"Nidaros","Ceiling","Europe, Africa, Asia, Australia and Oceania, North America, South America",2,1,2.8,0,"",null,null,null,null,null,null,null,"2122XX0010.png",2,1,1,1,2,1,66,"CE","","","Class I",null,null,null,null,null,0.23,0.12,0.12,null,null,null,null,"2122XX0010.ldt",1,null,null,null,null,0,null,null,null,null,null,null,"LED",16,null,"",null,null,23,null,3000,80,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"","",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"Poland"]
["2123","2123XX0010","NIDAROS CEILING 9CM LED 1051LM DOWN 24º 4000K DIM.",null,"A luminaire with a wide range of applications mounted on horizontal surfaces, including lighting: walls, facade surfaces and other architectural concepts.",null,"Nidaros","Ceiling","Europe, Africa, Asia, Australia and Oceania, North America, South America",2,1,2.8,0,"",null,null,null,null,null,null,null,"2123XX0010.png",2,1,1,1,2,1,66,"CE","","","Class I",null,null,null,null,null,0.09,0.12,0.12,null,null,null,null,"2123XX0010.ldt",1,null,null,null,null,0,null,null,null,null,null,null,"LED",16,null,"",null,null,24,null,4000,80,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"","",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"Poland"]
["2124","2124XX0010","NIDAROS CEILING 18CM LED 1051LM DOWN 24º 4000K DIM.",null,"A luminaire with a wide range of applications mounted on horizontal surfaces, including lighting: walls, facade surfaces and other architectural concepts.",null,"Nidaros","Ceiling","Europe, Africa, Asia, Australia and Oceania, North America, South America",2,1,2.8,0,"",null,null,null,null,null,null,null,"2124XX0010.png",2,1,1,1,2,1,66,"CE","","","Class I",null,null,null,null,null,0.18,0.12,0.12,null,null,null,null,"2124XX0010.ldt",1,null,null,null,null,0,null,null,null,null,null,null,"LED",16,null,"",null,null,24,null,4000,80,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"","",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"Poland"]
["2125","2125XX0010","NIDAROS CEILING 23CM LED 1051LM DOWN 24º 4000K DIM.",null,"A luminaire with a wide range of applications mounted on horizontal surfaces, including lighting: walls, facade surfaces and other architectural concepts.",null,"Nidaros","Ceiling","Europe, Africa, Asia, Australia and Oceania, North America, South America",2,1,2.8,{"$f":"IF(K334=4,2.5,IF(K334=64,0.5,0))","v":0},"",null,null,null,null,null,null,null,"2125XX0010.png",2,1,1,1,2,1,66,"CE","","","Class I",null,null,null,null,null,0.23,0.12,0.12,null,null,null,null,"2125XX0010.ldt",1,null,null,null,null,0,null,null,null,null,null,null,"LED",16,null,"",null,null,24,null,4000,80,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"","",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"Poland"]
["212","212XX0010","HALMSTAD BOLLARD 26CM E27 806LM 2700K DIM.",null,"Bollard luminaire of stable and durable construction. For lighting private areas and public spaces.",null,"Halmstad","Bollard","Europe, Africa, Asia, Australia and Oceania, North America, South America",2,2,0.13,0,"",null,null,null,null,null,null,null,"212XX0010.jpg",7,1,2,3,6,1,66,"CE","","IK10","Class II",null,null,null,null,null,0,0,0,null,null,null,null,"212XX0010.ldt",0,null,null,null,null,1,null,null,null,null,null,null,"LED",16,null,"E27",null,null,23,null,2700,80,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"","",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"Poland"]
["2240","2240XX0009","STAVANGER BOLLARD 95CM LED 1940LM 3000K DIM.",null,"Luminaire with a modern design For lighting gardens and other private land and public areas",null,"Stavanger","Bollard","Europe, Africa, Asia, Australia and Oceania, North America, South America",2,2,0.9,0,"",null,null,null,null,null,null,null,"2240XX0009.jpg",8,1,1,3,6,1,66,"CE","","IK08","Class II",null,null,null,null,null,0.2,0.2,0.95,null,null,null,null,"2240XX0009.ldt",1,null,null,null,null,0,null,null,null,null,null,null,"LED",16,null,"",null,null,23,null,3000,80,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"","",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"Poland"]
["2241","2241XX0009","STAVANGER BOLLARD 95CM LED 2058LM 4000K DIM.",null,"Luminaire with a modern design For lighting gardens and other private land and public areas",null,"Stavanger","Bollard","Europe, Africa, Asia, Australia and Oceania, North America, South America",2,2,0.9,0,"",null,null,null,null,null,null,null,"2241XX0009.jpg",8,1,1,3,6,1,66,"CE","","IK08","Class II",null,null,null,null,null,0.2,0.2,0.95,null,null,null,null,"2241XX0009.ldt",1,null,null,null,null,0,null,null,null,null,null,null,"LED",16,null,"",null,null,24,null,4000,80,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"","",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"Poland"]
["2244","2244XX0009","STAVANGER BOLLARD 50CM LED 1940LM 3000K DIM.",null,"A bollard luminaire with a stable and durable structure For lighting gardens, private areas and other architectural applications",null,"Stavanger","Bollard","Europe, Africa, Asia, Australia and Oceania, North America, South America",2,2,0.45,0,"",null,null,null,null,null,null,null,"2244XX0009.jpg",8,1,1,3,6,1,66,"CE","","IK08","Class II",null,null,null,null,null,0.2,0.2,0.5,null,null,null,null,"2244XX0009.ldt",1,null,null,null,null,0,null,null,null,null,null,null,"LED",16,null,"",null,null,23,null,3000,80,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"","",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"Poland"]
["2245","2245XX0009","STAVANGER BOLLARD 50CM LED 2058LM 4000K DIM.",null,"A bollard luminaire with a stable and durable structure For lighting gardens, private areas and other architectural applications",null,"Stavanger","Bollard","Europe, Africa, Asia, Australia and Oceania, North America, South America",2,2,0.45,0,"",null,null,null,null,null,null,null,"2245XX0009.jpg",8,1,1,3,6,1,66,"CE","","IK08","Class II",null,null,null,null,null,0.2,0.2,0.5,null,null,null,null,"2245XX0009.ldt",1,null,null,null,null,0,null,null,null,null,null,null,"LED",16,null,"",null,null,24,null,4000,80,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"","",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"Poland"]
["2248","2248XX0009","STAVANGER BOLLARD 28CM LED 1386LM 3000K DIM.",null,"A bollard luminaire with a stable and durable structure. For lighting gardens, private areas and other architectural applications",null,"Stavanger","Bollard","Europe, Africa, Asia, Australia and Oceania, North America, South America",2,2,0.23,0,"",null,null,null,null,null,null,null,"2248XX0009.jpg",8,1,1,3,6,1,66,"CE","","IK08","Class II",null,null,null,null,null,0.2,0.2,0.28000000000000003,null,null,null,null,"2248XX0009.ldt",1,null,null,null,null,0,null,null,null,null,null,null,"LED",16,null,"",null,null,23,null,3000,80,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"","",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"Poland"]
["2249","2249XX0009","STAVANGER BOLLARD 28CM LED 1470LM 4000K DIM.",null,"A bollard luminaire with a stable and durable structure For lighting gardens, private areas and other architectural applications",null,"Stavanger","Bollard","Europe, Africa, Asia, Australia and Oceania, North America, South America",2,2,0.23,0,"",null,null,null,null,null,null,null,"2249XX0009.jpg",8,1,1,3,6,1,66,"CE","","IK08","Class II",null,null,null,null,null,0.2,0.2,0.28000000000000003,null,null,null,null,"2249XX0009.ldt",1,null,null,null,null,0,null,null,null,null,null,null,"LED",16,null,"",null,null,24,null,4000,80,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"","",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"Poland"]
["2304","2304XX0009","EGERSUND WOOD BOLLARD 85CM LED 1370LM 3000K DIM.",null,"Luminaire with contemporary design. For lighting gardens, private areas, and other architectural applications",null,"Egersund Mini,Wood","Bollard","Europe, Africa, Asia, Australia and Oceania, North America, South America",2,2,0.69,0,"",null,null,null,null,null,null,null,"2304XX0009.png",3,1,1,3,6,1,66,"CE","","","Class II",null,null,null,null,null,0.12,0.12,0.85,null,null,null,null,"2304XX0009.ldt",1,null,null,null,null,1,null,null,null,null,null,null,"LED",16,null,"",null,null,23,null,3000,80,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"","",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"Poland"]
["2305","2305XX0009","EGERSUND WOOD BOLLARD 85CM LED 1462LM 4000K DIM.",null,"Luminaire with contemporary design. For lighting gardens, private areas, and other architectural applications",null,"Egersund Mini,Wood","Bollard","Europe, Africa, Asia, Australia and Oceania, North America, South America",2,2,0.69,0,"",null,null,null,null,null,null,null,"2305XX0009.png",3,1,1,3,6,1,66,"CE","","","Class II",null,null,null,null,null,0.12,0.12,0.85,null,null,null,null,"2305XX0009.ldt",1,null,null,null,null,1,null,null,null,null,null,null,"LED",16,null,"",null,null,24,null,4000,80,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"","",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"Poland"]
["2308","2308XX0009","EGERSUND WOOD BOLLARD 85CM LED 1370LM 3000K DIM.",null,"Luminaire with contemporary design. For lighting gardens, private areas, and other architectural applications",null,"Egersund Mini,Wood","Bollard","Europe, Africa, Asia, Australia and Oceania, North America, South America",2,2,0.69,0,"",null,null,null,null,null,null,null,"2308XX0009.png",3,1,1,3,6,1,66,"CE","","","Class II",null,null,null,null,null,0.12,0.12,0.85,null,null,null,null,"2308XX0009.ldt",1,null,null,null,null,1,null,null,null,null,null,null,"LED",16,null,"",null,null,23,null,3000,80,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"","",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"Poland"]
["2309","2309XX0009","EGERSUND WOOD BOLLARD 85CM LED 1462LM 4000K DIM.",null,"Luminaire with contemporary design. For lighting gardens, private areas, and other architectural applications",null,"Egersund Mini,Wood","Bollard","Europe, Africa, Asia, Australia and Oceania, North America, South America",2,2,0.69,0,"",null,null,null,null,null,null,null,"2309XX0009.png",3,1,1,3,6,1,66,"CE","","","Class II",null,null,null,null,null,0.12,0.12,0.85,null,null,null,null,"2309XX0009.ldt",1,null,null,null,null,1,null,null,null,null,null,null,"LED",16,null,"",null,null,24,null,4000,80,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"","",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"Poland"]
["2317","2317XX0009","EGERSUND WOOD BOLLARD 49CM LED 1462LM 4000K DIM.",null,"Luminaire with contemporary design. For lighting gardens, private areas, and other architectural applications",null,"Egersund Mini,Wood","Bollard","Europe, Africa, Asia, Australia and Oceania, North America, South America",2,2,0.33,0,"",null,null,null,null,null,null,null,"2317XX0009.png",3,1,1,3,6,1,66,"CE","","","Class II",null,null,null,null,null,0.12,0.12,0.49,null,null,null,null,"2317XX0009.ldt",1,null,null,null,null,1,null,null,null,null,null,null,"LED",16,null,"",null,null,24,null,4000,80,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"","",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"Poland"]
["2320","2320XX0009","EGERSUND WOOD BOLLARD 49CM LED 1370LM 3000K DIM.",null,"Luminaire with contemporary design. For lighting gardens, private areas, and other architectural applications",null,"Egersund Mini,Wood","Bollard","Europe, Africa, Asia, Australia and Oceania, North America, South America",2,2,0.33,0,"",null,null,null,null,null,null,null,"2320XX0009.png",3,1,1,3,6,1,66,"CE","","","Class II",null,null,null,null,null,0.12,0.12,0.49,null,null,null,null,"2320XX0009.ldt",1,null,null,null,null,1,null,null,null,null,null,null,"LED",16,null,"",null,null,23,null,3000,80,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"","",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"Poland"]
["2321","2321XX0009","EGERSUND WOOD BOLLARD 49CM LED 1462LM 4000K DIM.",null,"Luminaire with contemporary design. For lighting gardens, private areas, and other architectural applications",null,"Egersund Mini,Wood","Bollard","Europe, Africa, Asia, Australia and Oceania, North America, South America",2,2,0.33,0,"",null,null,null,null,null,null,null,"2321XX0009.png",3,1,1,3,6,1,66,"CE","","","Class II",null,null,null,null,null,0.12,0.12,0.49,null,null,null,null,"2321XX0009.ldt",1,null,null,null,null,1,null,null,null,null,null,null,"LED",16,null,"",null,null,24,null,4000,80,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"","",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"Poland"]
["2330","2330XX0009","LILLESAND BOLLARD 85CM LED 1370LM 3000K DIM.",null,"Luminaire with contemporary design. For lighting gardens, private areas, and other architectural structures",null,"Lillesand","Bollard","Europe, Africa, Asia, Australia and Oceania, North America, South America",2,2,0.74,0,"",null,null,null,null,null,null,null,"2330XX0009.png",3,1,1,3,6,1,66,"CE","","IK08","Class II",null,null,null,null,null,0,0,0,null,null,null,null,"2330XX0009.ldt",1,null,null,null,null,1,null,null,null,null,null,null,"LED",16,null,"",null,null,23,null,3000,80,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"","",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"Poland"]
["2331","2331XX0009","LILLESAND BOLLARD 85CM LED 1462LM 4000K DIM.",null,"Luminaire with contemporary design. For lighting gardens, private areas, and other architectural structures",null,"Lillesand","Bollard","Europe, Africa, Asia, Australia and Oceania, North America, South America",2,2,0.74,0,"",null,null,null,null,null,null,null,"2331XX0009.png",3,1,1,3,6,1,66,"CE","","IK08","Class II",null,null,null,null,null,0,0,0,null,null,null,null,"2331XX0009.ldt",1,null,null,null,null,1,null,null,null,null,null,null,"LED",16,null,"",null,null,24,null,4000,80,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"","",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"Poland"]
["2334","2334XX0009","LILLESAND WOOD BOLLARD 85CM LED 1370LM 3000K DIM.",null,"A luminaire with a contemporary design. For lighting gardens, private areas and other architectural concepts.",null,"Lillesand,Wood","Bollard","Europe, Africa, Asia, Australia and Oceania, North America, South America",2,2,0.74,0,"",null,null,null,null,null,null,null,"2334XX0009.png",3,1,1,3,6,1,66,"CE","","","Class II",null,null,null,null,null,0,0,0,null,null,null,null,"2334XX0009.ldt",1,null,null,null,null,1,null,null,null,null,null,null,"LED",16,null,"",null,null,23,null,3000,80,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"","",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"Poland"]
["2335","2335XX0009","LILLESAND WOOD BOLLARD 85CM LED 1462LM 4000K DIM.",null,"A luminaire with a contemporary design. For lighting gardens, private areas and other architectural concepts.",null,"Lillesand,Wood","Bollard","Europe, Africa, Asia, Australia and Oceania, North America, South America",2,2,0.74,0,"",null,null,null,null,null,null,null,"2335XX0009.png",3,1,1,3,6,1,66,"CE","","","Class II",null,null,null,null,null,0,0,0,null,null,null,null,"2335XX0009.ldt",1,null,null,null,null,1,null,null,null,null,null,null,"LED",16,null,"",null,null,24,null,4000,80,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"","",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"Poland"]
["2338","2338XX0009","LILLESAND WOOD BOLLARD 85CM LED 1370LM 3000K DIM.",null,"A luminaire with a contemporary design. For lighting gardens, private areas and other architectural concepts.",null,"Lillesand,Wood","Bollard","Europe, Africa, Asia, Australia and Oceania, North America, South America",2,2,0.74,0,"",null,null,null,null,null,null,null,"2338XX0009.png",3,1,1,3,6,1,66,"CE","","","Class II",null,null,null,null,null,0,0,0,null,null,null,null,"2338XX0009.ldt",1,null,null,null,null,1,null,null,null,null,null,null,"LED",16,null,"",null,null,23,null,3000,80,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"","",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"Poland"]
["2339","2339XX0009","LILLESAND WOOD BOLLARD 85CM LED 1462LM 4000K DIM.",null,"A luminaire with a contemporary design. For lighting gardens, private areas and other architectural concepts.",null,"Lillesand,Wood","Bollard","Europe, Africa, Asia, Australia and Oceania, North America, South America",2,2,0.74,0,"",null,null,null,null,null,null,null,"2339XX0009.png",3,1,1,3,6,1,66,"CE","","","Class II",null,null,null,null,null,0,0,0,null,null,null,null,"2339XX0009.ldt",1,null,null,null,null,1,null,null,null,null,null,null,"LED",16,null,"",null,null,24,null,4000,80,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"","",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"Poland"]
["2342","2342XX0009","LILLESAND BOLLARD 49CM LED 1370LM 3000K DIM.",null,"Luminaire with contemporary design. For lighting gardens, private areas, and other architectural structures",null,"Lillesand","Bollard","Europe, Africa, Asia, Australia and Oceania, North America, South America",2,2,0.38,0,"",null,null,null,null,null,null,null,"2342XX0009.png",3,1,1,3,6,1,66,"CE","","IK08","Class II",null,null,null,null,null,0,0,0,null,null,null,null,"2342XX0009.ldt",1,null,null,null,null,1,null,null,null,null,null,null,"LED",16,null,"",null,null,23,null,3000,80,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"","",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"Poland"]
["2343","2343XX0009","LILLESAND BOLLARD 49CM LED 1462LM 4000K DIM.",null,"Luminaire with contemporary design. For lighting gardens, private areas, and other architectural structures",null,"Lillesand","Bollard","Europe, Africa, Asia, Australia and Oceania, North America, South America",2,2,0.38,0,"",null,null,null,null,null,null,null,"2343XX0009.png",3,1,1,3,6,1,66,"CE","","IK08","Class II",null,null,null,null,null,0,0,0,null,null,null,null,"2343XX0009.ldt",1,null,null,null,null,1,null,null,null,null,null,null,"LED",16,null,"",null,null,24,null,4000,80,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"","",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"Poland"]
["2346","2346XX0009","LILLESAND WOOD BOLLARD 49CM LED 1370LM 3000K DIM.",null,"A luminaire with a contemporary design. For lighting gardens, private areas and other architectural concepts.",null,"Lillesand,Wood","Bollard","Europe, Africa, Asia, Australia and Oceania, North America, South America",2,2,0.38,0,"",null,null,null,null,null,null,null,"2346XX0009.png",3,1,1,3,6,1,66,"CE","","","Class II",null,null,null,null,null,0,0,0,null,null,null,null,"2346XX0009.ldt",1,null,null,null,null,1,null,null,null,null,null,null,"LED",16,null,"",null,null,23,null,3000,80,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"","",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"Poland"]
["2347","2347XX0009","LILLESAND WOOD BOLLARD 49CM LED 1462LM 4000K DIM.",null,"A luminaire with a contemporary design. For lighting gardens, private areas and other architectural concepts.",null,"Lillesand,Wood","Bollard","Europe, Africa, Asia, Australia and Oceania, North America, South America",2,2,0.38,0,"",null,null,null,null,null,null,null,"2347XX0009.png",3,1,1,3,6,1,66,"CE","","","Class II",null,null,null,null,null,0,0,0,null,null,null,null,"2347XX0009.ldt",1,null,null,null,null,1,null,null,null,null,null,null,"LED",16,null,"",null,null,24,null,4000,80,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"","",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"Poland"]
["2350","2350XX0009","LILLESAND WOOD BOLLARD 49CM LED 1370LM 3000K DIM.",null,"A luminaire with a contemporary design. For lighting gardens, private areas and other architectural concepts.",null,"Lillesand,Wood","Bollard","Europe, Africa, Asia, Australia and Oceania, North America, South America",2,2,0.38,0,"",null,null,null,null,null,null,null,"2350XX0009.png",3,1,1,3,6,1,66,"CE","","","Class II",null,null,null,null,null,0,0,0,null,null,null,null,"2350XX0009.ldt",1,null,null,null,null,1,null,null,null,null,null,null,"LED",16,null,"",null,null,23,null,3000,80,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"","",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"Poland"]
["2351","2351XX0009","LILLESAND WOOD BOLLARD 49CM LED 1462LM 4000K DIM.",null,"A luminaire with a contemporary design. For lighting gardens, private areas and other architectural concepts.",null,"Lillesand,Wood","Bollard","Europe, Africa, Asia, Australia and Oceania, North America, South America",2,2,0.38,0,"",null,null,null,null,null,null,null,"2351XX0009.png",3,1,1,3,6,1,66,"CE","","","Class II",null,null,null,null,null,0,0,0,null,null,null,null,"2351XX0009.ldt",1,null,null,null,null,1,null,null,null,null,null,null,"LED",16,null,"",null,null,24,null,4000,80,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"","",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"Poland"]
["2360","2360XX0009","OPPLAND WOOD BOLLARD 85CM LED 1294LM 3000K DIM.",null,"A bollard luminaire with a stable and durable structure. For lighting private areas and other architectural concepts",null,"Oppland,Wood","Bollard","Europe, Africa, Asia, Australia and Oceania, North America, South America",2,2,0.8,0,"",null,null,null,null,null,null,null,"2360XX0009.png",7,1,1,3,6,1,66,"CE","","IK09","Class II",null,null,null,null,null,0.12,0.12,0.85,null,null,null,null,"2360XX0009.ldt",1,null,null,null,null,0,null,null,null,null,null,null,"LED",16,null,"",null,null,23,null,3000,80,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"","",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"Poland"]
["2361","2361XX0009","OPPLAND WOOD BOLLARD 85CM LED 1371LM 4000K DIM.",null,"A bollard luminaire with a stable and durable structure. For lighting private areas and other architectural concepts",null,"Oppland,Wood","Bollard","Europe, Africa, Asia, Australia and Oceania, North America, South America",2,2,0.8,0,"",null,null,null,null,null,null,null,"2361XX0009.png",7,1,1,3,6,1,66,"CE","","IK09","Class II",null,null,null,null,null,0.12,0.12,0.85,null,null,null,null,"2361XX0009.ldt",1,null,null,null,null,0,null,null,null,null,null,null,"LED",16,null,"",null,null,24,null,4000,80,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"","",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"Poland"]
["2364","2364XX0009","OPPLAND WOOD BOLLARD 85CM LED 1294LM 3000K DIM.",null,"A bollard luminaire with a stable and durable structure. For lighting private areas and other architectural concepts",null,"Oppland,Wood","Bollard","Europe, Africa, Asia, Australia and Oceania, North America, South America",2,2,0.8,0,"",null,null,null,null,null,null,null,"2364XX0009.png",7,1,1,3,6,1,66,"CE","","IK09","Class II",null,null,null,null,null,0.12,0.12,0.85,null,null,null,null,"2364XX0009.ldt",1,null,null,null,null,0,null,null,null,null,null,null,"LED",16,null,"",null,null,23,null,3000,80,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"","",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"Poland"]
["2365","2365XX0009","OPPLAND WOOD BOLLARD 85CM LED 1371LM 4000K DIM.",null,"A bollard luminaire with a stable and durable structure. For lighting private areas and other architectural concepts",null,"Oppland,Wood","Bollard","Europe, Africa, Asia, Australia and Oceania, North America, South America",2,2,0.8,0,"",null,null,null,null,null,null,null,"2365XX0009.png",7,1,1,3,6,1,66,"CE","","IK09","Class II",null,null,null,null,null,0.12,0.12,0.85,null,null,null,null,"2365XX0009.ldt",1,null,null,null,null,0,null,null,null,null,null,null,"LED",16,null,"",null,null,24,null,4000,80,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"","",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"Poland"]
["2400","2400XX0010","HELLVIK BOLLARD 55CM LED 978LM 3000K DIM.",null,"A luminaire with a contemporary design. For lighting gardens, private areas and other architectural concepts.",null,"Hellvik","Bollard","Europe, Africa, Asia, Australia and Oceania, North America, South America",2,2,0.5,0,"",null,null,null,null,null,null,null,"2400XX0010.png",7.9,1,2,3,6,1,66,"CE","","","Class II",null,null,null,null,null,0.42,0.11,0.55000000000000004,null,null,null,null,"2400XX0010.ldt",1,null,null,null,null,0,null,null,null,null,null,null,"LED",16,null,"",null,null,23,null,3000,80,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"","",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"Poland"]
["2402","2402XX0009","HELLVIK BOLLARD 55CM LED 1344LM 3000K DALI",null,"A luminaire with a contemporary design. For lighting gardens, private areas and other architectural concepts",null,"Hellvik","Bollard","Europe, Africa, Asia, Australia and Oceania, North America, South America",2,2,0.5,0,"",null,null,null,null,null,null,null,"2402XX0009.png",7.9,1,2,3,6,3,66,"CE","","","Class I",null,null,null,null,null,0.42,0.11,0.55000000000000004,null,null,null,null,"2402XX0009.ldt",1,null,null,null,null,0,null,null,null,null,null,null,"LED",16,null,"",null,null,23,null,3000,80,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"DALI","",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"Poland"]
["2403","2403XX0009","HELLVIK BOLLARD 55CM LED 1426LM 4000K DALI",null,"A luminaire with a contemporary design. For lighting gardens, private areas and other architectural concepts",null,"Hellvik","Bollard","Europe, Africa, Asia, Australia and Oceania, North America, South America",2,2,0.5,0,"",null,null,null,null,null,null,null,"2403XX0009.png",7.9,1,2,3,6,3,66,"CE","","IK08","Class I",null,null,null,null,null,0.42,0.11,0.55000000000000004,null,null,null,null,"2403XX0009.ldt",1,null,null,null,null,0,null,null,null,null,null,null,"LED",16,null,"",null,null,24,null,4000,80,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"DALI","",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"Poland"]
["2404","2404XX0009","HELLVIK BOLLARD 55CM LED 1159LM 3000K DIM.",null,"A luminaire with a contemporary design. For lighting gardens, private areas and other architectural concepts.",null,"Hellvik","Bollard","Europe, Africa, Asia, Australia and Oceania, North America, South America",2,2,0.5,0,"",null,null,null,null,null,null,null,"2404XX0009.png",7.9,1,2,3,6,1,66,"CE","","IK08","Class II",null,null,null,null,null,0.42,0.11,0.55000000000000004,null,null,null,null,"2404XX0009.ldt",1,null,null,null,null,0,null,null,null,null,null,null,"LED",16,null,"",null,null,23,null,3000,70,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"","",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"Poland"]
["2405","2405XX0009","HELLVIK BOLLARD 55CM LED 1254LM 4000K DIM.",null,"A luminaire with a contemporary design. For lighting gardens, private areas and other architectural concepts.",null,"Hellvik","Bollard","Europe, Africa, Asia, Australia and Oceania, North America, South America",2,2,0.5,0,"",null,null,null,null,null,null,null,"2405XX0009.png",7.9,1,2,3,6,1,66,"CE","","IK08","Class II",null,null,null,null,null,0.42,0.11,0.55000000000000004,null,null,null,null,"2405XX0009.ldt",1,null,null,null,null,0,null,null,null,null,null,null,"LED",16,null,"",null,null,24,null,4000,70,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"","",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"Poland"]
["2406","2406XX0009","HELLVIK BOLLARD 55CM LED 1691LM 3000K DALI2",null,"A luminaire with a contemporary design. For lighting gardens, private areas and other architectural concepts.",null,"Hellvik","Bollard","Europe, Africa, Asia, Australia and Oceania, North America, South America",2,2,0.5,0,"",null,null,null,null,null,null,null,"2406XX0009.png",7.9,1,2,3,6,3,66,"CE","","IK08","Class I",null,null,null,null,null,0.42,0.11,0.55000000000000004,null,null,null,null,"2406XX0009.ldt",1,null,null,null,null,0,null,null,null,null,null,null,"LED",16,null,"",null,null,23,null,3000,70,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"DALI","",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"Poland"]
["2407","2407XX0009","HELLVIK BOLLARD 55CM LED 1831LM 4000K DALI2",null,"A luminaire with a contemporary design. For lighting gardens, private areas and other architectural concepts.",null,"Hellvik","Bollard","Europe, Africa, Asia, Australia and Oceania, North America, South America",2,2,0.5,0,"",null,null,null,null,null,null,null,"2407XX0009.png",7.9,1,2,3,6,3,66,"CE","","IK08","Class I",null,null,null,null,null,0.42,0.11,0.55000000000000004,null,null,null,null,"2407XX0009.ldt",1,null,null,null,null,0,null,null,null,null,null,null,"LED",16,null,"",null,null,24,null,4000,70,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"DALI","",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"Poland"]
["2410","2410XX0010","HELLVIK BOLLARD 85CM LED 1956LM 3000K DIM. TRIAC",null,"A luminaire with a contemporary design. For lighting gardens, private areas and other architectural concepts.",null,"Hellvik","Bollard","Europe, Africa, Asia, Australia and Oceania, North America, South America",2,2,0.8,0,"",null,null,null,null,null,null,null,"2410XX0010.jpg",7.9,1,2,3,6,1,66,"CE","","IK08","Class II",null,null,null,null,null,0.42,0.11,0.85,null,null,null,null,"2410XX0010.ldt",1,null,null,null,null,0,null,null,null,null,null,null,"LED",16,null,"",null,null,23,null,3000,80,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"","",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"Poland"]
["2411","2411XX0010","HELLVIK BOLLARD 85CM LED 1956LM 4000K DIM. TRIAC",null,"A luminaire with a contemporary design. For lighting gardens, private areas and other architectural concepts.",null,"Hellvik","Bollard","Europe, Africa, Asia, Australia and Oceania, North America, South America",2,2,0.8,0,"",null,null,null,null,null,null,null,"2411XX0010.jpg",7.9,1,2,3,6,1,66,"CE","","IK08","Class II",null,null,null,null,null,0.42,0.11,0.85,null,null,null,null,"2411XX0010.ldt",1,null,null,null,null,0,null,null,null,null,null,null,"LED",16,null,"",null,null,24,null,4000,80,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"","",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"Poland"]
["2412","2412XX0009","HELLVIK BOLLARD 85CM 2XLED 3075LM 3000K DALI",null,"A luminaire with a contemporary design. For lighting gardens, private areas and other architectural concepts",null,"Hellvik","Bollard","Europe, Africa, Asia, Australia and Oceania, North America, South America",2,2,0.8,0,"",null,null,null,null,null,null,null,"2412XX0009.jpg",7.9,1,2,3,6,3,66,"CE","","IK08","Class I",null,null,null,null,null,0.42,0.11,0.85,null,null,null,null,"2412XX0009.ldt",1,null,null,null,null,0,null,null,null,null,null,null,"LED",16,null,"",null,null,23,null,3000,80,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"DALI","",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"Poland"]
["2413","2413XX0009","HELLVIK BOLLARD 85CM 2XLED 3075LM 4000K DALI",null,"A luminaire with a contemporary design. For lighting gardens, private areas and other architectural concepts",null,"Hellvik","Bollard","Europe, Africa, Asia, Australia and Oceania, North America, South America",2,2,0.8,0,"",null,null,null,null,null,null,null,"2413XX0009.jpg",7.9,1,2,3,6,3,66,"CE","","IK08","Class I",null,null,null,null,null,0.42,0.11,0.85,null,null,null,null,"2413XX0009.ldt",1,null,null,null,null,0,null,null,null,null,null,null,"LED",16,null,"",null,null,24,null,4000,80,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"DALI","",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"Poland"]
["2414","2414XX0009","HELLVIK BOLLARD 85CM LED 1159LM 3000K DIM.",null,"A luminaire with a contemporary design. For lighting gardens, private areas and other architectural concepts.",null,"Hellvik","Bollard","Europe, Africa, Asia, Australia and Oceania, North America, South America",2,2,0.8,0,"",null,null,null,null,null,null,null,"2414XX0009.jpg",7.9,1,2,3,6,1,66,"CE","","IK08","Class II",null,null,null,null,null,0.42,0.11,0.85,null,null,null,null,"2414XX0009.ldt",1,null,null,null,null,0,null,null,null,null,null,null,"LED",16,null,"",null,null,23,null,3000,70,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"","",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"Poland"]
["2415","2415XX0009",{"$f":"INDEX(DB,MATCH($A377,ID,0),3)","v":"HELLVIK BOLLARD 85CM LED 1254LM 4000K DIM."},null,"A luminaire with a contemporary design. For lighting gardens, private areas and other architectural concepts.",null,"Hellvik",{"$f":"IF(INDEX(DB,MATCH($A377,ID,0),5)=0,\"\",INDEX(DB,MATCH($A377,ID,0),5))","v":"Bollard"},"Europe, Africa, Asia, Australia and Oceania, North America, South America",2,{"$f":"IFERROR(INDEX(TYPMONT,MATCH((INDEX(DB,MATCH($A377,ID,0),31)),ID_RODZ,0),3),\"\")","v":2},0.8,0,{"$f":"IFERROR(IF(INDEX(TYPMONT,MATCH((INDEX(DB,MATCH($A377,ID,0),31)),ID_RODZ,0),6)=0,\"\",INDEX(TYPMONT,MATCH((INDEX(DB,MATCH($A377,ID,0),31)),ID_RODZ,0),6)),\"\")","v":""},null,null,null,null,null,null,null,{"$f":"IF(INDEX(DB,MATCH($A377,ID,0),57)=0,\"\",INDEX(DB,MATCH($A377,ID,0),57))","v":"2415XX0009.jpg"},7.9,{"$f":"IF(INDEX(DB,MATCH($A377,ID,0),61)=0,\"\",INDEX(DB,MATCH($A377,ID,0),61))","v":1},2,{"$f":"IFERROR(INDEX(TYPMONT,MATCH((INDEX(DB,MATCH($A377,ID,0),31)),ID_RODZ,0),1),\"\")","v":3},{"$f":"IFERROR(INDEX(TYPMONT,MATCH((INDEX(DB,MATCH($A377,ID,0),31)),ID_RODZ,0),2),\"\")","v":6},{"$f":"IF(INDEX(DB,MATCH($A377,ID,0),59)=0,\"\",INDEX(DB,MATCH($A377,ID,0),59))","v":1},{"$f":"IFERROR(IF(INDEX(DB,MATCH($A377,ID,0),19)=0,\"\",INDEX(DB,MATCH($A377,ID,0),19)+1),\"\")","v":66},{"$f":"IF(INDEX(DB,MATCH($A377,ID,0),27)=0,\"\",INDEX(DB,MATCH($A377,ID,0),27))","v":"CE"},"",{"$f":"IF(INDEX(DB,MATCH($A377,ID,0),20)=0,\"\",INDEX(DB,MATCH($A377,ID,0),20))","v":"IK08"},{"$f":"IF(INDEX(DB,MATCH($A377,ID,0),21)=0,\"\",INDEX(DB,MATCH($A377,ID,0),21))","v":"Class II"},null,null,null,null,null,0.42,0.11,0.85,null,null,null,null,{"$f":"IF(INDEX(DB,MATCH($A377,ID,0),58)=0,\"\",INDEX(DB,MATCH($A377,ID,0),58))","v":"2415XX0009.ldt"},1,null,null,null,null,0,null,null,null,null,null,null,"LED",16,null,{"$f":"IF(INDEX(DB,MATCH($A377,ID,0),60)=0,\"\",INDEX(DB,MATCH($A377,ID,0),60))","v":""},null,null,24,null,{"$f":"IF(INDEX(DB,MATCH($A377,ID,0),22)=0,\"\",INDEX(DB,MATCH($A377,ID,0),22))","v":4000},{"$f":"IF(INDEX(DB,MATCH($A377,ID,0),53)=0,\"\",INDEX(DB,MATCH($A377,ID,0),53))","v":70},null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,{"$f":"IF(INDEX(DB,MATCH($A377,ID,0),29)=0,\"\",INDEX(DB,MATCH($A377,ID,0),29))","v":""},{"$f":"IF(INDEX(DB,MATCH($A377,ID,0),28)=0,\"\",INDEX(DB,MATCH($A377,ID,0),28))","v":""},null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"Poland"]
["2416","2416XX0009","HELLVIK BOLLARD 85CM LED 1691LM 3000K DALI2",null,"A luminaire with a contemporary design. For lighting gardens, private areas and other architectural concepts.",null,{"$f":"IF(INDEX(DB,MATCH($A378,ID,0),4)=0,\"\",INDEX(DB,MATCH($A378,ID,0),4))","v":"Hellvik"},"Bollard","Europe, Africa, Asia, Australia and Oceania, North America, South America",2,2,0.8,0,"",null,null,null,null,null,null,null,"2416XX0009.jpg",7.9,1,2,3,6,3,66,"CE",{"$f":"IFERROR(IF(FIND(\"RENA\",$C378)>0,\"Vehicle resistant\",\"\"),\"\")","v":""},"","Class I",null,null,null,null,null,0.42,0.11,0.85,null,null,null,null,"2416XX0009.ldt",1,null,null,null,null,0,null,null,null,null,null,null,"LED",16,null,"",null,null,{"$f":"IF($BO378=4000,24,23)","v":23},null,3000,70,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"DALI","",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"Poland"]
["2417","2417XX0009","HELLVIK BOLLARD 85CM LED 1831LM 4000K DALI2",null,"A luminaire with a contemporary design. For lighting gardens, private areas and other architectural concepts.",null,"Hellvik","Bollard","Europe, Africa, Asia, Australia and Oceania, North America, South America",2,2,0.8,0,"",null,null,null,null,null,null,null,"2417XX0009.jpg",7.9,1,2,3,6,3,66,"CE","","","Class I",null,null,null,null,null,0.42,0.11,0.85,null,null,null,null,"2417XX0009.ldt",1,null,null,null,null,0,null,null,null,null,null,null,"LED",16,null,"",null,null,24,null,4000,70,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"DALI","",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"Poland"]
["242","242XX0309","OSLO POLE-TOP E27",null,"Classic design luminaire, mounted on a telescopic lighting pole. Adjustable height 1700..2300mm. For lighting gardens, terraces and other architectural concepts.",null,"Oslo","Post,Post complete","Europe, Africa, Asia, Australia and Oceania, North America, South America",2,512,2.4,0,"",null,null,null,null,null,null,null,"242XX0309.jpg",3,1,1,5,9,4,56,"CE","","","Class II",null,null,null,null,null,0.78,0.28000000000000003,2.38,null,null,null,null,"242XX0309.ldt",0,null,null,null,null,1,null,null,null,null,null,null,"LED",16,null,"E27",null,null,23,null,"",80,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"","",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"Poland"]
["245","245XX0011","OSLO BOLLARD E27",null,"Scandinavian design luminaire. For lighting private areas and public spaces.",null,"Oslo","Bollard,Flower","Europe, Africa, Asia, Australia and Oceania, North America, South America",2,2,1,0,"",null,null,null,null,null,null,null,"245XX0011.jpg",9,1,1,3,6,4,56,"CE","","","Class II",null,null,null,null,null,0.28000000000000003,0.48,1.18,null,null,null,null,"245XX0011.ldt",0,null,null,null,null,1,null,null,null,null,null,null,"LED",16,null,"E27",null,null,23,null,"",80,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"","",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"Poland"]
["280","280XX0010","STOCKHOLM WALL E27",null,"Classic type, wall-mounted luminaire in scandinavian design for general use. Possibility to install on corners of architectural objects.",null,"Stockholm","Wall","Europe, Africa, Asia, Australia and Oceania, North America, South America",2,4,0,2.5,"",null,null,null,null,null,null,null,"280XX0010.jpg",9,1,1,2,2,4,55,"CE","","","Class II",null,null,null,null,null,0.28999999999999998,0.28999999999999998,0.31,null,null,null,null,"280XX0010.ldt",0,null,null,null,null,3,null,null,null,null,null,null,"LED",16,null,"E27",null,null,23,null,"",80,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"","",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"Poland"]
["281","281XX0309","STOCKHOLM POLE LUMINAIRE. E27",null,"Pole top luminaire in scandinavian design. For installation on a lighting pole with adjustable height 1510...2480mm. For lighting gardens, parks, and any other architectural concepts.",null,"Stockholm","Post,Post complete","Europe, Africa, Asia, Australia and Oceania, North America, South America",2,256,2.25,0,"",null,null,null,null,null,null,null,"281XX0309.jpg",9,1,1,5,8,4,55,"CE","","","Class II",null,null,null,null,null,0.35,0.35,2.48,null,null,null,null,"281XX0309.ldt",0,null,null,null,null,1,null,null,null,null,null,null,"LED",16,null,"E27",null,null,23,null,"",80,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"","",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"Poland"]
["283","283XX0309","STOCKHOLM POLE-TOP E27",null,"Pole top luminaire in scandinavian design. For installation on a lighting pole with adjustable height 1740...2520mm. For lighting gardens, parks, and any other architectural concepts.",null,"Stockholm","Post,Post complete","Europe, Africa, Asia, Australia and Oceania, North America, South America",2,512,2.25,0,"",null,null,null,null,null,null,null,"283XX0309.jpg",9,1,1,5,9,4,55,"CE","","","Class II",null,null,null,null,null,0.35,0.92,2.52,null,null,null,null,"283XX0309.ldt",0,null,null,null,null,1,null,null,null,null,null,null,"LED",16,null,"E27",null,null,23,null,"",80,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"","",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"Poland"]
["284","284XX0010","STOCKHOLM BOLLARD 345CM E27",null,"Scandinavian design luminaire. For lighting gardens, terraces and any others architectural concepts.",null,"Stockholm","Bollard,Pedestal","Europe, Africa, Asia, Australia and Oceania, North America, South America",2,2,0.1,0,"",null,null,null,null,null,null,null,"284XX0010.jpg",9,1,1,3,6,4,55,"CE","","","Class II",null,null,null,null,null,0.27,0.27,0.34,null,null,null,null,"284XX0010.ldt",0,null,null,null,null,1,null,null,null,null,null,null,"LED",16,null,"E27",null,null,23,null,"",80,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"","",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"Poland"]
["285","285XX0010","STOCKHOLM BOLLARD 118CM E27",null,"Scandinavian design luminaire for general use. For lighting gardens, terraces and any other architectural concepts.",null,"Stockholm","Bollard,Flower","Europe, Africa, Asia, Australia and Oceania, North America, South America",2,2,0.94,0,"",null,null,null,null,null,null,null,"285XX0010.jpg",9,1,1,3,6,4,55,"CE","","","Class II",null,null,null,null,null,0.27,0.27,1.18,null,null,null,null,"285XX0010.ldt",0,null,null,null,null,1,null,null,null,null,null,null,"LED",16,null,"E27",null,null,23,null,"",80,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"","",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"Poland"]
["286","286XX0010","STOCKHOLM WALL E27",null,"Scandinavian design, wall-mounted luminaire for general use. Possibility to install on corners of architectural objects.",null,"Stockholm,Big","Wall","Europe, Africa, Asia, Australia and Oceania, North America, South America",2,4,0.2,2.5,"",null,null,null,null,null,null,null,"286XX0010.jpg",9,1,1,2,2,4,55,"CE","","","Class II",null,null,null,null,null,0.39,0.39,0.38,null,null,null,null,"286XX0010.ldt",0,null,null,null,null,3,null,null,null,null,null,null,"LED",16,null,"E27",null,null,23,null,"",80,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"","",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"Poland"]
["287","287XX0010","STOCKHOLM BOLLARD E27",null,"Scandinavian design luminaire. For lighting gardens, terraces and any other architectural concepts.",null,"Stockholm,Big","Bollard,Pedestal","Europe, Africa, Asia, Australia and Oceania, North America, South America",2,2,0.3,0,"",null,null,null,null,null,null,null,"287XX0010.jpg",9,1,1,3,6,4,55,"CE","","","Class II",null,null,null,null,null,0.35,0.35,0.48,null,null,null,null,"287XX0010.ldt",0,null,null,null,null,1,null,null,null,null,null,null,"LED",16,null,"E27",null,null,23,null,"",80,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"","",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"Poland"]
["288","288XX0011","STOCKHOLM BOLLARD 85CM E27",null,"Bollard luminaire of stable and durable construction. For lighting private areas and public spaces.",null,"Stockholm","Bollard","Europe, Africa, Asia, Australia and Oceania, North America, South America",2,2,0.68,0,"",null,null,null,null,null,null,null,"288XX0011.jpg",7,1,1,3,6,4,66,"CE","","","Class II",null,null,null,null,null,0.17,0.17,0.85,null,null,null,null,"288XX0011.ldt",0,null,null,null,null,1,null,null,null,null,null,null,"LED",16,null,"E27",null,null,23,null,"",80,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"","",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"Poland"]
["289","289XX0011","STOCKHOLM BOLLARD 49CM E27",null,"Bollard luminaire of stable and durable construction. For lighting private areas and public spaces.",null,"Stockholm","Bollard","Europe, Africa, Asia, Australia and Oceania, North America, South America",2,2,0.32,0,"",null,null,null,null,null,null,null,"289XX0011.jpg",7,1,1,3,6,4,66,"CE","","","Class II",null,null,null,null,null,0.17,0.17,0.49,null,null,null,null,"289XX0011.ldt",0,null,null,null,null,1,null,null,null,null,null,null,"LED",16,null,"E27",null,null,23,null,"",80,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"","",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"Poland"]
["291",{"$f":"INDEX(DB,MATCH($A391,ID,0),2)","v":"291XX0011"},"ALTA BOLLARD 85CM E27",null,{"$f":"IF(INDEX(DB,MATCH($A391,ID,0),35)=0,\"\",INDEX(DB,MATCH($A391,ID,0),35))","v":"Bollard luminaire of stable and durable construction. For lighting private areas and public spaces."},null,"Alta","Bollard","Europe, Africa, Asia, Australia and Oceania, North America, South America",2,2,0.7,0,"",null,null,null,null,null,null,null,"291XX0011.jpg",{"$f":"IF((IFERROR(INDEX(BRYLA_FOTO,MATCH(INDEX(DB,MATCH($A391,ID,0),62),ID_BRYLAFOTO,0),6),\"\"))<>0,IFERROR(INDEX(BRYLA_FOTO,MATCH(INDEX(DB,MATCH($A391,ID,0),62),ID_BRYLAFOTO,0),6),\"\"),\"\")","v":7.3},1,1,3,6,4,66,"CE","","IK10","Class II",null,null,null,null,null,{"$f":"INDEX(DB,MATCH($A391,ID,0),24)","v":0.15},{"$f":"INDEX(DB,MATCH($A391,ID,0),25)","v":0.15},{"$f":"INDEX(DB,MATCH($A391,ID,0),26)","v":0.85},null,null,null,null,"291XX0011.ldt",0,null,null,null,null,1,null,null,null,null,null,null,"LED",16,null,"E27",null,null,23,null,"",80,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"","",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"Poland"]
["293","293XX0011","ALTA BOLLARD 49CM E27",null,"Bollard luminaire of stable and durable construction. For lighting private areas and public spaces.",null,"Alta","Bollard","Europe, Africa, Asia, Australia and Oceania, North America, South America",2,2,0.34,0,"",null,null,null,null,null,null,null,"293XX0011.jpg",7.3,1,1,3,6,4,66,"CE","","IK10","Class II",null,null,null,null,null,0.15,0.15,0.49,null,null,null,null,"293XX0011.ldt",{"$f":"IF($BJ392=\"\",1,0)","v":0},null,null,null,null,1,null,null,null,null,null,null,"LED",16,null,"E27",null,null,23,null,"",80,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"","",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"Poland"]
["295","295XX0011","HALMSTAD BOLLARD 49CM LED E27 DIM.",null,"Bollard luminaire of stable and durable construction For lighting private and public areas",null,"Halmstad","Bollard","Europe, Africa, Asia, Australia and Oceania, North America, South America",2,2,0.36,0,"",null,null,null,null,null,null,null,"295XX0011.jpg",7,1,2,3,6,1,66,"CE","","IK10","Class II",null,null,null,null,null,0.12,0.12,0.49,null,null,null,null,"295XX0011.ldt",0,null,null,null,null,1,null,null,null,null,null,null,"LED",16,null,"E27",null,null,23,null,"",80,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"","",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"Poland"]
["296","296XX0011","HALMSTAD BOLLARD 85CM E27",null,"Bollard luminaire of stable and durable construction For lighting private areas and public spaces",null,"Halmstad","Bollard","Europe, Africa, Asia, Australia and Oceania, North America, South America",2,2,0.72,0,"",null,null,null,null,null,null,null,"296XX0011.jpg",7,1,2,3,6,4,66,"CE","","IK10","Class II",null,null,null,null,null,0.12,0.12,0.85,null,null,null,null,"296XX0011.ldt",0,null,null,null,null,1,null,null,null,null,null,null,"LED",16,null,"E27",null,null,23,null,"",80,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"","",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"Poland"]
["297","297XX0010","STOCKHOLM BOLLARD 85CM E27",null,"Bollard luminaire of stable and durable construction. For lighting private areas and public spaces.",null,"Stockholm","Bollard","Europe, Africa, Asia, Australia and Oceania, North America, South America",2,2,0.68,0,"",null,null,null,null,null,null,null,"297XX0010.jpg",7,1,1,3,6,4,66,"CE","","IK10","Class II",null,null,null,null,null,0.17,0.17,0.85,null,null,null,null,"297XX0010.ldt",0,null,null,null,null,1,null,null,null,null,null,null,"LED",16,null,"E27",null,null,23,null,"",80,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"","",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"Poland"]
["298","298XX0012","STOCKHOLM BOLLARD 49CM E27",null,"Bollard luminaire of stable and durable construction. For lighting private areas and public spaces.",null,"Stockholm","Bollard","Europe, Africa, Asia, Australia and Oceania, North America, South America",2,2,0.32,{"$f":"IF(K396=4,2.5,IF(K396=64,0.5,0))","v":0},"",null,null,null,null,null,null,null,"298XX0012.jpg",7,1,1,3,6,4,66,"CE","","","Class II",null,null,null,null,null,0.17,0.17,0.49,null,null,null,null,"298XX0012.ldt",0,null,null,null,null,1,null,null,null,null,null,null,"LED",16,null,"E27",null,null,23,null,"",80,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"","",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"Poland"]
["299","299XX0010","STOCKHOLM BOLLARD 28CM E27",null,"Bollard luminaire of stable and durable construction. For lighting private areas and public spaces.",null,"Stockholm","Bollard","Europe, Africa, Asia, Australia and Oceania, North America, South America",2,2,0.1,0,"",null,null,null,null,null,null,null,"299XX0010.jpg",7,1,1,3,6,4,66,"CE","","IK10","Class II",null,null,null,null,null,0.16,0.16,0.28000000000000003,null,null,null,null,"299XX0010.ldt",0,null,null,null,null,1,null,null,null,null,null,null,"LED",16,null,"E27",null,null,23,null,"",80,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"","",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"Poland"]
["370","370XX0010","COMO WALL E27",null,"Classic type wall-mounted luminaire. Possibility to install on corners of architectural objects.",null,"Como","Wall","Europe, Africa, Asia, Australia and Oceania, North America, South America",2,4,0.2,2.5,"",null,null,null,null,null,null,null,"370XX0010.jpg",9,1,1,2,2,4,55,"CE","","","Class II",null,null,null,null,null,0,0,0,null,null,null,null,"370XX0010.ldt",0,null,null,null,null,0,null,null,null,null,null,null,"LED",16,null,"E27",null,null,23,null,"",80,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"","",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"Poland"]
["371","371XX0309","COMO POLE LUMINAIRE. E27",null,"Classic design luminaire, mounted on a telescopic lighting pole. Adjustable height 1820..2490mm. For lighting gardens, terraces and other architectural concepts.",null,"Como","Post,Post complete","Europe, Africa, Asia, Australia and Oceania, North America, South America",2,256,2.1,0,"",null,null,null,null,null,null,null,"371XX0309.jpg",9,1,1,5,8,4,55,"CE","","","Class II",null,null,null,null,null,0,0,0,null,null,null,null,"371XX0309.ldt",0,null,null,null,null,0,null,null,null,null,null,null,"LED",16,null,"E27",null,null,23,null,"",80,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"","",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"Poland"]
["372","372XX0309","COMO POLE LUMINAIRE. E27",null,"Classic design luminaire, mounted on a telescopic lighting pole. Adjustable height 1820..2490mm. For lighting gardens, terraces and other architectural concepts.",null,"Como","Post,Post complete","Europe, Africa, Asia, Australia and Oceania, North America, South America",2,256,2.1,0,"",null,null,null,null,null,null,null,"372XX0309.jpg",9,1,1,5,8,4,55,"CE","","","Class II",null,null,null,null,null,0,0,0,null,null,null,null,"372XX0309.ldt",0,null,null,null,null,0,null,null,null,null,null,null,"LED",16,null,"E27",null,null,23,null,"",80,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"","",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"Poland"]
["373","373XX0309","COMO POLE LUMINAIRE. E27",null,"Classic design luminaire, mounted on a telescopic lighting pole. Adjustable height 1820..2490mm. For lighting gardens, terraces and other architectural concepts.",null,"Como","Post,Post complete","Europe, Africa, Asia, Australia and Oceania, North America, South America",2,256,2.1,0,"",null,null,null,null,null,null,null,"373XX0309.jpg",9,1,1,5,8,4,55,"CE","","","Class II",null,null,null,null,null,0,0,0,null,null,null,null,"373XX0309.ldt",0,null,null,null,null,0,null,null,null,null,null,null,"LED",16,null,"E27",null,null,23,null,"",80,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"","",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"Poland"]
["375","375XX0010","COMO BOLLARD E27",null,"Classic design luminaire. For lighting private areas and public spaces.",null,"Como","Bollard,Flower","Europe, Africa, Asia, Australia and Oceania, North America, South America",2,2,0.9,0,"",null,null,null,null,null,null,null,"375XX0010.jpg",9,1,1,3,6,4,55,"CE","","","Class II",null,null,null,null,null,0,0,0,null,null,null,null,"375XX0010.ldt",0,null,null,null,null,0,null,null,null,null,null,null,"LED",16,null,"E27",null,null,23,null,"",80,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"","",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"Poland"]
["4051","4051XX0009","SOL CEILING LED 2200LM 3000K DIM.",null,"A luminaire with a contemporary design. For lighting gardens, private areas and other architectural concepts",null,"Sol","Ceiling","Europe, Africa, Asia, Australia and Oceania, North America, South America",2,1,2.8,0,"",null,null,null,null,null,null,null,"4051XX0009.png",3,1,1,1,2,1,66,"CE","","IK10","Class I",null,null,null,null,null,0.2,0.2,0.11,null,null,null,null,"4051XX0009.ldt",1,null,null,null,null,0,null,null,null,null,null,null,"LED",16,null,"",null,null,23,null,3000,80,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"","",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"Poland"]
["4052","4052XX0009","SOL CEILING LED 2499LM 4000K DIM.",null,"A luminaire with a contemporary design. For lighting gardens, private areas and other architectural concepts",null,"Sol","Ceiling","Europe, Africa, Asia, Australia and Oceania, North America, South America",2,1,2.8,0,"",null,null,null,null,null,null,null,"4052XX0009.png",3,1,1,1,2,1,66,"CE","","IK10","Class I",null,null,null,null,null,0.2,0.2,0.11,null,null,null,null,"4052XX0009.ldt",1,null,null,null,null,0,null,null,null,null,null,null,"LED",16,null,"",null,null,24,null,4000,80,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"","",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"Poland"]
["4053","4053XX0009","SOL CEILING LED 2200LM 3000K DIM.",null,"A luminaire with a contemporary design. For lighting gardens, private areas and other architectural concepts",null,"Sol","Ceiling","Europe, Africa, Asia, Australia and Oceania, North America, South America",2,1,2.8,0,"",null,null,null,null,null,null,null,"4053XX0009.png",3,1,1,1,2,1,66,"CE","","IK10","Class I",null,null,null,null,null,0.2,0.2,0.11,null,null,null,null,"4053XX0009.ldt",1,null,null,null,null,0,null,null,null,null,null,null,"LED",16,null,"",null,null,23,null,3000,80,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"","",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"Poland"]
["4054","4054XX0009","SOL CEILING LED 2400LM 4000K DIM.",null,"A luminaire with a contemporary design. For lighting gardens, private areas and other architectural concepts",null,"Sol","Ceiling","Europe, Africa, Asia, Australia and Oceania, North America, South America",2,1,2.8,0,"",null,null,null,null,null,null,null,"4054XX0009.png",3,1,1,1,2,1,66,"CE","","IK10","Class I",null,null,null,null,null,0.2,0.2,0.11,null,null,null,null,"4054XX0009.ldt",1,null,null,null,null,0,null,null,null,null,null,null,"LED",16,null,"",null,null,24,null,4000,80,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"","",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"Poland"]
["4055","4055XX0009","SOL CEILING LED 2200LM 3000K DALI2",null,"A luminaire with a contemporary design. For lighting gardens, private areas and other architectural concepts",null,"Sol","Ceiling","Europe, Africa, Asia, Australia and Oceania, North America, South America",2,1,2.8,0,"",null,null,null,null,null,null,null,"4055XX0009.png",3,1,1,1,2,3,66,"CE","","IK10","Class I",null,null,null,null,null,0.2,0.2,0.11,null,null,null,null,"4055XX0009.ldt",1,null,null,null,null,0,null,null,null,null,null,null,"LED",16,null,"",null,null,23,null,3000,80,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"DALI","",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"Poland"]
["4056","4056XX0009","SOL CEILING LED 2499LM 4000K DALI2",null,"A luminaire with a contemporary design. For lighting gardens, private areas and other architectural concepts",null,"Sol","Ceiling","Europe, Africa, Asia, Australia and Oceania, North America, South America",2,1,2.8,0,"",null,null,null,null,null,null,null,"4056XX0009.png",3,1,1,1,2,3,66,"CE","","IK10","Class I",null,null,null,null,null,0.2,0.2,0.11,null,null,null,null,"4056XX0009.ldt",1,null,null,null,null,0,null,null,null,null,null,null,"LED",16,null,"",null,null,24,null,4000,80,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"DALI","",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"Poland"]
["4057","4057XX0009","SOL CEILING LED 2200LM 3000K DALI2",null,"A luminaire with a contemporary design. For lighting gardens, private areas and other architectural concepts",null,"Sol","Ceiling","Europe, Africa, Asia, Australia and Oceania, North America, South America",2,1,2.8,0,"",null,null,null,null,null,null,null,"4057XX0009.png",3,1,1,1,2,3,66,"CE","","IK10","Class I",null,null,null,null,null,0.2,0.2,0.11,null,null,null,null,"4057XX0009.ldt",1,null,null,null,null,0,null,null,null,null,null,null,"LED",16,null,"",null,null,23,null,3000,80,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"DALI","",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"Poland"]
["4058","4058XX0009","SOL CEILING LED 2400LM 4000K DALI2",null,"A luminaire with a contemporary design. For lighting gardens, private areas and other architectural concepts",null,"Sol","Ceiling","Europe, Africa, Asia, Australia and Oceania, North America, South America",2,1,2.8,0,"",null,null,null,null,null,null,null,"4058XX0009.png",3,1,1,1,2,3,66,"CE","","IK10","Class I",null,null,null,null,null,0.2,0.2,0.11,null,null,null,null,"4058XX0009.ldt",1,null,null,null,null,0,null,null,null,null,null,null,"LED",16,null,"",null,null,24,null,4000,80,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"DALI","",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"Poland"]
["4113","4113XX0009","LONDON POLE-TOP LED 1950LM 4000K",null,"A luminaire with a classic design, mounted on a lighting pole, with a mounting base of Ø50mm For lighting gardens, parks and other architectural concepts.",null,"London,Big","Post,Head","Europe, Africa, Asia, Australia and Oceania, North America, South America",2,512,2.7,0,"",null,null,null,null,null,null,null,"4113XX0009.png",9,1,2,5,9,4,55,"CE","","","Class II",null,null,null,null,null,0,0,0,null,null,null,null,"4113XX0009.ldt",1,null,null,null,null,0,null,null,null,null,null,null,"LED",16,null,"",null,null,24,null,4000,80,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"","",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"Poland"]
["4114","4114XX0009","LONDON POLE-TOP LED 2000LM 3000K ON/OFF",null,"A luminaire with a classic design, mounted on a lighting pole, with a mounting base of Ø50mm For lighting gardens, parks and other architectural concepts.",null,"London,Big","Post,Head","Europe, Africa, Asia, Australia and Oceania, North America, South America",2,512,2.7,0,"",null,null,null,null,null,null,null,"4114XX0009.png",9,1,2,5,9,4,66,"CE","","","Class II",null,null,null,null,null,0,0,0,null,null,null,null,"4114XX0009.ldt",1,null,null,null,null,0,null,null,null,null,null,null,"LED",16,null,"",null,null,23,null,3000,70,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"","",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"Poland"]
["4116","4116XX0009","LONDON WALL-ARM LED 1100LM 3000K",null,"Wall lamp luminaire with a classic design for general use, Can be mounted on the corners of architectural structures",null,"London","Wall","Europe, Africa, Asia, Australia and Oceania, North America, South America",2,4,0.3,2.5,"",null,null,null,null,null,null,null,"4116XX0009.png",9,1,2,2,2,4,55,"CE","","","Class II",null,null,null,null,null,0,0,0,null,null,null,null,"4116XX0009.ldt",1,null,null,null,null,0,null,null,null,null,null,null,"LED",16,null,"",null,null,23,null,3000,80,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"","",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"Poland"]
["4117","4117XX0009","LONDON WALL-ARM LED 1100LM 4000K",null,"A wall lamp luminaire with a classic design for general use. Can be mounted on the corners of architectural structures.",null,"London","Wall","Europe, Africa, Asia, Australia and Oceania, North America, South America",2,4,0.3,2.5,"",null,null,null,null,null,null,null,"4117XX0009.png",9,1,2,2,2,4,55,"CE","","","Class II",null,null,null,null,null,0,0,0,null,null,null,null,"4117XX0009.ldt",1,null,null,null,null,0,null,null,null,null,null,null,"LED",16,null,"",null,null,24,null,4000,80,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"","",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"Poland"]
["4118","4118XX0009","LONDON WALL-ARM LED 2000LM 3000K",null,"A wall lamp luminaire with a classic design for general use. Can be mounted on the corners of architectural structures.",null,"London,Big","Wall","Europe, Africa, Asia, Australia and Oceania, North America, South America",2,4,0.3,2.5,"",null,null,null,null,null,null,null,"4118XX0009.png",9,1,2,2,2,4,55,"CE","","","Class II",null,null,null,null,null,0,0,0,null,null,null,null,"4118XX0009.ldt",1,null,null,null,null,0,null,null,null,null,null,null,"LED",16,null,"",null,null,23,null,3000,80,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"","",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"Poland"]
["4120","4120XX0009","LONDON POLE-TOP LED 1100LM 3000K",null,"Pole luminaire with a classic design for general use. With appropriate accessories, it can be mounted on the corners of architectural structures as a wall lamp.",null,"London,Big","Post,Head","Europe, Africa, Asia, Australia and Oceania, North America, South America",2,512,2.7,0,"",null,null,null,null,null,null,null,"4120XX0009.png",9,1,2,5,9,4,55,"CE","","","Class II",null,null,null,null,null,0,0,0,null,null,null,null,"4120XX0009.ldt",1,null,null,null,null,0,null,null,null,null,null,null,"LED",16,null,"",null,null,23,null,3000,80,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"","",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"Poland"]
["4121","4121XX0009","LONDON POLE-TOP LED 1100LM 4000K ON/OFF",null,"Pole luminaire with a classic design for general use. With appropriate accessories, it can be mounted on the corners of architectural structures as a wall lamp.",null,"London,Big","Post,Head","Europe, Africa, Asia, Australia and Oceania, North America, South America",2,512,2.7,0,"",null,null,null,null,null,null,null,"4121XX0009.png",9,1,2,5,9,4,55,"CE","","","Class II",null,null,null,null,null,0,0,0,null,null,null,null,"4121XX0009.ldt",1,null,null,null,null,0,null,null,null,null,null,null,"LED",16,null,"",null,null,24,null,4000,80,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"","",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"Poland"]
["4122","4122XX0009","LONDON LIGHT LUMINAIRES POLE LED 2000LM 3000K ON/OFF",null,"A luminaire with a classic design for general use. Designed to be mounted on poles equipped with a terminal.",null,"London,Big","Post/Wall,Head","Europe, Africa, Asia, Australia and Oceania, North America, South America",2,512,2.7,0,"",null,null,null,null,null,null,null,"4122XX0009.png",9,1,2,5,9,4,66,"CE","","","Class II",null,null,null,null,null,0,0,0,null,null,null,null,"4122XX0009.ldt",1,null,null,null,null,0,null,null,null,null,null,null,"LED",16,null,"",null,null,23,null,3000,80,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"","",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"Poland"]
["4126","4126XX0309","LONDON POLE LUMINAIRE. LED 2000LM 3000K ON/OFF",null,"A luminaire with a classic design, mounted on a telescopic lighting pole with adjustable height of 1910...2790 mm For lighting gardens, parks and other architectural concepts.",null,"London,Big","Post,Post complete","Europe, Africa, Asia, Australia and Oceania, North America, South America",2,512,2.7,0,"",null,null,null,null,null,null,null,"4126XX0309.jpg",9,1,2,5,8,4,66,"CE","","","Class II",null,null,null,null,null,0,0,0,null,null,null,null,"4126XX0309.ldt",1,null,null,null,null,0,null,null,null,null,null,null,"LED",16,null,"",null,null,23,null,3000,70,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"","",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"Poland"]
["4136","4136XX0009","LONDON WALL LED 1100LM 3000K",null,"A wall lamp luminaire with a classic design for general use. Can be mounted on the corners of architectural structures.",null,"London,Big","Wall","Europe, Africa, Asia, Australia and Oceania, North America, South America",2,4,0.3,2.5,"",null,null,null,null,null,null,null,"4136XX0009.jpg",9,1,2,2,2,4,55,"CE","","","Class II",null,null,null,null,null,0,0,0,null,null,null,null,"4136XX0009.ldt",1,null,null,null,null,0,null,null,null,null,null,null,"LED",16,null,"",null,null,23,null,3000,80,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"","",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"Poland"]
["4140","4140XX0009","LONDON CEILING-CHAIN 110CM LED 1950LM 3000K ON/OFF",null,"A luminaire on a chain with a classic design. For lighting gardens, terraces and other architectural concepts",null,"London,Big","Ceiling","Europe, Africa, Asia, Australia and Oceania, North America, South America",2,16,0.86,0,"",null,null,null,null,null,null,null,"4140XX0009.jpg",9,1,2,1,4,4,66,"CE","","","Class II",null,null,null,null,null,0,0,0,null,null,null,null,"4140XX0009.ldt",1,null,null,null,null,0,null,null,null,null,null,null,"LED",16,null,"",null,null,23,null,3000,80,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"","",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"Poland"]
["4300","4300XX0009","ASKER POLE-TOP LED 2904LM SCL 3000K DALI2",null,"Pole luminaire with a modern design. Mounted, intended for mounting on a lighting pole with a mounting base of Ø50, Ø60, Ø76 using an appropriate head (accessory)",null,"Asker","Pole","Europe, Africa, Asia, Australia and Oceania, North America, South America",2,512,6,0,"",null,null,null,null,null,null,null,"4300XX0009.jpg",6,1,2,5,9,3,66,"CE","","","Class I",null,null,null,null,null,0.47,0.11,7.0000000000000007E-2,null,null,null,null,"4300XX0009.ldt",1,null,null,null,null,0,null,null,null,null,null,null,"LED",16,null,"",null,null,23,null,3000,70,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"DALI","",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"Poland"]
["4301","4301XX0009","ASKER POLE-TOP LED 3036LM SCL 4000K DALI2",null,"Pole luminaire with a modern design. Mounted, intended for mounting on a lighting pole with a mounting base of Ø 50, Ø 60, Ø 76 using an appropriate head (accessory)",null,"Asker","Pole","Europe, Africa, Asia, Australia and Oceania, North America, South America",2,512,6,0,"",null,null,null,null,null,null,null,"4301XX0009.jpg",6,1,2,5,9,3,66,"CE","","","Class I",null,null,null,null,null,0.47,0.11,7.0000000000000007E-2,null,null,null,null,"4301XX0009.ldt",1,null,null,null,null,0,null,null,null,null,null,null,"LED",16,null,"",null,null,24,null,4000,70,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"DALI","",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"Poland"]
["4302","4302XX0009","ASKER POLE-TOP LED 2904LM VSM 3000K DALI2",null,"Pole luminaire with a modern design. Mounted, intended for mounting on a lighting pole with a mounting base of Ø 50, Ø 60, Ø 76 using an appropriate head (accessory)",null,"Asker","Pole","Europe, Africa, Asia, Australia and Oceania, North America, South America",2,512,6,0,"",null,null,null,null,null,null,null,"4302XX0009.jpg",4,1,2,5,9,3,66,"CE","","","Class I",null,null,null,null,null,0.47,0.11,7.0000000000000007E-2,null,null,null,null,"4302XX0009.ldt",1,null,null,null,null,0,null,null,null,null,null,null,"LED",16,null,"",null,null,23,null,3000,70,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"DALI","",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"Poland"]
["4303","4303XX0009","ASKER POLE-TOP LED 3036LM VSM 4000K DALI2",null,"Pole luminaire with a modern design. Mounted, intended for mounting on a lighting pole with a mounting base of Ø 50, Ø 60, Ø 76 using an appropriate head (accessory)",null,"Asker","Pole","Europe, Africa, Asia, Australia and Oceania, North America, South America",2,512,6,0,"",null,null,null,null,null,null,null,"4303XX0009.jpg",4,1,2,5,9,3,66,"CE","","","Class I",null,null,null,null,null,0.47,0.11,7.0000000000000007E-2,null,null,null,null,"4303XX0009.ldt",1,null,null,null,null,0,null,null,null,null,null,null,"LED",16,null,"",null,null,24,null,4000,70,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"DALI","",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"Poland"]
["4310","4310XX0009","ASKER POLE-TOP LED 6051LM SCL 3000K DALI2",null,"Pole luminaire with a modern design. Mounted, intended for mounting on a lighting pole with a mounting base of Ø50, Ø60, Ø76 using an appropriate head (accessory)",null,"Asker","Pole","Europe, Africa, Asia, Australia and Oceania, North America, South America",2,512,6,0,"",null,null,null,null,null,null,null,"4310XX0009.jpg",6,1,2,5,9,3,66,"CE","","","Class I",null,null,null,null,null,0.47,0.11,7.0000000000000007E-2,null,null,null,null,"4310XX0009.ldt",1,null,null,null,null,0,null,null,null,null,null,null,"LED",16,null,"",null,null,23,null,3000,70,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"DALI","",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"Poland"]
["4311","4311XX0009","ASKER POLE-TOP LED 6342LM SCL 4000K DALI2",null,"Pole luminaire with a modern design. Mounted, intended for mounting on a lighting pole with a mounting base of Ø50, Ø60, Ø76 using an appropriate head (accessory)",null,"Asker","Pole","Europe, Africa, Asia, Australia and Oceania, North America, South America",2,512,6,0,"",null,null,null,null,null,null,null,"4311XX0009.jpg",6,1,2,5,9,3,66,"CE","","","Class I",null,null,null,null,null,0.47,0.11,7.0000000000000007E-2,null,null,null,null,"4311XX0009.ldt",1,null,null,null,null,0,null,null,null,null,null,null,"LED",16,null,"",null,null,24,null,4000,70,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"DALI","",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"Poland"]
["4312","4312XX0009","ASKER POLE-TOP LED 6051LM VSM 3000K DALI2",null,"Pole luminaire with a modern design. Mounted, intended for mounting on a lighting pole with a mounting base of Ø50, Ø60, Ø76 using an appropriate head (accessory)",null,"Asker","Pole","Europe, Africa, Asia, Australia and Oceania, North America, South America",2,512,6,0,"",null,null,null,null,null,null,null,"4312XX0009.jpg",4,1,2,5,9,3,66,"CE","","","Class I",null,null,null,null,null,0.47,0.11,7.0000000000000007E-2,null,null,null,null,"4312XX0009.ldt",1,null,null,null,null,0,null,null,null,null,null,null,"LED",16,null,"",null,null,23,null,3000,70,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"DALI","",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"Poland"]
["4313","4313XX0009","ASKER POLE-TOP LED 6342LM VSM 4000K DALI2",null,"Pole luminaire with a modern design. Mounted, intended for mounting on a lighting pole with a mounting base of Ø50, Ø60, Ø76 using an appropriate head (accessory)",null,"Asker","Pole","Europe, Africa, Asia, Australia and Oceania, North America, South America",2,512,6,0,"",null,null,null,null,null,null,null,"4313XX0009.jpg",4,1,2,5,9,3,66,"CE","","","Class I",null,null,null,null,null,0.47,0.11,7.0000000000000007E-2,null,null,null,null,"4313XX0009.ldt",1,null,null,null,null,0,null,null,null,null,null,null,"LED",16,null,"",null,null,24,null,4000,70,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"DALI","",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"Poland"]
["4322","4322XX0309","ASKER HEAD POLE-TOP LED 2904LM SCL 3000K DALI2",null,"Pole luminaire with a modern design. Intended for mounting on a lighting pole with a Ø 60 mounting shaft",null,"Asker","Pole","Europe, Africa, Asia, Australia and Oceania, North America, South America",2,512,6,0,"",null,null,null,null,null,null,null,"4322XX0309.jpg",6,1,2,5,9,3,66,"CE","","","Class I",null,null,null,null,null,0.47,0.11,7.0000000000000007E-2,null,null,null,null,"4322XX0309.ldt",1,null,null,null,null,0,null,null,null,null,null,null,"LED",16,null,"",null,null,23,null,3000,70,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"DALI","",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"Poland"]
["4323","4323XX0309","ASKER HEAD POLE-TOP LED 3036LM SCL 4000K DALI2",null,"Pole luminaire with a modern design. Intended for mounting on a lighting pole with a Ø 60 mounting shaft",null,"Asker","Pole","Europe, Africa, Asia, Australia and Oceania, North America, South America",2,512,6,0,"",null,null,null,null,null,null,null,"4323XX0309.jpg",6,1,2,5,9,3,66,"CE","","","Class I",null,null,null,null,null,0.47,0.11,7.0000000000000007E-2,null,null,null,null,"4323XX0309.ldt",1,null,null,null,null,0,null,null,null,null,null,null,"LED",16,null,"",null,null,24,null,4000,70,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"DALI","",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"Poland"]
["4332","4332XX0309","ASKER HEAD POLE-TOP LED 6051LM SCL 3000K DALI2",null,"Pole luminaire with a modern design. Intended for mounting on a lighting pole with a Ø 60 mounting shaft",null,"Asker","Pole","Europe, Africa, Asia, Australia and Oceania, North America, South America",2,512,6,0,"",null,null,null,null,null,null,null,"4332XX0309.jpg",6,1,2,5,9,3,66,"CE","","","Class I",null,null,null,null,null,0.47,0.11,7.0000000000000007E-2,null,null,null,null,"4332XX0309.ldt",1,null,null,null,null,0,null,null,null,null,null,null,"LED",16,null,"",null,null,23,null,3000,70,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"DALI","",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"Poland"]
["4333","4333XX0309","ASKER HEAD POLE-TOP LED 6342LM SCL 4000K DALI2",null,"Pole luminaire with a modern design. Intended for mounting on a lighting pole with a Ø 60 mounting shaft",null,"Asker","Pole","Europe, Africa, Asia, Australia and Oceania, North America, South America",2,512,6,0,"",null,null,null,null,null,null,null,"4333XX0309.jpg",6,1,2,5,9,3,66,"CE","","","Class I",null,null,null,null,null,0.47,0.11,7.0000000000000007E-2,null,null,null,null,"4333XX0309.ldt",1,null,null,null,null,0,null,null,null,null,null,null,"LED",16,null,"",null,null,24,null,4000,70,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"DALI","",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"Poland"]
["4362","4362XX0309","ASKER HEAD POLE-TOP LED 2904LM VSM 3000K DALI2",null,"Pole luminaire with a modern design. Intended for mounting on a lighting pole with a Ø 60 mounting shaft",null,"Asker","Pole","Europe, Africa, Asia, Australia and Oceania, North America, South America",2,512,6,0,"",null,null,null,null,null,null,null,"4362XX0309.jpg",4,1,2,5,9,3,66,"CE","","","Class I",null,null,null,null,null,0.47,0.11,7.0000000000000007E-2,null,null,null,null,"4362XX0309.ldt",1,null,null,null,null,0,null,null,null,null,null,null,"LED",16,null,"",null,null,23,null,3000,70,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"DALI","",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"Poland"]
["4363","4363XX0309","ASKER HEAD POLE-TOP LED 3036LM VSM 4000K DALI2",null,"Pole luminaire with a modern design. Intended for mounting on a lighting pole with a Ø 60 mounting shaft",null,"Asker","Pole","Europe, Africa, Asia, Australia and Oceania, North America, South America",2,512,6,0,"",null,null,null,null,null,null,null,"4363XX0309.jpg",4,1,2,5,9,3,66,"CE","","","Class I",null,null,null,null,null,0.47,0.11,7.0000000000000007E-2,null,null,null,null,"4363XX0309.ldt",1,null,null,null,null,0,null,null,null,null,null,null,"LED",16,null,"",null,null,24,null,4000,70,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"DALI","",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"Poland"]
["4372","4372XX0309","ASKER HEAD POLE-TOP LED 6051LM VSM 3000K DALI2",null,"Pole luminaire with a modern design. Intended for mounting on a lighting pole with a Ø 60 mounting shaft",null,"Asker","Pole","Europe, Africa, Asia, Australia and Oceania, North America, South America",2,512,6,0,"",null,null,null,null,null,null,null,"4372XX0309.jpg",4,1,2,5,9,3,66,"CE","","","Class I",null,null,null,null,null,0.47,0.11,7.0000000000000007E-2,null,null,null,null,"4372XX0309.ldt",1,null,null,null,null,0,null,null,null,null,null,null,"LED",16,null,"",null,null,23,null,3000,70,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"DALI","",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"Poland"]
["4373","4373XX0309","ASKER HEAD POLE-TOP LED 6342LM VSM 4000K DALI2",null,"Pole luminaire with a modern design. Intended for mounting on a lighting pole with a Ø 60 mounting shaft",null,"Asker","Pole","Europe, Africa, Asia, Australia and Oceania, North America, South America",2,512,6,0,"",null,null,null,null,null,null,null,"4373XX0309.jpg",4,1,2,5,9,3,66,"CE","","","Class I",null,null,null,null,null,0.47,0.11,7.0000000000000007E-2,null,null,null,null,"4373XX0309.ldt",1,null,null,null,null,0,null,null,null,null,null,null,"LED",16,null,"",null,null,24,null,4000,70,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"DALI","",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"Poland"]
["450","450XX0009","VASA WALL LED 799LM DOWN 3000K DIM.",null,"A luminaire with a wide range of applications, including lighting: wall surfaces and other architectural concepts",null,"Vasa","Wall","Europe, Africa, Asia, Australia and Oceania, North America, South America",2,4,0,2.5,"",null,null,null,null,null,null,null,"450XX0009.png",7,1,5,2,2,1,66,"CE","","IK08","Class I",null,null,null,null,null,0.31,0.12,0.16,null,null,null,null,"450XX0009.ldt",1,null,null,null,null,0,null,null,null,null,null,null,"LED",16,null,"",null,null,23,null,3000,80,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"","",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"Poland"]
["454","454XX0009","VASA WALL LED 799LM UP 3000K DIM.",null,"A luminaire with a wide range of applications, including lighting: wall surfaces and other architectural concepts",null,"Vasa","Wall","Europe, Africa, Asia, Australia and Oceania, North America, South America",2,4,0,2.5,"",null,null,null,null,null,null,null,"454XX0009.jpg",7,1,5,2,2,1,66,"CE","","IK08","Class I",null,null,null,null,null,0.31,0.12,0.16,null,null,null,null,"454XX0009.ldt",1,null,null,null,null,2,null,null,null,null,null,null,"LED",16,null,"",null,null,23,null,3000,80,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"","",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"Poland"]
["5002","5002XX0309",{"$f":"INDEX(DB,MATCH($A440,ID,0),3)","v":"VISBY POLE-TOP 2XLED 5200LM 4000K"},null,"Pole top luminaire for installation on a lighting pole with Ø60mm mounting shaft.",null,"Visby",{"$f":"IF(INDEX(DB,MATCH($A440,ID,0),5)=0,\"\",INDEX(DB,MATCH($A440,ID,0),5))","v":"Post,Head"},"Europe, Africa, Asia, Australia and Oceania, North America, South America",2,{"$f":"IFERROR(INDEX(TYPMONT,MATCH((INDEX(DB,MATCH($A440,ID,0),31)),ID_RODZ,0),3),\"\")","v":512},3.67,0,{"$f":"IFERROR(IF(INDEX(TYPMONT,MATCH((INDEX(DB,MATCH($A440,ID,0),31)),ID_RODZ,0),6)=0,\"\",INDEX(TYPMONT,MATCH((INDEX(DB,MATCH($A440,ID,0),31)),ID_RODZ,0),6)),\"\")","v":""},null,null,null,null,null,null,null,{"$f":"IF(INDEX(DB,MATCH($A440,ID,0),57)=0,\"\",INDEX(DB,MATCH($A440,ID,0),57))","v":"5002XX0309.jpg"},9,{"$f":"IF(INDEX(DB,MATCH($A440,ID,0),61)=0,\"\",INDEX(DB,MATCH($A440,ID,0),61))","v":1},1,{"$f":"IFERROR(INDEX(TYPMONT,MATCH((INDEX(DB,MATCH($A440,ID,0),31)),ID_RODZ,0),1),\"\")","v":5},{"$f":"IFERROR(INDEX(TYPMONT,MATCH((INDEX(DB,MATCH($A440,ID,0),31)),ID_RODZ,0),2),\"\")","v":9},{"$f":"IF(INDEX(DB,MATCH($A440,ID,0),59)=0,\"\",INDEX(DB,MATCH($A440,ID,0),59))","v":4},{"$f":"IFERROR(IF(INDEX(DB,MATCH($A440,ID,0),19)=0,\"\",INDEX(DB,MATCH($A440,ID,0),19)+1),\"\")","v":66},{"$f":"IF(INDEX(DB,MATCH($A440,ID,0),27)=0,\"\",INDEX(DB,MATCH($A440,ID,0),27))","v":"CE"},"",{"$f":"IF(INDEX(DB,MATCH($A440,ID,0),20)=0,\"\",INDEX(DB,MATCH($A440,ID,0),20))","v":""},{"$f":"IF(INDEX(DB,MATCH($A440,ID,0),21)=0,\"\",INDEX(DB,MATCH($A440,ID,0),21))","v":"Class I"},null,null,null,null,null,0,0,0,null,null,null,null,{"$f":"IF(INDEX(DB,MATCH($A440,ID,0),58)=0,\"\",INDEX(DB,MATCH($A440,ID,0),58))","v":"5002XX0309.ldt"},1,null,null,null,null,0,null,null,null,null,null,null,"LED",16,null,{"$f":"IF(INDEX(DB,MATCH($A440,ID,0),60)=0,\"\",INDEX(DB,MATCH($A440,ID,0),60))","v":""},null,null,24,null,{"$f":"IF(INDEX(DB,MATCH($A440,ID,0),22)=0,\"\",INDEX(DB,MATCH($A440,ID,0),22))","v":4000},{"$f":"IF(INDEX(DB,MATCH($A440,ID,0),53)=0,\"\",INDEX(DB,MATCH($A440,ID,0),53))","v":80},null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,{"$f":"IF(INDEX(DB,MATCH($A440,ID,0),29)=0,\"\",INDEX(DB,MATCH($A440,ID,0),29))","v":""},{"$f":"IF(INDEX(DB,MATCH($A440,ID,0),28)=0,\"\",INDEX(DB,MATCH($A440,ID,0),28))","v":""},null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"Poland"]
["5003","5003XX0309","VISBY POLE-TOP LED 3150LM 4000K",null,"Pole top luminaire for installation on a lighting pole with Ø60mm mounting shaft.",null,{"$f":"IF(INDEX(DB,MATCH($A441,ID,0),4)=0,\"\",INDEX(DB,MATCH($A441,ID,0),4))","v":"Visby"},"Post,Head","Europe, Africa, Asia, Australia and Oceania, North America, South America",2,512,3.67,0,"",null,null,null,null,null,null,null,"5003XX0309.jpg",9,1,1,5,9,4,66,"CE",{"$f":"IFERROR(IF(FIND(\"RENA\",$C441)>0,\"Vehicle resistant\",\"\"),\"\")","v":""},"","Class I",null,null,null,null,null,0,0,0,null,null,null,null,"5003XX0309.ldt",1,null,null,null,null,0,null,null,null,null,null,null,"LED",16,null,"",null,null,{"$f":"IF($BO441=4000,24,23)","v":24},null,4000,80,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"","",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"Poland"]
["5004","5004XX0012","KOSTER WALL-ARM LED 2050LM 4000K ON/OFF",null,"Classic type wall-mounted luminaire. Possibility to install on corners of architectural objects.",null,"Koster","Wall","Europe, Africa, Asia, Australia and Oceania, North America, South America",2,4,0.22,2.5,"",null,null,null,null,null,null,null,"5004XX0012.jpg",3,1,1,2,2,4,55,"CE","","IK10","Class I",null,null,null,null,null,0,0,0,null,null,null,null,"5004XX0012.ldt",1,null,null,null,null,0,null,null,null,null,null,null,"LED",16,null,"",null,null,24,null,4000,80,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"","",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"Poland"]
["5006","5006XX0011","KOSTER POLE-TOP LED 2050LM 4000K",null,"Luminaire mounted on a straight arm, for assembly on a telescopic lighting pole with a diameter of Ø60mm.",null,"Koster","Post,Head","Europe, Africa, Asia, Australia and Oceania, North America, South America",2,512,4,0,"",null,null,null,null,null,null,null,"5006XX0011.jpg",3,1,1,5,9,4,55,"CE","","IK10","Class I",null,null,null,null,null,0.45,0.24,0.24,null,null,null,null,"5006XX0011.ldt",1,null,null,null,null,0,null,null,null,null,null,null,"LED",16,null,"",null,null,24,null,4000,80,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"","",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"Poland"]
["5007","5007XX0309","KOSTER POLE-TOP LED 2050LM 4000K",null,"Classic design luminaire, mounted on a telescopic lighting pole. Adjustable height 2360..3360mm.",null,"Koster","Post,Post complete","Europe, Africa, Asia, Australia and Oceania, North America, South America",2,512,4,0,"",null,null,null,null,null,null,null,"5007XX0309.jpg",3,1,1,5,9,4,55,"CE","","IK10","Class I",null,null,null,null,null,0.45,0.24,0.24,null,null,null,null,"5007XX0309.ldt",1,null,null,null,null,0,null,null,null,null,null,null,"LED",16,null,"",null,null,24,null,4000,80,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"","",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"Poland"]
["5008","5008XX0011","STAVANGER BOLLARD 95CM LED 1171LM 4000K DIM.",null,"Bollard luminaire of stable and durable construction For lighting private areas and public spaces",null,"Stavanger","Bollard","Europe, Africa, Asia, Australia and Oceania, North America, South America",2,2,0.9,0,"",null,null,null,null,null,null,null,"5008XX0011.jpg",9,1,1,3,6,1,66,"CE","","IK10","Class I",null,null,null,null,null,0.2,0.2,0.95,null,null,null,null,"5008XX0011.ldt",1,null,null,null,null,0,null,null,null,null,null,null,"LED",16,null,"",null,null,24,null,4000,80,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"","",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"Poland"]
["5009","5009XX0010","STAVANGER BOLLARD 50CM LED 1171LM 4000K DIM.",null,"Bollard luminaire of stable and durable construction. For lighting private areas and public spaces.",null,"Stavanger","Bollard","Europe, Africa, Asia, Australia and Oceania, North America, South America",2,2,0.45,0,"",null,null,null,null,null,null,null,"5009XX0010.jpg",9,1,1,3,6,1,66,"CE","","IK10","Class I",null,null,null,null,null,0.2,0.2,0.5,null,null,null,null,"5009XX0010.ldt",1,null,null,null,null,0,null,null,null,null,null,null,"LED",16,null,"",null,null,24,null,4000,80,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"","",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"Poland"]
["5010","5010XX0011","STAVANGER BOLLARD 28CM LED 854LM 4000K DIM.",null,"Bollard luminaire of stable and durable construction. For lighting private areas and public spaces.",null,"Stavanger","Bollard","Europe, Africa, Asia, Australia and Oceania, North America, South America",2,2,0.23,0,"",null,null,null,null,null,null,null,"5010XX0011.jpg",9,1,1,3,6,1,66,"CE","","IK10","Class I",null,null,null,null,null,0.2,0.2,0.28000000000000003,null,null,null,null,"5010XX0011.ldt",1,null,null,null,null,0,null,null,null,null,null,null,"LED",16,null,"",null,null,24,null,4000,80,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"","",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"Poland"]
["5011","5011XX0016","NAMSOS WALL-RECESSED LED 1247LM 4000K DIM.",null,"The luminaire is adapted to illuminate stairs, steps, staircases, pathways, ceiling lighting and implementation of other architectural concepts",null,"Namsos","Recessed","Europe, Africa, Asia, Australia and Oceania, North America, South America",2,64,0,0.5,"",null,null,null,null,null,null,null,"5011XX0016.jpg",7,1,2,2,1,1,66,"CE","","IK08","Class I",null,null,null,null,null,0.22,0.22,0.12,null,null,null,null,"5011XX0016.ldt",1,null,null,null,null,4,null,null,null,null,null,null,"LED",16,null,"",null,null,24,null,4000,80,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"","",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"Poland"]
["5012","5012XX0014","NAMSOS BOLLARD 95CM LED 1247LM 4000K DIM.",null,"Luminaire with a modern design. For lighting gardens and other private and public areas",null,"Namsos","Bollard","Europe, Africa, Asia, Australia and Oceania, North America, South America",2,2,0.83,0,"",null,null,null,null,null,null,null,"5012XX0014.jpg",7,1,2,3,6,1,66,"CE","","IK08","Class I",null,null,null,null,null,0.24,0.12,0.95,null,null,null,null,"5012XX0014.ldt",1,null,null,null,null,1,null,null,null,null,null,null,"LED",16,null,"",null,null,24,null,4000,80,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"","",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"Poland"]
["5013","5013XX0013","NAMSOS BOLLARD 65CM LED 1247LM 4000K DIM.",null,"Luminaire with a modern design. For lighting gardens and other private and public areas",null,"Namsos","Bollard","Europe, Africa, Asia, Australia and Oceania, North America, South America",2,2,0.53,0,"",null,null,null,null,null,null,null,"5013XX0013.jpg",7,1,2,3,6,1,66,"CE","","IK08","Class I",null,null,null,null,null,0.24,0.12,0.65,null,null,null,null,"5013XX0013.ldt",1,null,null,null,null,1,null,null,null,null,null,null,"LED",16,null,"",null,null,24,null,4000,80,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"","",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"Poland"]
["5014","5014XX0013","EGERSUND BOLLARD 108CM LED 2655LM 4000K DIM.",null,"Contemporary design luminaire. For lighting gardens and other private and public spaces",null,"Egersund","Bollard","Europe, Africa, Asia, Australia and Oceania, North America, South America",2,2,1.04,0,"",null,null,null,null,null,null,null,"5014XX0013.jpg",3,1,1,3,6,1,66,"CE","","IK08","Class II",null,null,null,null,null,0.2,0.2,1.08,null,null,null,null,"5014XX0013.ldt",1,null,null,null,null,1,null,null,null,null,null,null,"LED",16,null,"",null,null,24,null,4000,80,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"","",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"Poland"]
["5015","5015XX0012","EGERSUND BOLLARD 63CM LED 2655LM 4000K DIM.",null,"Luminaire with a contemporary design. For lighting gardens and other private and public areas",null,"Egersund","Bollard","Europe, Africa, Asia, Australia and Oceania, North America, South America",2,2,0.59,0,"",null,null,null,null,null,null,null,"5015XX0012.jpg",3,1,1,3,6,1,66,"CE","","IK08","Class II",null,null,null,null,null,0.2,0.2,0.63,null,null,null,null,"5015XX0012.ldt",1,null,null,null,null,1,null,null,null,null,null,null,"LED",16,null,"",null,null,24,null,4000,80,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"","",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"Poland"]
["5016","5016XX0015","NORDLAND CEILING/WALL LED 594LM 4000K DIM.",null,"A ceiling-type luminaire with a modern design For lighting private areas and other architectural concepts",null,"Nordland","Wall,Ceiling","Europe, Africa, Asia, Australia and Oceania, North America, South America",2,4,0,2.5,"Ceiling mounted",null,null,null,null,null,null,null,"5016XX0015.jpg",8,1,2,2,2,1,66,"CE","","IK10","Class I",null,null,null,null,null,0.28000000000000003,0.28000000000000003,0.1,null,null,null,null,"5016XX0015.ldt",1,null,null,null,null,0,null,null,null,null,1,null,"LED",16,null,"",null,null,24,null,4000,80,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"","",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"Poland"]
["5018","5018XX0013","ASKER BIG WALL 2XLED 1188LM UP-DOWN 4000K DIM.",null,"A luminaire with a wide range of applications, for illuminating wall surfaces, facades and other architectural concepts",null,"Asker,Big","Wall","Europe, Africa, Asia, Australia and Oceania, North America, South America",2,4,0,2.5,"",null,null,null,null,null,null,null,"5018XX0013.jpg",8,1,2,2,2,1,66,"CE","","IK08","Class I",null,null,null,null,null,0.3,0.12,0.12,null,null,null,null,"5018XX0013.ldt",1,null,null,null,null,1,null,null,null,null,null,null,"LED",16,null,"",null,null,24,null,4000,80,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"","",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"Poland"]
["5019",{"$f":"INDEX(DB,MATCH($A455,ID,0),2)","v":"5019XX0013"},"VASA WALL 2XLED 1188LM UP-DOWN 4000K DIM.",null,{"$f":"IF(INDEX(DB,MATCH($A455,ID,0),35)=0,\"\",INDEX(DB,MATCH($A455,ID,0),35))","v":"A luminaire with a wide range of applications, for lighting: wall and facade surfaces and other architectural concepts"},null,"Vasa","Wall","Europe, Africa, Asia, Australia and Oceania, North America, South America",2,4,0,2.5,"",null,null,null,null,null,null,null,"5019XX0013.jpg",{"$f":"IF((IFERROR(INDEX(BRYLA_FOTO,MATCH(INDEX(DB,MATCH($A455,ID,0),62),ID_BRYLAFOTO,0),6),\"\"))<>0,IFERROR(INDEX(BRYLA_FOTO,MATCH(INDEX(DB,MATCH($A455,ID,0),62),ID_BRYLAFOTO,0),6),\"\"),\"\")","v":8},1,5,2,2,1,66,"CE","","IK08","Class I",null,null,null,null,null,{"$f":"INDEX(DB,MATCH($A455,ID,0),24)","v":0},{"$f":"INDEX(DB,MATCH($A455,ID,0),25)","v":0},{"$f":"INDEX(DB,MATCH($A455,ID,0),26)","v":0},null,null,null,null,"5019XX0013.ldt",1,null,null,null,null,1,null,null,null,null,null,null,"LED",16,null,"",null,null,24,null,4000,80,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"","",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"Poland"]
["5020","5020XX0013","HALDEN WALL LED 1121LM DOWN 4000K DIM.",null,"Luminaire with a wide range of applications for example for illumination of walls and facade surfaces or any other architectural concepts.",null,"Halden","Wall","Europe, Africa, Asia, Australia and Oceania, North America, South America",2,4,0,2.5,"",null,null,null,null,null,null,null,"5020XX0013.jpg",7,1,5,2,2,1,66,"CE","","IK10","Class I",null,null,null,null,null,3.1,1.55,1.5,null,null,null,null,"5020XX0013.ldt",{"$f":"IF($BJ456=\"\",1,0)","v":1},null,null,null,null,0,null,null,null,null,null,null,"LED",16,null,"",null,null,24,null,4000,80,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"","",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"Poland"]
["5021","5021XX0012","ALTA BOLLARD 85CM LED 1164LM 4000K DIM.",null,"A bollard luminaire with a stable and durable structure. For lighting private areas and public areas",null,"Alta","Bollard","Europe, Africa, Asia, Australia and Oceania, North America, South America",2,2,0.7,0,"",null,null,null,null,null,null,null,"5021XX0012.jpg",7.3,1,1,3,6,1,66,"CE","","","Class I",null,null,null,null,null,0,0,0,null,null,null,null,"5021XX0012.ldt",1,null,null,null,null,1,null,null,null,null,null,null,"LED",16,null,"",null,null,24,null,4000,80,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"","",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"Poland"]
["5022","5022XX0013","HALMSTAD BOLLARD 85CM LED 1121LM 4000K DIM.",null,"A bollard luminaire with a stable and durable structure For lighting private areas and other architectural concepts",null,"Halmstad","Bollard","Europe, Africa, Asia, Australia and Oceania, North America, South America",2,2,0.7,0,"",null,null,null,null,null,null,null,"5022XX0013.jpg",7,1,2,3,6,1,66,"CE","","IK10","Class II",null,null,null,null,null,0,0,0,null,null,null,null,"5022XX0013.ldt",1,null,null,null,null,1,null,null,null,null,null,null,"LED",16,null,"",null,null,24,null,4000,80,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"","",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"Poland"]
["5023","5023XX0012","STOCKHOLM BOLLARD 85CM LED 1164LM 4000K DIM.",null,"Bollard luminaire of stable and durable construction. For lighting private areas and public spaces.",null,"Stockholm","Bollard","Europe, Africa, Asia, Australia and Oceania, North America, South America",2,2,0.68,{"$f":"IF(K459=4,2.5,IF(K459=64,0.5,0))","v":0},"",null,null,null,null,null,null,null,"5023XX0012.jpg",7,1,1,3,6,1,66,"CE","","IK10","Class I",null,null,null,null,null,0,0,0,null,null,null,null,"5023XX0012.ldt",1,null,null,null,null,1,null,null,null,null,null,null,"LED",16,null,"",null,null,24,null,4000,80,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"","",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"Poland"]
["5024","5024XX0016","NARVIK BOLLARD LED 3264LM 4000K ON/OFF",null,"A bollard luminaire with a stable and durable structure. For lighting private and public areas",null,"Narvik","Bollard","Europe, Africa, Asia, Australia and Oceania, North America, South America",2,2,0.7,0,"",null,null,null,null,null,null,null,"5024XX0016.jpg",4,1,1,3,6,4,66,"CE","","IK10","Class I",null,null,null,null,null,0.24,0.24,0.95,null,null,null,null,"5024XX0016.ldt",1,null,null,null,null,0,null,null,null,null,null,null,"LED",16,null,"",null,null,24,null,4000,80,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"","",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"Poland"]
["5028","5028XX0016","LILLEHAMMER WALL 2XLED 1069LM UP60º & DOWN60º 4000K DIM.",null,"A luminaire with a wide range of applications, including for lighting: wall surfaces and facades as well as other architectural concepts",null,"Lillehammer","Wall","Europe, Africa, Asia, Australia and Oceania, North America, South America",2,4,0,2.5,"",null,null,null,null,null,null,null,"5028XX0016.jpg",10,1,2,2,2,1,66,"CE","","IK08","Class I",null,null,null,null,null,0.18,0.11,0.08,null,null,null,null,"5028XX0016.ldt",1,null,null,null,null,1,null,null,null,null,null,null,"LED",16,null,"",null,null,24,null,4000,80,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"","",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"Poland"]
["5029","5029XX0016","LILLEHAMMER WALL LED 534LM DOWN60º 4000K DIM.",null,"A luminaire with a wide range of applications, including lighting wall surfaces, facades and other architectural concepts",null,"Lillehammer","Wall","Europe, Africa, Asia, Australia and Oceania, North America, South America",2,4,0,2.5,"",null,null,null,null,null,null,null,"5029XX0016.jpg",10,1,2,2,2,1,66,"CE","","IK08","Class I",null,null,null,null,null,0.18,0.11,0.08,null,null,null,null,"5029XX0016.ldt",1,null,null,null,null,0,null,null,null,null,null,null,"LED",16,null,"",null,null,24,null,4000,80,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"","",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"Poland"]
["5030","5030XX0017","LILLEHAMMER WALL 2XLED 1069LM UP4º & DOWN4º 4000K DIM.",null,"A luminaire with a wide range of applications, including lighting: wall surfaces, facades and other architectural concepts",null,"Lillehammer","Wall","Europe, Africa, Asia, Australia and Oceania, North America, South America",2,4,0,2.5,"",null,null,null,null,null,null,null,"5030XX0017.jpg",10,1,2,2,2,1,66,"CE","","IK08","Class I",null,null,null,null,null,0.18,0.11,0.08,null,null,null,null,"5030XX0017.ldt",1,null,null,null,null,1,null,null,null,null,null,null,"LED",16,null,"",null,null,24,null,4000,80,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"","",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"Poland"]
["5031","5031XX0017","LILLEHAMMER WALL LED 534LM DOWN 4º 4000K DIM.",null,"A luminaire with a wide range of applications, including lighting wall surfaces, facades and other architectural concepts",null,"Lillehammer","Wall","Europe, Africa, Asia, Australia and Oceania, North America, South America",2,4,0,2.5,"",null,null,null,null,null,null,null,"5031XX0017.jpg",10,1,2,2,2,1,66,"CE","","IK08","Class I",null,null,null,null,null,0.18,0.11,0.08,null,null,null,null,"5031XX0017.ldt",1,null,null,null,null,0,null,null,null,null,null,null,"LED",16,null,"",null,null,24,null,4000,80,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"","",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"Poland"]
["5032","5032XX0B10","VOSS WALL 3XLED 2301LM 4000K ON/OFF",null,"A luminaire with a wide range of applications, for lighting: wall and facade surfaces and other architectural concepts",null,"Voss","Wall","Europe, Africa, Asia, Australia and Oceania, North America, South America",2,4,0,2.5,"",null,null,null,null,null,null,null,"5032XX0B10.jpg",10,1,2,2,2,4,55,"CE","","IK06","Class I",null,null,null,null,null,0.18,0.16,0.27,null,null,null,null,"5032XX0B10.ldt",1,null,null,null,null,1,null,null,null,null,null,null,"LED",16,null,"",null,null,24,null,4000,80,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"","",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"Poland"]
["5033","5033XX0F10","VOSS WALL 4XLED 3068LM 4000K ON/OFF",null,"A luminaire with a wide range of applications, for lighting: walls, facades surfaces, and other architectural concepts",null,"Voss","Wall","Europe, Africa, Asia, Australia and Oceania, North America, South America",2,4,0,2.5,"",null,null,null,null,null,null,null,"5033XX0F10.jpg",10,1,2,2,2,4,55,"CE","","IK06","Class I",null,null,null,null,null,0.18,0.16,0.27,null,null,null,null,"5033XX0F10.ldt",1,null,null,null,null,1,null,null,null,null,null,null,"LED",16,null,"",null,null,24,null,4000,80,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"","",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"Poland"]
["5038","5038XX0013","PARIS SMALL WALL LED 681LM DOWN 4000K DIM.",null,"Classic and simple design luminaire with a wide range of applications",null,"Paris","Wall","Europe, Africa, Asia, Australia and Oceania, North America, South America",2,4,0,2.5,"",null,null,null,null,null,null,null,"5038XX0013.jpg",7,1,5,2,2,1,44,"CE","","","Class I",null,null,null,null,null,0.23,0.12,0.14000000000000001,null,null,null,null,"5038XX0013.ldt",1,null,null,null,null,0,null,null,null,null,null,null,"LED",16,null,"",null,null,24,null,4000,80,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"","",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"Poland"]
["5039","5039XX0013","PARIS WALL LED 683LM DOWN 4000K DIM.",null,"Classic design luminaire with a wide range of applications for example for illumination of walls and facade surfaces or any other architectural concepts.",null,"Paris,Big","Wall","Europe, Africa, Asia, Australia and Oceania, North America, South America",2,4,0,2.5,"",null,null,null,null,null,null,null,"5039XX0013.jpg",7,1,5,2,2,1,44,"CE","","","Class I",null,null,null,null,null,0,0,0,null,null,null,null,"5039XX0013.ldt",1,null,null,null,null,0,null,null,null,null,null,null,"LED",16,null,"",null,null,24,null,4000,80,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"","",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"Poland"]
["5045","5045XX0010","NORDLAND CEILING/WALL LED 2050LM 4000K MD",null,"Luminaire with modern design. Equipped with a motion sensor with a twilight switch and movement sustain sensor",null,"Nordland","Wall","Europe, Africa, Asia, Australia and Oceania, North America, South America",2,4,0,2.5,"Ceiling mounted",null,null,null,null,null,null,null,"5045XX0010.jpg",8,1,2,2,2,3,66,"CE","","IK10","Class I",null,null,null,null,null,0.28000000000000003,0.28000000000000003,0.1,null,null,null,null,"5045XX0010.ldt",1,null,null,null,null,0,null,null,null,null,1,null,"LED",16,null,"",null,null,24,null,4000,80,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"","Daylight sensor,Motion sensor",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"Poland"]
["5046","5046XX0009","NORDLAND CEILING/WALL LED 1419LM 3000K DIM.",null,"A ceiling-type luminaire with a modern design For lighting private areas and other architectural concepts",null,"Nordland","Wall,Ceiling","Europe, Africa, Asia, Australia and Oceania, North America, South America",2,4,0,2.5,"Ceiling mounted",null,null,null,null,null,null,null,"5046XX0009.jpg",8,1,2,2,2,1,66,"CE","","IK10","Class I",null,null,null,null,null,2.8,2.8,0.95,null,null,null,null,"5046XX0009.ldt",1,null,null,null,null,0,null,null,null,null,1,null,"LED",16,null,"",null,null,23,null,3000,80,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"","",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"Poland"]
["5047","5047XX0009","NORDLAND CEILING/WALL LED 1467LM 4000K DIM.",null,"A ceiling-type luminaire with a modern design For lighting private areas and other architectural concepts",null,"Nordland","Wall,Ceiling","Europe, Africa, Asia, Australia and Oceania, North America, South America",2,4,0,2.5,"Ceiling mounted",null,null,null,null,null,null,null,"5047XX0009.jpg",8,1,2,2,2,1,66,"CE","","IK10","Class I",null,null,null,null,null,2.8,2.8,0.95,null,null,null,null,"5047XX0009.ldt",1,null,null,null,null,0,null,null,null,null,1,null,"LED",16,null,"",null,null,24,null,4000,80,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"","",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"Poland"]
["5060","5060XX0010","STAVANGER BOLLARD 95CM LED 1171LM 4000K DALI2",null,"A bollard luminaire with a stable and durable structure For lighting private and public areas",null,"Stavanger","Bollard","Europe, Africa, Asia, Australia and Oceania, North America, South America",2,2,0.9,0,"",null,null,null,null,null,null,null,"5060XX0010.jpg",9,1,1,3,6,3,66,"CE","","IK10","Class I",null,null,null,null,null,0.2,0.2,0.95,null,null,null,null,"5060XX0010.ldt",1,null,null,null,null,0,null,null,null,null,null,null,"LED",16,null,"",null,null,24,null,4000,80,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"DALI","",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"Poland"]
["5061","5061XX0010","STAVANGER BOLLARD 50CM LED 1171LM 4000K DALI2",null,"A bollard luminaire with a stable and durable structure. For lighting private and public areas",null,"Stavanger","Bollard","Europe, Africa, Asia, Australia and Oceania, North America, South America",2,2,0.45,0,"",null,null,null,null,null,null,null,"5061XX0010.jpg",9,1,1,3,6,3,66,"CE","","IK08","Class I",null,null,null,null,null,0.2,0.2,0.5,null,null,null,null,"5061XX0010.ldt",1,null,null,null,null,0,null,null,null,null,null,null,"LED",16,null,"",null,null,24,null,4000,80,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"DALI","",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"Poland"]
["5062","5062XX0009","STAVANGER BOLLARD 28CM LED 1092LM 4000K DALI",null,"A bollard luminaire with a stable and durable structure. For lighting gardens, private areas and other architectural applications",null,"Stavanger","Bollard","Europe, Africa, Asia, Australia and Oceania, North America, South America",2,2,0.23,0,"",null,null,null,null,null,null,null,"5062XX0009.jpg",9,1,1,3,6,3,66,"CE","","IK08","Class I",null,null,null,null,null,0.2,0.2,0.28000000000000003,null,null,null,null,"5062XX0009.ldt",1,null,null,null,null,0,null,null,null,null,null,null,"LED",16,null,"",null,null,24,null,4000,80,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"DALI","",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"Poland"]
["5063","5063XX0010","STAVANGER BOLLARD 95CM LED 1179LM 3000K DALI2",null,"Bollard luminaire of stable and durable construction For lighting private areas and public spaces",null,"Stavanger","Bollard","Europe, Africa, Asia, Australia and Oceania, North America, South America",2,2,0.9,0,"",null,null,null,null,null,null,null,"5063XX0010.jpg",9,1,1,3,6,3,66,"CE","","IK08","Class I",null,null,null,null,null,0.2,0.2,0.95,null,null,null,null,"5063XX0010.ldt",1,null,null,null,null,0,null,null,null,null,null,null,"LED",16,null,"",null,null,23,null,3000,80,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"DALI","",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"Poland"]
["5065","5065XX0009","STAVANGER BOLLARD 28CM LED 854LM 3000K DALI",null,"A bollard luminaire with a stable and durable structure, For lighting private areas and public areas",null,"Stavanger","Bollard","Europe, Africa, Asia, Australia and Oceania, North America, South America",2,2,0.23,0,"",null,null,null,null,null,null,null,"5065XX0009.jpg",9,1,1,3,6,3,66,"CE","","","Class I",null,null,null,null,null,0.2,0.2,0.28000000000000003,null,null,null,null,"5065XX0009.ldt",1,null,null,null,null,0,null,null,null,null,null,null,"LED",16,null,"",null,null,23,null,3000,80,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"DALI","",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"Poland"]
["5066","5066XX0011","EGERSUND BOLLARD 108CM LED 2655LM 4000K DALI2",null,"Luminaire with a contemporary design. For lighting gardens and other private and public areas",null,"Egersund","Bollard","Europe, Africa, Asia, Australia and Oceania, North America, South America",2,2,1.04,0,"",null,null,null,null,null,null,null,"5066XX0011.jpg",3,1,1,3,6,3,66,"CE","","IK08","Class I",null,null,null,null,null,0.2,0.2,1.08,null,null,null,null,"5066XX0011.ldt",1,null,null,null,null,1,null,null,null,null,null,null,"LED",16,null,"",null,null,24,null,4000,80,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"DALI","",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"Poland"]
["5068","5068XX0011","EGERSUND BOLLARD 108CM LED 2617LM 3000K DALI2",null,"Luminaire with a contemporary design. For lighting gardens and other private and public areas",null,"Egersund","Bollard","Europe, Africa, Asia, Australia and Oceania, North America, South America",2,2,1.04,0,"",null,null,null,null,null,null,null,"5068XX0011.jpg",3,1,1,3,6,3,66,"CE","","IK08","Class I",null,null,null,null,null,0.2,0.2,1.08,null,null,null,null,"5068XX0011.ldt",1,null,null,null,null,1,null,null,null,null,null,null,"LED",16,null,"",null,null,23,null,3000,80,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"DALI","",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"Poland"]
["5069","5069XX0010","EGERSUND BOLLARD 63CM 5XLED 2434LM 3000K DALI2",null,"Luminaire with contemporary design. For lighting gardens and other private and public areas",null,"Egersund","Bollard","Europe, Africa, Asia, Australia and Oceania, North America, South America",2,2,0.59,0,"",null,null,null,null,null,null,null,"5069XX0010.jpg",3,1,1,3,6,3,66,"CE","","IK08","Class I",null,null,null,null,null,0.2,0.2,0.63,null,null,null,null,"5069XX0010.ldt",1,null,null,null,null,1,null,null,null,null,null,null,"LED",16,null,"",null,null,23,null,3000,80,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"DALI","",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"Poland"]
["5070","5070XX0011","KOSTER POLE-TOP LED 2050LM 4000K",null,"Classic design luminaire for mounting on a telescopic lighting pole with cap diameter Ø50mm.",null,"Koster","Post,Head","Europe, Africa, Asia, Australia and Oceania, North America, South America",2,512,4,0,"",null,null,null,null,null,null,null,"5070XX0011.jpg",3,1,1,5,9,4,55,"CE","","IK10","Class I",null,null,null,null,null,0,0,0,null,null,null,null,"5070XX0011.ldt",1,null,null,null,null,0,null,null,null,null,null,null,"LED",16,null,"",null,null,24,null,4000,80,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"","",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"Poland"]
["5080","5080XX0010","ASKER BIG PRO WALL 4XLED 2587LM UP-DOWN 3000K DALI2",null,"A luminaire with a wide range of applications, for illuminating wall and facade surfaces as well as other architectural concepts",null,"Asker,Big","Wall","Europe, Africa, Asia, Australia and Oceania, North America, South America",2,4,0,2.5,"",null,null,null,null,null,null,null,"5080XX0010.jpg",8,1,2,2,2,3,66,"CE","","IK08","Class I",null,null,null,null,null,0.3,0.12,0.12,null,null,null,null,"5080XX0010.ldt",1,null,null,null,null,1,null,null,null,null,null,null,"LED",16,null,"",null,null,23,null,3000,80,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"DALI","",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"Poland"]
["5085","5085XX0010","ASKER BIG PRO WALL 2XLED 1231LM DOWN 3000K DALI2",null,"A luminaire with a wide range of applications, including lighting of wall surfaces, facades and other architectural concepts",null,"Asker,Big","Wall","Europe, Africa, Asia, Australia and Oceania, North America, South America",2,4,0,2.5,"",null,null,null,null,null,null,null,"5085XX0010.jpg",7,1,2,2,2,3,66,"CE","","","Class I",null,null,null,null,null,0.3,0.12,0.12,null,null,null,null,"5085XX0010.ldt",1,null,null,null,null,0,null,null,null,null,null,null,"LED",16,null,"",null,null,23,null,3000,80,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"DALI","",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"Poland"]
["5086","5086XX0010","ASKER BIG PRO WALL 4XLED 2740LM UP-DOWN 4000K DALI2",null,"A luminaire with a wide range of applications, for illuminating wall and facade surfaces and other architectural concepts.",null,"Asker,Big","Wall","Europe, Africa, Asia, Australia and Oceania, North America, South America",2,4,0,2.5,"",null,null,null,null,null,null,null,"5086XX0010.jpg",8,1,2,2,2,3,66,"CE","","IK08","Class I",null,null,null,null,null,0.3,0.12,0.12,null,null,null,null,"5086XX0010.ldt",1,null,null,null,null,1,null,null,null,null,null,null,"LED",16,null,"",null,null,24,null,4000,80,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"DALI","",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"Poland"]
["5087","5087XX0010","ASKER BIG PRO WALL 2XLED 1303LM DOWN 4000K DALI2",null,"A luminaire with a wide range of applications, for illuminating wall and facade surfaces as well as other architectural concepts",null,"Asker,Big","Wall","Europe, Africa, Asia, Australia and Oceania, North America, South America",2,4,0,2.5,"",null,null,null,null,null,null,null,"5087XX0010.jpg",7,1,2,2,2,3,66,"CE","","","Class I",null,null,null,null,null,0.3,0.12,0.12,null,null,null,null,"5087XX0010.ldt",1,null,null,null,null,0,null,null,null,null,null,null,"LED",16,null,"",null,null,24,null,4000,80,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"DALI","",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"Poland"]
["5088","5088XX0009","NICE POLE-TOP LED 4000K DALI2",null,"A mounted luminaire designed to be mounted on a lighting pole with a Ø60mm mounting shaft",null,"Nice","Post,Head","Europe, Africa, Asia, Australia and Oceania, North America, South America",2,512,3.84,0,"",null,null,null,null,null,null,null,"5088XX0009.jpg",9,1,1,5,9,3,66,"CE","","","Class I",null,null,null,null,null,0.7,0.55000000000000004,0.55000000000000004,null,null,null,null,"5088XX0009.ldt",1,null,null,null,null,0,null,null,null,null,null,null,"LED",16,null,"",null,null,24,null,4000,80,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"DALI","",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"Poland"]
["5089","5089XX0010","NICE POLE-TOP LED 3029LM 3000K DALI2",null,"Top-mounted luminaire designed for mounting on a lighting pole with a Ø60mm mounting shaft",null,"Nice","Post,Head","Europe, Africa, Asia, Australia and Oceania, North America, South America",2,512,3.84,0,"",null,null,null,null,null,null,null,"5089XX0010.jpg",9,1,1,5,9,3,66,"CE","","","Class I",null,null,null,null,null,0.55000000000000004,0.55000000000000004,0.7,null,null,null,null,"5089XX0010.ldt",1,null,null,null,null,0,null,null,null,null,null,null,"LED",16,null,"",null,null,23,null,3000,80,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"DALI","",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"Poland"]
["5090","5090XX0011","NARVIK BOLLARD LED 3264LM 4000K DALI2",null,"A bollard luminaire with a stable and durable structure. For lighting private and public areas",null,"Narvik","Bollard","Europe, Africa, Asia, Australia and Oceania, North America, South America",2,2,0.7,0,"",null,null,null,null,null,null,null,"5090XX0011.jpg",4,1,1,3,6,3,66,"CE","","IK10","Class I",null,null,null,null,null,0.24,0.24,0.95,null,null,null,null,"5090XX0011.ldt",1,null,null,null,null,0,null,null,null,null,null,null,"LED",16,null,"",null,null,24,null,4000,80,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"DALI","",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"Poland"]
["5091","5091XX0010","NARVIK BOLLARD LED 3137LM 3000K DALI2",null,"A post luminaire with a stable and durable construction For lighting private and public areas",null,"Narvik","Bollard","Europe, Africa, Asia, Australia and Oceania, North America, South America",2,2,0.7,0,"",null,null,null,null,null,null,null,"5091XX0010.jpg",4,1,1,3,6,3,66,"CE","","IK10","Class I",null,null,null,null,null,0,0,0,null,null,null,null,"5091XX0010.ldt",1,null,null,null,null,0,null,null,null,null,null,null,"LED",16,null,"",null,null,23,null,3000,80,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"DALI","",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"Poland"]
["5092","5092XX0010","VASA WALL 2XLED 1303LM UP-DOWN 4000K DALI2",null,"A luminaire with a wide range of applications, for lighting: wall surfaces, facade and other architectural concepts",null,"Vasa","Wall","Europe, Africa, Asia, Australia and Oceania, North America, South America",2,4,0,2.5,"",null,null,null,null,null,null,null,"5092XX0010.jpg",8,1,5,2,2,3,66,"CE","","IK08","Class I",null,null,null,null,null,0.31,0.12,0.16,null,null,null,null,"5092XX0010.ldt",1,null,null,null,null,1,null,null,null,null,null,null,"LED",16,null,"",null,null,24,null,4000,80,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"DALI","",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"Poland"]
["5093","5093XX0010","VASA WALL 2XLED 1231LM UP-DOWN 3000K DALI2",null,"A luminaire with a wide range of applications, for lighting: wall surfaces, facades and other architectural concepts",null,"Vasa","Wall","Europe, Africa, Asia, Australia and Oceania, North America, South America",2,4,0,2.5,"",null,null,null,null,null,null,null,"5093XX0010.jpg",8,1,5,2,2,3,66,"CE","","IK08","Class I",null,null,null,null,null,0.31,0.12,0.16,null,null,null,null,"5093XX0010.ldt",1,null,null,null,null,1,null,null,null,null,null,null,"LED",16,null,"",null,null,23,null,3000,80,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"DALI","",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"Poland"]
["5096","5096XX0010","HALDEN WALL LED 1059LM DOWN 3000K DALI2",null,"A luminaire with a wide range of applications, among others for lighting: wall surfaces, facade, and other architectural concepts",null,"Halden","Wall","Europe, Africa, Asia, Australia and Oceania, North America, South America",2,4,0,2.5,"",null,null,null,null,null,null,null,"5096XX0010.jpg",7,1,5,2,2,3,66,"CE","","IK10","Class I",null,null,null,null,null,0.31,0.16,0.15,null,null,null,null,"5096XX0010.ldt",1,null,null,null,null,0,null,null,null,null,null,null,"LED",16,null,"",null,null,23,null,3000,80,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"DALI","",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"Poland"]
["5097","5097XX0009","HALDEN WALL LED 1121LM 4000K DALI2",null,"Luminaire with a wide range of applications for example for illumination of walls and facade surfaces or any other architectural concepts.",null,"Halden","Wall","Europe, Africa, Asia, Australia and Oceania, North America, South America",2,4,0,2.5,"",null,null,null,null,null,null,null,"5097XX0009.jpg",7,1,5,2,2,3,66,"CE","","IK10","Class I",null,null,null,null,null,0.31,0.16,0.15,null,null,null,null,"5097XX0009.ldt",1,null,null,null,null,0,null,null,null,null,null,null,"LED",16,null,"",null,null,24,null,4000,80,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"DALI","",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"Poland"]
["5100","5100XX0010","ASKER WALL LED 961LM UP-DOWN 4000K DIM.",null,"Luminaire with a wide range of applications for example for illumination of walls and facade surfaces or any other architectural concepts.",null,"Asker","Wall","Europe, Africa, Asia, Australia and Oceania, North America, South America",2,4,0,2.5,"",null,null,null,null,null,null,null,"5100XX0010.jpg",8,1,2,2,2,1,45,"CE","","IK08","Class I",null,null,null,null,null,0,0,0,null,null,null,null,"5100XX0010.ldt",1,null,null,null,null,1,null,null,null,null,null,null,"LED",16,null,"",null,null,24,null,4000,80,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"","",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"Poland"]
["5101","5101XX0010","ASKER WALL LED 961LM DOWN 4000K DIM.",null,"Luminaire with a wide range of applications for example for illumination of walls and facade surfaces or any other architectural concepts.",null,"Asker","Wall","Europe, Africa, Asia, Australia and Oceania, North America, South America",2,4,0,2.5,"",null,null,null,null,null,null,null,"5101XX0010.jpg",7,1,2,2,2,1,45,"CE","","","Class I",null,null,null,null,null,0,0,0,null,null,null,null,"5101XX0010.ldt",1,null,null,null,null,0,null,null,null,null,null,null,"LED",16,null,"",null,null,24,null,4000,80,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"","",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"Poland"]
["5102","5102XX0010","ASKER WALL LED UP-DOWN 4000K DIM.",null,"A luminaire with a wide range of applications, including lighting wall surfaces, facades and other architectural concepts",null,"Asker","Wall","Europe, Africa, Asia, Australia and Oceania, North America, South America",2,4,0,2.5,"",null,null,null,null,null,null,null,"5102XX0010.jpg",8,1,2,2,2,1,66,"CE","","IK08","Class I",null,null,null,null,null,0.22,0.08,0.11,null,null,null,null,"5102XX0010.ldt",1,null,null,null,null,1,null,null,null,null,null,null,"LED",16,null,"",null,null,24,null,4000,80,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"","",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"Poland"]
["5103","5103XX0010","ASKER WALL LED DOWN 4000K DIM.",null,"A luminaire with a wide range of applications, including lighting wall surfaces, facades and other architectural concepts",null,"Asker","Wall","Europe, Africa, Asia, Australia and Oceania, North America, South America",2,4,0,2.5,"",null,null,null,null,null,null,null,"5103XX0010.jpg",7,1,2,2,2,1,66,"CE","","IK08","Class I",null,null,null,null,null,0.22,0.08,0.11,null,null,null,null,"5103XX0010.ldt",1,null,null,null,null,0,null,null,null,null,null,null,"LED",16,null,"",null,null,24,null,4000,80,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"","",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"Poland"]
["5104","5104XX0010","ASKER BIG WALL LED 681LM DOWN 4000K DIM.",null,"A luminaire with a wide range of applications, for lighting wall and facade surfaces as well as other architectural concepts.",null,"Asker,Big","Wall","Europe, Africa, Asia, Australia and Oceania, North America, South America",2,4,0,2.5,"",null,null,null,null,null,null,null,"5104XX0010.jpg",7,1,2,2,2,1,66,"CE","","IK08","Class I",null,null,null,null,null,0,0,0,null,null,null,null,"5104XX0010.ies",1,null,null,null,null,0,null,null,null,null,null,null,"LED",16,null,"",null,null,24,null,4000,80,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"","",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"Poland"]
["5105","5105XX0010","ASKER BIG PRO WALL 4XLED 2108LM UP-DOWN 4000K DIM.",null,"A luminaire with a wide range of applications, for illuminating wall and facade surfaces as well as other architectural concepts",null,"Asker,Big","Wall","Europe, Africa, Asia, Australia and Oceania, North America, South America",2,4,0,2.5,"",null,null,null,null,null,null,null,"5105XX0010.jpg",8,1,2,2,2,1,66,"CE","","IK08","Class I",null,null,null,null,null,0.3,0.12,0.12,null,null,null,null,"5105XX0010.ldt",1,null,null,null,null,1,null,null,null,null,null,null,"LED",16,null,"",null,null,24,null,4000,80,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"","",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"Poland"]
["5106","5106XX0010","ASKER BIG PRO WALL 2XLED 1196LM DOWN 4000K DIM.",null,"A luminaire with a wide range of applications, for illuminating wall and facade surfaces as well as other architectural concepts",null,"Asker,Big","Wall","Europe, Africa, Asia, Australia and Oceania, North America, South America",2,4,0,2.5,"",null,null,null,null,null,null,null,"5106XX0010.jpg",7,1,2,2,2,1,66,"CE","","IK08","Class I",null,null,null,null,null,0.3,0.12,0.12,null,null,null,null,"5106XX0010.ldt",1,null,null,null,null,0,null,null,null,null,null,null,"LED",16,null,"",null,null,24,null,4000,80,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"","",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"Poland"]
["5107","5107XX0012","MOLDE BOLLARD 80CM LED 772LM 4000K DIM.",null,"Luminaire with contemporary design. For lighting private areas, parks and other architectural concepts",null,"Molde","Bollard","Europe, Africa, Asia, Australia and Oceania, North America, South America",2,2,0.75,0,"",null,null,null,null,null,null,null,"5107XX0012.jpg",7,1,2,3,6,1,55,"CE","","IK07","Class I",null,null,null,null,null,0.8,0.16,0.11,null,null,null,null,"5107XX0012.ldt",1,null,null,null,null,0,null,null,null,null,null,null,"LED",16,null,"",null,null,24,null,4000,80,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"","",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"Poland"]
["510","510XX0009","HALDEN WALL E27 DOWN",null,"Luminaire with a wide range of applications for example for illumination of walls and facade surfaces or any other architectural concepts.",null,"Halden","Wall","Europe, Africa, Asia, Australia and Oceania, North America, South America",2,4,0,2.5,"",null,null,null,null,null,null,null,"510XX0009.jpg",7,1,5,2,2,4,66,"CE","","","Class I",null,null,null,null,null,0.31,0.15,0,null,null,null,null,"510XX0009.ldt",0,null,null,null,null,0,null,null,null,null,null,null,"LED",16,null,"E27",null,null,23,null,"",80,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"","",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"Poland"]
["5110","5110XX0009","STOCKHOLM WALL LED 961LM 4000K DIM.",null,"Scandinavian design luminaire. For lighting gardens, private areas and public spaces.",null,"Stockholm,Połówka","Wall,Ceiling","Europe, Africa, Asia, Australia and Oceania, North America, South America",2,4,0,2.5,"",null,null,null,null,null,null,null,"5110XX0009.jpg",8,1,2,2,2,1,55,"CE","","IK10","Class I",null,null,null,null,null,0,0,0,null,null,null,null,"5110XX0009.ldt",1,null,null,null,null,3,null,null,null,null,null,null,"LED",16,null,"",null,null,24,null,4000,80,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"","",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"Poland"]
["5113","5113XX0009",{"$f":"INDEX(DB,MATCH($A503,ID,0),3)","v":"SKI WALL LED 681LM DOWN 4000K DIM."},null,"Luminaire with a wide range of applications for example for illumination of walls and facade surfaces or any other architectural concepts",null,"Ski",{"$f":"IF(INDEX(DB,MATCH($A503,ID,0),5)=0,\"\",INDEX(DB,MATCH($A503,ID,0),5))","v":"Wall"},"Europe, Africa, Asia, Australia and Oceania, North America, South America",2,{"$f":"IFERROR(INDEX(TYPMONT,MATCH((INDEX(DB,MATCH($A503,ID,0),31)),ID_RODZ,0),3),\"\")","v":4},0,2.5,{"$f":"IFERROR(IF(INDEX(TYPMONT,MATCH((INDEX(DB,MATCH($A503,ID,0),31)),ID_RODZ,0),6)=0,\"\",INDEX(TYPMONT,MATCH((INDEX(DB,MATCH($A503,ID,0),31)),ID_RODZ,0),6)),\"\")","v":""},null,null,null,null,null,null,null,{"$f":"IF(INDEX(DB,MATCH($A503,ID,0),57)=0,\"\",INDEX(DB,MATCH($A503,ID,0),57))","v":"5113XX0009.jpg"},7,{"$f":"IF(INDEX(DB,MATCH($A503,ID,0),61)=0,\"\",INDEX(DB,MATCH($A503,ID,0),61))","v":1},2,{"$f":"IFERROR(INDEX(TYPMONT,MATCH((INDEX(DB,MATCH($A503,ID,0),31)),ID_RODZ,0),1),\"\")","v":2},{"$f":"IFERROR(INDEX(TYPMONT,MATCH((INDEX(DB,MATCH($A503,ID,0),31)),ID_RODZ,0),2),\"\")","v":2},{"$f":"IF(INDEX(DB,MATCH($A503,ID,0),59)=0,\"\",INDEX(DB,MATCH($A503,ID,0),59))","v":1},{"$f":"IFERROR(IF(INDEX(DB,MATCH($A503,ID,0),19)=0,\"\",INDEX(DB,MATCH($A503,ID,0),19)+1),\"\")","v":45},{"$f":"IF(INDEX(DB,MATCH($A503,ID,0),27)=0,\"\",INDEX(DB,MATCH($A503,ID,0),27))","v":"CE"},"",{"$f":"IF(INDEX(DB,MATCH($A503,ID,0),20)=0,\"\",INDEX(DB,MATCH($A503,ID,0),20))","v":"IK09"},{"$f":"IF(INDEX(DB,MATCH($A503,ID,0),21)=0,\"\",INDEX(DB,MATCH($A503,ID,0),21))","v":"Class I"},null,null,null,null,null,0.2,0.14000000000000001,0.13,null,null,null,null,{"$f":"IF(INDEX(DB,MATCH($A503,ID,0),58)=0,\"\",INDEX(DB,MATCH($A503,ID,0),58))","v":"5113XX0009.ldt"},1,null,null,null,null,0,null,null,null,null,null,null,"LED",16,null,{"$f":"IF(INDEX(DB,MATCH($A503,ID,0),60)=0,\"\",INDEX(DB,MATCH($A503,ID,0),60))","v":""},null,null,24,null,{"$f":"IF(INDEX(DB,MATCH($A503,ID,0),22)=0,\"\",INDEX(DB,MATCH($A503,ID,0),22))","v":4000},{"$f":"IF(INDEX(DB,MATCH($A503,ID,0),53)=0,\"\",INDEX(DB,MATCH($A503,ID,0),53))","v":80},null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,{"$f":"IF(INDEX(DB,MATCH($A503,ID,0),29)=0,\"\",INDEX(DB,MATCH($A503,ID,0),29))","v":""},{"$f":"IF(INDEX(DB,MATCH($A503,ID,0),28)=0,\"\",INDEX(DB,MATCH($A503,ID,0),28))","v":""},null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"Poland"]
["5114","5114XX0009","HITRA WALL LED 1150LM 4000K ON/OFF",null,"Modern design luminaire. For lighting private areas and public spaces.",null,{"$f":"IF(INDEX(DB,MATCH($A504,ID,0),4)=0,\"\",INDEX(DB,MATCH($A504,ID,0),4))","v":"Hitra"},"Wall","Europe, Africa, Asia, Australia and Oceania, North America, South America",2,4,0,2.5,"",null,null,null,null,null,null,null,"5114XX0009.jpg",7,1,2,2,2,4,66,"CE",{"$f":"IFERROR(IF(FIND(\"RENA\",$C504)>0,\"Vehicle resistant\",\"\"),\"\")","v":""},"IK06","Class I",null,null,null,null,null,0.2,0.15,0.06,null,null,null,null,"5114XX0009.ldt",1,null,null,null,null,0,null,null,null,null,null,null,"LED",16,null,"",null,null,{"$f":"IF($BO504=4000,24,23)","v":24},null,4000,80,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"","",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"Poland"]
["5115","5115XX0009","HITRA WALL LED 2050LM 4000K ON/OFF",null,"Luminaire with contemporary design. For lighting private areas and other architectural concepts",null,"Hitra","Wall","Europe, Africa, Asia, Australia and Oceania, North America, South America",2,4,0,2.5,"",null,null,null,null,null,null,null,"5115XX0009.jpg",7,1,2,2,2,4,66,"CE","","IK06","Class I",null,null,null,null,null,0.2,0.15,0.06,null,null,null,null,"5115XX0009.ldt",1,null,null,null,null,0,null,null,null,null,null,null,"LED",16,null,"",null,null,24,null,4000,80,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"","",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"Poland"]
["5116","5116XX0009","NAMSOS WALL-RECESSED LED 4000K DIM.",null,"Luminaire designed to illuminate stairs, steps, staircases, communication lines, ceiling illumination and many other architectural applications.",null,"Namsos","Recessed","Europe, Africa, Asia, Australia and Oceania, North America, South America",2,64,0,0.5,"",null,null,null,null,null,null,null,"5116XX0009.jpg",7,1,2,2,1,1,45,"CE","","IK10","Class I",null,null,null,null,null,0,0,0,null,null,null,null,"5116XX0009.ldt",1,null,null,null,null,4,null,null,null,null,null,null,"LED",16,null,"",null,null,24,null,4000,80,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"","",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"Poland"]
["5117","5117XX0010","EGERSUND MINI BOLLARD 85CM LED 1462LM 4000K DIM.",null,"Luminaire with contemporary design For lighting gardens and other private and public areas",null,"Egersund Mini","Bollard","Europe, Africa, Asia, Australia and Oceania, North America, South America",2,2,0.69,0,"",null,null,null,null,null,null,null,"5117XX0010.jpg",3,1,1,3,6,1,66,"CE","","IK08","Class II",null,null,null,null,null,0,0,0,null,null,null,null,"5117XX0010.ldt",1,null,null,null,null,1,null,null,null,null,null,null,"LED",16,null,"",null,null,24,null,4000,80,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"","",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"Poland"]
["5118","5118XX0010","EGERSUND MINI BOLLARD 49CM LED 1462LM 4000K DIM.",null,"Luminaire with contemporary design For lighting gardens, private areas, parks, and other architectural concepts",null,"Egersund Mini","Bollard","Europe, Africa, Asia, Australia and Oceania, North America, South America",2,2,0.33,0,"",null,null,null,null,null,null,null,"5118XX0010.jpg",3,1,1,3,6,1,66,"CE","","IK08","Class II",null,null,null,null,null,0,0,0,null,null,null,null,"5118XX0010.ldt",1,null,null,null,null,1,null,null,null,null,null,null,"LED",16,null,"",null,null,24,null,4000,80,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"","",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"Poland"]
["5120","5120XX0009","ASKER BOLLARD 55CM LED 1100LM 4000K ON/OFF",null,"Luminaire with contemporary design. For lighting private areas and other architectural concepts",null,"Asker","Bollard","Europe, Africa, Asia, Australia and Oceania, North America, South America",2,2,0.5,0,"",null,null,null,null,null,null,null,"5120XX0009.jpg",7,1,2,3,6,4,66,"CE","","IK09","Class I",null,null,null,null,null,0,0,0,null,null,null,null,"5120XX0009.ldt",1,null,null,null,null,0,null,null,null,null,null,null,"LED",16,null,"",null,null,24,null,4000,80,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"","",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"Poland"]
["5121","5121XX0011","BORNHOLM CEILING/WALL LED 1121LM 4000K DIM.",null,"A ceiling-type luminaire with a modern design",null,"Bornholm","Wall,Ceiling","Europe, Africa, Asia, Australia and Oceania, North America, South America",2,4,0,2.5,"Ceiling mounted",null,null,null,null,null,null,null,"5121XX0011.jpg",8,1,1,2,2,1,66,"CE","","IK10","Class I",null,null,null,null,null,0,0,0,null,null,null,null,"5121XX0011.ldt",1,null,null,null,null,4,null,null,null,null,1,null,"LED",16,null,"",null,null,24,null,4000,80,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"","",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"Poland"]
["5122","5122XX0010","BORNHOLM CEILING/WALL LED 2050LM 4000K ON/OFF",null,"A ceiling lamp with a modern design",null,"Bornholm","Wall,Ceiling","Europe, Africa, Asia, Australia and Oceania, North America, South America",2,4,0,2.5,"Ceiling mounted",null,null,null,null,null,null,null,"5122XX0010.jpg",8,1,1,2,2,4,66,"CE","","IK10","Class I",null,null,null,null,null,0,0,0,null,null,null,null,"5122XX0010.ldt",1,null,null,null,null,4,null,null,null,null,null,null,"LED",16,null,"",null,null,24,null,4000,80,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"","",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"Poland"]
["5124","5124XX0010","ASKER BOLLARD LED 1150LM 4000K",null,"Luminaire with contemporary design. For lighting gardens and other private land and public areas",null,"Asker","Bollard","Europe, Africa, Asia, Australia and Oceania, North America, South America",2,2,0.8,0,"",null,null,null,null,null,null,null,"5124XX0010.jpg",7,1,2,3,6,4,66,"CE","","IK09","Class I",null,null,null,null,null,0,0,0,null,null,null,null,"5124XX0010.ldt",1,null,null,null,null,0,null,null,null,null,null,null,"LED",16,null,"",null,null,24,null,4000,80,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"","",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"Poland"]
["5126","5126XX0009","ASKER POLE LIGHT LUMINAIRES POLE 216CM 2XLED 1778LM 4000K DIM.",null,"Luminaire for lighting private areas, and other architectural concepts. The tightness of the lighting and connection chamber is IP65.",null,"Asker","Post,Post complete","Europe, Africa, Asia, Australia and Oceania, North America, South America",2,512,2.16,0,"",null,null,null,null,null,null,null,"5126XX0009.jpg",7,1,2,5,9,1,66,"CE","","IK09","Class I",null,null,null,null,null,0,0,0,null,null,null,null,"5126XX0009.ldt",1,null,null,null,null,0,null,null,null,null,null,null,"LED",16,null,"",null,null,24,null,4000,80,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"","",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"Poland"]
["5127","5127XX0010","ASKER POLE LIGHT LUMINAIRES POLE 2XLED 1778LM 4000K DIM.",null,"For lighting private areas and other concepts architectural",null,"Asker","Post,Post complete","Europe, Africa, Asia, Australia and Oceania, North America, South America",2,512,2.36,0,"",null,null,null,null,null,null,null,"5127XX0010.jpg",3,1,2,5,9,1,66,"CE","","IK09","Class I",null,null,null,null,null,0.11,2.36,0.39,null,null,null,null,"5127XX0010.ldt",1,null,null,null,null,0,null,null,null,null,null,null,"LED",16,null,"",null,null,24,null,4000,80,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"","",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"Poland"]
["5128","5128XX0C10","VOSS WALL LED 767LM UP 4º 4000K DIM.",null,"A luminaire with a wide range of applications, for lighting: walls and facade surfaces and other architectural concepts",null,"Voss","Wall","Europe, Africa, Asia, Australia and Oceania, North America, South America",2,4,0,2.5,"",null,null,null,null,null,null,null,"5128XX0C10.jpg",10,1,2,2,2,1,55,"CE","","IK06","Class I",null,null,null,null,null,0.18,0.16,0.27,null,null,null,null,"5128XX0C10.ldt",1,null,null,null,null,2,null,null,null,null,null,null,"LED",16,null,"",null,null,24,null,4000,80,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"","",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"Poland"]
["5130","5130XX0010","HAMMERFEST POLE-TOP LED 4503LM 4000K ON/OFF",null,"A mounted luminaire designed to be mounted on a lighting pole with Ø60mm mounting shaft",null,"Hammerfest","Post,Head","Europe, Africa, Asia, Australia and Oceania, North America, South America",2,512,4,0,"",null,null,null,null,null,null,null,"5130XX0010.jpg",7.9,1,1,5,9,4,66,"CE","","IK07","Class I",null,null,null,null,null,0.55000000000000004,0.76,0.55000000000000004,null,null,null,null,"5130XX0010.ldt",1,null,null,null,null,0,null,null,null,null,null,null,"LED",16,null,"",null,null,24,null,4000,80,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"","",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"Poland"]
["5131","5131XX0009","HAMMERFEST POLE-TOP LED 4311LM 3000K DALI2",null,"Luminaire mounted on a telescopic lighting pole with a diameter Ø60mm. Other components need to be ordered separately",null,"Hammerfest","Post,Head","Europe, Africa, Asia, Australia and Oceania, North America, South America",2,512,4,0,"",null,null,null,null,null,null,null,"5131XX0009.jpg",7,1,1,5,9,3,66,"CE","","IK07","Class I",null,null,null,null,null,0.76,0.55000000000000004,0.55000000000000004,null,null,null,null,"5131XX0009.ldt",1,null,null,null,null,0,null,null,null,null,null,null,"LED",16,null,"",null,null,23,null,3000,80,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"DALI","",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"Poland"]
["5135","5135XX0010","HAMMERFEST POLE-TOP LED 4503LM 4000K ON/OFF",null,"Modern design luminaire mounted on a lighting pole with a cap diameter Ø60mm",null,"Hammerfest","Post,Head","Europe, Africa, Asia, Australia and Oceania, North America, South America",2,512,4,0,"",null,null,null,null,null,null,null,"5135XX0010.jpg",7.9,1,1,5,9,4,66,"CE","","IK07","Class I",null,null,null,null,null,0.55000000000000004,0.55000000000000004,0.76,null,null,null,null,"5135XX0010.ldt",1,null,null,null,null,0,null,null,null,null,null,null,"LED",16,null,"",null,null,24,null,4000,80,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"","",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"Poland"]
["5136",{"$f":"INDEX(DB,MATCH($A519,ID,0),2)","v":"5136XX0009"},"HAMMERFEST POLE-TOP LED 4311LM 3000K DALI2",null,{"$f":"IF(INDEX(DB,MATCH($A519,ID,0),35)=0,\"\",INDEX(DB,MATCH($A519,ID,0),35))","v":"Luminaire mounted on a telescopic lighting pole with a diameter Ø60mm. Other components need to be ordered separately"},null,"Hammerfest","Post,Head","Europe, Africa, Asia, Australia and Oceania, North America, South America",2,512,4,{"$f":"IF(K519=4,2.5,IF(K519=64,0.5,0))","v":0},"",null,null,null,null,null,null,null,"5136XX0009.jpg",{"$f":"IF((IFERROR(INDEX(BRYLA_FOTO,MATCH(INDEX(DB,MATCH($A519,ID,0),62),ID_BRYLAFOTO,0),6),\"\"))<>0,IFERROR(INDEX(BRYLA_FOTO,MATCH(INDEX(DB,MATCH($A519,ID,0),62),ID_BRYLAFOTO,0),6),\"\"),\"\")","v":7},1,1,5,9,3,66,"CE","","IK07","Class I",null,null,null,null,null,{"$f":"INDEX(DB,MATCH($A519,ID,0),24)","v":0.76},{"$f":"INDEX(DB,MATCH($A519,ID,0),25)","v":0.55000000000000004},{"$f":"INDEX(DB,MATCH($A519,ID,0),26)","v":0.55000000000000004},null,null,null,null,"5136XX0009.ldt",1,null,null,null,null,0,null,null,null,null,null,null,"LED",16,null,"",null,null,23,null,3000,80,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"DALI","",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"Poland"]
["5137","5137XX0009","HAMMERFEST POLE-TOP LED 4503LM 4000K DALI2",null,"Luminaire mounted on a telescopic lighting pole with a diameter Ø60mm. Other components need to be ordered separately",null,"Hammerfest","Post,Head","Europe, Africa, Asia, Australia and Oceania, North America, South America",2,512,4,0,"",null,null,null,null,null,null,null,"5137XX0009.jpg",7,1,1,5,9,3,66,"CE","","IK07","Class I",null,null,null,null,null,0.76,0.55000000000000004,0.55000000000000004,null,null,null,null,"5137XX0009.ldt",{"$f":"IF($BJ520=\"\",1,0)","v":1},null,null,null,null,0,null,null,null,null,null,null,"LED",16,null,"",null,null,24,null,4000,80,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"DALI","",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"Poland"]
["5140","5140XX0009","BORG POLE-TOP LED 4380LM 4000K ON/OFF",null,"Mounted on a telescopic lighting pole with a cap diameter Ø60mm. Other accessories have to be ordered separately.",null,"Borg","Post,Head","Europe, Africa, Asia, Australia and Oceania, North America, South America",2,512,4,0,"",null,null,null,null,null,null,null,"5140XX0009.jpg",7,1,1,5,9,4,66,"CE","","IK08","Class I",null,null,null,null,null,0,0,0,null,null,null,null,"5140XX0009.ldt",1,null,null,null,null,0,null,null,null,null,null,null,"LED",16,null,"",null,null,24,null,4000,80,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"","",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"Poland"]
["5142","5142XX0009","BORG POLE-TOP LED 4380LM 4000K DALI2",null,"Luminaire mounted on a telescopic lighting pole with a shaft diameter of Ø60mm",null,"Borg","Post,Head","Europe, Africa, Asia, Australia and Oceania, North America, South America",2,512,4,0,"",null,null,null,null,null,null,null,"5142XX0009.jpg",7,1,1,5,9,3,66,"CE","","IK08","Class I",null,null,null,null,null,0,0,0,null,null,null,null,"5142XX0009.ldt",1,null,null,null,null,0,null,null,null,null,null,null,"LED",16,null,"",null,null,24,null,4000,80,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"DALI","",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"Poland"]
["5145","5145XX0009","BORG POLE-TOP LED 4380LM 4000K ON/OFF",null,"Modern design luminaire mounted on a telescopic lighting pole with a cap diameter Ø60mm. Other accessories need to be purchased separately.",null,"Borg","Post,Head","Europe, Africa, Asia, Australia and Oceania, North America, South America",2,512,4,0,"",null,null,null,null,null,null,null,"5145XX0009.jpg",7,1,1,5,9,4,66,"CE","","IK08","Class I",null,null,null,null,null,0,0,0,null,null,null,null,"5145XX0009.ldt",1,null,null,null,null,0,null,null,null,null,null,null,"LED",16,null,"",null,null,24,null,4000,80,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"","",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"Poland"]
["5147","5147XX0009","BORG POLE-TOP LED 4380LM 4000K DALI2",null,"Luminaire mounted on a telescopic lighting pole with a shaft diameter of Ø60mm",null,"Borg","Post,Head","Europe, Africa, Asia, Australia and Oceania, North America, South America",2,512,4,0,"",null,null,null,null,null,null,null,"5147XX0009.jpg",7,1,1,5,9,3,66,"CE","","IK08","Class I",null,null,null,null,null,0,0,0,null,null,null,null,"5147XX0009.ldt",1,null,null,null,null,0,null,null,null,null,null,null,"LED",16,null,"",null,null,24,null,4000,80,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"DALI","",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"Poland"]
["5150","5150XX0010","ASKER SMALL PRO WALL 2XLED 1188LM UP-DOWN 4000K DIM.",null,"A luminaire with a wide range of applications, including lighting wall surfaces, facades, and other architectural concepts",null,"Asker","Wall","Europe, Africa, Asia, Australia and Oceania, North America, South America",2,4,0,2.5,"",null,null,null,null,null,null,null,"5150XX0010.jpg",8,1,2,2,2,1,66,"CE","","IK08","Class I",null,null,null,null,null,0,0,0,null,null,null,null,"5150XX0010.ldt",1,null,null,null,null,1,null,null,null,null,null,null,"LED",16,null,"",null,null,24,null,4000,80,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"","",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"Poland"]
["5151","5151XX0009","ASKER SMALL PRO WALL LED 681LM DOWN 4000K DIM.",null,"Luminaire with a wide range of applications for example for illumination of walls and facade surfaces or any other architectural concepts",null,"Asker","Wall","Europe, Africa, Asia, Australia and Oceania, North America, South America",2,4,0,2.5,"",null,null,null,null,null,null,null,"5151XX0009.jpg",7,1,2,2,2,1,66,"CE","","IK08","Class I",null,null,null,null,null,0.22,0.11,0.08,null,null,null,null,"5151XX0009.ldt",1,null,null,null,null,0,null,null,null,null,null,null,"LED",16,null,"",null,null,24,null,4000,80,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"","",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"Poland"]
["5152","5152XX0009","SANDVIK WALL 2XLED 1604LM UP36D&DOWN36D 4000K DIM.",null,"Classic design ceiling luminaire. For lighting private areas and public spaces.",null,"Sandvik","Wall","Europe, Africa, Asia, Australia and Oceania, North America, South America",2,4,0,2.5,"",null,null,null,null,null,null,null,"5152XX0009.jpg",2,1,2,2,2,1,66,"CE","","IK08","Class I",null,null,null,null,null,0,0,0,null,null,null,null,"5152XX0009.ldt",1,null,null,null,null,1,null,null,null,null,null,null,"LED",16,null,"",null,null,24,null,4000,80,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"","",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"Poland"]
["5153","5153XX0009","SANDVIK DOWN WALL LED 802LM DOWN 36D 4000K DIM.",null,"Classic design wall luminaire. For lighting private areas and public spaces",null,"Sandvik","Wall","Europe, Africa, Asia, Australia and Oceania, North America, South America",2,4,0,2.5,"",null,null,null,null,null,null,null,"5153XX0009.jpg",2,1,2,2,2,1,66,"CE","","IK08","Class I",null,null,null,null,null,0,0,0,null,null,null,null,"5153XX0009.ldt",1,null,null,null,null,0,null,null,null,null,null,null,"LED",16,null,"",null,null,24,null,4000,80,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"","",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"Poland"]
["5157","5157XX0009","ASKER SMALL PRO WALL LED 688LM DOWN 4000K DALI2",null,"A luminaire with a wide range of applications, including lighting wall surfaces, facades, and other architectural concepts",null,"Asker","Wall","Europe, Africa, Asia, Australia and Oceania, North America, South America",2,4,0,2.5,"",null,null,null,null,null,null,null,"5157XX0009.jpg",7,1,2,2,2,3,66,"CE","","","Class I",null,null,null,null,null,0,0,0,null,null,null,null,"5157XX0009.ldt",1,null,null,null,null,0,null,null,null,null,null,null,"LED",16,null,"",null,null,24,null,4000,80,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"DALI","",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"Poland"]
["515","515XX0009","HALDEN WALL LED E27 806LM DOWN 2700K DIM.",null,"Luminaire with a wide range of applications for example for illumination of walls and facade surfaces or any other architectural concepts.",null,"Halden","Wall","Europe, Africa, Asia, Australia and Oceania, North America, South America",2,4,0,2.5,"",null,null,null,null,null,null,null,"515XX0009.jpg",7,1,5,2,2,1,66,"CE","","IK10","Class I",null,null,null,null,null,0.31,0,0.15,null,null,null,null,"515XX0009.ldt",0,null,null,null,null,0,null,null,null,null,null,null,"LED",16,null,"E27",null,null,23,null,2700,80,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"","",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"Poland"]
["5160","5160XX0009","ASKER SMALL PRO WALL LED 1376LM UP-DOWN 4000K DALI2",null,"A luminaire with a wide range of applications, including lighting wall surfaces, facades, and other architectural concepts",null,"Asker","Wall","Europe, Africa, Asia, Australia and Oceania, North America, South America",2,4,0,2.5,"",null,null,null,null,null,null,null,"5160XX0009.jpg",8,1,2,2,2,3,66,"CE","","","Class I",null,null,null,null,null,0,0,0,null,null,null,null,"5160XX0009.ldt",1,null,null,null,null,1,null,null,null,null,null,null,"LED",16,null,"",null,null,24,null,4000,80,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"DALI","",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"Poland"]
["5164","5164XX0009","ASKER POLE PRO LIGHT LUMINAIRES POLE 236CM LED 1169LM VSM 4000K ON/OFF",null,"Luminaire for lighting private areas, public spaces, and other architectural concepts",null,"Asker","Post,Post complete","Europe, Africa, Asia, Australia and Oceania, North America, South America",2,512,2.36,0,"",null,null,null,null,null,null,null,"5164XX0009.jpg",4,1,2,5,9,4,66,"CE","","IK08","Class I",null,null,null,null,null,0.24,2.36,0.39,null,null,null,null,"5164XX0009.ldt",1,null,null,null,null,0,null,null,null,null,null,null,"LED",16,null,"",null,null,24,null,4000,70,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"","",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"Poland"]
["5165","5165XX0009","ASKER POLE PRO LIGHT LUMINAIRES POLE 236CM LED 1221LM VSM 4000K DALI2",null,"Luminaire for lighting private areas, public spaces, and other architectural concepts",null,"Asker","Post,Post complete","Europe, Africa, Asia, Australia and Oceania, North America, South America",2,512,2.36,0,"",null,null,null,null,null,null,null,"5165XX0009.jpg",4,1,2,5,9,3,66,"CE","","IK08","Class I",null,null,null,null,null,0.39,0.11,2.36,null,null,null,null,"5165XX0009.ldt",1,null,null,null,null,0,null,null,null,null,null,null,"LED",16,null,"",null,null,24,null,4000,70,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"DALI","",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"Poland"]
["5167","5167XX0009","ASKER POLE PRO LIGHT LUMINAIRES POLE 236CM LED 1169LM T2-L 4000K ON/OFF",null,"Luminaire for lighting private areas, public spaces, and other architectural concepts",null,"Asker","Post,Post complete","Europe, Africa, Asia, Australia and Oceania, North America, South America",2,512,2.36,0,"",null,null,null,null,null,null,null,"5167XX0009.jpg",6,1,2,5,9,4,66,"CE","","IK08","Class I",null,null,null,null,null,2.36,0.11,0.39,null,null,null,null,"5167XX0009.ldt",1,null,null,null,null,0,null,null,null,null,null,null,"LED",16,null,"",null,null,24,null,4000,70,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"","",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"Poland"]
["5169","5169XX0009","ASKER POLE PRO LIGHT LUMINAIRES POLE 236CM LED 1221LM T2-L 4000K DALI2",null,"Luminaire for lighting private areas, public spaces, and other architectural concepts",null,"Asker","Post,Post complete","Europe, Africa, Asia, Australia and Oceania, North America, South America",2,512,2.36,0,"",null,null,null,null,null,null,null,"5169XX0009.jpg",6,1,2,5,9,3,66,"CE","","IK08","Class I",null,null,null,null,null,0,0,0,null,null,null,null,"5169XX0009.ldt",1,null,null,null,null,0,null,null,null,null,null,null,"LED",16,null,"",null,null,24,null,4000,70,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"DALI","",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"Poland"]
["5170","5170XX0009","KISA HEAD POLE-TOP 90CM 3XLED 1175LM 180D 3000K DIM.",null,"Luminaire with a contemporary design. For lighting gardens and other private and public areas",null,"Kisa","Other,Head","Europe, Africa, Asia, Australia and Oceania, North America, South America",2,512,2.0699999999999998,0,"",null,null,null,null,null,null,null,"5170XX0009.jpg",9,1,1,5,9,1,66,"CE","","IK08","Class I",null,null,null,null,null,0.14000000000000001,0.14000000000000001,0.9,null,null,null,null,"5170XX0009.ldt",1,null,null,null,null,1,null,null,null,null,null,null,"LED",16,null,"",null,null,23,null,3000,80,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"","",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"Poland"]
["517","517XX0013","HALDEN WALL LED 1059LM DOWN 3000K DIM.",null,"Luminaire with a wide range of applications for example for illumination of walls and facade surfaces or any other architectural concepts",null,"Halden","Wall","Europe, Africa, Asia, Australia and Oceania, North America, South America",2,4,0,2.5,"",null,null,null,null,null,null,null,"517XX0013.jpg",7,1,5,2,2,1,66,"CE","","IK10","Class I",null,null,null,null,null,0.31,0.16,0.15,null,null,null,null,"517XX0013.ldt",1,null,null,null,null,0,null,null,null,null,null,null,"LED",16,null,"",null,null,23,null,3000,80,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"","",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"Poland"]
["5180","5180XX0010","KISA BOLLARD 85CM 3XLED 1175LM 180D 3000K DIM.",null,"Luminaire with contemporary design For lighting gardens and other private and public areas",null,"Kisa","Bollard","Europe, Africa, Asia, Australia and Oceania, North America, South America",2,2,0.42,0,"",null,null,null,null,null,null,null,"5180XX0010.png",9,1,1,3,6,1,56,"CE","","IK08","Class I",null,null,null,null,null,0.12,0.12,0.85,null,null,null,null,"5180XX0010.ldt",1,null,null,null,null,1,null,null,null,null,null,null,"LED",16,null,"",null,null,23,null,3000,80,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"","",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"Poland"]
["5181","5181XX0010","KISA BOLLARD 85CM 3XLED 1246LM 180D 4000K DIM. TRIAC",null,"Luminaire with contemporary design For lighting gardens and other private and public areas",null,"Kisa","Bollard","Europe, Africa, Asia, Australia and Oceania, North America, South America",2,2,0.42,0,"",null,null,null,null,null,null,null,"5181XX0010.png",9,1,1,3,6,1,56,"CE","","IK08","Class I",null,null,null,null,null,0.12,0.12,0.85,null,null,null,null,"5181XX0010.ldt",1,null,null,null,null,1,null,null,null,null,null,null,"LED",16,null,"",null,null,24,null,4000,80,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"","",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"Poland"]
["5182","5182XX0009","KISA BOLLARD 85CM 3XLED 2002LM 180D 3000K DALI2",null,"Luminaire with contemporary design, For lighting gardens and other private and public areas",null,"Kisa","Bollard","Europe, Africa, Asia, Australia and Oceania, North America, South America",2,2,0.42,0,"",null,null,null,null,null,null,null,"5182XX0009.png",9,1,1,3,6,3,56,"CE","","IK08","Class I",null,null,null,null,null,0.85,0.12,0.12,null,null,null,null,"5182XX0009.ldt",1,null,null,null,null,1,null,null,null,null,null,null,"LED",16,null,"",null,null,23,null,3000,80,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"DALI","",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"Poland"]
["5183","5183XX0009","KISA BOLLARD 85CM 3XLED 2122LM 180D 4000K DALI2",null,"Luminaire with contemporary design, For lighting gardens and other private and public areas",null,"Kisa","Bollard","Europe, Africa, Asia, Australia and Oceania, North America, South America",2,2,0.42,0,"",null,null,null,null,null,null,null,"5183XX0009.png",9,1,1,3,6,3,56,"CE","","IK08","Class I",null,null,null,null,null,0.85,0.12,0.12,null,null,null,null,"5183XX0009.ldt",1,null,null,null,null,1,null,null,null,null,null,null,"LED",16,null,"",null,null,24,null,4000,80,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"DALI","",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"Poland"]
["5184","5184XX0010","KISA BOLLARD 85CM 6XLED 2009LM 3000K DIM.",null,"Luminaire with contemporary design For lighting gardens and other private and public areas",null,"Kisa","Bollard","Europe, Africa, Asia, Australia and Oceania, North America, South America",2,2,0.42,0,"",null,null,null,null,null,null,null,"5184XX0010.png",8,1,1,3,6,1,56,"CE","","IK08","Class I",null,null,null,null,null,0.12,0.12,0.85,null,null,null,null,"5184XX0010.ldt",1,null,null,null,null,1,null,null,null,null,null,null,"LED",16,null,"",null,null,23,null,3000,80,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"","",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"Poland"]
["5185","5185XX0010","KISA BOLLARD 85CM 6XLED 2131LM 4000K DIM.",null,"Luminaire with contemporary design For lighting gardens and other private and public areas",null,"Kisa","Bollard","Europe, Africa, Asia, Australia and Oceania, North America, South America",2,2,0.42,0,"",null,null,null,null,null,null,null,"5185XX0010.png",8,1,1,3,6,1,56,"CE","","IK08","Class I",null,null,null,null,null,0.12,0.12,0.85,null,null,null,null,"5185XX0010.ldt",1,null,null,null,null,1,null,null,null,null,null,null,"LED",16,null,"",null,null,24,null,4000,80,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"","",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"Poland"]
["5187","5187XX0009","KISA BOLLARD 85CM 6XLED 4126LM 4000K DALI2",null,"Luminaire with contemporary design For lighting gardens and other private and public areas",null,"Kisa","Bollard","Europe, Africa, Asia, Australia and Oceania, North America, South America",2,2,0.42,0,"",null,null,null,null,null,null,null,"5187XX0009.png",8,1,1,3,6,3,56,"CE","","IK08","Class I",null,null,null,null,null,0.85,0.12,0.12,null,null,null,null,"5187XX0009.ldt",1,null,null,null,null,1,null,null,null,null,null,null,"LED",16,null,"",null,null,24,null,4000,80,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"DALI","",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"Poland"]
["5190","5190XX0309","KISA LIGHT LUMINAIRES POLE 3XLED 1175LM 180D 3000K DIM.",null,"Pole luminaire, mounting ø120mm",null,"Kisa","Post,Post complete","Europe, Africa, Asia, Australia and Oceania, North America, South America",2,512,2.0699999999999998,0,"",null,null,null,null,null,null,null,"5190XX0309.jpg",9,1,1,5,9,1,66,"CE","","IK08","Class I",null,null,null,null,null,0.12,0.12,2.5,null,null,null,null,"5190XX0309.ldt",1,null,null,null,null,1,null,null,null,null,null,null,"LED",16,null,"",null,null,23,null,3000,80,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"","",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"Poland"]
["5191","5191XX0309","KISA LIGHT LUMINAIRES POLE 3XLED 1246LM 180D 4000K DIM.",null,"Pole luminaire, mounted ø120mm",null,"Kisa","Post,Post complete","Europe, Africa, Asia, Australia and Oceania, North America, South America",2,512,2.0699999999999998,0,"",null,null,null,null,null,null,null,"5191XX0309.jpg",9,1,1,5,9,1,66,"CE","","IK08","Class I",null,null,null,null,null,0.12,0.12,2.5,null,null,null,null,"5191XX0309.ldt",1,null,null,null,null,1,null,null,null,null,null,null,"LED",16,null,"",null,null,24,null,4000,80,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"","",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"Poland"]
["5192","5192XX0309","KISA LIGHT LUMINAIRES POLE 3XLED 2002LM 180D 3000K DALI2",null,"Luminaire with a contemporary design For lighting gardens and other private and public areas Top-mounted pole luminaire ø120mm, equipped with: - Pole art. 5188xx0009 equipped with an revision door - Head art. 5172xx0009 equipped with LED module and hermetic electric box Other accessories must be ordered separately",null,"Kisa","Pole","Europe, Africa, Asia, Australia and Oceania, North America, South America",2,512,2.0699999999999998,0,"",null,null,null,null,null,null,null,"5192XX0309.jpg",9,1,1,5,9,3,66,"CE","","IK08","Class I",null,null,null,null,null,0.12,0.12,2.5,null,null,null,null,"5192XX0309.ldt",1,null,null,null,null,1,null,null,null,null,null,null,"LED",16,null,"",null,null,23,null,3000,80,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"DALI","",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"Poland"]
["5193","5193XX0309","KISA LIGHT LUMINAIRES POLE 3XLED 2122LM 180D 4000K DALI2",null,"Luminaire with a contemporary design For lighting gardens and other private and public areas Top-mounted pole luminaire ø120mm, equipped with: - Pole art. 5188xx0009 equipped with an revision door - Head art. 5173xx0009 equipped with LED module and hermetic electric box Other accessories must be ordered separately",null,"Kisa,Pole","Pole","Europe, Africa, Asia, Australia and Oceania, North America, South America",2,512,2.0699999999999998,0,"",null,null,null,null,null,null,null,"5193XX0309.jpg",9,1,1,5,9,3,66,"CE","","IK08","Class I",null,null,null,null,null,0.12,0.12,2.5,null,null,null,null,"5193XX0309.ldt",1,null,null,null,null,1,null,null,null,null,null,null,"LED",16,null,"",null,null,24,null,4000,80,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"DALI","",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"Poland"]
["5194","5194XX0309","KISA LIGHT LUMINAIRES POLE 6XLED 2009LM 3000K DIM.",null,"Luminaire with a contemporary design For lighting gardens and other private and public areas Top-mounted pole luminaire ø120mm, equipped with: - Pole art. 5188xx0009 equipped with an revision door - Head art. 5174xx0009 equipped with LED module and hermetic electric box Other accessories must be ordered separately",null,"Kisa","Pole","Europe, Africa, Asia, Australia and Oceania, North America, South America",2,512,2.0699999999999998,0,"",null,null,null,null,null,null,null,"5194XX0309.png",8,1,1,5,9,1,66,"CE","","IK08","Class I",null,null,null,null,null,0.12,0.12,1.2,null,null,null,null,"5194XX0309.ldt",1,null,null,null,null,1,null,null,null,null,null,null,"LED",16,null,"",null,null,23,null,3000,80,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"","",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"Poland"]
["5195","5195XX0309","KISA LIGHT LUMINAIRES POLE 6XLED 2131LM 4000K DIM.",null,"Luminaire with a contemporary design For lighting gardens and other private and public areas Top-mounted pole luminaire ø120mm, equipped with: - Pole art. 5188xx0009 equipped with an revision door - Head art. 5175xx0009 equipped with LED module and hermetic electric box Other accessories must be ordered separately",null,"Kisa","Pole","Europe, Africa, Asia, Australia and Oceania, North America, South America",2,512,2.0699999999999998,0,"",null,null,null,null,null,null,null,"5195XX0309.png",8,1,1,5,9,1,66,"CE","","IK08","Class I",null,null,null,null,null,0.12,0.12,2.5,null,null,null,null,"5195XX0309.ldt",1,null,null,null,null,1,null,null,null,null,null,null,"LED",16,null,"",null,null,24,null,4000,80,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"","",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"Poland"]
["5196","5196XX0309","KISA LIGHT LUMINAIRES POLE 6XLED 3891LM 3000K DALI2",null,"Pole luminaire, mounted ø120mm",null,"Kisa","Pole,Post complete","Europe, Africa, Asia, Australia and Oceania, North America, South America",2,512,2.0699999999999998,0,"",null,null,null,null,null,null,null,"5196XX0309.png",8,1,1,5,9,3,66,"CE","","IK08","Class I",null,null,null,null,null,0.12,0.12,2.5,null,null,null,null,"5196XX0309.ldt",1,null,null,null,null,1,null,null,null,null,null,null,"LED",16,null,"",null,null,23,null,3000,80,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"DALI","",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"Poland"]
["5197","5197XX0309","KISA LIGHT LUMINAIRES POLE 6XLED 4126LM 4000K DALI2",null,"Luminaire with a contemporary design For lighting gardens and other private and public areas Top-mounted pole luminaire ø120mm, equipped with: - Pole art. 5188xx0009 equipped with an revision door - Head art. 5177xx0009 equipped with LED module and hermetic electric box Other accessories must be ordered separately",null,"Kisa","Pole,Post complete","Europe, Africa, Asia, Australia and Oceania, North America, South America",2,512,2.0699999999999998,0,"",null,null,null,null,null,null,null,"5197XX0309.png",8,1,1,5,9,3,66,"CE","","IK08","Class I",null,null,null,null,null,0.12,0.12,2.5,null,null,null,null,"5197XX0309.ldt",1,null,null,null,null,1,null,null,null,null,null,null,"LED",16,null,"",null,null,24,null,4000,80,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"DALI","",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"Poland"]
["5200","5200XX0010","ASKER POLE PRO 350CM LED 2628LM VSM 3000K DALI2",null,"For lighting private areas, parks and other architectural concepts",null,"Asker","Post","Europe, Africa, Asia, Australia and Oceania, North America, South America",2,256,3.45,0,"",null,null,null,null,null,null,null,"5200XX0010.jpg",4,1,2,5,8,3,66,"CE","","IK08","Class I",null,null,null,null,null,0,0,0,null,null,null,null,"5200XX0010.ldt",1,null,null,null,null,0,null,null,null,null,null,null,"LED",16,null,"",null,null,23,null,3000,70,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"DALI","",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"Poland"]
["5201","5201XX0010","ASKER POLE PRO 350CM LED 2772LM VSM 4000K DALI2",null,"For lighting private areas, parks and other architectural concepts",null,"Asker","Post","Europe, Africa, Asia, Australia and Oceania, North America, South America",2,256,3.45,0,"",null,null,null,null,null,null,null,"5201XX0010.jpg",4,1,2,5,8,3,66,"CE","","IK08","Class I",null,null,null,null,null,0,0,0,null,null,null,null,"5201XX0010.ldt",1,null,null,null,null,0,null,null,null,null,null,null,"LED",16,null,"",null,null,24,null,4000,70,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"DALI","",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"Poland"]
["5202","5202XX0011","ASKER POLE PRO 350CM LED 2667LM VSM 3000K DIM.",null,"For lighting private areas, parks and other architectural concepts",null,"Asker,Pole","Post,Post complete","Europe, Africa, Asia, Australia and Oceania, North America, South America",2,256,3.45,0,"",null,null,null,null,null,null,null,"5202XX0011.jpg",4,1,2,5,8,1,66,"CE","","IK08","Class I",null,null,null,null,null,0.24,0.48,3.5,null,null,null,null,"5202XX0011.ldt",1,null,null,null,null,0,null,null,null,null,null,null,"LED",16,null,"",null,null,23,null,3000,70,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"","",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"Poland"]
["5203","5203XX0010","ASKER POLE PRO 350CM LED 2772LM VSM 4000K ON/OFF",null,"For lighting private areas, parks and other architectural concepts",null,"Asker,Pole","Post,Post complete","Europe, Africa, Asia, Australia and Oceania, North America, South America",2,256,3.45,0,"",null,null,null,null,null,null,null,"5203XX0010.jpg",4,1,2,5,8,4,66,"CE","","IK08","Class I",null,null,null,null,null,0,0,0,null,null,null,null,"5203XX0010.ldt",1,null,null,null,null,0,null,null,null,null,null,null,"LED",16,null,"",null,null,24,null,4000,70,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"","",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"Poland"]
["5204","5204XX0010","ASKER POLE PRO 350CM LED 2628LM T2-L 3000K DALI2",null,"For lighting private areas, parks and other architectural concepts",null,"Asker","Post","Europe, Africa, Asia, Australia and Oceania, North America, South America",2,256,3.45,0,"",null,null,null,null,null,null,null,"5204XX0010.jpg",6,1,2,5,8,3,66,"CE","","IK08","Class I",null,null,null,null,null,3.5,0.39,0.11,null,null,null,null,"5204XX0010.ldt",1,null,null,null,null,0,null,null,null,null,null,null,"LED",16,null,"",null,null,23,null,3000,70,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"DALI","",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"Poland"]
["5205","5205XX0010","ASKER POLE PRO 350CM LED 2772LM T2-L 4000K DALI2",null,"For lighting private areas, parks and other architectural concepts",null,"Asker","Post","Europe, Africa, Asia, Australia and Oceania, North America, South America",2,256,3.45,0,"",null,null,null,null,null,null,null,"5205XX0010.jpg",6,1,2,5,8,3,66,"CE","","IK08","Class I",null,null,null,null,null,0,0,0,null,null,null,null,"5205XX0010.ldt",1,null,null,null,null,0,null,null,null,null,null,null,"LED",16,null,"",null,null,24,null,4000,70,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"DALI","",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"Poland"]
["5206","5206XX0011","ASKER POLE PRO 350CM LED 2687LM T2-L 3000K DIM.",null,"For lighting private areas, parks and other architectural concepts",null,"Asker,Pole","Post,Post complete","Europe, Africa, Asia, Australia and Oceania, North America, South America",2,256,3.45,0,"",null,null,null,null,null,null,null,"5206XX0011.jpg",6,1,2,5,8,1,66,"CE","","IK08","Class I",null,null,null,null,null,3.5,0.39,0.24,null,null,null,null,"5206XX0011.ldt",1,null,null,null,null,0,null,null,null,null,null,null,"LED",16,null,"",null,null,23,null,3000,70,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"","",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"Poland"]
["5207","5207XX0011","ASKER POLE PRO 350CM LED 2910LM T2-L 4000K DIM.",null,"For lighting private areas, parks and other architectural concepts",null,"Asker,Pole","Post,Post complete","Europe, Africa, Asia, Australia and Oceania, North America, South America",2,256,3.45,0,"",null,null,null,null,null,null,null,"5207XX0011.jpg",6,1,2,5,8,1,66,"CE","","IK08","Class I",null,null,null,null,null,3.5,0.39,0.24,null,null,null,null,"5207XX0011.ldt",1,null,null,null,null,0,null,null,null,null,null,null,"LED",16,null,"",null,null,24,null,4000,70,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"","",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"Poland"]
["5210","5210XX0009","ASKER BOLLARD 85CM LED 929LM 3000K DIM.",null,"Luminaire with a contemporary design. For lighting private areas and other architectural concepts",null,"Asker","Bollard","Europe, Africa, Asia, Australia and Oceania, North America, South America",2,2,0.8,0,"",null,null,null,null,null,null,null,"5210XX0009.jpg",7,1,2,3,6,1,66,"CE","","IK10","Class I",null,null,null,null,null,0.85,0.2,0.11,null,null,null,null,"5210XX0009.ldt",1,null,null,null,null,0,null,null,null,null,null,null,"LED",16,null,"",null,null,23,null,3000,80,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"","",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"Poland"]
["5211","5211XX0009","ASKER BOLLARD 85CM LED 966LM 4000K DIM.",null,"Luminaire with a contemporary design. For lighting private areas and other architectural concepts",null,"Asker","Bollard","Europe, Africa, Asia, Australia and Oceania, North America, South America",2,2,0.8,0,"",null,null,null,null,null,null,null,"5211XX0009.jpg",7,1,2,3,6,1,66,"CE","","IK10","Class I",null,null,null,null,null,0.85,0.2,0.11,null,null,null,null,"5211XX0009.ldt",1,null,null,null,null,0,null,null,null,null,null,null,"LED",16,null,"",null,null,24,null,4000,80,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"","",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"Poland"]
["5212","5212XX0009","ASKER BOLLARD 55CM LED 929LM 3000K DIM.",null,"Luminaire with a contemporary design. For lighting private areas and other architectural concepts",null,"Asker","Bollard","Europe, Africa, Asia, Australia and Oceania, North America, South America",2,2,0.5,0,"",null,null,null,null,null,null,null,"5212XX0009.jpg",7,1,2,3,6,1,66,"CE","","IK10","Class I",null,null,null,null,null,0.55000000000000004,0.2,0.11,null,null,null,null,"5212XX0009.ldt",1,null,null,null,null,0,null,null,null,null,null,null,"LED",16,null,"",null,null,23,null,3000,80,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"","",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"Poland"]
["5213","5213XX0009",{"$f":"INDEX(DB,MATCH($A564,ID,0),3)","v":"ASKER BOLLARD 55CM LED 966LM 4000K DIM."},null,"Luminaire with a contemporary design. For lighting private areas and other architectural concepts",null,"Asker",{"$f":"IF(INDEX(DB,MATCH($A564,ID,0),5)=0,\"\",INDEX(DB,MATCH($A564,ID,0),5))","v":"Bollard"},"Europe, Africa, Asia, Australia and Oceania, North America, South America",2,{"$f":"IFERROR(INDEX(TYPMONT,MATCH((INDEX(DB,MATCH($A564,ID,0),31)),ID_RODZ,0),3),\"\")","v":2},0.5,0,{"$f":"IFERROR(IF(INDEX(TYPMONT,MATCH((INDEX(DB,MATCH($A564,ID,0),31)),ID_RODZ,0),6)=0,\"\",INDEX(TYPMONT,MATCH((INDEX(DB,MATCH($A564,ID,0),31)),ID_RODZ,0),6)),\"\")","v":""},null,null,null,null,null,null,null,{"$f":"IF(INDEX(DB,MATCH($A564,ID,0),57)=0,\"\",INDEX(DB,MATCH($A564,ID,0),57))","v":"5213XX0009.jpg"},7,{"$f":"IF(INDEX(DB,MATCH($A564,ID,0),61)=0,\"\",INDEX(DB,MATCH($A564,ID,0),61))","v":1},2,{"$f":"IFERROR(INDEX(TYPMONT,MATCH((INDEX(DB,MATCH($A564,ID,0),31)),ID_RODZ,0),1),\"\")","v":3},{"$f":"IFERROR(INDEX(TYPMONT,MATCH((INDEX(DB,MATCH($A564,ID,0),31)),ID_RODZ,0),2),\"\")","v":6},{"$f":"IF(INDEX(DB,MATCH($A564,ID,0),59)=0,\"\",INDEX(DB,MATCH($A564,ID,0),59))","v":1},{"$f":"IFERROR(IF(INDEX(DB,MATCH($A564,ID,0),19)=0,\"\",INDEX(DB,MATCH($A564,ID,0),19)+1),\"\")","v":66},{"$f":"IF(INDEX(DB,MATCH($A564,ID,0),27)=0,\"\",INDEX(DB,MATCH($A564,ID,0),27))","v":"CE"},"",{"$f":"IF(INDEX(DB,MATCH($A564,ID,0),20)=0,\"\",INDEX(DB,MATCH($A564,ID,0),20))","v":"IK10"},{"$f":"IF(INDEX(DB,MATCH($A564,ID,0),21)=0,\"\",INDEX(DB,MATCH($A564,ID,0),21))","v":"Class I"},null,null,null,null,null,0.55000000000000004,0.2,0.11,null,null,null,null,{"$f":"IF(INDEX(DB,MATCH($A564,ID,0),58)=0,\"\",INDEX(DB,MATCH($A564,ID,0),58))","v":"5213XX0009.ldt"},1,null,null,null,null,0,null,null,null,null,null,null,"LED",16,null,{"$f":"IF(INDEX(DB,MATCH($A564,ID,0),60)=0,\"\",INDEX(DB,MATCH($A564,ID,0),60))","v":""},null,null,24,null,{"$f":"IF(INDEX(DB,MATCH($A564,ID,0),22)=0,\"\",INDEX(DB,MATCH($A564,ID,0),22))","v":4000},{"$f":"IF(INDEX(DB,MATCH($A564,ID,0),53)=0,\"\",INDEX(DB,MATCH($A564,ID,0),53))","v":80},null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,{"$f":"IF(INDEX(DB,MATCH($A564,ID,0),29)=0,\"\",INDEX(DB,MATCH($A564,ID,0),29))","v":""},{"$f":"IF(INDEX(DB,MATCH($A564,ID,0),28)=0,\"\",INDEX(DB,MATCH($A564,ID,0),28))","v":""},null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"Poland"]
["5214","5214XX0009","ASKER PRO BOLLARD 55CM LED 828LM SCL 3000K DIM.",null,"Luminaire with a contemporary design For lighting gardens, private areas and other architectural concepts",null,{"$f":"IF(INDEX(DB,MATCH($A565,ID,0),4)=0,\"\",INDEX(DB,MATCH($A565,ID,0),4))","v":"Asker"},"Bollard","Europe, Africa, Asia, Australia and Oceania, North America, South America",2,2,0.5,0,"",null,null,null,null,null,null,null,"5214XX0009.jpg",6,1,2,3,6,1,66,"CE",{"$f":"IFERROR(IF(FIND(\"RENA\",$C565)>0,\"Vehicle resistant\",\"\"),\"\")","v":""},"IK08","Class I",null,null,null,null,null,0.55000000000000004,0.2,0.11,null,null,null,null,"5214XX0009.ldt",1,null,null,null,null,0,null,null,null,null,null,null,"LED",16,null,"",null,null,{"$f":"IF($BO565=4000,24,23)","v":23},null,3000,80,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"","",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"Poland"]
["5215","5215XX0009","ASKER PRO BOLLARD 55CM LED 828LM SCL 4000K DIM.",null,"Luminaire with a contemporary design For lighting gardens, private areas and other architectural concepts",null,"Asker","Bollard","Europe, Africa, Asia, Australia and Oceania, North America, South America",2,2,0.5,0,"",null,null,null,null,null,null,null,"5215XX0009.jpg",6,1,2,3,6,1,66,"CE","","IK08","Class I",null,null,null,null,null,0.55000000000000004,0.2,0.11,null,null,null,null,"5215XX0009.ldt",1,null,null,null,null,0,null,null,null,null,null,null,"LED",16,null,"",null,null,24,null,4000,80,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"","",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"Poland"]
["5216","5216XX0009","ASKER PRO BOLLARD 55CM LED 828LM VSM 3000K DIM.",null,"Luminaire with a contemporary design For lighting gardens, private areas and other architectural concepts",null,"Asker","Bollard","Europe, Africa, Asia, Australia and Oceania, North America, South America",2,2,0.5,0,"",null,null,null,null,null,null,null,"5216XX0009.jpg",4,1,2,3,6,1,66,"CE","","IK08","Class I",null,null,null,null,null,0.55000000000000004,0.2,0.11,null,null,null,null,"5216XX0009.ldt",1,null,null,null,null,0,null,null,null,null,null,null,"LED",16,null,"",null,null,23,null,3000,80,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"","",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"Poland"]
["5217","5217XX0009","ASKER PRO BOLLARD 55CM LED 828LM VSM 4000K DIM.",null,"A luminaire with a contemporary design. For lighting gardens, private areas and other architectural concepts.",null,"Asker","Bollard","Europe, Africa, Asia, Australia and Oceania, North America, South America",2,2,0.5,0,"",null,null,null,null,null,null,null,"5217XX0009.jpg",4,1,2,3,6,1,66,"CE","","IK08","Class I",null,null,null,null,null,0.55000000000000004,0.2,0.11,null,null,null,null,"5217XX0009.ldt",1,null,null,null,null,0,null,null,null,null,null,null,"LED",16,null,"",null,null,24,null,4000,80,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"","",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"Poland"]
["5218","5218XX0009","ASKER PRO BOLLARD 55CM LED 828LM SCL 3000K DALI",null,"A luminaire with a contemporary design. For lighting gardens, private areas and other architectural concepts.",null,"Asker","Bollard","Europe, Africa, Asia, Australia and Oceania, North America, South America",2,2,0.5,0,"",null,null,null,null,null,null,null,"5218XX0009.jpg",6,1,2,3,6,3,66,"CE","","IK08","Class I",null,null,null,null,null,0,0,0,null,null,null,null,"5218XX0009.ldt",1,null,null,null,null,0,null,null,null,null,null,null,"LED",16,null,"",null,null,23,null,3000,80,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"DALI","",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"Poland"]
["5222","5222XX0009","ASKER POLE PRO 300CM LED 2667LM VSM 3000K DALI2",null,"For lighting private areas, parks and other architectural concepts",null,"Asker,Pole","Post,Post complete","Europe, Africa, Asia, Australia and Oceania, North America, South America",2,256,2.95,0,"",null,null,null,null,null,null,null,"5222XX0009.jpg",4,1,2,5,8,3,66,"CE","","IK08","Class I",null,null,null,null,null,0.24,0.48,3,null,null,null,null,"5222XX0009.ldt",1,null,null,null,null,0,null,null,null,null,null,null,"LED",16,null,"",null,null,23,null,3000,70,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"DALI","",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"Poland"]
["5223","5223XX0009","ASKER POLE PRO 300CM LED VSM 4000K DALI2",null,"For lighting private areas, parks and other architectural concepts",null,"Asker","Post","Europe, Africa, Asia, Australia and Oceania, North America, South America",2,256,2.95,0,"",null,null,null,null,null,null,null,"5223XX0009.jpg",4,1,2,5,8,3,66,"CE","","IK08","Class I",null,null,null,null,null,0.24,0.48,3,null,null,null,null,"5223XX0009.ldt",1,null,null,null,null,0,null,null,null,null,null,null,"LED",16,null,"",null,null,24,null,4000,70,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"DALI","",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"Poland"]
["5224","5224XX0009","ASKER POLE PRO 300CM LED 2667LM VSM 3000K DIM.",null,"For lighting outdoor areas, parks and other architectural concepts",null,"Asker,Pole","Post,Post complete","Europe, Africa, Asia, Australia and Oceania, North America, South America",2,256,2.95,0,"",null,null,null,null,null,null,null,"5224XX0009.jpg",4,1,2,5,8,1,66,"CE","","IK08","Class I",null,null,null,null,null,0.24,0.48,3,null,null,null,null,"5224XX0009.ldt",1,null,null,null,null,0,null,null,null,null,null,null,"LED",16,null,"",null,null,23,null,3000,70,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"","",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"Poland"]
["5225","5225XX0009","ASKER POLE PRO 300CM LED 2772LM VSM 4000K DIM.",null,"For lighting outdoor areas, parks and other architectural concepts",null,"Asker,Pole","Post,Post complete","Europe, Africa, Asia, Australia and Oceania, North America, South America",2,256,2.95,0,"",null,null,null,null,null,null,null,"5225XX0009.jpg",4,1,2,5,8,1,66,"CE","","IK08","Class I",null,null,null,null,null,0.24,0.48,3,null,null,null,null,"5225XX0009.ldt",1,null,null,null,null,0,null,null,null,null,null,null,"LED",16,null,"",null,null,24,null,4000,70,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"","",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"Poland"]
["5226","5226XX0009","ASKER POLE PRO 300CM LED 2628LM T2-L 3000K DALI2",null,"For lighting outdoor areas, parks and other architectural concepts",null,"Asker,Pole","Post,Post complete","Europe, Africa, Asia, Australia and Oceania, North America, South America",2,256,2.95,0,"",null,null,null,null,null,null,null,"5226XX0009.jpg",6,1,2,5,8,3,66,"CE","","IK08","Class I",null,null,null,null,null,0.24,0.48,3,null,null,null,null,"5226XX0009.ldt",1,null,null,null,null,0,null,null,null,null,null,null,"LED",16,null,"",null,null,23,null,3000,70,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"DALI","",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"Poland"]
["5227","5227XX0009","ASKER POLE PRO 300CM LED 2910LM T2-L 4000K DALI2",null,"For lighting outdoor areas, parks and other architectural concepts",null,"Asker,Pole","Post,Post complete","Europe, Africa, Asia, Australia and Oceania, North America, South America",2,256,2.95,0,"",null,null,null,null,null,null,null,"5227XX0009.jpg",6,1,2,5,8,3,66,"CE","","IK08","Class I",null,null,null,null,null,0.24,0.48,3,null,null,null,null,"5227XX0009.ldt",1,null,null,null,null,0,null,null,null,null,null,null,"LED",16,null,"",null,null,24,null,4000,70,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"DALI","",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"Poland"]
["5228","5228XX0009","ASKER POLE PRO 300CM LED 2687LM T2-L 3000K DIM.",null,"For lighting outdoor areas, parks and other architectural concepts",null,"Asker,Pole","Post,Post complete","Europe, Africa, Asia, Australia and Oceania, North America, South America",2,256,2.95,0,"",null,null,null,null,null,null,null,"5228XX0009.jpg",6,1,2,5,8,1,66,"CE","","IK08","Class I",null,null,null,null,null,0.24,0.48,3,null,null,null,null,"5228XX0009.ldt",1,null,null,null,null,0,null,null,null,null,null,null,"LED",16,null,"",null,null,23,null,3000,70,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"","",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"Poland"]
["5229","5229XX0009","ASKER POLE PRO 300CM LED 2910LM T2-L 4000K DIM.",null,"For lighting outdoor areas, parks and other architectural concepts",null,"Asker,Pole","Post,Post complete","Europe, Africa, Asia, Australia and Oceania, North America, South America",2,256,2.95,0,"",null,null,null,null,null,null,null,"5229XX0009.jpg",6,1,2,5,8,1,66,"CE","","IK08","Class I",null,null,null,null,null,0.24,0.48,3,null,null,null,null,"5229XX0009.ldt",1,null,null,null,null,0,null,null,null,null,null,null,"LED",16,null,"",null,null,24,null,4000,70,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"","",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"Poland"]
["5253","5253XX0009","NORDLAND CEILING/WALL LED 3796LM 3000K DALI2",null,"A ceiling type luminaire with a modern design For lighting private areas and other architectural concepts",null,"Nordland","Wall,Ceiling","Europe, Africa, Asia, Australia and Oceania, North America, South America",2,4,0,2.5,"Ceiling mounted",null,null,null,null,null,null,null,"5253XX0009.jpg",8,1,2,2,2,3,66,"CE","","IK10","Class I",null,null,null,null,null,0.28000000000000003,0.28000000000000003,0.1,null,null,null,null,"5253XX0009.ldt",1,null,null,null,null,0,null,null,null,null,1,null,"LED",16,null,"",null,null,23,null,3000,80,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"DALI","",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"Poland"]
["5255","5255XX0009","NORDLAND CEILING/WALL LED 3996LM 4000K DALI2",null,"A ceiling type luminaire with a modern design For lighting private areas and other architectural concepts",null,"Nordland","Wall,Ceiling","Europe, Africa, Asia, Australia and Oceania, North America, South America",2,4,0,2.5,"Ceiling mounted",null,null,null,null,null,null,null,"5255XX0009.jpg",8,1,2,2,2,3,66,"CE","","IK10","Class I",null,null,null,null,null,0.28000000000000003,0.28000000000000003,0.1,null,null,null,null,"5255XX0009.ldt",1,null,null,null,null,0,null,null,null,null,1,null,"LED",16,null,"",null,null,24,null,4000,80,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"DALI","",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"Poland"]
["537","537XX0014","RONDANE CEILING/WALL LED 1059LM 3000K DIM.",null,"A ceiling-type luminaire with a modern design",null,"Rondane","Wall,Ceiling","Europe, Africa, Asia, Australia and Oceania, North America, South America",2,4,0,2.5,"Ceiling mounted",null,null,null,null,null,null,null,"537XX0014.jpg",8,1,1,2,2,1,66,"CE","","IK10","Class I",null,null,null,null,null,0,0,0,null,null,null,null,"537XX0014.ldt",1,null,null,null,null,3,null,null,null,null,1,null,"LED",16,null,"",null,null,23,null,3000,80,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"","",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"Poland"]
["539","539XX0011","RONDANE CEILING/WALL LED 1950LM 3000K ON/OFF",null,"A ceiling-type luminaire with a modern design",null,"Rondane","Wall,Ceiling","Europe, Africa, Asia, Australia and Oceania, North America, South America",2,4,0,2.5,"Ceiling mounted",null,null,null,null,null,null,null,"539XX0011.jpg",8,1,1,2,2,4,66,"CE","","IK10","Class I",null,null,null,null,null,0,0,0,null,null,null,null,"539XX0011.ldt",1,null,null,null,null,3,null,null,null,null,1,null,"LED",16,null,"",null,null,23,null,3000,80,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"","",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"Poland"]
["542","542XX0011","BORNHOLM CEILING/WALL LED 1950LM 3000K ON/OFF",null,"A ceiling lauminaire with a modern design",null,"Bornholm","Wall,Ceiling","Europe, Africa, Asia, Australia and Oceania, North America, South America",2,4,0,{"$f":"IF(K582=4,2.5,IF(K582=64,0.5,0))","v":2.5},"Ceiling mounted",null,null,null,null,null,null,null,"542XX0011.jpg",8,1,1,2,2,4,66,"CE","","IK10","Class I",null,null,null,null,null,0,0,0,null,null,null,null,"542XX0011.ldt",1,null,null,null,null,4,null,null,null,null,1,null,"LED",16,null,"",null,null,23,null,3000,80,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"","",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"Poland"]
["545",{"$f":"INDEX(DB,MATCH($A583,ID,0),2)","v":"545XX0009"},"BORNHOLM CEILING/WALL LED 1150LM 4000K MD",null,{"$f":"IF(INDEX(DB,MATCH($A583,ID,0),35)=0,\"\",INDEX(DB,MATCH($A583,ID,0),35))","v":"A ceiling type luminaire with a modern design"},null,"Bornholm","Wall","Europe, Africa, Asia, Australia and Oceania, North America, South America",2,4,0,2.5,"Ceiling mounted",null,null,null,null,null,null,null,"545XX0009.jpg",{"$f":"IF((IFERROR(INDEX(BRYLA_FOTO,MATCH(INDEX(DB,MATCH($A583,ID,0),62),ID_BRYLAFOTO,0),6),\"\"))<>0,IFERROR(INDEX(BRYLA_FOTO,MATCH(INDEX(DB,MATCH($A583,ID,0),62),ID_BRYLAFOTO,0),6),\"\"),\"\")","v":8},1,1,2,2,3,66,"CE","","","Class I",null,null,null,null,null,{"$f":"INDEX(DB,MATCH($A583,ID,0),24)","v":0.28999999999999998},{"$f":"INDEX(DB,MATCH($A583,ID,0),25)","v":0.28999999999999998},{"$f":"INDEX(DB,MATCH($A583,ID,0),26)","v":0.09},null,null,null,null,"545XX0009.ldt",1,null,null,null,null,4,null,null,null,null,1,null,"LED",16,null,"",null,null,24,null,4000,80,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"","Daylight sensor,Motion sensor",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"Poland"]
["548","548XX0009","RONDANE CEILING/WALL LED 1080LM 3000K MD",null,"A ceiling type luminaire with a modern design",null,"Rondane","Wall,Ceiling","Europe, Africa, Asia, Australia and Oceania, North America, South America",2,4,0,2.5,"Ceiling mounted",null,null,null,null,null,null,null,"548XX0009.jpg",8,1,1,2,2,3,66,"CE","","IK10","Class I",null,null,null,null,null,0.26,0.26,0.1,null,null,null,null,"548XX0009.ldt",{"$f":"IF($BJ584=\"\",1,0)","v":1},null,null,null,null,3,null,null,null,null,1,null,"LED",16,null,"",null,null,23,null,3000,80,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"","Daylight sensor,Motion sensor",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"Poland"]
["549","549XX0009","RONDANE CEILING/WALL LED 1150LM 4000K MD",null,"A ceiling type luminaire with a modern design",null,"Rondane","Wall,Ceiling","Europe, Africa, Asia, Australia and Oceania, North America, South America",2,4,0,2.5,"Ceiling mounted",null,null,null,null,null,null,null,"549XX0009.jpg",8,1,1,2,2,3,66,"CE","","IK10","Class I",null,null,null,null,null,0.26,0.26,0.1,null,null,null,null,"549XX0009.ldt",1,null,null,null,null,3,null,null,null,null,1,null,"LED",16,null,"",null,null,24,null,4000,80,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"","Daylight sensor,Motion sensor",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"Poland"]
["553","553XX0010","NARVIK II BOLLARD LED 1940LM 3000K DIM.",null,"A bollard luminaire with a stable and durable structure. For lighting private and public areas",null,"Narvik","Bollard","Europe, Africa, Asia, Australia and Oceania, North America, South America",2,2,0.7,0,"",null,null,null,null,null,null,null,"553XX0010.png",4,1,1,3,6,1,66,"CE","","IK10","Class II",null,null,null,null,null,0.24,0.24,0.95,null,null,null,null,"553XX0010.LDT",1,null,null,null,null,0,null,null,null,null,null,null,"LED",16,null,"",null,null,23,null,3000,80,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"","",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"Poland"]
["557","557XX0017","NARVIK BOLLARD LED 3137LM 3000K ON/OFF",null,"A bollard luminaire with a stable and durable structure. For lighting private and public areas",null,"Narvik","Bollard","Europe, Africa, Asia, Australia and Oceania, North America, South America",2,2,0.7,0,"",null,null,null,null,null,null,null,"557XX0017.jpg",4,1,1,3,6,4,66,"CE","","IK10","Class I",null,null,null,null,null,0.24,0.24,0.95,null,null,null,null,"557XX0017.ldt",1,null,null,null,null,0,null,null,null,null,null,null,"LED",16,null,"",null,null,23,null,3000,80,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"","",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"Poland"]
["559","559XX0010","NARVIK II BOLLARD LED 1940LM 3000K DIM.",null,"A bollard luminaire with a stable and durable structure. For lighting private and public areas.",null,"Narvik","Bollard","Europe, Africa, Asia, Australia and Oceania, North America, South America",2,2,0.7,0,"",null,null,null,null,null,null,null,"559XX0010.png",4,1,1,3,6,1,66,"CE","","IK10","Class II",null,null,null,null,null,0.24,0.24,0.95,null,null,null,null,"559XX0010.ldt",1,null,null,null,null,0,null,null,null,null,null,null,"LED",16,null,"",null,null,23,null,3000,80,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"","",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"Poland"]
["577","577XX0309","VISBY POLE-TOP LED 2950LM 3000K",null,"Pole top luminaire for installation on a lighting pole with Ø60mm mounting cap.",null,"Visby","Post,Head","Europe, Africa, Asia, Australia and Oceania, North America, South America",2,512,3.85,0,"",null,null,null,null,null,null,null,"577XX0309.jpg",9,1,1,5,9,4,66,"CE","","","Class I",null,null,null,null,null,0,0,0,null,null,null,null,"577XX0309.ldt",1,null,null,null,null,0,null,null,null,null,null,null,"LED",16,null,"",null,null,23,null,3000,80,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"","",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"Poland"]
["596","596XX0011","KIRUNA WALL LED 1950LM 3000K",null,"Luminaire with stable and durable construction. For use in private and public areas requiring high resistance to external mechanical damage.",null,"Kiruna","Wall,Ceiling","Europe, Africa, Asia, Australia and Oceania, North America, South America",2,4,0,2.5,"",null,null,null,null,null,null,null,"596XX0011.jpg",7.9,1,1,2,2,4,66,"CE","","IK10","Class I",null,null,null,null,null,0,0,0,null,null,null,null,"596XX0011.ldt",1,null,null,null,null,4,null,null,null,null,null,null,"LED",16,null,"",null,null,23,null,3000,80,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"","",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"Poland"]
["6031","6031XX0010","NAMSOS WALL-RECESSED LED 2006LM 4000K DALI2",null,"The luminaire is adapted to illuminate stairs, steps, staircases, pathways for ceiling lighting and implementation of other architectural concepts",null,"Namsos","Recessed","Europe, Africa, Asia, Australia and Oceania, North America, South America",2,64,0,0.5,"",null,null,null,null,null,null,null,"6031XX0010.jpg",7,1,2,2,1,3,66,"CE","","IK08","Class I",null,null,null,null,null,0.22,0.22,0.12,null,null,null,null,"6031XX0010.ldt",1,null,null,null,null,4,null,null,null,null,null,null,"LED",16,null,"",null,null,24,null,4000,80,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"DALI","",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"Poland"]
["6032","6032XX0010","NAMSOS WALL-RECESSED LED 1891LM 3000K DALI2",null,"The luminaire is adapted to illuminate stairs, steps, staircases, pathways for ceiling lighting and implementation of other architectural concepts",null,"Namsos","Recessed","Europe, Africa, Asia, Australia and Oceania, North America, South America",2,64,0,0.5,"",null,null,null,null,null,null,null,"6032XX0010.jpg",7,1,2,2,1,3,66,"CE","","IK08","Class I",null,null,null,null,null,0.22,0.22,0.12,null,null,null,null,"6032XX0010.ldt",1,null,null,null,null,4,null,null,null,null,null,null,"LED",16,null,"",null,null,23,null,3000,80,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"DALI","",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"Poland"]
["6033","6033XX0009","NAMSOS BOLLARD 95CM LED 1891LM 3000K DALI2",null,"Luminaire with a modern design. For lighting gardens and other private and public areas",null,"Namsos","Bollard","Europe, Africa, Asia, Australia and Oceania, North America, South America",2,2,0.71,0,"",null,null,null,null,null,null,null,"6033XX0009.jpg",7,1,2,3,6,3,66,"CE","","IK07","Class I",null,null,null,null,null,0.24,0.12,0.95,null,null,null,null,"6033XX0009.ldt",1,null,null,null,null,1,null,null,null,null,null,null,"LED",16,null,"",null,null,23,null,3000,80,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"DALI","",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"Poland"]
["6034","6034XX0009","NAMSOS BOLLARD 65CM LED 1891LM 3000K DALI2",null,"Luminaire with a modern design. For lighting gardens and other private and public areas",null,"Namsos","Bollard","Europe, Africa, Asia, Australia and Oceania, North America, South America",2,2,0.41,0,"",null,null,null,null,null,null,null,"6034XX0009.jpg",7,1,2,3,6,3,66,"CE","","IK08","Class I",null,null,null,null,null,0.24,0.12,0.65,null,null,null,null,"6034XX0009.ldt",1,null,null,null,null,1,null,null,null,null,null,null,"LED",16,null,"",null,null,23,null,3000,80,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"DALI","",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"Poland"]
["6035","6035XX0009","NAMSOS BOLLARD 95CM LED 2006LM 4000K DALI2",null,"Luminaire with a modern design. For lighting gardens and other private and public areas",null,"Namsos","Bollard","Europe, Africa, Asia, Australia and Oceania, North America, South America",2,2,0.71,0,"",null,null,null,null,null,null,null,"6035XX0009.jpg",7,1,2,3,6,3,66,"CE","","","Class I",null,null,null,null,null,0.24,0.12,0.95,null,null,null,null,"6035XX0009.ldt",1,null,null,null,null,1,null,null,null,null,null,null,"LED",16,null,"",null,null,24,null,4000,80,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"DALI","",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"Poland"]
["6036","6036XX0009","NAMSOS BOLLARD 65CM LED 2006LM 4000K DALI2",null,"Luminaire with a modern design. For lighting gardens and other private and public areas",null,"Namsos","Bollard","Europe, Africa, Asia, Australia and Oceania, North America, South America",2,2,0.41,0,"",null,null,null,null,null,null,null,"6036XX0009.jpg",7,1,2,3,6,3,66,"CE","","IK08","Class I",null,null,null,null,null,0.24,0.12,0.65,null,null,null,null,"6036XX0009.ldt",1,null,null,null,null,1,null,null,null,null,null,null,"LED",16,null,"",null,null,24,null,4000,80,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"DALI","",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"Poland"]
["6081","6081XX0009","EGERSUND PARK BOLLARD 105CM LED 1462LM 4000K DIM.",null,"Luminaire with a contemporary design. For garden illumination and other private and public areas",null,"Egersund,Park","Bollard","Europe, Africa, Asia, Australia and Oceania, North America, South America",2,2,1.01,0,"",null,null,null,null,null,null,null,"6081XX0009.png",3,1,1,3,6,1,66,"CE","","IK08","Class II",null,null,null,null,null,1.05,0.12,0.12,null,null,null,null,"6081XX0009.ldt",1,null,null,null,null,1,null,null,null,null,null,null,"LED",16,null,"",null,null,24,null,4000,80,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"","",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"Poland"]
["6082","6082XX0009","EGERSUND PARK BOLLARD 105CM LED 3363LM 3000K DALI2",null,"Luminaire with a contemporary design For lighting gardens and other private and public areas",null,"Egersund,Park","Bollard","Europe, Africa, Asia, Australia and Oceania, North America, South America",2,2,1.01,0,"",null,null,null,null,null,null,null,"6082XX0009.png",3,1,1,3,6,3,66,"CE","","IK08","Class I",null,null,null,null,null,1.05,0.12,0.12,null,null,null,null,"6082XX0009.ldt",1,null,null,null,null,1,null,null,null,null,null,null,"LED",16,null,"",null,null,23,null,3000,80,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"DALI","",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"Poland"]
["6083","6083XX0009","EGERSUND PARK BOLLARD 105CM LED 3566LM 4000K DALI2",null,"Luminaire with a contemporary design For lighting gardens and other private and public areas",null,"Egersund,Park","Bollard","Europe, Africa, Asia, Australia and Oceania, North America, South America",2,2,1.01,0,"",null,null,null,null,null,null,null,"6083XX0009.png",3,1,1,3,6,3,66,"CE","","IK08","Class I",null,null,null,null,null,1.05,0.12,0.12,null,null,null,null,"6083XX0009.ldt",1,null,null,null,null,1,null,null,null,null,null,null,"LED",16,null,"",null,null,24,null,4000,80,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"DALI","",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"Poland"]
["6090","6090XX0009","EGERSUND PARK BOLLARD 85CM LED 1370LM 3000K DIM.",null,"Luminaire with a contemporary design. For garden illumination and other private and public areas",null,"Egersund,Park","Bollard","Europe, Africa, Asia, Australia and Oceania, North America, South America",2,2,0.81,0,"",null,null,null,null,null,null,null,"6090XX0009.png",3,1,1,3,6,1,66,"CE","","IK08","Class II",null,null,null,null,null,0.85,0.12,0.12,null,null,null,null,"6090XX0009.ldt",1,null,null,null,null,1,null,null,null,null,null,null,"LED",16,null,"",null,null,23,null,3000,80,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"","",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"Poland"]
["6091","6091XX0009","EGERSUND PARK BOLLARD 85CM LED 1462LM 4000K DIM.",null,"Luminaire with a contemporary design. For garden illumination and other private and public areas",null,"Egersund,Park","Bollard","Europe, Africa, Asia, Australia and Oceania, North America, South America",2,2,0.81,0,"",null,null,null,null,null,null,null,"6091XX0009.png",3,1,1,3,6,1,66,"CE","","IK08","Class II",null,null,null,null,null,0.85,0.12,0.12,null,null,null,null,"6091XX0009.ldt",1,null,null,null,null,1,null,null,null,null,null,null,"LED",16,null,"",null,null,24,null,4000,80,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"","",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"Poland"]
["6092","6092XX0009","EGERSUND PARK BOLLARD 85CM LED 3363LM 3000K DALI2",null,"Luminaire with a contemporary design For lighting gardens and other private and public areas",null,"Egersund,Park","Bollard","Europe, Africa, Asia, Australia and Oceania, North America, South America",2,2,0.81,0,"",null,null,null,null,null,null,null,"6092XX0009.png",3,1,1,3,6,3,66,"CE","","IK08","Class I",null,null,null,null,null,0.85,0.12,0.12,null,null,null,null,"6092XX0009.ldt",1,null,null,null,null,1,null,null,null,null,null,null,"LED",16,null,"",null,null,23,null,3000,80,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"DALI","",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"Poland"]
["6093","6093XX0009","EGERSUND PARK BOLLARD 85CM LED 3566LM 4000K DALI2",null,"Luminaire with a contemporary design For lighting gardens and other private and public areas",null,"Egersund,Park","Bollard","Europe, Africa, Asia, Australia and Oceania, North America, South America",2,2,0.81,0,"",null,null,null,null,null,null,null,"6093XX0009.png",3,1,1,3,6,3,66,"CE","","IK08","Class I",null,null,null,null,null,0.85,0.12,0.12,null,null,null,null,"6093XX0009.ldt",1,null,null,null,null,1,null,null,null,null,null,null,"LED",16,null,"",null,null,24,null,4000,80,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"DALI","",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"Poland"]
["6105","6105XX0311","EGERSUND PARK LIGHT LUMINAIRES POLE 250CM LED 1370LM 3000K DIM.",null,"Pole mounted luminaire ø120mm",null,"Egersund,Park","Post,Post complete","Europe, Africa, Asia, Australia and Oceania, North America, South America",2,512,2.31,0,"",null,null,null,null,null,null,null,"6105XX0311.jpg",3,1,1,5,9,1,66,"CE","","","Class II",null,null,null,null,null,0,0,0,null,null,null,null,"6105XX0311.ldt",1,null,null,null,null,1,null,null,null,null,null,null,"LED",16,null,"",null,null,23,null,3000,80,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"","",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"Poland"]
["6106","6106XX0011","EGERSUND PARK POLE-TOP LED 1370LM 3000K DIM.",null,"Pole mounted luminaire ø120mm",null,"Egersund,Park","Post,Head","Europe, Africa, Asia, Australia and Oceania, North America, South America",2,512,2.31,0,"",null,null,null,null,null,null,null,"6106XX0011.png",3,1,1,5,9,1,66,"CE","","IK05","Class II",null,null,null,null,null,0.12,0.12,0.52,null,null,null,null,"6106XX0011.ldt",1,null,null,null,null,1,null,null,null,null,null,null,"LED",16,null,"",null,null,23,null,3000,80,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"","",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"Poland"]
["6108","6108XX0011","EGERSUND PARK POLE-TOP LED 1462LM 4000K DIM.",null,"Pole mounted luminaire ø120mm",null,"Egersund,Park","Post,Head","Europe, Africa, Asia, Australia and Oceania, North America, South America",2,512,2.31,0,"",null,null,null,null,null,null,null,"6108XX0011.png",3,1,1,5,9,1,66,"CE","","","Class II",null,null,null,null,null,0,0,0,null,null,null,null,"6108XX0011.ldt",1,null,null,null,null,1,null,null,null,null,null,null,"LED",16,null,"",null,null,24,null,4000,80,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"","",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"Poland"]
["610","610XX0011","BERLIN WALL E27",null,"Classic design plafon type luminaire.",null,"Berlin","Wall","Europe, Africa, Asia, Australia and Oceania, North America, South America",2,4,0,2.5,"",null,null,null,null,null,null,null,"610XX0011.jpg",7,1,1,2,2,4,55,"CE","","IK10","Class I",null,null,null,null,null,0.27,0.27,0.14000000000000001,null,null,null,null,"610XX0011.ldt",0,null,null,null,null,3,null,null,null,null,null,null,"LED",16,null,"E27",null,null,23,null,"",80,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"","",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"Poland"]
["6111","6111XX0309","EGERSUND PARK PRO LIGHT LUMINAIRES POLE 250CM LED 3363LM 3000K DALI2",null,"Pole mounted luminaire, mounted on a ø120mm base",null,"Egersund,Park","Post,Post complete","Europe, Africa, Asia, Australia and Oceania, North America, South America",2,512,2.31,0,"",null,null,null,null,null,null,null,"6111XX0309.png",3,1,1,5,9,3,66,"CE","","","Class I",null,null,null,null,null,0.12,0.12,2.5,null,null,null,null,"6111XX0309.ldt",1,null,null,null,null,1,null,null,null,null,null,null,"LED",16,null,"",null,null,23,null,3000,80,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"DALI","",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"Poland"]
["6112","6112XX0309","EGERSUND PARK PRO LIGHT LUMINAIRES POLE 250CM LED 3566LM 4000K DALI2",null,"Pole mounted luminaire, mounted on a ø120mm base",null,"Egersund,Park","Post,Post complete","Europe, Africa, Asia, Australia and Oceania, North America, South America",2,512,2.31,0,"",null,null,null,null,null,null,null,"6112XX0309.png",3,1,1,5,9,3,66,"CE","","","Class I",null,null,null,null,null,0.12,0.12,2.5,null,null,null,null,"6112XX0309.ldt",1,null,null,null,null,1,null,null,null,null,null,null,"LED",16,null,"",null,null,24,null,4000,80,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"DALI","",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"Poland"]
["6113","6113XX0309","EGERSUND PARK PRO LIGHT LUMINAIRES POLE 250CM LED 3363LM 3000K DALI2",null,"Pole mounted luminaire, mounted on a ø120mm base",null,"Egersund,Park","Post,Post complete","Europe, Africa, Asia, Australia and Oceania, North America, South America",2,512,2.31,0,"",null,null,null,null,null,null,null,"6113XX0309.png",3,1,1,5,9,3,66,"CE","","","Class I",null,null,null,null,null,0.12,0.12,2.5,null,null,null,null,"6113XX0309.ldt",1,null,null,null,null,1,null,null,null,null,null,null,"LED",16,null,"",null,null,23,null,3000,80,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"DALI","",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"Poland"]
["6114","6114XX0009","EGERSUND PARK PRO POLE-TOP LED 3363LM 3000K DALI2",null,"Pole mounted luminaire ø120mm",null,"Egersund,Park","Post,Head","Europe, Africa, Asia, Australia and Oceania, North America, South America",2,512,2.31,0,"",null,null,null,null,null,null,null,"6114XX0009.png",3,1,1,5,9,3,66,"CE","","","Class I",null,null,null,null,null,0.12,0.12,0.66,null,null,null,null,"6114XX0009.ldt",1,null,null,null,null,1,null,null,null,null,null,null,"LED",16,null,"",null,null,23,null,3000,80,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"DALI","",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"Poland"]
["6115","6115XX0309","EGERSUND PARK PRO LIGHT LUMINAIRES POLE 250CM LED 3566LM 4000K DALI2",null,"Pole mounted luminaire, mounted on a ø120mm base",null,"Egersund,Park","Post,Post complete","Europe, Africa, Asia, Australia and Oceania, North America, South America",2,512,2.31,0,"",null,null,null,null,null,null,null,"6115XX0309.png",3,1,1,5,9,3,66,"CE","","","Class I",null,null,null,null,null,0.12,0.12,2.5,null,null,null,null,"6115XX0309.ldt",1,null,null,null,null,1,null,null,null,null,null,null,"LED",16,null,"",null,null,24,null,4000,80,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"DALI","",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"Poland"]
["6116","6116XX0009","EGERSUND PARK PRO POLE-TOP 250CM LED 3566LM 4000K DALI2",null,"Pole mounted luminaire ø120mm",null,"Egersund,Park","Post,Head","Europe, Africa, Asia, Australia and Oceania, North America, South America",2,512,2.31,0,"",null,null,null,null,null,null,null,"6116XX0009.png",3,1,1,5,9,3,66,"CE","","","Class I",null,null,null,null,null,0.12,0.12,0.66,null,null,null,null,"6116XX0009.ldt",1,null,null,null,null,1,null,null,null,null,null,null,"LED",16,null,"",null,null,24,null,4000,80,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"DALI","",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"Poland"]
["6118","6118XX0309","EGERSUND PARK BOLLARD 250CM LED 1170LM 4000K DIM.",null,"Pole luminaire, mounted ø120mm.",null,"Egersund,Park","Post,Post complete","Europe, Africa, Asia, Australia and Oceania, North America, South America",2,2,2.31,0,"",null,null,null,null,null,null,null,"6118XX0309.jpg",7,1,1,3,6,1,66,"CE","","","Class I",null,null,null,null,null,0,0,0,null,null,null,null,"6118XX0309.ldt",1,null,null,null,null,1,null,null,null,null,null,null,"LED",16,null,"",null,null,24,null,4000,80,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"","",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"Poland"]
["611","611XX0010","BERLIN WALL E27",null,"Classic design plafon type luminaire for normal use.",null,"Berlin","Wall","Europe, Africa, Asia, Australia and Oceania, North America, South America",2,4,0,2.5,"",null,null,null,null,null,null,null,"611XX0010.jpg",7,1,1,2,2,4,55,"CE","","IK10","Class I",null,null,null,null,null,0.27,0.27,0.14000000000000001,null,null,null,null,"611XX0010.ldt",0,null,null,null,null,3,null,null,null,null,null,null,"LED",16,null,"E27",null,null,23,null,"",80,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"","",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"Poland"]
["6120","6120XX0010","BORG BOLLARD BOLLARD 35CM LED 2093LM 3000K DIM.",null,"Luminaire with contemporary design. For lighting gardens and other private and public areas",null,"Borg","Bollard","Europe, Africa, Asia, Australia and Oceania, North America, South America",2,2,0.32,0,"",null,null,null,null,null,null,null,"6120XX0010.png",3,1,1,3,6,1,66,"CE","","IK08","Class I",null,null,null,null,null,0.2,0.2,0.35,null,null,null,null,"6120XX0010.ldt",1,null,null,null,null,0,null,null,null,null,null,null,"LED",16,null,"",null,null,23,null,3000,80,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"","",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"Poland"]
["6121","6121XX0010","BORG BOLLARD BOLLARD 35CM LED 2214LM 4000K DIM.",null,"Luminaire with contemporary design. For lighting gardens and other private and public areas",null,"Borg","Bollard","Europe, Africa, Asia, Australia and Oceania, North America, South America",2,2,0.32,0,"",null,null,null,null,null,null,null,"6121XX0010.png",3,1,1,3,6,1,66,"CE","","IK08","Class I",null,null,null,null,null,0.2,0.2,0.35,null,null,null,null,"6121XX0010.ldt",1,null,null,null,null,0,null,null,null,null,null,null,"LED",16,null,"",null,null,24,null,4000,80,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"","",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"Poland"]
["6122","6122XX0009","BORG BOLLARD BOLLARD 35CM LED 2093LM 3000K DALI2",null,"Luminaire with contemporary design. For lighting gardens, other private areas and architectural concepts",null,"Borg","Bollard","Europe, Africa, Asia, Australia and Oceania, North America, South America",2,2,0.32,0,"",null,null,null,null,null,null,null,"6122XX0009.png",3,1,1,3,6,3,66,"CE","","IK08","Class I",null,null,null,null,null,0.2,0.2,0.35,null,null,null,null,"6122XX0009.ldt",1,null,null,null,null,0,null,null,null,null,null,null,"LED",16,null,"",null,null,23,null,3000,80,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"DALI","",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"Poland"]
["6123","6123XX0009","BORG BOLLARD BOLLARD 35CM LED 2216LM 4000K DALI2",null,"Luminaire with a contemporary design. For garden lighting and other private areas and architectural concepts",null,"Borg","Bollard","Europe, Africa, Asia, Australia and Oceania, North America, South America",2,2,0.32,0,"",null,null,null,null,null,null,null,"6123XX0009.png",3,1,1,3,6,3,66,"CE","","IK08","Class I",null,null,null,null,null,0.2,0.2,0.35,null,null,null,null,"6123XX0009.ldt",1,null,null,null,null,0,null,null,null,null,null,null,"LED",16,null,"",null,null,24,null,4000,80,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"DALI","",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"Poland"]
["6140","6140XX0009","HAMMERFEST POLE-TOP LED 4246LM 3000K ON/OFF",null,"Mounted on a telescopic lighting pole with a cap diameter Ø60mm. Other accessories have to be ordered separately.",null,"Hammerfest","Post,Head","Europe, Africa, Asia, Australia and Oceania, North America, South America",2,512,4,0,"",null,null,null,null,null,null,null,"6140XX0009.jpg",7,1,1,5,9,4,66,"CE","","IK07","Class I",null,null,null,null,null,0.55000000000000004,0.55000000000000004,0.76,null,null,null,null,"6140XX0009.ldt",1,null,null,null,null,0,null,null,null,null,null,null,"LED",16,null,"",null,null,23,null,3000,70,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"","",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"Poland"]
["6141","6141XX0010","HAMMERFEST POLE-TOP LED 4311LM 3000K ON/OFF",null,"A mounted luminaire designed to be mounted on a lighting pole with a Ø60mm shaft",null,"Hammerfest","Post,Head","Europe, Africa, Asia, Australia and Oceania, North America, South America",2,512,4,0,"",null,null,null,null,null,null,null,"6141XX0010.jpg",7,1,1,5,9,4,66,"CE","","IK07","Class I",null,null,null,null,null,0.55000000000000004,0.55000000000000004,0.76,null,null,null,null,"6141XX0010.ldt",1,null,null,null,null,0,null,null,null,null,null,null,"LED",16,null,"",null,null,23,null,3000,80,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"","",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"Poland"]
["6146","6146XX0009","HAMMERFEST POLE-TOP 3XLED VSM 3000K DALI2",null,"Mounted luminaire designed to be mounted on a lighting pole with a mounting shaft Ø60mm",null,"Hammerfest","Post,Head","Europe, Africa, Asia, Australia and Oceania, North America, South America",2,512,4,0,"",null,null,null,null,null,null,null,"6146XX0009.jpg",4,1,1,5,9,3,66,"CE","","IK07","Class I",null,null,null,null,null,0.76,0.55000000000000004,0.55000000000000004,null,null,null,null,"6146XX0009.ldt",1,null,null,null,null,0,null,null,null,null,null,null,"LED",16,null,"",null,null,23,null,3000,70,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"DALI","",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"Poland"]
["6148","6148XX0009","HAMMERFEST POLE-TOP 3XLED VSM 4000K DALI2",null,"Mounted luminaire designed to be mounted on a lighting pole with a mounting shaft Ø60mm",null,"Hammerfest","Post,Head","Europe, Africa, Asia, Australia and Oceania, North America, South America",2,512,4,0,"",null,null,null,null,null,null,null,"6148XX0009.jpg",4,1,1,5,9,3,66,"CE","","IK07","Class I",null,null,null,null,null,0.76,0.55000000000000004,0.55000000000000004,null,null,null,null,"6148XX0009.ldt",1,null,null,null,null,0,null,null,null,null,null,null,"LED",16,null,"",null,null,24,null,4000,70,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"DALI","",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"Poland"]
["6150","6150XX0009","BORG POLE-TOP LED 4180LM 3000K ON/OFF",null,"Mounted on a telescopic lighting pole with a cap diameter Ø60mm. Other accessories have to be ordered separately.",null,"Borg","Post,Head","Europe, Africa, Asia, Australia and Oceania, North America, South America",2,512,4,0,"",null,null,null,null,null,null,null,"6150XX0009.jpg",7,1,1,5,9,4,66,"CE","","IK08","Class I",null,null,null,null,null,0.51,0.51,0.15,null,null,null,null,"6150XX0009.ldt",1,null,null,null,null,0,null,null,null,null,null,null,"LED",16,null,"",null,null,23,null,3000,80,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"","",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"Poland"]
["6151","6151XX0009",{"$f":"INDEX(DB,MATCH($A625,ID,0),3)","v":"BORG POLE-TOP LED 4180LM 3000K ON/OFF"},null,"Modern design luminaire mounted on a telescopic lighting pole with a cap diameter Ø60mm. Other accessories have to be ordered separately.",null,"Borg",{"$f":"IF(INDEX(DB,MATCH($A625,ID,0),5)=0,\"\",INDEX(DB,MATCH($A625,ID,0),5))","v":"Post,Head"},"Europe, Africa, Asia, Australia and Oceania, North America, South America",2,{"$f":"IFERROR(INDEX(TYPMONT,MATCH((INDEX(DB,MATCH($A625,ID,0),31)),ID_RODZ,0),3),\"\")","v":512},4,0,{"$f":"IFERROR(IF(INDEX(TYPMONT,MATCH((INDEX(DB,MATCH($A625,ID,0),31)),ID_RODZ,0),6)=0,\"\",INDEX(TYPMONT,MATCH((INDEX(DB,MATCH($A625,ID,0),31)),ID_RODZ,0),6)),\"\")","v":""},null,null,null,null,null,null,null,{"$f":"IF(INDEX(DB,MATCH($A625,ID,0),57)=0,\"\",INDEX(DB,MATCH($A625,ID,0),57))","v":"6151XX0009.jpg"},7,{"$f":"IF(INDEX(DB,MATCH($A625,ID,0),61)=0,\"\",INDEX(DB,MATCH($A625,ID,0),61))","v":1},1,{"$f":"IFERROR(INDEX(TYPMONT,MATCH((INDEX(DB,MATCH($A625,ID,0),31)),ID_RODZ,0),1),\"\")","v":5},{"$f":"IFERROR(INDEX(TYPMONT,MATCH((INDEX(DB,MATCH($A625,ID,0),31)),ID_RODZ,0),2),\"\")","v":9},{"$f":"IF(INDEX(DB,MATCH($A625,ID,0),59)=0,\"\",INDEX(DB,MATCH($A625,ID,0),59))","v":4},{"$f":"IFERROR(IF(INDEX(DB,MATCH($A625,ID,0),19)=0,\"\",INDEX(DB,MATCH($A625,ID,0),19)+1),\"\")","v":66},{"$f":"IF(INDEX(DB,MATCH($A625,ID,0),27)=0,\"\",INDEX(DB,MATCH($A625,ID,0),27))","v":"CE"},"",{"$f":"IF(INDEX(DB,MATCH($A625,ID,0),20)=0,\"\",INDEX(DB,MATCH($A625,ID,0),20))","v":"IK08"},{"$f":"IF(INDEX(DB,MATCH($A625,ID,0),21)=0,\"\",INDEX(DB,MATCH($A625,ID,0),21))","v":"Class I"},null,null,null,null,null,0,0,0,null,null,null,null,{"$f":"IF(INDEX(DB,MATCH($A625,ID,0),58)=0,\"\",INDEX(DB,MATCH($A625,ID,0),58))","v":"6151XX0009.ldt"},1,null,null,null,null,0,null,null,null,null,null,null,"LED",16,null,{"$f":"IF(INDEX(DB,MATCH($A625,ID,0),60)=0,\"\",INDEX(DB,MATCH($A625,ID,0),60))","v":""},null,null,23,null,{"$f":"IF(INDEX(DB,MATCH($A625,ID,0),22)=0,\"\",INDEX(DB,MATCH($A625,ID,0),22))","v":3000},{"$f":"IF(INDEX(DB,MATCH($A625,ID,0),53)=0,\"\",INDEX(DB,MATCH($A625,ID,0),53))","v":80},null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,{"$f":"IF(INDEX(DB,MATCH($A625,ID,0),29)=0,\"\",INDEX(DB,MATCH($A625,ID,0),29))","v":""},{"$f":"IF(INDEX(DB,MATCH($A625,ID,0),28)=0,\"\",INDEX(DB,MATCH($A625,ID,0),28))","v":""},null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"Poland"]
["6154","6154XX0010","BORG PRO POLE-TOP 3XLED 7218LM VSM 3000K D4I",null,"Mounted luminaire designed to be mounted on a lighting pole with mounting shaft Ø60mm",null,{"$f":"IF(INDEX(DB,MATCH($A626,ID,0),4)=0,\"\",INDEX(DB,MATCH($A626,ID,0),4))","v":"Borg"},"Post,Head","Europe, Africa, Asia, Australia and Oceania, North America, South America",2,512,4,0,"",null,null,null,null,null,null,null,"6154XX0010.png",4,1,1,5,9,3,66,"CE",{"$f":"IFERROR(IF(FIND(\"RENA\",$C626)>0,\"Vehicle resistant\",\"\"),\"\")","v":""},"IK08","Class I",null,null,null,null,null,0,0,0,null,null,null,null,"6154XX0010.ldt",1,null,null,null,null,0,null,null,null,null,null,null,"LED",16,null,"",null,null,{"$f":"IF($BO626=4000,24,23)","v":23},null,3000,80,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"","",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"Poland"]
["6155","6155XX0009","BORG POLE-TOP LED 7426LM VSM 4000K DALI2",null,"A mounted luminaire designed to be mounted on a lighting pole with a Ø60mm mounting shaft",null,"Borg","Post,Head","Europe, Africa, Asia, Australia and Oceania, North America, South America",2,512,4,0,"",null,null,null,null,null,null,null,"6155XX0009.png",4,1,1,5,9,3,66,"CE","","IK08","Class I",null,null,null,null,null,0,0,0,null,null,null,null,"6155XX0009.ldt",1,null,null,null,null,0,null,null,null,null,null,null,"LED",16,null,"",null,null,24,null,4000,80,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"DALI","",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"Poland"]
["6156","6156XX0009","BORG POLE-TOP LED 7426LM VSM 4000K D4I",null,"Mounted luminaire designed to be mounted on a lighting pole with a mounting shaft Ø60mm",null,"Borg","Post,Head","Europe, Africa, Asia, Australia and Oceania, North America, South America",2,512,4,0,"",null,null,null,null,null,null,null,"6156XX0009.png",4,1,1,5,9,3,66,"CE","","IK08","Class I",null,null,null,null,null,0.51,0.51,0.15,null,null,null,null,"6156XX0009.ldt",1,null,null,null,null,0,null,null,null,null,null,null,"LED",16,null,"",null,null,24,null,4000,80,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"","",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"Poland"]
["615","615XX0012","BERLIN WALL LED E27 DIM.",null,"Plafond type luminaire with modern design.",null,"Berlin","Wall","Europe, Africa, Asia, Australia and Oceania, North America, South America",2,4,0,2.5,"",null,null,null,null,null,null,null,"615XX0012.jpg",7,1,1,2,2,1,55,"CE","","IK10","Class I",null,null,null,null,null,0.27,0.27,0.14000000000000001,null,null,null,null,"615XX0012.ldt",0,null,null,null,null,3,null,null,null,null,null,null,"LED",16,null,"E27",null,null,23,null,"",80,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"","",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"Poland"]
["6161","6161XX0009","MOSS CEILING/WALL LED 439LM 36D 3000K DIM.",null,"For lighting gardens, private areas, and other architectural concepts. The light direction can also be adjusted vertically",null,"Moss","Spot,Wall","Europe, Africa, Asia, Australia and Oceania, North America, South America",2,4,0,2.5,"Ceiling mounted",null,null,null,null,null,null,null,"6161XX0009.jpg",2,4,1,2,2,1,66,"CE","","","Class I",null,null,null,null,null,0.08,0.08,0.13,null,null,null,null,"6161XX0009.ldt",1,null,null,null,null,4,null,null,null,null,1,null,"LED",16,null,"",null,null,23,null,3000,80,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"","",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"Poland"]
["6163","6163XX0009","MOSS CEILING/WALL LED 840LM 36D 3000K DIM.",null,"For lighting gardens, private areas, and other architectural concepts, The light direction can also be adjusted vertically",null,"Moss","Spot,Wall","Europe, Africa, Asia, Australia and Oceania, North America, South America",2,4,0,2.5,"Ceiling mounted",null,null,null,null,null,null,null,"6163XX0009.jpg",2,4,1,2,2,1,66,"CE","","","Class I",null,null,null,null,null,0,0,0,null,null,null,null,"6163XX0009.ldt",1,null,null,null,null,4,null,null,null,null,1,null,"LED",16,null,"",null,null,23,null,3000,80,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"","",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"Poland"]
["6164","6164XX0009","MOSS CEILING/WALL LED 891LM 36D 4000K DIM.",null,"For lighting gardens, private areas, and other architectural concepts, The light direction can also be adjusted vertically",null,"Moss","Spot,Wall","Europe, Africa, Asia, Australia and Oceania, North America, South America",2,4,0,2.5,"Ceiling mounted",null,null,null,null,null,null,null,"6164XX0009.jpg",2,4,1,2,2,1,66,"CE","","","Class I",null,null,null,null,null,0.08,0.08,0.13,null,null,null,null,"6164XX0009.ldt",1,null,null,null,null,4,null,null,null,null,1,null,"LED",16,null,"",null,null,24,null,4000,80,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"","",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"Poland"]
["6165","6165XX0009","MOSS FLOODLIGHT-EARTHSPIKE LED 439LM 36D 3000K DIM.",null,"For lighting gardens, private areas, and other architectural concepts, The light direction can also be adjusted vertically",null,"Moss","Ground","Europe, Africa, Asia, Australia and Oceania, North America, South America",2,2,7.0000000000000007E-2,0,"",null,null,null,null,null,null,null,"6165XX0009.jpg",2,4,1,3,7,1,66,"CE","","","Class I",null,null,null,null,null,0,0,0,null,null,null,null,"6165XX0009.ldt",1,null,null,null,null,2,null,null,null,null,1,null,"LED",16,null,"",null,null,23,null,3000,80,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"","",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"Poland"]
["6166","6166XX0010","MOSS FLOODLIGHT-EARTHSPIKE LED 466LM 36D 4000K DIM.",null,"For illuminating gardens, private areas and other architectural concepts. Possibility to adjust the direction of light also in the vertical plane.",null,"Moss","Ground","Europe, Africa, Asia, Australia and Oceania, North America, South America",2,2,7.0000000000000007E-2,0,"",null,null,null,null,null,null,null,"6166XX0010.jpg",2,4,1,3,7,1,66,"CE","","","Class I",null,null,null,null,null,0,0,0,null,null,null,null,"6166XX0010.ldt",1,null,null,null,null,2,null,null,null,null,1,null,"LED",16,null,"",null,null,24,null,4000,80,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"","",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"Poland"]
["6168","6168XX0009","MOSS FLOODLIGHT-EARTHSPIKE LED 891LM 36D 4000K DIM.",null,"For lighting gardens, private areas, and other concepts architectural. The light direction can also be adjusted vertically",null,"Moss","Ground","Europe, Africa, Asia, Australia and Oceania, North America, South America",2,2,7.0000000000000007E-2,0,"",null,null,null,null,null,null,null,"6168XX0009.jpg",2,4,1,3,7,1,66,"CE","","","Class I",null,null,null,null,null,0,0,0,null,null,null,null,"6168XX0009.ldt",1,null,null,null,null,2,null,null,null,null,1,null,"LED",16,null,"",null,null,24,null,4000,80,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"","",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"Poland"]
["6170","6170XX0010","BORG BOLLARD BOLLARD 55CM LED 2093LM 3000K DIM.",null,"Luminaire with contemporary design. For lighting gardens and other private and public areas",null,"Borg","Bollard","Europe, Africa, Asia, Australia and Oceania, North America, South America",2,2,0.52,0,"",null,null,null,null,null,null,null,"6170XX0010.jpg",3,1,1,3,6,1,66,"CE","","IK08","Class I",null,null,null,null,null,0.2,0.2,0.55000000000000004,null,null,null,null,"6170XX0010.ldt",1,null,null,null,null,0,null,null,null,null,null,null,"LED",16,null,"",null,null,23,null,3000,80,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"","",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"Poland"]
["6171","6171XX0010","BORG BOLLARD BOLLARD 55CM LED 2214LM 4000K DIM.",null,"Luminaire with contemporary design. For lighting gardens and other private and public areas",null,"Borg","Bollard","Europe, Africa, Asia, Australia and Oceania, North America, South America",2,2,0.52,0,"",null,null,null,null,null,null,null,"6171XX0010.jpg",3,1,1,3,6,1,66,"CE","","IK08","Class I",null,null,null,null,null,0.2,0.2,0.55000000000000004,null,null,null,null,"6171XX0010.ldt",1,null,null,null,null,0,null,null,null,null,null,null,"LED",16,null,"",null,null,24,null,4000,80,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"","",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"Poland"]
["6172","6172XX0009","BORG BOLLARD BOLLARD 55CM LED 2093LM 3000K DALI2",null,"Luminaire with a contemporary design. For lighting gardens and other private and public areas",null,"Borg","Bollard","Europe, Africa, Asia, Australia and Oceania, North America, South America",2,2,0.52,0,"",null,null,null,null,null,null,null,"6172XX0009.jpg",3,1,1,3,6,3,66,"CE","","IK08","Class I",null,null,null,null,null,0.2,0.2,0.55000000000000004,null,null,null,null,"6172XX0009.ldt",1,null,null,null,null,0,null,null,null,null,null,null,"LED",16,null,"",null,null,23,null,3000,80,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"DALI","",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"Poland"]
["6173","6173XX0009","BORG BOLLARD BOLLARD 55CM LED 2216LM 4000K DALI2",null,"Luminaire with a contemporary design. For lighting gardens and other private and public areas",null,"Borg","Bollard","Europe, Africa, Asia, Australia and Oceania, North America, South America",2,2,0.52,0,"",null,null,null,null,null,null,null,"6173XX0009.jpg",3,1,1,3,6,3,66,"CE","","IK08","Class I",null,null,null,null,null,0.2,0.2,0.55000000000000004,null,null,null,null,"6173XX0009.ldt",1,null,null,null,null,0,null,null,null,null,null,null,"LED",16,null,"",null,null,24,null,4000,80,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"DALI","",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"Poland"]
["617","617XX0013","BERLIN WALL LED 880LM 3000K DIM.",null,"A ceiling-type luminaire with a contemporary design for general use",null,"Berlin","Wall","Europe, Africa, Asia, Australia and Oceania, North America, South America",2,4,0,2.5,"",null,null,null,null,null,null,null,"617XX0013.jpg",7,1,1,2,2,1,55,"CE","","IK10","Class I",null,null,null,null,null,0.27,0.27,0.14000000000000001,null,null,null,null,"617XX0013.ldt",1,null,null,null,null,3,null,null,null,null,null,null,"LED",16,null,"",null,null,23,null,3000,80,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"","",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"Poland"]
["6180","6180XX0010","BORG BOLLARD BOLLARD 85CM LED 2093LM 3000K DIM.",null,"Luminaire with contemporary design. For lighting gardens and other private and public areas",null,"Borg","Bollard","Europe, Africa, Asia, Australia and Oceania, North America, South America",2,2,0.82,{"$f":"IF(K641=4,2.5,IF(K641=64,0.5,0))","v":0},"",null,null,null,null,null,null,null,"6180XX0010.jpg",3,1,1,3,6,1,66,"CE","","IK08","Class I",null,null,null,null,null,0.2,0.2,0.85,null,null,null,null,"6180XX0010.ldt",1,null,null,null,null,0,null,null,null,null,null,null,"LED",16,null,"",null,null,23,null,3000,80,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"","",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"Poland"]
["6181","6181XX0010","BORG BOLLARD BOLLARD 85CM LED 2241LM 4000K DIM.",null,"Luminaire with contemporary design. For lighting gardens and other private and public areas",null,"Borg","Bollard","Europe, Africa, Asia, Australia and Oceania, North America, South America",2,2,0.82,0,"",null,null,null,null,null,null,null,"6181XX0010.jpg",3,1,1,3,6,1,66,"CE","","IK08","Class I",null,null,null,null,null,0.2,0.2,0.85,null,null,null,null,"6181XX0010.ldt",1,null,null,null,null,0,null,null,null,null,null,null,"LED",16,null,"",null,null,24,null,4000,80,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"","",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"Poland"]
["6182","6182XX0009","BORG BOLLARD BOLLARD 85CM LED 2093LM 3000K DALI2",null,"Luminaire with a contemporary design For lighting gardens, other private and public areas",null,"Borg","Bollard","Europe, Africa, Asia, Australia and Oceania, North America, South America",2,2,0.82,0,"",null,null,null,null,null,null,null,"6182XX0009.jpg",3,1,1,3,6,3,66,"CE","","IK08","Class I",null,null,null,null,null,0.2,0.2,0.85,null,null,null,null,"6182XX0009.ldt",1,null,null,null,null,0,null,null,null,null,null,null,"LED",16,null,"",null,null,23,null,3000,80,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"DALI","",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"Poland"]
["6183","6183XX0009","BORG BOLLARD BOLLARD 85CM LED 2216LM 4000K DALI2",null,"Luminaire with a contemporary design. For lighting gardens and other private and public areas",null,"Borg","Bollard","Europe, Africa, Asia, Australia and Oceania, North America, South America",2,2,0.82,0,"",null,null,null,null,null,null,null,"6183XX0009.jpg",3,1,1,3,6,3,66,"CE","","IK08","Class I",null,null,null,null,null,0.2,0.2,0.85,null,null,null,null,"6183XX0009.ldt",1,null,null,null,null,0,null,null,null,null,null,null,"LED",16,null,"",null,null,24,null,4000,80,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"DALI","",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"Poland"]
["6190","6190XX0010","BORG BOLLARD BOLLARD 110CM LED 2093LM 3000K DIM.",null,"Luminaire with contemporary design. For lighting gardens and other private and public areas",null,"Borg","Bollard","Europe, Africa, Asia, Australia and Oceania, North America, South America",2,2,1.07,0,"",null,null,null,null,null,null,null,"6190XX0010.png",3,1,1,3,6,1,66,"CE","","IK08","Class I",null,null,null,null,null,0.2,0.2,1.05,null,null,null,null,"6190XX0010.ldt",1,null,null,null,null,0,null,null,null,null,null,null,"LED",16,null,"",null,null,23,null,3000,80,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"","",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"Poland"]
["6191","6191XX0010","BORG BOLLARD BOLLARD 110CM LED 2241LM 4000K DIM.",null,"Luminaire with contemporary design. For lighting gardens and other private and public areas",null,"Borg","Bollard","Europe, Africa, Asia, Australia and Oceania, North America, South America",2,2,1.07,0,"",null,null,null,null,null,null,null,"6191XX0010.png",3,1,1,3,6,1,66,"CE","","IK08","Class I",null,null,null,null,null,0.2,0.2,1.05,null,null,null,null,"6191XX0010.ldt",1,null,null,null,null,0,null,null,null,null,null,null,"LED",16,null,"",null,null,24,null,4000,80,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"","",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"Poland"]
["6192",{"$f":"INDEX(DB,MATCH($A647,ID,0),2)","v":"6192XX0009"},"BORG BOLLARD BOLLARD 110CM LED 2093LM 3000K DALI2",null,{"$f":"IF(INDEX(DB,MATCH($A647,ID,0),35)=0,\"\",INDEX(DB,MATCH($A647,ID,0),35))","v":"Luminaire with a contemporary design. For garden lighting and other private and public areas."},null,"Borg","Bollard","Europe, Africa, Asia, Australia and Oceania, North America, South America",2,2,1.07,0,"",null,null,null,null,null,null,null,"6192XX0009.png",{"$f":"IF((IFERROR(INDEX(BRYLA_FOTO,MATCH(INDEX(DB,MATCH($A647,ID,0),62),ID_BRYLAFOTO,0),6),\"\"))<>0,IFERROR(INDEX(BRYLA_FOTO,MATCH(INDEX(DB,MATCH($A647,ID,0),62),ID_BRYLAFOTO,0),6),\"\"),\"\")","v":3},1,1,3,6,3,66,"CE","","IK08","Class I",null,null,null,null,null,{"$f":"INDEX(DB,MATCH($A647,ID,0),24)","v":0.2},{"$f":"INDEX(DB,MATCH($A647,ID,0),25)","v":0.2},{"$f":"INDEX(DB,MATCH($A647,ID,0),26)","v":1.05},null,null,null,null,"6192XX0009.ldt",1,null,null,null,null,0,null,null,null,null,null,null,"LED",16,null,"",null,null,23,null,3000,80,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"DALI","",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"Poland"]
["6193","6193XX0009","BORG BOLLARD BOLLARD 110CM LED 2216LM 4000K DALI2",null,"Luminaire with a contemporary design. For lighting gardens and other private and public areas",null,"Borg","Bollard","Europe, Africa, Asia, Australia and Oceania, North America, South America",2,2,1.07,0,"",null,null,null,null,null,null,null,"6193XX0009.png",3,1,1,3,6,3,66,"CE","","IK08","Class I",null,null,null,null,null,1.05,0.2,0.2,null,null,null,null,"6193XX0009.ldt",{"$f":"IF($BJ648=\"\",1,0)","v":1},null,null,null,null,0,null,null,null,null,null,null,"LED",16,null,"",null,null,24,null,4000,80,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"DALI","",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"Poland"]
["630","630XX0011","BREMEN WALL E27",null,"Classic design plafond type luminaire.",null,"Bremen","Wall","Europe, Africa, Asia, Australia and Oceania, North America, South America",2,4,0,2.5,"",null,null,null,null,null,null,null,"630XX0011.jpg",9,1,1,2,2,4,55,"CE","","IK10","Class I",null,null,null,null,null,0.28000000000000003,0.28000000000000003,0.14000000000000001,null,null,null,null,"630XX0011.ldt",0,null,null,null,null,3,null,null,null,null,1,null,"LED",16,null,"E27",null,null,23,null,"",80,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"","",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"Poland"]
["631","631XX0010","BREMEN WALL E27",null,"Classic design plafond type luminaire",null,"Bremen","Wall","Europe, Africa, Asia, Australia and Oceania, North America, South America",2,4,0,2.5,"",null,null,null,null,null,null,null,"631XX0010.jpg",8,1,1,2,2,4,55,"CE","","IK10","Class I",null,null,null,null,null,0.28000000000000003,0.28000000000000003,0.14000000000000001,null,null,null,null,"631XX0010.ldt",0,null,null,null,null,3,null,null,null,null,1,null,"LED",16,null,"E27",null,null,23,null,"",80,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"","",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"Poland"]
["6346","6346XX0009","MOSS LED 439LM 36D 3000K DIM.",null,"For illuminating gardens, private areas and other architectural concepts. Possibility to adjust the direction of light",null,"Moss","Recessed","Europe, Africa, Asia, Australia and Oceania, North America, South America",2,8,2.5,0,"",null,null,null,null,null,null,null,"6346XX0009.png",2,4,1,2,1,1,66,"CE","","","Class I",null,null,null,null,null,0.12,0.12,7.0000000000000007E-2,null,null,null,null,"6346XX0009.ldt",1,null,null,null,null,0,null,null,null,null,null,null,"LED",16,null,"",null,null,23,null,3000,80,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"","",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"Poland"]
["6352","6352XX0009","MOSS LED 466LM 36D 4000K DIM.",null,"For illuminating gardens, private areas and other concepts architectural. Possibility to adjust the direction of light.",null,"Moss","Recessed","Europe, Africa, Asia, Australia and Oceania, North America, South America",2,8,2.5,0,"",null,null,null,null,null,null,null,"6352XX0009.png",2,4,1,2,1,1,66,"CE","","","Class I",null,null,null,null,null,0.12,0.12,7.0000000000000007E-2,null,null,null,null,"6352XX0009.ldt",1,null,null,null,null,0,null,null,null,null,null,null,"LED",16,null,"",null,null,24,null,4000,80,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"","",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"Poland"]
["6355","6355XX0009","MOSS LED 439LM 36D 3000K DIM.",null,"For illuminating gardens, private areas and other concepts architectural. Possibility to adjust the direction of light also in the vertical plane",null,"Moss","Recessed","Europe, Africa, Asia, Australia and Oceania, North America, South America",2,8,2.5,0,"",null,null,null,null,null,null,null,"6355XX0009.png",2,4,1,2,1,1,66,"CE","","","Class I",null,null,null,null,null,0.13,0.13,0.06,null,null,null,null,"6355XX0009.ldt",1,null,null,null,null,0,null,null,null,null,null,null,"LED",16,null,"",null,null,23,null,3000,80,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"","",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"Poland"]
["6361","6361XX0009","MOSS LED 466LM 36D 4000K DIM.",null,"For illuminating gardens, private areas and other concepts architectural. Possibility to adjust the direction of light.",null,"Moss","Recessed","Europe, Africa, Asia, Australia and Oceania, North America, South America",2,8,2.5,0,"",null,null,null,null,null,null,null,"6361XX0009.png",2,4,1,2,1,1,66,"CE","","","Class I",null,null,null,null,null,0.13,0.13,0.06,null,null,null,null,"6361XX0009.ldt",1,null,null,null,null,0,null,null,null,null,null,null,"LED",16,null,"",null,null,24,null,4000,80,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"","",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"Poland"]
["6370","6370XX0009","MOSS LED 840LM 36D 3000K DIM.",null,"For illuminating gardens, private areas and other concepts architectural. Possibility to adjust the direction of light.",null,"Moss","Recessed","Europe, Africa, Asia, Australia and Oceania, North America, South America",2,8,2.5,0,"",null,null,null,null,null,null,null,"6370XX0009.png",2,4,1,2,1,1,66,"CE","","","Class I",null,null,null,null,null,0.12,0.12,7.0000000000000007E-2,null,null,null,null,"6370XX0009.ldt",1,null,null,null,null,0,null,null,null,null,null,null,"LED",16,null,"",null,null,23,null,3000,80,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"","",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"Poland"]
["6376","6376XX0009","MOSS LED 891LM 36D 4000K DIM.",null,"For illuminating gardens, private areas and other concepts architectural. Possibility to adjust the direction of light.",null,"Moss","Recessed","Europe, Africa, Asia, Australia and Oceania, North America, South America",2,8,2.5,0,"",null,null,null,null,null,null,null,"6376XX0009.png",2,4,1,2,1,1,66,"CE","","","Class I",null,null,null,null,null,0.12,0.12,7.0000000000000007E-2,null,null,null,null,"6376XX0009.ldt",1,null,null,null,null,0,null,null,null,null,null,null,"LED",16,null,"",null,null,24,null,4000,80,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"","",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"Poland"]
["6379","6379XX0009","MOSS LED 840LM 36D 3000K DIM.",null,"For illuminating gardens, private areas and other concepts architectural. Possibility to adjust the direction of light also in the vertical plane",null,"Moss","Recessed","Europe, Africa, Asia, Australia and Oceania, North America, South America",2,8,2.5,0,"",null,null,null,null,null,null,null,"6379XX0009.png",2,4,1,2,1,1,66,"CE","","","Class I",null,null,null,null,null,0.13,0.13,0.06,null,null,null,null,"6379XX0009.ldt",1,null,null,null,null,0,null,null,null,null,null,null,"LED",16,null,"",null,null,23,null,3000,80,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"","",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"Poland"]
["637","637XX0013","BREMEN WALL LED 880LM 3000K DIM.",null,"A ceiling-type luminaire with a contemporary design for general use",null,"Bremen","Wall","Europe, Africa, Asia, Australia and Oceania, North America, South America",2,4,0,2.5,"",null,null,null,null,null,null,null,"637XX0013.jpg",8,1,1,2,2,1,55,"CE","","IK10","Class I",null,null,null,null,null,0,0,0,null,null,null,null,"637XX0013.ldt",1,null,null,null,null,3,null,null,null,null,1,null,"LED",16,null,"",null,null,23,null,3000,80,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"","",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"Poland"]
["6385","6385XX0009","MOSS LED 891LM 36D 4000K DIM.",null,"For illuminating gardens, private areas and other concepts architectural. Possibility to adjust the direction of light.",null,"Moss","Recessed","Europe, Africa, Asia, Australia and Oceania, North America, South America",2,8,2.5,0,"",null,null,null,null,null,null,null,"6385XX0009.png",2,4,1,2,1,1,66,"CE","","","Class I",null,null,null,null,null,0.13,0.13,0.06,null,null,null,null,"6385XX0009.ldt",1,null,null,null,null,0,null,null,null,null,null,null,"LED",16,null,"",null,null,24,null,4000,80,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"","",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"Poland"]
["638","638XX0009","BREMEN WALL LED 1080LM 3000K MD",null,"A ceiling-type luminaire with a contemporary design for general use. Equipped with a wave motion sensor, a twilight switch, and motion support",null,"Bremen","Wall","Europe, Africa, Asia, Australia and Oceania, North America, South America",2,4,0,2.5,"",null,null,null,null,null,null,null,"638XX0009.jpg",8,1,1,2,2,3,55,"CE","","","Class I",null,null,null,null,null,0,0,0,null,null,null,null,"638XX0009.ldt",1,null,null,null,null,3,null,null,null,null,1,null,"LED",16,null,"",null,null,23,null,3000,80,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"","Daylight sensor,Motion sensor",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"Poland"]
["6401","6401XX0009","LYSFJORD WALL 2XLED 4144LM UP4º & DOWN60º 3000K DALI2",null,"A luminaire with a wide range of applications, including lighting: wall surfaces, facades and other architectural concepts.",null,"Lysfjord","Wall","Europe, Africa, Asia, Australia and Oceania, North America, South America",2,4,0.2,2.5,"",null,null,null,null,null,null,null,"6401XX0009.png",10,1,1,2,2,3,66,"CE","","IK08","Class I",null,null,null,null,null,0.43,0.15,0.2,null,null,null,null,"6401XX0009.ldt",1,null,null,null,null,1,null,null,null,null,null,null,"LED",16,null,"",null,null,23,null,3000,80,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"DALI","",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"Poland"]
["6403","6403XX0009","LYSFJORD WALL 2XLED 4144LM UP60º & DOWN60º 3000K DALI2",null,"A luminaire with a wide range of applications, including lighting: wall surfaces, facades and other architectural concepts.",null,"Lysfjord","Wall","Europe, Africa, Asia, Australia and Oceania, North America, South America",2,4,0.2,2.5,"",null,null,null,null,null,null,null,"6403XX0009.png",10,1,1,2,2,3,66,"CE","","IK08","Class I",null,null,null,null,null,0.43,0.15,0.12,null,null,null,null,"6403XX0009.ldt",1,null,null,null,null,1,null,null,null,null,null,null,"LED",16,null,"",null,null,23,null,3000,80,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"DALI","",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"Poland"]
["6404","6404XX0009","LYSFJORD WALL 2XLED 4144LM UP4º & DOWN4º 3000K DALI2",null,"A luminaire with a wide range of applications, including lighting: wall surfaces, facades and other architectural concepts.",null,"Lysfjord","Wall","Europe, Africa, Asia, Australia and Oceania, North America, South America",2,4,0.2,2.5,"",null,null,null,null,null,null,null,"6404XX0009.png",10,1,1,2,2,3,66,"CE","","IK08","Class I",null,null,null,null,null,0.43,0.15,0.2,null,null,null,null,"6404XX0009.ldt",1,null,null,null,null,1,null,null,null,null,null,null,"LED",16,null,"",null,null,23,null,3000,80,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"DALI","",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"Poland"]
["6405","6405XX0009","LYSFJORD WALL LED 2072LM UP 4º 3000K DALI2",null,"A luminaire with a wide range of applications, including lighting: wall surfaces, facades and other architectural concepts.",null,"Lysfjord","Wall","Europe, Africa, Asia, Australia and Oceania, North America, South America",2,4,0.2,2.5,"",null,null,null,null,null,null,null,"6405XX0009.png",10,1,1,2,2,3,66,"CE","","IK08","Class I",null,null,null,null,null,0.34,0.15,0.2,null,null,null,null,"6405XX0009.ldt",1,null,null,null,null,2,null,null,null,null,null,null,"LED",16,null,"",null,null,23,null,3000,80,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"DALI","",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"Poland"]
["6406","6406XX0009","LYSFJORD WALL LED 2072LM DOWN 4º 3000K DALI2",null,"A luminaire with a wide range of applications, including lighting: wall surfaces, facades and other architectural concepts.",null,"Lysfjord","Wall","Europe, Africa, Asia, Australia and Oceania, North America, South America",2,4,0.2,2.5,"",null,null,null,null,null,null,null,"6406XX0009.png",10,1,1,2,2,3,66,"CE","","IK08","Class I",null,null,null,null,null,0.34,0.15,0.2,null,null,null,null,"6406XX0009.ldt",1,null,null,null,null,0,null,null,null,null,null,null,"LED",16,null,"",null,null,23,null,3000,80,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"DALI","",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"Poland"]
["6407","6407XX0009","LYSFJORD WALL LED 2072LM UP60º 3000K DALI2",null,"A luminaire with a wide range of applications, including lighting: wall surfaces, facades and other architectural concepts.",null,"Lysfjord","Wall","Europe, Africa, Asia, Australia and Oceania, North America, South America",2,4,0.2,2.5,"",null,null,null,null,null,null,null,"6407XX0009.png",10,1,1,2,2,3,66,"CE","","IK08","Class I",null,null,null,null,null,0.34,0.15,0.2,null,null,null,null,"6407XX0009.ldt",1,null,null,null,null,2,null,null,null,null,null,null,"LED",16,null,"",null,null,23,null,3000,80,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"DALI","",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"Poland"]
["6408","6408XX0009","LYSFJORD WALL LED 2072LM DOWN60º 3000K DALI2",null,"A luminaire with a wide range of applications, including lighting: wall surfaces, facades and other architectural concepts.",null,"Lysfjord","Wall","Europe, Africa, Asia, Australia and Oceania, North America, South America",2,4,0.2,2.5,"",null,null,null,null,null,null,null,"6408XX0009.png",10,1,1,2,2,3,66,"CE","","IK08","Class I",null,null,null,null,null,0.34,0.15,0.2,null,null,null,null,"6408XX0009.ldt",1,null,null,null,null,0,null,null,null,null,null,null,"LED",16,null,"",null,null,23,null,3000,80,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"DALI","",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"Poland"]
["6421","6421XX0009","LYSFJORD WALL 2XLED 4144LM UP4º & DOWN60º 4000K DALI2",null,"A luminaire with a wide range of applications, including lighting: wall surfaces, facades and other architectural concepts.",null,"Lysfjord","Wall","Europe, Africa, Asia, Australia and Oceania, North America, South America",2,4,0.2,2.5,"",null,null,null,null,null,null,null,"6421XX0009.png",10,1,1,2,2,3,66,"CE","","IK08","Class I",null,null,null,null,null,0.43,0.15,0.2,null,null,null,null,"6421XX0009.ldt",1,null,null,null,null,1,null,null,null,null,null,null,"LED",16,null,"",null,null,24,null,4000,80,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"DALI","",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"Poland"]
["6422","6422XX0009","LYSFJORD WALL 2XLED 4144LM UP60º & DOWN4º 4000K DALI2",null,"A luminaire with a wide range of applications, including lighting: wall surfaces, facades and other architectural concepts.",null,"Lysfjord","Wall","Europe, Africa, Asia, Australia and Oceania, North America, South America",2,4,0.2,2.5,"",null,null,null,null,null,null,null,"6422XX0009.png",10,1,1,2,2,3,66,"CE","","IK08","Class I",null,null,null,null,null,0.43,0.15,0.2,null,null,null,null,"6422XX0009.ldt",1,null,null,null,null,1,null,null,null,null,null,null,"LED",16,null,"",null,null,24,null,4000,80,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"DALI","",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"Poland"]
["6423","6423XX0009","LYSFJORD WALL 2XLED 4144LM UP60º & DOWN60º 4000K DALI2",null,"A luminaire with a wide range of applications, including lighting: wall surfaces, facades and other architectural concepts.",null,"Lysfjord","Wall","Europe, Africa, Asia, Australia and Oceania, North America, South America",2,4,0.2,2.5,"",null,null,null,null,null,null,null,"6423XX0009.png",10,1,1,2,2,3,66,"CE","","IK08","Class I",null,null,null,null,null,0.43,0.15,0.2,null,null,null,null,"6423XX0009.ldt",1,null,null,null,null,1,null,null,null,null,null,null,"LED",16,null,"",null,null,24,null,4000,80,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"DALI","",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"Poland"]
["6424","6424XX0009","LYSFJORD WALL 2XLED 4144LM UP4º & DOWN4º 4000K DALI2",null,"A luminaire with a wide range of applications, including lighting: wall surfaces, facades and other architectural concepts.",null,"Lysfjord","Wall","Europe, Africa, Asia, Australia and Oceania, North America, South America",2,4,0.2,2.5,"",null,null,null,null,null,null,null,"6424XX0009.png",10,1,1,2,2,3,66,"CE","","IK08","Class I",null,null,null,null,null,0.43,0.15,0.2,null,null,null,null,"6424XX0009.ldt",1,null,null,null,null,1,null,null,null,null,null,null,"LED",16,null,"",null,null,24,null,4000,80,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"DALI","",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"Poland"]
["6425","6425XX0009","LYSFJORD WALL LED 2072LM UP 4º 4000K DALI2",null,"A luminaire with a wide range of applications, including lighting: wall surfaces, facades and other architectural concepts.",null,"Lysfjord","Wall","Europe, Africa, Asia, Australia and Oceania, North America, South America",2,4,0.2,2.5,"",null,null,null,null,null,null,null,"6425XX0009.png",10,1,1,2,2,3,66,"CE","","IK08","Class I",null,null,null,null,null,0.34,0.15,0.2,null,null,null,null,"6425XX0009.ldt",1,null,null,null,null,2,null,null,null,null,null,null,"LED",16,null,"",null,null,24,null,4000,80,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"DALI","",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"Poland"]
["6426","6426XX0009","LYSFJORD WALL LED 2072LM DOWN 4º 4000K DALI2",null,"A luminaire with a wide range of applications, including lighting: wall surfaces, facades and other architectural concepts.",null,"Lysfjord","Wall","Europe, Africa, Asia, Australia and Oceania, North America, South America",2,4,0.2,2.5,"",null,null,null,null,null,null,null,"6426XX0009.png",10,1,1,2,2,3,66,"CE","","IK08","Class I",null,null,null,null,null,0.34,0.15,0.2,null,null,null,null,"6426XX0009.ldt",1,null,null,null,null,0,null,null,null,null,null,null,"LED",16,null,"",null,null,24,null,4000,80,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"DALI","",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"Poland"]
["6427","6427XX0009","LYSFJORD WALL LED 2072LM UP60º 4000K DALI2",null,"A luminaire with a wide range of applications, including lighting: wall surfaces, facades and other architectural concepts.",null,"Lysfjord","Wall","Europe, Africa, Asia, Australia and Oceania, North America, South America",2,4,0.2,2.5,"",null,null,null,null,null,null,null,"6427XX0009.png",10,1,1,2,2,3,66,"CE","","IK08","Class I",null,null,null,null,null,0.34,0.15,0.2,null,null,null,null,"6427XX0009.ldt",1,null,null,null,null,2,null,null,null,null,null,null,"LED",16,null,"",null,null,24,null,4000,80,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"DALI","",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"Poland"]
["6428","6428XX0009","LYSFJORD WALL LED 2072LM DOWN60º 4000K DALI2",null,"A luminaire with a wide range of applications, including lighting: wall surfaces, facades and other architectural concepts.",null,"Lysfjord","Wall","Europe, Africa, Asia, Australia and Oceania, North America, South America",2,4,0.2,2.5,"",null,null,null,null,null,null,null,"6428XX0009.png",10,1,1,2,2,3,66,"CE","","IK08","Class I",null,null,null,null,null,0.34,0.15,0.2,null,null,null,null,"6428XX0009.ldt",1,null,null,null,null,0,null,null,null,null,null,null,"LED",16,null,"",null,null,24,null,4000,80,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"DALI","",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"Poland"]
["6471","6471XX0009","MOSS LED 840LM 36D 3000K DIM.",null,"For illuminating gardens, private areas and other concepts architectural. Possibility to adjust the direction of light also in the vertical plane",null,"Moss,Move","Spot,Ground","Europe, Africa, Asia, Australia and Oceania, North America, South America",2,2,1,0,"",null,null,null,null,null,null,null,"6471XX0009.png",2,4,1,3,7,1,66,"CE","","","Class I",null,null,null,null,null,0,0,0,null,null,null,null,"6471XX0009.ldt",1,null,null,null,null,2,null,null,null,null,null,null,"LED",16,null,"",null,null,23,null,3000,80,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"","",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"Poland"]
["6483","6483XX0009","MOSS LED 840LM 36D 3000K DIM.",null,"For illuminating gardens, private areas and other concepts architectural. Possibility to adjust the direction of light also in the vertical plane",null,"Moss,Move","Spot,Ground","Europe, Africa, Asia, Australia and Oceania, North America, South America",2,2,1,0,"",null,null,null,null,null,null,null,"6483XX0009.png",2,4,1,3,7,1,66,"CE","","","Class I",null,null,null,null,null,0.22,0.2,1.19,null,null,null,null,"6483XX0009.ldt",1,null,null,null,null,2,null,null,null,null,null,null,"LED",16,null,"",null,null,23,null,3000,80,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"","",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"Poland"]
["6485","6485XX0009","MOSS LED 439LM 36D 3000K DIM.",null,"For illuminating gardens, private areas and other concepts architectural. Possibility to adjust the direction of light also in the vertical plane",null,"Moss,Move","Spot,Ground","Europe, Africa, Asia, Australia and Oceania, North America, South America",2,2,1,0,"",null,null,null,null,null,null,null,"6485XX0009.png",2,4,1,3,7,1,66,"CE","","","Class I",null,null,null,null,null,0.22,0.2,1.19,null,null,null,null,"6485XX0009.ldt",1,null,null,null,null,2,null,null,null,null,null,null,"LED",16,null,"",null,null,23,null,3000,80,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"","",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"Poland"]
["655","655XX0013","BERN WALL LED 667LM 3000K DIM.",null,"A ceiling-type luminaire with a contemporary design",null,"Bern","Wall","Europe, Africa, Asia, Australia and Oceania, North America, South America",2,4,0,2.5,"",null,null,null,null,null,null,null,"655XX0013.jpg",8,1,2,2,2,1,55,"CE","","IK07","Class I",null,null,null,null,null,0.24,0.24,0.12,null,null,null,null,"655XX0013.ldt",1,null,null,null,null,3,null,null,null,null,1,null,"LED",16,null,"",null,null,23,null,3000,80,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"","",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"Poland"]
["6600","6600XX0009","MOSS FLOODLIGHT-EARTHSPIKE LED 840LM 36D 3000K DIM.",null,"For illuminating gardens, private areas and other concepts architectural. Possibility to adjust the direction of light also in the vertical plane",null,"Moss,Move","Spot,Ground","Europe, Africa, Asia, Australia and Oceania, North America, South America",2,2,0.5,0,"",null,null,null,null,null,null,null,"6600XX0009.png",2,4,1,3,7,1,66,"CE","","","Class I",null,null,null,null,null,0,0,0,null,null,null,null,"6600XX0009.ldt",1,null,null,null,null,2,null,null,null,null,1,null,"LED",16,null,"",null,null,23,null,3000,80,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"","",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"Poland"]
["6601","6601XX0009","MOSS FLOODLIGHT-EARTHSPIKE LED 891LM 36D 4000K DIM.",null,"For illuminating gardens, private areas and other concepts architectural. Possibility to adjust the direction of light also in the vertical plane",null,"Moss,Move","Spot,Ground","Europe, Africa, Asia, Australia and Oceania, North America, South America",2,2,0.5,0,"",null,null,null,null,null,null,null,"6601XX0009.png",2,4,1,3,7,1,66,"CE","","","Class I",null,null,null,null,null,0,0,0,null,null,null,null,"6601XX0009.ldt",1,null,null,null,null,2,null,null,null,null,1,null,"LED",16,null,"",null,null,24,null,4000,80,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"","",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"Poland"]
["6602","6602XX0009","MOSS FLOODLIGHT-EARTHSPIKE LED 439LM 36D 3000K DIM.",null,"For lighting gardens, private areas and other architectural concepts. The light direction can also be adjusted in the vertical plane",null,"Moss,Move","Spot,Ground","Europe, Africa, Asia, Australia and Oceania, North America, South America",2,2,0.5,0,"",null,null,null,null,null,null,null,"6602XX0009.png",2,4,1,3,7,1,66,"CE","","","Class I",null,null,null,null,null,0,0,0,null,null,null,null,"6602XX0009.ldt",1,null,null,null,null,2,null,null,null,null,1,null,"LED",16,null,"",null,null,23,null,3000,80,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"","",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"Poland"]
["6603","6603XX0009","MOSS FLOODLIGHT-EARTHSPIKE LED 466LM 36D 4000K DIM.",null,"For illuminating gardens, private areas and other architectural concepts. Possibility to adjust the direction of light also in the vertical plane.",null,"Moss,Move","Spot,Ground","Europe, Africa, Asia, Australia and Oceania, North America, South America",2,2,0.5,0,"",null,null,null,null,null,null,null,"6603XX0009.png",2,4,1,3,7,1,66,"CE","","","Class I",null,null,null,null,null,0,0,0,null,null,null,null,"6603XX0009.ldt",1,null,null,null,null,2,null,null,null,null,1,null,"LED",16,null,"",null,null,24,null,4000,80,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"","",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"Poland"]
["660","660XX0009",{"$f":"INDEX(DB,MATCH($A684,ID,0),3)","v":"BASEL WALL E27"},null,"Modern design plafon type luminaire.",null,"Basel",{"$f":"IF(INDEX(DB,MATCH($A684,ID,0),5)=0,\"\",INDEX(DB,MATCH($A684,ID,0),5))","v":"Wall"},"Europe, Africa, Asia, Australia and Oceania, North America, South America",2,{"$f":"IFERROR(INDEX(TYPMONT,MATCH((INDEX(DB,MATCH($A684,ID,0),31)),ID_RODZ,0),3),\"\")","v":4},0,2.5,{"$f":"IFERROR(IF(INDEX(TYPMONT,MATCH((INDEX(DB,MATCH($A684,ID,0),31)),ID_RODZ,0),6)=0,\"\",INDEX(TYPMONT,MATCH((INDEX(DB,MATCH($A684,ID,0),31)),ID_RODZ,0),6)),\"\")","v":""},null,null,null,null,null,null,null,{"$f":"IF(INDEX(DB,MATCH($A684,ID,0),57)=0,\"\",INDEX(DB,MATCH($A684,ID,0),57))","v":"660XX0009.jpg"},9,{"$f":"IF(INDEX(DB,MATCH($A684,ID,0),61)=0,\"\",INDEX(DB,MATCH($A684,ID,0),61))","v":1},2,{"$f":"IFERROR(INDEX(TYPMONT,MATCH((INDEX(DB,MATCH($A684,ID,0),31)),ID_RODZ,0),1),\"\")","v":2},{"$f":"IFERROR(INDEX(TYPMONT,MATCH((INDEX(DB,MATCH($A684,ID,0),31)),ID_RODZ,0),2),\"\")","v":2},{"$f":"IF(INDEX(DB,MATCH($A684,ID,0),59)=0,\"\",INDEX(DB,MATCH($A684,ID,0),59))","v":4},{"$f":"IFERROR(IF(INDEX(DB,MATCH($A684,ID,0),19)=0,\"\",INDEX(DB,MATCH($A684,ID,0),19)+1),\"\")","v":55},{"$f":"IF(INDEX(DB,MATCH($A684,ID,0),27)=0,\"\",INDEX(DB,MATCH($A684,ID,0),27))","v":"CE"},"",{"$f":"IF(INDEX(DB,MATCH($A684,ID,0),20)=0,\"\",INDEX(DB,MATCH($A684,ID,0),20))","v":"IK07"},{"$f":"IF(INDEX(DB,MATCH($A684,ID,0),21)=0,\"\",INDEX(DB,MATCH($A684,ID,0),21))","v":"Class I"},null,null,null,null,null,0.21,0.13,0.31,null,null,null,null,{"$f":"IF(INDEX(DB,MATCH($A684,ID,0),58)=0,\"\",INDEX(DB,MATCH($A684,ID,0),58))","v":"660XX0009.ldt"},0,null,null,null,null,3,null,null,null,null,null,null,"LED",16,null,{"$f":"IF(INDEX(DB,MATCH($A684,ID,0),60)=0,\"\",INDEX(DB,MATCH($A684,ID,0),60))","v":"E27"},null,null,23,null,{"$f":"IF(INDEX(DB,MATCH($A684,ID,0),22)=0,\"\",INDEX(DB,MATCH($A684,ID,0),22))","v":""},{"$f":"IF(INDEX(DB,MATCH($A684,ID,0),53)=0,\"\",INDEX(DB,MATCH($A684,ID,0),53))","v":80},null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,{"$f":"IF(INDEX(DB,MATCH($A684,ID,0),29)=0,\"\",INDEX(DB,MATCH($A684,ID,0),29))","v":""},{"$f":"IF(INDEX(DB,MATCH($A684,ID,0),28)=0,\"\",INDEX(DB,MATCH($A684,ID,0),28))","v":""},null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"Poland"]
["661","661XX0009","BASEL WALL E27",null,"Modern design plafon type luminaire",null,{"$f":"IF(INDEX(DB,MATCH($A685,ID,0),4)=0,\"\",INDEX(DB,MATCH($A685,ID,0),4))","v":"Basel"},"Wall","Europe, Africa, Asia, Australia and Oceania, North America, South America",2,4,0,2.5,"",null,null,null,null,null,null,null,"661XX0009.jpg",8,1,2,2,2,4,55,"CE",{"$f":"IFERROR(IF(FIND(\"RENA\",$C685)>0,\"Vehicle resistant\",\"\"),\"\")","v":""},"IK07","Class I",null,null,null,null,null,0.21,0.13,0.31,null,null,null,null,"661XX0009.ldt",0,null,null,null,null,3,null,null,null,null,null,null,"LED",16,null,"E27",null,null,{"$f":"IF($BO685=4000,24,23)","v":23},null,"",80,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"","",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"Poland"]
["668","668XX0013","BASEL WALL LED 667LM 3000K DIM. TE",null,"Modern design plafon type luminaire",null,"Basel","Wall","Europe, Africa, Asia, Australia and Oceania, North America, South America",2,4,0,2.5,"",null,null,null,null,null,null,null,"668XX0013.jpg",8,1,2,2,2,1,55,"CE","","IK07","Class I",null,null,null,null,null,0,0,0,null,null,null,null,"668XX0013.ldt",1,null,null,null,null,3,null,null,null,null,null,null,"LED",16,null,"",null,null,23,null,3000,80,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"","",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"Poland"]
["6702","6702XX0309","MOSS FLOODLIGHT-BOX LED 840LM 36º 3000K DIM.",null,"For lighting gardens, private areas and other architectural concepts. Possibility to adjust the lighting direction also in the vertical plane.",null,"Moss,Arm","Spot,Wall","Europe, Africa, Asia, Australia and Oceania, North America, South America",2,2,0.5,0,"",null,null,null,null,null,null,null,"6702XX0309.png",2,4,1,3,6.7,1,66,"CE","","","Class I",null,null,null,null,null,0,0,0,null,null,null,null,"6702XX0309.ldt",1,null,null,null,null,2,null,null,null,null,1,null,"LED",16,null,"",null,null,23,null,3000,80,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"","",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"Poland"]
["6732","6732XX0309","MOSS FLOODLIGHT-BOX LED 439LM 36D 3000K DIM.",null,"For illuminating gardens, private areas and other architectural concepts. Possibility to adjust the direction of light also in the vertical plane.",null,"Moss","Spot,Ø50 pipe","Europe, Africa, Asia, Australia and Oceania, North America, South America",2,2,1,0,"",null,null,null,null,null,null,null,"6732XX0309.png",2,4,1,3,6.7,1,66,"CE","","","Class I",null,null,null,null,null,0,0,0,null,null,null,null,"6732XX0309.ldt",1,null,null,null,null,2,null,null,null,null,1,null,"LED",16,null,"",null,null,23,null,3000,80,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"","",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"Poland"]
["6735","6735XX0309","MOSS FLOODLIGHT-BOX LED 439LM 36D 3000K DIM.",null,"For illuminating gardens, private areas and other architectural concepts. Possibility to adjust the direction of light also in the vertical plane.",null,"Moss","Spot,Ø60 pipe","Europe, Africa, Asia, Australia and Oceania, North America, South America",2,2,1,0,"",null,null,null,null,null,null,null,"6735XX0309.png",2,4,1,3,6.7,1,66,"CE","","","Class I",null,null,null,null,null,0,0,0,null,null,null,null,"6735XX0309.ldt",1,null,null,null,null,2,null,null,null,null,1,null,"LED",16,null,"",null,null,23,null,3000,80,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"","",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"Poland"]
["6738","6738XX0309","MOSS FLOODLIGHT-BOX LED 439LM 36D 3000K DIM.",null,"For illuminating gardens, private areas and other architectural concepts. Possibility to adjust the direction of light also in the vertical plane.",null,"Moss","Spot,Ø76 pipe","Europe, Africa, Asia, Australia and Oceania, North America, South America",2,2,1,0,"",null,null,null,null,null,null,null,"6738XX0309.png",2,4,1,3,6.7,1,66,"CE","","","Class I",null,null,null,null,null,0,0,0,null,null,null,null,"6738XX0309.ldt",1,null,null,null,null,2,null,null,null,null,1,null,"LED",16,null,"",null,null,23,null,3000,80,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"","",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"Poland"]
["6750","6750XX0309","MOSS FLOODLIGHT-BOX LED 840LM 36D 3000K DIM.",null,"For illuminating gardens, private areas and other architectural concepts. Possibility to adjust the direction of light also in the vertical plane.",null,"Moss","Spot,Ø50 pipe","Europe, Africa, Asia, Australia and Oceania, North America, South America",2,2,1,0,"",null,null,null,null,null,null,null,"6750XX0309.png",2,4,1,3,6.7,1,66,"CE","","","Class I",null,null,null,null,null,0,0,0,null,null,null,null,"6750XX0309.ldt",1,null,null,null,null,2,null,null,null,null,1,null,"LED",16,null,"",null,null,23,null,3000,80,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"","",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"Poland"]
["6753","6753XX0309","MOSS FLOODLIGHT-BOX LED 840LM 36D 3000K DIM.",null,"For illuminating gardens, private areas and other architectural concepts. Possibility to adjust the direction of light also in the vertical plane.",null,"Moss","Spot,Ø60 pipe","Europe, Africa, Asia, Australia and Oceania, North America, South America",2,2,1,0,"",null,null,null,null,null,null,null,"6753XX0309.png",2,4,1,3,6.7,1,66,"CE","","","Class I",null,null,null,null,null,0,0,0,null,null,null,null,"6753XX0309.ldt",1,null,null,null,null,2,null,null,null,null,1,null,"LED",16,null,"",null,null,23,null,3000,80,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"","",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"Poland"]
["6756","6756XX0309","MOSS FLOODLIGHT-BOX LED 840LM 36D 3000K DIM.",null,"For illuminating gardens, private areas and other architectural concepts. Possibility to adjust the direction of light also in the vertical plane.",null,"Moss","Spot,Ø76 pipe","Europe, Africa, Asia, Australia and Oceania, North America, South America",2,2,1,0,"",null,null,null,null,null,null,null,"6756XX0309.png",2,4,1,3,6.7,1,66,"CE","","","Class I",null,null,null,null,null,0,0,0,null,null,null,null,"6756XX0309.ldt",1,null,null,null,null,2,null,null,null,null,1,null,"LED",16,null,"",null,null,23,null,3000,80,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"","",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"Poland"]
["675","675XX0009","BERN WALL LED 1080LM 3000K MD",null,"A ceiling-type luminaire with a contemporary design",null,"Bern","Wall,Ceiling","Europe, Africa, Asia, Australia and Oceania, North America, South America",2,4,0,2.5,"",null,null,null,null,null,null,null,"675XX0009.jpg",8,1,2,2,2,3,55,"CE","","IK07","Class I",null,null,null,null,null,0.24,0.12,0.24,null,null,null,null,"675XX0009.ldt",1,null,null,null,null,3,null,null,null,null,1,null,"LED",16,null,"",null,null,23,null,3000,80,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"","Daylight sensor,Motion sensor",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"Poland"]
["676","676XX0009","BERN WALL LED 1150LM 4000K MD",null,"A ceiling-type luminaire with a contemporary design",null,"Bern","Wall","Europe, Africa, Asia, Australia and Oceania, North America, South America",2,4,0,2.5,"",null,null,null,null,null,null,null,"676XX0009.jpg",8,1,2,2,2,3,55,"CE","","IK07","Class I",null,null,null,null,null,0.24,0.12,0.24,null,null,null,null,"676XX0009.ldt",1,null,null,null,null,3,null,null,null,null,1,null,"LED",16,null,"",null,null,24,null,4000,80,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"","Daylight sensor,Motion sensor",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"Poland"]
["6772","6772XX0309","MOSS FLOODLIGHT-BOX LED 840LM 36D 3000K DIM.",null,"For illuminating gardens, private areas and other architectural concepts. Possibility to adjust the direction of light also in the vertical plane.",null,"Moss","Spot,Wall","Europe, Africa, Asia, Australia and Oceania, North America, South America",2,2,0.1,0,"",null,null,null,null,null,null,null,"6772XX0309.png",2,4,1,3,6.7,1,66,"CE","","","Class I",null,null,null,null,null,0,0,0,null,null,null,null,"6772XX0309.ldt",1,null,null,null,null,2,null,null,null,null,1,null,"LED",16,null,"",null,null,23,null,3000,80,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"","",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"Poland"]
["6778","6778XX0309","MOSS FLOODLIGHT-BOX LED 438LM 36D 3000K DIM.",null,"For illuminating gardens, private areas and other architectural concepts. Possibility to adjust the direction of light also in the vertical plane.",null,"Moss","Spot,Wall","Europe, Africa, Asia, Australia and Oceania, North America, South America",2,2,0.1,0,"",null,null,null,null,null,null,null,"6778XX0309.png",2,4,1,3,6.7,1,66,"CE","","","Class I",null,null,null,null,null,0,0,0,null,null,null,null,"6778XX0309.ldt",1,null,null,null,null,2,null,null,null,null,1,null,"LED",16,null,"",null,null,23,null,3000,80,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"","",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"Poland"]
["7120","7120XX0011","NORDLAND CEILING/WALL 2XLED E27",null,"A ceiling luminaire with a modern design For lighting private areas and other architectural concepts",null,"Nordland","Wall,Ceiling","Europe, Africa, Asia, Australia and Oceania, North America, South America",2,4,0,2.5,"Ceiling mounted",null,null,null,null,null,null,null,"7120XX0011.jpg",8,1,2,2,2,4,66,"CE","","IK10","Class I",null,null,null,null,null,0.28000000000000003,0.28000000000000003,0.1,null,null,null,null,"7120XX0011.ldt",0,null,null,null,null,0,null,null,null,null,1,null,"LED",16,null,"E27",null,null,23,null,"",80,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"","",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"Poland"]
["718","718XX0015","NORDLAND CEILING/WALL LED 911LM 3000K DIM.",null,"A ceiling-type luminaire with a modern design For lighting private areas and other architectural concepts",null,"Nordland","Wall,Ceiling","Europe, Africa, Asia, Australia and Oceania, North America, South America",2,4,0,2.5,"Ceiling mounted",null,null,null,null,null,null,null,"718XX0015.jpg",8,1,2,2,2,1,66,"CE","","IK10","Class I",null,null,null,null,null,0.28000000000000003,0.28000000000000003,0.1,null,null,null,null,"718XX0015.ldt",1,null,null,null,null,0,null,null,null,null,1,null,"LED",16,null,"",null,null,23,null,3000,80,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"","",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"Poland"]
["724","724XX0010","KOSTER WALL E27",null,"Modern design wall-mounted luminaire. Possibility to install on corners of architectural objects.",null,"Koster","Wall","Europe, Africa, Asia, Australia and Oceania, North America, South America",2,4,0.22,2.5,"",null,null,null,null,null,null,null,"724XX0010.jpg",3,1,1,2,2,4,55,"CE","","IK10","Class I",null,null,null,null,null,0,0,0,null,null,null,null,"724XX0010.ldt",0,null,null,null,null,0,null,null,null,null,null,null,"LED",16,null,"E27",null,null,23,null,"",80,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"","",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"Poland"]
["725","725XX0012","KOSTER WALL LED 1080LM 3000K ON/OFF",null,"Modern design wall-mounted luminaire. Possibility to install on corners of architectural objects.",null,"Koster","Wall","Europe, Africa, Asia, Australia and Oceania, North America, South America",2,4,0.22,2.5,"",null,null,null,null,null,null,null,"725XX0012.jpg",3,1,1,2,2,4,55,"CE","","","Class I",null,null,null,null,null,0,0,0,null,null,null,null,"725XX0012.ldt",1,null,null,null,null,0,null,null,null,null,null,null,"LED",16,null,"",null,null,23,null,3000,80,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"","",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"Poland"]
["750","750XX0010","TORINO WALL E27",null,"Classic design wall-mounted luminaire. For lighting gardens, terraces and other architectural concepts.",null,"Torino","Wall","Europe, Africa, Asia, Australia and Oceania, North America, South America",2,4,0,{"$f":"IF(K702=4,2.5,IF(K702=64,0.5,0))","v":2.5},"",null,null,null,null,null,null,null,"750XX0010.jpg",9,1,2,2,2,4,55,"CE","","","Class II",null,null,null,null,null,0.38,0.28000000000000003,0.34,null,null,null,null,"750XX0010.ldt",0,null,null,null,null,3,null,null,null,null,null,null,"LED",16,null,"E27",null,null,23,null,"",80,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"","",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"Poland"]
["777","777XX0017","NICE POLE-TOP LED 5127LM 3000K ON/OFF",null,"Top-mounted luminaire designed for mounting on a lighting pole with a Ø60mm mounting shaft",null,"Nice","Post,Head","Europe, Africa, Asia, Australia and Oceania, North America, South America",2,512,3.84,0,"",null,null,null,null,null,null,null,"777XX0017.jpg",9,1,1,5,9,4,66,"CE","","","Class I",null,null,null,null,null,0.7,0.55000000000000004,0.55000000000000004,null,null,null,null,"777XX0017.ldt",1,null,null,null,null,0,null,null,null,null,null,null,"LED",16,null,"",null,null,23,null,3000,80,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"","",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"Poland"]
["796","796XX0011","SANDVIK CEILING LED GU10 265LM DOWN 25D 2700K DIM.",null,"Classic design ceiling luminaire. For lighting private areas and public spaces.",null,"Sandvik","Ceiling","Europe, Africa, Asia, Australia and Oceania, North America, South America",2,1,2.8,0,"",null,null,null,null,null,null,null,"796XX0011.jpg",2,1,2,1,2,1,55,"CE","","IK08","Class I",null,null,null,null,null,0,0,0,null,null,null,null,"796XX0011.ldt",0,null,null,null,null,0,null,null,null,null,null,null,"LED",16,null,"GU10",null,null,23,null,2700,90,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"","",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"Poland"]
["800","800XX0012","FIRENZE WALL E27",null,"Classic type wall-mounted luminaire. Possibility to install on corners of architectural objects.",null,"Florence","Wall","Europe, Africa, Asia, Australia and Oceania, North America, South America",2,4,0.3,2.5,"",null,null,null,null,null,null,null,"800XX0012.jpg",9,1,1,2,2,4,55,"CE","","","Class II",null,null,null,null,null,0,0,0,null,null,null,null,"800XX0012.ldt",0,null,null,null,null,1,null,null,null,null,null,null,"LED",16,null,"E27",null,null,23,null,"",80,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"","",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"Poland"]
["800A","800XX0110","FIRENZE CEILING-CHAIN E27",null,"Classic design luminaire with chain suspension. For lighting gardens, terraces and other architectural concepts.",null,"Florence","Ceiling","Europe, Africa, Asia, Australia and Oceania, North America, South America",2,16,0.65,0,"",null,null,null,null,null,null,null,"800XX0110.jpg",9,1,1,1,4,4,55,"CE","","","Class II",null,null,null,null,null,0,0,0,null,null,null,null,"800XX0110.ldt",0,null,null,null,null,1,null,null,null,null,null,null,"LED",16,null,"E27",null,null,23,null,"",80,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"","",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"Poland"]
["805","805XX0011","FIRENZE BOLLARD E27",null,"Classic design luminaire. For lighting gardens, private areas and public spaces. Other accessories need to be purchased separately.",null,"Florence","Bollard,Flower","Europe, Africa, Asia, Australia and Oceania, North America, South America",2,2,0.9,0,"",null,null,null,null,null,null,null,"805XX0011.jpg",7,1,1,3,6,4,55,"CE","","","Class II",null,null,null,null,null,0,0,0,null,null,null,null,"805XX0011.ldt",0,null,null,null,null,1,null,null,null,null,null,null,"LED",16,null,"E27",null,null,23,null,"",80,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"","",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"Poland"]
["810","810XX0309","FIRENZE POLE LUMINAIRE. E27",null,"Classic design luminaire, mounted on a telescopic lighting pole. Adjustable height 1930..2560mm. For lighting gardens, terraces and other architectural concepts.",null,"Florence","Post,Post complete","Europe, Africa, Asia, Australia and Oceania, North America, South America",2,256,2.2999999999999998,0,"",null,null,null,null,null,null,null,"810XX0309.jpg",9,1,1,5,8,4,55,"CE","","","Class II",null,null,null,null,null,0,0,0,null,null,null,null,"810XX0309.ldt",0,null,null,null,null,1,null,null,null,null,null,null,"LED",16,null,"E27",null,null,23,null,"",80,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"","",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"Poland"]
["820","820XX0309","FIRENZE POLE LUMINAIRE. E27",null,"Classic design luminaire, mounted on a telescopic lighting pole. Adjustable height 1930..2560mm. For lighting gardens, terraces and other architectural concepts.",null,"Florence","Post,Post complete","Europe, Africa, Asia, Australia and Oceania, North America, South America",2,256,2.2999999999999998,0,"",null,null,null,null,null,null,null,"820XX0309.jpg",9,1,1,5,8,4,55,"CE","","","Class II",null,null,null,null,null,0,0,0,null,null,null,null,"820XX0309.ldt",0,null,null,null,null,1,null,null,null,null,null,null,"LED",16,null,"E27",null,null,23,null,"",80,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"","",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"Poland"]
["830","830XX0309","FIRENZE POLE LUMINAIRE. E27",null,"Classic design luminaire, mounted on a telescopic lighting pole. Adjustable height 1930..2560mm. For lighting gardens, terraces and other architectural concepts.",null,"Florence","Post,Post complete","Europe, Africa, Asia, Australia and Oceania, North America, South America",2,256,2.2999999999999998,0,"",null,null,null,null,null,null,null,"830XX0309.jpg",9,1,1,5,8,4,55,"CE","","","Class II",null,null,null,null,null,0,0,0,null,null,null,null,"830XX0309.ldt",0,null,null,null,null,1,null,null,null,null,null,null,"LED",16,null,"E27",null,null,23,null,"",80,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"","",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"Poland"]
["866","866XX0013","BODEN WALL LED 743LM 3000K DIM.",null,{"$f":"IF(INDEX(DB,MATCH($A711,ID,0),35)=0,\"\",INDEX(DB,MATCH($A711,ID,0),35))","v":"A ceiling-type luminaire with a contemporary design"},null,"Boden","Wall","Europe, Africa, Asia, Australia and Oceania, North America, South America",2,4,0,2.5,"",null,null,null,null,null,null,null,"866XX0013.jpg",8,1,2,2,2,1,55,"CE","","","Class I",null,null,null,null,null,0,0,0,null,null,null,null,"866XX0013.ldt",1,null,null,null,null,1,null,null,null,null,1,null,"LED",16,null,"",null,null,23,null,3000,80,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"","",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"Poland"]
["891","891XX0013","ARVIKA BOLLARD LED 1370LM 3000K ON/OFF",null,"Bollard luminaire for lighting private areas, gardens and other architectural concepts",null,"Arvika","Bollard","Europe, Africa, Asia, Australia and Oceania, North America, South America",2,2,0.75,0,"",null,null,null,null,null,null,null,"891XX0013.jpg",4,1,2,3,6,4,45,"CE","","","Class I",null,null,null,null,null,0.14000000000000001,0.14000000000000001,0.89,null,null,null,null,"891XX0013.ldt",{"$f":"IF($BJ712=\"\",1,0)","v":1},null,null,null,null,1,null,null,null,null,null,null,"LED",16,null,"",null,null,23,null,3000,80,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"","",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"Poland"]
["893","893XX0013","ARVIKA BOLLARD-CONNECTORS LED 1370LM 3000K ON/OFF",null,"Bollard luminaire and electricity distributor 220...240V. For lighting private and public areas such as gardens, campsites, etc",null,"Arvika","Bollard","Europe, Africa, Asia, Australia and Oceania, North America, South America",2,2,0.75,0,"",null,null,null,null,null,null,null,"893XX0013.jpg",4,1,2,3,6,4,45,"CE","","","Class I",null,null,null,null,null,0.14000000000000001,0.14000000000000001,0.89,null,null,null,null,"893XX0013.ldt",1,null,null,null,null,1,null,null,null,null,null,null,"LED",16,null,"",null,null,23,null,3000,80,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"","",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"Poland"]
["901","901XX0009","ARVIKA BOLLARD - CONNECTORS E [UNI] 4XLED 1424LM 3000K ON/OFF",null,"E [Uni] sockets",null,"Arvika","Bollard","Europe, Africa, Asia, Australia and Oceania, North America, South America",2,2,0.75,0,"",null,null,null,null,null,null,null,"901XX0009.jpg",4,1,2,3,6,4,45,"CE","","","Class I",null,null,null,null,null,0.14000000000000001,0.14000000000000001,0.89,null,null,null,null,"901XX0009.ldt",1,null,null,null,null,1,null,null,null,null,null,null,"LED",16,null,"",null,null,23,null,3000,80,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"","",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"Poland"]
["XX"]
["1489",{"$f":"INDEX(DB,MATCH($A716,ID,0),2)","v":"1489XX0012"},"HALMSTAD BOLLARD 49CM LED 1098LM 3000K DIM.",null,"A bollard luminaire with a stable and durable structure. For lighting private areas and public areas",null,"Halmstad","Bollard","Europe, Africa, Asia, Australia and Oceania, North America, South America",2,2,0.36,{"$f":"IF(K716=4,2.5,IF(K716=64,0.5,0))","v":0},"",null,null,null,null,null,null,null,"1489XX0012.jpg",{"$f":"IF((IFERROR(INDEX(BRYLA_FOTO,MATCH(INDEX(DB,MATCH($A716,ID,0),62),ID_BRYLAFOTO,0),6),\"\"))<>0,IFERROR(INDEX(BRYLA_FOTO,MATCH(INDEX(DB,MATCH($A716,ID,0),62),ID_BRYLAFOTO,0),6),\"\"),\"\")","v":7},1,2,3,6,1,66,"CE","","IK10","Class I",null,null,null,null,null,{"$f":"INDEX(DB,MATCH($A716,ID,0),24)","v":0},{"$f":"INDEX(DB,MATCH($A716,ID,0),25)","v":0},{"$f":"INDEX(DB,MATCH($A716,ID,0),26)","v":0},null,null,null,null,"1489XX0012.ldt",1,null,null,null,null,1,null,null,null,null,null,null,"LED",16,null,"",null,null,23,null,3000,80,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"","",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"Poland"]
["1950","1950XX0B11","VOSS WALL 3XLED 2166LM 3000K ON/OFF",null,"A luminaire with a wide range of applications, for lighting: wall and facade surfaces and other architectural concepts",null,"Voss","Wall","Europe, Africa, Asia, Australia and Oceania, North America, South America",2,4,0,2.5,"",null,null,null,null,null,null,null,"1950XX0B11.jpg",10,1,2,2,2,4,55,"CE","","IK06","Class I",null,null,null,null,null,0.18,0.16,0.27,null,null,null,null,"1950XX0B11.ldt",1,null,null,null,null,1,null,null,null,null,null,null,"LED",16,null,"",null,null,23,null,3000,80,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"","",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"Poland"]
["5123","5123XX0009",{"$f":"INDEX(DB,MATCH($A718,ID,0),3)","v":"OPPLAND BOLLARD LED 1371LM 4000K DIM."},null,"Bollard luminaire of stable and durable construction. For lighting private areas and public spaces. IP of lighting chamber - 65.",null,"Oppland","Bollard","Europe, Africa, Asia, Australia and Oceania, North America, South America",2,2,0.8,0,"",null,null,null,null,null,null,null,"5123XX0009.jpg",7,1,1,3,6,1,66,"CE","","IK09","Class I",null,null,null,null,null,0,0,0,null,null,null,null,"5123XX0009.ldt",1,null,null,null,null,0,null,null,null,null,null,null,"LED",16,null,"",null,null,24,null,4000,80,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"","",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"Poland"]
["6167","6167XX0009","MOSS FLOODLIGHT-EARTHSPIKE LED 840LM 36D 3000K DIM.",null,"For lighting gardens, private areas, and other architectural concepts, The light direction can also be adjusted vertically",null,"Moss","Ground","Europe, Africa, Asia, Australia and Oceania, North America, South America",2,2,7.0000000000000007E-2,0,"",null,null,null,null,null,null,null,"6167XX0009.jpg",2,4,1,3,7,1,66,"CE","","","Class I",null,null,null,null,null,0,0,0,null,null,null,null,"6167XX0009.ldt",1,null,null,null,null,2,null,null,null,null,1,null,"LED",16,null,"",null,null,23,null,3000,80,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"","",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"Poland"]
["6460","6460XX0009","MORA POLE-TOP LED 2501LM 30D 3000K DALI2",null,"A mounting luminaire with a contemporary design, for mounting on a lighting pole with a base of Ø60mm",null,"Mora","Pole","Europe, Africa, Asia, Australia and Oceania, North America, South America",2,512,3.73,0,"",null,null,null,null,null,null,null,"6460XX0009.png",2,1,1,5,9,3,66,"CE","","IK08","Class I",null,null,null,null,null,0.46,0.15,0.27,null,null,null,null,"6460XX0009.ldt",1,null,null,null,null,0,null,null,null,null,null,null,"LED",16,null,"",null,null,23,null,3000,80,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"DALI","",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"Poland"]
["6461","6461XX0009","MORA POLE-TOP LED 2601LM DOWN 4000K DALI2",null,"A mounting luminaire with a contemporary design, for mounting on a lighting pole with a base of Ø60mm",null,"Mora","Pole","Europe, Africa, Asia, Australia and Oceania, North America, South America",2,512,3.73,0,"",null,null,null,null,null,null,null,"6461XX0009.png",2,1,1,5,9,3,66,"CE","","IK08","Class I",null,null,null,null,null,0.46,0.15,0.27,null,null,null,null,"6461XX0009.ldt",1,null,null,null,null,0,null,null,null,null,null,null,"LED",16,null,"",null,null,24,null,4000,80,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"DALI","",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"Poland"]
["6466","6466XX0009","MORA POLE-TOP LED 5002LM DOWN 3000K DALI2",null,"A mounting luminaire with a contemporary design, for mounting on a lighting pole with a base of Ø60mm",null,"Mora","Pole","Europe, Africa, Asia, Australia and Oceania, North America, South America",2,512,3.73,0,"",null,null,null,null,null,null,null,"6466XX0009.png",2,1,1,5,9,3,66,"CE","","IK08","Class I",null,null,null,null,null,0.85,0.15,0.27,null,null,null,null,"6466XX0009.ldt",1,null,null,null,null,0,null,null,null,null,null,null,"LED",16,null,"",null,null,23,null,3000,80,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"DALI","",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"Poland"]
["6467","6467XX0009","MORA POLE-TOP LED 5202LM DOWN 4000K DALI2",null,"A mounting luminaire with a contemporary design, for mounting on a lighting pole with a base of Ø60mm",null,"Mora","Pole","Europe, Africa, Asia, Australia and Oceania, North America, South America",2,512,3.73,0,"",null,null,null,null,null,null,null,"6467XX0009.png",2,1,1,5,9,3,66,"CE","","IK08","Class I",null,null,null,null,null,0.85,0.15,0.27,null,null,null,null,"6467XX0009.ldt",1,null,null,null,null,0,null,null,null,null,null,null,"LED",16,null,"",null,null,24,null,4000,80,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"DALI","",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"Poland"]
["XX","2024-04-08"]
["2935","2935XX0009","SKARA BOLLARD LED 828LM SCL 3000K DIM.",null,"A luminaire with a contemporary design. For lighting private areas and other architectural concepts.",null,"Skara","Bollard","Europe, Africa, Asia, Australia and Oceania, North America, South America",2,2,0.82,{"$f":"IF(K725=4,2.5,IF(K725=64,0.5,0))","v":0},"",null,null,null,null,null,null,null,"2935XX0009.png",6,1,2,3,6,1,66,"CE","","IK08","Class II",null,null,null,null,null,0,0,0,null,null,null,null,"2935XX0009.ldt",1,null,null,null,null,0,null,null,null,null,null,null,"LED",16,null,"",null,null,23,null,3000,80,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"","",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"Poland"]
["2937","2937XX0009","SKARA BOLLARD LED 856LM SCL 4000K DIM.",null,"A luminaire with a contemporary design. For lighting private areas and other architectural concepts.",null,"Skara","Bollard","Europe, Africa, Asia, Australia and Oceania, North America, South America",2,2,0.82,0,"",null,null,null,null,null,null,null,"2937XX0009.png",6,1,2,3,6,1,66,"CE","","IK08","Class II",null,null,null,null,null,0,0,0,null,null,null,null,"2937XX0009.ldt",1,null,null,null,null,0,null,null,null,null,null,null,"LED",16,null,"",null,null,24,null,4000,80,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"","",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"Poland"]
["2939","2939XX0009","SKARA BOLLARD LED 828LM VSM 3000K DIM.",null,"A luminaire with a contemporary design. For lighting private areas and other architectural concepts.",null,"Skara","Bollard","Europe, Africa, Asia, Australia and Oceania, North America, South America",2,2,0.82,0,"",null,null,null,null,null,null,null,"2939XX0009.png",4,1,2,3,6,1,66,"CE","","IK08","Class II",null,null,null,null,null,0,0,0,null,null,null,null,"2939XX0009.ldt",1,null,null,null,null,0,null,null,null,null,null,null,"LED",16,null,"",null,null,23,null,3000,80,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"","",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"Poland"]
["2941","2941XX0009","SKARA BOLLARD LED 856LM VSM 4000K DIM.",null,"A luminaire with a contemporary design. For lighting private areas and other architectural concepts.",null,"Skara","Bollard","Europe, Africa, Asia, Australia and Oceania, North America, South America",2,2,0.82,0,"",null,null,null,null,null,null,null,"2941XX0009.png",4,1,2,3,6,1,66,"CE","","IK08","Class II",null,null,null,null,null,0,0,0,null,null,null,null,"2941XX0009.ldt",1,null,null,null,null,0,null,null,null,null,null,null,"LED",16,null,"",null,null,24,null,4000,80,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"","",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"Poland"]
["2943","2943XX0009","SKARA BOLLARD - CONNECTORS E [UNI] LED 828LM SCL 3000K DIM.",null,"A luminaire with a contemporary design. For lighting private areas and other architectural concepts.",null,"Skara","Bollard","Europe, Africa, Asia, Australia and Oceania, North America, South America",2,2,0.82,0,"",null,null,null,null,null,null,null,"2943XX0009.png",6,1,2,3,6,1,66,"CE","","IK08","Class II",null,null,null,null,null,0,0,0,null,null,null,null,"2943XX0009.ldt",1,null,null,null,null,0,null,null,null,null,null,null,"LED",16,null,"",null,null,23,null,3000,80,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"","",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"Poland"]
["2945","2945XX0009","SKARA BOLLARD - CONNECTORS E [UNI] LED 828LM SCL 4000K DIM.",null,"A luminaire with a contemporary design. For lighting private areas and other architectural concepts.",null,"Skara","Bollard","Europe, Africa, Asia, Australia and Oceania, North America, South America",2,2,0.82,0,"",null,null,null,null,null,null,null,"2945XX0009.png",6,1,2,3,6,1,66,"CE","","IK08","Class II",null,null,null,null,null,0,0,0,null,null,null,null,"2945XX0009.ldt",1,null,null,null,null,0,null,null,null,null,null,null,"LED",16,null,"",null,null,24,null,4000,80,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"","",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"Poland"]
["2947","2947XX0009","SKARA BOLLARD - CONNECTORS E [UNI] LED 828LM VSM 3000K DIM.",null,"A luminaire with a contemporary design. For lighting private areas and other architectural concepts.",null,"Skara","Bollard","Europe, Africa, Asia, Australia and Oceania, North America, South America",2,2,0.82,0,"",null,null,null,null,null,null,null,"2947XX0009.png",4,1,2,3,6,1,66,"CE","","IK08","Class II",null,null,null,null,null,0,0,0,null,null,null,null,"2947XX0009.ldt",1,null,null,null,null,0,null,null,null,null,null,null,"LED",16,null,"",null,null,23,null,3000,80,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"","",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"Poland"]
["2949","2949XX0009","SKARA BOLLARD - CONNECTORS E [UNI] LED 856LM VSM 4000K DIM.",null,"A luminaire with a contemporary design. For lighting private areas and other architectural concepts.",null,"Skara","Bollard","Europe, Africa, Asia, Australia and Oceania, North America, South America",2,2,0.82,0,"",null,null,null,null,null,null,null,"2949XX0009.png",4,1,2,3,6,1,66,"CE","","IK08","Class II",null,null,null,null,null,0,0,0,null,null,null,null,"2949XX0009.ldt",1,null,null,null,null,0,null,null,null,null,null,null,"LED",16,null,"",null,null,24,null,4000,80,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"","",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"Poland"]
["4043","4043XX0009","SOL CEILING LED 2200LM 3000K DIM.",null,"A luminaire with a contemporary design. For lighting gardens, private areas and other architectural concepts",null,"Sol","Ceiling","Europe, Africa, Asia, Australia and Oceania, North America, South America",2,1,0,0,"",null,null,null,null,null,null,null,"4043XX0009.png",3,1,1,1,2,1,66,"CE","","IK06","Class I",null,null,null,null,null,0.2,0.2,0.11,null,null,null,null,"4043XX0009.ldt",1,null,null,null,null,0,null,null,null,null,null,null,"LED",16,null,"",null,null,23,null,3000,80,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"","",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"Poland"]
["4044","4044XX0009","SOL CEILING LED 2399LM 4000K DIM.",null,"A fixture with a contemporary design. For lighting gardens, private areas and other architectural concepts",null,"Sol","Ceiling","Europe, Africa, Asia, Australia and Oceania, North America, South America",2,1,0,0,"",null,null,null,null,null,null,null,"4044XX0009.png",3,1,1,1,2,1,66,"CE","","IK06","Class I",null,null,null,null,null,0.2,0.2,0.11,null,null,null,null,"4044XX0009.ldt",1,null,null,null,null,0,null,null,null,null,null,null,"LED",16,null,"",null,null,24,null,4000,80,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"","",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"Poland"]
["4045","4045XX0009","SOL CEILING LED 2200LM 3000K DIM.",null,"A luminaire with a contemporary design. For lighting gardens, private areas and other architectural concepts",null,"Sol","Ceiling","Europe, Africa, Asia, Australia and Oceania, North America, South America",2,1,0,0,"",null,null,null,null,null,null,null,"4045XX0009.png",3,1,1,1,2,1,66,"CE","","IK06","Class I",null,null,null,null,null,0.2,0.2,0.11,null,null,null,null,"4045XX0009.ldt",1,null,null,null,null,0,null,null,null,null,null,null,"LED",16,null,"",null,null,23,null,3000,80,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"","",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"Poland"]
["4046","4046XX0009","SOL CEILING LED 2399LM 4000K DIM.",null,"A luminaire with a contemporary design. For lighting gardens, private areas and other architectural concepts",null,"Sol","Ceiling","Europe, Africa, Asia, Australia and Oceania, North America, South America",2,1,0,0,"",null,null,null,null,null,null,null,"4046XX0009.png",3,1,1,1,2,1,66,"CE","","IK06","Class I",null,null,null,null,null,0.2,0.2,0.11,null,null,null,null,"4046XX0009.ldt",1,null,null,null,null,0,null,null,null,null,null,null,"LED",16,null,"",null,null,24,null,4000,80,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"","",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"Poland"]
["4047","4047XX0009","SOL CEILING LED 2200LM 3000K DALI2",null,"A luminaire with a contemporary design. For lighting gardens, private areas and other architectural concepts",null,"Sol","Ceiling","Europe, Africa, Asia, Australia and Oceania, North America, South America",2,1,0,0,"",null,null,null,null,null,null,null,"4047XX0009.png",3,1,1,1,2,3,66,"CE","","IK06","Class I",null,null,null,null,null,0.2,0.2,0.11,null,null,null,null,"4047XX0009.ldt",1,null,null,null,null,0,null,null,null,null,null,null,"LED",16,null,"",null,null,23,null,3000,80,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"DALI","",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"Poland"]
["4048","4048XX0009","SOL CEILING LED 2400LM 4000K DALI2",null,"A luminaire with a contemporary design. For lighting gardens, private areas and other architectural concepts",null,"Sol","Ceiling","Europe, Africa, Asia, Australia and Oceania, North America, South America",2,1,0,0,"",null,null,null,null,null,null,null,"4048XX0009.png",3,1,1,1,2,3,66,"CE","","IK06","Class I",null,null,null,null,null,0.2,0.2,0.11,null,null,null,null,"4048XX0009.ldt",1,null,null,null,null,0,null,null,null,null,null,null,"LED",16,null,"",null,null,24,null,4000,80,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"DALI","",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"Poland"]
["4049","4049XX0009","SOL CEILING LED 2200LM 3000K DALI2",null,"A luminaire with a contemporary design. For lighting gardens, private areas and other architectural concepts",null,"Sol","Ceiling","Europe, Africa, Asia, Australia and Oceania, North America, South America",2,1,0,0,"",null,null,null,null,null,null,null,"4049XX0009.png",3,1,1,1,2,3,66,"CE","","IK06","Class I",null,null,null,null,null,0.2,0.2,0.11,null,null,null,null,"4049XX0009.ldt",1,null,null,null,null,0,null,null,null,null,null,null,"LED",16,null,"",null,null,23,null,3000,80,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"DALI","",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"Poland"]
["4050","4050XX0009","SOL CEILING LED 2400LM 4000K DALI2",null,"A luminaire with a contemporary design. For lighting gardens, private areas and other architectural concepts",null,"Sol","Ceiling","Europe, Africa, Asia, Australia and Oceania, North America, South America",2,1,0,0,"",null,null,null,null,null,null,null,"4050XX0009.png",3,1,1,1,2,3,66,"CE","","IK06","Class I",null,null,null,null,null,0.2,0.2,0.11,null,null,null,null,"4050XX0009.ldt",1,null,null,null,null,0,null,null,null,null,null,null,"LED",16,null,"",null,null,24,null,4000,80,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"DALI","",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"Poland"]
["4119","4119XX0009","LONDON WALL-ARM LED 2000LM 4000K ON/OFF",null,"A wall luminaire with a classic design for general use. Can be mounted on the corners of architectural structures.",null,"London","Wall","Europe, Africa, Asia, Australia and Oceania, North America, South America",2,4,0.3,2.5,"",null,null,null,null,null,null,null,"4119XX0009.png",9,1,2,2,2,4,55,"CE","","","Class II",null,null,null,null,null,0,0,0,null,null,null,null,"4119XX0009.ldt",1,null,null,null,null,1,null,null,null,null,null,null,"LED",16,null,"",null,null,24,null,4000,80,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"","",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"Poland"]
["7150","7150XX0009","VARBERG LED T4-B 3000K DALI2",null,"For illuminating building facades, gardens, private areas and other architectural concepts. Possibility to adjust the direction of light also in the vertical plane. The luminaire is also suitable for direct voltage: DC 168 ÷ 275 V",null,"Varberg","Ground,Ground/Wall","Europe, Africa, Asia, Australia and Oceania, North America, South America",2,2,7.0000000000000007E-2,0,"",null,null,null,null,null,null,null,"7150XX0009.png",5,1,2,3,6,3,66,"CE","","IK10","Class I",null,null,null,null,null,0,0,0,null,null,null,null,"7150XX0009.ldt",1,null,null,null,null,1,null,null,null,null,null,null,"LED",16,null,"",null,null,23,null,3000,70,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"DALI","",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"Poland"]
["7151","7151XX0009","VARBERG LED T4-B 4000K DALI2",null,"Luminaire for illuminating facades, gardens, private areas and other architectural concepts. Possibility to adjust the direction of light also in the vertical plane. The luminaire is also suitable for direct voltage: DC 168 ÷ 275 V",null,"Varberg","Ground,Ground/Wall","Europe, Africa, Asia, Australia and Oceania, North America, South America",2,2,7.0000000000000007E-2,{"$f":"IF(K743=4,2.5,IF(K743=64,0.5,0))","v":0},"",null,null,null,null,null,null,null,"7151XX0009.png",5,1,2,3,6,3,66,"CE","","IK10","Class I",null,null,null,null,null,0,0,0,null,null,null,null,"7151XX0009.ldt",1,null,null,null,null,1,null,null,null,null,null,null,"LED",16,null,"",null,null,24,null,4000,70,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"DALI",""]
["7153","7153XX0009","VARBERG LED T4-B 3000K DALI2",null,"Luminaire for illuminating facades, gardens, private areas and other architectural concepts. Possibility to adjust the direction of light also in the vertical plane.",null,"Varberg","Ground,Ground/Wall","Europe, Africa, Asia, Australia and Oceania, North America, South America",2,2,7.0000000000000007E-2,0,"",null,null,null,null,null,null,null,"7153XX0009.png",5,1,2,3,6,3,66,"CE","","IK08","Class I",null,null,null,null,null,0,0,0,null,null,null,null,"7153XX0009.ldt",1,null,null,null,null,1,null,null,null,null,null,null,"LED",16,null,"",null,null,23,null,3000,80,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"DALI",""]
["7152","7152XX0009","VARBERG LED T4-B 3000K DIM. TRIAC",null,"Luminaire for illuminating facades, gardens, private areas and other architectural concepts. Possibility to adjust the direction of light also in the vertical plane.",null,"Varberg","Ground,Ground/Wall","Europe, Africa, Asia, Australia and Oceania, North America, South America",2,2,7.0000000000000007E-2,0,"",null,null,null,null,null,null,null,"7152XX0009.png",5,1,2,3,6,1,66,"CE","","IK08","Class I",null,null,null,null,null,0,0,0,null,null,null,null,"7152XX0009.ldt",1,null,null,null,null,1,null,null,null,null,null,null,"LED",16,null,"",null,null,23,null,3000,80,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"","",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"Poland"]
["7154","7154XX0009","VARBERG LED T4-B 4000K DIM. TRIAC",null,"Luminaire for illuminating facades, gardens, private areas and other architectural concepts. Possibility to adjust the direction of light also in the vertical plane.",null,"Varberg","Ground,Ground/Wall","Europe, Africa, Asia, Australia and Oceania, North America, South America",2,2,7.0000000000000007E-2,0,"",null,null,null,null,null,null,null,"7154XX0009.png",5,1,2,3,6,1,66,"CE","","IK08","Class I",null,null,null,null,null,0,0,0,null,null,null,null,"7154XX0009.ldt",1,null,null,null,null,1,null,null,null,null,null,null,"LED",16,null,"",null,null,24,null,4000,80,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"","",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"Poland"]
["7155","7155XX0009","VARBERG LED T4-B 4000K DALI2",null,"Luminaire for illuminating facades, gardens, private areas and other architectural concepts. Possibility to adjust the direction of light also in the vertical plane.",null,"Varberg","Ground,Ground/Wall","Europe, Africa, Asia, Australia and Oceania, North America, South America",2,2,7.0000000000000007E-2,0,"",null,null,null,null,null,null,null,"7155XX0009.png",5,1,2,3,6,3,66,"CE","","IK08","Class I",null,null,null,null,null,0,0,0,null,null,null,null,"7155XX0009.ldt",1,null,null,null,null,1,null,null,null,null,null,null,"LED",16,null,"",null,null,24,null,4000,80,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"DALI","",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"Poland"]

{"sheet":"Arkusz1","index":3,"n_rows":25,"n_cols":4,"rows_kept":25,"cut":false,"hidden":false,"merged":[]}
["6146",null,"6146","6153"]
["6148",null,"6148"]
["6352"]
["6355"]
["6361"]
["6370"]
["6376"]
["6379"]
["6385"]
["6471",null,"6471"]
["6483",null,"6483"]
["6485",null,"6485"]
["6600",null,"6600"]
["6601",null,"6601"]
["6603",null,"6603"]
["6732",null,"6732"]
["6735",null,"6735"]
["6738",null,"6738"]
["6750",null,"6750"]
["6753",null,"6753"]
["6756",null,"6756"]
["6772",null,"6772"]
["6778",null,"6778"]
["7120",null,"7120"]
["891",null,"891"]

{"sheet":"Regions","index":4,"n_rows":55,"n_cols":6,"rows_kept":55,"cut":false,"hidden":false,"merged":[]}
[]
[]
["Africa","Asia","Australia and Oceania","Europe","North America","South America"]
["Algeria","Afghanistan","Australia","Åland Islands","Antigua and Barbuda","Argentina"]
["Angola","Bahrain","Cocos (Keeling) Islands","Albania","Bahamas","Bolivia"]
["Benin","Bangladesh","Federated States of Micronesia","Andorra","Barbados","Brazil"]
["Botswana","Bhutan","Fiji","Armenia","Belize","Chile"]
["Burkina Faso","British Indian Ocean Territory","Kiribati","Austria","Canada","Colombia"]
["Burundi","Brunei","Marshall Islands","Azerbaijan","Caribbean Netherlands","Ecuador"]
["Cabo Verde","Cambodia","Nauru","Belarus","Costa Rica","Falkland Islands"]
["Cameroon","China","New Zealand","Belgium","Cuba","Guyana"]
["Central African Republic","India","Palau","Bosnia and Herzegovina","Dominica","Paraguay"]
["Chad","Indonesia","Papua New Guinea","Bulgaria","Dominican Republic","Peru"]
["Comoros","Iran","Samoa","Croatia","El Salvador","Suriname"]
["Djibouti","Iraq","Solomon Islands","Cyprus","Grenada","Uruguay"]
["Egypt","Israel","Tonga","Czech Republic","Guatemala","Venezuela"]
["Equatorial Guinea","Japan","Tuvalu","Denmark","Haiti"]
["Eritrea","Jordan","Vanuatu","Estonia","Honduras"]
["Ethiopia","Kazakhstan",null,"Finland","Jamaica"]
["Gabon","Kuwait",null,"France","Monaco"]
["Gambia","Kyrgyzstan",null,"Georgia","Nicaragua"]
["Ghana","Laos",null,"Germany","Panama"]
["Guinea","Lebanon",null,"Greece","Saint Barthélemy"]
["Guinea-Bissau","Malaysia",null,"Holy See (Vatican City State)","Saint Kitts and Nevis"]
["Ivory Coast","Maldives",null,"Hungary","Saint Vincent"]
["Kenya","Mongolia",null,"Iceland","Trinidad and Tobago"]
["Lesotho","Myanmar",null,"Ireland","United States"]
["Liberia","Nepal",null,"Italy"]
["Libya","North Korea",null,"Jersey"]
["Madagascar","Oman",null,"Latvia"]
["Malawi","Pakistan",null,"Liechtenstein"]
["Mali","Philippines",null,"Lithuania"]
["Mauritania","Qatar",null,"Luxembourg"]
["Mauritius","Russia",null,"Malta"]
["Morocco","Saudi Arabia",null,"Moldova"]
["Mozambique","Singapore",null,"Monaco"]
["Namibia","South Korea",null,"Montenegro"]
["Niger","Sri Lanka",null,"Netherlands"]
["Nigeria","Syrian Arab Republic",null,"North Macedonia"]
["Republic of the Congo","Taiwan",null,"Norway"]
["Rwanda","United Arab Emirates",null,"Poland"]
["Sao Tome and Principe","Uzbekistan",null,"Portugal"]
["Senegal","Vietnam",null,"Romania"]
["Seychelles","Yemen",null,"San Marino"]
["Sierra Leone",null,null,"Serbia"]
["South Africa",null,null,"Slovakia"]
["South Sudan",null,null,"Slovenia"]
["Sudan",null,null,"Spain"]
["Tanzania",null,null,"Sweden"]
["The Democratic Republic of the Congo",null,null,"Switzerland"]
["Togo",null,null,"Turkey"]
["Tunisia",null,null,"Ukraine"]
["Uganda",null,null,"United Kingdom"]
["Zambia"]
["Zimbabwe"]

{"sheet":"Article translations","index":5,"n_rows":7,"n_cols":8,"rows_kept":7,"cut":false,"hidden":false,"merged":[[1,0,1,6]]}
["Add optional translations for product texts"]
["A R T I C L E ",null,null,null,null,null,null,"L A M P"]
["InternalIdentifier","LanguageID","ArticleNumber","ArticleName","DescriptionText","FamilyName","AssortmentName","LampName"]
[2,1031,"A-0002","Beispiel 2","Das zweite Beispielprodukt: Eine Wandleuchte, die nicht in Gebrauchslage sondern als Deckenleuchte gemessen wurde.","Beispiele","Wohnbereich","AGL"]
[2,1034,"A-0002","Ejemplo 2","[…]","[…]","[…]","[…]"]
[3,1031,"2GT","Zwei Gruppen mit Übersetzungen","Dies ist der Beschreibungstext des dritten Beispielprodukts.\nIm Beschreibungstext können \nZeilenumbrüche\nverwendet werden!","Beispiele, noch mehr, asdkpoasdkopads","Büro & Bildung","T5"]
[3,1034,"2GT","Ejemplo 1","[…]","[…], [...]","[…]","[…]"]

{"sheet":"Region translations","index":6,"n_rows":3,"n_cols":3,"rows_kept":3,"cut":false,"hidden":false,"merged":[[1,0,1,2],[0,0,0,2]]}
["Add optional translations for regions"]
["R E G I O N"]
["Region name","LanguageID","Translation"]

{"sheet":"Possible values","index":7,"n_rows":589,"n_cols":13,"rows_kept":589,"cut":false,"hidden":false,"merged":[]}
["ProductTypeID","Product type",null,null,null,null,null,"Typ montażu"]
[1,"Interior Luminaire",null,null,"DcMountingPlaceId","DcMountingTypeId","MountingTypeID","id_rodzaj","rodz_nazwa","AdditionalMountingType","DcMountingTypeId","Mounting type"]
[2,"Exterior Luminaire",null,null,3,6,2,1,"Oprawa słupkowa.",null,1,"recessed"]
[3,"Interior and Exterior Luminaire",null,null,5,9,512,2,"Oprawa słupowa (nasadzana).",null,2,"surface"]
[null,null,null,null,2,1,8,3,"Oprawa wbudowana.",null,3,"semi recessed"]
["MountingTypeID","Mounting type",null,null,3,6.7,2,4,"Oprawa typu reflektor.",null,4,"suspended"]
[1,"Surface-Mounted on ceiling",null,null,1,2,1,6,"Oprawa sufitowa.",null,5,"track"]
[2,"Standing",null,null,2,2,4,7,"Oprawa sufitowo-ścienna.","Ceiling mounted",6,"bollard"]
[4,"Surface-Mounted on wall",null,null,3,6,2,8,"Oprawa słupkowa-dystrybutor energii.",null,7,"movable"]
[8,"Recessed",null,null,2,1,64,11,"Oprawa wbudowana ścienna.",null,8,"pole integrated"]
[16,"Suspended",null,null,2,2,4,12,"Oprawa ścienna.",null,9,"pole top"]
[32,"Table luminaire",null,null,3,6,2,13,"Oprawa słupkowa.",null,10,"other"]
[64,"Recessed in wall",null,null,3,1,128,14,"Oprawa wbudowana w podłoże."]
[128,"Recessed in floor",null,null,1,4,16,16,"Oprawa wisząca."]
[256,"Pole-integrated",null,null,3,7,2,17,"Oprawa typu reflektor, przenośna gruntowa."]
[512,"Pole-top",null,null,2,2,4,19,"Oprawa ścienna- dystrybutor energii."]
[null,null,null,null,5,9,512,20,"Oprawa słupowa (lekka konstrukcja)."]
["AdditionalMountingType",null,null,null,2,2,4,21,"Oprawa ścienna na ramieniu."]
["Ceiling mounted",null,null,null,5,8,256,23,"Oprawa słupowa."]
["Ceiling recessed",null,null,null,3,6,2,24,"Oprawa słupkowa (podest)."]
["Wall mounted",null,null,null,3,2,4,25,"Oprawa typu reflektor na ramieniu."]
["Wall recessed",null,null,null,3,6,2,27,"Oprawa słupkowa (filar)."]
["Floor mounted",null,null,null,5,9,512,29,"Oprawa słupowa (do montażu na słupie)."]
["Floor recessed",null,null,null,3,7,2,40,"Oprawa typu reflektor, przenośna."]
["Pendant",null,null,null,3,6,2,41,"Oprawa słupkowa - dystrybutor energii E [Uni]."]
["Mounting rail / light-band",null,null,null,3,6,2,42,"Oprawa słupkowa - dystrybutor bez osprzętu."]
["Pole integrated",null,null,null,1,2,1,47,"Oprawa liniowa sufitowa."]
["Pole top",null,null,null,3,6,2,50,"Oprawa typu naświetlacz"]
["Guy cables"]
["Standing / Bolladrd"]
["Standard 3-phase system"]
["Other system"]
["Light system"]
["Table luminaire"]
["Clamp fixture"]
[]
["DcLightDistributionId","Light distribution"]
[1,"(Symmetrical) narrow beam (half value angle <=15°)"]
[2,"(Symmetrical) Medium flood (half value angle 15°…45°)"]
[3,"(Symmetrical) Wide flood (half value angle 45°…125°)"]
[4,"2-axis symmetrical"]
[5,"Asymmetrical flood (wall washer)"]
[6,"Asymmetrical wide flood"]
[7,"Diffuse - half spherical"]
[8,"Diffuse - full spherical"]
[9," "]
[10,"other"]
[]
["DcAdjustabilityId","Adjustibility"]
[1,"fixed"]
[2,"rotatable"]
[3,"tiltable"]
[4,"rotatable and tiltable"]
[5,"adjustable"]
[6,"cardanic"]
[7,"height adjustable"]
[]
["DcShapeId","Shape"]
[1,"round","Okrągła"]
[2,"quadratic (compact rectangular)","Prostokątna"]
[3,"linear","Liniowa"]
[4,"area luminaire (A>0.5 sqm)","Powierzchnia > 0,5m2"]
[5,"special","Specjalna"]
[]
["DcMountingPlaceId","Mounting place"]
[1,"ceiling"]
[2,"wall"]
[3,"floor"]
[4,"table"]
[5,"pole"]
[6,"other"]
[]
["DcMountingTypeId","Mounting type"]
[1,"recessed"]
[2,"surface"]
[3,"semi recessed"]
[4,"suspended"]
[5,"track"]
[6,"bollard"]
[7,"movable"]
[8,"pole integrated"]
[9,"pole top"]
[10,"other"]
[]
["DcControllabilityId","Controllability"]
[1,"dimmable",null,null,null,null,null,null,null,null,null,null,"(Symmetrical) Wide flood (half value angle 45°…125°)"]
[2,"color adjustable"]
[3,"embedded sensor system"]
[4,"none"]
[]
["DcProtectionId","IP"]
[1,"00"]
[2,"01"]
[3,"02"]
[4,"03"]
[5,"04"]
[6,"05"]
[7,"06"]
[8,"07"]
[9,"08"]
[10,"0X"]
[11,"10"]
[12,"11"]
[13,"12"]
[14,"13"]
[15,"14"]
[16,"15"]
[17,"16"]
[18,"17"]
[19,"18"]
[20,"1X"]
[21,"20"]
[22,"21",null,null,null,null,null,null,null,null,{"$f":"IFERROR(INDEX($A$38:$B$47,MATCH($L113,$B$38:$B$47,0),1),\"\")","v":""}]
[23,"22",null,null,null,null,null,null,null,null,""]
[24,"23",null,null,null,null,null,null,null,null,""]
[25,"24",null,null,null,null,null,null,null,null,""]
[26,"25",null,null,null,null,null,null,null,null,""]
[27,"26",null,null,null,null,null,null,null,null,""]
[28,"27",null,null,null,null,null,null,null,null,""]
[29,"28",null,null,null,null,null,null,null,null,""]
[30,"2X",null,null,null,null,null,null,null,null,""]
[31,"30",null,null,null,null,null,null,null,null,""]
[32,"31",null,null,null,null,null,null,null,null,""]
[33,"32",null,null,null,null,null,null,null,null,""]
[34,"33",null,null,null,null,null,null,null,null,""]
[35,"34",null,null,null,null,null,null,null,null,""]
[36,"35",null,null,null,null,null,null,null,null,""]
[37,"36",null,null,null,null,null,null,null,null,""]
[38,"37",null,null,null,null,null,null,null,null,""]
[39,"38",null,null,null,null,null,null,null,null,""]
[40,"3X",null,null,null,null,null,null,null,null,""]
[41,"40",null,null,null,null,null,null,null,null,""]
[42,"41",null,null,null,null,null,null,null,null,""]
[43,"42"]
[44,"43"]
[45,"44"]
[46,"45"]
[47,"46"]
[48,"47"]
[49,"48"]
[50,"4X"]
[51,"50"]
[52,"51"]
[53,"52"]
[54,"53"]
[55,"54"]
[56,"55"]
[57,"56"]
[58,"57"]
[59,"58"]
[60,"5X"]
[61,"60"]
[62,"61"]
[63,"62"]
[64,"63"]
[65,"64"]
[66,"65"]
[67,"66"]
[68,"67"]
[69,"68"]
[70,"6X"]
[71,"X0"]
[72,"X1"]
[73,"X2"]
[74,"X3"]
[75,"X4"]
[76,"X5"]
[77,"X6"]
[78,"X7"]
[79,"X8"]
[80,"XX"]
[]
["Labelling"]
["ENEC"]
["GS"]
["MM"]
["Luke warm"]
["UL"]
["CCC"]
["CE"]
["F"]
["FF"]
["MM"]
[]
["Safety"]
["Suitable for clean rooms"]
["Resistant to impact of balls"]
["Vehicle resistant"]
["Slip resistant"]
[]
["IK Code"]
["IK00"]
["IK01"]
["IK02"]
["IK03"]
["IK04"]
["IK05"]
["IK06"]
["IK07"]
["IK08"]
["IK09"]
["IK10"]
[]
["Appliance class"]
["Class 0"]
["Class I"]
["Class II"]
["Class III"]
[]
["ExplosionProtection"]
["Zone 0"]
["Zone 1"]
["Zone 2"]
["Zone 10"]
["Zone 11"]
[]
["Accessory","Details"]
["Color filter"]
["UV protection filter"]
["IR protection filter"]
["Glare protection","Honeycomb or ring-shaped anti-dazzle screen"]
["Gobo"]
["Decorative elements","E.g. saturn ring, glass cylinder"]
["Installation housing","Installation housing for stonework or concrete surface"]
["Mounting foot"]
["Installation peg"]
["Poles"]
["Boom"]
[]
["Shape3DID","Shape 3D"]
[1,"Cuboid"]
[2,"Vertical Cylinder"]
[4,"Horizontal Cylinder"]
[8,"Sphere"]
[16,"Cone"]
[32,"Horizontal Cylinder in X"]
[64,"Horizontal Cone in Y"]
[128,"Horizontal Cone in X"]
[]
["LumDistTypeID","Light distribution"]
[1,"direct"]
[2,"indirect"]
[4,"direct/indirect"]
[]
["Shape2DID","Shape 2D"]
[1,"Rectangular"]
[2,"Circular"]
[]
["LeoPositionRelativeToCaseID","LeoPositionRelativeToCase"]
[0,"Horizontal Bottom\nPossible for:\n  - Surface-Mounted on ceiling\n  - Surface-Mounted on wall\n  - Recessed\n  - Suspended\n  - Pole-integrated\n  - Pole-top","Pionowo, dół"]
[1,"Horizontal Middle\nPossible for:\n  - Surface-Mounted on ceiling\n  - Surface-Mounted on wall\n  - Suspended\n  - Pole-integrated\n  - Pole-top\n  - Standing ","Pionowo, środek"]
[2,"Horizontal Top\nPossible for:\n  - Standing\n  - Surface-Mounted on wall\n  - Suspended\n  - Table luminaire\n  - Recessed in floor","Pionowo, góra"]
[3,"Vertical Center\nPossible for:\n  - Surface-Mounted on wall","Poziomo, środek"]
[4,"Vertical Front\nPossible for:\n  - Surface-Mounted on wall\n  - Recessed in wall","Poziomo, front"]
[]
["LanguageID","Language"]
[1028,"Chinese (Traditional)"]
[1029,"Czech"]
[1030,"Danish"]
[1031,"German"]
[1032,"Greek"]
[1033,"American"]
[1034,"Spanish (Standard/Traditional)"]
[1035,"Finnish"]
[1036,"French"]
[1038,"Hungarian"]
[1039,"Icelandic"]
[1040,"Italian"]
[1043,"Dutch"]
[1044,"Norwegian (Bokmal)"]
[1045,"Polish"]
[1046,"Portuguese (Brazilian)"]
[1041,"Japanese"]
[1049,"Russian"]
[1051,"Slovak"]
[1053,"Swedish"]
[1055,"Turkish"]
[2052,"Chinese (Simplified)"]
[2055,"Swiss"]
[2057,"British"]
[2058,"Mexican"]
[2060,"Belgian"]
[2064,"Swiss"]
[2067,"Belgian (Flemish)"]
[2068,"Norwegian (Nynorsk)"]
[2070,"Portuguese"]
[3079,"Austrian"]
[3081,"Australian"]
[3082,"Spanish (Modern)"]
[3084,"Canadian"]
[4105,"Canadian"]
[4108,"Swiss"]
[5129,"New Zealand"]
[6153,"Ireland"]
[]
["RotatePhotometryForMountingTypeID","RotatePhotometryForMountingType"]
[0,"Do nothing"]
[1,"Rotate"]
[]
["LampTypeID","Lamp type ID"]
[1,"Other"]
[2,"incandescent lamp"]
[3,"high voltage tungsten halogen lamp"]
[4,"low voltage tungsten halogen lamp"]
[5,"fluorescent lamp tube-shaped T 7"]
[6,"fluorescent lamp tube-shaped T 16"]
[7,"fluorescent lamp tube-shaped T 26"]
[8,"fluorescent lamp tube-shaped T 38"]
[9,"fluorescent lamp ring-shaped"]
[10,"compact fluorescent lamps"]
[11,"induction lamp"]
[12,"metal halide lamp"]
[13,"high pressure mercury vapour lamp"]
[14,"high pressure sodium vapour lamp"]
[15,"low pressure sodium vapour lamp"]
[16,"LED"]
[]
["SpectrumID","Spectrum"]
[1,"LED blue"]
[2,"LED green"]
[3,"LED red"]
[4,"Metal halide discharge lamp 830"]
[5,"Metal halide discharge lamp 942"]
[6,"Halogen incandescent lamp (high-voltage)"]
[7,"Illuminant A"]
[8,"Illuminant D65"]
[9,"Flourescent lamp 640"]
[10,"Flourescent lamp 827"]
[11,"Flourescent lamp 830"]
[12,"Flourescent lamp 840"]
[13,"Flourescent lamp 930"]
[14,"Flourescent lamp 940"]
[15,"Flourescent lamp 950"]
[16,"Halogen incandescent lamp (low-voltage)"]
[17,"Mercury discharge lamp"]
[18,"Sodium discharge lamp professional"]
[19,"Sodium discharge lamp standard"]
[20,"Standard incandescent lamp"]
[21,"Flourescent lamp 880"]
[22,"Flourescent lamp 15000K"]
[23,"LED 3000K"]
[24,"LED 4000K"]
[25,"LED 5500K"]
[26,"LED 6800K"]
[]
["Application","Details"]
["Streets","Streets moving traffic and parking lots"]
["Tunnel"]
["Lighting elements ","Luminous ceiling / wall elements"]
["Orientation and safety"]
["Sports","Sports and recreational facilities"]
["Facade illumination"]
["Industry and workshops"]
["Health care"]
["Shops and display"]
["Hotels","Hotels and prestige objects"]
["Kitchens"]
["Bathrooms"]
["Living rooms","Living and dining rooms and bedrooms"]
["Children´s rooms"]
["Furniture","Luminaires for furniture, pictures and mirrors"]
["Private outdoor","Gardens, patios and pathways"]
["Administration","Administration, education and research"]
["Basements and garages"]
[]
["BallastType"]
["CCG"]
["ECG"]
[]
["Controller"]
["DALI"]
["DMX"]
["Dimmable 0..10V"]
["Dimmable 1..10V"]
["Integrated control gear"]
["Hot restartable"]
[]
["IntegratedSensor"]
["Daylight sensor"]
["Motion sensor"]
["Presence sensor"]
[]
["LightDeflection"]
["Clear glass"]
["Bowl"]
["Reflector with louver: bright"]
["Reflector with louver: matt"]
["Reflector with louver: white"]
["Prisms and lenses"]
["Diffuser"]
[]
["SaturatedLightColor"]
["blue"]
["green"]
["yellow"]
["red"]
["violet"]
[]
["Voltage type"]
["AC"]
["DC"]
[]
["Integrated switch"]
["Has integrated switch in cord"]
["Has integrated switch in housing"]
["No integrated switch"]
[]
["Impression"]
["Decorative"]
["Technical"]
[]
["ImpressionSurface"]
["Gloss"]
["Matt"]
["Transparent"]
["Aluminium"]
["Bronze"]
["Chrome"]
["Stainless steel"]
["COR-TEN steel"]
["Glass"]
["Wood"]
["Ceramic"]
["Plastic"]
["Copper"]
["Leather"]
["Brass"]
["Nickel"]
["Porcelain"]
["Stone"]
["Textile"]
[]
["Color"]
["White"]
["Black"]
["Silver"]
["Gold"]
["Anthracite / graphite"]
["Blue"]
["Green"]
["Yellow"]
["Orange"]
["Red"]
[]
["UnitOfLengthID","Unit of lenth"]
[1,"Meter"]
[2,"Feet"]
[]
["DesignerOriginCountry"]
["Afghanistan"]
["Albania"]
["Algeria"]
["Argentina"]
["Armenia"]
["Australia"]
["Austria"]
["Azerbaijan"]
["Bahrain"]
["Bangladesh"]
["Belarus"]
["Belgium"]
["Belize"]
["Bhutan"]
["Bolivia"]
["Bosnia and Herzegovina"]
["Botswana"]
["Brazil"]
["Brunei"]
["Bulgaria"]
["Cambodia"]
["Cameroon"]
["Canada"]
["Caribbean"]
["Chile"]
["China"]
["Colombia"]
["Congo (DRC)"]
["Costa Rica"]
["Côte d’Ivoire"]
["Croatia"]
["Cuba"]
["Czech Republic"]
["Denmark"]
["Dominican Republic"]
["Ecuador"]
["Egypt"]
["El Salvador"]
["Eritrea"]
["Estonia"]
["Ethiopia"]
["Faroe Islands"]
["Finland"]
["France"]
["Georgia"]
["Germany"]
["Greece"]
["Greenland"]
["Guatemala"]
["Haiti"]
["Honduras"]
["Hong Kong SAR"]
["Hungary"]
["Iceland"]
["India"]
["Indonesia"]
["Iran"]
["Iraq"]
["Ireland"]
["Israel"]
["Italy"]
["Jamaica"]
["Japan"]
["Jordan"]
["Kazakhstan"]
["Kenya"]
["Korea"]
["Kuwait"]
["Kyrgyzstan"]
["Laos"]
["Latin America"]
["Latvia"]
["Lebanon"]
["Libya"]
["Liechtenstein"]
["Lithuania"]
["Luxembourg"]
["Macao SAR"]
["Macedonia, FYRO"]
["Malaysia"]
["Maldives"]
["Mali"]
["Malta"]
["Mexico"]
["Moldova"]
["Monaco"]
["Mongolia"]
["Montenegro"]
["Morocco"]
["Myanmar"]
["Nepal"]
["Netherlands"]
["New Zealand"]
["Nicaragua"]
["Nigeria"]
["Norway"]
["Oman"]
["Pakistan"]
["Panama"]
["Paraguay"]
["Peru"]
["Philippines"]
["Poland"]
["Portugal"]
["Puerto Rico"]
["Qatar"]
["Réunion"]
["Romania"]
["Russia"]
["Rwanda"]
["Saudi Arabia"]
["Senegal"]
["Serbia"]
["Singapore"]
["Slovakia"]
["Slovenia"]
["Somalia"]
["South Africa"]
["Spain"]
["Sri Lanka"]
["Sweden"]
["Switzerland"]
["Syria"]
["Taiwan"]
["Tajikistan"]
["Thailand"]
["Trinidad and Tobago"]
["Tunisia"]
["Turkey"]
["Turkmenistan"]
["Ukraine"]
["United Arab Emirates"]
["United Kingdom"]
["United States"]
["Uruguay"]
["Uzbekistan"]
["Venezuela"]
["Vietnam"]
["Yemen"]
["Zimbabwe"]

{"sheet":"DATA","index":8,"n_rows":771,"n_cols":63,"rows_kept":771,"cut":false,"hidden":false,"merged":[]}
[1,2,3,4,5,6,7,8,9,10,11,12,13,14,15,16,17,18,19,20,21,22,23,24,25,26,27,28,29,30,31,32,33,34,35,36,37,38,39,40,41,42,43,44,45,46,47,48,49,50,51,52,53,54,55,56,57,58,59,60,61,62,62]
["InternalIdentifier","ArticleNumber","ArticleName","Group1Name","zastosowanie","material_glowny","material_dodatkowy","material_kolor_dod","pro","zrodlo_swiatla_wymienialnosc","zrodlo_swiatla_typ","zrodlo_swiatla_opcja","moc_lampy","moc_oprawy","strumien_swietlny_lampy","strumien_swietlny_oprawy","material_klosz_material","material_klosz_kolor","ip","ik","klasa_bezpieczenstwa","barwa_led","kierunek_swiecenia","wymiary_oprawy_dl","wymiary_oprawy_szer","wymiary_oprawy_wys","labelling","IntegratedSensor","Controller","trwalosc_zrodel_swiatla","id_rodzaj","rodzaj","bryla_fotometryczna","bryla_fotometryczna_skrot","charakterystyka","charakterystyka_dodatkowa","prad_staly","info_zrodlo_swiatla","material_1","material_2","material_klosz","material_uszczelka","material_inne","cecha_specjalna_1","cecha_specjalna_2","sterowanie_swiatlem","nazwa_lampy","modul_led","zasilacz","zasilacz_trwalosc","sterowanie_zewnetrzne","ulor","cri","klasa_eei","akcesoria","przylacze_elektryczne","zdjecie","photometry","Controllability","SocketName","regulation","id_brylafoto"]
["1000","1000XX0009","TRYSIL 263CM 4XLED 3976LM DOWN 3000K DIM.","Trysil","Post","Aluminium",null,null,null,"LED zintegrowane","AC","DIM.","21,2W","25W","3976lm","2433lm",null,null,"65","IK10","Class I",3000,"szerokie dół",1.18,0.24,2.63,"CE",null,null,"> 102000h",23,"Oprawa słupowa.","Światło rozproszone półsferyczne ukierunkowane w dół",null,"Luminaire with a contemporary design. For lighting gardens, private areas, and other architectural concepts",null,null,null,"Profil aluminiowy wyciskany, malowany proszkowo.",null,"Klosz- poliwęglan przeźroczysty ze strukturą, stabilizowany UV.","Uszczelka silikonowa.",null,"263cm","Podwójna","Oprawa ściemnialna fazowo TRAILING EDGE (TE) - LEADING EDGE (LE)","4 Moduły LED","Cree DK200305 V3 JB2835 3V 3K","TCI Mini MD 12,5W 250mA code 127036 Triac",0,null,null,80,"C","3091GA0009","Zaciski podłączeniowe: max 3x4mm², możliwość podłączenia oprawy w pętle max 3x2,5mm². Przewód w oponie okrągłej o średnicy max ø12,5 mm.","1000XX0009.png","1000XX0009.ldt",1,null,1,76]
["1001","1001XX0009","TRYSIL 263CM 4XLED 4168LM DOWN 4000K DIM.","Trysil","Post","Aluminium",null,null,null,"LED zintegrowane","AC","DIM.","21,2W","25W","4168lm","2476,1lm",null,null,"65","IK10",null,4000,"szerokie dół",1.18,0.24,2.63,"CE",null,null,"> 102000h",23,"Oprawa słupowa.","Światło rozproszone półsferyczne ukierunkowane w dół",null,"Luminaire with a contemporary design. For lighting gardens, private areas, and other architectural concepts",null,null,null,"Profil aluminiowy wyciskany, malowany proszkowo.",null,"Klosz- poliwęglan przeźroczysty ze strukturą, stabilizowany UV.","Uszczelka silikonowa.",null,"263cm","Podwójna","Oprawa ściemnialna fazowo TRAILING EDGE (TE) - LEADING EDGE (LE)","4 Moduły LED","Cree DK200305 V3 JB2835 3V 4K","TCI Mini MD 12,5W 250mA code 127036 Triac",0,null,null,80,"C","3091GA0009","Zaciski podłączeniowe: max 3x4mm², możliwość podłączenia oprawy w pętle max 3x2,5mm². Przewód w oponie okrągłej o średnicy max ø12,5 mm.","1001XX0009.png","1001XX0009.ldt",1,null,1,76]
["1002","1002XX0009","TRYSIL 263CM 4XLED 6256LM DOWN 3000K DALI","Trysil","Post","Aluminium",null,null,null,"LED zintegrowane","AC","DALI","34,8W","40W","6256lm","3901lm",null,null,"65","IK10","Class I",3000,"szerokie dół",1.18,0.24,2.63,"CE",null,"DALI","> 102 000h",23,"Oprawa słupowa.","Światło rozproszone półsferyczne ukierunkowane w dół",null,"Luminaire with a contemporary design. For lighting gardens, private areas, and other architectural concepts",null,null,null,"Profil aluminiowy wyciskany, malowany proszkowo.",null,"Klosz- poliwęglan przeźroczysty ze strukturą, stabilizowany UV.","Uszczelka silikonowa.",null,"263cm","Podwójna","Sterowanie światłem w systemie: DALI2","4 Moduły LED","Cree DK200305 V3 JB2835 3V 3K","TCI Mini JOLLY 20W code 151403 DALI",0,null,null,80,"C","3091GA0009","Zaciski podłączeniowe: max 5x4mm², możliwość podłączenia oprawy w pętle max 5x2,5mm². Przewód w oponie okrągłej o średnicy max ø13,6mm.","1002XX0009.png","1002XX0009.ldt",3,null,1,76]
["1003","1003XX0009","TRYSIL 263CM 4XLED 6648LM DOWN 4000K DALI","Trysil","Post","Aluminium",null,null,null,"LED zintegrowane","AC","DALI","34,8W","40W","6648lm","4145lm",null,null,"65","IK10",null,4000,"szerokie dół",1.18,0.24,2.63,"CE",null,"DALI","> 102000h",23,"Oprawa słupowa.","Światło rozproszone półsferyczne ukierunkowane w dół",null,"Luminaire with a contemporary design. For lighting gardens, private areas, and other architectural concepts",null,null,null,"Profil aluminiowy wyciskany, malowany proszkowo.",null,"Klosz- poliwęglan przeźroczysty ze strukturą, stabilizowany UV.","Uszczelka silikonowa.",null,"263cm","Podwójna","Sterowanie światłem w systemie: DALI2","4 Moduły LED","Cree DK200305 V3 JB2835 3V 4K","TCI Mini JOLLY 20W code 151403 DALI",0,null,null,80,"C","3091GA0009","Zaciski podłączeniowe: max 5x4mm², możliwość podłączenia oprawy w pętle max 5x2,5mm². Przewód w oponie okrągłej o średnicy max ø13,6mm.","1003XX0009.png","1003XX0009.ldt",3,null,1,76]
["1006","1006XX0009","TRYSIL 263CM 2XLED 2317LM VSM 3000K DALI2","Trysil","Pole","Aluminium",null,null,"PRO","LED zintegrowane","AC","DALI2","13W","16,3W","2317lm","2282lm",null,null,"65","IK10","Class I",3000,"szerokie dół",1.18,0.24,2.63,"CE",null,"DALI","> 100 000h",23,"Oprawa słupowa.","Soczewka firmy Ledil typu VSM (IESNA typ V).","VSM","Luminaire with a contemporary design. For lighting gardens, private areas, and other architectural concepts",null,null,null,"Profil aluminiowy wyciskany, malowany proszkowo.",null,"Klosz- poliwęglan przeźroczysty, stabilizowany UV.",null,null,"263cm","Podwójna","Sterowanie światłem w systemie: DALI outdoor pełny program. Zasilacz zaprogramowany na max prąd. Programowanie pozostałych parametrów po uzgodnieniu z Działem Handlowym firmy Norlys.","2 Moduły LED","Philips Fortimo FastFlex LED 2x6 DP G5 3K","Philips Xi FP 40W 0.2-0.7A SNLDAE 230V S175 929002128306",100000,"DALI2 / NightDim (XI FP NLD)",null,70,"D","3091GA0009","Zaciski podłączeniowe: max 5x4mm², możliwość podłączenia oprawy w pętle max 5x2,5mm². Przewód w oponie okrągłej o średnicy max ø13,6mm.","1006XX0009.png","1006XX0009.ldt",3,null,1,47]
["1007","1007XX0009","TRYSIL 263CM 2XLED 2509LM VSM 4000K DALI2","Trysil","Pole","Aluminium",null,null,"PRO","LED zintegrowane","AC","DALI2","13W","16,3W","2509lm","2377lm",null,null,"65",null,"Class I",4000,"szerokie dół",1.18,0.24,2.63,"CE",null,"DALI","> 100 000h",23,"Oprawa słupowa.","Soczewka firmy Ledil typu VSM (IESNA typ V).","VSM","Luminaire with a contemporary design. For lighting gardens, private areas, and other architectural concepts",null,null,null,"Profil aluminiowy wyciskany, malowany proszkowo.",null,"Klosz- poliwęglan przeźroczysty, stabilizowany UV.",null,null,"263cm","Podwójna","Sterowanie światłem w systemie: DALI outdoor pełny program. Zasilacz zaprogramowany na max prąd. Programowanie pozostałych parametrów po uzgodnieniu z Działem Handlowym firmy Norlys.","2 Moduły LED","Philips Fortimo FastFlex LED 2x6 DP G5 4K","Philips Xi FP 40W 0.2-0.7A SNLDAE 230V S175 929002128306",100000,"DALI2 / NightDim (XI FP NLD)",null,70,"D","3091GA0009","Zaciski podłączeniowe: max 5x4mm², możliwość podłączenia oprawy w pętle max 5x2,5mm². Przewód w oponie okrągłej o średnicy max ø13,6mm.","1007XX0009.png","1007XX0009.ldt",3,null,1,47]
["1010","1010XX0009","TRYSIL 263CM 2XLED 2317LM SCL 3000K DALI2","Trysil","Pole","Aluminium",null,null,"PRO","LED zintegrowane","AC","DALI2","13W","16,3W","2317lm","2216lm",null,null,"65","IK10","Class I",3000,"szerokie dół",1.18,0.24,2.63,"CE",null,"DALI","> 100 000h",23,"Oprawa słupowa.","Soczewka firmy Ledil typu SCL (IESNA typ II / III).","SCL","Luminaire with a contemporary design. For lighting gardens, private areas, and other architectural concepts",null,null,null,"Profil aluminiowy wyciskany, malowany proszkowo.",null,"Klosz- poliwęglan przeźroczysty, stabilizowany UV.",null,null,"263cm","Podwójna","Sterowanie światłem w systemie: DALI outdoor pełny program. Zasilacz zaprogramowany na max prąd. Programowanie pozostałych parametrów po uzgodnieniu z Działem Handlowym firmy Norlys.","2 Moduły LED","Philips Fortimo FastFlex LED 2x6 DP G5 3K","Philips Xi FP 40W 0.2-0.7A SNLDAE 230V S175 929002128306",100000,"DALI2 / NightDim (XI FP NLD)",null,70,"D","3091GA0009","Zaciski podłączeniowe: max 5x4mm², możliwość podłączenia oprawy w pętle max 5x2,5mm². Przewód w oponie okrągłej o średnicy max ø13,6 mm.","1010XX0009.png","1010XX0009.ldt",3,null,1,46]
["1011","1011XX0009","TRYSIL 263CM 2XLED 2509LM SCL 4000K DALI2","Trysil","Pole","Aluminium",null,null,"PRO","LED zintegrowane","AC","DALI2","13W","16,3W","2509lm","2293lm",null,null,"65","IK10","Class I",4000,"szerokie dół",1.18,0.24,2.63,"CE",null,"DALI","> 100 000h",23,"Oprawa słupowa.","Soczewka firmy Ledil typu SCL (IESNA typ II / III).","SCL","Luminaire with a contemporary design. For lighting gardens, private areas, and other architectural concepts",null,null,null,"Profil aluminiowy wyciskany, malowany proszkowo.",null,"Klosz- poliwęglan przeźroczysty, stabilizowany UV.",null,null,"263cm","Podwójna","Sterowanie światłem w systemie: DALI outdoor pełny program. Zasilacz zaprogramowany na max prąd. Programowanie pozostałych parametrów po uzgodnieniu z Działem Handlowym firmy Norlys.","2 Moduły LED","Philips Fortimo FastFlex LED 2x6 DP G5 4K","Philips Xi FP 40W 0.2-0.7A SNLDAE 230V S175 929002128306",100000,"DALI2 / NightDim (XI FP NLD)",null,70,"D","3091GA0009","Zaciski podłączeniowe: max 5x4mm², możliwość podłączenia oprawy w pętle max 5x2,5mm². Przewód w oponie okrągłej o średnicy max ø 13,6 mm.","1011XX0009.png","1011XX0009.ldt",3,null,1,46]
["1012","1012XX0009","TRYSIL 300CM 4XLED 5496LM 3000K DIM.","Trysil","Post","Aluminium",null,null,null,"LED zintegrowane","AC","DIM.","30,2W","34W","5496lm","3347lm",null,null,"65","IK10","Class I",3000,"szerokie dół",1.18,0.24,3,"CE",null,null,"> 102 000h",23,"Oprawa słupowa.","Światło rozproszone półsferyczne ukierunkowane w dół",null,"For lighting private areas and other architectural concepts",null,null,null,"Profil aluminiowy wyciskany, malowany proszkowo.",null,"Klosz- poliwęglan przeźroczysty ze strukturą, stabilizowany UV.","Uszczelka silikonowa.",null,"300cm","Podwójna","Oprawa ściemnialna fazowo TRAILING EDGE (TE) - LEADING EDGE (LE)","4 Moduły LED","Cree DK200305 V3 JB2835 3V 3K","TCI Mini JOLLY 20W code 127556 Triac",0,null,null,80,"C","3091GA0009","Zaciski podłączeniowe: max 3x4mm², możliwość podłączenia oprawy w pętle max 3x2,5mm². Przewód w oponie okrągłej o średnicy max ø12,5 mm.","1012XX0009.png","1012XX0009.ldt",1,null,1,76]
["1013","1013XX0009","TRYSIL 300CM 4XLED 5840LM 4000K DIM.","Trysil","Post","Aluminium",null,null,null,"LED zintegrowane","AC","DIM.","30,2W","33W","5840lm","3448lm",null,null,"65","IK10","Class I",4000,"szerokie dół",1.18,0.24,3,"CE",null,null,"> 102 000h",23,"Oprawa słupowa.","Światło rozproszone półsferyczne ukierunkowane w dół",null,"For lighting private areas and other architectural concepts",null,null,null,"Profil aluminiowy wyciskany, malowany proszkowo.",null,"Klosz- poliwęglan przeźroczysty ze strukturą, stabilizowany UV.","Uszczelka silikonowa.",null,"300cm","Podwójna","Oprawa ściemnialna fazowo TRAILING EDGE (TE) - LEADING EDGE (LE)","4 Moduły LED","Cree DK200305 V3 JB2835 3V 4K","TCI Mini JOLLY 20W code 127556 Triac",0,null,null,80,"C","3091GA0009","Zaciski podłączeniowe: max 3x4mm², możliwość podłączenia oprawy w pętle max 3x2,5mm². Przewód w oponie okrągłej o średnicy max ø12,5 mm.","1013XX0009.png","1013XX0009.ldt",1,null,1,76]
["1014","1014XX0009","TRYSIL 300CM 4XLED 6256LM DOWN 3000K DALI","Trysil","Post","Aluminium",null,null,null,"LED zintegrowane","AC","DALI","34,8W","40W","6256lm","3901lm",null,null,"65","IK10","Class I",3000,"szerokie dół",1.18,0.24,3,"CE",null,"DALI","> 102 000h",23,"Oprawa słupowa.","Światło rozproszone półsferyczne ukierunkowane w dół",null,"Luminaire with a contemporary design. For lighting gardens, private areas and other architectural concepts",null,null,null,"Profil aluminiowy wyciskany, malowany proszkowo.",null,"Klosz- poliwęglan przeźroczysty ze strukturą, stabilizowany UV.","Uszczelka silikonowa.",null,"300cm","Podwójna","Sterowanie światłem w systemie: DALI2","4 Moduły LED","Cree DK200305 V3 JB2835 3V 3K","TCI Mini JOLLY 20W code 151403 DALI",0,null,null,80,"C","3091GA0009","Zaciski podłączeniowe: max 5x4mm², możliwość podłączenia oprawy w pętle max 5x2,5mm². Przewód w oponie okrągłej o średnicy max ø13,6mm.","1014XX0009.png","1014XX0009.ldt",3,null,1,76]
["1015","1015XX0009","TRYSIL 300CM 4XLED 6648LM DOWN 4000K DALI","Trysil","Post","Aluminium",null,null,null,"LED zintegrowane","AC","DALI","34,8W","40W","6648lm","4145lm",null,null,"65","IK10","Class I",4000,"szerokie dół",1.18,0.24,3,"CE",null,"DALI","> 102000h",23,"Oprawa słupowa.","Światło rozproszone półsferyczne ukierunkowane w dół",null,"Luminaire with a contemporary design. For lighting gardens, private areas and other architectural concepts",null,null,null,"Profil aluminiowy wyciskany, malowany proszkowo.",null,"Klosz- poliwęglan przeźroczysty ze strukturą, stabilizowany UV.","Uszczelka silikonowa.",null,"300cm","Podwójna","Sterowanie światłem w systemie: DALI2","4 Moduły LED","Cree DK200305 V3 JB2835 3V 4K","TCI Mini JOLLY 20W code 151403 DALI",0,null,null,80,"C","3091GA0009","Zaciski podłączeniowe: max 5x4mm², możliwość podłączenia oprawy w pętle max 5x2,5mm². Przewód w oponie okrągłej o średnicy max ø13,6mm.","1015XX0009.png","1015XX0009.ldt",3,null,1,76]
["1018","1018XX0009","TRYSIL 300CM 2XLED 3382LM VSM 3000K DALI2","Trysil","Pole","Aluminium",null,null,"PRO","LED zintegrowane","AC","DALI2","19,7W","23,3W","3382lm","3277lm",null,null,"65","IK10","Class I",3000,"szerokie dół",1.18,0.24,3,"CE",null,"DALI","> 100 000h",23,"Oprawa słupowa.","Soczewka firmy Ledil typu VSM (IESNA typ V).","VSM","Luminaire with a contemporary design. For lighting gardens, private areas and other architectural concepts",null,null,null,"Profil aluminiowy wyciskany, malowany proszkowo.",null,"Klosz- poliwęglan przeźroczysty, stabilizowany UV.",null,null,"300cm","Podwójna","Sterowanie światłem w systemie: DALI outdoor pełny program. Zasilacz zaprogramowany na max prąd. Programowanie pozostałych parametrów po uzgodnieniu z Działem Handlowym firmy Norlys.","2 Moduły LED","Philips Fortimo FastFlex LED 2x6 DP G5 3K","Philips Xi FP 40W 0.2-0.7A SNLDAE 230V S175 929002128306",100000,"DALI2 / NightDim (XI FP NLD)",null,70,"D","3091GA0009","Zaciski podłączeniowe: max 5x4mm², możliwość podłączenia oprawy w pętle max 5x2,5mm². Przewód w oponie okrągłej o średnicy max ø13,6mm.","1018XX0009.png","1018XX0009.ldt",3,null,1,47]
["1019","1019XX0009","TRYSIL 300CM 2XLED 3663LM VSM 4000K DALI2","Trysil","Pole","Aluminium",null,null,"PRO","LED zintegrowane","AC","DALI2","19,7W","23,3W","3663lm","3425lm",null,null,"65","IK10","Class I",4000,"szerokie dół",1.18,0.24,3,"CE",null,"DALI","> 100 000h",23,"Oprawa słupowa.","Soczewka firmy Ledil typu VSM (IESNA typ V).","VSM","Luminaire with a contemporary design. For lighting gardens, private areas and other architectural concepts",null,null,null,"Profil aluminiowy wyciskany, malowany proszkowo.",null,"Klosz- poliwęglan przeźroczysty, stabilizowany UV.",null,null,"300cm","Podwójna","Sterowanie światłem w systemie: DALI outdoor pełny program. Zasilacz zaprogramowany na max prąd. Programowanie pozostałych parametrów po uzgodnieniu z Działem Handlowym firmy Norlys.","2 Moduły LED","Philips Fortimo FastFlex LED 2x6 DP G5 4K","Philips Xi FP 40W 0.2-0.7A SNLDAE 230V S175 929002128306",100000,"DALI2 / NightDim (XI FP NLD)",null,70,"D","3091GA0009","Zaciski podłączeniowe: max 5x4mm², możliwość podłączenia oprawy w pętle max 5x2,5mm². Przewód w oponie okrągłej o średnicy max ø13,6mm.","1019XX0009.png","1019XX0009.ldt",3,null,1,47]
["1022","1022XX0009","TRYSIL 300CM 2XLED 3382LM SCL 3000K DALI2","Trysil","Pole","Aluminium",null,null,"PRO","LED zintegrowane","AC","DALI2","19,7W","23,3W","3382lm","3194lm",null,null,"65","IK10","Class I",3000,"szerokie dół",1.18,0.24,3,"CE",null,"DALI","> 100 000h",23,"Oprawa słupowa.","Soczewka firmy Ledil typu SCL (IESNA typ II / III).","SCL","Luminaire with a contemporary design. For lighting gardens, private areas and other architectural concepts",null,null,null,"Profil aluminiowy wyciskany, malowany proszkowo.",null,"Klosz- poliwęglan przeźroczysty, stabilizowany UV.",null,null,"300cm","Podwójna","Sterowanie światłem w systemie: DALI outdoor pełny program. Zasilacz zaprogramowany na max prąd. Programowanie pozostałych parametrów po uzgodnieniu z Działem Handlowym firmy Norlys.","2 Moduły LED","Philips Fortimo FastFlex LED 2x6 DP G5 3K","Philips Xi FP 40W 0.2-0.7A SNLDAE 230V S175 929002128306",100000,"DALI2 / NightDim (XI FP NLD)",null,70,"D","3091GA0009","Zaciski podłączeniowe: max 5x4mm², możliwość podłączenia oprawy w pętle max 5x2,5mm². Przewód w oponie okrągłej o średnicy max ø 13,6mm.","1022XX0009.png","1022XX0009.ldt",3,null,1,46]
["1023","1023XX0009","TRYSIL 300CM 2XLED 3663LM SCL 4000K DALI2","Trysil","Pole","Aluminium",null,null,"PRO","LED zintegrowane","AC","DALI2","19,7W","23,3W","3663lm","3308lm",null,null,"65","IK10","Class I",4000,"szerokie dół",1.18,0.24,3,"CE",null,"DALI","> 100 000h",23,"Oprawa słupowa.","Soczewka firmy Ledil typu SCL (IESNA typ II / III).","SCL","Luminaire with a contemporary design. For lighting gardens, private areas and other architectural concepts",null,null,null,"Profil aluminiowy wyciskany, malowany proszkowo.",null,"Klosz- poliwęglan przeźroczysty, stabilizowany UV.",null,null,"300cm","Podwójna","Sterowanie światłem w systemie: DALI outdoor pełny program. Zasilacz zaprogramowany na max prąd. Programowanie pozostałych parametrów po uzgodnieniu z Działem Handlowym firmy Norlys.","2 Moduły LED","Philips Fortimo FastFlex LED 2x6 DP G5 4K","Philips Xi FP 40W 0.2-0.7A SNLDAE 230V S175 929002128306",100000,"DALI2 / NightDim (XI FP NLD)",null,70,"D","3091GA0009","Zaciski podłączeniowe: max 5x4mm², możliwość podłączenia oprawy w pętle max 5x2,5mm². Przewód w oponie okrągłej o średnicy max ø 13,6 mm.","1023XX0009.png","1023XX0009.ldt",3,null,1,46]
["1024","1024XX0009","TRYSIL 350CM 4XLED 5496LM 3000K DIM.","Trysil","Post","Aluminium",null,null,null,"LED zintegrowane","AC","DIM.","30,2W","34W","5496lm","3347lm",null,null,"65","IK10","Class I",3000,"szerokie dół",1.18,0.24,3.5,"CE",null,null,"> 102 000h",23,"Oprawa słupowa.","Światło rozproszone półsferyczne ukierunkowane w dół",null,"For lighting private areas and other architectural concepts",null,null,null,"Profil aluminiowy wyciskany, malowany proszkowo.",null,"Klosz- poliwęglan przeźroczysty ze strukturą, stabilizowany UV.","Uszczelka silikonowa.",null,"350cm","Podwójna","Oprawa ściemnialna fazowo TRAILING EDGE (TE) - LEADING EDGE (LE)","4 Moduły LED","Cree DK200305 V3 JB2835 3V 3K","TCI Mini JOLLY 20W code 127556 Triac",0,null,null,80,"C","3091GA0009","Zaciski podłączeniowe: max 3x4mm², możliwość podłączenia oprawy w pętle max 3x2,5mm². Przewód w oponie okrągłej o średnicy max ø12,5 mm.","1024XX0009.png","1024XX0009.ldt",1,null,1,76]
["1025","1025XX0009","TRYSIL 350CM 4XLED 5840LM 4000K DIM.","Trysil","Post","Aluminium",null,null,null,"LED zintegrowane","AC","DIM.","30,2W","34W","5840lm","3448lm",null,null,"65","IK10","Class I",4000,"szerokie dół",1.18,0.24,3.5,"CE",null,null,"> 102 000h",23,"Oprawa słupowa.","Światło rozproszone półsferyczne ukierunkowane w dół",null,"For lighting private areas and other architectural concepts",null,null,null,"Profil aluminiowy wyciskany, malowany proszkowo.",null,"Klosz- poliwęglan przeźroczysty ze strukturą, stabilizowany UV.","Uszczelka silikonowa.",null,"350cm","Podwójna","Oprawa ściemnialna fazowo TRAILING EDGE (TE) - LEADING EDGE (LE)","4 Moduły LED","Cree DK200305 V3 JB2835 3V 4K","TCI Mini JOLLY 20W code 127556 Triac",0,null,null,80,"C","3091GA0009","Zaciski podłączeniowe: max 3x4mm², możliwość podłączenia oprawy w pętle max 3x2,5mm². Przewód w oponie okrągłej o średnicy max ø12,5 mm.","1025XX0009.png","1025XX0009.ldt",1,null,1,76]
["1026","1026XX0009","TRYSIL 350CM 4XLED 6256LM DOWN 3000K DALI","Trysil","Post","Aluminium",null,null,null,"LED zintegrowane","AC","DALI","34,8W","40W","6256lm","3901lm",null,null,"65","IK10","Class I",3000,"szerokie dół",1.18,0.24,3.5,"CE",null,"DALI","> 102 000h",23,"Oprawa słupowa.","Światło rozproszone półsferyczne ukierunkowane w dół",null,"Luminaire with a contemporary design. For lighting gardens, private areas and other architectural concepts",null,null,null,"Profil aluminiowy wyciskany, malowany proszkowo.",null,"Klosz- poliwęglan przeźroczysty ze strukturą, stabilizowany UV.","Uszczelka silikonowa.",null,"350cm","Podwójna","Sterowanie światłem w systemie: DALI2","4 Moduły LED","Cree DK200305 V3 JB2835 3V 3K","TCI Mini JOLLY 20W code 151403 DALI",0,null,null,80,"C","3091GA0009","Zaciski podłączeniowe: max 5x4mm², możliwość podłączenia oprawy w pętle max 5x2,5mm². Przewód w oponie okrągłej o średnicy max ø13,6mm.","1026XX0009.png","1026XX0009.ldt",3,null,1,76]
["1027","1027XX0009","TRYSIL 350CM 4XLED 6648LM DOWN 4000K DALI","Trysil","Post","Aluminium",null,null,null,"LED zintegrowane","AC","DALI","34,8W","40W","6648lm","4145lm",null,null,"65","IK10","Class I",4000,"szerokie dół",1.18,0.24,3.5,"CE",null,"DALI","> 102000h",23,"Oprawa słupowa.","Światło rozproszone półsferyczne ukierunkowane w dół",null,"Luminaire with a contemporary design. For lighting gardens, private areas and other architectural concepts",null,null,null,"Profil aluminiowy wyciskany, malowany proszkowo.",null,"Klosz- poliwęglan przeźroczysty ze strukturą, stabilizowany UV.","Uszczelka silikonowa.",null,"350cm","Podwójna","Sterowanie światłem w systemie: DALI2","4 Moduły LED","Cree DK200305 V3 JB2835 3V 4K","TCI Mini JOLLY 20W code 151403 DALI",0,null,null,80,"C","3091GA0009","Zaciski podłączeniowe: max 5x4mm², możliwość podłączenia oprawy w pętle max 5x2,5mm². Przewód w oponie okrągłej o średnicy max ø13,6mm.","1027XX0009.png","1027XX0009.ldt",3,null,1,76]
["1030","1030XX0009","TRYSIL 350CM 2XLED 3382LM VSM 3000K DALI2","Trysil","Pole","Aluminium",null,null,"PRO","LED zintegrowane","AC","DALI2","19,7W","23,3W","3382lm","3277lm",null,null,"65","IK10","Class I",3000,"szerokie dół",1.18,0.24,3.5,"CE",null,"DALI","> 100 000h",23,"Oprawa słupowa.","Soczewka firmy Ledil typu VSM (IESNA typ V).","VSM","Luminaire with a contemporary design. For lighting gardens, private areas and other architectural concepts",null,null,null,"Profil aluminiowy wyciskany, malowany proszkowo.",null,"Klosz- poliwęglan przeźroczysty, stabilizowany UV.",null,null,"350cm","Podwójna","Sterowanie światłem w systemie: DALI outdoor pełny program. Zasilacz zaprogramowany na max prąd. Programowanie pozostałych parametrów po uzgodnieniu z Działem Handlowym firmy Norlys.","2 Moduły LED","Philips Fortimo FastFlex LED 2x6 DP G5 3K","Philips Xi FP 40W 0.2-0.7A SNLDAE 230V S175 929002128306",100000,"DALI2 / NightDim (XI FP NLD)",null,70,"D","3091GA0009","Zaciski podłączeniowe: max 5x4mm², możliwość podłączenia oprawy w pętle max 5x2,5mm². Przewód w oponie okrągłej o średnicy max ø13,6mm.","1030XX0009.png","1030XX0009.ldt",3,null,1,47]
["1031","1031XX0009","TRYSIL 350CM 2XLED 3663LM VSM 4000K DALI2","Trysil","Pole","Aluminium",null,null,"PRO","LED zintegrowane","AC","DALI2","19,7W","23,3W","3663lm","3425lm",null,null,"65","IK10","Class I",4000,"szerokie dół",1.18,0.24,3.5,"CE",null,"DALI","> 100 000h",23,"Oprawa słupowa.","Soczewka firmy Ledil typu VSM (IESNA typ V).","VSM","Luminaire with a contemporary design. For lighting gardens, private areas and other architectural concepts",null,null,null,"Profil aluminiowy wyciskany, malowany proszkowo.",null,"Klosz- poliwęglan przeźroczysty, stabilizowany UV.",null,null,"350cm","Podwójna","Sterowanie światłem w systemie: DALI outdoor pełny program. Zasilacz zaprogramowany na max prąd. Programowanie pozostałych parametrów po uzgodnieniu z Działem Handlowym firmy Norlys.","2 Moduły LED","Philips Fortimo FastFlex LED 2x6 DP G5 4K","Philips Xi FP 40W 0.2-0.7A SNLDAE 230V S175 929002128306",100000,"DALI2 / NightDim (XI FP NLD)",null,70,"D","3091GA0009","Zaciski podłączeniowe: max 5x4mm², możliwość podłączenia oprawy w pętle max 5x2,5mm². Przewód w oponie okrągłej o średnicy max ø13,6mm.","1031XX0009.png","1031XX0009.ldt",3,null,1,47]
["1034","1034XX0009","TRYSIL 350CM 2XLED 3382LM SCL 3000K DALI2","Trysil","Pole","Aluminium",null,null,"PRO","LED zintegrowane","AC","DALI2","19,7W","23,3W","3382lm","3194lm",null,null,"65","IK10","Class I",3000,"szerokie dół",1.18,0.24,3.5,"CE",null,"DALI","> 100 000h",23,"Oprawa słupowa.","Soczewka firmy Ledil typu SCL (IESNA typ II / III).","SCL","Luminaire with a contemporary design. For lighting gardens, private areas and other architectural concepts",null,null,null,"Profil aluminiowy wyciskany, malowany proszkowo.",null,"Klosz- poliwęglan przeźroczysty, stabilizowany UV.",null,null,"350cm","Podwójna","Sterowanie światłem w systemie: DALI outdoor pełny program. Zasilacz zaprogramowany na max prąd. Programowanie pozostałych parametrów po uzgodnieniu z Działem Handlowym firmy Norlys.","2 Moduły LED","Philips Fortimo FastFlex LED 2x6 DP G5 3K","Philips Xi FP 40W 0.2-0.7A SNLDAE 230V S175 929002128306",100000,"DALI2 / NightDim (XI FP NLD)",null,70,"D","3091GA0009","Zaciski podłączeniowe: max 5x4mm², możliwość podłączenia oprawy w pętle max 5x2,5mm². Przewód w oponie okrągłej o średnicy max ø 13,6mm.","1034XX0009.png","1034XX0009.ldt",3,null,1,46]
["1035","1035XX0009","TRYSIL 350CM 2XLED 3663LM SCL 4000K DALI2","Trysil","Pole","Aluminium",null,null,"PRO","LED zintegrowane","AC","DALI2","19,7W","23,3W","3663lm","3308lm",null,null,"65","IK10","Class I",4000,"szerokie dół",1.18,0.24,3.5,"CE",null,"DALI","> 100 000h",23,"Oprawa słupowa.","Soczewka firmy Ledil typu SCL (IESNA typ II / III).","SCL","Luminaire with a contemporary design. For lighting gardens, private areas and other architectural concepts",null,null,null,"Profil aluminiowy wyciskany, malowany proszkowo.",null,"Klosz- poliwęglan przeźroczysty, stabilizowany UV.",null,null,"350cm","Podwójna","Sterowanie światłem w systemie: DALI outdoor pełny program. Zasilacz zaprogramowany na max prąd. Programowanie pozostałych parametrów po uzgodnieniu z Działem Handlowym firmy Norlys.","2 Moduły LED","Philips Fortimo FastFlex LED 2x6 DP G5 4K","Philips Xi FP 40W 0.2-0.7A SNLDAE 230V S175 929002128306",100000,"DALI2 / NightDim (XI FP NLD)",null,70,"D","3091GA0009","Zaciski podłączeniowe: max 5x4mm², możliwość podłączenia oprawy w pętle max 5x2,5mm². Przewód w oponie okrągłej o średnicy max ø 13,6 mm.","1035XX0009.png","1035XX0009.ldt",3,null,1,46]
["1036","1036XX0009","TRYSIL 400CM 4XLED 5496LM DOWN 3000K DIM.","Trysil","Post","Aluminium",null,null,null,"LED zintegrowane","AC","DIM.","30,2W","34W","5496lm","3347lm",null,null,"65","IK10","Class I",3000,"szerokie dół",1.18,0.24,4,"CE",null,null,"> 102 000h",23,"Oprawa słupowa.","Światło rozproszone półsferyczne ukierunkowane w dół",null,"For lighting private areas and other architectural concepts",null,null,null,"Profil aluminiowy wyciskany, malowany proszkowo.",null,"Klosz- poliwęglan przeźroczysty ze strukturą, stabilizowany UV.","Uszczelka silikonowa.",null,"400cm","Podwójna","Oprawa ściemnialna fazowo TRAILING EDGE (TE) - LEADING EDGE (LE)","4 Moduły LED","Cree DK200305 V3 JB2835 3V 3K","TCI Mini JOLLY 20W code 127556 Triac",0,null,null,80,"C","3091GA0009","Zaciski podłączeniowe: max 3x4mm², możliwość podłączenia oprawy w pętle max 3x2,5mm². Przewód w oponie okrągłej o średnicy max ø12,5 mm.","1036XX0009.png","1036XX0009.ldt",1,null,1,76]
["1037","1037XX0009","TRYSIL 400CM 4XLED 5840LM 4000K DIM.","Trysil","Post","Aluminium",null,null,null,"LED zintegrowane","AC","DIM.","30,2W","34W","5840lm","3448lm",null,null,"65","IK10","Class I",4000,"szerokie dół",1.18,0.24,4,"CE",null,null,"> 102 000h",23,"Oprawa słupowa.","Światło rozproszone półsferyczne ukierunkowane w dół",null,"For lighting private areas and other architectural concepts",null,null,null,"Profil aluminiowy wyciskany, malowany proszkowo.",null,"Klosz- poliwęglan przeźroczysty ze strukturą, stabilizowany UV.","Uszczelka silikonowa.",null,"400cm","Podwójna","Oprawa ściemnialna fazowo TRAILING EDGE (TE) - LEADING EDGE (LE)","4 Moduły LED","Cree DK200305 V3 JB2835 3V 4K","TCI Mini JOLLY 20W code 127556 Triac",0,null,null,80,"C","3091GA0009","Zaciski podłączeniowe: max 3x4mm², możliwość podłączenia oprawy w pętle max 3x2,5mm². Przewód w oponie okrągłej o średnicy max ø12,5 mm.","1037XX0009.png","1037XX0009.ldt",1,null,1,76]
["1038","1038XX0009","TRYSIL 400CM 4XLED 6256LM DOWN 3000K DALI","Trysil","Post","Aluminium",null,null,null,"LED zintegrowane","AC","DALI","34,8W","40W","6256lm","3901lm",null,null,"65","IK10","Class I",3000,"szerokie dół",1.18,0.24,4,"CE",null,"DALI","> 102 000h",23,"Oprawa słupowa.","Światło rozproszone półsferyczne ukierunkowane w dół",null,"Luminaire with a contemporary design. For lighting gardens, private areas and other architectural concepts",null,null,null,"Profil aluminiowy wyciskany, malowany proszkowo.",null,"Klosz- poliwęglan przeźroczysty ze strukturą, stabilizowany UV.","Uszczelka silikonowa.",null,"400cm","Podwójna","Sterowanie światłem w systemie: DALI2","4 Moduły LED","Cree DK200305 V3 JB2835 3V 3K","TCI Mini JOLLY 20W code 151403 DALI",0,null,null,80,"C","3091GA0009","Zaciski podłączeniowe: max 5x4mm², możliwość podłączenia oprawy w pętle max 5x2,5mm². Przewód w oponie okrągłej o średnicy max ø13,6mm.","1038XX0009.png","1038XX0009.ldt",3,null,1,76]
["1039","1039XX0009","TRYSIL 400CM 4XLED 6648LM DOWN 4000K DALI","Trysil","Post","Aluminium",null,null,null,"LED zintegrowane","AC","DALI","34,8W","40W","6648lm","4145lm",null,null,"65","IK10","Class I",4000,"szerokie dół",1.18,0.24,4,"CE",null,"DALI","> 102000h",23,"Oprawa słupowa.","Światło rozproszone półsferyczne ukierunkowane w dół",null,"Luminaire with a contemporary design. For lighting gardens, private areas and other architectural concepts",null,null,null,"Profil aluminiowy wyciskany, malowany proszkowo.",null,"Klosz- poliwęglan przeźroczysty ze strukturą, stabilizowany UV.","Uszczelka silikonowa.",null,"400cm","Podwójna","Sterowanie światłem w systemie: DALI2","4 Moduły LED","Cree DK200305 V3 JB2835 3V 4K","TCI Mini JOLLY 20W code 151403 DALI",0,null,null,80,"C","3091GA0009","Zaciski podłączeniowe: max 5x4mm², możliwość podłączenia oprawy w pętle max 5x2,5mm². Przewód w oponie okrągłej o średnicy max ø13,6mm.","1039XX0009.png","1039XX0009.ldt",3,null,1,76]
["1042","1042XX0009","TRYSIL 400CM 2XLED 3382LM VSM 3000K DALI2","Trysil","Pole","Aluminium",null,null,"PRO","LED zintegrowane","AC","DALI2","19,7W","23,3W","3382lm","3277lm",null,null,"65","IK10","Class I",3000,"szerokie dół",1.18,0.24,4,"CE",null,"DALI","> 100 000h",23,"Oprawa słupowa.","Soczewka firmy Ledil typu VSM (IESNA typ V).","VSM","Luminaire with a contemporary design. For lighting gardens, private areas and other architectural concepts",null,null,null,"Profil aluminiowy wyciskany, malowany proszkowo.",null,"Klosz- poliwęglan przeźroczysty, stabilizowany UV.",null,null,"400cm","Podwójna","Sterowanie światłem w systemie: DALI outdoor pełny program. Zasilacz zaprogramowany na max prąd. Programowanie pozostałych parametrów po uzgodnieniu z Działem Handlowym firmy Norlys.","2 Moduły LED","Philips Fortimo FastFlex LED 2x6 DP G5 3K","Philips Xi FP 40W 0.2-0.7A SNLDAE 230V S175 929002128306",100000,"DALI2 / NightDim (XI FP NLD)",null,70,"D","3091GA0009","Zaciski podłączeniowe: max 5x4mm², możliwość podłączenia oprawy w pętle max 5x2,5mm². Przewód w oponie okrągłej o średnicy max ø13,6mm.","1042XX0009.png","1042XX0009.ldt",3,null,1,47]
["1043","1043XX0009","TRYSIL 400CM 2XLED 3663LM VSM 4000K DALI2","Trysil","Pole","Aluminium",null,null,"PRO","LED zintegrowane","AC","DALI2","19,7W","23,3W","3663lm","3425lm",null,null,"65","IK10","Class I",4000,"szerokie dół",1.18,0.24,4,"CE",null,"DALI","> 100 000h",23,"Oprawa słupowa.","Soczewka firmy Ledil typu VSM (IESNA typ V).","VSM","Luminaire with a contemporary design. For lighting gardens, private areas and other architectural concepts",null,null,null,"Profil aluminiowy wyciskany, malowany proszkowo.",null,"Klosz- poliwęglan przeźroczysty, stabilizowany UV.",null,null,"400cm","Podwójna","Sterowanie światłem w systemie: DALI outdoor pełny program. Zasilacz zaprogramowany na max prąd. Programowanie pozostałych parametrów po uzgodnieniu z Działem Handlowym firmy Norlys.","2 Moduły LED","Philips Fortimo FastFlex LED 2x6 DP G5 4K","Philips Xi FP 40W 0.2-0.7A SNLDAE 230V S175 929002128306",100000,"DALI2 / NightDim (XI FP NLD)",null,70,"D","3091GA0009","Zaciski podłączeniowe: max 5x4mm², możliwość podłączenia oprawy w pętle max 5x2,5mm². Przewód w oponie okrągłej o średnicy max ø13,6mm.","1043XX0009.png","1043XX0009.ldt",3,null,1,47]
["1046","1046XX0009","TRYSIL 400CM 2XLED 3382LM SCL 3000K DALI2","Trysil","Pole","Aluminium",null,null,"PRO","LED zintegrowane","AC","DALI2","19,7W","23,3W","3382lm","3194lm",null,null,"65","IK10","Class I",3000,"szerokie dół",1.18,0.24,4,"CE",null,"DALI","> 100 000h",23,"Oprawa słupowa.","Soczewka firmy Ledil typu SCL (IESNA typ II / III).","SCL","Luminaire with a contemporary design. For lighting gardens, private areas and other architectural concepts",null,null,null,"Profil aluminiowy wyciskany, malowany proszkowo.",null,"Klosz- poliwęglan przeźroczysty, stabilizowany UV.",null,null,"400cm","Podwójna","Sterowanie światłem w systemie: DALI outdoor pełny program. Zasilacz zaprogramowany na max prąd. Programowanie pozostałych parametrów po uzgodnieniu z Działem Handlowym firmy Norlys.","2 Moduły LED","Philips Fortimo FastFlex LED 2x6 DP G5 3K","Philips Xi FP 40W 0.2-0.7A SNLDAE 230V S175 929002128306",100000,"DALI2 / NightDim (XI FP NLD)",null,70,"D","3091GA0009","Zaciski podłączeniowe: max 5x4mm², możliwość podłączenia oprawy w pętle max 5x2,5mm². Przewód w oponie okrągłej o średnicy max ø 13,6mm.","1046XX0009.png","1046XX0009.ldt",3,null,1,46]
["1047","1047XX0009","TRYSIL 400CM 2XLED 3663LM SCL 4000K DALI2","Trysil","Pole","Aluminium",null,null,"PRO","LED zintegrowane","AC","DALI2","19,7W","23,3W","3663lm","3308lm",null,null,"65","IK10","Class I",4000,"szerokie dół",1.18,0.24,4,"CE",null,"DALI","> 100 000h",23,"Oprawa słupowa.","Soczewka firmy Ledil typu SCL (IESNA typ II / III).","SCL","Luminaire with a contemporary design. For lighting gardens, private areas and other architectural concepts",null,null,null,"Profil aluminiowy wyciskany, malowany proszkowo.",null,"Klosz- poliwęglan przeźroczysty, stabilizowany UV.",null,null,"400cm","Podwójna","Sterowanie światłem w systemie: DALI outdoor pełny program. Zasilacz zaprogramowany na max prąd. Programowanie pozostałych parametrów po uzgodnieniu z Działem Handlowym firmy Norlys.","2 Moduły LED","Philips Fortimo FastFlex LED 2x6 DP G5 4K","Philips Xi FP 40W 0.2-0.7A SNLDAE 230V S175 929002128306",100000,"DALI2 / NightDim (XI FP NLD)",null,70,"D","3091GA0009","Zaciski podłączeniowe: max 5x4mm², możliwość podłączenia oprawy w pętle max 5x2,5mm². Przewód w oponie okrągłej o średnicy max ø 13,6 mm.","1047XX0009.png","1047XX0009.ldt",3,null,1,46]
["1048","1048XX0009","TRYSIL 263CM 2XLED 1988LM 3000K DIM.","Trysil","Post,Post complete","Aluminium",null,null,null,"LED zintegrowane","AC","DIM.","10,6W","12,5W","1988lm","1260lm",null,null,"65","IK10","Class I",3000,"szerokie dół",0.71,0.24,2.63,"CE",null,null,"> 72 000h",23,"Oprawa słupowa.","Światło jednostronne: symetryczne, ukierunkowane w dół.",null,"For lighting private areas and other architectural concepts",null,null,null,"Profil aluminiowy wyciskany, malowany proszkowo.",null,"Klosz- poliwęglan przeźroczysty ze strukturą, stabilizowany UV.","Uszczelka silikonowa.",null,"263cm","Pojedyncza","Oprawa ściemnialna fazowo TRAILING EDGE (TE) - LEADING EDGE (LE)","2 Moduły LED","Cree DK200305 V3 JB2835 3V 3K","TCI Mini MD 12,5W 250mA code 127036 Triac",0,null,0,80,"C","3091GA0009","Zaciski podłączeniowe: max 3x4mm², możliwość podłączenia oprawy w pętle max 3x2,5mm². Przewód w oponie okrągłej o średnicy max ø12,5 mm.","1048XX0009.png","1048XX0009.ldt",1,null,1,27]
["1049","1049XX0009","TRYSIL 263CM 2XLED 2084LM 4000K DIM.","Trysil","Post,Post complete","Aluminium",null,null,null,"LED zintegrowane","AC","DIM.","10,6W","12,5W","2084lm","1300lm",null,null,"65","IK10","Class I",4000,"szerokie dół",0.71,0.24,2.63,"CE",null,null,"> 72 000h",23,"Oprawa słupowa.","Światło jednostronne: symetryczne, ukierunkowane w dół.",null,"For lighting private areas and other architectural concepts",null,null,null,"Profil aluminiowy wyciskany, malowany proszkowo.",null,"Klosz- poliwęglan przeźroczysty ze strukturą, stabilizowany UV.","Uszczelka silikonowa.",null,"263cm","Pojedyncza","Oprawa ściemnialna fazowo TRAILING EDGE (TE) - LEADING EDGE (LE)","2 Moduły LED","Cree DK200305 V3 JB2835 3V 4K","TCI Mini MD 12,5W 250mA code 127036 Triac",0,null,0,80,"C","3091GA0009","Zaciski podłączeniowe: max 3x4mm², możliwość podłączenia oprawy w pętle max 3x2,5mm². Przewód w oponie okrągłej o średnicy max ø12,5 mm.","1049XX0009.png","1049XX0009.ldt",1,null,1,27]
["1050","1050XX0009","TRYSIL 263CM 2XLED 3128LM DOWN 3000K DALI","Trysil","Post","Aluminium",null,null,null,"LED zintegrowane","AC","DALI","17,4W","20W","3128lm","1973lm",null,null,"65","IK10","Class I",3000,"szerokie dół",0.71,0.24,2.63,"CE",null,"DALI","> 102 000h",23,"Oprawa słupowa.","Światło rozproszone półsferyczne ukierunkowane w dół",null,"For lighting gardens, private areas and other architectural concepts",null,null,null,"Profil aluminiowy wyciskany, malowany proszkowo.",null,"Klosz- poliwęglan przeźroczysty ze strukturą, stabilizowany UV.","Uszczelka silikonowa.",null,"263cm","Pojedyncza","Sterowanie światłem w systemie: DALI2","2 Moduły LED","Cree DK200305 V3 JB2835 3V 3K","TCI Mini JOLLY 20W code 151403 DALI",0,null,null,80,"C","3091GA0009","Zaciski podłączeniowe: max 5x4mm², możliwość podłączenia oprawy w pętle max 5x2,5mm². Przewód w oponie okrągłej o średnicy max ø12,5 mm.","1050XX0009.png","1050XX0009.ldt",3,null,1,76]
["1051","1051XX0009","TRYSIL 263CM 2XLED 3324LM DOWN 4000K DALI","Trysil","Post","Aluminium",null,null,null,"LED zintegrowane","AC","DALI","17,4W","20W","3324lm","2054lm",null,null,"65","IK10","Class I",4000,"szerokie dół",0.71,0.24,2.63,"CE",null,"DALI","> 102 000h",23,"Oprawa słupowa.","Światło rozproszone półsferyczne ukierunkowane w dół",null,null,null,null,null,"Profil aluminiowy wyciskany, malowany proszkowo.",null,"Klosz- poliwęglan przeźroczysty ze strukturą, stabilizowany UV.","Uszczelka silikonowa.",null,"263cm","Pojedyncza","Sterowanie światłem w systemie: DALI2","2 Moduły LED","Cree DK200305 V3 JB2835 3V 4K","TCI Mini JOLLY 20W code 151403 DALI",0,null,null,80,"C","3091GA0009","Zaciski podłączeniowe: max 5x4mm², możliwość podłączenia oprawy w pętle max 5x2,5mm². Przewód w oponie okrągłej o średnicy max ø12,5 mm.","1051XX0009.png","1051XX0009.ldt",3,null,1,76]
["1054","1054XX0009","TRYSIL 263CM LED 1158LM VSM 3000K DALI2","Trysil","Pole","Aluminium",null,null,"PRO","LED zintegrowane","AC","DALI2","6,5W","8,4W","1158lm","1081lm",null,null,"65","IK10","Class I",3000,"szerokie dół",0.71,0.24,2.63,"CE",null,"DALI","> 100 000h",23,"Oprawa słupowa.","Soczewka firmy Ledil typu VSM (IESNA typ V).","VSM","Luminaire with a contemporary design For lighting gardens, private areas and other architectural concepts",null,null,null,"Profil aluminiowy wyciskany, malowany proszkowo.",null,"Klosz- poliwęglan przeźroczysty, stabilizowany UV.",null,null,"263cm","Pojedyncza","Sterowanie światłem w systemie: DALI outdoor pełny program. Zasilacz zaprogramowany na max prąd. Programowanie pozostałych parametrów po uzgodnieniu z Działem Handlowym firmy Norlys.","Moduł LED","Philips Fortimo FastFlex LED 2x6 DP G5 3K","Philips Xi FP 40W 0.2-0.7A SNLDAE 230V S175 929002128306",100000,"DALI2 / NightDim (XI FP NLD)",0,70,"D","3091GA0009","Zaciski podłączeniowe: max 5x4mm², możliwość podłączenia oprawy w pętle max 5x2,5mm². Przewód w oponie okrągłej o średnicy max ø13,6mm.","1054XX0009.png","1054XX0009.ldt",3,null,1,47]
["1055","1055XX0009","TRYSIL 263CM LED 1254LM VSM 4000K DALI2","Trysil","Pole","Aluminium",null,null,"PRO","LED zintegrowane","AC","DALI2","6,5W","8,7W","1254lm","1141lm",null,null,"65","IK10","Class I",4000,"szerokie dół",0.71,0.24,2.63,"CE",null,"DALI","> 100 000h",23,"Oprawa słupowa.","Soczewka firmy Ledil typu VSM (IESNA typ V).","VSM","Luminaire with a contemporary design For lighting gardens, private areas and other architectural concepts",null,null,null,"Profil aluminiowy wyciskany, malowany proszkowo.",null,"Klosz- poliwęglan przeźroczysty, stabilizowany UV.",null,null,"263cm","Pojedyncza","Sterowanie światłem w systemie: DALI outdoor pełny program. Zasilacz zaprogramowany na max prąd. Programowanie pozostałych parametrów po uzgodnieniu z Działem Handlowym firmy Norlys.","Moduł LED","Philips Fortimo FastFlex LED 2x6 DP G5 4K","Philips Xi FP 40W 0.2-0.7A SNLDAE 230V S175 929002128306",100000,"DALI2 / NightDim (XI FP NLD)",0,70,"D","3091GA0009","Zaciski podłączeniowe: max 5x4mm², możliwość podłączenia oprawy w pętle max 5x2,5mm². Przewód w oponie okrągłej o średnicy max ø13,6mm.","1055XX0009.png","1055XX0009.ldt",3,null,1,47]
["1058","1058XX0009","TRYSIL 263CM LED 11585LM SCL 3000K DALI2","Trysil","Pole","Aluminium",null,null,"PRO","LED zintegrowane","AC","DALI2","6,5W","8,6W","1158,5lm","1111lm",null,null,"65","IK10","Class I",3000,"szerokie dół",0.71,0.24,2.63,"CE",null,"DALI","> 100 000h",23,"Oprawa słupowa.","Soczewka firmy Ledil typu SCL (IESNA typ II / III).","SCL","Luminaire with a contemporary design For lighting gardens, private areas and other architectural concepts",null,null,null,"Profil aluminiowy wyciskany, malowany proszkowo.",null,"Klosz- poliwęglan przeźroczysty, stabilizowany UV.",null,null,"263cm","Pojedyncza","Sterowanie światłem w systemie: DALI outdoor pełny program. Zasilacz zaprogramowany na max prąd. Programowanie pozostałych parametrów po uzgodnieniu z Działem Handlowym firmy Norlys.","Moduł LED","Philips Fortimo FastFlex LED 2x6 DP G5 3K","Philips Xi FP 40W 0.2-0.7A SNLDAE 230V S175 929002128306",100000,"DALI2 / NightDim (XI FP NLD)",0,70,"D","3091GA0009","Zaciski podłączeniowe: max 5x4mm², możliwość podłączenia oprawy w pętle max 5x2,5mm². Przewód w oponie okrągłej o średnicy max ø13,6mm.","1058XX0009.png","1058XX0009.ldt",3,null,1,46]
["1059","1059XX0009","TRYSIL 263CM LED 1254LM SCL 4000K DALI2","Trysil","Pole","Aluminium",null,null,"PRO","LED zintegrowane","AC","DALI2","6,5","8,7","1254lm","1161lm",null,null,"65",null,"Class I",4000,"szerokie dół",0.71,0.24,2.63,"CE",null,"DALI","> 100 000h",23,"Oprawa słupowa.","Soczewka firmy Ledil typu SCL (IESNA typ II / III).","SCL","Luminaire with a contemporary design For lighting gardens, private areas and other architectural concepts",null,null,null,"Profil aluminiowy wyciskany, malowany proszkowo.",null,"Klosz- poliwęglan przeźroczysty, stabilizowany UV.",null,null,"263cm","Pojedyncza","Sterowanie światłem w systemie: DALI outdoor pełny program. Zasilacz zaprogramowany na max prąd. Programowanie pozostałych parametrów po uzgodnieniu z Działem Handlowym firmy Norlys.","Moduł LED","Philips Fortimo FastFlex LED 2x6 DP G5 4K","Philips Xi FP 40W 0.2-0.7A SNLDAE 230V S175 929002128306",100000,"DALI2 / NightDim (XI FP NLD)",0,70,"D","3091GA0009","Zaciski podłączeniowe: max 5x4mm², możliwość podłączenia oprawy w pętle max 5x2,5mm². Przewód w oponie okrągłej o średnicy max ø13,6mm.","1059XX0009.png","1059XX0009.ldt",3,null,1,46]
["1060","1060XX0009","TRYSIL 300CM 2XLED 2748LM DOWN 3000K DIM.","Trysil","Post","Aluminium",null,null,null,"LED zintegrowane","AC","DIM.","15,1W","17W","2748lm","1667lm",null,null,"65","IK10","Class I",3000,"szerokie dół",0.71,0.24,3,"CE",null,null,"> 102 000h",23,"Oprawa słupowa.","Światło rozproszone półsferyczne ukierunkowane w dół",null,"For lighting private areas and other architectural concepts",null,null,null,"Profil aluminiowy wyciskany, malowany proszkowo.",null,"Klosz- poliwęglan przeźroczysty ze strukturą, stabilizowany UV.","Uszczelka silikonowa.",null,"300cm","Pojedyncza","Oprawa ściemnialna fazowo TRAILING EDGE (TE) - LEADING EDGE (LE)","2 Moduły LED","Cree DK200305 V3 JB2835 3V 3K","TCI Mini JOLLY 20W code 127556 Triac",0,null,0,80,"C","3091GA0009","Zaciski podłączeniowe: max 3x4mm², możliwość podłączenia oprawy w pętle max 3x2,5mm². Przewód w oponie okrągłej o średnicy max ø12,5 mm.","1060XX0009.png","1060XX0009.ldt",1,null,1,76]
["1061","1061XX0009","TRYSIL 300CM 2XLED 2920LM DOWN 4000K DIM.","Trysil","Post","Aluminium",null,null,null,"LED zintegrowane","AC","DIM.","15,1W","17W","2920lm","1719lm",null,null,"65","IK10","Class I",4000,"szerokie dół",0.71,0.24,3,"CE",null,null,"> 102 000h",23,"Oprawa słupowa.","Światło rozproszone półsferyczne ukierunkowane w dół",null,"For lighting private areas and other architectural concepts",null,null,null,"Profil aluminiowy wyciskany, malowany proszkowo.",null,"Klosz- poliwęglan przeźroczysty ze strukturą, stabilizowany UV.","Uszczelka silikonowa.",null,"300cm","Pojedyncza","Oprawa ściemnialna fazowo TRAILING EDGE (TE) - LEADING EDGE (LE)","2 Moduły LED","Cree DK200305 V3 JB2835 3V 4K","TCI Mini JOLLY 20W code 127556 Triac",0,null,0,80,"C","3091GA0009","Zaciski podłączeniowe: max 3x4mm², możliwość podłączenia oprawy w pętle max 3x2,5mm². Przewód w oponie okrągłej o średnicy max ø12,5 mm.","1061XX0009.png","1061XX0009.ldt",1,null,1,76]
["1062","1062XX0009","TRYSIL 300CM 2XLED 3128LM DOWN 3000K DALI","Trysil","Post","Aluminium",null,null,null,"LED zintegrowane","AC","DALI","17,4W","20W","3128lm","1973lm",null,null,"65","IK10","Class I",3000,"szerokie dół",0.71,0.24,3,"CE",null,"DALI","> 102 000h",23,"Oprawa słupowa.","Światło rozproszone półsferyczne ukierunkowane w dół",null,"For lighting private areas and other architectural concepts",null,null,null,"Profil aluminiowy wyciskany, malowany proszkowo.",null,"Klosz- poliwęglan przeźroczysty ze strukturą, stabilizowany UV.","Uszczelka silikonowa.",null,"300cm","Pojedyncza","Sterowanie światłem w systemie: DALI2","2 Moduły LED","Cree DK200305 V3 JB2835 3V 3K","TCI Mini JOLLY 20W code 151403 DALI",0,null,null,80,"C","3091GA0009","Zaciski podłączeniowe: max 5x4mm², możliwość podłączenia oprawy w pętle max 5x2,5mm². Przewód w oponie okrągłej o średnicy max ø12,5 mm.","1062XX0009.png","1062XX0009.ldt",3,null,1,76]
["1063","1063XX0009","TRYSIL 300CM 2XLED 3324LM DOWN 4000K DALI","Trysil","Post","Aluminium",null,null,null,"LED zintegrowane","AC","DALI","17,4W","20W","3324lm","2054lm",null,null,"65","IK10","Class I",4000,"szerokie dół",0.71,0.24,3,"CE",null,"DALI","> 102 000h",23,"Oprawa słupowa.","Światło rozproszone półsferyczne ukierunkowane w dół",null,"For lighting private areas and other architectural concepts",null,null,null,"Profil aluminiowy wyciskany, malowany proszkowo.",null,"Klosz- poliwęglan przeźroczysty ze strukturą, stabilizowany UV.","Uszczelka silikonowa.",null,"300cm","Pojedyncza","Sterowanie światłem w systemie: DALI2","2 Moduły LED","Cree DK200305 V3 JB2835 3V 4K","TCI Mini JOLLY 20W code 151403 DALI",0,null,null,80,"C","3091GA0009","Zaciski podłączeniowe: max 5x4mm², możliwość podłączenia oprawy w pętle max 5x2,5mm². Przewód w oponie okrągłej o średnicy max ø12,5 mm.","1063XX0009.png","1063XX0009.ldt",3,null,1,76]
["1066","1066XX0009","TRYSIL 300CM LED 1691LM VSM 3000K DALI2","Trysil","Pole","Aluminium",null,null,"PRO","LED zintegrowane","AC","DALI2","9,9W","12,2W","1691lm","1638lm",null,null,"65","IK10","Class I",3000,"szerokie dół",0.71,0.24,3,"CE",null,"DALI","> 100 000h",23,"Oprawa słupowa.","Soczewka firmy Ledil typu VSM (IESNA typ V).","VSM","Luminaire with a contemporary design For lighting gardens, private areas and other architectural concepts",null,null,null,"Profil aluminiowy wyciskany, malowany proszkowo.",null,"Klosz- poliwęglan przeźroczysty, stabilizowany UV.",null,null,"300cm","Pojedyncza","Sterowanie światłem w systemie: DALI outdoor pełny program. Zasilacz zaprogramowany na max prąd. Programowanie pozostałych parametrów po uzgodnieniu z Działem Handlowym firmy Norlys.","Moduł LED","Philips Fortimo FastFlex LED 2x6 DP G5 3K","Philips Xi FP 22W 0,2-0,7A SNLDAE 230V S175 sXt 929002172306",100000,"DALI2 / NightDim (XI FP NLD)",null,70,"D","3091GA0009","Zaciski podłączeniowe: max 5x4mm², możliwość podłączenia oprawy w pętle max 5x2,5mm². Przewód w oponie okrągłej o średnicy max ø13,6mm.","1066XX0009.png","1066XX0009.ldt",3,null,1,47]
["1067","1067XX0009","TRYSIL 300CM LED 1831LM VSM 4000K DALI2","Trysil","Pole","Aluminium",null,null,"PRO","LED zintegrowane","AC","DALI2","9,9W","12,2W","1831lm","1705lm",null,null,"65","IK10","Class I",4000,"szerokie dół",0.71,0.24,3,"CE",null,"DALI","> 100 000h",23,"Oprawa słupowa.","Soczewka firmy Ledil typu VSM (IESNA typ V).","VSM","Luminaire with a contemporary design For lighting gardens, private areas and other architectural concepts",null,null,null,"Profil aluminiowy wyciskany, malowany proszkowo.",null,"Klosz- poliwęglan przeźroczysty, stabilizowany UV.",null,null,"300cm","Pojedyncza","Sterowanie światłem w systemie: DALI outdoor pełny program. Zasilacz zaprogramowany na max prąd. Programowanie pozostałych parametrów po uzgodnieniu z Działem Handlowym firmy Norlys.","Moduł LED","Philips Fortimo FastFlex LED 2x6 DP G5 4K","Philips Xi FP 22W 0,2-0,7A SNLDAE 230V S175 sXt 929002172306",100000,"DALI2 / NightDim (XI FP NLD)",null,70,"D","3091GA0009","Zaciski podłączeniowe: max 5x4mm², możliwość podłączenia oprawy w pętle max 5x2,5mm². Przewód w oponie okrągłej o średnicy max ø13,6mm.","1067XX0009.png","1067XX0009.ldt",3,null,1,47]
["1070","1070XX0009","TRYSIL 300CM LED 1691LM SCL 3000K DALI2","Trysil","Pole","Aluminium",null,null,"PRO","LED zintegrowane","AC","DALI2","9,9W","12,2W","1691lm","1594lm",null,null,"65","IK10","Class I",3000,"szerokie dół",0.71,0.24,3,"CE",null,"DALI","> 100 000h",23,"Oprawa słupowa.","Soczewka firmy Ledil typu SCL (IESNA typ II / III).","SCL","Luminaire with a contemporary design For lighting gardens, private areas and other architectural concepts",null,null,null,"Profil aluminiowy wyciskany, malowany proszkowo.",null,"Klosz- poliwęglan przeźroczysty, stabilizowany UV.",null,null,"300cm","Pojedyncza","Sterowanie światłem w systemie: DALI outdoor pełny program. Zasilacz zaprogramowany na max prąd. Programowanie pozostałych parametrów po uzgodnieniu z Działem Handlowym firmy Norlys.","Moduł LED","Philips Fortimo FastFlex LED 2x6 DP G5 3K","Philips Xi FP 22W 0,2-0,7A SNLDAE 230V S175 sXt 929002172306",100000,"DALI2 / NightDim (XI FP NLD)",null,70,"D","3091GA0009","Zaciski podłączeniowe: max 5x4mm², możliwość podłączenia oprawy w pętle max 5x2,5mm². Przewód w oponie okrągłej o średnicy max ø13,6mm.","1070XX0009.png","1070XX0009.ldt",3,null,1,46]
["1071","1071XX0009","TRYSIL 300CM LED 1831LM SCL 4000K DALI2","Trysil","Pole","Aluminium",null,null,"PRO","LED zintegrowane","AC","DALI2","9,9W","12,2W","1831lm","1667lm",null,null,"65","IK10","Class I",4000,"szerokie dół",0.71,0.24,3,"CE",null,"DALI","> 100 000h",23,"Oprawa słupowa.","Soczewka firmy Ledil typu SCL (IESNA typ II / III).","SCL","Luminaire with a contemporary design For lighting gardens, private areas and other architectural concepts",null,null,null,"Profil aluminiowy wyciskany, malowany proszkowo.",null,"Klosz- poliwęglan przeźroczysty, stabilizowany UV.",null,null,"300cm","Pojedyncza","Sterowanie światłem w systemie: DALI outdoor pełny program. Zasilacz zaprogramowany na max prąd. Programowanie pozostałych parametrów po uzgodnieniu z Działem Handlowym firmy Norlys.","Moduł LED","Philips Fortimo FastFlex LED 2x6 DP G5 4K","Philips Xi FP 22W 0,2-0,7A SNLDAE 230V S175 sXt 929002172306",100000,"DALI2 / NightDim (XI FP NLD)",null,70,"D","3091GA0009","Zaciski podłączeniowe: max 5x4mm², możliwość podłączenia oprawy w pętle max 5x2,5mm². Przewód w oponie okrągłej o średnicy max ø13,6mm.","1071XX0009.png","1071XX0009.ldt",3,null,1,46]
["1072","1072XX0009","TRYSIL 350CM 2XLED 2748LM DOWN 3000K DIM.","Trysil","Post","Aluminium",null,null,null,"LED zintegrowane","AC","DIM.","15,1W","17W","2748lm","1667lm",null,null,"65","IK10","Class I",3000,"szerokie dół",0.71,0.24,3.5,"CE",null,null,"> 102 000h",23,"Oprawa słupowa.","Światło rozproszone półsferyczne ukierunkowane w dół",null,"For lighting private areas and other architectural concepts",null,null,null,"Profil aluminiowy wyciskany, malowany proszkowo.",null,"Klosz- poliwęglan przeźroczysty ze strukturą, stabilizowany UV.","Uszczelka silikonowa.",null,"350cm","Pojedyncza","Oprawa ściemnialna fazowo TRAILING EDGE (TE) - LEADING EDGE (LE)","2 Moduły LED","Cree DK200305 V3 JB2835 3V 3K","TCI Mini JOLLY 20W code 127556 Triac",0,null,0,80,"C","3091GA0009","Zaciski podłączeniowe: max 3x4mm², możliwość podłączenia oprawy w pętle max 3x2,5mm². Przewód w oponie okrągłej o średnicy max ø12,5 mm.","1072XX0009.png","1072XX0009.ldt",1,null,1,76]
["1073","1073XX0009","TRYSIL 350CM 2XLED 2920LM DOWN 4000K DIM.","Trysil","Post","Aluminium",null,null,null,"LED zintegrowane","AC","DIM.","15,1W","17W","2920lm","1719lm",null,null,"65","IK10","Class I",4000,"szerokie dół",0.71,0.24,3.5,"CE",null,null,"> 102 000h",23,"Oprawa słupowa.","Światło rozproszone półsferyczne ukierunkowane w dół",null,"For lighting private areas and other architectural concepts",null,null,null,"Profil aluminiowy wyciskany, malowany proszkowo.",null,"Klosz- poliwęglan przeźroczysty ze strukturą, stabilizowany UV.","Uszczelka silikonowa.",null,"350cm","Pojedyncza","Oprawa ściemnialna fazowo TRAILING EDGE (TE) - LEADING EDGE (LE)","2 Moduły LED","Cree DK200305 V3 JB2835 3V 4K","TCI Mini JOLLY 20W code 127556 Triac",0,null,0,80,"C","3091GA0009","Zaciski podłączeniowe: max 3x4mm², możliwość podłączenia oprawy w pętle max 3x2,5mm². Przewód w oponie okrągłej o średnicy max ø12,5 mm.","1073XX0009.png","1073XX0009.ldt",1,null,1,76]
["1078","1078XX0009","TRYSIL 350CM LED 1691LM VSM 3000K DALI2","Trysil","Pole","Aluminium",null,null,"PRO","LED zintegrowane","AC","DALI2","9,9W","12,2W","1691lm","1638lm",null,null,"65","IK10","Class I",3000,"szerokie dół",0.71,0.24,3.5,"CE",null,"DALI","> 100 000h",23,"Oprawa słupowa.","Soczewka firmy Ledil typu VSM (IESNA typ V).","VSM","Luminaire with a contemporary design For lighting gardens, private areas and other architectural concepts",null,null,null,"Profil aluminiowy wyciskany, malowany proszkowo.",null,"Klosz- poliwęglan przeźroczysty, stabilizowany UV.",null,null,"350cm","Pojedyncza","Sterowanie światłem w systemie: DALI outdoor pełny program. Zasilacz zaprogramowany na max prąd. Programowanie pozostałych parametrów po uzgodnieniu z Działem Handlowym firmy Norlys.","Moduł LED","Philips Fortimo FastFlex LED 2x6 DP G5 3K","Philips Xi FP 22W 0,2-0,7A SNLDAE 230V S175 sXt 929002172306",100000,"DALI2 / NightDim (XI FP NLD)",null,70,"D","3091GA0009","Zaciski podłączeniowe: max 5x4mm², możliwość podłączenia oprawy w pętle max 5x2,5mm². Przewód w oponie okrągłej o średnicy max ø13,6mm.","1078XX0009.png","1078XX0009.ldt",3,null,1,47]
["1079","1079XX0009","TRYSIL 350CM LED 1831LM VSM 4000K DALI2","Trysil","Pole","Aluminium",null,null,"PRO","LED zintegrowane","AC","DALI2","9,9W","12,2W","1831lm","1705lm",null,null,"65","IK10","Class I",4000,"szerokie dół",0.71,0.24,3.5,"CE",null,"DALI","> 100 000h",23,"Oprawa słupowa.","Soczewka firmy Ledil typu VSM (IESNA typ V).","VSM","Luminaire with a contemporary design For lighting gardens, private areas and other architectural concepts",null,null,null,"Profil aluminiowy wyciskany, malowany proszkowo.",null,"Klosz- poliwęglan przeźroczysty, stabilizowany UV.",null,null,"350cm","Pojedyncza","Sterowanie światłem w systemie: DALI outdoor pełny program. Zasilacz zaprogramowany na max prąd. Programowanie pozostałych parametrów po uzgodnieniu z Działem Handlowym firmy Norlys.","Moduł LED","Philips Fortimo FastFlex LED 2x6 DP G5 4K","Philips Xi FP 22W 0,2-0,7A SNLDAE 230V S175 sXt 929002172306",100000,"DALI2 / NightDim (XI FP NLD)",null,70,"D","3091GA0009","Zaciski podłączeniowe: max 5x4mm², możliwość podłączenia oprawy w pętle max 5x2,5mm². Przewód w oponie okrągłej o średnicy max ø13,6mm.","1079XX0009.png","1079XX0009.ldt",3,null,1,47]
["1082","1082XX0009","TRYSIL 350CM LED 1691LM SCL 3000K DALI2","Trysil","Pole","Aluminium",null,null,"PRO","LED zintegrowane","AC","DALI2","9,9W","12,2W","1691lm","1594lm",null,null,"65","IK10","Class I",3000,"szerokie dół",0.71,0.24,3.5,"CE",null,"DALI","> 100 000h",23,"Oprawa słupowa.","Soczewka firmy Ledil typu SCL (IESNA typ II / III).","SCL","Luminaire with a contemporary design For lighting gardens, private areas and other architectural concepts",null,null,null,"Profil aluminiowy wyciskany, malowany proszkowo.",null,"Klosz- poliwęglan przeźroczysty, stabilizowany UV.",null,null,"350cm","Pojedyncza","Sterowanie światłem w systemie: DALI outdoor pełny program. Zasilacz zaprogramowany na max prąd. Programowanie pozostałych parametrów po uzgodnieniu z Działem Handlowym firmy Norlys.","Moduł LED","Philips Fortimo FastFlex LED 2x6 DP G5 3K","Philips Xi FP 22W 0,2-0,7A SNLDAE 230V S175 sXt 929002172306",100000,"DALI2 / NightDim (XI FP NLD)",null,70,"D","3091GA0009","Zaciski podłączeniowe: max 5x4mm², możliwość podłączenia oprawy w pętle max 5x2,5mm². Przewód w oponie okrągłej o średnicy max ø13,6mm.","1082XX0009.png","1082XX0009.ldt",3,null,1,46]
["1083","1083XX0009","TRYSIL 350CM LED 1831LM SCL 4000K DALI2","Trysil","Pole","Aluminium",null,null,"PRO","LED zintegrowane","AC","DALI2","9,9W","12,2W","1831lm","1667lm",null,null,"65","IK10","Class I",4000,"szerokie dół",0.71,0.24,3.5,"CE",null,"DALI","> 100 000h",23,"Oprawa słupowa.","Soczewka firmy Ledil typu SCL (IESNA typ II / III).","SCL","Luminaire with a contemporary design For lighting gardens, private areas and other architectural concepts",null,null,null,"Profil aluminiowy wyciskany, malowany proszkowo.",null,"Klosz- poliwęglan przeźroczysty, stabilizowany UV.",null,null,"350cm","Pojedyncza","Sterowanie światłem w systemie: DALI outdoor pełny program. Zasilacz zaprogramowany na max prąd. Programowanie pozostałych parametrów po uzgodnieniu z Działem Handlowym firmy Norlys.","Moduł LED","Philips Fortimo FastFlex LED 2x6 DP G5 4K","Philips Xi FP 22W 0,2-0,7A SNLDAE 230V S175 sXt 929002172306",100000,"DALI2 / NightDim (XI FP NLD)",null,70,"D","3091GA0009","Zaciski podłączeniowe: max 5x4mm², możliwość podłączenia oprawy w pętle max 5x2,5mm². Przewód w oponie okrągłej o średnicy max ø13,6mm.","1083XX0009.png","1083XX0009.ldt",3,null,1,46]
["1084","1084XX0009","TRYSIL 400CM 2XLED 2748LM DOWN 3000K DIM.","Trysil","Post","Aluminium",null,null,null,"LED zintegrowane","AC","DIM.","15,1W","17W","2748lm","1667lm",null,null,"65","IK10","Class I",3000,"szerokie dół",0.71,0.24,4,"CE",null,null,"> 102 000h",23,"Oprawa słupowa.","Światło rozproszone półsferyczne ukierunkowane w dół",null,"For lighting gardens, private areas and other architectural concepts",null,null,null,"Profil aluminiowy wyciskany, malowany proszkowo.",null,"Klosz- poliwęglan przeźroczysty ze strukturą, stabilizowany UV.","Uszczelka silikonowa.",null,"400cm","Pojedyncza","Oprawa ściemnialna fazowo TRAILING EDGE (TE) - LEADING EDGE (LE)","2 Moduły LED","Cree DK200305 V3 JB2835 3V 3K","TCI Mini JOLLY 20W code 127556 Triac",0,null,0,80,"C","3091GA0009","Zaciski podłączeniowe: max 3x4mm², możliwość podłączenia oprawy w pętle max 3x2,5mm². Przewód w oponie okrągłej o średnicy max ø12,5 mm.","1084XX0009.png","1084XX0009.ldt",1,null,1,76]
["1085","1085XX0009","TRYSIL 400CM 2XLED 2920LM DOWN 4000K DIM.","Trysil","Post","Aluminium",null,null,null,"LED zintegrowane","AC","DIM.","15,1W","17W","2920lm","1719lm",null,null,"65","IK10","Class I",4000,"szerokie dół",0.71,0.24,4,"CE",null,null,"> 102 000h",23,"Oprawa słupowa.","Światło rozproszone półsferyczne ukierunkowane w dół",null,"For lighting gardens, private areas and other architectural concepts",null,null,null,"Profil aluminiowy wyciskany, malowany proszkowo.",null,"Klosz- poliwęglan przeźroczysty ze strukturą, stabilizowany UV.","Uszczelka silikonowa.",null,"400cm","Pojedyncza","Oprawa ściemnialna fazowo TRAILING EDGE (TE) - LEADING EDGE (LE)","2 Moduły LED","Cree DK200305 V3 JB2835 3V 4K","TCI Mini JOLLY 20W code 127556 Triac",0,null,null,80,"C","3091GA0009","Zaciski podłączeniowe: max 3x4mm², możliwość podłączenia oprawy w pętle max 3x2,5mm². Przewód w oponie okrągłej o średnicy max ø12,5 mm.","1085XX0009.png","1085XX0009.ldt",1,null,1,76]
["1086","1086XX0009","TRYSIL 400CM 2XLED 3128LM DOWN 3000K DALI","Trysil","Post","Aluminium",null,null,null,"LED zintegrowane","AC","DALI","17,4W","20W","3128lm","1973lm",null,null,"65","IK10","Class I",3000,"szerokie dół",0.71,0.24,4,"CE",null,"DALI","> 102 000h",23,"Oprawa słupowa.","Światło rozproszone półsferyczne ukierunkowane w dół",null,"For lighting private areas and other architectural concepts",null,null,null,"Profil aluminiowy wyciskany, malowany proszkowo.",null,"Klosz- poliwęglan przeźroczysty ze strukturą, stabilizowany UV.","Uszczelka silikonowa.",null,"400cm","Pojedyncza","Sterowanie światłem w systemie: DALI2","2 Moduły LED","Cree DK200305 V3 JB2835 3V 3K","TCI Mini JOLLY 20W code 151403 DALI",0,null,null,80,"C","3091GA0009","Zaciski podłączeniowe: max 5x4mm², możliwość podłączenia oprawy w pętle max 5x2,5mm². Przewód w oponie okrągłej o średnicy max ø12,5 mm.","1086XX0009.png","1086XX0009.ldt",3,null,1,76]
["1087","1087XX0009","TRYSIL 400CM 2XLED 3324LM DOWN 4000K DALI","Trysil","Post","Aluminium",null,null,null,"LED zintegrowane","AC","DALI","17,4W","20W","3324lm","2054lm",null,null,"65","IK10","Class I",4000,"szerokie dół",0.71,0.24,4,"CE",null,"DALI","> 102 000h",23,"Oprawa słupowa.","Światło rozproszone półsferyczne ukierunkowane w dół",null,"For lighting private areas and other architectural concepts",null,null,null,"Profil aluminiowy wyciskany, malowany proszkowo.",null,"Klosz- poliwęglan przeźroczysty ze strukturą, stabilizowany UV.","Uszczelka silikonowa.",null,"400cm","Pojedyncza","Sterowanie światłem w systemie: DALI2","2 Moduły LED","Cree DK200305 V3 JB2835 3V 4K","TCI Mini JOLLY 20W code 151403 DALI",0,null,null,80,"C","3091GA0009","Zaciski podłączeniowe: max 5x4mm², możliwość podłączenia oprawy w pętle max 5x2,5mm². Przewód w oponie okrągłej o średnicy max ø12,5 mm.","1087XX0009.png","1087XX0009.ldt",3,null,1,76]
["1090","1090XX0009","TRYSIL 400CM LED 1691LM VSM 3000K DALI2","Trysil","Pole","Aluminium",null,null,"PRO","LED zintegrowane","AC","DALI2","9,9W","12,2W","1691lm","1638lm",null,null,"65","IK10","Class I",3000,"szerokie dół",0.71,0.24,4,"CE",null,"DALI","> 100 000h",23,"Oprawa słupowa.","Soczewka firmy Ledil typu VSM (IESNA typ V).","VSM","Luminaire with a contemporary design For lighting gardens, private areas and other architectural concepts",null,null,null,"Profil aluminiowy wyciskany, malowany proszkowo.",null,"Klosz- poliwęglan przeźroczysty, stabilizowany UV.",null,null,"400cm","Pojedyncza","Sterowanie światłem w systemie: DALI outdoor pełny program. Zasilacz zaprogramowany na max prąd. Programowanie pozostałych parametrów po uzgodnieniu z Działem Handlowym firmy Norlys.","Moduł LED","Philips Fortimo FastFlex LED 2x6 DP G5 3K","Philips Xi FP 22W 0,2-0,7A SNLDAE 230V S175 sXt 929002172306",100000,"DALI2 / NightDim (XI FP NLD)",null,70,"D","3091GA0009","Zaciski podłączeniowe: max 5x4mm², możliwość podłączenia oprawy w pętle max 5x2,5mm². Przewód w oponie okrągłej o średnicy max ø13,6mm.","1090XX0009.png","1090XX0009.ldt",3,null,1,47]
["1091","1091XX0009","TRYSIL 400CM LED 1831LM VSM 4000K DALI2","Trysil","Pole","Aluminium",null,null,"PRO","LED zintegrowane","AC","DALI2","9,9W","12,2W","1831lm","1705lm",null,null,"65","IK10","Class I",4000,"szerokie dół",0.71,0.24,4,"CE",null,"DALI",null,23,"Oprawa słupowa.","Soczewka firmy Ledil typu VSM (IESNA typ V).","VSM","Luminaire with a contemporary design For lighting gardens, private areas and other architectural concepts",null,null,null,"Profil aluminiowy wyciskany, malowany proszkowo.",null,"Klosz- poliwęglan przeźroczysty, stabilizowany UV.",null,null,"400cm","Pojedyncza","Sterowanie światłem w systemie: DALI outdoor pełny program. Zasilacz zaprogramowany na max prąd. Programowanie pozostałych parametrów po uzgodnieniu z Działem Handlowym firmy Norlys.","Moduł LED","Philips Fortimo FastFlex LED 2x6 DP G5 4K","Philips Xi FP 22W 0,2-0,7A SNLDAE 230V S175 sXt 929002172306",100000,"DALI2 / NightDim (XI FP NLD)",0,70,"D","3091GA0009","Zaciski podłączeniowe: max 5x4mm², możliwość podłączenia oprawy w pętle max 5x2,5mm². Przewód w oponie okrągłej o średnicy max ø13,6mm.","1091XX0009.png","1091XX0009.ldt",3,null,1,47]
["1094","1094XX0009","TRYSIL 400CM LED 1691LM SCL 3000K DALI2","Trysil","Pole","Aluminium",null,null,"PRO","LED zintegrowane","AC","DALI2","9,9W","12,2W","1691lm","1594lm",null,null,"65","IK10","Class I",3000,"szerokie dół",0.71,0.24,4,"CE",null,"DALI","> 100 000h",23,"Oprawa słupowa.","Soczewka firmy Ledil typu SCL (IESNA typ II / III).","SCL","Luminaire with a contemporary design For lighting gardens, private areas and other architectural concepts",null,null,null,"Profil aluminiowy wyciskany, malowany proszkowo.",null,"Klosz- poliwęglan przeźroczysty, stabilizowany UV.",null,null,"400cm","Pojedyncza","Sterowanie światłem w systemie: DALI outdoor pełny program. Zasilacz zaprogramowany na max prąd. Programowanie pozostałych parametrów po uzgodnieniu z Działem Handlowym firmy Norlys.","Moduł LED","Philips Fortimo FastFlex LED 2x6 DP G5 3K","Philips Xi FP 22W 0,2-0,7A SNLDAE 230V S175 sXt 929002172306",100000,"DALI2 / NightDim (XI FP NLD)",0,70,"D","3091GA0009","Zaciski podłączeniowe: max 5x4mm², możliwość podłączenia oprawy w pętle max 5x2,5mm². Przewód w oponie okrągłej o średnicy max ø13,6mm.","1094XX0009.png","1094XX0009.ldt",3,null,1,46]
["1095","1095XX0009","TRYSIL 400CM LED 1831LM SCL 4000K DALI2","Trysil","Pole","Aluminium",null,null,"PRO","LED zintegrowane","AC","DALI2","9,9W","12,2W","1831lm","1667lm",null,null,"65","IK10","Class I",4000,"szerokie dół",0.71,0.24,4,"CE",null,"DALI","> 100 000h",23,"Oprawa słupowa.","Soczewka firmy Ledil typu SCL (IESNA typ II / III).","SCL","Luminaire with a contemporary design For lighting gardens, private areas and other architectural concepts",null,null,null,"Profil aluminiowy wyciskany, malowany proszkowo.",null,"Klosz- poliwęglan przeźroczysty, stabilizowany UV.",null,null,"400cm","Pojedyncza","Sterowanie światłem w systemie: DALI outdoor pełny program. Zasilacz zaprogramowany na max prąd. Programowanie pozostałych parametrów po uzgodnieniu z Działem Handlowym firmy Norlys.","Moduł LED","Philips Fortimo FastFlex LED 2x6 DP G5 4K","Philips Xi FP 22W 0,2-0,7A SNLDAE 230V S175 sXt 929002172306",100000,"DALI2 / NightDim (XI FP NLD)",0,70,"D","3091GA0009","Zaciski podłączeniowe: max 5x4mm², możliwość podłączenia oprawy w pętle max 5x2,5mm². Przewód w oponie okrągłej o średnicy max ø13,6mm.","1095XX0009.png","1095XX0009.ldt",3,null,1,46]
["1096","1096XX0009","TRYSIL BOLLARD 85CM 2XLED 1010LM 3000K DIM.","Trysil","Bollard","Aluminium",null,null,"PRO","LED zintegrowane","AC","DIM.","5,6W","7,3W","1010lm","620lm",null,null,"65","IK10",null,3000,"szerokie dół",0.34,0.11,0.85,"CE",null,null,">102 000h",1,"Oprawa słupkowa.","Światło ukierunkowane w dół.",null,"Luminaire with a contemporary design For lighting gardens, private areas and other architectural concepts",null,null,null,"Profil aluminiowy wyciskany, malowany proszkowo.",null,"Klosz- poliwęglan przeźroczysty ze strukturą, stabilizowany UV.","Uszczelka silikonowa.",null,"85cm",null,"Oprawa ściemnialna fazowo TRAILING EDGE (TE)","2 Moduły LED","Cree DK180501 V8 JB2835 3V 3K","Philips Xitanium 7W 0,35A 20V TE SC 230V [2019]",50000,"Philips Xitanium TE",0,80,"C","1907ZX0009, 1908GA0009, 1909GA0009, 3081XX0009","Zaciski podłączeniowe: max 3x2,5mm², możliwość podłączenia oprawy w pętle max 3x1,5mm². Przewód w oponie okrągłej o średnicy max ø12,5mm.","1096XX0009.png","1096XX0009.ldt",1,null,1,45]
["1097","1097XX0009","TRYSIL BOLLARD 85CM 2XLED 1069LM 4000K DIM.","Trysil","Bollard","Aluminium",null,null,"PRO","LED zintegrowane","AC","DIM.","5,6W","7,3W","1069lm","647lm",null,null,"65","IK10",null,4000,"szerokie dół",0.34,0.11,0.85,"CE",null,null,">171 460h",1,"Oprawa słupkowa.","Światło ukierunkowane w dół.",null,"Luminaire with a contemporary design For lighting gardens, private areas and other architectural concepts",null,null,null,"Odlew aluminiowy malowany proszkowo.",null,"Klosz- poliwęglan przeźroczysty ze strukturą, stabilizowany UV.","Uszczelka silikonowa.",null,"85cm",null,"Oprawa ściemnialna fazowo TRAILING EDGE (TE)","2 Moduły LED","Cree DK180501 V8 JB2835 3V 4K","Philips Xitanium 7W 0,35A 20V TE SC 230V [2019]",50000,"Philips Xitanium TE",0,80,"C","1907ZX0009, 1908GA0009, 1909GA0009, 3081XX0009","Zaciski podłączeniowe: max 3x2,5mm², możliwość podłączenia oprawy w pętle max 3x1,5mm². Przewód w oponie okrągłej o średnicy max ø12,5mm.","1097XX0009.png","1097XX0009.ldt",1,null,1,45]
["1100","1100XX0009","TRYSIL BOLLARD 85CM LED 828LM VSM 3000K DIM.","Trysil","Bollard","Aluminium",null,null,"PRO","LED zintegrowane","AC","DIM.","5,8W","7,4W","828lm","703lm",null,null,"65","IK08","Class I",3000,"szerokie dół",0.34,0.11,0.85,"CE",null,null,"> 109 000h",1,"Oprawa słupkowa.","Soczewka firmy Ledil typu VSM (IESNA typ V).","VSM","Luminaire with a contemporary design For lighting gardens, private areas and other architectural concepts",null,null,null,"Profil aluminiowy wyciskany, malowany proszkowo.",null,"Soczewka hermetyczna zewnętrzna- tworzywo sztuczne PMMA przeźroczyste.","Uszczelka silikonowa.",null,"85cm",null,"Oprawa ściemnialna fazowo TRAILING EDGE (TE)","Moduł LED","Cree DK200402 V1 XTE-HE 3K","Philips Xitanium 10W 0,5A 20V TE SC 230V",0,"Philips Xitanium TE",0,80,"E","1907ZX0009, 1908GA0009, 1909GA0009, 3081XX0009","Zaciski podłączeniowe: max 3x2,5mm², możliwość podłączenia oprawy w pętle max 3x1,5mm². Przewód w oponie okrągłej o średnicy max ø12,5mm.","1100XX0009.png","1100XX0009.ldt",1,null,1,47]
["1101","1101XX0009","TRYSIL BOLLARD 85CM LED 828LM VSM 4000K DIM.","Trysil","Bollard","Aluminium",null,null,"PRO","LED zintegrowane","AC","DIM.","5,8W","7,4W","828lm","694,8lm",null,null,"65","IK08","Class I",4000,"szerokie dół",0.34,0.11,0.85,"CE",null,null,"> 109 000h",1,"Oprawa słupkowa.","Soczewka firmy Ledil typu VSM (IESNA typ V).","VSM","Luminaire with a contemporary design For lighting gardens, private areas and other architectural concepts",null,null,null,"Profil aluminiowy wyciskany, malowany proszkowo.",null,"Soczewka hermetyczna zewnętrzna- tworzywo sztuczne PMMA przeźroczyste.","Uszczelka silikonowa.",null,"85cm",null,"Oprawa ściemnialna fazowo TRAILING EDGE (TE)","Moduł LED","Cree DK200402 V1 XTE-HE 3V 4K.","Philips Xitanium 10W 0,5A 20V TE SC 230V",0,"Philips Xitanium TE",0,80,"E","1907ZX0009, 1908GA0009, 1909GA0009, 3081XX0009","Zaciski podłączeniowe: max 3x2,5mm², możliwość podłączenia oprawy w pętle max 3x1,5mm². Przewód w oponie okrągłej o średnicy max ø12,5mm.","1101XX0009.png","1101XX0009.ldt",1,null,1,47]
["1102","1102XX0009","TRYSIL BOLLARD 85CM LED 828LM VSM 3000K DALI2","Trysil","Bollard","Aluminium",null,null,"PRO","LED zintegrowane","AC","DALI2","5,8W","8W","828lm","689lm",null,null,"65","IK08","Class I",3000,"szerokie dół",0.34,0.11,0.85,"CE",null,"DALI",">109 000h",1,"Oprawa słupkowa.","Soczewka firmy Ledil typu VSM (IESNA typ V).","VSM","Luminaire with a contemporary design For lighting gardens, private areas and other architectural concepts",null,null,null,"Profil aluminiowy wyciskany, malowany proszkowo.",null,"Soczewka hermetyczna zewnętrzna- tworzywo sztuczne PMMA przeźroczyste.","Uszczelka silikonowa.",null,"85cm",null,"Sterowanie światłem w systemie: DALI/TD.","Moduł LED","Cree DK200402 V1 XTE-HE 3K","Osram OTi DALI 15/220…240/1A0 LT2 NFC",100000,null,0,80,"E","1907ZX0009, 1908GA0009, 1909GA0009, 3081XX0009","Zaciski podłączeniowe: max 5x2,5mm², możliwość podłączenia oprawy w pętle max 5x1,5mm². Przewód w oponie okrągłej o średnicy max ø12,5mm.","1102XX0009.png","1102XX0009.ldt",3,null,1,47]
["1103","1103XX0009","TRYSIL BOLLARD 85CM LED 828LM VSM 4000K DALI2","Trysil","Bollard","Aluminium",null,null,"PRO","LED zintegrowane","AC","DALI2","5,8W","8W","828lm","674lm",null,null,"65","IK08","Class I",4000,"szerokie dół",0.34,0.11,0.85,"CE",null,"DALI",">109 000h",1,"Oprawa słupkowa.","Soczewka firmy Ledil typu VSM (IESNA typ V).","VSM","Luminaire with a contemporary design For lighting gardens, private areas and other architectural concepts",null,null,null,"Profil aluminiowy wyciskany, malowany proszkowo.",null,"Soczewka hermetyczna zewnętrzna- tworzywo sztuczne PMMA przeźroczyste.","Uszczelka silikonowa.",null,"85cm",null,"Sterowanie światłem w systemie: DALI/TD.","Moduł LED","Cree DK200402 V1 XTE-HE 3V 4K.","Osram OTi DALI 15/220…240/1A0 LT2 NFC",100000,null,0,80,"E","1907ZX0009, 1908GA0009, 1909GA0009, 3081XX0009","Zaciski podłączeniowe: max 3x2,5mm², możliwość podłączenia oprawy w pętle max 3x1,5mm². Przewód w oponie okrągłej o średnicy max ø12,5mm.","1103XX0009.png","1103XX0009.ldt",3,null,1,47]
["1104","1104XX0009","TRYSIL BOLLARD 85CM LED 828LM SCL 3000K DIM.","Trysil","Bollard","Aluminium",null,null,"PRO","LED zintegrowane","AC","DIM.","5,8W","7,5W","828lm","738lm",null,null,"65","IK08","Class I",3000,"szerokie dół",0.34,0.11,0.85,"CE",null,null,"> 109 000h",1,"Oprawa słupkowa.","Soczewka firmy Ledil typu SCL (IESNA typ II / III).","SCL","Luminaire with a contemporary design For lighting gardens, private areas and other architectural concepts",null,null,null,"Profil aluminiowy wyciskany, malowany proszkowo.",null,"Soczewka hermetyczna zewnętrzna- tworzywo sztuczne PMMA przeźroczyste.","Uszczelka silikonowa.",null,"85cm",null,"Oprawa ściemnialna fazowo TRAILING EDGE (TE)","Moduł LED","Cree DK200402 V1 XTE-HE 3K","Philips Xitanium 10W 0,5A 20V TE SC 230V",0,"Philips Xitanium TE",0,80,"E","1907ZX0009, 1908GA0009, 1909GA0009, 3081XX0009","Zaciski podłączeniowe: max 3x2,5mm², możliwość podłączenia oprawy w pętle max 3x1,5mm². Przewód w oponie okrągłej o średnicy max ø12,5mm.","1104XX0009.png","1104XX0009.ldt",1,null,1,46]
["1105","1105XX0009","TRYSIL BOLLARD 85CM LED 828LM SCL 4000K DIM.","Trysil","Bollard","Aluminium",null,null,"PRO","LED zintegrowane","AC","DIM.","5,8W","7,4W","828lm","706lm",null,null,"65","IK08","Class I",4000,"szerokie dół",0.34,0.11,0.85,"CE",null,null,"> 109 000h",1,"Oprawa słupkowa.","Soczewka firmy Ledil typu SCL (IESNA typ II / III).","SCL","Luminaire with a contemporary design For lighting gardens, private areas and other architectural concepts",null,null,null,"Profil aluminiowy wyciskany, malowany proszkowo.",null,"Soczewka hermetyczna zewnętrzna- tworzywo sztuczne PMMA przeźroczyste.","Uszczelka silikonowa.",null,"85cm",null,"Oprawa ściemnialna fazowo TRAILING EDGE (TE)","Moduł LED","Cree DK200402 V1 XTE-HE 3V 4K.","Philips Xitanium 10W 0,5A 20V TE SC 230V",0,"Philips Xitanium TE",0,80,"E","1907ZX0009, 1908GA0009, 1909GA0009, 3081XX0009","Zaciski podłączeniowe: max 3x2,5mm², możliwość podłączenia oprawy w pętle max 3x1,5mm². Przewód w oponie okrągłej o średnicy max ø12,5mm.","1105XX0009.png","1105XX0009.ldt",1,null,1,46]
["1106","1106XX0009","TRYSIL BOLLARD 85CM LED 828LM SCL 3000K DALI2","Trysil","Bollard","Aluminium",null,null,"PRO","LED zintegrowane","AC","DALI2","5,8W","8W","828lm","707lm",null,null,"65","IK08","Class I",3000,"szerokie dół",0.34,0.11,0.85,"CE",null,"DALI",">109 000h",1,"Oprawa słupkowa.","Soczewka firmy Ledil typu SCL (IESNA typ II / III).","SCL","Luminaire with a contemporary design For lighting gardens, private areas and other architectural concepts",null,null,null,"Profil aluminiowy wyciskany, malowany proszkowo.",null,"Soczewka hermetyczna zewnętrzna- tworzywo sztuczne PMMA przeźroczyste.","Uszczelka silikonowa.",null,"85cm",null,"Sterowanie światłem w systemie: DALI/TD.","Moduł LED","Cree DK200402 V1 XTE-HE 3V 4K.","Osram OTi DALI 15/220…240/1A0 LT2 NFC",100000,null,0,80,"E","1907ZX0009, 1908GA0009, 1909GA0009, 3081XX0009","Zaciski podłączeniowe: max 3x2,5mm², możliwość podłączenia oprawy w pętle max 3x1,5mm². Przewód w oponie okrągłej o średnicy max ø12,5mm.","1106XX0009.png","1106XX0009.ldt",3,null,1,46]
["1107","1107XX0009","TRYSIL BOLLARD 85CM LED 828LM SCL 4000K DALI2","Trysil","Bollard","Aluminium",null,null,"PRO","LED zintegrowane","AC","DALI2","5,8W","8W","828lm","693lm",null,null,"65","IK08","Class I",4000,"szerokie dół",0.34,0.11,0.85,"CE",null,"DALI",">109 000h",1,"Oprawa słupkowa.","Soczewka firmy Ledil typu SCL (IESNA typ II / III).","SCL","Luminaire with a contemporary design For lighting gardens, private areas and other architectural concepts",null,null,null,"Profil aluminiowy wyciskany, malowany proszkowo.",null,"Soczewka hermetyczna zewnętrzna- tworzywo sztuczne PMMA przeźroczyste.","Uszczelka silikonowa.",null,"85cm",null,"Sterowanie światłem w systemie: DALI/TD.","Moduł LED","Cree DK200402 V1 XTE-HE 3V 4K.","Osram OTi DALI 15/220…240/1A0 LT2 NFC",100000,null,0,80,"E","1907ZX0009, 1908GA0009, 1909GA0009, 3081XX0009","Zaciski podłączeniowe: max 3x2,5mm², możliwość podłączenia oprawy w pętle max 3x1,5mm². Przewód w oponie okrągłej o średnicy max ø12,5mm.","1107XX0009.png","1107XX0009.ldt",3,null,1,46]
["1108","1108XX0009","TRYSIL BOLLARD 85CM LED 1080LM 3000K ON/OFF","Trysil","Bollard","Aluminium",null,null,null,"LED zintegrowane","AC","ON/OFF","9,5W","9,5W","1080lm","660lm",null,null,"65","IK08","Class I",3000,"szerokie dół",0.34,0.11,0.85,"CE",null,null,"50 000h",1,"Oprawa słupkowa.","Światło rozproszone półsferyczne ukierunkowane w dół",null,"Luminaire with a contemporary design. For lighting gardens and other private and public areas",null,null,null,"Profil aluminiowy wyciskany, malowany proszkowo.",null,"Klosz- poliwęglan przeźroczysty ze strukturą, stabilizowany UV.","Uszczelka silikonowa.",null,"85cm",null,"Oprawa nieściemnialna","Moduł LED","Philips Fortimo DLM ES 1100/8xx G2 3K",null,0,null,0,80,"E","1907ZX0009, 1908GA0009, 1909GA0009, 3081XX0009","Zaciski podłączeniowe: max 3x2,5mm², możliwość podłączenia oprawy w pętle max 3x1,5mm². Przewód w oponie okrągłej o średnicy max ø12,5mm.","1108XX0009.png","1108XX0009.ldt",4,null,1,76]
["1109","1109XX0009","TRYSIL BOLLARD 85CM LED 1150LM 4000K ON/OFF","Trysil","Bollard","Aluminium",null,null,null,"LED zintegrowane","AC","ON/OFF","9,5W","9,5W","1150lm","700lm",null,null,"65","IK08","Class I",4000,"szerokie dół",0.34,0.11,0.85,"CE",null,null,"50000",1,"Oprawa słupkowa.","Światło rozproszone półsferyczne ukierunkowane w dół",null,"Luminaire with a contemporary design For lighting gardens and other private and public areas",null,null,"Oprawa wyposażona w wymienne źródło światła typu moduł LED, który zapewnia trwałość i optymalny rozsył światła, przy zachowaniu stosunkowo niskiego zużycia energii.","Profil aluminiowy wyciskany, malowany proszkowo.",null,"Klosz- poliwęglan przeźroczysty ze strukturą, stabilizowany UV.","Uszczelka silikonowa.",null,"85cm","on/off","Oprawa nieściemnialna","Moduł LED","Philips Fortimo DLM ES 1100/8xx G2 4K",null,0,null,0,80,"D","1907ZX0009, 1908GA0009, 1909GA0010, 3081XX0009","Zaciski podłączeniowe: max 3x2,5mm², możliwość podłączenia oprawy w pętle max 3x1,5mm². Przewód w oponie okrągłej o średnicy max ø12,5mm.","1109XX0009.png","1109XX0009.ldt",4,null,1,76]
["1157","1157XX0009","KOSTER DOUBLE HEAD POLE-TOP 2XLED 3960LM 3000K ON/OFF","Koster","Post,Head","Aluminium",null,null,null,"LED zintegrowane","AC","ON/OFF","35W","35W","3960lm","3136lm","Tworzywo sztuczne","Transparentny","65","IK10","Class I",3000,"szerokie dół",0.82,0.24,0.22,"CE",null,null,">50000h",2,"Oprawa słupowa (nasadzana).","Światło jednostronne: symetryczne, ukierunkowane w dół.",null,"Top-mounted luminaire, designed to be mounted on a lighting pole with a Ø50mm mounting shaft",null,null,null,"Odlew aluminiowy malowany proszkowo.",null,"Klosz- poliwęglan przeźroczysty ze strukturą, stabilizowany UV.",null,null,"Ø50",null,"Oprawa nieściemnialna","2 Moduły LED","Philips Fortimo DLM ES 2000/8xx G2 3K",null,0,null,0,80,"E","1255XX0009, 1275XX0009","Przewód H05VV-F 3G1 o długości 3,7m do podłączenia wewnątrz słupa oświetleniowego (w odpowiednio dobranej puszce elektroinstalacyjnej).","1157XX0009.png","1157XX0009.ldt",4,null,1,27]
["1159","1159XX0009","KOSTER DOUBLE HEAD POLE-TOP 2XLED 4100LM 4000K ON/OFF","Koster","Post,Head","Aluminium",null,null,null,"LED zintegrowane","AC","ON/OFF","35W","35W","4100lm","3250lm","Tworzywo sztuczne","Transparentny","65","IK10","Class I",4000,"szerokie dół",0.82,0.24,0.22,"CE",null,null,">50000h",2,"Oprawa słupowa (nasadzana).","Światło jednostronne: symetryczne, ukierunkowane w dół.",null,"Top-mounted luminaire, designed to be mounted on a lighting pole with a Ø50mm mounting shaft",null,null,null,"Odlew aluminiowy malowany proszkowo.",null,"Klosz- poliwęglan przeźroczysty ze strukturą, stabilizowany UV.",null,null,"Ø50",null,"Oprawa nieściemnialna","2 Moduły LED","Philips Fortimo DLM ES 2000/8xx G2 4K",null,0,null,0,80,"E","111GA0009, 1255XX0009, 1275XX0009","Przewód H05VV-F 3G1 o długości 3,7m do podłączenia wewnątrz słupa oświetleniowego (w odpowiednio dobranej puszce elektroinstalacyjnej).","1159XX0009.png","1159XX0009.ldt",4,null,1,27]
["1165","1165XX0009","KOSTER DOUBLE HEAD POLE-TOP 4XLED 5200LM VSM 3000K DIM. TRIAC","Koster","Post","Aluminium",null,null,"PRO","LED zintegrowane","AC","DIM. TRIAC","32W","34W","5200lm","3422lm","Tworzywo sztuczne","Transparentny","65","IK10","Class II",3000,"szerokie dół",0.82,0.24,0.22,"CE",null,null,">120000h",2,"Oprawa słupowa (nasadzana).","Soczewka firmy Ledil typu VSM (IESNA typ V).","VSM","Top-mounted luminaire, designed to be mounted on a lighting pole with a Ø50mm mounting shaft",null,null,null,"Odlew aluminiowy malowany proszkowo.",null,"Klosz- poliwęglan przeźroczysty ze strukturą, stabilizowany UV.",null,null,"Ø50",null,"Oprawa ściemnialna fazowo TRAILING EDGE (TE) - LEADING EDGE (LE)","4 Moduły LED","Philips Fortimo FastFlex LED 2x4 G5 3K","TCI Mini JOLLY 20W code 127556 Triac",0,null,0,70,"D","1255XX0009, 1275XX0009","Przewód H05VV-F 2G1 o długości 3,7m do podłączenia wewnątrz słupa oświetleniowego (w odpowiednio dobranej puszce elektroinstalacyjnej).","1165XX0009.png","1165XX0009.ldt",1,null,1,47]
["1167","1167XX0009","KOSTER DOUBLE HEAD POLE-TOP 4XLED 5480LM VSM 4000K DIM. TRIAC","Koster","Post,Head","Aluminium",null,null,"PRO","LED zintegrowane","AC","DIM. TRIAC","32W","34W","5480lm","3624lm","Tworzywo sztuczne","Transparentny","65","IK10","Class II",4000,"szerokie dół",0.82,0.24,0.22,"CE",null,null,">120000h",2,"Oprawa słupowa (nasadzana).","Soczewka firmy Ledil typu VSM (IESNA typ V).","VSM","Top-mounted luminaire, designed to be mounted on a lighting pole with a Ø60mm mounting shaft",null,null,null,"Odlew aluminiowy malowany proszkowo.",null,"Klosz- poliwęglan przeźroczysty ze strukturą, stabilizowany UV.",null,null,"Ø50",null,"Oprawa ściemnialna fazowo TRAILING EDGE (TE)","4 Moduły LED","Philips Fortimo FastFlex LED 2x4 G5 4K","TCI Mini JOLLY 20W code 127556 Triac",0,null,0,70,"D","1255XX0009, 1275XX0009","Przewód H05VV-F 2G1 o długości 3,7m do podłączenia wewnątrz słupa oświetleniowego (w odpowiednio dobranej puszce elektroinstalacyjnej).","1167XX0009.png","1167XX0009.ldt",1,null,1,47]
["1173","1173XX0009","KOSTER DOUBLE HEAD POLE-TOP 4XLED 5200LM VSM 3000K DALI2","Koster","Post,Head","Aluminium",null,null,"PRO","LED zintegrowane","AC","DALI2","32W","37W","5200lm","3654lm","Tworzywo sztuczne","Transparentny","65","IK10","Class I",3000,"szerokie dół",0.82,0.24,0.22,"CE",null,"DALI",">120000",2,"Oprawa słupowa (nasadzana).","Soczewka firmy Ledil typu VSM (IESNA typ V).","VSM","Top-mounted luminaire, designed to be mounted on a lighting pole with a Ø60mm mounting shaft",null,null,null,"Odlew aluminiowy malowany proszkowo.",null,"Klosz- poliwęglan przeźroczysty ze strukturą, stabilizowany UV.",null,null,"Ø50",null,"Sterowanie światłem w systemie: DALI outdoor pełny program. Zasilacz zaprogramowany na max prąd. Programowanie pozostałych parametrów po uzgodnieniu z Działem Handlowym firmy Norlys.","4 Moduły LED","Philips Fortimo FastFlex LED 2x4 G5 3K","Philips Xi FP 22W 0,2-0,7A SNLDAE 230V S175 sXt 929002172306",100000,"DALI2 / NightDim (XI FP NLD)",0,70,"D","1255XX0009, 1275XX0009","Przewód H05VV-F 5G1 o długości 3,7m do podłączenia wewnątrz słupa oświetleniowego (w odpowiednio dobranej puszce elektroinstalacyjnej).","1173XX0009.png","1173XX0009.ldt",3,null,1,47]
["1175","1175XX0009","KOSTER DOUBLE HEAD POLE-TOP 4XLED 5480LM VSM 4000K DALI2","Koster","Post,Head","Aluminium",null,null,"PRO","LED zintegrowane","AC","DALI2","32W","37W","5480lm","3825lm","Tworzywo sztuczne","Transparentny","65","IK10","Class I",4000,"szerokie dół",0.82,0.24,0.22,"CE",null,"DALI",">120000h",2,"Oprawa słupowa (nasadzana).","Soczewka firmy Ledil typu VSM (IESNA typ V).","VSM","Top-mounted luminaire, designed to be mounted on a lighting pole with a Ø60mm mounting shaft",null,null,null,"Odlew aluminiowy malowany proszkowo.",null,"Klosz- poliwęglan przeźroczysty ze strukturą, stabilizowany UV.",null,null,"Ø50",null,"Sterowanie światłem w systemie: DALI outdoor pełny program. Zasilacz zaprogramowany na max prąd. Programowanie pozostałych parametrów po uzgodnieniu z Działem Handlowym firmy Norlys.","4 Moduły LED","Philips Fortimo FastFlex LED 2x4 G5 4K","Philips Xi FP 22W 0,2-0,7A SNLDAE 230V S175 sXt 929002172306",100000,"DALI2 / NightDim (XI FP NLD)",0,70,"D","1255XX0009, 1275XX0009","Przewód H05VV-F 5G1 o długości 3,7m do podłączenia wewnątrz słupa oświetleniowego (w odpowiednio dobranej puszce elektroinstalacyjnej).","1175XX0009.png","1175XX0009.ldt",3,null,1,47]
["1179","1179XX0009","KOSTER DOUBLE HEAD POLE-TOP 2XLED 3960LM 3000K ON/OFF","Koster","Post,Head","Aluminium",null,null,null,"LED zintegrowane","AC","ON/OFF","35W","35W","3960lm","3136lm","Tworzywo sztuczne","Transparentny","65","IK10","Class I",3000,"szerokie dół",0.82,0.24,0.22,"CE",null,null,">50000h",2,"Oprawa słupowa (nasadzana).","Światło jednostronne: symetryczne, ukierunkowane w dół.",null,"Top-mounted luminaire, designed to be mounted on a lighting pole with a Ø60mm mounting shaft",null,null,null,"Odlew aluminiowy malowany proszkowo.",null,"Klosz- poliwęglan przeźroczysty ze strukturą, stabilizowany UV.",null,null,"Ø60",null,"Oprawa nieściemnialna","2 Moduły LED","Philips Fortimo DLM ES 2000/8xx G2 3K",null,0,null,null,80,"E","1257XX0009, 1277XX0009, 2000XX0009","Przewód H05VV-F 3G1 o długości 3,7m do podłączenia wewnątrz słupa oświetleniowego (w odpowiednio dobranej puszce elektroinstalacyjnej).","1179XX0009.png","1179XX0009.ldt",4,null,1,27]
["1181","1181XX0009","KOSTER DOUBLE HEAD POLE-TOP 2XLED 4100LM 4000K ON/OFF","Koster","Post,Head","Aluminium",null,null,null,"LED zintegrowane","AC","ON/OFF","35W","35W","4100lm","3250lm","Tworzywo sztuczne","Transparentny","65","IK10","Class I",4000,"szerokie dół",0.82,0.24,0.22,"CE",null,null,">50000h",2,"Oprawa słupowa (nasadzana).","Światło jednostronne: symetryczne, ukierunkowane w dół.",null,"Top-mounted luminaire, designed to be mounted on a lighting pole with a Ø60mm mounting shaft",null,null,null,"Odlew aluminiowy malowany proszkowo.",null,"Klosz- poliwęglan przeźroczysty ze strukturą, stabilizowany UV.",null,null,"Ø60",null,"Oprawa nieściemnialna","2 Moduły LED","Philips Fortimo DLM ES 2000/8xx G2 4K",null,0,null,null,80,"E","1257XX0009, 1277XX0009, 2000XX0009","Przewód H05VV-F 3G1 o długości 3,7m do podłączenia wewnątrz słupa oświetleniowego (w odpowiednio dobranej puszce elektroinstalacyjnej).","1181XX0009.png","1181XX0009.ldt",4,null,1,27]
["1187","1187XX0009","KOSTER DOUBLE HEAD POLE-TOP 4XLED 5200LM VSM 3000K DIM. TRIAC","Koster","Post,Head","Aluminium",null,null,"PRO","LED zintegrowane","AC","DIM. TRIAC","32W","34W","5200lm","3422lm","Tworzywo sztuczne","Transparentny","65","IK10","Class II",3000,"szerokie dół",0.82,0.24,0.22,"CE",null,null,">120000h",2,"Oprawa słupowa (nasadzana).","Soczewka firmy Ledil typu VSM (IESNA typ V).","VSM","Top-mounted luminaire, designed to be mounted on a lighting pole with a Ø60mm mounting shaft",null,null,null,"Odlew aluminiowy malowany proszkowo.",null,"Klosz- poliwęglan przeźroczysty ze strukturą, stabilizowany UV.",null,null,"Ø60",null,"Oprawa ściemnialna fazowo TRAILING EDGE (TE) - LEADING EDGE (LE)","4 Moduły LED","Philips Fortimo FastFlex LED 2x4 G5 3K","TCI Mini JOLLY 20W code 127556 Triac",0,null,null,70,"D","1257XX0009, 1277XX0009, 2000XX0009","Przewód H05VV-F 2G1 o długości 3,7m do podłączenia wewnątrz słupa oświetleniowego (w odpowiednio dobranej puszce elektroinstalacyjnej).","1187XX0009.png","1187XX0009.ldt",1,null,1,47]
["1189","1189XX0009","KOSTER DOUBLE HEAD POLE-TOP 4XLED 5480LM VSM 4000K DIM. TRIAC","Koster","Post,Head","Aluminium",null,null,"PRO","LED zintegrowane","AC","DIM. TRIAC","32W","34W","5480lm","3624lm","Tworzywo sztuczne","Transparentny","65","IK10","Class II",4000,"szerokie dół",0.82,0.24,0.22,"CE",null,null,"> 100 000h",2,"Oprawa słupowa (nasadzana).","Soczewka firmy Ledil typu VSM (IESNA typ V).","VSM","Top-mounted luminaire, designed to be mounted on a lighting pole with a Ø60mm mounting shaft",null,null,null,"Odlew aluminiowy malowany proszkowo.",null,"Klosz- poliwęglan przeźroczysty ze strukturą, stabilizowany UV.",null,null,"Ø60",null,"Oprawa ściemnialna fazowo TRAILING EDGE (TE) - LEADING EDGE (LE)","4 Moduły LED","Philips Fortimo FastFlex LED 2x4 G5 4K","TCI Mini JOLLY 20W code 127556 Triac",0,null,null,80,"D","1257XX0009, 1277XX0009, 2000XX0009","Przewód H05VV-F 2G1 o długości 3,7m do podłączenia wewnątrz słupa oświetleniowego (w odpowiednio dobranej puszce elektroinstalacyjnej).","1189XX0009.png","1189XX0009.ldt",1,null,1,47]
["1195","1195XX0009","KOSTER DOUBLE HEAD POLE-TOP 4XLED 5200LM VSM 3000K DALI2","Koster","Post,Head","Aluminium",null,null,"PRO","LED zintegrowane","AC","DALI2","32W","37W","5200lm","3654lm","Tworzywo sztuczne","Transparentny","65","IK10","Class I",3000,"szerokie dół",0.82,0.24,0.22,"CE",null,"DALI",">120000h",2,"Oprawa słupowa (nasadzana).","Soczewka firmy Ledil typu VSM (IESNA typ V).","VSM","Top-mounted luminaire, designed to be mounted on a lighting pole with a Ø60mm mounting shaft",null,null,null,"Odlew aluminiowy malowany proszkowo.",null,"Klosz- poliwęglan przeźroczysty ze strukturą, stabilizowany UV.",null,null,"Ø60",null,"Sterowanie światłem w systemie: DALI outdoor pełny program. Zasilacz zaprogramowany na max prąd. Programowanie pozostałych parametrów po uzgodnieniu z Działem Handlowym firmy Norlys.","4 Moduły LED","Philips Fortimo FastFlex LED 2x4 G5 3K","Philips Xi FP 22W 0,2-0,7A SNLDAE 230V S175 sXt 929002172306",100000,"DALI2 / NightDim (XI FP NLD)",0,70,"D","1257XX0009, 1277XX0009, 2000XX0009","Przewód H05VV-F 5G1 o długości 3,7m do podłączenia wewnątrz słupa oświetleniowego (w odpowiednio dobranej puszce elektroinstalacyjnej).","1195XX0009.png","1195XX0009.ldt",3,null,1,47]
["1197","1197XX0009","KOSTER DOUBLE HEAD POLE-TOP 4XLED 5480LM VSM 4000K DALI2","Koster","Post,Head","Aluminium",null,null,"PRO","LED zintegrowane","AC","DALI2","32W","37W","5480lm","3825lm","Tworzywo sztuczne","Transparentny","65","IK10","Class I",4000,"szerokie dół",0.82,0.24,0.22,"CE",null,"DALI",">120000h",2,"Oprawa słupowa (nasadzana).","Soczewka firmy Ledil typu VSM (IESNA typ V).","VSM","Top-mounted luminaire, designed to be mounted on a lighting pole with a Ø60mm mounting shaft",null,null,null,"Odlew aluminiowy malowany proszkowo.",null,"Klosz- poliwęglan przeźroczysty ze strukturą, stabilizowany UV.",null,null,"Ø60",null,"Sterowanie światłem w systemie: DALI outdoor pełny program. Zasilacz zaprogramowany na max prąd. Programowanie pozostałych parametrów po uzgodnieniu z Działem Handlowym firmy Norlys.","4 Moduły LED","Philips Fortimo FastFlex LED 2x4 G4+ 4K","Philips Xi FP 22W 0,2-0,7A SNLDAE 230V S175 sXt 929002172306",100000,"DALI2 / NightDim (XI FP NLD)",0,70,"D","1257XX0009, 1277XX0009, 2000XX0009","Przewód H05VV-F 5G1 o długości 3,7m do podłączenia wewnątrz słupa oświetleniowego (w odpowiednio dobranej puszce elektroinstalacyjnej).","1197XX0009.png","1197XX0009.ldt",3,null,1,47]
["120","120XX0011","VASA WALL E27 UP-DOWN","Vasa","Wall","Aluminium",null,null,null,"Wymienne","E27",null,"LED max 9W","LED max 9W",null,null,null,null,"65","IK08","Class I",null,"szerokie góra / szerokie dół",0.31,0.12,0.16,"CE",null,null,null,12,"Oprawa ścienna.","Światło dwustronne: ukierunkowane do góry i w dół.","Up-Down","A luminaire with a wide range of applications, among others for lighting: wall and facade surfaces and other architectural concepts",null,null,"Oprawa na wymienne źródło światła typu: lampa LED, świetlówka TC-SE, tradycyjna żarówka (halogenowa) o trzonku E27. Źródło światła należy dokupić oddzielnie.","Odlew aluminiowy malowany proszkowo.",null,"Klosz- poliwęglan przeźroczysty ze strukturą, stabilizowany UV.","Uszczelka silikonowa.","Dławnica EPDM.",null,null,null,"Lampa E27","A55..60",null,0,null,null,80,null,"46999021","Zaciski podłączeniowe: max 3x2,5mm², możliwość podłączenia oprawy w pętle max 3x1,5mm². Przewód w oponie okrągłej o średnicy ø7...10,5mm.","120XX0011.jpg","120XX0011.ldt",4,"E27",1,4]
["1240","1240XX0013","STAVANGER BOLLARD 95CM LED 1179LM 3000K DIM.","Stavanger","Bollard","Aluminium",null,null,null,"LED zintegrowane","AC","DIM.","9,6W","12,2W","1179lm","428lm",null,null,"65","IK10","Class I",3000,"szerokie dół",0.2,0.2,0.95,"CE",null,null,"> 145 000h",1,"Oprawa słupkowa.","Światło pośrednie, obrotowo- symetryczne, ukierunkowane w dół.",null,"Bollard luminaire of stable and durable construction For lighting private areas and public spaces",null,null,null,"Odlew aluminiowy malowany proszkowo.",null,"Klosz- poliwęglan przeźroczysty, stabilizowany UV.","Uszczelka silikonowa.","Dławnica nylon6.","95cm","przeźroczysty PC","Oprawa ściemnialna fazowo TRAILING EDGE (TE)","Moduł LED","Cree DK1305003 V2 XPG3 3K","Philips Xitanium 10W 0,5A 20V TE SC 230V",0,null,null,80,"D","1230ZX0009, 1231GA0009, 1232GA0009, 6139ZX0009, 7662ZX0009","Zaciski podłączeniowe: max 3x4mm², możliwość podłączenia oprawy w pętle max 3x2,5mm². Przewód w oponie okrągłej o średnicy ø8...17mm. Oprawa wyposażona w otwory do zamontowania szyny montażowej TH-35, o długości 10cm.","1240XX0013.jpg","1240XX0013.ldt",1,null,1,33]
["1244","1244XX0013","STAVANGER BOLLARD 50CM LED 1179LM 3000K DIM.","Stavanger","Bollard","Aluminium",null,null,null,"LED zintegrowane","AC","DIM.","9,6W","12,2W","1179lm","428lm",null,null,"65","IK10","Class I",3000,"szerokie dół",0.2,0.2,0.5,"CE",null,null,"> 145 000h",1,"Oprawa słupkowa.","Światło pośrednie, obrotowo- symetryczne, ukierunkowane w dół.",null,"Bollard luminaire of stable and durable construction. For lighting private areas and public spaces",null,null,null,"Odlew aluminiowy malowany proszkowo.",null,"Klosz- poliwęglan przeźroczysty, stabilizowany UV.","Uszczelka silikonowa.","Dławnica nylon6.","50cm","przeźroczysty PC","Oprawa ściemnialna fazowo TRAILING EDGE (TE)","Moduł LED","Cree DK1305003 V2 XPG3 3K","Philips Xitanium 10W 0,5A 20V TE SC 230V",0,null,null,80,"D","1230ZX0009, 1231GA0009, 1232GA0009","Zaciski podłączeniowe: max 3x4mm², możliwość podłączenia oprawy w pętle max 3x2,5mm². Przewód w oponie okrągłej o średnicy ø8...17mm. Oprawa wyposażona w otwory do zamontowania szyny montażowej TH-35, o długości 10cm.","1244XX0013.jpg","1244XX0013.ldt",1,null,1,33]
["1247","1247XX0013","STAVANGER BOLLARD 28CM LED 854LM 3000K DIM.","Stavanger","Bollard","Aluminium",null,null,null,"LED zintegrowane","AC","DIM.","6,6W","8,4W","854lm","312lm",null,null,"65","IK10","Class I",3000,"szerokie dół",0.2,0.2,0.28000000000000003,"CE",null,null,"> 145 000h",1,"Oprawa słupkowa.","Światło pośrednie, obrotowo- symetryczne, ukierunkowane w dół.",null,"Bollard luminaire of stable and durable construction. For lighting private areas and public spaces",null,null,null,"Odlew aluminiowy malowany proszkowo.",null,"Klosz- poliwęglan przeźroczysty, stabilizowany UV.","Uszczelka silikonowa.","Dławnica nylon6.","28cm","przeźroczysty PC","Oprawa ściemnialna fazowo TRAILING EDGE (TE)","Moduł LED","Cree DK1305003 V2 XPG3 3K","Philips Xitanium 7W 0,35A 20V TE SC 230V [2017]",50000,null,null,80,"D","1230ZX0009, 1231GA0009, 1232GA0009","Zaciski podłączeniowe: max 3x2,5mm², możliwość podłączenia oprawy w pętle max 3x2,5mm². Przewód w oponie okrągłej o średnicy ø8...17mm.","1247XX0013.jpg","1247XX0013.ldt",1,null,1,33]
["1260","1260XX0013","STOCKHOLM BOLLARD 49CM LED 1059LM 3000K DIM.","Stockholm","Bollard","Stal",null,null,null,"LED zintegrowane","AC","DIM.","6,7W","8,5W","1059lm","342lm",null,null,"65","IK10","Class II",3000,null,0,0,0,"CE",null,null,"> 50 000h",1,"Oprawa słupkowa.","Światło odkryte, rozproszone z obrotowo- symetrycznym rozsyłem światła.",null,"A bollard luminaire with a stable and durable structure For lighting private areas and other architectural concepts",null,null,null,"Stal cynkowana ogniowo.","Stal cynkowana ogniowo i malowana proszkowo.","Klosz- tworzywo sztuczne PMMA w kolorze mlecznym.","Uszczelka silikonowa.",null,"49cm","mleczny","Oprawa ściemnialna fazowo TRAILING EDGE (TE) - LEADING EDGE (LE)","Moduł LED","Philips Fortimo SLM C 1203 L09 1619 G7 3K","KGP CC10W180-270CG",50000,"Dim. TRIAC (KGP)",null,80,"D","205ZX0010, 206GA0010, 206GA0S10, 2951ZX0009","Zaciski podłączeniowe: max 2x4mm², możliwość podłączenia oprawy w pętle max 2x2,5mm². Przewód w oponie okrągłej o średnicy max ø12,5mm.","1260XX0013.jpg","1260XX0013.ldt",1,null,1,24]
["1261","1261XX0009","GLODE BOLLARD 65CM LED 7479LM T4-B 3000K DALI2","Glode","Bollard","Aluminium",null,null,null,"LED zintegrowane","AC","DALI2","48,5W","53W","7479lm","7320lm",null,null,"65","IK10","Class I",3000,"szerokie góra",0.65,0.24,0.12,"CE",null,"DALI","> 70 000h",13,"Oprawa słupkowa.","Soczewka firmy Ledil typu T4-B (IESNA typ IV).","T4-B","A luminaire with a modern design. For lighting buildings and other architectural concepts",null,null,null,"Odlew aluminiowy malowany proszkowo.",null,"Soczewka hermetyczna zewnętrzna- tworzywo sztuczne PMMA przeźroczyste.","Uszczelka silikonowa.","Dławnica nylon6.","65cm","DALI2","Sterowanie światłem w systemie: DALI outdoor pełny program. Zasilacz zaprogramowany na max prąd. Programowanie pozostałych parametrów po uzgodnieniu z Działem Handlowym firmy Norlys.","Moduł LED","Philips Fortimo FastFlex LED 2x6 DP G5 3K","Philips Xi FP 75W 0,2-0,7A SNLDAE 230V C133 sXt kod. 929002101406",100000,null,null,80,"D","112ZX0009, 113GA0009, 114GA0009",null,"1261XX0009.png","1261XX0009.ldt",3,null,1,64]
["1262","1262XX0009","GLODE BOLLARD 65CM LED 8099LM T4-B 4000K DALI2","Glode","Bollard","Aluminium",null,null,null,"LED zintegrowane","AC","DALI2","48,5W","53W","8099lm","7746lm",null,null,"65","IK10","Class I",4000,"szerokie góra",0.65,0.24,0.12,"CE",null,"DALI","> 70 000h",13,"Oprawa słupkowa.","Soczewka firmy Ledil typu T4-B (IESNA typ IV).","T4-B","A luminaire with a modern design. For lighting buildings and other architectural concepts",null,null,null,"Odlew aluminiowy malowany proszkowo.",null,"Soczewka hermetyczna zewnętrzna- tworzywo sztuczne PMMA przeźroczyste.","Uszczelka silikonowa.","Dławnica nylon6.","65cm","DALI2","Sterowanie światłem w systemie: DALI outdoor pełny program. Zasilacz zaprogramowany na max prąd. Programowanie pozostałych parametrów po uzgodnieniu z Działem Handlowym firmy Norlys.","Moduł LED","Philips Fortimo FastFlex LED 2x6 DP G5 4K","Philips Xi FP 75W 0,2-0,7A SNLDAE 230V C133 sXt kod. 929002101406",100000,null,null,80,"D","112ZX0009, 113GA0009, 114GA0009",null,"1262XX0009.png","1262XX0009.ldt",3,null,1,64]
["1263","1263XX0009","GLODE BOLLARD 40CM LED 7479LM T4-B 3000K DALI2","Glode","Bollard","Aluminium",null,null,null,"LED zintegrowane","AC","DALI2","48,5W","53W","7479lm","7320lm",null,null,"65","IK10","Class I",3000,"szerokie góra",0.4,0.24,0.12,"CE",null,"DALI","> 70 000h",13,"Oprawa słupkowa.","Soczewka firmy Ledil typu T4-B (IESNA typ IV).","T4-B","A luminaire with a modern design. For lighting buildings and other architectural concepts",null,null,null,"Odlew aluminiowy malowany proszkowo.",null,"Soczewka hermetyczna zewnętrzna- tworzywo sztuczne PMMA przeźroczyste.","Uszczelka silikonowa.","Dławnica nylon6.","40cm","DALI2","Sterowanie światłem w systemie: DALI outdoor pełny program. Zasilacz zaprogramowany na max prąd. Programowanie pozostałych parametrów po uzgodnieniu z Działem Handlowym firmy Norlys.","Moduł LED","Philips Fortimo FastFlex LED 2x6 DP G5 3K","Philips Xi FP 75W 0,2-0,7A SNLDAE 230V C133 sXt kod. 929002101406",100000,null,null,80,"D","112ZX0009, 113GA0009, 114GA0009",null,"1263XX0009.png","1263XX0009.ldt",3,null,1,64]
["1264","1264XX0009","GLODE BOLLARD 40CM LED 8099LM T4-B 4000K DALI2","Glode","Bollard","Aluminium",null,null,null,"LED zintegrowane","AC","DALI2","48,5W","53W","8099lm","7746lm",null,null,"65","IK10","Class I",4000,"szerokie góra",0.4,0.24,0.12,"CE",null,"DALI","> 70 000h",13,"Oprawa słupkowa.","Soczewka firmy Ledil typu T4-B (IESNA typ IV).","T4-B","A luminaire with a modern design. For lighting buildings and other architectural concepts",null,null,null,"Odlew aluminiowy malowany proszkowo.",null,"Soczewka hermetyczna zewnętrzna- tworzywo sztuczne PMMA przeźroczyste.","Uszczelka silikonowa.","Dławnica nylon6.","40cm","DALI2","Sterowanie światłem w systemie: DALI outdoor pełny program. Zasilacz zaprogramowany na max prąd. Programowanie pozostałych parametrów po uzgodnieniu z Działem Handlowym firmy Norlys.","Moduł LED","Philips Fortimo FastFlex LED 2x6 DP G5 4K","Philips Xi FP 75W 0,2-0,7A SNLDAE 230V C133 sXt kod. 929002101406",100000,null,null,80,"D","112ZX0009, 113GA0009, 114GA0009",null,"1264XX0009.png","1264XX0009.ldt",3,null,1,64]
["1265","1265XX0013","STOCKHOLM BOLLARD 85CM LED 1059LM 3000K DIM.","Stockholm","Bollard","Stal",null,null,null,"LED zintegrowane","AC","DIM.","6,7W","8,5W","1059lm","342lm",null,null,"65","IK10","Class II",3000,null,0,0,0,"CE",null,null,"> 50 000h",1,"Oprawa słupkowa.","Światło odkryte, rozproszone z obrotowo- symetrycznym rozsyłem światła.",null,"A bollard luminaire with a stable and durable structure. For lighting gardens, private areas, and other architectural structures",null,null,null,"Stal cynkowana ogniowo.","Stal cynkowana ogniowo i malowana proszkowo.","Klosz- tworzywo sztuczne PMMA w kolorze mlecznym.","Uszczelka silikonowa.",null,"85cm","mleczny","Oprawa ściemnialna fazowo TRAILING EDGE (TE) - LEADING EDGE (LE)","Moduł LED","Philips Fortimo SLM C 1203 L09 1619 G7 3K","KGP CC10W180-270CG",50000,"Dim. TRIAC (KGP)",null,80,"D","205ZX0010, 206GA0010, 206GA0S10, 2951ZX0009, 6138ZX0009","Zaciski podłączeniowe: max 2x4mm², możliwość podłączenia oprawy w pętle max 2x2,5mm². Przewód w oponie okrągłej o średnicy max ø12,5mm.","1265XX0013.jpg","1265XX0013.ldt",1,null,1,24]
["1268","1268XX0010","STOCKHOLM BOLLARD 28CM LED 1150LM 3000K DIM.","Stockholm","Bollard","Stal",null,null,null,"LED zintegrowane","AC","DIM.",null,"10W","1150lm","333lm",null,null,"65","IK10","Class I",3000,null,0,0,0,"CE",null,null,"> 50 000h",1,"Oprawa słupkowa.","Światło odkryte, rozproszone z obrotowo- symetrycznym rozsyłem światła.",null,"Bollard luminaire of stable and durable construction. For lighting private areas and public spaces.",null,null,null,"Stal cynkowana ogniowo.","Stal cynkowana ogniowo i malowana proszkowo.","Klosz- tworzywo sztuczne PMMA w kolorze mlecznym.","Uszczelka silikonowa.",null,"28cm","mleczny","Oprawa ściemnialna fazowo TRAILING EDGE (TE) - LEADING EDGE (LE)","Moduł LED","Lumens EDC 47C 10W xxx 230V A101 3K",null,0,"Ściemnianie fazowe Lumens LED AC",null,80,"E","205ZX0010, 206GA0010","Zaciski podłączeniowe: max 3x2,5mm². Przewód w oponie okrągłej o średnicy max ø12,5mm.","1268XX0010.jpg","1268XX0010.ldt",1,null,1,24]
["1269","1269XX0010","STOCKHOLM BOLLARD 28CM LED E27 806LM 2700K DIM.","Stockholm","Bollard","Stal",null,null,null,"Wymienne","E27",null,"5,9W","5,9W","~ 806lm","100lm",null,null,"65","IK10","Class II",2700,null,0.16,0.16,0.28000000000000003,"CE",null,null,"25 000h",1,"Oprawa słupkowa.","Światło odkryte, częściowo przysłonięte od góry.",null,"Bollard luminaire of stable and durable construction. For lighting private areas and public spaces.",null,null,"Oprawa na wymienne źródło światła typu: lampa LED, świetlówka TC-SE, Źródło światła dołączone do oprawy","Stal cynkowana ogniowo.",null,"Klosz- tworzywo sztuczne PMMA w kolorze mlecznym.","Uszczelka silikonowa.",null,"28cm","mleczny","Oprawa ściemnialna fazowo TRAILING EDGE (TE) - LEADING EDGE (LE)","Lampa LED E27","Philips MAS LEDBulb DT5.9-60W E27 927 A60 FR G",null,0,"Ściemnianie fazowe LED GU10 E27",null,80,"F","205ZX0010, 206GA0010, 206GA0S10","Zaciski podłączeniowe: max 3x2,5mm², Przewód w oponie okrągłej o średnicy max ø12mm.","1269XX0010.jpg","1269XX0010.ldt",1,"E27",1,23]
["127","127XX0012","VASA WALL LED E27 806LM UP-DOWN 2700K DIM.","Vasa","Wall","Aluminium",null,null,null,"Wymienne","E27",null,"8W","8W","806lm","384lm",null,null,"65","IK08","Class I",2700,"szerokie góra / szerokie dół",0.31,0.12,0.16,"CE",null,null,"25000",12,"Oprawa ścienna.","Światło dwustronne: ukierunkowane do góry i w dół.","Up-Down","Luminaire with a wide range of applications for example for illumination of walls and facade surfaces or any other architectural concepts.",null,null,null,"Odlew aluminiowy malowany proszkowo.",null,"Klosz- poliwęglan przeźroczysty ze strukturą, stabilizowany UV.","Uszczelka silikonowa.","Dławnica EPDM.",null,null,"Oprawa ściemnialna fazowo TRAILING EDGE (TE) - LEADING EDGE (LE)","Lampa LED E27","Philips Master LEDbulb DT 8-60W E27 A60 CL 806lm/827",null,0,"Ściemnianie fazowe LED GU10 E27",null,80,"F",null,"Zaciski podłączeniowe: max 3x2,5mm², możliwość podłączenia oprawy w pętle max 3x1,5mm². Przewód w oponie okrągłej o średnicy ø7...10,5mm.","127XX0012.jpg","127XX0012.ldt",1,"E27",1,4]
["1280","1280XX0014","EGERSUND BOLLARD 108CM LED 2617LM 3000K DIM.","Egersund","Bollard","Aluminium",null,null,null,"LED zintegrowane","AC","DIM.","18W","20,3W","2617lm","1681lm",null,null,"65","IK08","Class II",3000,null,0.2,0.2,1.08,"CE",null,null,"> 162 000h",1,"Oprawa słupkowa.","Światło obrotowo-symetryczne.",null,"Luminaire with a contemporary design. For lighting gardens and other private and public areas",null,null,null,"Odlew aluminiowy malowany proszkowo.",null,"Klosz- tworzywo sztuczne PMMA przeźroczyste.","Uszczelka silikonowa.","Dławnica nylon6.","108cm",null,"Oprawa ściemnialna fazowo TRAILING EDGE (TE) - LEADING EDGE (LE)","Moduł LED","Cree DK201002 V1 JK3030 6V 3K","TCI Mini JOLLY 20W code 127556 Triac",0,null,null,80,"E","1230ZX0009, 1231GA0009, 1232GA0010","Zaciski podłączeniowe: max 2x4mm², możliwość podłączenia oprawy w pętle max 2x4mm². Przewód w oponie okrągłej o średnicy ø8...17mm.","1280XX0014.jpg","1280XX0014.ldt",1,null,1,17]
["1281","1281XX0009","GLODE BOLLARD 65CM LED 7479LM T4-B 3000K ON/OFF","Glode","Bollard","Aluminium",null,null,null,"LED zintegrowane","AC","ON/OFF","48W","54W","7479lm","7320lm",null,null,"65","IK10","Class I",3000,"szerokie góra",0.65,0.24,0.12,"CE",null,null,"> 70 000h",13,"Oprawa słupkowa.","Soczewka firmy Ledil typu T4-B (IESNA typ IV).","T4-B","A luminaire with a modern design. For lighting buildings and other architectural concepts",null,null,null,"Odlew aluminiowy malowany proszkowo.",null,"Soczewka hermetyczna zewnętrzna- tworzywo sztuczne PMMA przeźroczyste.","Uszczelka silikonowa.","Dławnica nylon6.","65cm",null,"Oprawa nieściemnialna","Moduł LED","Philips Fortimo FastFlex LED 2x6 DP G5 3K","Philips Xi BP 75W 0.2-0.7A S 230V C133 929002817006",100000,null,null,80,"D","112ZX0009, 113GA0009, 114GA0009",null,"1281XX0009.png","1281XX0009.ldt",4,null,1,64]
["1282","1282XX0009","GLODE BOLLARD 65CM LED 8099LM T4-B 4000K ON/OFF","Glode","Bollard","Aluminium",null,null,null,"LED zintegrowane","AC","ON/OFF","48W","54W","8099lm","7745lm",null,null,"65","IK10","Class I",4000,"szerokie góra",0.65,0.24,0.12,"CE",null,null,"> 70 000h",13,"Oprawa słupkowa.","Soczewka firmy Ledil typu T4-B (IESNA typ IV).","T4-B","A luminaire with a modern design. For lighting buildings and other architectural concepts",null,null,null,"Odlew aluminiowy malowany proszkowo.",null,"Soczewka hermetyczna zewnętrzna- tworzywo sztuczne PMMA przeźroczyste.","Uszczelka silikonowa.","Dławnica nylon6.","65cm",null,"Oprawa nieściemnialna","Moduł LED","Philips Fortimo FastFlex LED 2x6 DP G5 4K","Philips Xi BP 75W 0.2-0.7A S 230V C133 929002817006",100000,null,null,80,"D","112ZX0009, 113GA0009, 114GA0009",null,"1282XX0009.png","1282XX0009.ldt",4,null,1,64]
["1283","1283XX0009","GLODE BOLLARD 40CM LED 7479LM T4-B 3000K ON/OFF","Glode","Bollard","Aluminium",null,null,null,"LED zintegrowane","AC","ON/OFF","48W","54W","7479lm","7320lm",null,null,"65","IK10","Class I",3000,"szerokie góra",0.4,0.24,0.12,"CE",null,null,"> 70 000h",13,"Oprawa słupkowa.","Soczewka firmy Ledil typu T4-B (IESNA typ IV).","T4-B","A luminaire with a modern design. For lighting buildings and other architectural concepts",null,null,null,"Odlew aluminiowy malowany proszkowo.",null,"Soczewka hermetyczna zewnętrzna- tworzywo sztuczne PMMA przeźroczyste.","Uszczelka silikonowa.","Dławnica nylon6.","40cm",null,null,"Moduł LED","Philips Fortimo FastFlex LED 2x6 DP G5 3K","Philips Xi BP 75W 0.2-0.7A S 230V C133 929002817006",100000,null,null,80,"D","112ZX0009, 113GA0009, 114GA0009",null,"1283XX0009.png","1283XX0009.ldt",4,null,1,64]
["1284","1284XX0009","GLODE BOLLARD 40CM LED 8099LM T4-B 4000K ON/OFF","Glode","Bollard","Aluminium",null,null,null,"LED zintegrowane","AC","ON/OFF","48W","54W","8099lm","7745lm",null,null,"65","IK10","Class I",4000,"szerokie góra",0.4,0.24,0.12,"CE",null,null,"> 70 000h",13,"Oprawa słupkowa.","Soczewka firmy Ledil typu T4-B (IESNA typ IV).","T4-B","A luminaire with a modern design. For lighting buildings and other architectural concepts",null,null,null,"Odlew aluminiowy malowany proszkowo.",null,"Soczewka hermetyczna zewnętrzna- tworzywo sztuczne PMMA przeźroczyste.","Uszczelka silikonowa.","Dławnica nylon6.","40cm",null,"Oprawa nieściemnialna","Moduł LED","Philips Fortimo FastFlex LED 2x6 DP G5 4K","Philips Xi BP 75W 0.2-0.7A S 230V C133 929002817006",100000,null,null,80,"D","112ZX0009, 113GA0009, 114GA0009",null,"1284XX0009.png","1284XX0009.ldt",4,null,1,64]
["128","128XX0014","VASA WALL 2XLED 1128LM UP-DOWN 3000K DIM.","Vasa","Wall","Aluminium",null,null,null,"LED zintegrowane","AC","DIM.","6,6W","8,5W","1128lm","631lm",null,null,"65","IK08","Class I",3000,"szerokie góra / szerokie dół",0.31,0.12,0.16,"CE",null,null,"> 72 000h",12,"Oprawa ścienna.","Światło dwustronne: ukierunkowane do góry i w dół.","Up-Down","Luminaire with a wide range of applications for example for illumination of walls and facade surfaces or any other architectural concepts",null,null,null,"Odlew aluminiowy malowany proszkowo.",null,"Klosz- poliwęglan przeźroczysty ze strukturą, stabilizowany UV.","Uszczelka silikonowa.","Dławnica EPDM.",null,null,"Oprawa ściemnialna fazowo TRAILING EDGE (TE)","2 Moduły LED","Philips Fortimo Strip 0,5ft MF FC LV6 3K","Philips Xitanium 8W 0,2A 40V TE SC 230V",0,"Philips Xitanium TE",null,80,"D",null,"Zaciski podłączeniowe: max 3x2,5mm², możliwość podłączenia oprawy w pętle max 3x1,5mm². Przewód w oponie okrągłej o średnicy ø7...10,5mm.","128XX0014.jpg","128XX0014.ldt",1,null,1,4]
["1290","1290XX0014","EGERSUND MINI BOLLARD 85CM LED 1370LM 3000K DIM.","Egersund Mini","Bollard","Aluminium",null,null,null,"LED zintegrowane","AC","DIM.","7,4W","9,1W","1370lm","864lm",null,null,"65","IK08","Class II",3000,null,0,0,0,"CE",null,null,"> 72 000h",1,"Oprawa słupkowa.","Światło obrotowo-symetryczne.",null,"Luminaire with contemporary design, for lighting gardens and other private and public areas",null,null,null,"Odlew aluminiowy malowany proszkowo.",null,"Klosz- tworzywo sztuczne PMMA przeźroczyste.","Uszczelka silikonowa.","Dławnica nylon6.","85cm",null,"Oprawa ściemnialna fazowo TRAILING EDGE (TE) - LEADING EDGE (LE)","Moduł LED","Cree DK210704 V2 JB2835 3V 3K","TCI MICRO MD 10W 350mA 127040 Triac",0,null,null,80,"E","205ZX0010, 206GA0010, 206GA0S10, 2951ZX0009, 6138ZX0009","Zaciski podłączeniowe: max 2x4mm², możliwość podłączenia oprawy w pętle max 2x2,5mm². Przewód w oponie okrągłej o średnicy ø8...12,5mm. Pozostałe systemy podłączeniowe jako akcesoria, które należy dokupić oddzielnie.","1290XX0014.jpg","1290XX0014.ldt",1,null,1,17]
["1291","1291XX0013","EGERSUND MINI BOLLARD 49CM LED 1370LM 3000K DIM.","Egersund Mini","Bollard","Aluminium",null,null,null,"LED zintegrowane","AC","DIM.","7,4W","9,1W","1370lm","864lm",null,null,"65","IK08","Class II",3000,null,0,0,0,"CE",null,null,"> 72 000h",1,"Oprawa słupkowa.","Światło obrotowo-symetryczne.",null,"Luminaire with contemporary design, for lighting gardens and other private and public areas",null,null,null,"Odlew aluminiowy malowany proszkowo.",null,"Klosz- tworzywo sztuczne PMMA przeźroczyste.","Uszczelka silikonowa.","Dławnica nylon6.","49cm",null,"Oprawa ściemnialna fazowo TRAILING EDGE (TE) - LEADING EDGE (LE)","Moduł LED","Cree DK210704 V2 JB2835 3V 3K","TCI MICRO MD 10W 350mA 127040 Triac",0,null,null,80,"C","205ZX0010, 206GA0010, 206GA0S10, 2951ZX0009, 6138ZX0009","Zaciski podłączeniowe: max 2x4mm², możliwość podłączenia oprawy w pętle max 2x2,5mm². Przewód w oponie okrągłej o średnicy ø8...12,5mm.","1291XX0013.jpg","1291XX0013.ldt",1,null,1,17]
["1300","1300XX0014","ASKER BIG WALL 2XLED 1128LM UP-DOWN 3000K DIM.","Asker,Big","Wall","Aluminium",null,null,null,"LED zintegrowane","AC","DIM.","6,6W","8,3","1128lm","547lm",null,null,"65","IK08","Class I",3000,"szerokie góra / szerokie dół",0.3,0.12,0.12,"CE",null,null,"> 72 000h",12,"Oprawa ścienna.","Światło dwustronne: ukierunkowane do góry i w dół.","Up-Down","Luminaire with a wide range of applications, for illumination of walls and facade surfaces or any other architectural concepts",null,null,null,"Odlew aluminiowy malowany proszkowo.",null,"Klosz- poliwęglan przeźroczysty ze strukturą, stabilizowany UV.","Uszczelka silikonowa.","Dławnica EPDM.","góra/dół",null,"Oprawa ściemnialna fazowo TRAILING EDGE (TE)","2 Moduły LED","Philips Fortimo_LED_Strip_0.5ft_MF_8xx_HV6 3K","Philips Xitanium 8W 0,2A 40V TE SC 230V",0,"Philips Xitanium TE",null,80,"D",null,"Zaciski podłączeniowe: max 3x2,5mm², możliwość podłączenia oprawy w pętle max 3x1,5mm². Przewód w oponie okrągłej o średnicy ø7...10,5mm.","1300XX0014.jpg","1300XX0014.ldt",1,null,1,4]
["1302","1302XX0013","ASKER BIG WALL LED 653LM DOWN 3000K DIM.","Asker,Big","Wall","Aluminium",null,null,null,"LED zintegrowane","AC","DIM.","3,9W","5,2W","653lm","306lm",null,null,"65","IK08","Class I",3000,"szerokie dół",0,0,0,"CE",null,null,"> 70000",12,"Oprawa ścienna.","Światło rozproszone półsferyczne ukierunkowane w dół",null,"A luminaire with a wide range of applications, for illuminating wall and facade surfaces as well as other architectural concepts",null,null,null,"Odlew aluminiowy malowany proszkowo.",null,"Klosz- poliwęglan przeźroczysty ze strukturą, stabilizowany UV.","Uszczelka silikonowa.","Dławnica EPDM.","dół",null,"Oprawa ściemnialna fazowo TRAILING EDGE (TE)","Moduł LED","Philips Strip OC 0.5ft 550lm 8xx FC HV5 3K","Philips Xitanium 7W 0,35A 20V TE SC 230V [2017]",50000,null,null,80,"C",null,"Zaciski podłączeniowe: max 3x2,5mm², możliwość podłączenia oprawy w pętle max 3x1,5mm². Przewód w oponie okrągłej o średnicy ø7...10,5mm.","1302XX0013.jpg","1302XX0013.ldt",1,null,1,76]
["1303","1303XX0010","ASKER BIG WALL E27 UP-DOWN","Asker,Big","Wall","Aluminium",null,null,null,"Wymienne","E27",null,"LED max 9W","LED max 9W",null,null,null,null,"65","IK08","Class I",null,"szerokie góra / szerokie dół",0.3,0.12,0.12,"CE",null,null,null,12,"Oprawa ścienna.","Światło dwustronne: ukierunkowane do góry i w dół.","Up-Down","Luminaire with a wide range of applications for example for illumination of walls and facade surfaces or any other architectural concepts.",null,null,"Oprawa na wymienne źródło światła typu: lampa LED, świetlówka TC-SE, tradycyjna żarówka (halogenowa) o trzonku E27. Źródło światła należy dokupić oddzielnie.","Odlew aluminiowy malowany proszkowo.",null,"Klosz- poliwęglan przeźroczysty ze strukturą, stabilizowany UV.","Uszczelka silikonowa.","Dławnica EPDM.","góra/dół",null,null,"Lampa E27","LED A55..60",null,0,null,null,80,null,"46999021","Zaciski podłączeniowe: max 3x2,5mm², możliwość podłączenia oprawy w pętle max 3x1,5mm². Przewód w oponie okrągłej o średnicy ø7...10,5mm.","1303XX0010.jpg","1303XX0010.ldt",4,"E27",1,4]
["1305","1305XX0010","ASKER BIG WALL E27 DOWN","Asker,Big","Wall","Aluminium",null,null,null,"Wymienne","E27",null,"LED max 9W",null,null,null,null,null,"65","IK08","Class I",null,"szerokie dół",0,0,0,"CE",null,null,null,12,"Oprawa ścienna.","Światło rozproszone półsferyczne ukierunkowane w dół",null,"Luminaire with a wide range of applications for example for illumination of walls and facade surfaces or any other architectural concepts.",null,null,"Oprawa na wymienne źródło światła typu: lampa LED, świetlówka TC-SE, tradycyjna żarówka (halogenowa) o trzonku E27. Źródło światła należy dokupić oddzielnie.","Odlew aluminiowy malowany proszkowo.",null,"Klosz- poliwęglan przeźroczysty ze strukturą, stabilizowany UV.","Uszczelka silikonowa.","Dławnica EPDM.","dół",null,null,"Lampa E27","LED A55..60",null,null,null,null,80,null,"46999021","Zaciski podłączeniowe: max 3x2,5mm², możliwość podłączenia oprawy w pętle max 3x1,5mm². Przewód w oponie okrągłej o średnicy ø7...10,5mm.","1305XX0010.jpg","1305XX0010.ldt",4,"E27",1,76]
["1306","1306XX0010","ASKER BIG PRO WALL 4XLED 2043LM UP-DOWN 3000K DIM.","Asker,Big","Wall","Aluminium",null,null,"PRO","LED zintegrowane","AC","DIM.","11,6 W","13,7 W","2043lm","1280lm",null,null,"65","IK08","Class I",3000,"szerokie góra / szerokie dół",null,null,null,"CE",null,null,"> 70 000h",12,"Oprawa ścienna.","Światło dwustronne: ukierunkowane do góry i w dół.","Up-Down","A luminaire with a wide range of applications, including lighting of wall surfaces, facades and other architectural concepts",null,null,null,"Odlew aluminiowy malowany proszkowo.",null,"Klosz- poliwęglan przeźroczysty ze strukturą, stabilizowany UV.","Uszczelka silikonowa.","Dławnica EPDM.","góra/dół",null,"Oprawa ściemnialna fazowo TRAILING EDGE (TE)","4 Moduły LED","Philips Fortimo Strip 0,5ft MF FC LV6 3K","Philips Xitanium 14W 0,35A 40V TE SC 230V",0,"Philips Xitanium TE",null,80,"C",null,"Zaciski podłączeniowe: max 3x2,5mm², możliwość podłączenia oprawy w pętle max 3x1,5mm². Przewód w oponie okrągłej o średnicy ø7...10,5mm.","1306XX0010.jpg","1306XX0010.ldt",1,null,1,4]
["1308","1308XX0012","ASKER BIG WALL 2XLED 1122LM DOWN 3000K DIM.","Asker,Big","Wall","Aluminium",null,null,null,"LED zintegrowane","AC","DIM.","6,6 W","8,4W","1122lm","732lm",null,null,"65","IK08","Class I",3000,"szerokie dół",0.3,0.12,0.12,"CE",null,null,"> 72 000h",12,"Oprawa ścienna.","Światło rozproszone półsferyczne ukierunkowane w dół",null,"A luminaire with a wide range of applications, for illuminating wall, facade surfaces and other architectural concepts",null,null,null,"Odlew aluminiowy malowany proszkowo.",null,"Klosz- poliwęglan przeźroczysty ze strukturą, stabilizowany UV.","Uszczelka silikonowa.","Dławnica EPDM.","dół",null,"Oprawa ściemnialna fazowo TRAILING EDGE (TE)","2 Moduły LED","Philips Fortimo_LED_Strip_0.5ft_MF_8xx_HV6 3K","Philips Xitanium 8W 0,2A 40V TE SC 230V",0,"Philips Xitanium TE",null,80,"D",null,"Zaciski podłączeniowe: max 3x2,5mm², możliwość podłączenia oprawy w pętle max 3x1,5mm². Przewód w oponie okrągłej o średnicy ø7...10,5mm.","1308XX0012.jpg","1308XX0012.ldt",1,null,1,76]
["1310","1310XX0009","ASKER BOLLARD 55CM LED 1080LM 3000K ON/OFF","Asker","Bollard","Aluminium",null,null,null,"LED zintegrowane","AC","ON/OFF","9,5W","9,5W","1080lm","585lm",null,null,"65","IK10","Class I",3000,"szerokie dół",0.56999999999999995,0.23,0.14000000000000001,"CE",null,null,"50 000h",1,"Oprawa słupkowa.","Światło rozproszone półsferyczne ukierunkowane w dół",null,"Luminaire with contemporary design. For lighting private areas and other architectural concepts",null,null,null,"Odlew aluminiowy malowany proszkowo.",null,"Klosz- poliwęglan przeźroczysty ze strukturą, stabilizowany UV.","Uszczelka silikonowa.","Dławnica EPDM.","55cm",null,"Oprawa nieściemnialna","Moduł LED","Philips Fortimo DLM ES 1100/8xx G2 3K",null,0,null,0,80,"E","1907ZX0009, 1908GA0009, 3081XX0009","Zaciski podłączeniowe: max 3x2,5mm², możliwość podłączenia oprawy w pętle max 3x1,5mm². Przewód w oponie okrągłej o średnicy max ø12,5mm.","1310XX0009.jpg","1310XX0009.ldt",4,null,1,76]
["1311","1311XX0012","ASKER BOLLARD 85CM LED 1080LM 3000K ON/OFF","Asker","Bollard","Aluminium",null,null,null,"LED zintegrowane","AC","ON/OFF","9,5W","9,5W","1080lm","585lm",null,null,"65","IK10","Class I",3000,null,0.85,0.2,0.11,"CE",null,null,"50 000h",1,"Oprawa słupkowa.","Światło rozproszone półsferyczne ukierunkowane w dół",null,"Luminaire with a contemporary design. For lighting gardens, private areas and other architectural applications",null,null,null,"Odlew aluminiowy malowany proszkowo.",null,"Klosz- poliwęglan przeźroczysty ze strukturą, stabilizowany UV.","Uszczelka silikonowa.","Dławnica EPDM.","85cm",null,"Oprawa nieściemnialna","Moduł LED","Philips Fortimo DLM ES 1100/8xx G2 3K",null,0,null,0,80,"E","1907ZX0009, 1908GA0009, 1909GA0009","Zaciski podłączeniowe: max 3x2,5mm², możliwość podłączenia oprawy w pętle max 3x1,5mm². Przewód w oponie okrągłej o średnicy max ø12,5mm.","1311XX0012.jpg","1311XX0012.ldt",4,null,1,76]
["1312","1312XX0013","ASKER BOLLARD 2XLED 1190LM 3000K DALI2","Asker","Bollard","Aluminium",null,null,null,"LED zintegrowane","AC","DALI2","6,5W","8,5W","1190lm","642lm",null,null,"65","IK10","Class I",3000,"szerokie dół",0.85,0.2,0.11,"CE",null,"DALI","> 171 460hrs",1,"Oprawa słupkowa.","Światło ukierunkowane w dół.",null,"A fixture with a contemporary design. For lighting gardens, private areas and other architectural concepts.","A luminaire with a contemporary design. For lighting gardens, private areas and other architectural concepts. Suitable for emergency installations with direct voltage: DC 180 ÷ 280 V",null,null,"Odlew aluminiowy malowany proszkowo.",null,"Klosz- poliwęglan przeźroczysty ze strukturą, stabilizowany UV.","Uszczelka silikonowa.","Dławnica EPDM.",null,null,"Sterowanie światłem w systemie: DALI2","2 Moduły LED","Cree DK180501 V8 JB2835 3V 3K","KGP CC10W150-500 DALI",100000,null,0,80,"C","1907ZX0009, 1908GA0009, 1909GA0009","Zaciski podłączeniowe: max 5x2,5mm², możliwość podłączenia oprawy w pętle max 5x2,5mm². Przewód w oponie okrągłej o średnicy: ø4…8mm; ø8...12mm lub ø10...13,6mm","1312XX0013.jpg","1312XX0013.ldt",3,null,1,45]
["1314","1314XX0011","ASKER PRO BOLLARD 85CM LED 828LM SCL 3000K DIM. TE","Asker","Bollard","Aluminium",null,null,"PRO","LED zintegrowane","AC","DIM. TE","5,8W","7,7W","828lm","697lm",null,null,"65","IK08","Class I",3000,"szerokie dół",0,0,0,"CE",null,null,"> 109 000h",1,"Oprawa słupkowa.","Soczewka firmy Ledil typu SCL (IESNA typ II / III).","SCL","A luminaire with a contemporary design. For lighting gardens and other private areas.",null,null,null,"Odlew aluminiowy malowany proszkowo.",null,"Soczewka hermetyczna zewnętrzna- tworzywo sztuczne PMMA przeźroczyste.","Uszczelka silikonowa.","Dławnica EPDM.","85cm",null,"Oprawa ściemnialna fazowo TRAILING EDGE (TE)","Moduł LED","Cree DK200402 V1 XTE-HE 3K","Philips Xitanium 10W 0,5A 20V TE SC 230V",0,null,0.01,80,"E","1907ZX0009, 1908GA0009, 3081XX0009","Zaciski podłączeniowe: max 3x2,5mm², możliwość podłączenia oprawy w pętle max 3x1,5mm². Przewód w oponie okrągłej o średnicy max ø12,5mm.","1314XX0011.jpg","1314XX0011.ldt",1,null,1,46]
["1315","1315XX0011","ASKER PRO BOLLARD 85CM LED 828LM SCL 3000K DALI2","Asker","Bollard","Aluminium",null,null,"PRO","LED zintegrowane","AC","DALI2","5,8W","7,8W","828lm","683lm",null,null,"65","IK08","Class I",3000,"szerokie dół",0,0,0,"CE",null,"DALI",">109 000h",1,"Oprawa słupkowa.","Soczewka firmy Ledil typu SCL (IESNA typ II / III).","SCL","A luminaire with a contemporary design. For lighting gardens and other private areas.",null,null,null,"Odlew aluminiowy malowany proszkowo.",null,"Soczewka hermetyczna zewnętrzna- tworzywo sztuczne PMMA przeźroczyste.","Uszczelka silikonowa.","Dławnica EPDM.","85cm",null,"Sterowanie światłem w systemie: DALI/TD.","Moduł LED","Cree DK200402 V1 XTE-HE 3K","Osram OTi DALI 15/220…240/1A0 LT2 NFC",100000,null,0.01,80,"E","1907ZX0009, 1908GA0009, 3081XX0009","Zaciski podłączeniowe: max 5x2,5mm², możliwość podłączenia oprawy w pętle max 5x1,5mm². Przewód w oponie okrągłej o średnicy max ø12,5mm.","1315XX0011.jpg","1315XX0011.ldt",3,null,1,46]
["1316","1316XX0011","ASKER PRO BOLLARD 85CM LED 828LM VSM 3000K DIM. TE","Asker","Bollard","Aluminium",null,null,"PRO","LED zintegrowane","AC","DIM. TE","5,8W","7,7W","828lm","604lm",null,null,"65","IK08","Class I",3000,"szerokie dół",0,0,0,"CE",null,null,"> 109 000h",1,"Oprawa słupkowa.","Soczewka firmy Ledil typu VSM (IESNA typ V).","VSM","A luminaire with a contemporary design. For lighting gardens and other private areas.",null,null,null,"Odlew aluminiowy malowany proszkowo.",null,"Soczewka hermetyczna zewnętrzna- tworzywo sztuczne PMMA przeźroczyste.","Uszczelka silikonowa.","Dławnica EPDM.","85cm",null,"Oprawa ściemnialna fazowo TRAILING EDGE (TE)","Moduł LED","Cree DK200402 V1 XTE-HE 3K","Philips Xitanium 10W 0,5A 20V TE SC 230V",0,null,0.02,80,"E","1907ZX0009, 1908GA0009, 3081XX0009","Zaciski podłączeniowe: max 3x2,5mm², możliwość podłączenia oprawy w pętle max 3x1,5mm². Przewód w oponie okrągłej o średnicy max ø12,5mm.","1316XX0011.jpg","1316XX0011.ldt",1,null,1,47]
["1317","1317XX0011","ASKER PRO BOLLARD 85CM LED 828LM VSM 3000K DALI2","Asker","Bollard","Aluminium",null,null,"PRO","LED zintegrowane","AC","DALI2","5,8W","7,8W","828lm","599lm",null,null,"65","IK08","Class I",3000,"szerokie dół",0,0,0,"CE",null,"DALI","> 109 000h",1,"Oprawa słupkowa.","Soczewka firmy Ledil typu VSM (IESNA typ V).","VSM","A luminaire with a contemporary design. For lighting gardens and other private areas.",null,null,"Oprawa wyposażona w wymienne źródło światła typu moduł LED, który zapewnia trwałość i optymalny rozsył światła, przy zachowaniu stosunkowo niskiego zużycia energii.","Odlew aluminiowy malowany proszkowo.",null,"Soczewka hermetyczna zewnętrzna- tworzywo sztuczne PMMA przeźroczyste.","Uszczelka silikonowa.","Dławnica EPDM.","85cm",null,"Sterowanie światłem w systemie: DALI/TD.","Moduł LED","Cree DK200402 V1 XTE-HE 3K","Osram OTi DALI 15/220…240/1A0 LT2 NFC",100000,null,0.02,80,"E","1907ZX0009, 1908GA0009, 3081XX0009","Zaciski podłączeniowe: max 5x2,5mm², możliwość podłączenia oprawy w pętle max 5x1,5mm². Przewód w oponie okrągłej o średnicy max ø12,5mm.","1317XX0011.jpg","1317XX0011.ldt",3,null,1,47]
["1318","1318XX0011","ASKER PRO BOLLARD 85CM LED 828LM SCL 4000K DIM. TE","Asker","Bollard","Aluminium",null,null,"PRO","LED zintegrowane","AC","DIM. TE","5,8W","7,7W","828lm","724lm",null,null,"65","IK08","Class I",4000,"szerokie dół",0.2,0.11,0.85,"CE",null,null,"> 109 000h",1,"Oprawa słupkowa.","Soczewka firmy Ledil typu SCL (IESNA typ II / III).","SCL","A luminaire with a contemporary design. For lighting gardens and other private areas.",null,null,null,"Odlew aluminiowy malowany proszkowo.",null,"Soczewka hermetyczna zewnętrzna- tworzywo sztuczne PMMA przeźroczyste.","Uszczelka silikonowa.","Dławnica EPDM.","85cm",null,"Oprawa ściemnialna fazowo TRAILING EDGE (TE)","Moduł LED","Cree DK200402 V1 XTE-HE 3V 4K.","Philips Xitanium 10W 0,5A 20V TE SC 230V",0,"Philips Xitanium TE",0.01,80,"E","1907ZX0009, 1908GA0009, 3081XX0009","Zaciski podłączeniowe: max 3x2,5mm², możliwość podłączenia oprawy w pętle max 3x1,5mm². Przewód w oponie okrągłej o średnicy max ø12,5mm.","1318XX0011.jpg","1318XX0011.ldt",1,null,1,46]
["1319","1319XX0011","ASKER PRO BOLLARD 85CM LED 828LM SCL 4000K DALI2","Asker","Bollard","Aluminium",null,null,"PRO","LED zintegrowane","AC","DALI2","5,8W","7,8W","828lm","706lm",null,null,"65","IK08","Class I",4000,"szerokie dół",0,0,0,"CE",null,"DALI",">109 000h",1,"Oprawa słupkowa.","Soczewka firmy Ledil typu SCL (IESNA typ II / III).","SCL","A luminaire with a contemporary design. For lighting gardens and other private areas.",null,null,null,"Odlew aluminiowy malowany proszkowo.",null,"Soczewka hermetyczna zewnętrzna- tworzywo sztuczne PMMA przeźroczyste.","Uszczelka silikonowa.","Dławnica EPDM.","85cm",null,"Sterowanie światłem w systemie: DALI/TD.","Moduł LED","Cree DK200402 V1 XTE-HE 3V 4K.","Osram OTi DALI 15/220…240/1A0 LT2 NFC",100000,null,0.01,80,"E","1907ZX0009, 1908GA0009, 3081XX0009","Zaciski podłączeniowe: max 3x2,5mm², możliwość podłączenia oprawy w pętle max 3x1,5mm². Przewód w oponie okrągłej o średnicy max ø12,5mm.","1319XX0011.jpg","1319XX0011.ldt",3,null,1,46]
["1320","1320XX0011","ASKER PRO BOLLARD 85CM LED 856LM VSM 4000K DIM. TE","Asker","Bollard","Aluminium",null,null,"PRO","LED zintegrowane","AC","DIM. TE","5,8W","7,7W","856lm","617lm",null,null,"65","IK08","Class I",4000,"szerokie dół",0.85,0.2,0.11,"CE",null,null,"> 109 000h",1,"Oprawa słupkowa.","Soczewka firmy Ledil typu VSM (IESNA typ V).","VSM","A luminaire with a contemporary design. For lighting gardens and other private areas.",null,null,null,"Odlew aluminiowy malowany proszkowo.",null,"Soczewka hermetyczna zewnętrzna- tworzywo sztuczne PMMA przeźroczyste.","Uszczelka silikonowa.","Dławnica EPDM.","85cm",null,"Oprawa ściemnialna fazowo TRAILING EDGE (TE)","Moduł LED","Cree DK200402 V1 XTE-HE 3V 4K.","Philips Xitanium 10W 0,5A 20V TE SC 230V",0,null,0.02,80,"E","1907ZX0009, 1908GA0009, 3081XX0009","Zaciski podłączeniowe: max 3x2,5mm², możliwość podłączenia oprawy w pętle max 3x1,5mm². Przewód w oponie okrągłej o średnicy max ø12,5mm.","1320XX0011.jpg","1320XX0011.ldt",1,null,1,47]
["1321","1321XX0012","OPPLAND BOLLARD LED 984LM 3000K DIM.","Oppland","Bollard","Aluminium",null,null,null,"LED zintegrowane","AC","DIM.","6,1W","8,2W","984lm","304lm",null,null,"65","IK09","Class II",3000,"szerokie dół",0.85,0.12,0.12,"CE",null,null,">171 460h",1,"Oprawa słupkowa.","Światło rozproszone półsferyczne ukierunkowane w dół",null,"A bollard luminaire with a stable and durable construction. For lighting private areas and other architectural concepts",null,null,null,"Odlew aluminiowy malowany proszkowo.",null,"Klosz- poliwęglan przeźroczysty ze strukturą, stabilizowany UV.","Uszczelka silikonowa.","Dławnica nylon6.",null,null,"Oprawa ściemnialna fazowo TRAILING EDGE (TE) - LEADING EDGE (LE)","Moduł LED","Cree DK180501 V8 JB2835 3V 3K","TCI Micro MD 10W 700mA code 127046 Triac",0,null,0,80,"C","205ZX0010, 206GA0010, 206GA0S10","Zaciski podłączeniowe: max 2x4mm², możliwość podłączenia oprawy w pętle max 2x4mm². Przewód w oponie okrągłej o średnicy: ø4…8mm; ø8...12mm lub ø10...13,6mm","1321XX0012.jpg","1321XX0012.ldt",1,null,1,76]
["1322","1322XX0011","ASKER PRO BOLLARD 85CM LED 828LM VSM 4000K DALI2","Asker","Bollard","Aluminium",null,null,"PRO","LED zintegrowane","AC","DALI2","5,8W","7,8W","828lm","616lm",null,null,"65","IK08","Class I",4000,"szerokie dół",0,0,0,"CE",null,"DALI","> 109 000h",1,"Oprawa słupkowa.","Soczewka firmy Ledil typu VSM (IESNA typ V).","VSM","A luminaire with a contemporary design. For lighting gardens and other private areas.",null,null,null,"Odlew aluminiowy malowany proszkowo.",null,"Soczewka hermetyczna zewnętrzna- tworzywo sztuczne PMMA przeźroczyste.","Uszczelka silikonowa.","Dławnica EPDM.","85cm",null,"Sterowanie światłem w systemie: DALI/TD.","Moduł LED","Cree DK200402 V1 XTE-HE 3K","Osram OTi DALI 15/220…240/1A0 LT2 NFC",100000,null,0.02,80,"E","1907ZX0009, 1908GA0009, 3081XX0009","Zaciski podłączeniowe: max 3x2,5mm², możliwość podłączenia oprawy w pętle max 3x1,5mm². Przewód w oponie okrągłej o średnicy max ø12,5mm.","1322XX0011.jpg","1322XX0011.ldt",3,null,1,47]
["1324","1324XX0009","OPPLAND BOLLARD LED 984LM 3000K DALI2","Oppland","Bollard","Aluminium",null,null,null,"LED zintegrowane","AC","DALI2","6,1W","8,2W","984lm","304lm",null,null,"65","IK09","Class I",3000,null,0.85,0.12,0.12,"CE",null,"DALI","> 171 460h",1,"Oprawa słupkowa.","Światło rozproszone półsferyczne ukierunkowane w dół",null,"A bollard luminaire with a stable and durable construction For lighting private and public areas","A bollard luminaire with a stable and durable construction For lighting private and public areas Suitable for DC emergency installations: DC 198 ÷ 264 V",null,null,"Odlew aluminiowy malowany proszkowo.",null,"Klosz- poliwęglan przeźroczysty ze strukturą, stabilizowany UV.","Uszczelka silikonowa.","Dławnica nylon6.",null,null,"Sterowanie światłem w systemie: DALI2","Moduł LED","Cree DK180501 V8 JB2835 3V 3K","Osram OTi DALI 15W 220-240V 1A0 NFC EAN 4062172061766",0,null,0,80,"C","205ZX0010, 206GA0010, 206GA0S10","Zaciski podłączeniowe: max 5x2,5mm², możliwość podłączenia oprawy w pętle max 5x2,5mm². Przewód w oponie okrągłej o średnicy: ø4…8mm; ø8...12mm lub ø10...13,6mm","1324XX0009.jpg","1324XX0009.ldt",3,null,1,76]
["1330","1330XX0009","HITRA WALL LED 1080LM 3000K ON/OFF","Hitra","Wall","Aluminium",null,null,null,"LED zintegrowane","AC","ON/OFF","9,5W","9,5W","1080lm","920lm",null,null,"65","IK06","Class I",3000,"szerokie dół",0.2,0.15,0.06,"CE",null,null,"50000",12,"Oprawa ścienna.","Światło rozproszone półsferyczne ukierunkowane w dół",null,"Modern design luminaire. For lighting private areas and public spaces.",null,null,null,"Odlew aluminiowy malowany proszkowo.",null,"Klosz- szkło bezpieczne, przeźroczyste.","Uszczelka silikonowa.","Dławnica EPDM.",null,null,"Oprawa nieściemnialna","Moduł LED","Philips Fortimo DLM ES 1100/8xx G2 3K",null,0,null,0,80,"E","151XX0009","Zaciski podłączeniowe: max 3x2,5mm², możliwość podłączenia oprawy w pętle max 3x1,5mm². Przewód w oponie okrągłej o średnicy ø7...10,5mm.","1330XX0009.jpg","1330XX0009.ldt",4,null,1,76]
["1331","1331XX0009","HITRA WALL LED 1950LM 3000K ON/OFF","Hitra","Wall","Aluminium",null,null,null,"LED zintegrowane","AC","ON/OFF","17,5W","17,5W","1950lm","1599lm",null,null,"65","IK08","Class I",3000,"szerokie dół",0,0,0,"CE",null,null,"50000",12,"Oprawa ścienna.","Światło rozproszone półsferyczne ukierunkowane w dół",null,"Modern design luminaire. For lighting private areas and public spaces.",null,null,null,"Odlew aluminiowy malowany proszkowo.",null,"Klosz- szkło bezpieczne, przeźroczyste.","Uszczelka silikonowa.","Dławnica EPDM.",null,null,"Oprawa nieściemnialna","Moduł LED","Philips Fortimo DLM ES 2000/8xx G2 3K",null,null,null,0,80,"E","151XX0009","Zaciski podłączeniowe: max 3x2,5mm², możliwość podłączenia oprawy w pętle max 3x1,5mm². Przewód w oponie okrągłej o średnicy ø7...10,5mm.","1331XX0009.jpg","1331XX0009.ldt",4,null,1,76]
["1336","1336XX0009","ASKER BOLLARD 55CM LED 1080LM 3000K ON/OFF MD","Asker","Bollard","Aluminium",null,null,null,"LED zintegrowane","AC","ON/OFF","9,5W","9,7W","1080lm","585lm",null,null,"65",null,"Class I",3000,"szerokie dół",0.55000000000000004,0.2,0.11,"CE","Daylight sensor,Motion sensor",null,"50 000h",1,"Oprawa słupkowa.","Światło rozproszone półsferyczne ukierunkowane w dół",null,"Luminaire with a contemporary design. For lighting private areas and other architectural concepts",null,null,null,"Odlew aluminiowy malowany proszkowo.",null,"Klosz- poliwęglan przeźroczysty ze strukturą, stabilizowany UV.","Uszczelka silikonowa.","Dławnica EPDM.","55cm","PIR","Oprawa wyposażona w czujnik ruchu typu PIR, z wyłącznikiem zmierzchowym i podtrzymaniem ruchu. Zaprogramowany na: maksymalny zasięg działania, czas świecenia 1 minuta, zmierzch 10lux.","Moduł LED","Philips Fortimo DLM ES 1100/8xx G2 3K",null,0,"Czujnik ruchu PIR ESYLUX MD-C 360I/6 mini",0,80,"E","1907ZX0009, 1908GA0009, 3081XX0009, 4699990003","Zaciski podłączeniowe: max 3x4mm², możliwość podłączenia oprawy w pętle max 3x4mm². Przewód w oponie okrągłej o średnicy: ø4…8mm; ø8...12mm lub ø10...13,6mm","1336XX0009.png","1336XX0009.ldt",3,null,1,76]
["1337","1337XX0009","ASKER BOLLARD 55CM LED 1150LM 4000K ON/OFF MD","Asker","Bollard","Aluminium",null,null,null,"LED zintegrowane","AC","ON/OFF","9,5W","9,7W","1150lm","636lm",null,null,"65",null,"Class I",4000,"szerokie dół",0.55000000000000004,0.2,0.11,"CE","Daylight sensor,Motion sensor",null,"50 000h",1,"Oprawa słupkowa.","Światło rozproszone półsferyczne ukierunkowane w dół",null,"Luminaire with a contemporary design. For lighting private areas and other architectural concepts",null,null,null,"Odlew aluminiowy malowany proszkowo.",null,"Klosz- poliwęglan przeźroczysty ze strukturą, stabilizowany UV.","Uszczelka silikonowa.","Dławnica EPDM.","55cm","PIR","Oprawa wyposażona w czujnik ruchu typu PIR, z wyłącznikiem zmierzchowym i podtrzymaniem ruchu. Zaprogramowany na: maksymalny zasięg działania, czas świecenia 1 minuta, zmierzch 10lux.","Moduł LED","Philips Fortimo DLM ES 1100/8xx G2 4K",null,0,"Czujnik ruchu PIR ESYLUX MD-C 360I/6 mini",0,80,"D","1907ZX0009, 1908GA0009, 3081XX0009, 4699990003","Zaciski podłączeniowe: max 3x4mm², możliwość podłączenia oprawy w pętle max 3x4mm². Przewód w oponie okrągłej o średnicy: ø4…8mm; ø8...12mm lub ø10...13,6mm","1337XX0009.png","1337XX0009.ldt",3,null,1,76]
["1338","1338XX0009","ASKER BOLLARD 85CM LED 1080LM 3000K ON/OFF MD","Asker","Bollard","Aluminium",null,null,null,"LED zintegrowane","AC","ON/OFF","9,5W","9,7W","1080lm","585lm",null,null,"65",null,"Class I",3000,null,0.85,0.2,0.11,"CE","Daylight sensor,Motion sensor",null,"50 000h",1,"Oprawa słupkowa.","Światło rozproszone półsferyczne ukierunkowane w dół",null,"Luminaire with a contemporary design. For lighting private areas and other architectural concepts",null,null,null,"Odlew aluminiowy malowany proszkowo.",null,"Klosz- poliwęglan przeźroczysty ze strukturą, stabilizowany UV.","Uszczelka silikonowa.","Dławnica EPDM.","85cm","PIR","Oprawa wyposażona w czujnik ruchu typu PIR, z wyłącznikiem zmierzchowym i podtrzymaniem ruchu. Zaprogramowany na: maksymalny zasięg działania, czas świecenia 1 minuta, zmierzch 10lux.","Moduł LED","Philips Fortimo DLM ES 1100/8xx G2 3K",null,0,"Czujnik ruchu PIR ESYLUX MD-C 360I/6 mini",0,80,"E","1907ZX0009, 1908GA0009, 1909GA0009, 4699990003","Zaciski podłączeniowe: max 3x4mm², możliwość podłączenia oprawy w pętle max 3x4mm². Przewód w oponie okrągłej o średnicy: ø4…8mm; ø8...12mm lub ø10...13,6mm","1338XX0009.png","1338XX0009.ldt",3,null,1,76]
["1339","1339XX0009","ASKER BOLLARD 85CM LED 1150LM 4000K ON/OFF MD","Asker","Bollard","Aluminium",null,null,null,"LED zintegrowane","AC","ON/OFF","9,5W","9,7W","1150lm","640lm",null,null,"65",null,"Class I",4000,null,0.85,0.2,0.11,"CE","Daylight sensor,Motion sensor",null,"50 000h",1,"Oprawa słupkowa.","Światło rozproszone półsferyczne ukierunkowane w dół",null,"Luminaire with a contemporary design. For lighting private areas and other architectural concepts",null,null,null,"Odlew aluminiowy malowany proszkowo.",null,"Klosz- poliwęglan przeźroczysty ze strukturą, stabilizowany UV.","Uszczelka silikonowa.","Dławnica EPDM.","85cm","PIR","Oprawa wyposażona w czujnik ruchu typu PIR, z wyłącznikiem zmierzchowym i podtrzymaniem ruchu. Zaprogramowany na: maksymalny zasięg działania, czas świecenia 1 minuta, zmierzch 10lux.","Moduł LED","Philips Fortimo DLM ES 1100/8xx G2 4K",null,0,"Czujnik ruchu PIR ESYLUX MD-C 360I/6 mini",0,80,"E","1907ZX0009, 1908GA0009, 1909GA0009, 4699990003","Zaciski podłączeniowe: max 3x4mm², możliwość podłączenia oprawy w pętle max 3x4mm². Przewód w oponie okrągłej o średnicy: ø4…8mm; ø8...12mm lub ø10...13,6mm","1339XX0009.png","1339XX0009.ldt",3,null,1,76]
["1340","1340XX0011","NAMSOS MINI WALL-RECESSED LED 439LM 3000K DIM.","Namsos,Mini","Recessed","Aluminium",null,null,null,"LED zintegrowane","AC","DIM.","4W","4W","439lm","47lm",null,null,"65","IK10","Class I",3000,null,0,0,0,"CE",null,null,"> 50 000h",11,"Oprawa wbudowana ścienna.","Światło rozproszone półsferyczne ukierunkowane w dół",null,"The luminaire is adapted to illuminate stairs, steps, staircases, passageways, ceilings, and for the implementation of other architectural concepts",null,null,null,"Odlew aluminiowy malowany proszkowo.",null,"Klosz- szkło bezpieczne, satynowane.","Uszczelka silikonowa.","Dławnica EPDM.",null,null,"Oprawa ściemnialna fazowo TRAILING EDGE (TE) - LEADING EDGE (LE)","Moduł LED","Lumens EDC 38C 4W xxx 230V A101 3K",null,0,"Ściemnianie fazowe Lumens LED AC",null,80,"E",null,"Zaciski podłączeniowe: max 3x2,5mm², możliwość podłączenia oprawy w pętle max 3x1,5mm². Przewód w oponie okrągłej o średnicy ø7...10,5mm.","1340XX0011.jpg","1340XX0011.ldt",1,null,1,76]
["1341","1341XX0010","NAMSOS MINI WALL LED 439LM 3000K DIM.","Namsos,Mini","Wall","Aluminium",null,null,null,"LED zintegrowane","AC","DIM.","4W","4W","439lm","123lm",null,null,"65","IK09","Class I",3000,null,0,0,0,"CE",null,null,"> 50000",12,"Oprawa ścienna.","Światło rozproszone półsferyczne ukierunkowane w dół",null,"Luminaire designed to illuminate stairs, steps, staircases, communication routes, ceiling illumination, and many other architectural applications",null,null,null,"Odlew aluminiowy malowany proszkowo.","Korpus- odlew aluminiowy malowany proszkowo.","Klosz- szkło bezpieczne, satynowane.","Uszczelka silikonowa.",null,null,null,"Oprawa ściemnialna fazowo TRAILING EDGE (TE) - LEADING EDGE (LE)","Moduł LED","Lumens EDC 38C 4W xxx 230V A101 3K",null,null,"Ściemnianie fazowe Lumens LED AC",null,80,"E","157XX0009","Zaciski podłączeniowe: max 3x2,5mm², możliwość podłączenia oprawy w pętle max 3x1,5mm². Przewód w oponie okrągłej o średnicy ø7...10,5mm.","1341XX0010.jpg","1341XX0010.ldt",1,null,1,76]
["1346","1346XX0009","HALMSTAD BOLLARD 49CM LED 1059LM 4000K DIM. TE","Halmstad","Bollard","Stal",null,null,null,"LED zintegrowane","AC","DIM. TE","6,7W","8,5W","1059lm","310lm",null,null,"65","IK10","Class II",4000,null,0.12,0.12,0.49,"CE",null,null,"> 50 000h",1,"Oprawa słupkowa.","Światło odkryte, częściowo przysłonięte od góry.",null,"A bollard luminaire with a stable and durable structure For lighting private areas and other architectural concepts",null,null,null,"Stal cynkowana ogniowo.","Stal cynkowana ogniowo i malowana proszkowo.","Klosz- tworzywo sztuczne PMMA w kolorze mlecznym.","Uszczelka silikonowa.",null,"49cm",null,"Oprawa ściemnialna fazowo TRAILING EDGE (TE) - LEADING EDGE (LE)","Moduł LED","Philips Fortimo SLM C 1203 L09 1619 G7 4K","KGP CC10W180-270CG",50000,"Dim. TRIAC (KGP)",null,80,"D","205ZX0010, 206GA0010, 206GA0S10, 2951ZX0009","Zaciski podłączeniowe: max 2x4mm², możliwość podłączenia oprawy w pętle max x2,5mm². Przewód w oponie okrągłej o średnicy max ø12,5mm.","1346XX0009.jpg","1346XX0009.ldt",1,null,1,23]
["1347","1347XX0009","HALMSTAD BOLLARD 49CM LED 1121LM 4000K DIM.","Halmstad,Wood","Bollard","Drewno","Impregnowane",null,null,"LED zintegrowane","AC","DIM.","6,7W","8,5W","1121lm","310lm",null,null,"65","IK10","Class II",4000,null,0.12,0.12,0.49,"CE",null,null,"> 50 000h",1,"Oprawa słupkowa.","Światło odkryte, częściowo przysłonięte od góry.",null,"A bollard luminaire with a stable and durable structure For lighting private areas and other architectural concepts",null,null,null,"Drewno- sosna skandynawska impregnowana i stal cynkowana ogniowo.","Drewno- sosna skandynawska impregnowana, stal cynkowana ogniowo i malowana proszkowo.","Klosz- tworzywo sztuczne PMMA w kolorze mlecznym.","Uszczelka silikonowa.",null,"49cm",null,"Oprawa ściemnialna fazowo TRAILING EDGE (TE) - LEADING EDGE (LE)","Moduł LED","Philips Fortimo SLM C 1203 L09 1619 G7 4K","KGP CC10W180-270CG",50000,"Dim. TRIAC (KGP)",null,80,"D","205ZX0010, 206GA0010, 206GA0S10","Zaciski podłączeniowe: max 2x4mm², możliwość podłączenia oprawy w pętle max 2x4mm². Przewód w oponie okrągłej o średnicy max ø12,5mm.","1347XX0009.png","1347XX0009.ldt",1,null,1,23]
["1350","1350XX0009","HALMSTAD BOLLARD 85CM LED 1121LM 4000K DIM.","Halmstad,Wood","Bollard","Drewno","Impregnowane",null,null,"LED zintegrowane","AC","DIM.","6,7W","8,5W","1121lm","310lm",null,null,"65","IK10","Class II",4000,null,0.12,0.12,0.85,"CE",null,null,"> 50 000h",1,"Oprawa słupkowa.","Światło odkryte, częściowo przysłonięte od góry.",null,"A bollard luminaire with a stable and durable structure For lighting private areas and other architectural concepts",null,null,null,"Drewno- sosna skandynawska impregnowana i stal cynkowana ogniowo.","Drewno- sosna skandynawska impregnowana, stal cynkowana ogniowo i malowana proszkowo.","Klosz- tworzywo sztuczne PMMA w kolorze mlecznym.","Uszczelka silikonowa.",null,"85cm",null,"Oprawa ściemnialna fazowo TRAILING EDGE (TE) - LEADING EDGE (LE)","Moduł LED","Philips Fortimo SLM C 1203 L09 1619 G7 4K","KGP CC10W180-270CG",50000,"Dim. TRIAC (KGP)",null,80,"D","205ZX0010, 206GA0010, 206GA0S10","Zaciski podłączeniowe: max 2x4mm², możliwość podłączenia oprawy w pętle max 2x4mm². Przewód w oponie okrągłej o średnicy max ø12,5mm.","1350XX0009.png","1350XX0009.ldt",1,null,1,23]
["1353","1353XX0009","HALMSTAD BOLLARD 49CM LED 1121LM 4000K DIM.","Halmstad,Wood","Bollard","Drewno","Malowane",null,null,"LED zintegrowane","AC","DIM.","6,7W","8,5W","1121lm","310lm",null,null,"65","IK10","Class II",4000,null,0.12,0.12,0.49,"CE",null,null,"> 50 000h",1,"Oprawa słupkowa.","Światło odkryte, częściowo przysłonięte od góry.",null,"A bollard luminaire with a stable and durable structure For lighting private areas and other architectural concepts",null,null,null,"Drewno- sosna skandynawska malowana i stal cynkowana ogniowo.","Drewno- sosna skandynawska malowana, stal cynkowana ogniowo i malowana proszkowo.","Klosz- tworzywo sztuczne PMMA w kolorze mlecznym.","Uszczelka silikonowa.",null,"49cm",null,"Oprawa ściemnialna fazowo TRAILING EDGE (TE) - LEADING EDGE (LE)","Moduł LED","Philips Fortimo SLM C 1203 L09 1619 G7 4K","KGP CC10W180-270CG",50000,"Dim. TRIAC (KGP)",null,80,"D","205ZX0010, 206GA0010, 206GA0S10","Zaciski podłączeniowe: max 2x4mm², możliwość podłączenia oprawy w pętle max 2x4mm². Przewód w oponie okrągłej o średnicy max ø12,5mm.","1353XX0009.png","1353XX0009.ldt",1,null,1,23]
["1356","1356XX0009","HALMSTAD BOLLARD 85CM LED 1121LM 4000K DIM.","Halmstad,Wood","Bollard","Drewno","Malowane",null,null,"LED zintegrowane","AC","DIM.","6,7W","8,5W","1121lm","310lm",null,null,"65",null,"Class II",4000,null,0.12,0.12,0.85,"CE",null,null,"> 50 000h",1,"Oprawa słupkowa.","Światło odkryte, częściowo przysłonięte od góry.",null,"A bollard luminaire with a stable and durable structure For lighting private areas and other architectural concepts",null,null,null,"Drewno- sosna skandynawska malowana i stal cynkowana ogniowo.","Drewno- sosna skandynawska malowana, stal cynkowana ogniowo i malowana proszkowo.","Klosz- tworzywo sztuczne PMMA w kolorze mlecznym.","Uszczelka silikonowa.",null,"85cm",null,"Oprawa ściemnialna fazowo TRAILING EDGE (TE) - LEADING EDGE (LE)","Moduł LED","Philips Fortimo SLM C 1203 L09 1619 G7 4K","KGP CC10W180-270CG",50000,"Dim. TRIAC (KGP)",null,80,"D","205ZX0010, 206GA0010, 206GA0S10","Zaciski podłączeniowe: max 2x4mm², możliwość podłączenia oprawy w pętle max 2x4mm². Przewód w oponie okrągłej o średnicy max ø12,5mm.","1356XX0009.png","1356XX0009.ldt",1,null,1,23]
["1360","1360XX0011","ASKER POLE LIGHT LUMINAIRES POLE 216CM 2XLED 1988LM 3000K DIM.","Asker","Post,Post complete","Aluminium",null,null,null,"LED zintegrowane","AC","DIM.","10,6W","12W","1988lm","1128lm",null,null,"65",null,"Class I",3000,"szerokie dół",0,0,0,"CE",null,null,"> 72 000h",20,"Oprawa słupowa (lekka konstrukcja).","Światło jednostronne: symetryczne, ukierunkowane w dół.",null,"For lighting private areas and other architectural concepts",null,null,null,"Profil aluminiowy wyciskany, malowany proszkowo.",null,"Klosz- poliwęglan przeźroczysty ze strukturą, stabilizowany UV.","Uszczelka silikonowa.",null,"216cm","dwu-segmentowy","Oprawa ściemnialna fazowo TRAILING EDGE (TE) - LEADING EDGE (LE)","2 Moduły LED","Cree DK200305 V3 JB2835 3V 3K","TCI Mini MD 12,5W 250mA code 127036 Triac",0,null,0,80,"C","116ZX0009, 117GA0009, 2951ZX0009","Zaciski podłączeniowe: max 3x4mm², możliwość podłączenia oprawy w pętle max 3x2,5mm². Przewód w oponie okrągłej o średnicy max ø12,5 mm.","1360XX0011.jpg","1360XX0011.ldt",1,null,1,27]
["1361","1361XX0009","ASKER POLE PRO LIGHT LUMINAIRES POLE 216CM LED 1099LM VSM 3000K ON/OFF","Asker","Post,Post complete","Aluminium",null,null,"PRO","LED zintegrowane","AC","ON/OFF","6,1W","8,4W","1099lm","1081lm",null,null,"65","IK08","Class I",3000,"szerokie dół",0.11,2.16,0.39,"CE",null,null,">100 000h",20,"Oprawa słupowa (lekka konstrukcja).","Soczewka firmy Ledil typu VSM (IESNA typ V).","VSM","Luminaire for lighting private areas, public spaces, and other architectural concepts","For lighting private areas, parks, and other architectural concepts The wide and even luminous flux Lighting and connection chamber tightness IP65",null,null,"Profil aluminiowy wyciskany, malowany proszkowo.",null,"Soczewka hermetyczna zewnętrzna- tworzywo sztuczne PMMA przeźroczyste.","Uszczelka silikonowa.",null,"216cm","dwu-segmentowy","Oprawa nieściemnialna","Moduł LED","Philips Fortimo FastFlex LED 2x6 DP G5 3K","Philips Xi BP 12 W 0,1-0,5AS 230 V C100",100000,null,null,70,"D","116ZX0009, 117GA0009, 118GA0009, 119ZX0009, 7666ZX0009","Zaciski podłączeniowe: max 3x4mm², możliwość podłączenia oprawy w pętle max 3x4mm². Przewód w oponie okrągłej o średnicy: ø4…8mm, ø8...12mm lub ø10...13,6mm","1361XX0009.jpg","1361XX0009.ldt",4,null,1,47]
["1362","1362XX0009","ASKER POLE PRO LIGHT LUMINAIRES POLE 216CM LED 1158LM VSM 3000K DALI2","Asker","Post,Post complete","Aluminium",null,null,"PRO","LED zintegrowane","AC","DALI2","6,4W","8,5W","1158lm","1081lm",null,null,"65","IK08","Class I",3000,"szerokie dół",0.11,0.39,2.16,"CE",null,"DALI",">100 000h",20,"Oprawa słupowa (lekka konstrukcja).","Soczewka firmy Ledil typu VSM (IESNA typ V).","VSM","For lighting private areas, parks, and other architectural concepts","For lighting private areas, parks, and other architectural concepts The wide and even luminous flux.",null,null,"Profil aluminiowy wyciskany, malowany proszkowo.",null,"Soczewka hermetyczna zewnętrzna- tworzywo sztuczne PMMA przeźroczyste.","Uszczelka silikonowa.",null,"216cm","dwu-segmentowy","Sterowanie światłem w systemie: DALI outdoor pełny program. Zasilacz zaprogramowany na max prąd. Programowanie pozostałych parametrów po uzgodnieniu z Działem Handlowym firmy Norlys.","Moduł LED","Philips Fortimo FastFlex LED 2x6 DP G5 3K","Philips Xi FP 22W 0,2-0,7A SNLDAE 230V S175 sXt",100000,"DALI2 / NightDim (XI FP NLD)",0.01,70,"D","116ZX0009, 117GA0009, 118GA0009, 119ZX0009, 7666ZX0009","Zaciski podłączeniowe: max 5x4mm², możliwość podłączenia oprawy w pętle max 5x2,5mm². Przewód w oponie okrągłej o średnicy: ø4…8mm, ø8...12mm lub ø10...13,6mm","1362XX0009.jpg","1362XX0009.ldt",3,null,1,47]
["1363","1363XX0011","ASKER POLE LIGHT LUMINAIRES POLE 2XLED 1988LM 3000K DIM.","Asker","Post,Post complete","Aluminium",null,null,null,"LED zintegrowane","AC","DIM.","10,6W","12W","1988lm","1128lm",null,null,"65",null,"Class I",3000,"szerokie dół",0,0,0,"CE",null,null,"> 72 000h",20,"Oprawa słupowa (lekka konstrukcja).","Światło jednostronne: symetryczne, ukierunkowane w dół.",null,"For lighting private areas and other architectural concepts",null,null,null,"Profil aluminiowy wyciskany, malowany proszkowo.",null,"Klosz- poliwęglan przeźroczysty ze strukturą, stabilizowany UV.","Uszczelka silikonowa.",null,null,"jedno-segmentowy","Oprawa ściemnialna fazowo TRAILING EDGE (TE) - LEADING EDGE (LE)","2 Moduły LED","Cree DK200305 V3 JB2835 3V 3K","TCI Mini MD 12,5W 250mA code 127036 Triac",0,null,0,80,"C","116ZX0009, 117GA0009, 2951ZX0009","Zaciski podłączeniowe: max 3x4mm², możliwość podłączenia oprawy w pętle max 3x2,5mm². Przewód w oponie okrągłej o średnicy max ø12,5mm.","1363XX0011.jpg","1363XX0011.ldt",1,null,1,27]
["1364","1364XX0009","ASKER POLE PRO LIGHT LUMINAIRES POLE 236CM LED 1099LM VSM 3000K ON/OFF","Asker","Post,Post complete","Aluminium",null,null,"PRO","LED zintegrowane","AC","ON/OFF","6,1W","8,4W","1099lm","1033lm",null,null,"65","IK08","Class I",3000,"szerokie dół",0.24,2.36,0.39,"CE",null,null,">100 000h",20,"Oprawa słupowa (lekka konstrukcja).","Soczewka firmy Ledil typu VSM (IESNA typ V).","VSM","Luminaire for lighting private areas, public spaces, and other architectural concepts",null,null,null,"Profil aluminiowy wyciskany, malowany proszkowo.",null,"Soczewka hermetyczna zewnętrzna- tworzywo sztuczne PMMA przeźroczyste.","Uszczelka silikonowa.",null,"236cm","jedno-segmentowy","Oprawa nieściemnialna","Moduł LED","Philips Fortimo FastFlex LED 2x6 DP G5 3K","Philips Xi BP 12 W 0,1-0,5AS 230 V C100",100000,null,0.01,70,"D","116ZX0009, 117GA0009, 118GA0009, 119ZX0009, 7666ZX0009","Zaciski podłączeniowe: max 3x4mm², możliwość podłączenia oprawy w pętle max 3x4mm². Przewód w oponie okrągłej o średnicy: ø4…8mm, ø8...12mm lub ø10...13,6mm","1364XX0009.jpg","1364XX0009.ldt",4,null,1,47]
["1365","1365XX0009","ASKER POLE PRO LIGHT LUMINAIRES POLE 236CM LED 1158LM VSM 3000K DALI2","Asker","Post,Post complete","Aluminium",null,null,"PRO","LED zintegrowane","AC","DALI2","6,4W","8,5W","1158lm","1085lm",null,null,"65","IK06","Class I",3000,"szerokie dół",0.39,0.11,2.36,"CE",null,"DALI",">100 000h",20,"Oprawa słupowa (lekka konstrukcja).","Soczewka firmy Ledil typu VSM (IESNA typ V).","VSM","Luminaire for lighting private areas, public spaces, and other architectural concepts","For lighting private areas, parks, and other architectural concepts The wide and even luminous flux.",null,null,"Profil aluminiowy wyciskany, malowany proszkowo.",null,"Soczewka hermetyczna zewnętrzna- tworzywo sztuczne PMMA przeźroczyste.","Uszczelka silikonowa.",null,"236cm","jedno-segmentowy","Sterowanie światłem w systemie: DALI outdoor pełny program. Zasilacz zaprogramowany na max prąd. Programowanie pozostałych parametrów po uzgodnieniu z Działem Handlowym firmy Norlys.","Moduł LED","Philips Fortimo FastFlex LED 2x6 DP G5 3K","Philips Xi FP 22W 0,2-0,7A SNLDAE 230V S175 sXt",100000,"DALI2 / NightDim (XI FP NLD)",0.01,70,"D","116ZX0009, 117GA0009, 118GA0009, 119ZX0009, 7666ZX0009","Zaciski podłączeniowe: max 5x4mm², możliwość podłączenia oprawy w pętle max 5x2,5mm². Przewód w oponie okrągłej o średnicy: ø4…8mm, ø8...12mm lub ø10...13,6mm","1365XX0009.jpg","1365XX0009.ldt",3,null,1,47]
["1366","1366XX0009","ASKER POLE PRO LIGHT LUMINAIRES POLE 216CM LED 1099LM T2-L 3000K ON/OFF","Asker","Post,Post complete","Aluminium",null,null,"PRO","LED zintegrowane","AC","ON/OFF","6,1W","8,4W","1099lm","1018lm",null,null,"65","IK08","Class I",3000,"szerokie dół",2.16,0.11,0.39,"CE",null,null,">100 000h",20,"Oprawa słupowa (lekka konstrukcja).","Soczewka firmy Ledil typu T2-L (IESNA typ III).","T2-L","Luminaire for lighting private areas, public spaces, and other architectural concepts","For lighting private areas, parks, and other architectural concepts The wide and even luminous flux ideal for lighting: paths, pavements, etc. Lighting and connection chamber tightness IP65",null,null,"Profil aluminiowy wyciskany, malowany proszkowo.",null,"Soczewka hermetyczna zewnętrzna- tworzywo sztuczne PMMA przeźroczyste.","Uszczelka silikonowa.",null,"216cm","dwu-segmentowy","Oprawa nieściemnialna","Moduł LED","Philips Fortimo FastFlex LED 2x6 DP G5 3K","Philips Xi BP 12 W 0,1-0,5AS 230 V C100",100000,null,0.01,70,"D","116ZX0009, 117GA0009, 118GA0009, 119ZX0009, 7666ZX0009","Zaciski podłączeniowe: max 3x4mm², możliwość podłączenia oprawy w pętle max 3x4mm². Przewód w oponie okrągłej o średnicy: ø4…8mm, ø8...12mm lub ø10...13,6mm","1366XX0009.jpg","1366XX0009.ldt",4,null,1,48]
["1367","1367XX0009","ASKER POLE PRO LIGHT LUMINAIRES POLE 236CM LED 1099LM T2-L 3000K ON/OFF","Asker","Post,Post complete","Aluminium",null,null,"PRO","LED zintegrowane","AC","ON/OFF","6,1W","8,4W","1099lm","1018lm",null,null,"65","IK06","Class I",3000,"szerokie dół",2.36,0.11,0.39,"CE",null,null,">100 000h",20,"Oprawa słupowa (lekka konstrukcja).","Soczewka firmy Ledil typu T2-L (IESNA typ III).","T2-L","Luminaire for lighting private areas, public spaces, and other architectural concepts",null,null,null,"Profil aluminiowy wyciskany, malowany proszkowo.",null,"Soczewka hermetyczna zewnętrzna- tworzywo sztuczne PMMA przeźroczyste.","Uszczelka silikonowa.",null,"236cm","jedno-segmentowy","Oprawa nieściemnialna","Moduł LED","Philips Fortimo FastFlex LED 2x6 DP G5 3K","Philips Xi BP 12 W 0,1-0,5AS 230 V C100",100000,null,0.01,70,"D","116ZX0009, 117GA0009, 118GA0009, 119ZX0009, 7666ZX0009","Zaciski podłączeniowe: max 3x4mm², możliwość podłączenia oprawy w pętle max 3x4mm². Przewód w oponie okrągłej o średnicy: ø4…8mm, ø8...12mm lub ø10...13,6mm","1367XX0009.jpg","1367XX0009.ldt",4,null,1,48]
["1368","1368XX0009","ASKER POLE PRO LIGHT LUMINAIRES POLE 216CM LED 1158LM T2-L 3000K DALI2","Asker","Post,Post complete","Aluminium",null,null,"PRO","LED zintegrowane","AC","DALI2","6,4W","8,7W","1158lm","1018lm",null,null,"65","IK08","Class I",3000,"szerokie dół",3.9,0.24,2.16,"CE",null,"DALI","> 120 000h",20,"Oprawa słupowa (lekka konstrukcja).","Soczewka firmy Ledil typu T2-L (IESNA typ III).","T2-L","For lighting private areas, parks, and other architectural concepts","For lighting private areas, parks, and other architectural concepts, The wide and even luminous flux is ideal for lighting: paths, sidewalks, etc. IP65 for lighting chamber and connections",null,null,"Profil aluminiowy wyciskany, malowany proszkowo.",null,"Soczewka hermetyczna zewnętrzna- tworzywo sztuczne PMMA przeźroczyste.","Uszczelka silikonowa.",null,"216cm","dwu-segmentowy","Sterowanie światłem w systemie: DALI outdoor pełny program. Zasilacz zaprogramowany na max prąd. Programowanie pozostałych parametrów po uzgodnieniu z Działem Handlowym firmy Norlys.","Moduł LED","Philips Fortimo FastFlex LED 2x6 DP G4+ 3K","Philips Xi FP 22W 0,2-0,7A SNLDAE 230V S175 sXt",100000,"DALI2 / NightDim (XI FP NLD)",0.01,70,"D","116ZX0009, 117GA0009, 118GA0009, 119ZX0009, 7666ZX0009","Zaciski podłączeniowe: max 5x4mm², możliwość podłączenia oprawy w pętle max 5x4mm². Przewód w oponie okrągłej o średnicy max ø12,5mm.","1368XX0009.jpg","1368XX0009.ldt",3,null,1,48]
["1369","1369XX0009","ASKER POLE PRO LIGHT LUMINAIRES POLE 236CM LED 1158LM T2-L 3000K DALI2","Asker","Post,Post complete","Aluminium",null,null,"PRO","LED zintegrowane","AC","DALI2","6,4W","8,7W","1158lm","1081lm",null,null,"65","IK06","Class I",3000,"szerokie dół",null,null,null,"CE",null,"DALI","> 120 000h",20,"Oprawa słupowa (lekka konstrukcja).","Soczewka firmy Ledil typu T2-L (IESNA typ III).","T2-L","Luminaire for lighting private areas, public spaces, and other architectural concepts",null,null,null,"Profil aluminiowy wyciskany, malowany proszkowo.",null,"Soczewka hermetyczna zewnętrzna- tworzywo sztuczne PMMA przeźroczyste.","Uszczelka silikonowa.",null,"236cm","jedno-segmentowy","Sterowanie światłem w systemie: DALI outdoor pełny program. Zasilacz zaprogramowany na max prąd. Programowanie pozostałych parametrów po uzgodnieniu z Działem Handlowym firmy Norlys.","Moduł LED","Philips Fortimo FastFlex LED 2x6 DP G4+ 3K","Philips Xi FP 22W 0,2-0,7A SNLDAE 230V S175 sXt",100000,"DALI2 / NightDim (XI FP NLD)",0.01,70,"D","116ZX0009, 117GA0009, 118GA0009, 119ZX0009, 7666ZX0009","Zaciski podłączeniowe: max 5x4mm², możliwość podłączenia oprawy w pętle max 5x4mm². Przewód w oponie okrągłej o średnicy max ø12,5mm.","1369XX0009.jpg","1369XX0009.ldt",3,null,1,48]
["1370","1370XX0010","MANDAL WALL 2XLED GU10 530LM UP25D & DOWN25D 2700K DIM.","Mandal","Wall","Stal",null,null,null,"Wymienne","GU10",null,"7,8W","7,8W","530lm","500lm",null,null,"44","IK08","Class I",2700,"szerokie góra / szerokie dół",0.09,0.12,0.18,"CE",null,null,"40000",12,"Oprawa ścienna.","Światło dwustronne: o kącie 25D do góry i w dół.","Up25D & Down25D","Wall-mounted luminaire with modern design. For lighting private areas and public spaces.",null,null,null,null,"Front- stal cynkowana ogniowo lub stal malowana proszkowo.","Klosz- szkło bezpieczne, przeźroczyste.","Uszczelka silikonowa.","Podstawa- stal cynkowana ogniowo.","góra/dół",null,"Oprawa ściemnialna fazowo TRAILING EDGE (TE) - LEADING EDGE (LE)","2 Lampy LED GU10","Philips MASTER LED ExpertColor 3.9-35W GU10 927 25D",null,0,"Ściemnianie fazowe LED GU10 E27",null,97,"G",null,"Zaciski podłączeniowe: max 3x2,5mm², możliwość podłączenia oprawy w pętle max 3x1,5mm². Przewód w oponie okrągłej o średnicy ø7...10,5mm.","1370XX0010.jpg","1370XX0010.ldt",1,"GU10",1,73]
["1371","1371XX0010","MANDAL WALL 2XLED GU10 UP25D & DOWN25D","Mandal","Wall","Stal",null,null,null,"Wymienne","GU10",null,"2 x max 4W","2 x max 4W",null,null,null,null,"44",null,"Class I",null,"szerokie góra / szerokie dół",0.09,0.12,0.18,"CE",null,null,null,12,"Oprawa ścienna.","Światło dwustronne: o kącie 25D do góry i w dół.","Up25D & Down25D","Wall-mounted luminaire with modern design. For lighting private areas and public spaces.",null,null,"Oprawa na wymienne źródło światła typu lampa LED, o trzonku Gu10. Źródło światła należy dokupić oddzielnie.",null,"Front- stal cynkowana ogniowo lub stal malowana proszkowo.","Klosz- szkło bezpieczne, przeźroczyste.","Uszczelka silikonowa.","Podstawa- stal cynkowana ogniowo.","góra/dół",null,null,"2 Lampy LED GU10","LED PAR16",null,0,null,null,80,null,"46102507","Zaciski podłączeniowe: max 3x2,5mm², możliwość podłączenia oprawy w pętle max 3x1,5mm². Przewód w oponie okrągłej o średnicy ø7...10,5mm.","1371XX0010.jpg","1371XX0010.ldt",4,"GU10",1,73]
["1373","1373XX0010","MANDAL WALL LED GU10 265LM DOWN 25D 2700K DIM.","Mandal","Wall","Stal",null,null,null,"Wymienne","GU10",null,"3,9W","3,9W","265lm","250lm",null,null,"44","IK08","Class I",2700,"szerokie dół",0.12,0.09,0.1,"CE",null,null,"40000",12,"Oprawa ścienna.","Światło jednostronne: ukierunkowane w dół o kącie 25D","Down 25D","Wall-mounted luminaire with modern design. For lighting private areas and public spaces.",null,null,null,null,"Front- stal cynkowana ogniowo lub stal malowana proszkowo.","Klosz- szkło bezpieczne, przeźroczyste.","Uszczelka silikonowa.","Podstawa- stal cynkowana ogniowo.","dół",null,"Oprawa ściemnialna fazowo TRAILING EDGE (TE) - LEADING EDGE (LE)","Lampa LED GU10","Philips MASTER LED ExpertColor 3.9-35W GU10 927 25D",null,0,"Ściemnianie fazowe LED GU10 E27",null,97,"G",null,"Zaciski podłączeniowe: max 3x2,5mm², możliwość podłączenia oprawy w pętle max 3x1,5mm². Przewód w oponie okrągłej o średnicy ø7...10,5mm.","1373XX0010.jpg","1373XX0010.ldt",1,"GU10",1,74]
["1374","1374XX0010","MANDAL WALL LED GU10 DOWN 25D","Mandal","Wall","Stal",null,null,null,"Wymienne","GU10",null,"LED max 4W","LED max 4W",null,null,null,null,"44","IK08","Class I",null,"szerokie dół",0.09,0.12,0.1,"CE",null,null,null,12,"Oprawa ścienna.","Światło jednostronne: ukierunkowane w dół o kącie 25D","Down 25D","Wall-mounted luminaire with modern design. For lighting private areas and public spaces.",null,null,null,null,"Front- stal cynkowana ogniowo lub stal malowana proszkowo.","Klosz- szkło bezpieczne, przeźroczyste.","Uszczelka silikonowa.","Podstawa- stal cynkowana ogniowo.","dół",null,null,"Lampa LED GU10","LED PAR16",null,0,null,null,80,null,"46102507","Zaciski podłączeniowe: max 3x2,5mm², możliwość podłączenia oprawy w pętle max 3x1,5mm². Przewód w oponie okrągłej o średnicy ø7...10,5mm.","1374XX0010.jpg","1374XX0010.ldt",4,"GU10",1,74]
["1380","1380XX0010","LILLESAND BOLLARD 85CM E27","Lillesand","Bollard","Aluminium",null,null,null,"Wymienne","E27",null,"LED max 9W","LED max 9W",null,null,null,null,"55","IK08","Class II",null,null,0.12,0.12,0.85,"CE",null,null,null,1,"Oprawa słupkowa.","Światło obrotowo-symetryczne.",null,"Luminaire with a contemporary design For lighting gardens and other private and public areas","A bollard luminaire with a stable and durable construction For lighting private and public areas Functions: control, color change 2700K…6500K (TW), WiZ, WiZ Pro. - Available after mounting in the luminaire, Signify WiZ Pro A60 E27 TW 8W lamps 230V - Full control of the luminaire after installing the free application https://pro.wizconnected.com/ - Technical support: Information Sales Department of Norlys",null,null,"Odlew aluminiowy malowany proszkowo.",null,"Klosz- tworzywo sztuczne PMMA satynowane.","Uszczelka silikonowa.","Dławnica nylon6.","85cm",null,null,"Lampa E27","LED A55..60",null,0,null,null,80,null,"205ZX0010, 206GA0010, 206GA0S10, 46999021, 4699990100, 4699990101","Zaciski podłączeniowe: max 2x2,5mm², możliwość podłączenia oprawy w pętle max 2x2,5mm². Przewód w oponie okrągłej o średnicy ø7...10,5mm.","1380XX0010.jpg","1380XX0010.ldt",4,"E27",1,17]
["1382","1382XX0010","LILLESAND BOLLARD 85CM LED E27 806LM 2700K DIM.","Lillesand","Bollard","Aluminium",null,null,null,"Wymienne","E27",null,"5,9W","5,9W","~806lm","495lm",null,null,"55","IK08","Class II",2700,null,0.12,0.12,0.85,"CE",null,null,"25000",1,"Oprawa słupkowa.","Światło obrotowo-symetryczne.",null,"Modern design luminaire. For lighting gardens, private areas and public spaces.",null,null,null,"Odlew aluminiowy malowany proszkowo.",null,"Klosz- tworzywo sztuczne PMMA satynowane.","Uszczelka silikonowa.","Dławnica nylon6.","85cm",null,"Oprawa ściemnialna fazowo TRAILING EDGE (TE) - LEADING EDGE (LE)","Lampa LED E27","Philips MAS LEDBulb DT5.9-60W E27 927 A60 FR G",null,0,"Ściemnianie fazowe LED GU10 E27",null,80,"F","205ZX0010, 206GA0010, 206GA0S10","Zaciski podłączeniowe: max 2x2,5mm², możliwość podłączenia oprawy w pętle max 2x2,5mm². Przewód w oponie okrągłej o średnicy ø8...12,5mm.","1382XX0010.jpg","1382XX0010.ldt",1,"E27",1,17]
["1383","1383XX0009","LILLESAND BOLLARD 49CM LED E27","Lillesand","Bollard","Aluminium",null,null,null,"Wymienne","E27",null,"LED max 9W","LED max 9W",null,null,null,null,"55","IK08","Class II",null,null,0.49,0.12,0.12,"CE",null,null,null,1,"Oprawa słupkowa.","Światło obrotowo-symetryczne.",null,"A luminaire with a contemporary design. For lighting gardens and other private areas.",null,null,null,"Odlew aluminiowy malowany proszkowo.",null,"Klosz- tworzywo sztuczne PMMA satynowane.","Uszczelka silikonowa.","Dławnica nylon6.","49cm",null,null,"Lampa LED E27","LED E27 A55..60",null,0,null,null,80,null,"205ZX0010, 206GA0010, 206GA0S10, 46999021","Zaciski podłączeniowe: max 2x2,5mm², możliwość podłączenia oprawy w pętle max 2x2,5mm². Przewód w oponie okrągłej o średnicy ø7...12,5mm.","1383XX0009.jpg","1383XX0009.ldt",4,"E27",1,17]
["1384","1384XX0009","LILLESAND BOLLARD 49CM LED E27 806LM 2700K DIM.","Lillesand","Bollard","Aluminium",null,null,null,"Wymienne","E27",null,"8W","8W","806lm","495lm",null,null,"65","IK08","Class II",2700,null,0.12,0.12,0.49,"CE",null,null,"25 000h",1,"Oprawa słupkowa.","Światło obrotowo-symetryczne.",null,"Luminaire with a contemporary design. For lighting gardens, private areas, and for other architectural uses",null,null,null,"Odlew aluminiowy malowany proszkowo.",null,"Klosz- tworzywo sztuczne PMMA satynowane.","Uszczelka silikonowa.",null,"49cm",null,"Oprawa ściemnialna fazowo TRAILING EDGE (TE) - LEADING EDGE (LE)","Lampa LED E27","Philips Master LEDbulb DT 8-60W E27 A60 CL 806lm/827",null,0,"Ściemnianie fazowe LED GU10 E27",null,80,"F","205ZX0010, 206GA0010, 206GA0S10, 2951ZX0009","Zaciski podłączeniowe: max 2x4mm², możliwość podłączenia oprawy w pętle max 2x2,5mm². Przewód w oponie okrągłej o średnicy ø8...12,5mm.","1384XX0009.png","1384XX0009.ldt",1,"E27",1,17]
["1390","1390XX0011","SKI WALL-CONNECTORS LED 653LM DOWN 3000K DIM.","Ski","Wall","Stal",null,null,null,"LED zintegrowane","AC","DIM.","4W","5,2W","653lm","371lm",null,null,"44","IK09","Class I",3000,"szerokie dół",0.2,0.14000000000000001,0.13,"CE",null,null,"70000",19,"Oprawa ścienna- dystrybutor energii.","Światło rozproszone półsferyczne ukierunkowane w dół",null,"Wall luminaire and 220 ... 240V electricity distributor. For lighting private areas and other applications","Wall luminaire and 220 ... 240V electricity distributor. For lighting private areas and other applications. Luminaire equipped with: - two F-type sockets (SCHUKO) with a maximum total load of 16A",null,null,null,"Front- stal cynkowana ogniowo lub stal malowana proszkowo.","Klosz- poliwęglan przeźroczysty ze strukturą, stabilizowany UV.","Uszczelka silikonowa.","Podstawa- stal cynkowana ogniowo.",null,"F (SCHUKO)","Oprawa ściemnialna fazowo TRAILING EDGE (TE)","Moduł LED","Philips Fortimo_LED_Strip_0.5ft_MF_8xx_HV6 3K","Philips Xitanium 7W 0,35A 20V TE SC 230V [2017]",50000,null,null,80,"C",null,"Zaciski podłączeniowe: max 3x2,5mm². Przewód w oponie okrągłej o średnicy ø7...10,5mm.","1390XX0011.jpg","1390XX0011.ldt",1,null,1,76]
["1392","1392XX0010","SKI WALL LED 653LM DOWN 3000K DIM.","Ski","Wall","Stal",null,null,null,"LED zintegrowane","AC","DIM.","4W","5,2W","653lm","346lm",null,null,"44","IK09","Class I",3000,"szerokie dół",0.2,0.14000000000000001,0.13,"CE",null,null,"> 70000",12,"Oprawa ścienna.","Światło rozproszone półsferyczne ukierunkowane w dół",null,"A luminaire with a wide range of applications, used for general and decorative lighting of wall surfaces, facades, and other architectural concepts",null,null,null,null,"Front- stal cynkowana ogniowo lub stal malowana proszkowo.","Klosz- poliwęglan przeźroczysty ze strukturą, stabilizowany UV.","Uszczelka silikonowa.","Podstawa- stal cynkowana ogniowo.",null,null,"Oprawa ściemnialna fazowo TRAILING EDGE (TE)","Moduł LED","Philips Fortimo_LED_Strip_0.5ft_MF_8xx_HV6 3K","Philips Xitanium 7W 0,35A 20V TE SC 230V [2017]",50000,null,null,80,"C",null,"Zaciski podłączeniowe: max 3x2,5mm², możliwość podłączenia oprawy w pętle max 3x1,5mm². Przewód w oponie okrągłej o średnicy ø7...10,5mm.","1392XX0010.jpg","1392XX0010.ldt",1,null,1,76]
["1400","1400XX0010","HALMSTAD BOLLARD 49CM E27","Halmstad,Wood","Bollard","Drewno","Malowane",null,null,"Wymienne","E27",null,"LED max 9W","LED max 9W",null,null,null,null,"65","IK10","Class II",null,null,0.49,0.12,0.12,"CE",null,null,null,1,"Oprawa słupkowa.","Światło odkryte, częściowo przysłonięte od góry.",null,"Bollard luminaire of stable and durable construction For lighting private areas and public spaces","Bollard luminaire of stable and durable construction For lighting private areas and public spaces Functions: control, color change 2700K…6500K (TW), WiZ, WiZ Pro - Available after mounting in the luminaire, Signify WiZ Pro A60 E27 TW 8W 230V - Full control of the luminaire after installing the free application https://pro.wizconnected.com/ - Technical support: Information Sales Department of Norlys",null,null,"Drewno- sosna skandynawska malowana i stal cynkowana ogniowo.","Drewno- sosna skandynawska malowana, stal cynkowana ogniowo i malowana proszkowo.","Klosz- tworzywo sztuczne PMMA w kolorze mlecznym.","Uszczelka silikonowa.",null,"49cm","Drewno malowane",null,"Lampa E27","LED A55..60",null,0,null,null,80,null,"205ZX0010, 206GA0010, 206GA0S10","Zaciski podłączeniowe: max 3x2,5mm², możliwość podłączenia oprawy w pętle max 3x1,5mm². Przewód w oponie okrągłej o średnicy max ø12,5mm.","1400XX0010.jpg","1400XX0010.ldt",4,"E27",1,23]
["1403","1403XX0010","HALMSTAD BOLLARD 49CM E27","Halmstad","Bollard","Drewno","Impregnowane",null,null,"Wymienne","E27",null,"LED max 9W","LED max 9W",null,null,null,null,"65","IK10","Class II",null,null,null,null,null,"CE",null,null,null,1,"Oprawa słupkowa.","Światło odkryte, częściowo przysłonięte od góry.",null,"Bollard luminaire of stable and durable construction. For lighting private areas and public spaces.",null,null,"Oprawa na wymienne źródło światła typu: lampa LED, świetlówka TC-SE, tradycyjna żarówka (halogenowa) o trzonku E27. Źródło światła należy dokupić oddzielnie.","Drewno- sosna skandynawska impregnowana i stal cynkowana ogniowo.","Drewno- sosna skandynawska impregnowana, stal cynkowana ogniowo i malowana proszkowo.","Klosz- tworzywo sztuczne PMMA w kolorze mlecznym.","Uszczelka silikonowa.",null,"49cm","Drewno impregnowane",null,"Lampa E27","LED A55..60",null,0,null,null,80,null,"205ZX0010, 206GA0010, 206GA0S10","Zaciski podłączeniowe: max 3x2,5mm², możliwość podłączenia oprawy w pętle max 3x1,5mm². Przewód w oponie okrągłej o średnicy max ø12,5mm.","1403XX0010.jpg","1403XX0010.ldt",4,"E27",1,23]
["1407","1407XX0009","HALMSTAD BOLLARD 49CM LED 1059LM 3000K DIM.","Halmstad,Wood","Bollard","Drewno","Impregnowane",null,null,"LED zintegrowane","AC","DIM.","6,7W","8,5W","1059lm","292lm",null,null,"65","IK10","Class II",3000,null,0,0,0,"CE",null,null,"> 50 000h",1,"Oprawa słupkowa.","Światło odkryte, częściowo przysłonięte od góry.",null,"A bollard luminaire with a stable and durable structure For lighting private areas and other architectural concepts",null,null,null,"Drewno- sosna skandynawska impregnowana i stal cynkowana ogniowo.","Drewno- sosna skandynawska impregnowana, stal cynkowana ogniowo i malowana proszkowo.","Klosz- tworzywo sztuczne PMMA w kolorze mlecznym.","Uszczelka silikonowa.",null,"49cm",null,"Oprawa ściemnialna fazowo TRAILING EDGE (TE) - LEADING EDGE (LE)","Moduł LED","Philips Fortimo SLM C 1203 L09 1619 G7 3K","KGP CC10W180-270CG",50000,"Dim. TRIAC (KGP)",null,80,"D","205ZX0010, 206GA0010, 206GA0S10","Zaciski podłączeniowe: max 2x4mm², możliwość podłączenia oprawy w pętle max 2x4mm². Przewód w oponie okrągłej o średnicy max ø12,5mm.","1407XX0009.png","1407XX0009.ldt",1,null,1,23]
["1409","1409XX0009","HALMSTAD BOLLARD 49CM LED 1059LM 3000K DIM.","Halmstad,Wood","Bollard","Drewno","Malowane",null,null,"LED zintegrowane","AC","DIM.","6,7W","8,5W","1059lm","292lm",null,null,"65","IK10","Class II",3000,null,0,0,0,"CE",null,null,"> 50 000h",1,"Oprawa słupkowa.","Światło odkryte, częściowo przysłonięte od góry.",null,"A bollard luminaire with a stable and durable structure For lighting private areas and other architectural concepts",null,null,null,"Drewno- sosna skandynawska malowana i stal cynkowana ogniowo.","Drewno- sosna skandynawska malowana, stal cynkowana ogniowo i malowana proszkowo.","Klosz- tworzywo sztuczne PMMA w kolorze mlecznym.","Uszczelka silikonowa.",null,"49cm",null,"Oprawa ściemnialna fazowo TRAILING EDGE (TE) - LEADING EDGE (LE)","Moduł LED","Philips Fortimo SLM C 1203 L09 1619 G7 3K","KGP CC10W180-270CG",50000,"Dim. TRIAC (KGP)",null,80,"D","205ZX0010, 206GA0010, 206GA0S10","Zaciski podłączeniowe: max 2x4mm², możliwość podłączenia oprawy w pętle max 2x4mm². Przewód w oponie okrągłej o średnicy max ø12,5mm.","1409XX0009.png","1409XX0009.ldt",1,null,1,23]
["1410","1410XX0010","HALMSTAD BOLLARD 85CM E27","Halmstad,Wood","Bollard","Drewno","Malowane",null,null,"Wymienne","E27",null,"LED max 9W","LED max 9W",null,null,null,null,"65","IK10","Class II",null,null,null,null,null,"CE",null,null,null,1,"Oprawa słupkowa.","Światło odkryte, częściowo przysłonięte od góry.",null,"Bollard luminaire of stable and durable construction For lighting private areas and public spaces","Bollard luminaire of stable and durable construction For lighting private and public areas Functions: control, color change 2700K…6500K (TW), WiZ, WiZ Pro - Available after mounting in the luminaire, Signify WiZ Pro A60 E27 TW 8W 230V - Full control of the luminaire after installing the free application https://pro.wizconnected.com/ - Technical support: Information Sales Department of Norlys",null,null,"Drewno- sosna skandynawska malowana i stal cynkowana ogniowo.","Drewno- sosna skandynawska malowana, stal cynkowana ogniowo i malowana proszkowo.","Klosz- tworzywo sztuczne PMMA w kolorze mlecznym.","Uszczelka silikonowa.",null,"85cm","Drewno malowane",null,"Lampa E27","LED A55..60",null,0,"Cataloge E27 TW Wiz Pro",null,80,null,"205ZX0010, 206GA0010, 206GA0S10, 46999021","Zaciski podłączeniowe: max 3x2,5mm², możliwość podłączenia oprawy w pętle max 3x1,5mm². Przewód w oponie okrągłej o średnicy max ø12,5mm.","1410XX0010.jpg","1410XX0010.ldt",4,"E27",1,23]
["1413","1413XX0010","HALMSTAD BOLLARD 85CM E27","Halmstad","Bollard","Drewno","Impregnowane",null,null,"Wymienne","E27",null,"LED max 9W","LED max 9W",null,null,null,null,"65","IK10","Class II",null,null,null,null,null,"CE",null,null,null,1,"Oprawa słupkowa.","Światło odkryte, częściowo przysłonięte od góry.",null,"Bollard luminaire of stable and durable construction. For lighting private areas and public spaces.",null,null,"Oprawa na wymienne źródło światła typu: lampa LED, świetlówka TC-SE, tradycyjna żarówka (halogenowa) o trzonku E27. Źródło światła należy dokupić oddzielnie.","Drewno- sosna skandynawska impregnowana i stal cynkowana ogniowo.","Drewno- sosna skandynawska impregnowana, stal cynkowana ogniowo i malowana proszkowo.","Klosz- tworzywo sztuczne PMMA w kolorze mlecznym.","Uszczelka silikonowa.",null,"85cm","Drewno impregnowane",null,"Lampa E27","LED A55..60",null,0,null,null,80,null,"205ZX0010, 206GA0010, 206GA0S10","Zaciski podłączeniowe: max 3x2,5mm², możliwość podłączenia oprawy w pętle max 3x1,5mm². Przewód w oponie okrągłej o średnicy max ø12,5mm.","1413XX0010.jpg","1413XX0010.ldt",4,"E27",1,23]
["1417","1417XX0009","HALMSTAD BOLLARD 85CM LED 1059LM 3000K DIM.","Halmstad,Wood","Bollard","Drewno","Impregnowane",null,null,"LED zintegrowane","AC","DIM.","6,7W","8,5W","1059lm","292lm",null,null,"65",null,"Class II",3000,null,0,0,0,"CE",null,null,"> 50 000h",1,"Oprawa słupkowa.","Światło odkryte, częściowo przysłonięte od góry.",null,"A bollard luminaire with a stable and durable structure For lighting private areas and other architectural concepts",null,null,null,"Drewno- sosna skandynawska impregnowana i stal cynkowana ogniowo.","Drewno- sosna skandynawska impregnowana, stal cynkowana ogniowo i malowana proszkowo.","Klosz- tworzywo sztuczne PMMA w kolorze mlecznym.","Uszczelka silikonowa.",null,"85cm",null,"Oprawa ściemnialna fazowo TRAILING EDGE (TE) - LEADING EDGE (LE)","Moduł LED","Philips Fortimo SLM C 1203 L09 1619 G7 3K","KGP CC10W180-270CG",50000,"Dim. TRIAC (KGP)",null,80,"D","205ZX0010, 206GA0010, 206GA0S10","Zaciski podłączeniowe: max 2x4mm², możliwość podłączenia oprawy w pętle max 2x4mm². Przewód w oponie okrągłej o średnicy max ø12,5mm.","1417XX0009.png","1417XX0009.ldt",1,null,1,23]
["1419","1419XX0009","HALMSTAD BOLLARD 85CM LED 1059LM 3000K DIM.","Halmstad,Wood","Bollard","Drewno","Malowane",null,null,"LED zintegrowane","AC","DIM.","6,7W","8,5W","1059lm","292lm",null,null,"65",null,"Class II",3000,null,0,0,0,"CE",null,null,"> 50 000h",1,"Oprawa słupkowa.","Światło odkryte, częściowo przysłonięte od góry.",null,"A bollard luminaire with a stable and durable structure For lighting private areas and other architectural concepts",null,null,null,"Drewno- sosna skandynawska malowana i stal cynkowana ogniowo.","Drewno- sosna skandynawska malowana, stal cynkowana ogniowo i malowana proszkowo.","Klosz- tworzywo sztuczne PMMA w kolorze mlecznym.","Uszczelka silikonowa.",null,"85cm",null,"Oprawa ściemnialna fazowo TRAILING EDGE (TE) - LEADING EDGE (LE)","Moduł LED","Philips Fortimo SLM C 1203 L09 1619 G7 3K","KGP CC10W180-270CG",50000,"Dim. TRIAC (KGP)",null,80,"D","205ZX0010, 206GA0010, 206GA0S10","Zaciski podłączeniowe: max 2x4mm², możliwość podłączenia oprawy w pętle max 2x4mm². Przewód w oponie okrągłej o średnicy max ø12,5mm.","1419XX0009.png","1419XX0009.ldt",1,null,1,23]
["1420","1420XX0010","STOCKHOLM BOLLARD 85CM E27","Stockholm,Wood","Bollard","Drewno","Malowane",null,null,"Wymienne","E27",null,"LED max 9W","LED max 9W",null,null,null,null,"65","IK10","Class II",null,null,0.17,0.17,0.85,"CE",null,null,null,1,"Oprawa słupkowa.","Światło odkryte, rozproszone z obrotowo- symetrycznym rozsyłem światła.",null,"Bollard luminaire of stable and durable construction. For lighting private areas and public spaces.",null,null,"Oprawa na wymienne źródło światła typu: lampa LED, świetlówka TC-SE, tradycyjna żarówka (halogenowa) o trzonku E27. Źródło światła należy dokupić oddzielnie.","Drewno- sosna skandynawska malowana i stal cynkowana ogniowo.","Drewno- sosna skandynawska malowana, stal cynkowana ogniowo i malowana proszkowo.","Klosz- tworzywo sztuczne PMMA w kolorze mlecznym.","Uszczelka silikonowa.",null,"85cm","Drewno malowane",null,"Lampa E27","LED A55..60",null,0,null,null,80,null,"205ZX0010, 206GA0010, 206GA0S10","Zaciski podłączeniowe: max 3x2,5mm², możliwość podłączenia oprawy w pętle max 3x1,5mm². Przewód w oponie okrągłej o średnicy max ø12,5mm.","1420XX0010.jpg","1420XX0010.ldt",4,"E27",1,24]
["1423","1423XX0010","STOCKHOLM BOLLARD 85CM E27","Stockholm,Wood","Bollard","Drewno","Impregnowane",null,null,"Wymienne","E27",null,"LED max 9W","LED max 9W",null,null,null,null,"65","IK10","Class II",null,null,0.17,0.17,0.85,"CE",null,null,null,1,"Oprawa słupkowa.","Światło odkryte, rozproszone z obrotowo- symetrycznym rozsyłem światła.",null,"Bollard luminaire of stable and durable construction. For lighting private areas and public spaces.",null,null,"Oprawa na wymienne źródło światła typu: lampa LED, świetlówka TC-SE, tradycyjna żarówka (halogenowa) o trzonku E27. Źródło światła należy dokupić oddzielnie.","Drewno- sosna skandynawska impregnowana i stal cynkowana ogniowo.","Drewno- sosna skandynawska impregnowana, stal cynkowana ogniowo i malowana proszkowo.","Klosz- tworzywo sztuczne PMMA w kolorze mlecznym.","Uszczelka silikonowa.",null,"85cm","Drewno impregnowane",null,"Lampa E27","LED A55..60",null,0,null,null,80,null,"205ZX0010, 206GA0010, 206GA0S10","Zaciski podłączeniowe: max 3x2,5mm², możliwość podłączenia oprawy w pętle max 3x1,5mm². Przewód w oponie okrągłej o średnicy max ø12,5mm.","1423XX0010.jpg","1423XX0010.ldt",4,"E27",1,24]
["1426","1426XX0009","STOCKHOLM BOLLARD 85CM LED 1059LM 3000K DIM.","Stockholm,Wood","Bollard","Drewno","Impregnowane",null,null,"LED zintegrowane","AC","DIM.","6,7W","8,5W","1059lm","342lm",null,null,"65",null,"Class II",3000,null,0.17,0.17,0.85,"CE",null,null,"> 50 000h",1,"Oprawa słupkowa.","Światło odkryte, rozproszone z obrotowo- symetrycznym rozsyłem światła.",null,"A bollard luminaire with a stable and durable structure For lighting gardens, private areas, and other architectural applications",null,null,null,"Drewno- sosna skandynawska impregnowana i stal cynkowana ogniowo.","Drewno- sosna skandynawska impregnowana, stal cynkowana ogniowo i malowana proszkowo.","Klosz- tworzywo sztuczne PMMA w kolorze mlecznym.","Uszczelka silikonowa.",null,"85cm","Drewno impregnowane","Oprawa ściemnialna fazowo TRAILING EDGE (TE) - LEADING EDGE (LE)","Moduł LED","Philips Fortimo SLM C 1203 L09 1619 G7 3K","KGP CC10W180-270CG",50000,"Dim. TRIAC (KGP)",null,80,"D","205ZX0010, 206GA0010, 206GA0S10","Zaciski podłączeniowe: max 2x4mm², możliwość podłączenia oprawy w pętle max 2x4mm². Przewód w oponie okrągłej o średnicy max ø12,5mm.","1426XX0009.png","1426XX0009.ldt",1,null,1,24]
["1429","1429XX0009","STOCKHOLM BOLLARD 85CM LED 1059LM 3000K DIM.","Stockholm,Wood","Bollard","Drewno","Malowane",null,null,"LED zintegrowane","AC","DIM.","6,7W","8,5W","1059lm","342lm",null,null,"65",null,"Class II",3000,null,0.17,0.17,0.85,"CE",null,null,"> 50 000h",1,"Oprawa słupkowa.","Światło odkryte, rozproszone z obrotowo- symetrycznym rozsyłem światła.",null,"A bollard luminaire with a stable and durable structure For lighting gardens, private areas, and other architectural applications",null,null,null,"Drewno- sosna skandynawska malowana i stal cynkowana ogniowo.","Drewno- sosna skandynawska malowana, stal cynkowana ogniowo i malowana proszkowo.","Klosz- tworzywo sztuczne PMMA w kolorze mlecznym.","Uszczelka silikonowa.",null,"85cm","Drewno malowane","Oprawa ściemnialna fazowo TRAILING EDGE (TE) - LEADING EDGE (LE)","Moduł LED","Philips Fortimo SLM C 1203 L09 1619 G7 3K","KGP CC10W180-270CG",50000,"Dim. TRIAC (KGP)",null,80,"D","205ZX0010, 206GA0010, 206GA0S10","Zaciski podłączeniowe: max 2x4mm², możliwość podłączenia oprawy w pętle max 2x4mm². Przewód w oponie okrągłej o średnicy max ø12,5mm.","1429XX0009.png","1429XX0009.ldt",1,null,1,24]
["1430","1430XX0010","STOCKHOLM BOLLARD 49CM E27","Stockholm,Wood","Bollard","Drewno","Malowane",null,null,"Wymienne","E27",null,"LED max 9W","LED max 9W",null,null,null,null,"65","IK10","Class II",null,null,0.17,0.17,0.49,"CE",null,null,null,1,"Oprawa słupkowa.","Światło odkryte, rozproszone z obrotowo- symetrycznym rozsyłem światła.",null,"Bollard luminaire of stable and durable construction. For lighting private areas and public spaces.",null,null,"Oprawa na wymienne źródło światła typu: lampa LED, świetlówka TC-SE, tradycyjna żarówka (halogenowa) o trzonku E27. Źródło światła należy dokupić oddzielnie.","Drewno- sosna skandynawska malowana i stal cynkowana ogniowo.","Drewno- sosna skandynawska malowana, stal cynkowana ogniowo i malowana proszkowo.","Klosz- tworzywo sztuczne PMMA w kolorze mlecznym.","Uszczelka silikonowa.",null,"49cm","Drewno malowane",null,"Lampa E27","LED A55..60",null,0,null,null,80,null,"205ZX0010, 206GA0010, 206GA0S10","Zaciski podłączeniowe: max 3x2,5mm², możliwość podłączenia oprawy w pętle max 3x1,5mm². Przewód w oponie okrągłej o średnicy max ø12,5mm.","1430XX0010.jpg","1430XX0010.ldt",4,"E27",1,24]
["1433","1433XX0010","STOCKHOLM BOLLARD 49CM E27","Stockholm,Wood","Bollard","Drewno","Impregnowane",null,null,"Wymienne","E27",null,"LED max 9W","LED max 9W",null,null,null,null,"65","IK10","Class II",null,null,0.17,0.17,0.49,"CE",null,null,null,1,"Oprawa słupkowa.","Światło odkryte z obrotowo-symetrycznym rozsyłem światła.",null,"A bollard luminaire with a stable and durable structure. For lighting private areas and public areas",null,null,"Oprawa na wymienne źródło światła typu: lampa LED, świetlówka TC-SE, tradycyjna żarówka (halogenowa) o trzonku E27. Źródło światła należy dokupić oddzielnie.","Drewno- sosna skandynawska impregnowana i stal cynkowana ogniowo.","Drewno- sosna skandynawska impregnowana, stal cynkowana ogniowo i malowana proszkowo.","Klosz- tworzywo sztuczne PMMA w kolorze mlecznym.","Uszczelka silikonowa.",null,"49cm","Drewno impregnowane",null,"Lampa E27","LED A55..60",null,0,null,null,80,null,"205ZX0010, 206GA0010, 206GA0S10","Zaciski podłączeniowe: max 3x2,5mm², możliwość podłączenia oprawy w pętle max 3x1,5mm². Przewód w oponie okrągłej o średnicy max ø12,5mm.","1433XX0010.jpg","1433XX0010.ldt",4,"E27",1,26]
["1436","1436XX0009","STOCKHOLM BOLLARD 49CM LED 1059LM 3000K DIM.","Stockholm,Wood","Bollard","Drewno","Impregnowane",null,null,"LED zintegrowane","AC","DIM.","6,7W","8,5W","1059lm","342lm",null,null,"65",null,"Class II",3000,null,0.17,0.17,0.49,"CE",null,null,"> 50 000h",1,"Oprawa słupkowa.","Światło odkryte, rozproszone z obrotowo- symetrycznym rozsyłem światła.",null,"A bollard luminaire with a stable and durable structure For lighting gardens, private areas, parks, and other concepts architectural",null,null,null,"Drewno- sosna skandynawska impregnowana i stal cynkowana ogniowo.","Drewno- sosna skandynawska impregnowana, stal cynkowana ogniowo i malowana proszkowo.","Klosz- tworzywo sztuczne PMMA w kolorze mlecznym.","Uszczelka silikonowa.",null,"49cm","Drewno impregnowane","Oprawa ściemnialna fazowo TRAILING EDGE (TE) - LEADING EDGE (LE)","Moduł LED","Philips Fortimo SLM C 1203 L09 1619 G7 3K","KGP CC10W180-270CG",50000,"Dim. TRIAC (KGP)",null,80,"D","205ZX0010, 206GA0010, 206GA0S10","Zaciski podłączeniowe: max 2x4mm², możliwość podłączenia oprawy w pętle max 2x4mm². Przewód w oponie okrągłej o średnicy max ø12,5mm.","1436XX0009.png","1436XX0009.ldt",1,null,1,24]
["1439","1439XX0009","STOCKHOLM BOLLARD 49CM LED 1059LM 3000K DIM.","Stockholm,Wood","Bollard","Drewno","Malowane",null,null,"LED zintegrowane","AC","DIM.","6,7W","8,5W","1059lm","342lm",null,null,"65",null,"Class II",3000,null,0,0,0,"CE",null,null,"> 50 000h",1,"Oprawa słupkowa.","Światło odkryte, rozproszone z obrotowo- symetrycznym rozsyłem światła.",null,"A bollard luminaire with a stable and durable structure For lighting gardens, private areas, parks, and other concepts architectural",null,null,null,"Drewno- sosna skandynawska malowana i stal cynkowana ogniowo.","Drewno- sosna skandynawska malowana, stal cynkowana ogniowo i malowana proszkowo.","Klosz- tworzywo sztuczne PMMA w kolorze mlecznym.","Uszczelka silikonowa.",null,"49cm","mleczny","Oprawa ściemnialna fazowo TRAILING EDGE (TE) - LEADING EDGE (LE)","Moduł LED","Philips Fortimo SLM C 1203 L09 1619 G7 3K","KGP CC10W180-270CG",50000,"Dim. TRIAC (KGP)",null,80,"D","205ZX0010, 206GA0010, 206GA0S10","Zaciski podłączeniowe: max 2x4mm², możliwość podłączenia oprawy w pętle max 2x4mm². Przewód w oponie okrągłej o średnicy max ø12,5mm.","1439XX0009.png","1439XX0009.ldt",1,null,1,24]
["1440","1440XX0010","ALTA BOLLARD 85CM E27","Alta,Wood","Bollard","Drewno","Malowane",null,null,"Wymienne","E27",null,"LED max 9W","LED max 9W",null,null,"Tworzywo sztuczne","Mleczny","65","IK10","Class II",null,null,0.15,0.15,0.85,"CE",null,null,null,1,"Oprawa słupkowa.","Światło obrotowo symetryczne przysłonięte od góry.",null,"Bollard luminaire of stable and durable construction. For lighting private areas and public spaces.",null,null,"Oprawa na wymienne źródło światła typu: lampa LED, świetlówka TC-SE, tradycyjna żarówka (halogenowa) o trzonku E27. Źródło światła należy dokupić oddzielnie.","Drewno- sosna skandynawska malowana i stal cynkowana ogniowo.","Drewno- sosna skandynawska malowana, stal cynkowana ogniowo i malowana proszkowo.","Klosz- tworzywo sztuczne PMMA w kolorze mlecznym.","Uszczelka silikonowa.",null,"85cm","Drewno malowane",null,"Lampa E27","LED A55..60",null,0,null,null,80,null,"205ZX0010, 206GA0010, 206GA0S10, 46999021","Zaciski podłączeniowe: max 3x2,5mm², możliwość podłączenia oprawy w pętle max 3x1,5mm². Przewód w oponie okrągłej o średnicy max ø12,5mm.","1440XX0010.jpg","1440XX0010.ldt",4,"E27",1,1]
["1443","1443XX0010","ALTA BOLLARD 85CM E27","Alta","Bollard","Drewno","Impregnowane",null,null,"Wymienne","E27",null,"LED max 9W","LED max 9W",null,null,null,null,"65","IK10","Class II",null,null,0.15,0.15,0.85,"CE",null,null,null,1,"Oprawa słupkowa.","Światło obrotowo symetryczne przysłonięte od góry.",null,"Bollard luminaire of stable and durable construction. For lighting private areas and public spaces.",null,null,null,"Drewno- sosna skandynawska impregnowana i stal cynkowana ogniowo.","Drewno- sosna skandynawska impregnowana, stal cynkowana ogniowo i malowana proszkowo.","Klosz- tworzywo sztuczne PMMA w kolorze mlecznym.","Uszczelka silikonowa.",null,"85cm","Drewno impregnowane",null,"Lampa E27","LED A55..60",null,0,null,null,80,null,"205ZX0010, 206GA0010, 206GA0S10, 46999021","Zaciski podłączeniowe: max 3x2,5mm², możliwość podłączenia oprawy w pętle max 3x1,5mm². Przewód w oponie okrągłej o średnicy max ø12,5mm.","1443XX0010.jpg","1443XX0010.ldt",4,"E27",1,1]
["1450","1450XX0010","ALTA BOLLARD 49CM E27","Alta,Wood","Bollard","Drewno","Malowane",null,null,"Wymienne","E27",null,"LED max 9W","LED max 9W",null,null,null,null,"65","IK10","Class II",null,null,0.15,0.15,0.49,"CE",null,null,null,1,"Oprawa słupkowa.","Światło obrotowo symetryczne przysłonięte od góry.",null,"Bollard luminaire of stable and durable construction. For lighting private areas and public spaces.",null,null,null,"Drewno- sosna skandynawska malowana i stal cynkowana ogniowo.","Drewno- sosna skandynawska malowana, stal cynkowana ogniowo i malowana proszkowo.","Klosz- tworzywo sztuczne PMMA w kolorze mlecznym.","Uszczelka silikonowa.",null,"49cm","Drewno malowane",null,"Lampa E27","LED A55..60",null,0,null,null,80,null,"205ZX0010, 206GA0010, 206GA0S10, 46999021","Zaciski podłączeniowe: max 3x2,5mm², możliwość podłączenia oprawy w pętle max 3x1,5mm². Przewód w oponie okrągłej o średnicy max ø12,5mm.","1450XX0010.jpg","1450XX0010.ldt",4,"E27",1,1]
["1453","1453XX0010","ALTA BOLLARD 49CM E27","Alta","Bollard","Drewno","Impregnowane",null,null,"Wymienne","E27",null,"LED max 9W","LED max 9W",null,null,null,null,"65","IK10","Class II",null,null,0.15,0.15,0.49,"CE",null,null,null,1,"Oprawa słupkowa.","Światło obrotowo symetryczne przysłonięte od góry.",null,"Bollard luminaire of stable and durable construction. For lighting private areas and public spaces.",null,null,"Oprawa na wymienne źródło światła typu: lampa LED, świetlówka TC-SE, tradycyjna żarówka (halogenowa) o trzonku E27. Źródło światła należy dokupić oddzielnie.","Drewno- sosna skandynawska impregnowana i stal cynkowana ogniowo.","Drewno- sosna skandynawska impregnowana, stal cynkowana ogniowo i malowana proszkowo.","Klosz- tworzywo sztuczne PMMA w kolorze mlecznym.","Uszczelka silikonowa.",null,"49cm","Drewno impregnowane",null,"Lampa E27","LED A55..60",null,0,null,null,80,null,"205ZX0010, 206GA0010, 206GA0S10, 46999021","Zaciski podłączeniowe: max 3x2,5mm², możliwość podłączenia oprawy w pętle max 3x1,5mm². Przewód w oponie okrągłej o średnicy max ø12,5mm.","1453XX0010.jpg","1453XX0010.ldt",4,"E27",1,1]
["1464","1464XX0012","STOCKHOLM BOLLARD 85CM LED E27 806LM 2700K DIM.","Stockholm","Bollard","Stal",null,null,null,"Wymienne","E27",null,"5,9W","5,9W","806lm","806lm",null,null,"65","IK10","Class II",2700,null,0.17,0.17,0.85,"CE",null,null,"25000",1,"Oprawa słupkowa.","Światło odkryte, rozproszone z obrotowo- symetrycznym rozsyłem światła.",null,"Bollard luminaire of stable and durable construction. For lighting private areas and public spaces.",null,null,"Oprawa wyposażona w wymienne źródło światła typu lampa LED o trzonku E27, który zapewnia trwałość i optymalny rozsył światła, przy zachowaniu stosunkowo małego zużycia energii.","Stal cynkowana ogniowo.",null,"Klosz- tworzywo sztuczne PMMA w kolorze mlecznym.","Uszczelka silikonowa.",null,"85cm","mleczny",null,"Lampa LED E27","Philips MAS LEDBulb DT5.9-60W E27 927 A60 FR G",null,0,"Ściemnianie fazowe LED GU10 E27",null,80,"F","205ZX0010, 206GA0010, 46999021","Zaciski podłączeniowe: max 3x2,5mm², możliwość podłączenia oprawy w pętle max 3x2,5mm². Przewód w oponie okrągłej o średnicy max ø12,5mm.","1464XX0012.jpg","1464XX0012.ldt",1,"E27",1,24]
["1468","1468XX0009","ALTA BOLLARD 49CM LED 1121LM 4000K DIM.","Alta","Bollard","Stal",null,null,null,"LED zintegrowane","AC","DIM.","6,7W","8,5W","1121lm","151lm",null,null,"65",null,"Class II",4000,null,0,0,0,"CE",null,null,"> 50 000h",1,"Oprawa słupkowa.","Światło obrotowo symetryczne przysłonięte od góry.",null,"A bollard luminaire with a stable and durable structure For lighting private areas and other architectural concepts",null,null,null,"Stal cynkowana ogniowo.","Stal cynkowana ogniowo i malowana proszkowo.","Klosz- tworzywo sztuczne PMMA w kolorze mlecznym.","Uszczelka silikonowa.",null,"49cm",null,"Oprawa ściemnialna fazowo TRAILING EDGE (TE) - LEADING EDGE (LE)","Moduł LED","Philips Fortimo SLM C 1203 L09 1619 G7 4K","KGP CC10W180-270CG",50000,"Dim. TRIAC (KGP)",null,80,"D","205ZX0010, 206GA0010, 206GA0S10, 2951ZX0009","Zaciski podłączeniowe: max 2x4mm², możliwość podłączenia oprawy w pętle max 2x2,5mm². Przewód w oponie okrągłej o średnicy max ø12,5mm.","1468XX0009.jpg","1468XX0009.ldt",1,null,1,1]
["1469","1469XX0011","STOCKHOLM BOLLARD 49CM LED E27 806LM 2700K DIM.","Stockholm","Bollard","Stal",null,null,null,"Wymienne","E27",null,"5,9W","5,9W","806lm","806lm",null,null,"65","IK10","Class II",2700,null,0.17,0.17,0.49,"CE",null,null,"25000",1,"Oprawa słupkowa.","Światło odkryte, rozproszone z obrotowo- symetrycznym rozsyłem światła.",null,"Bollard luminaire of stable and durable construction. For lighting private areas and public spaces.",null,null,"Oprawa wyposażona w wymienne źródło światła typu lampa LED o trzonku E27, który zapewnia trwałość i optymalny rozsył światła, przy zachowaniu stosunkowo małego zużycia energii.","Stal cynkowana ogniowo.",null,"Klosz- tworzywo sztuczne PMMA w kolorze mlecznym.","Uszczelka silikonowa.",null,"49cm","mleczny","Oprawa ściemnialna fazowo TRAILING EDGE (TE) - LEADING EDGE (LE)","Lampa LED E27","Philips MAS LEDBulb DT5.9-60W E27 927 A60 FR G",null,0,"Ściemnianie fazowe LED GU10 E27",null,80,"F","205ZX0010, 206GA0010, 46999021","Zaciski podłączeniowe: max 3x2,5mm², możliwość podłączenia oprawy w pętle max 3x2,5mm². Przewód w oponie okrągłej o średnicy max ø12,5mm.","1469XX0011.jpg","1469XX0011.ldt",1,"E27",1,24]
["1475","1475XX0012","ALTA BOLLARD 85CM LED E27 806LM 2700K DIM.","Alta","Bollard","Stal",null,null,null,"Wymienne","E27",null,"5,9W","5,9W","806lm","100lm",null,null,"65","IK10","Class II",2700,null,0.15,0.15,0.85,"CE",null,null,"25000",1,"Oprawa słupkowa.","Światło obrotowo symetryczne przysłonięte od góry.",null,"Bollard luminaire of stable and durable construction. For lighting private areas and public spaces.",null,null,null,"Stal cynkowana ogniowo.",null,"Klosz- tworzywo sztuczne PMMA w kolorze mlecznym.","Uszczelka silikonowa.",null,"85cm",null,"Oprawa ściemnialna fazowo TRAILING EDGE (TE) - LEADING EDGE (LE)","Lampa LED E27","Philips MAS LEDBulb DT5.9-60W E27 927 A60 FR G",null,0,"Ściemnianie fazowe LED GU10 E27",null,80,"F","205ZX0010, 206GA0010, 206GA0S10","Zaciski podłączeniowe: max 3x2,5mm², możliwość podłączenia oprawy w pętle max 3x2,5mm². Przewód w oponie okrągłej o średnicy max ø12,5mm.","1475XX0012.jpg","1475XX0012.ldt",1,"E27",1,1]
["1476","1476XX0012","ALTA BOLLARD 49CM LED 1098LM 3000K DIM.","Alta","Bollard","Stal",null,null,null,"LED zintegrowane","AC","DIM.","10W","10W","1098lm","159lm",null,null,"65",null,"Class I",3000,null,0,0,0,"CE",null,null,"> 50 000h",1,"Oprawa słupkowa.","Światło obrotowo symetryczne przysłonięte od góry.",null,"A bollard luminaire with a stable and durable structure. For lighting private areas and public areas",null,null,null,"Stal cynkowana ogniowo.","Stal cynkowana ogniowo i malowana proszkowo.","Klosz- tworzywo sztuczne PMMA w kolorze mlecznym.","Uszczelka silikonowa.",null,"49cm",null,"Oprawa ściemnialna fazowo TRAILING EDGE (TE) - LEADING EDGE (LE)","Moduł LED","Lumens EDC 47C 10W xxx 230V A101 3K",null,null,"Ściemnianie fazowe Lumens LED AC",null,80,"E","205ZX0010, 206GA0010","Zaciski podłączeniowe: max 3x2,5mm², możliwość podłączenia oprawy w pętle max 3x1,5mm². Przewód w oponie okrągłej o średnicy max ø12,5mm.","1476XX0012.jpg","1476XX0012.ldt",1,null,1,1]
["1477","1477XX0012","ALTA BOLLARD 49CM LED E27 806LM 2700K DIM.","Alta","Bollard","Stal",null,null,null,"Wymienne","E27",null,"5,9W","5,9W","806lm","100lm",null,null,"65","IK10","Class II",2700,null,0.15,0.15,0.49,"CE",null,null,"25000",1,"Oprawa słupkowa.","Światło obrotowo symetryczne przysłonięte od góry.",null,"Bollard luminaire of stable and durable construction. For lighting private areas and public spaces.",null,null,null,"Stal cynkowana ogniowo.",null,"Klosz- tworzywo sztuczne PMMA w kolorze mlecznym.","Uszczelka silikonowa.",null,"49cm",null,"Oprawa ściemnialna fazowo TRAILING EDGE (TE) - LEADING EDGE (LE)","Lampa LED E27","Philips MAS LEDBulb DT5.9-60W E27 927 A60 FR G",null,0,"Ściemnianie fazowe LED GU10 E27",null,80,"F","205ZX0010, 206GA0010, 206GA0S10","Zaciski podłączeniowe: max 3x2,5mm², możliwość podłączenia oprawy w pętle max 3x2,5mm². Przewód w oponie okrągłej o średnicy max ø12,5mm.","1477XX0012.jpg","1477XX0012.ldt",1,"E27",1,1]
["1479","1479XX0012","ALTA BOLLARD 85CM LED 1098LM 3000K DIM.","Alta","Bollard","Stal",null,null,null,"LED zintegrowane","AC","DIM.","10W","10W","1098lm","159lm",null,null,"65",null,"Class I",3000,null,0,0,0,"CE",null,null,"> 50 000h",1,"Oprawa słupkowa.","Światło obrotowo symetryczne przysłonięte od góry.",null,"A bollard luminaire with a stable and durable structure. For lighting private areas and public areas",null,null,null,"Stal cynkowana ogniowo.","Stal cynkowana ogniowo i malowana proszkowo.","Klosz- tworzywo sztuczne PMMA w kolorze mlecznym.","Uszczelka silikonowa.",null,"85cm",null,"Oprawa ściemnialna fazowo TRAILING EDGE (TE) - LEADING EDGE (LE)","Moduł LED","Lumens EDC 47C 10W xxx 230V A101 3K",null,0,"Ściemnianie fazowe Lumens LED AC",null,80,"E","205ZX0010, 206GA0010","Zaciski podłączeniowe: max 3x2,5mm², możliwość podłączenia oprawy w pętle max 3x1,5mm². Przewód w oponie okrągłej o średnicy max ø12,5mm.","1479XX0012.jpg","1479XX0012.ldt",1,null,1,1]
["1482","1482XX0013","HALMSTAD BOLLARD 85CM LED 1059LM 3000K DIM.","Halmstad","Bollard","Stal",null,null,null,"LED zintegrowane","AC","DIM.","6,7W","8,5W","1059lm","292lm",null,null,"65","IK10","Class II",3000,null,0,0,0,"CE",null,null,"> 50 000h",1,"Oprawa słupkowa.","Światło odkryte, częściowo przysłonięte od góry.",null,"A bollard luminaire with a stable and durable structure. For lighting private areas and other architectural concepts",null,null,null,"Stal cynkowana ogniowo.",null,"Klosz- tworzywo sztuczne PMMA w kolorze mlecznym.","Uszczelka silikonowa.",null,"85cm",null,"Oprawa ściemnialna fazowo TRAILING EDGE (TE) - LEADING EDGE (LE)","Moduł LED","Philips Fortimo SLM C 1203 L09 1619 G7 3K","KGP CC10W180-270CG",50000,"Dim. TRIAC (KGP)",null,80,"D","205ZX0010, 206GA0010, 206GA0S10, 2951ZX0009, 6138ZX0009","Zaciski podłączeniowe: max 2x4mm², możliwość podłączenia oprawy w pętle max 2x2,5mm². Przewód w oponie okrągłej o średnicy max ø12,5mm.","1482XX0013.jpg","1482XX0013.ldt",1,null,1,23]
["1483","1483XX0012","HALMSTAD BOLLARD 85CM LED E27 806LM 2700K DIM.","Halmstad","Bollard","Stal",null,null,null,"Wymienne","E27",null,"5,9W","5,9W","806lm","252lm",null,null,"65","IK10","Class II",2700,null,null,null,null,"CE",null,null,"25000",1,"Oprawa słupkowa.","Światło odkryte, częściowo przysłonięte od góry.",null,"Bollard luminaire of stable and durable construction. For lighting private areas and public spaces.",null,null,null,"Stal cynkowana ogniowo.",null,"Klosz- tworzywo sztuczne PMMA w kolorze mlecznym.","Uszczelka silikonowa.",null,"85cm",null,"Oprawa ściemnialna fazowo TRAILING EDGE (TE) - LEADING EDGE (LE)","Lampa LED E27","Philips MAS LEDBulb DT5.9-60W E27 927 A60 FR G",null,0,"Ściemnianie fazowe LED GU10 E27",null,80,"F","205ZX0010, 206GA0010, 206GA0S10","Zaciski podłączeniowe: max 3x2,5mm², możliwość podłączenia oprawy w pętle max 3x1,5mm². Przewód w oponie okrągłej o średnicy max ø12,5mm.","1483XX0012.jpg","1483XX0012.ldt",1,"E27",1,23]
["1488","1488XX0012","HALMSTAD BOLLARD 49CM E27 806LM 2700K DIM.","Halmstad","Bollard","Stal",null,null,null,"Wymienne","E27",null,"5,9W","5,9W","806lm","252lm",null,null,"65","IK10","Class II",2700,null,null,null,null,"CE",null,null,"25000",1,"Oprawa słupkowa.","Światło odkryte, częściowo przysłonięte od góry.",null,"Bollard luminaire of stable and durable construction. For lighting private areas and public spaces.",null,null,"Oprawa wyposażona w wymienne źródło światła typu lampa LED o trzonku E27, która zapewnia trwałość i optymalny rozsył światła, przy zachowaniu stosunkowo małego zużycia energii.","Stal cynkowana ogniowo.",null,"Klosz- tworzywo sztuczne PMMA w kolorze mlecznym.","Uszczelka silikonowa.",null,"49cm",null,"Oprawa ściemnialna fazowo TRAILING EDGE (TE) - LEADING EDGE (LE)","Lampa E27","Philips MAS LEDBulb DT5.9-60W E27 927 A60 FR G",null,0,"Ściemnianie fazowe LED GU10 E27",null,80,"F","205ZX0010, 206GA0010, 206GA0S10","Zaciski podłączeniowe: max 3x2,5mm², możliwość podłączenia oprawy w pętle max 3x2,5mm². Przewód w oponie okrągłej o średnicy max ø12,5mm.","1488XX0012.jpg","1488XX0012.ldt",1,"E27",1,23]
["1489","1489XX0012","HALMSTAD BOLLARD 49CM LED 1098LM 3000K DIM.","Halmstad","Bollard","Stal",null,null,null,"LED zintegrowane","AC","DIM.","10W","10,5W","1098lm",null,null,null,"65","IK10","Class I",3000,null,0,0,0,"CE",null,null,"> 50 000h",1,"Oprawa słupkowa.","Światło odkryte, częściowo przysłonięte od góry.",null,"A bollard luminaire with a stable and durable structure. For lighting private areas and public areas",null,null,null,"Stal cynkowana ogniowo.","Stal cynkowana ogniowo i malowana proszkowo.","Klosz- tworzywo sztuczne PMMA w kolorze mlecznym.","Uszczelka silikonowa.",null,"49cm",null,"Oprawa ściemnialna fazowo TRAILING EDGE (TE) - LEADING EDGE (LE)","Moduł LED","Lumens EDC 47C 10W xxx 230V A101 3K",null,null,"Ściemnianie fazowe Lumens LED AC",0.44,80,"E","205ZX0010, 206GA0010","Zaciski podłączeniowe: max 3x2,5mm², możliwość podłączenia oprawy w pętle max 3x1,5mm². Przewód w oponie okrągłej o średnicy max ø12,5mm.","1489XX0012.jpg","1489XX0012.ldt",1,null,1,23]
["1489","1489XX0013","HALMSTAD BOLLARD 49CM LED 1059LM 3000K DIM.","Halmstad","Bollard","Stal",null,null,null,"LED zintegrowane","AC","DIM.","6,7W","8,5W","1059lm","292lm",null,null,"65","IK10","Class II",3000,null,0,0,0,"CE",null,null,"> 50 000h",1,"Oprawa słupkowa.","Światło odkryte, częściowo przysłonięte od góry.",null,"A bollard luminaire with a stable and durable structure. For lighting private areas and other architectural concepts",null,null,null,"Stal cynkowana ogniowo.","Stal cynkowana ogniowo i malowana proszkowo.","Klosz- tworzywo sztuczne PMMA w kolorze mlecznym.","Uszczelka silikonowa.",null,"49cm",null,"Oprawa ściemnialna fazowo TRAILING EDGE (TE) - LEADING EDGE (LE)","Moduł LED","Philips Fortimo SLM C 1203 L09 1619 G7 3K","KGP CC10W180-270CG",50000,"Dim. TRIAC (KGP)",null,80,"D","205ZX0010, 206GA0010, 206GA0S10, 2951ZX0009","Zaciski podłączeniowe: max 2x4mm², możliwość podłączenia oprawy w pętle max 2x2,5mm². Przewód w oponie okrągłej o średnicy max ø12,5mm.","1489XX0013.jpg","1489XX0013.ldt",1,null,1,23]
["1495","1495XX0013","PARIS WALL LED 653LM DOWN 3000K DIM.","Paris","Wall","Stal",null,null,null,"LED zintegrowane","AC","DIM.","3,9W","5,2W","653lm","508lm",null,null,"43",null,"Class I",3000,"szerokie dół",null,null,null,"CE",null,null,"> 70 000h",12,"Oprawa ścienna.","Światło rozproszone półsferyczne ukierunkowane w dół",null,"A luminaire with a classic and simple design for general use",null,null,null,"Stal cynkowana ogniowo.","Stal malowana proszkowo.","Klosz- poliwęglan satynowany, stabilizowany UV.",null,"Dławnica EPDM.",null,null,"Oprawa ściemnialna fazowo TRAILING EDGE (TE)","Moduł LED","Philips Fortimo_LED_Strip_0.5ft_MF_8xx_HV6 3K","Philips Xitanium 7W 0,35A 20V TE SC 230V [2017]",50000,null,0,80,"C",null,"Zaciski podłączeniowe: max 3x2,5mm², możliwość podłączenia oprawy w pętle max 3x1,5mm². Przewód w oponie okrągłej o średnicy ø7...10,5mm.","1495XX0013.jpg","1495XX0013.ldt",1,null,1,76]
["1496","1496XX0013","PARIS WALL LED 653LM DOWN 3000K DIM.","Paris,Big","Wall","Stal",null,null,null,"LED zintegrowane","AC","DIM.","3,9W","5,2W","653lm","471lm",null,null,"43",null,"Class I",3000,"szerokie dół",null,null,null,"CE",null,null,"> 70 000h",12,"Oprawa ścienna.","Światło rozproszone półsferyczne ukierunkowane w dół",null,"A luminaire with a classic and simple design for general use",null,null,null,"Stal cynkowana ogniowo.","Stal malowana proszkowo.","Klosz- poliwęglan satynowany, stabilizowany UV.",null,"Dławnica EPDM.",null,null,"Oprawa ściemnialna fazowo TRAILING EDGE (TE)","Moduł LED","Philips Fortimo_LED_Strip_0.5ft_MF_8xx_HV6 3K","Philips Xitanium 7W 0,35A 20V TE SC 230V [2017]",50000,null,0,80,"C",null,"Zaciski podłączeniowe: max 3x2,5mm², możliwość podłączenia oprawy w pętle max 3x1,5mm². Przewód w oponie okrągłej o średnicy ø7...10,5mm.","1496XX0013.jpg","1496XX0013.ldt",1,null,1,76]
["1510","1510XX0016","ASKER WALL LED 840LM UP-DOWN 3000K DIM.","Asker","Wall","Aluminium",null,null,null,"LED zintegrowane","AC","DIM.","8,8W","8,8W","840lm","312lm",null,null,"65","IK08","Class I",3000,"szerokie góra / szerokie dół",null,null,null,"CE",null,null,"50 000h",12,"Oprawa ścienna.","Światło dwustronne: ukierunkowane do góry i w dół.","Up-Down","Luminaire with a wide range of applications for example for illumination of walls and facade surfaces or any other architectural concepts",null,null,null,"Odlew aluminiowy malowany proszkowo.",null,"Klosz- poliwęglan przeźroczysty ze strukturą, stabilizowany UV.","Uszczelka silikonowa.","Dławnica EPDM.","góra/dół",null,"Oprawa ściemnialna fazowo TRAILING EDGE (TE) - LEADING EDGE (LE)","Moduł LED","Lumens EDC 57C 8W xxx 230V F201 3K",null,0,"Ściemnianie fazowe Lumens LED AC",null,80,"F",null,"Zaciski podłączeniowe: max 3x2,5mm², możliwość podłączenia oprawy w pętle max 3x1,5mm². Przewód w oponie okrągłej o średnicy ø7...10,5mm.","1510XX0016.jpg","1510XX0016.ldt",1,null,1,4]
["1511","1511XX0016","ASKER WALL LED 840LM DOWN 3000K DIM.","Asker","Wall","Aluminium",null,null,null,"LED zintegrowane","AC","DIM.","8,8W","8,8W","840lm","156lm",null,null,"65","IK08","Class I",3000,"szerokie dół",null,null,null,"CE",null,null,"50 000h",12,"Oprawa ścienna.","Światło rozproszone półsferyczne ukierunkowane w dół",null,"A luminaire with a wide range of applications, including lighting wall surfaces, facades, and other architectural concepts",null,null,null,"Odlew aluminiowy malowany proszkowo.",null,"Klosz- poliwęglan przeźroczysty ze strukturą, stabilizowany UV.","Uszczelka silikonowa.","Dławnica EPDM.","dół",null,"Oprawa ściemnialna fazowo TRAILING EDGE (TE) - LEADING EDGE (LE)","Moduł LED","Lumens EDC 57C 8W xxx 230V F201 3K",null,0,"Ściemnianie fazowe Lumens LED AC",null,80,"F",null,"Zaciski podłączeniowe: max 3x2,5mm², możliwość podłączenia oprawy w pętle max 3x1,5mm². Przewód w oponie okrągłej o średnicy ø7...10,5mm.","1511XX0016.jpg","1511XX0016.ldt",1,null,1,76]
["1513","1513XX0013","ASKER WALL E27 UP-DOWN","Asker","Wall","Aluminium",null,null,null,"Wymienne","E27",null,"LED max 9W","LED max 9W",null,null,null,null,"65","IK08","Class I",null,"szerokie góra / szerokie dół",0.22,0.11,0.08,"CE",null,null,null,12,"Oprawa ścienna.","Światło dwustronne: ukierunkowane do góry i w dół.","Up-Down","Luminaire with a wide range of applications for example for illumination of walls and facade surfaces or any other architectural concepts.",null,null,"Oprawa na wymienne źródło światła typu: lampa LED, świetlówka TC-SE, tradycyjna żarówka (halogenowa) o trzonku E27. Źródło światła należy dokupić oddzielnie.","Odlew aluminiowy malowany proszkowo.",null,"Klosz- poliwęglan przeźroczysty ze strukturą, stabilizowany UV.","Uszczelka silikonowa.","Dławnica EPDM.","góra/dół",null,null,"Lampa E27","LED A55..60",null,0,null,null,80,null,"46999021","Zaciski podłączeniowe: max 3x2,5mm², możliwość podłączenia oprawy w pętle max 3x1,5mm². Przewód w oponie okrągłej o średnicy ø7...10,5mm.","1513XX0013.jpg","1513XX0013.ldt",4,"E27",1,4]
["1514","1514XX0013","ASKER WALL E27","Asker","Wall","Aluminium",null,null,null,"Wymienne","E27",null,"LED max 9W","LED max 9W",null,null,null,null,"65","IK08","Class I",null,"szerokie dół",0.22,0.11,0.08,"CE",null,null,null,12,"Oprawa ścienna.","Światło jednostronne: symetryczne, ukierunkowane w dół.",null,"Luminaire with a wide range of applications for example for illumination of walls and facade surfaces or any other architectural concepts.",null,null,"Oprawa na wymienne źródło światła typu: lampa LED, świetlówka TC-SE, tradycyjna żarówka (halogenowa) o trzonku E27. Źródło światła należy dokupić oddzielnie.","Odlew aluminiowy malowany proszkowo.",null,"Klosz- poliwęglan przeźroczysty ze strukturą, stabilizowany UV.","Uszczelka silikonowa.","Dławnica EPDM.","dół",null,null,"Lampa E27","LED A55..60",null,0,null,null,80,null,"46999021","Zaciski podłączeniowe: max 3x2,5mm², możliwość podłączenia oprawy w pętle max 3x1,5mm². Przewód w oponie okrągłej o średnicy ø6...10mm.","1514XX0013.jpg","1514XX0013.ldt",4,"E27",1,27]
["1544","1544XX0014","GRIMSTAD WALL-RECESSED LED 653LM 3000K DIM.","Grimstad","Recessed","Aluminium",null,null,null,"LED zintegrowane","AC","DIM.","3,9W","5,3W","653lm","214lm",null,null,"65","IK08","Class I",3000,null,null,null,null,"CE",null,null,"> 70 000h",11,"Oprawa wbudowana ścienna.","Światło rozproszone.",null,"The luminaire is adapted to illuminate stairs, steps, staircases, pathways, and other places",null,null,null,"Odlew aluminiowy malowany proszkowo.",null,"Klosz- szkło bezpieczne, mleczne.","Uszczelka silikonowa.","Dławnica EPDM.",null,"Ramka","Oprawa ściemnialna fazowo TRAILING EDGE (TE)","Moduł LED","Philips Fortimo_LED_Strip_0.5ft_MF_8xx_HV6 3K","Philips Xitanium 7W 0,35A 20V TE SC 230V [2017]",50000,null,null,80,"C",null,"Zaciski podłączeniowe: max 3x2,5mm², możliwość podłączenia oprawy w pętle max 3x1,5mm². Przewód w oponie okrągłej o średnicy ø7...10,5mm.","1544XX0014.jpg","1544XX0014.ldt",1,null,1,7]
["1545","1545XX0012","GRIMSTAD WALL-RECESSED LED 981LM 3000K DIM.","Grimstad","Recessed","Aluminium",null,null,null,"LED zintegrowane","AC","DIM.","6,8W","8,3W","981lm","67lm",null,null,"65","IK09","Class I",3000,null,0,0,0,"CE",null,null,"> 100 000h",11,"Oprawa wbudowana ścienna.","Światło rozproszone półsferyczne ukierunkowane w dół",null,"The luminaire is adapted to illuminate stairs, steps, staircases, communication pathways and other applications",null,null,null,"Odlew aluminiowy malowany proszkowo.",null,"Klosz- szkło bezpieczne, mleczne.","Uszczelka silikonowa.","Dławnica EPDM.",null,"Żaluzje","Oprawa ściemnialna fazowo TRAILING EDGE (TE)","Moduł LED","Philips Fortimo DLM FLEX 1100/830 Gen2 3K","Philips Xitanium 8W 0,2A 40V TE SC 230V",0,"Philips Xitanium TE",0.02,80,"E",null,"Zaciski podłączeniowe: max 3x2,5mm², możliwość podłączenia oprawy w pętle max 3x1,5mm². Przewód w oponie okrągłej o średnicy ø7...10,5mm.","1545XX0012.jpg","1545XX0012.ldt",1,null,1,76]
["1550","1550XX0016","RENA IN-GROUND LED GU10 375LM 36D 3000K DIM.","Rena","Recessed","Stal nierdzewna",null,null,null,"Wymienne","GU10",null,"5,5W","5,5W","375lm","367lm",null,null,"68","IK09","Class I",3000,null,0,0,0,"CE",null,null,"40000",14,"Oprawa wbudowana w podłoże.","Światło symetryczne o kącie 36D","36D","An orientation luminaire that can be driven on by vehicles with pneumatic tires. Luminaires should not be used on traffic lanes where they would be exposed to horizontal weight load as a result of sudden braking, acceleration, and change of direction. The light direction angle can be adjusted, up to a maximum of 10 degrees",null,null,null,"Odlew aluminiowy malowany proszkowo.","Front- stal nierdzewna.","Klosz- szkło bezpieczne, przeźroczyste.","Uszczelka silikonowa.","Dławnica mosiężna niklowana.","Przeźroczysty","Okrąg","Oprawa ściemnialna fazowo TRAILING EDGE (TE) - LEADING EDGE (LE)","Lampa LED GU10","Philips MASTER LED ExpertColor 5.5-50W GU10 930 36D",null,0,"Ściemnianie fazowe LED GU10 E27",null,90,"G","139ZX0009, 142ZX0009, 143ZX0009, 145ZX0009, 146ZX0009","Oprawa wyposażona w przewód typu 05RN8-F 3G1 o długości 3m. Do podłączenia w odpowiednio dobranej puszce elektroinstalacyjnej. Maksymalne obciążenie oprawy 2000kg. Uwaga: na powierzchni szklanej w punkcie środkowym, osiągane są temperatury robocze zgodne z normą 60598 ( temperatura otoczenia 15ºC).","1550XX0016.jpg","1550XX0016.ldt",1,"GU10",3,68]
["1551","1551XX0016","RENA IN-GROUND LED GU10 375LM 36D 3000K DIM.","Rena","Recessed","Stal nierdzewna",null,null,null,"Wymienne","GU10",null,"5,5W","5,5W","375lm","367lm",null,null,"68","IK09","Class I",3000,null,0.13,0.13,0.16,"CE",null,null,"40000",14,"Oprawa wbudowana w podłoże.","Światło symetryczne o kącie 36D","36D","Indicative luminaire or as a spotlight on which you can ride with pneumatic tires. Luminaires should not be used on traffic lanes, where they would be exposed to horizontal weight due to sudden braking, acceleration, and reversing. Adjustable angle of the light max. up to 10 degrees",null,null,null,"Odlew aluminiowy malowany proszkowo.","Front- stal nierdzewna.","Klosz- szkło bezpieczne, przeźroczyste.","Uszczelka silikonowa.","Dławnica mosiężna niklowana.","Przeźroczysty","Kwadrat","Oprawa ściemnialna fazowo TRAILING EDGE (TE) - LEADING EDGE (LE)","Lampa LED GU10","Philips MASTER LED ExpertColor 5.5-50W GU10 930 36D",null,0,"Ściemnianie fazowe LED GU10 E27",null,90,"G","139ZX0009, 142ZX0009, 143ZX0009, 145ZX0009, 146ZX0009","Oprawa wyposażona w przewód typu 05RN8-F 3G1 o długości 3m. Do podłączenia w odpowiednio dobranej puszce elektroinstalacyjnej. Maksymalne obciążenie oprawy 2000kg. Uwaga: na powierzchni szklanej w punkcie środkowym, osiągane są temperatury robocze zgodne z normą 60598 (temperatura otoczenia 15ºC)","1551XX0016.jpg","1551XX0016.ldt",1,"GU10",3,68]
["1552","1552XX0014","RENA IN-GROUND LED GU10","Rena","Recessed","Stal nierdzewna",null,null,null,"Wymienne","GU10",null,"LED max 6W","LED max 6W",null,null,null,null,"68","IK09","Class I",null,null,0.13,0.13,0.17,"CE",null,null,null,14,"Oprawa wbudowana w podłoże.","Światło odkryte.",null,"An orientation luminaire that can be driven on by vehicles with pneumatic tires. Luminaires should not be used on traffic lanes where they would be exposed to horizontal weight load as a result of sudden braking, acceleration, and change of direction. The light direction angle can be adjusted, up to a maximum of 10 degrees",null,null,"Oprawa na wymienne źródło światła typu lampa LED o trzonku Gu10, która zapewnia trwałość i optymalny rozsył światła, przy zachowaniu stosunkowo małego zużycia energii. Źródło światła należy dokupić oddzielnie.","Odlew aluminiowy malowany proszkowo.","Front- stal nierdzewna.","Klosz- szkło bezpieczne, przeźroczyste.","Uszczelka silikonowa.","Dławnica mosiężna niklowana.","Przeźroczysty","Okrąg",null,"Lampa LED GU10","PAR16",null,0,null,null,80,null,"139ZX0009, 142ZX0009, 143ZX0009, 145ZX0009, 146ZX0009, 46102506","Oprawa wyposażona w przewód typu 05RN8-F 3G1 o długości 3m. Do podłączenia w odpowiednio dobranej puszce elektroinstalacyjnej. Maksymalne obciążenie oprawy 2000kg. Uwaga: na powierzchni szklanej w punkcie środkowym, osiągane są temperatury robocze zgodne z normą 60598 (temperatura otoczenia 15ºC)","1552XX0014.jpg","1552XX0014.ldt",4,"GU10",3,9]
["1553","1553XX0014","RENA IN-GROUND LED GU10","Rena","Recessed","Stal nierdzewna",null,null,null,"Wymienne","GU10",null,"LED max 6W","LED max 6W",null,null,null,null,"68","IK09","Class I",null,null,0.13,0.13,0.17,"CE",null,null,null,14,"Oprawa wbudowana w podłoże.","Światło odkryte.",null,"Indicative luminaire or as a spotlight on which you can ride with pneumatic tires. Luminaires should not be used on traffic lanes, where they would be exposed to horizontal weight due to sudden braking, acceleration, and reversing. Adjustable angle of the light maximum up to 10 degrees",null,null,"Oprawa na wymienne źródło światła typu lampa LED o trzonku Gu10, która zapewnia trwałość i optymalny rozsył światła, przy zachowaniu stosunkowo małego zużycia energii. Źródło światła należy dokupić oddzielnie.","Odlew aluminiowy malowany proszkowo.","Front- stal nierdzewna.","Klosz- szkło bezpieczne, przeźroczyste.","Uszczelka silikonowa.","Dławnica mosiężna niklowana.","Przeźroczysty","Kwadrat",null,"Lampa LED GU10","PAR16",null,0,null,null,80,null,"139ZX0009, 142ZX0009, 143ZX0009, 145ZX0009, 146ZX0009, 46102506","Oprawa wyposażona w przewód typu 05RN-F 3G1 o długości 3m. Do podłączenia w odpowiednio dobranej puszcze elektroinstalacyjnej. Maksymalne obciążenie oprawy 2000kg. Uwaga: na powierzchni szklanej w punkcie środkowym, osiągane są temperatury robocze zgodne z normą 60598 ( temperatura otoczenia 15ºC).","1553XX0014.jpg","1553XX0014.ldt",4,"GU10",3,9]
["1554","1554XX0016","RENA IN-GROUND LED GU10 375LM 36D 3000K DIM.","Rena","Recessed","Stal nierdzewna",null,null,null,"Wymienne","GU10",null,"5,5W","5,5W","375lm","237lm",null,null,"68","IK09","Class I",3000,null,0,0,0,"CE",null,null,"40000",14,"Oprawa wbudowana w podłoże.","Światło symetryczne o kącie 36D","36D","Indicative luminaire or as a spotlight on which you can ride with pneumatic tires. Luminaires should not be used on traffic lanes, where they would be exposed to horizontal weight due to sudden braking, acceleration, and reversing. Adjustable angle of the light max. up to 10 degrees",null,null,"Oprawa wyposażona w wymienne źródło światła typu lampa LED o trzonku Gu10, która zapewnia trwałość i optymalny rozsył światła, przy zachowaniu stosunkowo małego zużycia energii.","Odlew aluminiowy malowany proszkowo.","Front- stal nierdzewna.","Klosz- szkło bezpieczne, satynowane.","Uszczelka silikonowa.","Dławnica mosiężna niklowana.","Satynowany","Okrąg","Oprawa ściemnialna fazowo TRAILING EDGE (TE) - LEADING EDGE (LE)","Lampa LED GU10","Philips MASTER LED ExpertColor 5.5-50W GU10 930 36D",null,0,"Ściemnianie fazowe LED GU10 E27",null,90,"G","139ZX0009, 142ZX0009, 143ZX0009, 144ZX0009, 146ZX0009","Oprawa wyposażona w przewód typu 05RN8-F 3G1 o długości 3m. Do podłączenia w odpowiednio dobranej puszce elektroinstalacyjnej. Maksymalne obciążenie oprawy 2000kg. Uwaga: na powierzchni szklanej w punkcie środkowym, osiągane są temperatury robocze zgodne z normą 60598 (temperatura otoczenia 15ºC)","1554XX0016.jpg","1554XX0016.ldt",1,"GU10",3,68]
["1555","1555XX0016","RENA IN-GROUND LED GU10 375LM 36D 3000K DIM.","Rena","Recessed","Stal nierdzewna",null,null,null,"Wymienne","GU10",null,"5,5W","5,5W","375lm","237lm",null,null,"68","IK09","Class I",3000,null,0,0,0,"CE",null,null,"40000",14,"Oprawa wbudowana w podłoże.","Światło symetryczne o kącie 36D","36D","An orientation luminaire that can be driven on by vehicles with pneumatic tires. Luminaires should not be used on traffic lanes where they would be exposed to horizontal weight load as a result of sudden braking, acceleration, and change of direction. The light direction angle can be adjusted, up to a maximum of 10 degrees",null,null,"Oprawa wyposażona w wymienne źródło światła typu lampa LED o trzonku Gu10, która zapewnia trwałość i optymalny rozsył światła, przy zachowaniu stosunkowo małego zużycia energii.","Odlew aluminiowy malowany proszkowo.","Front- stal nierdzewna.","Klosz- szkło bezpieczne, satynowane.","Uszczelka silikonowa.","Dławnica mosiężna niklowana.","Satynowany","Kwadrat","Oprawa ściemnialna fazowo TRAILING EDGE (TE) - LEADING EDGE (LE)","Lampa LED GU10","Philips MASTER LED ExpertColor 5.5-50W GU10 930 36D",null,0,"Ściemnianie fazowe LED GU10 E27",null,90,"G","139ZX0009, 142ZX0009, 143ZX0009, 144ZX0009, 146ZX0009","Oprawa wyposażona w przewód typu 05RN8-F 3G1 o długości 3m. Do podłączenia w odpowiednio dobranej puszce elektroinstalacyjnej. Maksymalne obciążenie oprawy 2000kg. Uwaga: na powierzchni szklanej w punkcie środkowym, osiągane są temperatury robocze zgodne z normą 60598 (temperatura otoczenia 15ºC)","1555XX0016.jpg","1555XX0016.ldt",1,"GU10",3,68]
["1556","1556XX0014","RENA IN-GROUND LED GU10 375LM","Rena","Recessed","Stal nierdzewna",null,null,null,"Wymienne","GU10",null,"max 6W","LED max 6W","375lm",null,null,null,"68","IK09","Class I",null,null,0.13,0.13,0.17,"CE",null,null,null,14,"Oprawa wbudowana w podłoże.","Światło rozproszone.",null,"Indicative luminaire or as a spotlight on which you can ride with pneumatic tires. Luminaires should not be used on traffic lanes, where they would be exposed to horizontal weight due to sudden braking, acceleration, and reversing. Adjustable angle of the light maximum up to 10 degrees",null,null,"Oprawa na wymienne źródło światła typu lampa LED o trzonku Gu10, która zapewnia trwałość i optymalny rozsył światła, przy zachowaniu stosunkowo małego zużycia energii. Źródło światła należy dokupić oddzielnie.","Odlew aluminiowy malowany proszkowo.","Front- stal nierdzewna.","Klosz- szkło bezpieczne, satynowane.","Uszczelka silikonowa.","Dławnica mosiężna niklowana.","Satynowany","Okrąg",null,"Lampa LED GU10","PAR16",null,0,null,null,80,null,"139ZX0009, 142ZX0009, 143ZX0009, 145ZX0009, 146ZX0009, 46102506","Oprawa wyposażona w przewód typu 05RN8-F 3G1 o długości 3m. Do podłączenia w odpowiednio dobranej puszce elektroinstalacyjnej. Maksymalne obciążenie oprawy 2000kg. Uwaga: na powierzchni szklanej w punkcie środkowym, osiągane są temperatury robocze zgodne z normą 60598 (temperatura otoczenia 15ºC)","1556XX0014.jpg","1556XX0014.ldt",4,"GU10",3,7]
["1557","1557XX0014","RENA IN-GROUND LED GU10 375LM","Rena","Recessed","Stal nierdzewna",null,null,null,"Wymienne","GU10",null,"LED max 6W","LED max 6W","375lm",null,null,null,"68","IK09","Class I",null,null,0.13,0.13,0.16,"CE",null,null,null,14,"Oprawa wbudowana w podłoże.","Światło rozproszone.",null,"Indicative luminaire or as a spotlight on which you can ride with pneumatic tires. Luminaires should not be used on traffic lanes, where they would be exposed to horizontal weight due to sudden braking, acceleration, and reversing. Adjustable angle of the light maximum up to 10 degrees",null,null,"Oprawa na wymienne źródło światła typu lampa LED o trzonku Gu10, która zapewnia trwałość i optymalny rozsył światła, przy zachowaniu stosunkowo małego zużycia energii. Źródło światła należy dokupić oddzielnie.","Odlew aluminiowy malowany proszkowo.","Front- stal nierdzewna.","Klosz- szkło bezpieczne, satynowane.","Uszczelka silikonowa.","Dławnica mosiężna niklowana.","Satynowany","Kwadrat",null,"Lampa LED GU10","PAR16",null,0,null,null,80,null,"139ZX0009, 142ZX0009, 143ZX0009, 145ZX0009, 146ZX0009, 46102506","Oprawa wyposażona w przewód typu 05RN8-F 3G1 o długości 3m. Do podłączenia w odpowiednio dobranej puszce elektroinstalacyjnej. Maksymalne obciążenie oprawy 2000kg. Uwaga: na powierzchni szklanej w punkcie środkowym, osiągane są temperatury robocze zgodne z normą 60598 (temperatura otoczenia 15ºC)","1557XX0014.jpg","1557XX0014.ldt",4,"GU10",3,7]
["1561","1561XX0010","ARENDAL MINI BOLLARD 64CM LED 439LM 3000K DIM.","Arendal Mini","Bollard","Stal",null,null,null,"LED zintegrowane","AC","DIM.","4W","4W","439lm","330lm",null,null,"65","IK08","Class II",3000,null,0,0,0,"CE",null,null,"> 50 000h",1,"Oprawa słupkowa.","Światło odkryte.",null,"A luminaire with a modern design, which combines a decorative crystal lampshade with a durable and stable base.",null,null,null,"Stal cynkowana ogniowo.","Stal cynkowana ogniowo i malowana proszkowo.","Klosz- szkło kryształowe satynowane od wewnątrz.","Klosz z upływem czasu może nabierać bursztynowego koloru.",null,"64cm",null,"Oprawa ściemnialna fazowo TRAILING EDGE (TE) - LEADING EDGE (LE)","Moduł LED","Lumens EDC 38C 4W xxx 230V A101 3K",null,null,"Ściemnianie fazowe Lumens LED AC",null,80,"E","203ZX0009, 204GA0009","Zaciski podłączeniowe: max 2x2,5mm², możliwość podłączenia oprawy w pętle max 2x2,5mm². Przewód w oponie okrągłej o średnicy max ø12,5mm.","1561XX0010.jpg","1561XX0010.ldt",1,null,1,9]
["1562","1562XX0010","ARENDAL MINI BOLLARD 64CM LED 466LM 4000K DIM.","Arendal Mini","Bollard","Stal",null,null,null,"LED zintegrowane","AC","DIM.","4W","4W","466lm","345lm",null,null,"65","IK08","Class II",4000,null,null,null,null,"CE",null,null,"> 50 000h",1,"Oprawa słupkowa.","Światło odkryte.",null,"A luminaire with a modern design, which combines a decorative crystal lampshade with a durable and stable base.",null,null,null,"Stal cynkowana ogniowo.","Stal cynkowana ogniowo i malowana proszkowo.","Klosz- szkło kryształowe satynowane od wewnątrz.","Klosz z upływem czasu może nabierać bursztynowego koloru.",null,"64cm",null,"Oprawa ściemnialna fazowo TRAILING EDGE (TE) - LEADING EDGE (LE)","Moduł LED","Lumens EDC 38C 4W xxx 230V A101 4K",null,null,"Ściemnianie fazowe Lumens LED AC",null,80,null,"203ZX0009, 204GA0009","Zaciski podłączeniowe: max 2x2,5mm², możliwość podłączenia oprawy w pętle max 2x2,5mm². Przewód w oponie okrągłej o średnicy max ø12,5mm.","1562XX0010.jpg","1562XX0010.ldt",1,null,1,9]
["1566","1566XX0010","ARENDAL MINI BOLLARD 37CM LED 439LM 3000K DIM.","Arendal Mini","Bollard","Stal",null,null,null,"LED zintegrowane","AC","DIM.","4W","4W","439lm","330lm",null,null,"65","IK08","Class II",3000,null,0,0,0,"CE",null,null,"> 50 000h",1,"Oprawa słupkowa.","Światło odkryte.",null,"A luminaire with a modern design, in which a combination of a decorative crystal lampshade with a durable and stable structure of the luminaire.",null,null,null,"Stal cynkowana ogniowo.","Stal cynkowana ogniowo i malowana proszkowo.","Klosz- szkło kryształowe satynowane od wewnątrz.","Klosz z upływem czasu może nabierać bursztynowego koloru.",null,"37cm",null,"Oprawa ściemnialna fazowo TRAILING EDGE (TE) - LEADING EDGE (LE)","Moduł LED","Lumens EDC 38C 4W xxx 230V A101 3K",null,0,"Ściemnianie fazowe Lumens LED AC",null,80,"E","203ZX0009, 204GA0009","Zaciski podłączeniowe: max 2x2,5mm², możliwość podłączenia oprawy w pętle max 2x2,5mm². Przewód w oponie okrągłej o średnicy max ø12,5mm.","1566XX0010.jpg","1566XX0010.ldt",1,null,1,9]
["1567","1567XX0009","ARENDAL MINI BOLLARD 37CM LED 466LM 4000K DIM.","Arendal Mini","Bollard","Stal",null,null,null,"LED zintegrowane","AC","DIM.","4W","4W","466lm","345lm",null,null,"65","IK08","Class II",4000,null,0,0,0,"CE",null,null,"> 50 000h",1,"Oprawa słupkowa.","Światło odkryte.",null,"A luminaire with a modern design, combining a decorative crystal lampshade with a durable and stable luminaire base",null,null,null,"Stal cynkowana ogniowo.","Stal cynkowana ogniowo i malowana proszkowo.","Klosz- szkło kryształowe satynowane od wewnątrz.","Klosz z upływem czasu może nabierać bursztynowego koloru.",null,"37cm",null,"Oprawa ściemnialna fazowo TRAILING EDGE (TE) - LEADING EDGE (LE)","Moduł LED","Lumens EDC 38C 4W xxx 230V A101 4K",null,null,"Ściemnianie fazowe Lumens LED AC",null,80,null,"203ZX0009, 204GA0009","Zaciski podłączeniowe: max 2x2,5mm², możliwość podłączenia oprawy w pętle max 2x2,5mm². Przewód w oponie okrągłej o średnicy max ø12,5mm.","1567XX0009.jpg","1567XX0009.ldt",1,null,1,9]
["1580","1580XX0017","LILLEHAMMER WALL 2XLED 1008LM UP & DOWN 4º/60º 3000K DIM.","Lillehammer","Wall","Aluminium",null,null,null,"LED zintegrowane","AC","DIM.","5,6W","7,3W","1008lm","126lm",null,null,"65","IK08","Class I",3000,"wąskie / szerokie, obracany korpus",0.18,0.11,0.08,"CE",null,null,">102 000h",12,"Oprawa ścienna.","Światło dwustronne: o kącie 4º do góry i kącie 60º w dół, lub odwrotnie.","Up & Down 4º/60º","Luminaire with a wide range of applications, among others for lighting: wall surfaces, facades and other architectural concepts",null,null,null,"Odlew aluminiowy malowany proszkowo.",null,"Klosz- szkło bezpieczne, optyczne.","Uszczelka silikonowa.","Dławnica EPDM.","góra/dół","wąskie/szerokie","Oprawa ściemnialna fazowo TRAILING EDGE (TE)","2 Moduły LED","Cree DK180501 V8 JB2835 3V 3K","Philips Xitanium 7W 0,35A 20V TE SC 230V [2019]",50000,"Philips Xitanium TE",null,80,"C",null,"Zaciski podłączeniowe: max 3x2,5mm², możliwość podłączenia oprawy w pętle max 3x1,5mm². Przewód w oponie okrągłej o średnicy w zakresie ø7...10,5 mm.","1580XX0017.jpg","1580XX0017.ldt",1,null,1,22]
["1581","1581XX0016","LILLEHAMMER WALL 2XLED 1008LM UP60º & DOWN60º 3000K DIM.","Lillehammer","Wall","Aluminium",null,null,null,"LED zintegrowane","AC","DIM.","5,6W","7,3W","1008lm","216lm",null,null,"65","IK08","Class I",3000,"szerokie góra / szerokie dół",0.18,0.11,0.08,"CE",null,null,">102 000h",12,"Oprawa ścienna.","Światło dwustronne: o kącie 60º do góry i w dół.","Up60º & Down60º","Luminaire with a wide range of applications, among others for lighting: wall surfaces, facades and other architectural concepts",null,null,null,"Odlew aluminiowy malowany proszkowo.",null,"Klosz- szkło bezpieczne, optyczne.","Uszczelka silikonowa.","Dławnica EPDM.","góra/dół","szerokie/szerokie","Oprawa ściemnialna fazowo TRAILING EDGE (TE)","2 Moduły LED","Cree DK180501 V8 JB2835 3V 3K","Philips Xitanium 7W 0,35A 20V TE SC 230V [2019]",50000,"Philips Xitanium TE",null,80,"C",null,"Zaciski podłączeniowe: max 3x2,5mm², możliwość podłączenia oprawy w pętle max 3x1,5mm². Przewód w oponie okrągłej o średnicy w zakresie ø7...10,5 mm.","1581XX0016.jpg","1581XX0016.ldt",1,null,1,13]
["1582","1582XX0016","LILLEHAMMER WALL LED 504LM DOWN60º 3000K DIM. TE","Lillehammer","Wall","Aluminium",null,null,null,"LED zintegrowane","AC","DIM. TE","2,8W","4W","504lm","107lm",null,null,"65","IK08","Class I",3000,"szerokie dół",0.18,0.11,0.08,"CE",null,null,"> 102 000h",12,"Oprawa ścienna.","Światło jednostronne: o kącie 60º w dół.","Down60º","A luminaire with a wide range of applications, including lighting wall surfaces, facades and other architectural concepts",null,null,null,"Odlew aluminiowy malowany proszkowo.",null,"Klosz- szkło bezpieczne, przeźroczyste.","Uszczelka silikonowa.","Dławnica EPDM.","dół","szerokie","Oprawa ściemnialna fazowo TRAILING EDGE (TE)","Moduł LED","Cree DK180501 V8 JB2835 3V 3K","Philips Xitanium 7W 0,35A 20V TE SC 230V [2019]",50000,"Philips Xitanium TE",null,80,"C",null,"Zaciski podłączeniowe: max 3x2,5mm², możliwość podłączenia oprawy w pętle max 3x1,5mm². Przewód w oponie okrągłej o średnicy w zakresie ø7...10,5 mm.","1582XX0016.jpg","1582XX0016.ldt",1,null,1,38]
["1583","1583XX0017","LILLEHAMMER WALL 2XLED 1008LM UP4º & DOWN4º 3000K DIM.","Lillehammer","Wall","Aluminium",null,null,null,"LED zintegrowane","AC","DIM.","5,6W","7,3W","1008lm","34lm",null,null,"65","IK08","Class I",3000,"wąskie góra / wąskie dół",0.18,0.11,0.08,"CE",null,null,"> 102 000h",12,"Oprawa ścienna.","Światło dwustronne: o kącie 4º do góry i w dół.","Up4º & Down4º","A luminaire with a wide range of applications, including lighting: wall surfaces, facades and other architectural concepts",null,null,null,"Odlew aluminiowy malowany proszkowo.",null,"Klosz- szkło bezpieczne, optyczne.","Uszczelka silikonowa.","Dławnica EPDM.","góra/dół","wąskie/wąskie","Oprawa ściemnialna fazowo TRAILING EDGE (TE)","2 Moduły LED","Cree DK180501 V8 JB2835 3V 3K","Philips Xitanium 7W 0,35A 20V TE SC 230V [2019]",50000,"Philips Xitanium TE",null,80,"C",null,"Zaciski podłączeniowe: max 3x2,5mm², możliwość podłączenia oprawy w pętle max 3x1,5mm². Przewód w oponie okrągłej o średnicy w zakresie ø7...10,5 mm.","1583XX0017.jpg","1583XX0017.ldt",1,null,1,14]
["1584","1584XX0017","LILLEHAMMER WALL LED 504LM DOWN 4º 3000K DIM.","Lillehammer","Wall","Aluminium",null,null,null,"LED zintegrowane","AC","DIM.","2,8W","4W","504lm","17lm",null,null,"65","IK08","Class I",3000,"wąskie dół",0.18,0.11,0.08,"CE",null,null,"> 102 000h",12,"Oprawa ścienna.","Światło jednostronne: o kącie 4º w dół.","Down 4º","A luminaire with a wide range of applications, including lighting wall surfaces, facades and other architectural concepts",null,null,null,"Odlew aluminiowy malowany proszkowo.",null,"Klosz- szkło bezpieczne, optyczne.","Uszczelka silikonowa.","Dławnica EPDM.","dół","wąskie","Oprawa ściemnialna fazowo TRAILING EDGE (TE)","Moduł LED","Cree DK180501 V8 JB2835 3V 3K","Philips Xitanium 7W 0,35A 20V TE SC 230V [2019]",50000,"Philips Xitanium TE",null,80,"C",null,"Zaciski podłączeniowe: max 3x2,5mm², możliwość podłączenia oprawy w pętle max 3x1,5mm². Przewód w oponie okrągłej o średnicy w zakresie ø7...10,5 mm.","1584XX0017.jpg","1584XX0017.ldt",1,null,1,40]
["1585","1585XX0009","LILLEHAMMER WALL LED 504LM UP 4º 3000K DIM.","Lillehammer","Wall","Aluminium",null,null,null,"LED zintegrowane","AC","DIM.","2,8W","4W","504lm","17lm",null,null,"65","IK08","Class I",3000,"wąskie góra",0.18,0.11,0.08,"CE",null,null,"> 102 000h",12,"Oprawa ścienna.","Światło jednostronne: o kącie 4º do góry.","Up 4º","A luminaire with a wide range of applications, including lighting wall surfaces, facades and other architectural concepts",null,null,null,"Odlew aluminiowy malowany proszkowo.",null,"Klosz- szkło bezpieczne, optyczne.","Uszczelka silikonowa.","Dławnica EPDM.","góra","wąskie","Oprawa ściemnialna fazowo TRAILING EDGE (TE)","Moduł LED","Cree DK180501 V8 JB2835 3V 3K","Philips Xitanium 7W 0,35A 20V TE SC 230V [2019]",50000,null,null,80,"C",null,"Zaciski podłączeniowe: max 3x2,5mm², możliwość podłączenia oprawy w pętle max 3x1,5mm². Przewód w oponie okrągłej o średnicy w zakresie ø7mm ...10,5 mm.","1585XX0009.jpg","1585XX0009.ldt",1,null,1,39]
["1586","1586XX0010","LILLEHAMMER WALL LED 534LM UP 4º 4000K DIM.","Lillehammer","Wall","Aluminium",null,null,null,"LED zintegrowane","AC","DIM.","2,8W","4W","534lm","18lm",null,null,"65","IK08","Class I",4000,"wąskie góra",0.18,0.11,0.08,"CE",null,null,"> 102 000h",12,"Oprawa ścienna.","Światło jednostronne: o kącie 4º do góry.","Up 4º","A luminaire with a wide range of applications, including lighting wall surfaces, facades and other architectural concepts",null,null,null,"Odlew aluminiowy malowany proszkowo.",null,"Klosz- szkło bezpieczne, optyczne.","Uszczelka silikonowa.","Dławnica EPDM.","góra","wąskie","Oprawa ściemnialna fazowo TRAILING EDGE (TE)","Moduł LED","Cree DK180501 V8 JB2835 3V 4K","Philips Xitanium 7W 0,35A 20V TE SC 230V [2019]",50000,null,null,80,"C",null,"Zaciski podłączeniowe: max 3x2,5mm², możliwość podłączenia oprawy w pętle max 3x1,5mm². Przewód w oponie okrągłej o średnicy w zakresie ø7mm ...10,5 mm.","1586XX0010.jpg","1586XX0010.ldt",1,null,1,39]
["1587","1587XX0009","LILLEHAMMER WALL LED 504LM UP60º 3000K DIM.","Lillehammer","Wall","Aluminium",null,null,null,"LED zintegrowane","AC","DIM.","2,8W","4W","504lm","108lm",null,null,"65","IK08","Class I",3000,"szerokie góra",0.18,0.11,0.08,"CE",null,null,"> 102 000h",12,"Oprawa ścienna.","Światło jednostronne: o kącie 60º w górę.","Up60º","A luminaire with a wide range of applications, including lighting wall surfaces, facades and other architectural concepts",null,null,null,"Odlew aluminiowy malowany proszkowo.",null,"Klosz- szkło bezpieczne, przeźroczyste.","Uszczelka silikonowa.","Dławnica EPDM.","dół","szerokie","Oprawa ściemnialna fazowo TRAILING EDGE (TE)","Moduł LED","Cree DK180501 V8 JB2835 3V 3K","Philips Xitanium 7W 0,35A 20V TE SC 230V [2019]",50000,"Philips Xitanium TE",null,80,"C",null,"Zaciski podłączeniowe: max 3x2,5mm², możliwość podłączenia oprawy w pętle max 3x1,5mm². Przewód w oponie okrągłej o średnicy w zakresie ø7 mm-10,5 mm.","1587XX0009.jpg","1587XX0009.ldt",1,null,1,65]
["1588","1588XX0009","LILLEHAMMER WALL LED 534LM UP60º 4000K DIM.","Lillehammer","Wall","Aluminium",null,null,null,"LED zintegrowane","AC","DIM.","2,8W","4W","534lm","135lm",null,null,"65","IK08","Class I",4000,"szerokie góra",0.18,0.11,0.08,"CE",null,null,"> 102 000h",12,"Oprawa ścienna.","Światło jednostronne: o kącie 60º w górę.","Up60º","A luminaire with a wide range of applications, including lighting wall surfaces, facades and other architectural concepts",null,null,null,"Odlew aluminiowy malowany proszkowo.",null,"Klosz- szkło bezpieczne, przeźroczyste.","Uszczelka silikonowa.","Dławnica EPDM.","dół","szerokie","Oprawa ściemnialna fazowo TRAILING EDGE (TE)","Moduł LED","Cree DK180501 V8 JB2835 3V 4K","Philips Xitanium 7W 0,35A 20V TE SC 230V [2019]",50000,"Philips Xitanium TE",null,80,"C",null,"Zaciski podłączeniowe: max 3x2,5mm², możliwość podłączenia oprawy w pętle max 3x1,5mm². Przewód w oponie okrągłej o średnicy w zakresie ø7 mm-10,5 mm.","1588XX0009.jpg","1588XX0009.ldt",1,null,1,65]
["1592","1592XX0012","SANDE FLOODLIGHT-BOX LED GU10 375LM 36D 3000K DIM.","Sande,Stick","Spot,Ground","Aluminium",null,null,null,"Wymienne","GU10",null,"5,5W","5,5W","375lm","276lm",null,null,"65","IK08","Class I",3000,null,null,null,null,"CE",null,null,"40000",4,"Oprawa typu reflektor.","Światło symetryczne o kącie 36D","36D","Reflector type luminaire for permanent mounting. For lighting gardens and other private areas and public spaces. Possibility to adjust the direction of light in the vertical plane.",null,null,"Oprawa wyposażona w wymienne źródło światła typu lampa LED o trzonku Gu10, która zapewnia trwałość i optymalny rozsył światła, przy zachowaniu stosunkowo małego zużycia energii.","Odlew aluminiowy malowany proszkowo.",null,"Klosz- szkło bezpieczne, przeźroczyste.","Uszczelka silikonowa.","Dławnica nylon6.","Szpic",null,"Oprawa ściemnialna fazowo TRAILING EDGE (TE) - LEADING EDGE (LE)","Lampa LED GU10","Philips MASTER LED ExpertColor 5.5-50W GU10 930 36D",null,0,"Ściemnianie fazowe LED GU10 E27",null,90,"G","1233XX0009","Oprawa wyposażona w przewód typu H05RN-F 3G1 o długości 5m. Do podłączenia w odpowiednio dobranej puszcze elektroinstalacyjnej.","1592XX0012.jpg","1592XX0012.ldt",1,"GU10",4,68]
["1593","1593XX0015","SANDE FLOODLIGHT-EARTHSPIKE LED 854LM 40D 3000K DIM.","Sande,Stick","Spot,Ground","Aluminium",null,null,null,"LED zintegrowane","AC","DIM.","7W","8,6W","854lm","566lm",null,null,"65","IK08","Class I",3000,null,0.19,0.1,0.1,"CE",null,null,"> 145 000h",17,"Oprawa typu reflektor, przenośna gruntowa.","Światło symetryczne o kącie 40D","40D","Fixed and portable spotlight. For lighting private areas, parks, and other architectural concepts. Possibility to adjust the lighting direction vertically",null,null,null,"Odlew aluminiowy malowany proszkowo.",null,"Klosz- szkło bezpieczne, przeźroczyste.","Uszczelka silikonowa.","Dławnica nylon6.","Szpic",null,"Oprawa ściemnialna fazowo TRAILING EDGE (TE)","Moduł LED","Cree DK1305003 V2 XPG3 3K","Philips Xitanium 7W 0,35A 20V TE SC 230V [2017]",50000,"Philips Xitanium TE",null,90,"D","1233XX0009, 145ZX0009, 146ZX0009","Oprawa wyposażona w przewód typu H05RN-F 3G1 o długości 5m. Do podłączenia w odpowiednio dobranej puszce elektroinstalacyjnej.","1593XX0015.jpg","1593XX0015.ldt",1,null,4,29]
["1594","1594XX0014","SANDE FLOODLIGHT-BOX LED 854LM 40D 3000K DIM.","Sande,Base","Spot,Ground/Wall","Aluminium",null,null,null,"LED zintegrowane","AC","DIM.","7W","8,6W","854lm","738lm",null,null,"65","IK08","Class I",3000,null,0.15,0.09,0.24,"CE",null,null,"> 145 000h",4,"Oprawa typu reflektor.","Światło symetryczne o kącie 40D","40D","Spotlight for lighting private areas, parks, and other concepts architectural. The light direction can be adjusted vertically and horizontally",null,null,null,"Odlew aluminiowy malowany proszkowo.",null,"Klosz- szkło bezpieczne, przeźroczyste.","Uszczelka silikonowa.","Dławnica nylon6.","ramię krótkie",null,"Oprawa ściemnialna fazowo TRAILING EDGE (TE)","Moduł LED","Cree DK1305003 V2 XPG3 3K","Philips Xitanium 7W 0,35A 20V TE SC 230V [2017]",50000,"Philips Xitanium TE",null,80,"D","1233XX0009, 1234ZX0009","Zaciski podłączeniowe: max 3x2,5mm², możliwość podłączenia oprawy w pętle max 3x1,5mm². Przewód w oponie okrągłej o średnicy ø6...10,5mm.","1594XX0014.jpg","1594XX0014.ldt",1,null,4,29]
["1598","1598XX0012","SANDE FLOODLIGHT-BOX LED GU10 375LM 36D 3000K DIM.","Sande,Base","Spot,Ground/Wall","Aluminium",null,null,null,"Wymienne","GU10",null,"5,5W","5,5W","375lm","276lm",null,null,"65","IK08","Class I",3000,null,null,null,null,"CE",null,null,"40000",4,"Oprawa typu reflektor.","Światło symetryczne o kącie 36D","36D","Reflector type luminaire for permanent mounting. For lighting gardens and other private areas and public spaces. Possibility to adjust the direction of light in the vertical and horizontal plane.",null,null,null,"Odlew aluminiowy malowany proszkowo.",null,"Klosz- szkło bezpieczne, przeźroczyste.","Uszczelka silikonowa.","Dławnica nylon6.","ramię krótkie",null,"Oprawa ściemnialna fazowo TRAILING EDGE (TE) - LEADING EDGE (LE)","Lampa LED GU10","Philips MASTER LED ExpertColor 5.5-50W GU10 930 36D",null,0,"Ściemnianie fazowe LED GU10 E27",null,90,"G","1233XX0009, 1234ZX0009","Zaciski podłączeniowe: max 3x2,5mm², możliwość podłączenia oprawy w pętle max 3x1,5mm². Przewód w oponie okrągłej o średnicy ø6...10,5mm.","1598XX0012.jpg","1598XX0012.ldt",1,"GU10",4,68]
["1600","1600XX0013","STOCKHOLM WALL LED 743LM 3000K DIM.","Stockholm,Połówka","Wall,Ceiling","Stal",null,null,null,"LED zintegrowane","AC","DIM.","8W","8W","743lm","240lm",null,null,"54","IK10","Class I",3000,null,0,0,0,"CE",null,null,"50 000h",12,"Oprawa ścienna.","Światło rozproszone.",null,"Luminaire with Scandinavian design. For lighting gardens, private areas and other architectural concepts",null,null,null,null,"Front- stal cynkowana ogniowo, stal malowana proszkowo.","Klosz- poliwęglan mleczny, stabilizowany UV.","Uszczelka silikonowa.","Podstawa- odlew aluminiowy malowany proszkowo.",null,"mleczny","Oprawa ściemnialna fazowo TRAILING EDGE (TE) - LEADING EDGE (LE)","Moduł LED","Lumens EDC 57C 8W xxx 230V F201 3K",null,0,"Ściemnianie fazowe Lumens LED AC",null,80,"F",null,"Zaciski podłączeniowe: max 3x2,5mm², możliwość podłączenia oprawy w pętle max 3x1,5mm². Przewód w oponie okrągłej o średnicy ø7...10,5mm.","1600XX0013.jpg","1600XX0013.ldt",1,null,1,7]
["160","160XX0010","PARIS SMALL WALL E27 DOWN","Paris","Wall","Stal",null,null,null,"Wymienne","E27",null,"LED max 9W","LED max 9W",null,null,null,null,"43",null,"Class I",null,null,0.23,0.14000000000000001,0.12,"CE",null,null,null,12,"Oprawa ścienna.","Światło rozproszone półsferyczne ukierunkowane w dół",null,"A luminaire with a classic and simple design for general use",null,null,"Oprawa na wymienne źródło światła typu: lampa LED o trzonku E27. Źródło światła należy dokupić oddzielnie.","Stal cynkowana ogniowo. Miedź naturalna.","Stal malowana proszkowo.","Klosz- poliwęglan satynowany, stabilizowany UV.",null,"Dławnica EPDM.",null,null,null,"Lampa E27","LED A55...60",null,0,null,null,80,null,"46999021","Zaciski podłączeniowe: max 3x2,5mm², możliwość podłączenia oprawy w pętle max 3x1,5mm². Przewód w oponie okrągłej o średnicy ø7...10,5mm.","160XX0010.jpg","160XX0010.ldt",4,"E27",1,76]
["1620","1620XX0013","NORDKAPP WALL LED 1419LM 3000K DIM.","Nordkapp","Wall,Ceiling","Aluminium",null,null,null,"LED zintegrowane","AC","DIM.","16W","16W","1419lm","471lm",null,null,"65",null,"Class I",3000,null,0,0,0,"CE",null,null,"50 000h",12,"Oprawa ścienna.","Światło rozproszone.",null,"A ceiling-type luminaire with a modern design. For lighting private areas and other architectural concepts",null,null,null,"Odlew aluminiowy malowany proszkowo.",null,"Klosz- poliwęglan mleczny, stabilizowany UV.","Uszczelka silikonowa.","Dławnica EPDM.",null,null,"Oprawa ściemnialna fazowo TRAILING EDGE (TE) - LEADING EDGE (LE)","Moduł LED","Lumens DLM 100C 16W 830 230V F201 V0,5 3K",null,0,"Ściemnianie fazowe Lumens LED AC",null,80,"F",null,"Zaciski podłączeniowe: max 3x2,5mm², możliwość podłączenia oprawy w pętle max 3x1,5mm². Przewód w oponie okrągłej o średnicy ø7...10,5mm.","1620XX0013.jpg","1620XX0013.ldt",1,null,1,7]
["1630","1630XX0012","RENA IN-GROUND LED GU10","Rena","Recessed","Aluminium",null,null,null,"Wymienne","GU10",null,"LED max 6W","LED max 6W",null,null,null,null,"68","IK10","Class I",null,null,0.13,0.13,0.18,"CE",null,null,null,14,"Oprawa wbudowana w podłoże.","Czterostronny wylot światła przysłonięty od góry.",null,"An orientation luminaire that can be driven on by vehicles with pneumatic tires. Luminaires should not be used on traffic lanes where they would be exposed to horizontal weight load as a result of sudden braking, acceleration, and change of direction",null,null,"Oprawa na wymienne źródło światła typu lampa LED o trzonku Gu10, która zapewnia trwałość i optymalny rozsył światła, przy zachowaniu stosunkowo małego zużycia energii. Źródło światła należy dokupić oddzielnie.","Odlew aluminiowy malowany proszkowo.",null,"Klosz- poliwęglan satynowany, stabilizowany UV.","Uszczelka silikonowa.","Dławnica mosiężna niklowana.",null,"Okrąg",null,"Lampa LED GU10","PAR16",null,0,null,null,80,null,"139ZX0009, 142ZX0009, 143ZX0009, 145ZX0009, 146ZX0009, 46102506","Oprawa wyposażona w przewód typu 05RN8-F 3G1 o długości 3m. Do podłączenia w odpowiednio dobranej puszce elektroinstalacyjnej. Maksymalne obciążenie oprawy 1000kg.","1630XX0012.jpg","1630XX0012.ldt",4,"GU10",3,16]
["1631","1631XX0011","RENA IN-GROUND LED GU10 375LM 3000K DIM.","Rena","Recessed","Aluminium",null,null,null,"Wymienne","GU10",null,"5,5W","5,5W","375lm","13lm",null,null,"68","IK10","Class I",3000,null,0,0,0,"CE",null,null,"40 000",14,"Oprawa wbudowana w podłoże.","Czterostronny wylot światła przysłonięty od góry.",null,"An orientation luminaire on which vehicles with pneumatic tires can drive. The luminaires should not be used on roads, where they would be exposed to horizontal loads as a result of sudden braking, acceleration and changes in driving direction.",null,null,null,"Odlew aluminiowy malowany proszkowo.",null,"Klosz- poliwęglan satynowany, stabilizowany UV.","Uszczelka silikonowa.","Dławnica mosiężna niklowana.",null,"Okrąg","Oprawa ściemnialna fazowo TRAILING EDGE (TE) - LEADING EDGE (LE)","Lampa LED GU10","Philips MASTER LED ExpertColor 5.5-50W GU10 930 36D",null,0,"Ściemnianie fazowe LED GU10 E27",null,90,"G","139ZX0009, 142ZX0009, 143ZX0009, 145ZX0009, 146ZX0009","Oprawa wyposażona w przewód typu 05RN8-F 3G1 o długości 3m. Do podłączenia w odpowiednio dobranej puszce elektroinstalacyjnej. Maksymalne obciążenie oprawy 1000kg.","1631XX0011.jpg","1631XX0011.ldt",1,"GU10",3,16]
["1632","1632XX0012","RENA IN-GROUND LED GU10","Rena","Recessed","Aluminium",null,null,null,"Wymienne","GU10",null,"LED max 6W","LED max 6W",null,null,null,null,"68","IK10","Class I",null,null,0.13,0.13,0.18,"CE",null,null,null,14,"Oprawa wbudowana w podłoże.","Czterostronny wylot światła przysłonięty od góry.",null,"An orientation luminaire that can be driven on by vehicles with pneumatic tires. Luminaires should not be used on traffic lanes where they would be exposed to horizontal weight load as a result of sudden braking, acceleration, and change of direction",null,null,"Oprawa wyposażona w wymienne źródło światła typu lampa LED o trzonku Gu10, która zapewnia trwałość i optymalny rozsył światła, przy zachowaniu stosunkowo małego zużycia energii.","Odlew aluminiowy malowany proszkowo.",null,"Klosz- poliwęglan satynowany, stabilizowany UV.","Uszczelka silikonowa.","Dławnica mosiężna niklowana.",null,"Kwadrat",null,"Lampa LED GU10","PAR16",null,0,null,null,80,null,"139ZX0009, 142ZX0009, 143ZX0009, 145ZX0009, 146ZX0009, 46102506","Oprawa wyposażona w przewód typu 05RN8-F 3G1 o długości 3m. Do podłączenia w odpowiednio dobranej puszce elektroinstalacyjnej. Maksymalne obciążenie oprawy 1000kg.","1632XX0012.jpg","1632XX0012.ldt",4,"GU10",3,16]
["1633","1633XX0011","RENA IN-GROUND LED GU10 375LM 3000K DIM.","Rena","Recessed","Aluminium",null,null,null,"Wymienne","GU10",null,"5,5W","5,5W","375lm","13lm",null,null,"68","IK10","Class I",3000,null,0,0,0,"CE",null,null,"40000",14,"Oprawa wbudowana w podłoże.","Czterostronny wylot światła przysłonięty od góry.",null,"An orientation luminaire or as a reflector on which vehicles with pneumatic tires can be driven. Luminaires should not be used on standard road lanes, where they would be exposed to horizontal loads as a result of sudden braking, acceleration, and change of direction",null,null,"Oprawa wyposażona w wymienne źródło światła typu lampa LED o trzonku Gu10, która zapewnia trwałość i optymalny rozsył światła, przy zachowaniu stosunkowo małego zużycia energii.","Odlew aluminiowy malowany proszkowo.",null,"Klosz- poliwęglan satynowany, stabilizowany UV.","Uszczelka silikonowa.","Dławnica mosiężna niklowana.",null,"Kwadrat","Oprawa ściemnialna fazowo TRAILING EDGE (TE) - LEADING EDGE (LE)","Lampa LED GU10","Philips MASTER LED ExpertColor 5.5-50W GU10 930 36D",null,0,"Ściemnianie fazowe LED GU10 E27",null,90,"G","139ZX0009, 142ZX0009, 143ZX0009, 145ZX0009, 146XZ0009","Oprawa wyposażona w przewód typu 05RN8-F 3G1 o długości 3m. Do podłączenia w odpowiednio dobranej puszce elektroinstalacyjnej. Maksymalne obciążenie oprawy 1000kg.","1633XX0011.jpg","1633XX0011.ldt",1,"GU10",3,16]
["163","163XX0010","PARIS WALL E27 DOWN","Paris,Big","Wall","Stal",null,null,null,"Wymienne","E27",null,"LED max 9W","LED max 9W",null,null,null,null,"43",null,"Class I",null,null,0.28000000000000003,0.16,0.14000000000000001,"CE",null,null,null,12,"Oprawa ścienna.","Światło rozproszone półsferyczne ukierunkowane w dół",null,"Classic design luminaire with a wide range of applications for example for illumination of walls and facade surfaces or any other architectural concepts.",null,null,"Oprawa na wymienne źródło światła typu: lampa LED, świetlówka TC-SE, tradycyjna żarówka (halogenowa) o trzonku E27. Źródło światła należy dokupić oddzielnie.","Stal cynkowana ogniowo.","Stal malowana proszkowo.","Klosz- poliwęglan satynowany, stabilizowany UV.",null,"Dławnica EPDM.",null,null,null,"Lampa E27","LED A55..60",null,0,null,null,80,null,"46999021","Zaciski podłączeniowe: max 3x2,5mm², możliwość podłączenia oprawy w pętle max 3x1,5mm². Przewód w oponie okrągłej o średnicy ø7...10,5mm.","163XX0010.jpg","163XX0010.ldt",4,"E27",1,76]
["1640","1640XX0009","RENA IN-GROUND LED GU10 375LM 36D 3000K DIM.","Rena","Recessed","Stal nierdzewna",null,null,null,"Wymienne","GU10",null,"5,5W","5,5W","375lm","367lm",null,null,"68",null,"Class I",3000,null,0,0,0,"CE",null,null,"40000",14,"Oprawa wbudowana w podłoże.","Światło symetryczne o kącie 36D","36D","An orientation luminaire that can be driven on by vehicles with pneumatic tires. Luminaires should not be used on traffic lanes where they would be exposed to horizontal weight load as a result of sudden braking, acceleration, and change of direction. The light direction angle can be adjusted, up to a maximum of 10 degrees",null,null,null,"Odlew aluminiowy malowany proszkowo.","Front- stal nierdzewna.","Klosz- szkło bezpieczne, przeźroczyste.","Uszczelka silikonowa.","Dławnica mosiężna niklowana.","Przeźroczysty","Okrąg","Oprawa ściemnialna fazowo TRAILING EDGE (TE) - LEADING EDGE (LE)","Lampa LED GU10","Philips MASTER LED ExpertColor 5.5-50W GU10 930 36D",null,0,"Ściemnianie fazowe LED GU10 E27",null,90,"G","139ZX0009, 144ZX0009, 146ZX0009","Oprawa wyposażona w dedykowany system montażu i podłączeniowe złącze hermetyczne. Przewód w oponie okrągłej max 3 x 1,5...2.5 mm², o średnicy 9...12mm. Maksymalne obciążenie oprawy 2000kg. Uwaga: na powierzchni szklanej w punkcie środkowym, osiągane są temperatury robocze zgodne z normą 60598 ( temperatura otoczenia 15ºC).","1640XX0009.jpg","1640XX0009.ldt",1,"GU10",3,68]
["1641","1641XX0009","RENA IN-GROUND LED GU10 375LM 36D 3000K DIM.","Rena","Recessed","Stal nierdzewna",null,null,null,"Wymienne","GU10",null,"5,5W","5,5W","375lm","367lm",null,null,"68",null,"Class I",3000,null,0,0,0,"CE",null,null,"40000",14,"Oprawa wbudowana w podłoże.","Światło symetryczne o kącie 36D","36D","An orientation luminaire or as a reflector on which vehicles with pneumatic tires can be driven. Luminaires should not be used on road lanes where they would be exposed to horizontal loads as a result of sudden braking, acceleration, and direction changes. The angle of the lighting direction can be adjusted, up to a maximum of 10 degrees",null,null,null,"Odlew aluminiowy malowany proszkowo.","Front- stal nierdzewna.","Klosz- szkło bezpieczne, przeźroczyste.","Uszczelka silikonowa.","Dławnica mosiężna niklowana.","Przeźroczysty","Kwadrat","Oprawa ściemnialna fazowo TRAILING EDGE (TE) - LEADING EDGE (LE)","Lampa LED GU10","Philips MASTER LED ExpertColor 5.5-50W GU10 930 36D",null,0,"Ściemnianie fazowe LED GU10 E27",null,90,"G","139ZX0009, 144ZX0009, 146ZX0009","Oprawa wyposażona w dedykowany system montażu i podłączeniowe złącze hermetyczne. Przewód w oponie okrągłej max 3 x 1,5...2.5 mm², o średnicy 9...12mm. Maksymalne obciążenie oprawy 2000kg. Uwaga: na powierzchni szklanej w punkcie środkowym, osiągane są temperatury robocze zgodne z normą 60598 ( temperatura otoczenia 15ºC).","1641XX0009.jpg","1641XX0009.ldt",1,"GU10",3,68]
["1642","1642XX0009","RENA IN-GROUND LED GU10","Rena","Recessed","Stal nierdzewna",null,null,null,"Wymienne","GU10",null,"max 6W",null,null,null,null,null,"68",null,"Class I",null,null,0,0,0,"CE",null,null,null,14,"Oprawa wbudowana w podłoże.","Światło odkryte.",null,"An orientation luminaire or as a driveable reflector with pneumatic tires. Luminaires should not be used on road lanes where they would be exposed to horizontal loads as a result of sudden braking, acceleration, and direction changes. The angle of the lighting direction can be adjusted, up to a maximum of 10 degrees",null,null,null,"Odlew aluminiowy malowany proszkowo.","Front- stal nierdzewna.","Klosz- szkło bezpieczne, przeźroczyste.","Uszczelka silikonowa.","Dławnica mosiężna niklowana.","Przeźroczysty","Okrąg",null,"Lampa LED GU10","PAR16",null,null,null,null,80,null,"139ZX0009, 144ZX0009, 146ZX0009, 46102506","Oprawa wyposażona w dedykowany system montażu i podłączeniowe złącze hermetyczne. Przewód w oponie okrągłej max 3 x 1,5...2.5 mm², o średnicy 9...12mm. Maksymalne obciążenie oprawy 2000kg. Uwaga: na powierzchni szklanej w punkcie środkowym, osiągane są temperatury robocze zgodne z normą 60598 ( temperatura otoczenia 15ºC).","1642XX0009.jpg","1642XX0009.ldt",4,"GU10",3,9]
["1643","1643XX0009","RENA IN-GROUND LED GU10","Rena","Recessed","Stal nierdzewna",null,null,null,"Wymienne","GU10",null,"max 6W",null,null,null,null,null,"68",null,"Class I",null,null,0,0,0,"CE",null,null,null,14,"Oprawa wbudowana w podłoże.","Światło odkryte.",null,"An orientation luminaire or as a driveable reflector with pneumatic tires. Luminaires should not be used on the road lanes where they would be exposed to horizontal loads as a result of sudden braking, acceleration, and direction changes. The angle of the lighting direction can be adjusted, up to a maximum of 10 degrees",null,null,null,"Odlew aluminiowy malowany proszkowo.","Front- stal nierdzewna.","Klosz- szkło bezpieczne, przeźroczyste.","Uszczelka silikonowa.","Dławnica mosiężna niklowana.","Przeźroczysty","Kwadrat",null,"Lampa LED GU10","PAR16",null,null,null,null,80,null,"139ZX0009, 144ZX0009, 146ZX0009","Oprawa wyposażona w dedykowany system montażu i podłączeniowe złącze hermetyczne. Przewód w oponie okrągłej max 3 x 1,5...2.5 mm², o średnicy 9...12mm. Maksymalne obciążenie oprawy 2000kg. Uwaga: na powierzchni szklanej w punkcie środkowym, osiągane są temperatury robocze zgodne z normą 60598 ( temperatura otoczenia 15ºC).","1643XX0009.jpg","1643XX0009.ldt",4,"GU10",3,9]
["1644","1644XX0009","RENA IN-GROUND LED GU10 375LM 36D 3000K DIM.","Rena","Recessed","Stal nierdzewna",null,null,null,"Wymienne","GU10",null,"5,5W","5,5W","375lm","237lm",null,null,"68",null,"Class I",3000,null,0.13,0.13,0.28000000000000003,"CE",null,null,"40000",14,"Oprawa wbudowana w podłoże.","Światło symetryczne o kącie 36D","36D","An orientation luminaire or as a reflector on which vehicles with pneumatic tires can be driven. Luminaires should not be used on the road lanes where they would be exposed to horizontal loads as a result of sudden braking, acceleration, and direction changes. The angle of the lighting direction can be adjusted, up to a maximum of 10 degrees",null,null,null,"Odlew aluminiowy malowany proszkowo.","Front- stal nierdzewna.","Klosz- szkło bezpieczne, satynowane.","Uszczelka silikonowa.","Dławnica mosiężna niklowana.","Satynowany","Okrąg","Oprawa ściemnialna fazowo TRAILING EDGE (TE) - LEADING EDGE (LE)","Lampa LED GU10","Philips MASTER LED ExpertColor 5.5-50W GU10 930 36D",null,0,"Ściemnianie fazowe LED GU10 E27",null,90,"G","139ZX0009, 144ZX0009, 146ZX0009","Oprawa wyposażona w dedykowany system montażu i podłączeniowe złącze hermetyczne. Przewód w oponie okrągłej max 3 x 1,5...2.5 mm², o średnicy 9...12mm. Maksymalne obciążenie oprawy 2000kg. Uwaga: na powierzchni szklanej w punkcie środkowym, osiągane są temperatury robocze zgodne z normą 60598 ( temperatura otoczenia 15ºC).","1644XX0009.jpg","1644XX0009.ldt",1,"GU10",3,68]
["1645","1645XX0009","RENA IN-GROUND LED GU10 375LM 36D 3000K DIM.","Rena","Recessed","Stal nierdzewna",null,null,null,"Wymienne","GU10",null,"5,5W","5,5W","375lm","237lm",null,null,"68",null,"Class I",3000,null,0,0,0,"CE",null,null,"40000",14,"Oprawa wbudowana w podłoże.","Światło symetryczne o kącie 36D","36D","An orientation luminaire or as a reflector on which vehicles with pneumatic tires can be driven. Luminaires should not be used on the road lanes where they would be exposed to horizontal loads as a result of sudden braking, acceleration, and direction changes. The angle of the lighting direction can be adjusted, up to a maximum of 10 degrees",null,null,null,"Odlew aluminiowy malowany proszkowo.","Front- stal nierdzewna.","Klosz- szkło bezpieczne, satynowane.","Uszczelka silikonowa.","Dławnica mosiężna niklowana.","Satynowany","Kwadrat","Oprawa ściemnialna fazowo TRAILING EDGE (TE) - LEADING EDGE (LE)","Lampa LED GU10","Philips MASTER LED ExpertColor 5.5-50W GU10 930 36D",null,0,"Ściemnianie fazowe LED GU10 E27",null,90,"G","139ZX0009, 144ZX0009, 146ZX0009","Oprawa wyposażona w dedykowany system montażu i podłączeniowe złącze hermetyczne. Przewód w oponie okrągłej max 3 x 1,5...2.5 mm², o średnicy 9...12mm. Maksymalne obciążenie oprawy 2000kg. Uwaga: na powierzchni szklanej w punkcie środkowym, osiągane są temperatury robocze zgodne z normą 60598 ( temperatura otoczenia 15ºC).","1645XX0009.jpg","1645XX0009.ldt",1,"GU10",3,68]
["1646","1646XX0009","RENA IN-GROUND LED GU10","Rena","Recessed","Stal nierdzewna",null,null,null,"Wymienne","GU10",null,"max 6W",null,null,null,null,null,"68",null,"Class I",null,null,0,0,0,"CE",null,null,null,14,"Oprawa wbudowana w podłoże.","Światło rozproszone.",null,"An orientation luminaire or as a driveable reflector with pneumatic tires. Luminaires should not be used on the road lanes where they would be exposed to horizontal loads as a result of sudden braking, acceleration, and direction changes. The angle of the lighting direction can be adjusted, up to a maximum of 10 degrees",null,null,null,"Odlew aluminiowy malowany proszkowo.","Front- stal nierdzewna.","Klosz- szkło bezpieczne, satynowane.","Uszczelka silikonowa.","Dławnica mosiężna niklowana.","Satynowany","Okrąg",null,"Lampa LED GU10","PAR16",null,null,null,null,80,null,"139ZX0009, 144ZX0009, 146ZX0009, 46102506","Oprawa wyposażona w dedykowany system montażu i podłączeniowe złącze hermetyczne. Przewód w oponie okrągłej max 3 x 1,5...2.5 mm², o średnicy 9...12mm. Maksymalne obciążenie oprawy 2000kg. Uwaga: na powierzchni szklanej w punkcie środkowym, osiągane są temperatury robocze zgodne z normą 60598 ( temperatura otoczenia 15ºC).","1646XX0009.jpg","1646XX0009.ldt",4,"GU10",3,7]
["1647","1647XX0009","RENA IN-GROUND LED GU10","Rena","Recessed","Stal nierdzewna",null,null,null,"Wymienne","GU10",null,"max 6W",null,null,null,null,null,"68",null,"Class I",null,null,0,0,0,"CE",null,null,null,14,"Oprawa wbudowana w podłoże.","Światło rozproszone.",null,"An orientation luminaire or as a driveable reflector with pneumatic tires. Luminaires should not be used on the road lanes where they would be exposed to horizontal loads as a result of sudden braking, acceleration, and direction changes. The angle of the lighting direction can be adjusted, up to a maximum of 10 degrees",null,null,null,"Odlew aluminiowy malowany proszkowo.","Front- stal nierdzewna.","Klosz- szkło bezpieczne, satynowane.","Uszczelka silikonowa.","Dławnica mosiężna niklowana.","Satynowany","Kwadrat",null,"Lampa LED GU10","PAR16",null,null,null,null,80,null,"139ZX0009, 144ZX0009, 146ZX0009, 46102506","Oprawa wyposażona w dedykowany system montażu i podłączeniowe złącze hermetyczne. Przewód w oponie okrągłej max 3 x 1,5...2.5 mm², o średnicy 9...12mm. Maksymalne obciążenie oprawy 2000kg. Uwaga: na powierzchni szklanej w punkcie środkowym, osiągane są temperatury robocze zgodne z normą 60598 ( temperatura otoczenia 15ºC).","1647XX0009.jpg","1647XX0009.ldt",4,"GU10",3,7]
["1650","1650XX0009","RENA IN-GROUND LED GU10","Rena","Recessed","Aluminium",null,null,null,"Wymienne","GU10",null,"max 6W",null,null,null,null,null,"68",null,"Class I",null,null,0,0,0,"CE",null,null,null,14,"Oprawa wbudowana w podłoże.","Czterostronny wylot światła przysłonięty od góry.",null,"An orientation luminaire on which vehicles with pneumatic tires can be driven. Luminaires should not be used on the road lanes, where they would be exposed to horizontal loads as a result of sudden braking, acceleration, and change of direction",null,null,null,"Odlew aluminiowy malowany proszkowo.",null,"Klosz- poliwęglan satynowany, stabilizowany UV.","Uszczelka silikonowa.","Dławnica mosiężna niklowana.",null,"Okrąg",null,"Lampa LED GU10","PAR16",null,null,null,null,80,null,"139ZX0009, 144ZX0009, 146ZX0009, 46102506","Oprawa wyposażona w dedykowany system montażu i podłączeniowe złącze hermetyczne. Przewód w oponie okrągłej max 3 x 1,5...2.5 mm², o średnicy 9...12mm. Maksymalne obciążenie oprawy 1000kg.","1650XX0009.jpg","1650XX0009.ldt",4,"GU10",3,16]
["1651","1651XX0009","RENA IN-GROUND LED GU10 375LM 3000K DIM.","Rena","Recessed","Aluminium",null,null,null,"Wymienne","GU10",null,"5,5W","5,5W","375lm","13lm",null,null,"68",null,"Class I",3000,null,0,0,0,"CE",null,null,"40 000",14,"Oprawa wbudowana w podłoże.","Czterostronny wylot światła przysłonięty od góry.",null,"An orientation luminaire on which vehicles with pneumatic tires can be driven. Luminaires should not be used on the road lanes, where they would be exposed to horizontal loads as a result of sudden braking, acceleration, and change of direction",null,null,null,"Odlew aluminiowy malowany proszkowo.",null,"Klosz- poliwęglan satynowany, stabilizowany UV.","Uszczelka silikonowa.","Dławnica mosiężna niklowana.",null,"Okrąg","Oprawa ściemnialna fazowo TRAILING EDGE (TE) - LEADING EDGE (LE)","Lampa LED GU10","Philips MASTER LED ExpertColor 5.5-50W GU10 930 36D",null,0,"Ściemnianie fazowe LED GU10 E27",null,90,"G","139ZX0009, 144ZX0009, 146ZX0009","Oprawa wyposażona w dedykowany system montażu i podłączeniowe złącze hermetyczne. Przewód w oponie okrągłej max 3 x 1,5...2.5 mm², o średnicy 9...12mm Maksymalne obciążenie oprawy 1000kg.","1651XX0009.jpg","1651XX0009.ldt",1,"GU10",3,16]
["1652","1652XX0009","RENA IN-GROUND LED GU10","Rena","Recessed","Aluminium",null,null,null,"Wymienne","GU10",null,"max 6W",null,null,null,null,null,"68",null,"Class I",null,null,0,0,0,"CE",null,null,null,14,"Oprawa wbudowana w podłoże.","Czterostronny wylot światła przysłonięty od góry.",null,"An orientation luminaire on which vehicles with pneumatic tires can be driven. Luminaires should not be used on the road lanes, where they would be exposed to horizontal loads as a result of sudden braking, acceleration, and change of direction",null,null,null,"Odlew aluminiowy malowany proszkowo.",null,"Klosz- poliwęglan satynowany, stabilizowany UV.","Uszczelka silikonowa.","Dławnica mosiężna niklowana.",null,"Kwadrat",null,"Lampa LED GU10","PAR16",null,null,null,null,80,null,"139ZX0009, 144ZX0009, 146ZX0009, 46102506","Oprawa wyposażona w dedykowany system montażu i podłączeniowe złącze hermetyczne. Przewód w oponie okrągłej max 3 x 1,5...2.5 mm², o średnicy 9...12mm. Maksymalne obciążenie oprawy 1000kg.","1652XX0009.jpg","1652XX0009.ldt",4,"GU10",3,16]
["1653","1653XX0009","RENA IN-GROUND LED GU10 375LM 3000K DIM.","Rena","Recessed","Aluminium",null,null,null,"Wymienne","GU10",null,"5,5W","5,5W","375lm","13lm",null,null,"68",null,"Class I",3000,null,0,0,0,"CE",null,null,"40000",14,"Oprawa wbudowana w podłoże.","Czterostronny wylot światła przysłonięty od góry.",null,"An orientation luminaire on which vehicles with pneumatic tires can be driven. Luminaires should not be used on the road lanes, where they would be exposed to horizontal loads as a result of sudden braking, acceleration, and change of direction",null,null,null,"Odlew aluminiowy malowany proszkowo.",null,"Klosz- poliwęglan satynowany, stabilizowany UV.","Uszczelka silikonowa.","Dławnica mosiężna niklowana.",null,"Kwadrat","Oprawa ściemnialna fazowo TRAILING EDGE (TE) - LEADING EDGE (LE)","Lampa LED GU10","Philips MASTER LED ExpertColor 5.5-50W GU10 930 36D",null,0,"Ściemnianie fazowe LED GU10 E27",null,90,"G","139ZX0009, 144ZX0009, 146ZX0009","Oprawa wyposażona w dedykowany system montażu i podłączeniowe złącze hermetyczne. Przewód w oponie okrągłej max 3 x 1,5...2.5 mm², o średnicy 9...12mm. Maksymalne obciążenie oprawy 1000kg.","1653XX0009.jpg","1653XX0009.ldt",1,"GU10",3,16]
["1700","1700XX0011","ASKER WALL LED 743LM UP-DOWN 3000K DIM.","Asker","Wall","Stal","Ocynkowane",null,null,"LED zintegrowane","AC","DIM.","8W","8,4W","743lm","360lm",null,null,"44","IK08","Class I",3000,"szerokie góra / szerokie dół",0,0,0,"CE",null,null,"50 000h",12,"Oprawa ścienna.","Światło dwustronne: ukierunkowane do góry i w dół.","Up-Down","A luminaire with a wide range of applications, including lighting wall surfaces, facades and other architectural concepts",null,null,null,null,"Korpus- stal cynkowana ogniowo.","Klosz- poliwęglan przeźroczysty ze strukturą, stabilizowany UV.","Uszczelka silikonowa.","Podstawa- odlew aluminiowy malowany proszkowo.","góra/dół",null,"Oprawa ściemnialna fazowo TRAILING EDGE (TE) - LEADING EDGE (LE)","Moduł LED","Lumens EDC 57C 8W xxx 230V F201 3K",null,0,"Ściemnianie fazowe Lumens LED AC",null,80,"F",null,"Zaciski podłączeniowe: max 3x2,5mm², możliwość podłączenia oprawy w pętle max 3x1,5mm². Przewód w oponie okrągłej o średnicy ø7...10,5mm.","1700XX0011.jpg","1700XX0011.ldt",1,null,1,4]
["1702","1702XX0010","ASKER WALL E27 UP-DOWN","Asker","Wall","Stal","Ocynkowane",null,null,"Wymienne","E27",null,"LED max 9W","LED max 9W",null,null,null,null,"44",null,"Class I",null,"szerokie góra / szerokie dół",0.22,0.11,0.08,"CE",null,null,null,12,"Oprawa ścienna.","Światło dwustronne: ukierunkowane do góry i w dół.","Up-Down","Luminaire with a wide range of applications for example for illumination of walls and facade surfaces or any other architectural concepts.",null,null,"Oprawa na wymienne źródło światła typu: lampa LED, świetlówka TC-SE, tradycyjna żarówka (halogenowa) o trzonku E27. Źródło światła należy dokupić oddzielnie.",null,"Korpus- stal cynkowana ogniowo.","Klosz- poliwęglan przeźroczysty ze strukturą, stabilizowany UV.","Uszczelka silikonowa.","Podstawa- odlew aluminiowy malowany proszkowo.",null,null,null,"Lampa E27","LED A55..60",null,0,null,null,80,null,"46999021","Zaciski podłączeniowe: max 3x2,5mm², możliwość podłączenia oprawy w pętle max 3x1,5mm². Przewód w oponie okrągłej o średnicy ø7...10,5mm.","1702XX0010.jpg","1702XX0010.ldt",4,"E27",1,4]
["1705","1705XX0011","ASKER WALL LED 840LM DOWN 3000K DIM.","Asker","Wall","Stal","Ocynkowane",null,null,"LED zintegrowane","AC","DIM.","8W","8W","840lm","165lm",null,null,"44","IK08","Class I",3000,"szerokie dół",0,0,0,"CE",null,null,"50000",12,"Oprawa ścienna.","Światło rozproszone półsferyczne ukierunkowane w dół",null,"A luminaire with a wide range of applications, including lighting wall surfaces, facades, and other architectural concepts",null,null,null,null,"Korpus- stal cynkowana ogniowo.","Klosz- poliwęglan przeźroczysty ze strukturą, stabilizowany UV.","Uszczelka silikonowa.","Podstawa- odlew aluminiowy malowany proszkowo.",null,null,"Oprawa ściemnialna fazowo TRAILING EDGE (TE) - LEADING EDGE (LE)","Moduł LED","Lumens EDC 57C 8W xxx 230V F201 3K",null,null,"Ściemnianie fazowe Lumens LED AC",null,80,"F",null,"Zaciski podłączeniowe: max 3x2,5mm², możliwość podłączenia oprawy w pętle max 3x1,5mm². Przewód w oponie okrągłej o średnicy ø7...10,5mm.","1705XX0011.jpg","1705XX0011.ldt",1,null,1,76]
["1707","1707XX0010","ASKER WALL E27 DOWN","Asker","Wall","Stal","Ocynkowane",null,null,"Wymienne","E27",null,"LED max 9W","LED max 9W",null,null,null,null,"44","IK08","Class I",null,"szerokie dół",0.22,0.11,0.08,"CE",null,null,null,12,"Oprawa ścienna.","Światło rozproszone półsferyczne ukierunkowane w dół",null,"Luminaire with a wide range of applications for example for illumination of walls and facade surfaces or any other architectural concepts.",null,null,"Oprawa na wymienne źródło światła typu: lampa LED, świetlówka TC-SE, tradycyjna żarówka (halogenowa) o trzonku E27. Źródło światła należy dokupić oddzielnie.",null,"Korpus- stal cynkowana ogniowo.","Klosz- poliwęglan przeźroczysty ze strukturą, stabilizowany UV.","Uszczelka silikonowa.","Podstawa- odlew aluminiowy malowany proszkowo.",null,null,null,"Lampa E27","LED A55..60",null,0,null,null,80,null,"46999021","Zaciski podłączeniowe: max 3x2,5mm², możliwość podłączenia oprawy w pętle max 3x1,5mm². Przewód w oponie okrągłej o średnicy ø7...10,5mm.","1707XX0010.jpg","1707XX0010.ldt",4,"E27",1,76]
["1710","1710XX0011","ASKER BIG WALL 2XLED 1128LM UP-DOWN 3000K DIM.","Asker,Big","Wall","Stal",null,null,null,"LED zintegrowane","AC","DIM.","6,6W","7,1W","1128lm","649lm",null,null,"44","IK08","Class I",3000,"szerokie góra / szerokie dół",null,null,null,"CE",null,null,"> 70000",12,"Oprawa ścienna.","Światło dwustronne: ukierunkowane do góry i w dół.","Up-Down","Luminaire with a wide range of applications for example for illumination of walls and facade surfaces or any other architectural concepts",null,null,null,"Front- stal cynkowana ogniowo.","Korpus- odlew aluminiowy malowany proszkowo.","Klosz- poliwęglan przeźroczysty ze strukturą, stabilizowany UV.","Uszczelka silikonowa.","Dławnica EPDM.",null,null,"Oprawa ściemnialna fazowo TRAILING EDGE (TE)","2 Moduły LED","Philips Fortimo Strip 0,5ft MF FC LV6 3K","Philips Xitanium 8W 0,2A 40V TE SC 230V",0,null,null,80,"C",null,"Zaciski podłączeniowe: max 3x2,5mm², możliwość podłączenia oprawy w pętle max 3x1,5mm². Przewód w oponie okrągłej o średnicy ø7...10,5mm.","1710XX0011.jpg","1710XX0011.ldt",1,null,1,4]
["1712","1712XX0010","ASKER BIG WALL E27 UP-DOWN","Asker,Big","Wall","Stal",null,null,null,"Wymienne","E27",null,"LED max 9W",null,null,null,null,null,"44","IK08","Class I",null,"szerokie góra / szerokie dół",0,0,0,"CE",null,null,null,12,"Oprawa ścienna.","Światło dwustronne: ukierunkowane do góry i w dół.","Up-Down","Luminaire with a wide range of applications for example for illumination of walls and facade surfaces or any other architectural concepts.",null,null,null,"Front- stal cynkowana ogniowo.","Korpus- odlew aluminiowy malowany proszkowo.","Klosz- poliwęglan przeźroczysty ze strukturą, stabilizowany UV.","Uszczelka silikonowa.","Dławnica EPDM.",null,null,null,"Lampa E27","LED A55..60",null,null,null,null,80,null,"46999021","Zaciski podłączeniowe: max 3x2,5mm², możliwość podłączenia oprawy w pętle max 3x1,5mm². Przewód w oponie okrągłej o średnicy ø7...10,5mm.","1712XX0010.jpg","1712XX0010.ldt",4,"E27",1,4]
["1715","1715XX0011","ASKER BIG WALL LED 653LM DOWN 3000K DIM.","Asker,Big","Wall","Stal",null,null,null,"LED zintegrowane","AC","DIM.","4W","5,3W","653lm","347lm",null,null,"44","IK08","Class I",3000,"szerokie dół",null,null,null,"CE",null,null,"> 70000",12,"Oprawa ścienna.","Światło rozproszone półsferyczne ukierunkowane w dół",null,"A luminaire with a wide range of applications, for illuminating wall and facade surfaces as well as other architectural concepts",null,null,null,"Front- stal cynkowana ogniowo.","Korpus- odlew aluminiowy malowany proszkowo.","Klosz- poliwęglan przeźroczysty ze strukturą, stabilizowany UV.","Uszczelka silikonowa.","Dławnica EPDM.",null,null,"Oprawa ściemnialna fazowo TRAILING EDGE (TE)","Moduł LED","Philips Fortimo_LED_Strip_0.5ft_MF_8xx_HV6 3K","Philips Xitanium 7W 0,35A 20V TE SC 230V [2017]",50000,null,0,80,"C",null,"Zaciski podłączeniowe: max 3x2,5mm², możliwość podłączenia oprawy w pętle max 3x1,5mm². Przewód w oponie okrągłej o średnicy ø7...10,5mm.","1715XX0011.jpg","1715XX0011.ldt",1,null,1,76]
["1717","1717XX0010","ASKER BIG WALL E27 DOWN","Asker,Big","Wall","Stal",null,null,null,"Wymienne","E27",null,"LED max 9W",null,null,null,null,null,"44","IK08","Class I",null,"szerokie dół",0,0,0,"CE",null,null,null,12,"Oprawa ścienna.","Światło rozproszone półsferyczne ukierunkowane w dół",null,"Luminaire with a wide range of applications for example for illumination of walls and facade surfaces or any other architectural concepts.",null,null,null,"Front- stal cynkowana ogniowo.","Korpus- odlew aluminiowy malowany proszkowo.","Klosz- poliwęglan przeźroczysty ze strukturą, stabilizowany UV.","Uszczelka silikonowa.","Dławnica EPDM.",null,null,null,"Lampa E27","LED A55..60",null,null,null,null,80,null,"46999021","Zaciski podłączeniowe: max 3x2,5mm², możliwość podłączenia oprawy w pętle max 3x1,5mm². Przewód w oponie okrągłej o średnicy ø7...10,5mm.","1717XX0010.jpg","1717XX0010.ldt",4,"E27",1,76]
["1720","1720XX0010","ASKER SMALL PRO WALL 2XLED 1128LM UP-DOWN 3000K DIM.","Asker","Wall","Aluminium",null,null,"PRO","LED zintegrowane","AC","DIM.","6,6W","8,4W","1128lm","798lm",null,null,"65","IK08","Class I",3000,"szerokie góra / szerokie dół",null,null,null,"CE",null,null,"> 70 000h",12,"Oprawa ścienna.","Światło dwustronne: ukierunkowane do góry i w dół.","Up-Down","A luminaire with a wide range of applications, including lighting wall surfaces, facades, and other architectural concepts",null,null,null,"Odlew aluminiowy malowany proszkowo.",null,"Klosz- poliwęglan przeźroczysty ze strukturą, stabilizowany UV.","Uszczelka silikonowa.","Dławnica EPDM.","góra/dół",null,"Oprawa ściemnialna fazowo TRAILING EDGE (TE)","2 Moduły LED","Philips Fortimo Strip 0,5ft MF FC LV6 3K","Philips Xitanium 8W 0,2A 40V TE SC 230V",0,"Philips Xitanium TE",null,80,"C",null,"Zaciski podłączeniowe: max 3x2,5mm², możliwość podłączenia oprawy w pętle max 3x1,5mm². Przewód w oponie okrągłej o średnicy ø7...10,5mm.","1720XX0010.jpg","1720XX0010.ldt",1,null,1,4]
["1726","1726XX0010","ASKER SMALL PRO WALL LED 653LM DOWN 3000K DIM. TE","Asker","Wall","Aluminium",null,null,"PRO","LED zintegrowane","AC","DIM. TE","3,9W","5,4W","653lm","429lm",null,null,"65","IK08","Class I",3000,"szerokie dół",null,null,null,"CE",null,null,"> 70000",12,"Oprawa ścienna.","Światło rozproszone półsferyczne ukierunkowane w dół",null,"A luminaire with a wide range of applications, including lighting wall surfaces, facades, and other architectural concepts",null,null,null,"Odlew aluminiowy malowany proszkowo.",null,"Klosz- poliwęglan przeźroczysty ze strukturą, stabilizowany UV.","Uszczelka silikonowa.","Dławnica EPDM.","dół",null,"Oprawa ściemnialna fazowo TRAILING EDGE (TE)","Moduł LED","Philips Fortimo_LED_Strip_0.5ft_MF_8xx_HV6 3K","Philips Xitanium 7W 0,35A 20V TE SC 230V [2017]",50000,null,0,80,"C",null,"Zaciski podłączeniowe: max 3x2,5mm², możliwość podłączenia oprawy w pętle max 3x1,5mm². Przewód w oponie okrągłej o średnicy ø7...10,5mm.","1726XX0010.jpg","1726XX0010.ldt",1,null,1,76]
["1727","1727XX0009","ASKER SMALL PRO WALL LED 653LM DOWN 3000K DALI2","Asker","Wall","Aluminium",null,null,"PRO","LED zintegrowane","AC","DALI2","3,9W","5,5W","653lm","426lm",null,null,"65",null,"Class I",3000,"szerokie dół",0.22,0.11,0.08,"CE",null,"DALI","> 70000",12,"Oprawa ścienna.","Światło rozproszone półsferyczne ukierunkowane w dół",null,"A luminaire with a wide range of applications, including lighting wall surfaces, facades, and other architectural concepts",null,null,null,"Odlew aluminiowy malowany proszkowo.",null,"Klosz- poliwęglan przeźroczysty ze strukturą, stabilizowany UV.","Uszczelka silikonowa.","Dławnica EPDM.","dół",null,null,"Moduł LED","Philips Fortimo_LED_Strip_0.5ft_MF_8xx_HV6 3K","Osram OTI DALI 10/220-240/700 NFC",0,null,0,80,"D",null,"Zaciski podłączeniowe: max 5x2,5mm², możliwość podłączenia oprawy w pętle max 5x1,5mm². Przewód w oponie okrągłej o średnicy ø7...10,5mm.","1727XX0009.jpg","1727XX0009.ldt",3,null,1,76]
["1730","1730XX0009","SANDVIK WALL 2XLED GU10 UP-DOWN","Sandvik","Wall","Aluminium",null,null,null,"Wymienne","GU10",null,"2 x max 4W",null,null,null,null,null,"65","IK08","Class I",null,"szerokie góra / szerokie dół",0,0,0,"CE",null,null,null,12,"Oprawa ścienna.","Światło dwustronne: ukierunkowane do góry i w dół.","Up-Down","Classic design ceiling luminaire. For lighting private areas and public spaces.",null,null,"Oprawa na wymienne źródło światła o trzonku Gu10, które zapewnia trwałość i optymalny rozsył światła, przy zachowaniu stosunkowo małego zużycia energii. Źródło światła nalezy dokupić oddzielnie.","Odlew aluminiowy malowany proszkowo.",null,"Klosz- szkło bezpieczne, przeźroczyste.","Uszczelka silikonowa.","Dławnica EPDM.",null,null,null,"2 Lampy LED GU10","PAR16",null,null,null,null,80,null,null,"Zaciski podłączeniowe: max 3x2,5mm², możliwość podłączenia oprawy w pętle max 3x1,5mm². Przewód w oponie okrągłej o średnicy ø7...10,5mm.","1730XX0009.jpg","1730XX0009.ldt",4,"GU10",1,4]
["1731","1731XX0009","SANDVIK WALL 2XLED GU10 530LM UP-DOWN 2700K DIM.","Sandvik","Wall","Aluminium",null,null,null,"Wymienne","GU10",null,"2 x 3,9W","7,8W","530lm","420lm",null,null,"65","IK08","Class I",2700,"szerokie góra / szerokie dół",0,0,0,"CE",null,null,"40000",12,"Oprawa ścienna.","Światło dwustronne: ukierunkowane do góry i w dół.","Up-Down","Classic design ceiling luminaire. For lighting private areas and public spaces.",null,null,"Oprawa wyposażona w wymienne źródło światła typu lampa LED o trzonku Gu10, która zapewnia trwałość i optymalny rozsył światła, przy zachowaniu stosunkowo małego zużycia energii.","Odlew aluminiowy malowany proszkowo.",null,"Klosz- szkło bezpieczne, przeźroczyste.","Uszczelka silikonowa.","Dławnica EPDM.",null,null,"Oprawa ściemnialna fazowo TRAILING EDGE (TE) - LEADING EDGE (LE)","2 Lampy LED GU10","Philips MASTER LED ExpertColor 3.9-35W GU10 927 25D",null,null,"Ściemnianie fazowe LED GU10 E27",null,90,"G",null,"Zaciski podłączeniowe: max 3x2,5mm², możliwość podłączenia oprawy w pętle max 3x1,5mm². Przewód w oponie okrągłej o średnicy ø7...10,5mm.","1731XX0009.jpg","1731XX0009.ldt",1,"GU10",1,4]
["1732","1732XX0009","SANDVIK WALL 2XLED 1512LM UP36D&DOWN36D 3000K DIM.","Sandvik","Wall","Aluminium",null,null,null,"LED zintegrowane","AC","DIM.","2x8W","16W","1512lm","1126lm",null,null,"65","IK08","Class I",3000,"szerokie góra / szerokie dół",0,0,0,"CE",null,null,"> 50000",12,"Oprawa ścienna.","Światło dwustronne: o kącie 36D do góry i w dół.","Up36D&Down36D","Classic design ceiling luminaire. For lighting private areas and public spaces.",null,null,null,"Odlew aluminiowy malowany proszkowo.",null,"Klosz- szkło bezpieczne, przeźroczyste.","Uszczelka silikonowa.","Dławnica EPDM.",null,null,"Oprawa ściemnialna fazowo TRAILING EDGE (TE) - LEADING EDGE (LE)","2 Moduły LED","Lumens EDC 38C 8W xxx 230V A101 3K",null,0,"Ściemnianie fazowe Lumens LED AC",null,80,"E",null,"Zaciski podłączeniowe: max 3x2,5mm², możliwość podłączenia oprawy w pętle max 3x1,5mm². Przewód w oponie okrągłej o średnicy ø7...10,5mm.","1732XX0009.jpg","1732XX0009.ldt",1,null,1,70]
["1733","1733XX0010","NARVIK II BOLLARD LED 2058LM 4000K DIM.","Narvik","Bollard","Aluminium",null,null,null,"LED zintegrowane","AC","DIM.","10,9W","13,4W","2058lm","757lm",null,null,"65","IK10","Class II",4000,null,0.24,0.24,0.95,"CE",null,null,"> 72 000h",1,"Oprawa słupkowa.","Czterostronny wylot światła przysłonięty od góry.",null,"A bollard luminaire with a stable and durable structure. For lighting private and public areas",null,null,null,"Odlew aluminiowy malowany proszkowo.",null,"Klosz- tworzywo sztuczne PMMA satynowane.","Uszczelka silikonowa.",null,null,"satynowany","Oprawa ściemnialna fazowo TRAILING EDGE (TE) - LEADING EDGE (LE)","Moduł LED","Cree DK210704 V2 JB2835 3V 4K","TCI Mini MD 20W 500mA code 127032 Triak",0,null,null,80,"C","110GA0009, 505ZX0009, 7667ZX0009","Zaciski podłączeniowe: max 2x4mm², możliwość podłączenia oprawy w pętle max 2x4mm². Przewód w oponie okrągłej o średnicy: ø8...12mm lub ø10...14mm. Oprawa wyposażona w drzwiczki rewizyjne","1733XX0010.png","1733XX0010.ldt",1,null,1,16]
["1734","1734XX0010","NARVIK II BOLLARD LED 2058LM 4000K DIM.","Narvik","Bollard","Aluminium",null,null,null,"LED zintegrowane","AC","DIM.","10,9W","13,4W","2058lm","959lm",null,null,"65","IK10","Class II",4000,null,0.24,0.24,0.95,"CE",null,null,"> 72 000h",1,"Oprawa słupkowa.","Czterostronny wylot światła przysłonięty od góry.",null,"A bollard luminaire with a stable and durable structure. For lighting private and public areas",null,null,null,"Odlew aluminiowy malowany proszkowo.",null,"Klosz- tworzywo sztuczne PMMA przeźroczyste.","Uszczelka silikonowa.",null,null,"przeźroczysty","Oprawa ściemnialna fazowo TRAILING EDGE (TE) - LEADING EDGE (LE)","Moduł LED","Cree DK210704 V2 JB2835 3V 4K","TCI Mini MD 20W 500mA code 127032 Triak",0,null,null,80,"C","110GA0009, 505ZX0009, 7667ZX0009","Zaciski podłączeniowe: max 2x4mm², możliwość podłączenia oprawy w pętle max 2x4mm². Przewód w oponie okrągłej o średnicy: ø8...12mm lub ø10...14mm. Oprawa wyposażona w drzwiczki rewizyjne","1734XX0010.png","1734XX0010.ldt",1,null,1,16]
["1735","1735XX0010","NARVIK II BOLLARD LED 3017LM 3000K DALI2","Narvik","Bollard","Aluminium",null,null,null,"LED zintegrowane","AC","DALI2","18,1W","22,2W","3017lm","1123lm",null,null,"65","IK10","Class II",3000,null,0.24,0.24,0.95,"CE",null,"DALI","> 72 000h",1,"Oprawa słupkowa.","Czterostronny wylot światła przysłonięty od góry.",null,"A bollard luminaire with a stable and durable structure. For lighting private and public areas",null,null,null,"Odlew aluminiowy malowany proszkowo.",null,"Klosz- tworzywo sztuczne PMMA satynowane.",null,null,null,"satynowany","Sterowanie światłem w systemie: DALI outdoor pełny program. Zasilacz zaprogramowany na max prąd. Programowanie pozostałych parametrów po uzgodnieniu z Działem Handlowym firmy Norlys.","Moduł LED","Cree DK210704 V2 JB2835 3V 3K","Philips Xi FP 22W 0,3-1,0A SNLDAE 230V S175 sXt",100000,"DALI2 / NightDim (XI FP NLD)",null,80,"C","110GA0009, 505ZX0009, 7667ZX0009","Zaciski podłączeniowe: max 5x2,5mm², możliwość podłączenia oprawy w pętle max 5x2,5mm². Przewód w oponie okrągłej o średnicy: ø8...12mm lub ø10...14mm. Oprawa wyposażona w drzwiczki rewizyjne.","1735XX0010.png","1735XX0010.ldt",3,null,1,16]
["1736","1736XX0010","NARVIK II BOLLARD LED 3017LM 3000K DALI2","Narvik","Bollard","Aluminium",null,null,null,"LED zintegrowane","AC","DALI2","18,1W","22,2W","3017lm","1416lm",null,null,"65","IK10","Class II",3000,null,0.24,0.24,0.95,"CE",null,"DALI","> 72 000h",1,"Oprawa słupkowa.","Czterostronny wylot światła przysłonięty od góry.",null,"A bollard luminaire with a stable and durable structure. For lighting private and public areas",null,null,null,"Odlew aluminiowy malowany proszkowo.",null,"Klosz- tworzywo sztuczne PMMA przeźroczyste.","Uszczelka silikonowa.",null,null,"przeźroczysty","Sterowanie światłem w systemie: DALI outdoor pełny program. Zasilacz zaprogramowany na max prąd. Programowanie pozostałych parametrów po uzgodnieniu z Działem Handlowym firmy Norlys.","Moduł LED","Cree DK210704 V2 JB2835 3V 3K","Philips Xi FP 22W 0,3-1,0A SNLDAE 230V S175 sXt",100000,"DALI2 / NightDim (XI FP NLD)",null,80,"C","110GA0009, 505ZX0009, 7667ZX0009","Zaciski podłączeniowe: max 5x2,5mm², możliwość podłączenia oprawy w pętle max 5x2,5mm². Przewód w oponie okrągłej o średnicy: ø8...12mm lub ø10...14mm. Oprawa wyposażona w drzwiczki rewizyjne","1736XX0010.png","1736XX0010.ldt",3,null,1,16]
["1737","1737XX0010","NARVIK II BOLLARD LED 3200LM 4000K DALI2","Narvik","Bollard","Aluminium",null,null,null,"LED zintegrowane","AC","DALI2","18,1W","22,2W","3200lm","1162lm",null,null,"65","IK10","Class II",4000,null,0.24,0.24,0.95,"CE",null,"DALI","> 72 000h",1,"Oprawa słupkowa.","Czterostronny wylot światła przysłonięty od góry.",null,"A bollard luminaire with a stable and durable structure. For lighting private and public areas",null,null,null,"Odlew aluminiowy malowany proszkowo.",null,"Klosz- tworzywo sztuczne PMMA satynowane.",null,null,null,"satynowany","Sterowanie światłem w systemie: DALI outdoor pełny program. Zasilacz zaprogramowany na max prąd. Programowanie pozostałych parametrów po uzgodnieniu z Działem Handlowym firmy Norlys.","Moduł LED","Cree DK210704 V2 JB2835 3V 4K","Philips Xi FP 22W 0,3-1,0A SNLDAE 230V S175 sXt",100000,"DALI2 / NightDim (XI FP NLD)",null,80,"C","110GA0009, 505ZX0009, 7667ZX0009","Zaciski podłączeniowe: max 5x2,5mm², możliwość podłączenia oprawy w pętle max 5x2,5mm². Przewód w oponie okrągłej o średnicy: ø8...12mm lub ø10...14mm. Oprawa wyposażona w drzwiczki rewizyjne.","1737XX0010.png","1737XX0010.ldt",3,null,1,16]
["1738","1738XX0010","NARVIK II BOLLARD LED 3200LM 4000K DALI2","Narvik","Bollard","Aluminium",null,null,null,"LED zintegrowane","AC","DALI2","18,1W","22,2W","3200lm","1475lm",null,null,"65","IK10","Class II",4000,null,0.24,0.24,0.95,"CE",null,"DALI","> 72 000h",1,"Oprawa słupkowa.","Czterostronny wylot światła przysłonięty od góry.",null,"A bollard luminaire with a stable and durable structure. For lighting private and public areas",null,null,null,"Odlew aluminiowy malowany proszkowo.",null,"Klosz- tworzywo sztuczne PMMA przeźroczyste.","Uszczelka silikonowa.",null,null,"przeźroczysty","Sterowanie światłem w systemie: DALI outdoor pełny program. Zasilacz zaprogramowany na max prąd. Programowanie pozostałych parametrów po uzgodnieniu z Działem Handlowym firmy Norlys.","Moduł LED","Cree DK210704 V2 JB2835 3V 4K","Philips Xi FP 22W 0,3-1,0A SNLDAE 230V S175 sXt",100000,"DALI2 / NightDim (XI FP NLD)",null,80,"C","110GA0009, 505ZX0009, 7667ZX0009","Zaciski podłączeniowe: max 5x2,5mm², możliwość podłączenia oprawy w pętle max 5x2,5mm². Przewód w oponie okrągłej o średnicy: ø8...12mm lub ø10...14mm. Oprawa wyposażona w drzwiczki rewizyjne","1738XX0010.png","1738XX0010.ldt",3,null,1,16]
["1740","1740XX0009","SANDVIK DOWN WALL LED GU10 DOWN 25D","Sandvik","Wall","Aluminium",null,null,null,"Wymienne","GU10",null,"max 4W",null,null,null,null,null,"65","IK08","Class I",null,"szerokie dół",0,0,0,"CE",null,null,null,12,"Oprawa ścienna.","Światło jednostronne: ukierunkowane w dół o kącie 25D","Down 25D","Classic design wall luminaire. For lighting private areas and public spaces",null,null,null,"Odlew aluminiowy malowany proszkowo.",null,"Klosz- szkło bezpieczne, przeźroczyste.","Uszczelka silikonowa.","Dławnica EPDM.",null,null,null,"Lampa LED GU10","PAR16",null,0,null,0,80,null,null,"Zaciski podłączeniowe: max 3x2,5mm², możliwość podłączenia oprawy w pętle max 3x1,5mm². Przewód w oponie okrągłej o średnicy ø7...10,5mm.","1740XX0009.jpg","1740XX0009.ldt",4,"GU10",1,74]
["1741","1741XX0009","SANDVIK DOWN WALL LED GU10 265LM DOWN 25D 2700K DIM.","Sandvik","Wall","Aluminium",null,null,null,"Wymienne","GU10",null,"3,9W","3,9W","265lm","210lm",null,null,"65","IK08","Class I",2700,"szerokie dół",0,0,0,"CE",null,null,"40 000h",12,"Oprawa ścienna.","Światło jednostronne: ukierunkowane w dół o kącie 25D","Down 25D","Classic design ceiling luminaire. For lighting private areas and public spaces",null,null,null,"Odlew aluminiowy malowany proszkowo.",null,"Klosz- szkło bezpieczne, przeźroczyste.","Uszczelka silikonowa.","Dławnica EPDM.",null,null,"Oprawa ściemnialna fazowo TRAILING EDGE (TE) - LEADING EDGE (LE)","Lampa LED GU10","Philips MASTER LED ExpertColor 3.9-35W GU10 927 25D",null,0,"Ściemnianie fazowe LED GU10 E27",0,90,"G",null,"Zaciski podłączeniowe: max 3x2,5mm², możliwość podłączenia oprawy w pętle max 3x1,5mm². Przewód w oponie okrągłej o średnicy ø7...10,5mm.","1741XX0009.jpg","1741XX0009.ldt",1,"GU10",1,74]
["1742","1742XX0009","SANDVIK DOWN WALL LED 756LM DOWN 36D 3000K DIM.","Sandvik","Wall","Aluminium",null,null,null,"LED zintegrowane","AC","DIM.","8W","8W","756lm","563lm",null,null,"65","IK08","Class I",3000,"szerokie dół",0,0,0,"CE",null,null,"> 50 000h",12,"Oprawa ścienna.","Światło jednostronne: ukierunkowane w dół o kącie 36D.","Down 36D","Classic design wall luminaire. For lighting private areas and public spaces",null,null,null,"Odlew aluminiowy malowany proszkowo.",null,"Klosz- szkło bezpieczne, przeźroczyste.","Uszczelka silikonowa.","Dławnica EPDM.",null,null,"Oprawa ściemnialna fazowo TRAILING EDGE (TE) - LEADING EDGE (LE)","Moduł LED","Lumens EDC 38C 8W xxx 230V A101 3K",null,0,"Ściemnianie fazowe Lumens LED AC",0,80,"E",null,"Zaciski podłączeniowe: max 3x2,5mm², możliwość podłączenia oprawy w pętle max 3x1,5mm². Przewód w oponie okrągłej o średnicy ø7...10,5mm.","1742XX0009.jpg","1742XX0009.ldt",1,null,1,71]
["1751","1751XX0009","RENA IN-GROUND LED 466LM 4000K DIM.","Rena","Recessed","Stal nierdzewna",null,null,null,"LED zintegrowane","AC","DIM.","4W","4W","466lm","180lm",null,null,"68","IK09","Class I",4000,null,0.13,0.13,0.17,"CE",null,null,"> 50 000",14,"Oprawa wbudowana w podłoże.","Światło rozproszone.",null,"An orientation luminaire on which vehicles with pneumatic tires can be driven. Luminaires should not be used on the road lanes, where they would be exposed to horizontal loads as a result of sudden braking, acceleration, and change of direction",null,null,null,"Odlew aluminiowy malowany proszkowo.","Front- stal nierdzewna.","Klosz- szkło bezpieczne, satynowane.","Uszczelka silikonowa.","Dławnica mosiężna niklowana.","Satynowany","Okrąg",null,"Moduł LED","Lumens EDC 38C 4W xxx 230V A101 4K",null,0,"Ściemnianie fazowe Lumens LED AC",null,80,"E","139ZX0009, 143ZX0009, 145ZX0009, 146ZX0009","Oprawa wyposażona w przewód typu 05RN8-F 3G1 o długości 3m. Do podłączenia w odpowiednio dobranej puszce elektroinstalacyjnej. Maksymalne obciążenie oprawy 2000kg. Uwaga: na powierzchni szklanej w punkcie środkowym, osiągane są temperatury robocze zgodne z normą 60598 (temperatura otoczenia 15ºC)","1751XX0009.jpg","1751XX0009.ldt",1,null,1,7]
["1753","1753XX0009","RENA IN-GROUND LED 466LM 4000K DIM.","Rena","Recessed","Stal nierdzewna",null,null,null,"LED zintegrowane","AC","DIM.","4W","4W","466lm","180lm",null,null,"68","IK09","Class I",4000,null,0.13,0.13,0.16,"CE",null,null,"50 000h",14,"Oprawa wbudowana w podłoże.","Światło rozproszone.",null,"An orientation luminaire on which vehicles with pneumatic tires can be driven. Luminaires should not be used on the road lanes, where they would be exposed to horizontal loads as a result of sudden braking, acceleration, and change of direction",null,null,null,"Odlew aluminiowy malowany proszkowo.","Front- stal nierdzewna.","Klosz- szkło bezpieczne, satynowane.","Uszczelka silikonowa.","Dławnica mosiężna niklowana.","Satynowany","Kwadrat","Oprawa ściemnialna fazowo TRAILING EDGE (TE) - LEADING EDGE (LE)","Moduł LED","Lumens EDC 38C 4W xxx 230V A101 4K",null,0,"Ściemnianie fazowe Lumens LED AC",null,80,"E","139ZX0009, 142ZX0009, 143ZX0009, 144ZX0009, 146ZX0009","Oprawa wyposażona w przewód typu 05RN8-F 3G1 o długości 3m. Do podłączenia w odpowiednio dobranej puszce elektroinstalacyjnej. Maksymalne obciążenie oprawy 2000kg. Uwaga: na powierzchni szklanej w punkcie środkowym, osiągane są temperatury robocze zgodne z normą 60598 (temperatura otoczenia 15ºC)","1753XX0009.jpg","1753XX0009.ldt",1,null,1,7]
["1754","1754XX0009","RENA IN-GROUND LED 880LM 3000K DIM.","Rena","Recessed","Stal nierdzewna",null,null,null,"LED zintegrowane","AC","DIM.","8W","8W","880lm","314lm",null,null,"68","IK09","Class I",3000,null,0.13,0.13,0.17,"CE",null,null,"> 50 000",14,"Oprawa wbudowana w podłoże.","Światło rozproszone.",null,"An orientation luminaire on which vehicles with pneumatic tires can be driven. Luminaires should not be used on the road lanes, where they would be exposed to horizontal loads as a result of sudden braking, acceleration, and change of direction",null,null,null,"Odlew aluminiowy malowany proszkowo.","Front- stal nierdzewna.","Klosz- szkło bezpieczne, satynowane.","Uszczelka silikonowa.","Dławnica mosiężna niklowana.","Satynowany","Okrąg",null,"Moduł LED","Lumens EDC 38C 8W xxx 230V A101 3K",null,0,"Ściemnianie fazowe Lumens LED AC",null,80,"E","139ZX0009, 143ZX0009, 145ZX0009, 146ZX0009","Oprawa wyposażona w przewód typu 05RN8-F 3G1 o długości 3m. Do podłączenia w odpowiednio dobranej puszce elektroinstalacyjnej. Maksymalne obciążenie oprawy 2000kg. Uwaga: na powierzchni szklanej w punkcie środkowym, osiągane są temperatury robocze zgodne z normą 60598 (temperatura otoczenia 15ºC)","1754XX0009.jpg","1754XX0009.ldt",1,null,1,7]
["1755","1755XX0009","RENA IN-GROUND LED 891LM 4000K DIM.","Rena","Recessed","Stal nierdzewna",null,null,null,"LED zintegrowane","AC","DIM.","8W","8W","891lm","330lm",null,null,"68","IK09","Class I",4000,null,0.17,0.13,0.13,"CE",null,null,"> 50 000h",14,"Oprawa wbudowana w podłoże.","Światło rozproszone.",null,"An orientation luminaire on which vehicles with pneumatic tires can be driven. Luminaires should not be used on the road lanes, where they would be exposed to horizontal loads as a result of sudden braking, acceleration, and change of direction",null,null,null,"Odlew aluminiowy malowany proszkowo.","Front- stal nierdzewna.","Klosz- szkło bezpieczne, satynowane.","Uszczelka silikonowa.","Dławnica mosiężna niklowana.","Satynowany","Okrąg",null,"Moduł LED","Lumens EDC 38C 8W xxx 230V A101 4K",null,0,"Ściemnianie fazowe Lumens LED AC",null,80,"E","139ZX0009, 143ZX0009, 145ZX0009, 146ZX0009","Oprawa wyposażona w przewód typu 05RN8-F 3G1 o długości 3m. Do podłączenia w odpowiednio dobranej puszce elektroinstalacyjnej. Maksymalne obciążenie oprawy 2000kg. Uwaga: na powierzchni szklanej w punkcie środkowym, osiągane są temperatury robocze zgodne z normą 60598 (temperatura otoczenia 15ºC)","1755XX0009.jpg","1755XX0009.ldt",1,null,1,7]
["1756","1756XX0009","RENA IN-GROUND LED 880LM 3000K DIM.","Rena","Recessed","Stal nierdzewna",null,null,null,"LED zintegrowane","AC","DIM.","8W","8,8W","880lm","314lm",null,null,"68","IK09","Class I",3000,null,null,null,null,"CE",null,null,"50 000h",14,"Oprawa wbudowana w podłoże.","Światło rozproszone.",null,"An orientation luminaire on which vehicles with pneumatic tires can be driven. Luminaires should not be used on the road lanes, where they would be exposed to horizontal loads as a result of sudden braking, acceleration, and change of direction",null,null,null,"Odlew aluminiowy malowany proszkowo.","Front- stal nierdzewna.","Klosz- szkło bezpieczne, satynowane.","Uszczelka silikonowa.","Dławnica mosiężna niklowana.","Satynowany","Kwadrat","Oprawa ściemnialna fazowo TRAILING EDGE (TE) - LEADING EDGE (LE)","Moduł LED","Lumens EDC 38C 8W xxx 230V A101 3K",null,0,"Ściemnianie fazowe Lumens LED AC",null,80,"E","139ZX0009, 142ZX0009, 143ZX0009, 144ZX0009, 146ZX0009","Oprawa wyposażona w przewód typu 05RN8-F 3G1 o długości 3m. Do podłączenia w odpowiednio dobranej puszce elektroinstalacyjnej. Maksymalne obciążenie oprawy 2000kg. Uwaga: na powierzchni szklanej w punkcie środkowym, osiągane są temperatury robocze zgodne z normą 60598 (temperatura otoczenia 15ºC)","1756XX0009.jpg","1756XX0009.ldt",1,null,1,7]
["1757","1757XX0009","RENA IN-GROUND LED 891LM 4000K DIM.","Rena","Recessed","Stal nierdzewna",null,null,null,"LED zintegrowane","AC","DIM.","8W","8,5W","891lm","330lm",null,null,"68","IK09","Class I",4000,null,null,null,null,"CE",null,null,"50 000h",14,"Oprawa wbudowana w podłoże.","Światło rozproszone.",null,"An orientation luminaire on which vehicles with pneumatic tires can be driven. Luminaires should not be used on the road lanes, where they would be exposed to horizontal loads as a result of sudden braking, acceleration, and change of direction",null,null,null,"Odlew aluminiowy malowany proszkowo.","Front- stal nierdzewna.","Klosz- szkło bezpieczne, satynowane.","Uszczelka silikonowa.","Dławnica mosiężna niklowana.","Satynowany","Kwadrat","Oprawa ściemnialna fazowo TRAILING EDGE (TE) - LEADING EDGE (LE)","Moduł LED","Lumens EDC 38C 8W xxx 230V A101 4K",null,0,"Ściemnianie fazowe Lumens LED AC",null,80,"E","139ZX0009, 142ZX0009, 143ZX0009, 144ZX0009, 146ZX0009","Oprawa wyposażona w przewód typu 05RN8-F 3G1 o długości 3m. Do podłączenia w odpowiednio dobranej puszce elektroinstalacyjnej. Maksymalne obciążenie oprawy 2000kg. Uwaga: na powierzchni szklanej w punkcie środkowym, osiągane są temperatury robocze zgodne z normą 60598 (temperatura otoczenia 15ºC)","1757XX0009.jpg","1757XX0009.ldt",1,null,1,7]
["1760","1760XX0009","RENA IN-GROUND LED 460LM 36D 3000K DIM. TRIAC","Rena","Recessed","Stal nierdzewna",null,null,null,"LED zintegrowane","AC","DIM. TRIAC","4W","4W","460lm","318lm",null,null,"68","IK09","Class I",3000,null,0,0,0,"CE",null,null,"50 000h",14,"Oprawa wbudowana w podłoże.","Światło symetryczne o kącie 36D","36D","Indicative luminaire or as a spotlight on which you can ride with pneumatic tires. Luminaires should not be used on the road lanes, where they would be exposed to horizontal loads as a result of sudden braking, acceleration, and change of direction",null,null,null,"Odlew aluminiowy malowany proszkowo.","Front- stal nierdzewna.","Klosz- szkło bezpieczne, przeźroczyste.","Uszczelka silikonowa.","Dławnica mosiężna niklowana.","Przeźroczysty","Okrąg","Oprawa ściemnialna fazowo TRAILING EDGE (TE) - LEADING EDGE (LE)","Moduł LED","Lumens EDC 38C 4W xxx 230V A101 3K",null,0,"Ściemnianie fazowe Lumens LED AC",null,80,"E","139ZX0009, 140XX0009, 142ZX0009, 143ZX0009, 145ZX0009, 146ZX0009","Oprawa wyposażona w przewód typu H05RN8-F 3G1 o długości 3m. Do podłączenia w odpowiednio dobranej puszce elektroinstalacyjnej. Maksymalne obciążenie oprawy 2000kg. Uwaga: na powierzchni szklanej w punkcie środkowym, osiągane są temperatury robocze zgodne z normą 60598 ( temperatura otoczenia 15ºC).","1760XX0009.png","1760XX0009.ldt",1,null,1,68]
["1761","1761XX0009","RENA IN-GROUND LED 488LM 36D 4000K DIM. TRIAC","Rena","Recessed","Stal nierdzewna",null,null,null,"LED zintegrowane","AC","DIM. TRIAC","4W","4W","488lm","369lm",null,null,"68",null,"Class I",4000,null,0,0,0,"CE",null,null,"50 000h",14,"Oprawa wbudowana w podłoże.","Światło symetryczne o kącie 36D","36D","Indicative luminaire or as a spotlight on which you can ride with pneumatic tires. Luminaires should not be used on the road lanes, where they would be exposed to horizontal loads as a result of sudden braking, acceleration, and change of direction",null,null,null,"Odlew aluminiowy malowany proszkowo.","Front- stal nierdzewna.","Klosz- szkło bezpieczne, przeźroczyste.","Uszczelka silikonowa.","Dławnica mosiężna niklowana.","Przeźroczysty","Okrąg","Oprawa ściemnialna fazowo TRAILING EDGE (TE) - LEADING EDGE (LE)","Moduł LED","Lumens EDC 38C 4W xxx 230V A101 4K",null,0,"Ściemnianie fazowe Lumens LED AC",null,80,"E","139ZX0009, 140XX0009, 142ZX0009, 143ZX0009, 145ZX0009, 146ZX0009","Oprawa wyposażona w przewód typu H05RN8-F 3G1 o długości 3m. Do podłączenia w odpowiednio dobranej puszce elektroinstalacyjnej. Maksymalne obciążenie oprawy 2000kg. Uwaga: na powierzchni szklanej w punkcie środkowym, osiągane są temperatury robocze zgodne z normą 60598 ( temperatura otoczenia 15ºC).","1761XX0009.png","1761XX0009.ldt",1,null,1,68]
["1762","1762XX0009","RENA IN-GROUND LED 460LM 36D 3000K DIM.","Rena","Recessed","Stal nierdzewna",null,null,null,"LED zintegrowane","AC","DIM.","4W","4W","460lm","318lm",null,null,"68","IK09","Class I",3000,null,0.13,0.13,0.16,"CE",null,null,"50 000h",14,"Oprawa wbudowana w podłoże.","Światło symetryczne o kącie 36D","36D",null,null,null,null,"Odlew aluminiowy malowany proszkowo.","Front- stal nierdzewna.","Klosz- szkło bezpieczne, przeźroczyste.","Uszczelka silikonowa.","Dławnica mosiężna niklowana.","Przeźroczysty","Kwadrat","Oprawa ściemnialna fazowo TRAILING EDGE (TE) - LEADING EDGE (LE)","Moduł LED","Lumens EDC 38C 4W xxx 230V A101 3K",null,0,"Ściemnianie fazowe Lumens LED AC",null,80,"E","139ZX0009, 141XX0009, 142ZX0009, 143ZX0009, 145ZX0009, 146ZX0009","Oprawa wyposażona w przewód typu H05RN-F 3G1 o długości 3m. Do podłączenia w odpowiednio dobranej puszce elektroinstalacyjnej. Maksymalne obciążenie oprawy 2000kg. Uwaga: na powierzchni szklanej w punkcie środkowym, osiągane są temperatury robocze zgodne z normą 60598 ( temperatura otoczenia 15ºC).","1762XX0009.png","1762XX0009.ldt",1,null,1,68]
["1763","1763XX0009","RENA IN-GROUND LED 488LM 36D 4000K DIM.","Rena","Recessed","Stal nierdzewna",null,null,null,"LED zintegrowane","AC","DIM.","4W","4W","488lm","369lm",null,null,"68",null,"Class I",4000,null,0.13,0.13,0.16,"CE",null,null,"50 000h",14,"Oprawa wbudowana w podłoże.","Światło symetryczne o kącie 36D","36D","Indicative luminaire or as a spotlight on which you can ride with pneumatic tires. Luminaires should not be used on the road lanes, where they would be exposed to horizontal loads as a result of sudden braking, acceleration, and change of direction",null,null,null,"Odlew aluminiowy malowany proszkowo.","Front- stal nierdzewna.","Klosz- szkło bezpieczne, przeźroczyste.","Uszczelka silikonowa.","Dławnica mosiężna niklowana.","Przeźroczysty","Kwadrat","Oprawa ściemnialna fazowo TRAILING EDGE (TE) - LEADING EDGE (LE)","Moduł LED","Lumens EDC 38C 4W xxx 230V A101 4K",null,0,"Ściemnianie fazowe Lumens LED AC",null,80,"E","139ZX0009, 141XX0009, 142ZX0009, 143ZX0009, 145ZX0009, 146ZX0009","Oprawa wyposażona w przewód typu H05RN-F 3G1 o długości 3m. Do podłączenia w odpowiednio dobranej puszce elektroinstalacyjnej. Maksymalne obciążenie oprawy 2000kg. Uwaga: na powierzchni szklanej w punkcie środkowym, osiągane są temperatury robocze zgodne z normą 60598 ( temperatura otoczenia 15ºC).","1763XX0009.png","1763XX0009.ldt",1,null,1,68]
["1764","1764XX0009","RENA IN-GROUND LED 880LM 36D 3000K DIM. TRIAC","Rena","Recessed","Stal nierdzewna",null,null,null,"LED zintegrowane","AC","DIM. TRIAC","8W","8W","880lm","672lm",null,null,"68","IK09","Class I",3000,null,0,0,0,"CE",null,null,"50 000h",14,"Oprawa wbudowana w podłoże.","Światło symetryczne o kącie 36D","36D","Indicative luminaire or as a spotlight on which you can ride with pneumatic tires. Luminaires should not be used on the road lanes, where they would be exposed to horizontal loads as a result of sudden braking, acceleration, and change of direction",null,null,null,"Odlew aluminiowy malowany proszkowo.","Front- stal nierdzewna.","Klosz- szkło bezpieczne, przeźroczyste.","Uszczelka silikonowa.","Dławnica mosiężna niklowana.","Przeźroczysty","Okrąg","Oprawa ściemnialna fazowo TRAILING EDGE (TE) - LEADING EDGE (LE)","Moduł LED","Lumens EDC 38C 8W xxx 230V A101 3K",null,0,"Ściemnianie fazowe Lumens LED AC",null,80,"E","139ZX0009, 140XX0009, 142ZX0009, 143ZX0009, 145ZX0009, 146ZX0009","Oprawa wyposażona w przewód typu H05RN8-F 3G1 o długości 3m. Do podłączenia w odpowiednio dobranej puszce elektroinstalacyjnej. Maksymalne obciążenie oprawy 2000kg. Uwaga: na powierzchni szklanej w punkcie środkowym, osiągane są temperatury robocze zgodne z normą 60598 ( temperatura otoczenia 15ºC).","1764XX0009.png","1764XX0009.ldt",1,null,1,68]
["1765","1765XX0009","RENA IN-GROUND LED 933LM 36D 4000K DIM. TRIAC","Rena","Recessed","Stal nierdzewna",null,null,null,"LED zintegrowane","AC","DIM. TRIAC","8W","8W","933lm","731lm",null,null,"68",null,"Class I",4000,null,0,0,0,"CE",null,null,"50 000h",14,"Oprawa wbudowana w podłoże.","Światło symetryczne o kącie 36D","36D","Indicative luminaire or as a spotlight on which you can ride with pneumatic tires. Luminaires should not be used on the road lanes, where they would be exposed to horizontal loads as a result of sudden braking, acceleration, and change of direction",null,null,null,"Odlew aluminiowy malowany proszkowo.","Front- stal nierdzewna.","Klosz- szkło bezpieczne, przeźroczyste.","Uszczelka silikonowa.","Dławnica mosiężna niklowana.","Przeźroczysty","Okrąg","Oprawa ściemnialna fazowo TRAILING EDGE (TE) - LEADING EDGE (LE)","Moduł LED","Lumens EDC 38C 8W xxx 230V A101 4K",null,0,"Ściemnianie fazowe Lumens LED AC",null,80,"E","139ZX0009, 140XX0009, 142ZX0009, 143ZX0009, 145ZX0009, 146ZX0009","Oprawa wyposażona w przewód typu H05RN8-F 3G1 o długości 3m. Do podłączenia w odpowiednio dobranej puszce elektroinstalacyjnej. Maksymalne obciążenie oprawy 2000kg. Uwaga: na powierzchni szklanej w punkcie środkowym, osiągane są temperatury robocze zgodne z normą 60598 ( temperatura otoczenia 15ºC).","1765XX0009.png","1765XX0009.ldt",1,null,1,68]
["1766","1766XX0009","RENA IN-GROUND LED 880LM 36D 3000K DIM.","Rena","Recessed","Stal nierdzewna",null,null,null,"LED zintegrowane","AC","DIM.","8W","8W","880lm","672lm",null,null,"68","IK09","Class I",3000,null,0.13,0.13,0.16,"CE",null,null,"50 000h",14,"Oprawa wbudowana w podłoże.","Światło symetryczne o kącie 36D","36D","Indicative luminaire or as a spotlight on which you can ride with pneumatic tires. Luminaires should not be used on the road lanes, where they would be exposed to horizontal loads as a result of sudden braking, acceleration, and change of direction",null,null,null,"Odlew aluminiowy malowany proszkowo.","Front- stal nierdzewna.","Klosz- szkło bezpieczne, przeźroczyste.","Uszczelka silikonowa.","Dławnica mosiężna niklowana.","Przeźroczysty","Kwadrat","Oprawa ściemnialna fazowo TRAILING EDGE (TE) - LEADING EDGE (LE)","Moduł LED","Lumens EDC 38C 8W xxx 230V A101 3K",null,0,"Ściemnianie fazowe Lumens LED AC",null,80,"E","139ZX0009, 141XX0009, 142ZX0009, 143ZX0009, 145ZX0009, 146ZX0009","Oprawa wyposażona w przewód typu H05RN-F 3G1 o długości 3m. Do podłączenia w odpowiednio dobranej puszce elektroinstalacyjnej. Maksymalne obciążenie oprawy 2000kg. Uwaga: na powierzchni szklanej w punkcie środkowym, osiągane są temperatury robocze zgodne z normą 60598 ( temperatura otoczenia 15ºC).","1766XX0009.png","1766XX0009.ldt",1,null,1,68]
["1767","1767XX0009","RENA IN-GROUND LED 933LM 36D 4000K DIM.","Rena","Recessed","Stal nierdzewna",null,null,null,"LED zintegrowane","AC","DIM.","8W","8W","933lm","731lm",null,null,"68",null,"Class I",4000,null,0.13,0.13,0.16,"CE",null,null,"50 000h",14,"Oprawa wbudowana w podłoże.","Światło symetryczne o kącie 36D","36D","Indicative luminaire or as a spotlight on which you can ride with pneumatic tires. Luminaires should not be used on the road lanes, where they would be exposed to horizontal loads as a result of sudden braking, acceleration, and change of direction",null,null,null,"Odlew aluminiowy malowany proszkowo.","Front- stal nierdzewna.","Klosz- szkło bezpieczne, przeźroczyste.","Uszczelka silikonowa.","Dławnica mosiężna niklowana.","Przeźroczysty","Kwadrat","Oprawa ściemnialna fazowo TRAILING EDGE (TE) - LEADING EDGE (LE)","Moduł LED","Lumens EDC 38C 8W xxx 230V A101 4K",null,0,"Ściemnianie fazowe Lumens LED AC",null,80,"E","139ZX0009, 141XX0009, 142ZX0009, 143ZX0009, 145ZX0009, 146ZX0009","Oprawa wyposażona w przewód typu H05RN-F 3G1 o długości 3m. Do podłączenia w odpowiednio dobranej puszce elektroinstalacyjnej. Maksymalne obciążenie oprawy 2000kg. Uwaga: na powierzchni szklanej w punkcie środkowym, osiągane są temperatury robocze zgodne z normą 60598 ( temperatura otoczenia 15ºC).","1767XX0009.png","1767XX0009.ldt",1,null,1,68]
["1769","1769XX0009","RENA IN-GROUND LED 488LM 4000K DIM.","Rena","Recessed","Aluminium",null,null,null,"LED zintegrowane","AC","DIM.","4W","4W","488lm","28lm",null,null,"68",null,"Class I",4000,null,0.13,0.13,0.18,"CE",null,null,"50 000h",14,"Oprawa wbudowana w podłoże.","Czterostronny wylot światła przysłonięty od góry.",null,"Indicative luminaire or as a spotlight on which you can ride with pneumatic tires. Luminaires should not be used on the road lanes, where they would be exposed to horizontal loads as a result of sudden braking, acceleration, and change of direction",null,null,null,"Odlew aluminiowy malowany proszkowo.",null,"Klosz- poliwęglan satynowany, stabilizowany UV.","Uszczelka silikonowa.","Dławnica mosiężna niklowana.",null,"Okrąg","Oprawa ściemnialna fazowo TRAILING EDGE (TE) - LEADING EDGE (LE)","Moduł LED","Lumens EDC 38C 4W xxx 230V A101 4K",null,0,"Ściemnianie fazowe Lumens LED AC",null,80,"E","139ZX0009, 142ZX0009, 143ZX0009, 145ZX0009, 146ZX0009","Oprawa wyposażona w przewód typu H05RN-F 3G1 o długości 3m. Do podłączenia w odpowiednio dobranej puszcze elektroinstalacyjnej. Maksymalne obciążenie oprawy 1000kg.","1769XX0009.jpg","1769XX0009.ldt",1,null,1,16]
["1773","1773XX0009","RENA IN-GROUND LED 933LM 4000K DIM.","Rena","Recessed","Aluminium",null,null,null,"LED zintegrowane","AC","DIM.","8W","8W","933lm","56lm",null,null,"68",null,"Class I",4000,null,0.13,0.13,0.18,"CE",null,null,"50 000h",14,"Oprawa wbudowana w podłoże.","Czterostronny wylot światła przysłonięty od góry.",null,"Indicative luminaire or as a spotlight on which you can ride with pneumatic tires. Luminaires should not be used on the road lanes, where they would be exposed to horizontal loads as a result of sudden braking, acceleration, and change of direction",null,null,null,"Odlew aluminiowy malowany proszkowo.",null,"Klosz- poliwęglan satynowany, stabilizowany UV.","Uszczelka silikonowa.","Dławnica mosiężna niklowana.",null,"Okrąg","Oprawa ściemnialna fazowo TRAILING EDGE (TE) - LEADING EDGE (LE)","Moduł LED","Lumens EDC 38C 8W xxx 230V A101 4K",null,0,"Ściemnianie fazowe Lumens LED AC",null,80,"E","139ZX0009, 142ZX0009, 143ZX0009, 145ZX0009, 146ZX0009","Oprawa wyposażona w przewód typu H05RN-F 3G1 o długości 3m. Do podłączenia w odpowiednio dobranej puszcze elektroinstalacyjnej. Maksymalne obciążenie oprawy 1000kg.","1773XX0009.jpg","1773XX0009.ldt",1,null,1,16]
["1774","1774XX0009","RENA IN-GROUND LED 880LM 3000K DIM.","Rena","Recessed","Aluminium",null,null,null,"LED zintegrowane","AC","DIM.","8W","8,7W","880lm","48lm",null,null,"68",null,"Class I",3000,null,0.13,0.13,0.18,"CE",null,null,"50 000h",14,"Oprawa wbudowana w podłoże.","Czterostronny wylot światła przysłonięty od góry.",null,"Indicative luminaire or as a spotlight on which you can ride with pneumatic tires. Luminaires should not be used on the road lanes, where they would be exposed to horizontal loads as a result of sudden braking, acceleration, and change of direction",null,null,null,"Odlew aluminiowy malowany proszkowo.",null,"Klosz- poliwęglan satynowany, stabilizowany UV.","Uszczelka silikonowa.","Dławnica mosiężna niklowana.",null,"Kwadrat","Oprawa ściemnialna fazowo TRAILING EDGE (TE) - LEADING EDGE (LE)","Moduł LED","Lumens EDC 38C 8W xxx 230V A101 3K",null,0,"Ściemnianie fazowe Lumens LED AC",null,80,"E","139ZX0009, 142ZX0009, 143ZX0009, 145ZX0009, 146ZX0009","Oprawa wyposażona w przewód typu H05RN-F 3G1 o długości 3m. Do podłączenia w odpowiednio dobranej puszcze elektroinstalacyjnej. Maksymalne obciążenie oprawy 1000kg.","1774XX0009.jpg","1774XX0009.ldt",1,null,1,16]
["1814","1814XX0010","KOSTER PRO WALL-ARM 2XLED 2595LM VSM 3000K DIM.","Koster","Wall","Aluminium",null,null,"PRO","LED zintegrowane","AC","DIM.","15,4W","16,9W","2595lm","2007lm",null,null,"54",null,"Class I",3000,"szerokie dół",0.44,0.24,0.24,"CE",null,null,"> 100 000h",21,"Oprawa ścienna na ramieniu.","Soczewka firmy Ledil typu VSM (IESNA typ V).","VSM","Wall lamp luminaire with a modern design Can be mounted on the corners of architectural structures","A wall luminaire on a straight arm with a modern design, Can be mounted on the corners of architectural structures, Wide and even light distribution The luminaire is also adapted to DC voltage: DC 176 ÷ 280 V",null,null,"Odlew aluminiowy malowany proszkowo.",null,"Klosz- poliwęglan przeźroczysty ze strukturą, stabilizowany UV.",null,null,null,"Ramię proste","Oprawa ściemnialna fazowo TRAILING EDGE (TE) - LEADING EDGE (LE)","2 Moduły LED","Philips Fortimo FastFlex LED 2x4 G5 3K","TCI Mini JOLLY 20W code 127556 Triac",0,null,null,70,"D","158XX0009","Zaciski podłączeniowe: max 3x2,5mm², możliwość podłączenia oprawy w pętle max 3x1,5mm². Przewód w oponie okrągłej o średnicy ø7...10,5mm.","1814XX0010.jpg","1814XX0010.ldt",1,null,1,47]
["1815","1815XX0009","KOSTER PRO POLE-TOP LED 2035LM VSM 3000K ON/OFF","Koster","Post","Aluminium",null,null,"PRO","LED zintegrowane","AC","ON/OFF","11W","14,4W","2035lm","1991lm",null,null,"65",null,"Class I",3000,"szerokie dół",0,0,0,"CE",null,null,">120 000h",2,"Oprawa słupowa (nasadzana).","Soczewka firmy Ledil typu VSM (IESNA typ V).","VSM","Luminaire on a straight shoulder, intended for mounting on a lighting pole with a Ø50mm mounting shaft","Luminaire on a straight shoulder, intended for mounting on a lighting pole with a Ø50mm mounting shaft. Wide and even light distribution",null,null,"Odlew aluminiowy malowany proszkowo.",null,"Soczewka hermetyczna zewnętrzna- tworzywo sztuczne PMMA przeźroczyste.",null,null,"Ø50",null,"Oprawa nieściemnialna","Moduł LED","Philips Fortimo FastFlex LED 2x6 DP G4+ 3K","Philips Xi BP 12 W 0,1-0,5AS 230 V C100",100000,null,null,70,"D","1270XX0009, 405ZX0009, 406ZX0009","Przewód H05VV-F 3G1 o długości 3,7m do podłączenia wewnątrz słupa oświetleniowego (w odpowiednio dobranej puszce elektroinstalacyjnej).","1815XX0009.jpg","1815XX0009.ldt",4,null,1,47]
["1816","1816XX0309","KOSTER PRO LIGHT LUMINAIRES POLE LED 2035LM VSM 3000K ON/OFF","Koster","Post,Post complete","Aluminium",null,null,"PRO","LED zintegrowane","AC","ON/OFF","11W","14,4W","2035lm","1991lm",null,null,"65",null,"Class I",3000,"szerokie dół",0,0,0,"CE",null,null,">120 000h",20,"Oprawa słupowa (lekka konstrukcja).","Soczewka firmy Ledil typu VSM (IESNA typ V).","VSM","Luminaire with a classic design mounted on a telescopic pole with adjustable height 2360..3360mm, Pole equipped with a revision door",null,null,null,"Odlew aluminiowy malowany proszkowo.",null,"Klosz- tworzywo sztuczne PMMA optyczne, przeźroczyste.",null,null,"Komplet ze słupem",null,"Oprawa nieściemnialna","Moduł LED","Philips Fortimo FastFlex LED 2x6 DP G4+ 3K","Philips Xi BP 12 W 0,1-0,5AS 230 V C100",100000,null,null,70,null,"111GA0009, 405ZX0009, 406ZX0009","Złącze podłączeniowe: na przewód max 3x4mm², Przewód w oponie okrągłej o średnicy max ø12,5mm.","1816XX0309.jpg","1816XX0309.ldt",4,null,1,47]
["1817","1817XX0009","KOSTER PRO POLE-TOP LED 2035LM VSM 3000K ON/OFF","Koster","Post,Head","Aluminium",null,null,"PRO","LED zintegrowane","AC","ON/OFF","11W","14,4W","2035lm","1991lm",null,null,"65",null,"Class I",3000,"szerokie dół",0,0,0,"CE",null,null,">120 000h",2,"Oprawa słupowa (nasadzana).","Soczewka firmy Ledil typu VSM (IESNA typ V).","VSM","Luminaire on a straight shoulder, intended for mounting on a lighting pole with a Ø60mm mounting shaft","Luminaire on a straight shoulder, intended for mounting on a lighting pole with a Ø60mm mounting shaft. Wide and even light distribution",null,null,"Odlew aluminiowy malowany proszkowo.",null,"Soczewka hermetyczna zewnętrzna- tworzywo sztuczne PMMA przeźroczyste.",null,null,"Ø60",null,"Oprawa nieściemnialna","Moduł LED","Philips Fortimo FastFlex LED 2x6 DP G4+ 3K","Philips Xi BP 12 W 0,1-0,5AS 230 V C100",100000,null,null,70,"D","3004XX0009, 7660XX0009, 7663ZX0009","Przewód H05VV-F 3G1 o długości 3,7m do podłączenia wewnątrz słupa oświetleniowego (w odpowiednio dobranej puszce elektroinstalacyjnej).","1817XX0009.jpg","1817XX0009.ldt",4,null,1,47]
["1822","1822XX0009","KOSTER PRO WALL-ARM LED 2776LM VSM 3000K DALI2","Koster","Wall","Aluminium",null,null,"PRO","LED zintegrowane","AC","DALI2","16,9W","19,6W","2776lm","2747lm",null,null,"45",null,"Class I",3000,"szerokie dół",0,0,0,"CE",null,"DALI","> 120 000h",21,"Oprawa ścienna na ramieniu.","Soczewka firmy Ledil typu VSM (IESNA typ V).","VSM","Wall lamp luminaire with a modern design, Can be mounted on the corners of architectural structures","A wall luminaire on a straight arm with a modern design, Can be mounted on the corners of architectural structures, Wide and even light distribution",null,null,"Odlew aluminiowy malowany proszkowo.",null,"Soczewka hermetyczna zewnętrzna- tworzywo sztuczne PMMA przeźroczyste.",null,null,null,"Ramię proste","Sterowanie światłem w systemie: DALI outdoor pełny program. Zasilacz zaprogramowany na max prąd. Programowanie pozostałych parametrów po uzgodnieniu z Działem Handlowym firmy Norlys.","Moduł LED","Philips Fortimo FastFlex LED 2x6 DP G4+ 3K","Philips Xi FP 22W 0,2-0,7A SNLDAE 230V S175 sXt",100000,"DALI2 / NightDim (XI FP NLD)",null,70,"D","158XX0009","Zaciski podłączeniowe: max 5x2,5mm², możliwość podłączenia oprawy w pętle max 5x2,5mm². Przewód w oponie okrągłej o średnicy ø7...10,5mm.","1822XX0009.jpg","1822XX0009.ldt",3,null,1,47]
["1823","1823XX0009","KOSTER PRO POLE-TOP LED 2776LM VSM 3000K DALI2","Koster","Post,Head","Aluminium",null,null,"PRO","LED zintegrowane","AC","DALI2","16,9W","19,4W","2776lm","2747lm",null,null,"65",null,"Class I",3000,"szerokie dół",0,0,0,"CE",null,"DALI",">120 000h",2,"Oprawa słupowa (nasadzana).","Soczewka firmy Ledil typu VSM (IESNA typ V).","VSM","Luminaire on a straight arm, intended for mounting on a pole with a Ø50mm mounting shaft","Luminaire on a straight arm, intended for mounting on a pole with a Ø50mm mounting shaft, Wide and even light distribution",null,null,"Odlew aluminiowy malowany proszkowo.",null,"Soczewka hermetyczna zewnętrzna- tworzywo sztuczne PMMA przeźroczyste.",null,null,"Ø50",null,"Sterowanie światłem w systemie: DALI outdoor pełny program. Zasilacz zaprogramowany na max prąd. Programowanie pozostałych parametrów po uzgodnieniu z Działem Handlowym firmy Norlys.","Moduł LED","Philips Fortimo FastFlex LED 2x6 DP G4+ 3K","Philips Xi FP 22W 0,2-0,7A SNLDAE 230V S175 sXt",100000,"DALI2 / NightDim (XI FP NLD)",null,70,"D","1270XX0010, 405ZX0009, 406ZX0009","Przewód H05VV-F 5G1 o długości 3,7m do podłączenia wewnątrz słupa oświetleniowego (w odpowiednio dobranej puszce elektroinstalacyjnej).","1823XX0009.jpg","1823XX0009.ldt",3,null,1,47]
["1824","1824XX0309","KOSTER PRO LIGHT LUMINAIRES POLE LED 2776LM VSM 3000K DALI2","Koster","Post,Post complete","Aluminium",null,null,"PRO","LED zintegrowane","AC","DALI2","16,9W","19,4W","2776lm","2747lm",null,null,"65",null,"Class I",3000,"szerokie dół",0.45,0.24,0.24,"CE",null,"DALI",">120 000h",20,"Oprawa słupowa (lekka konstrukcja).","Soczewka firmy Ledil typu VSM (IESNA typ V).","VSM","Luminaire with a classic design mounted on a telescopic pole with adjustable height 2360..3360mm, Pole equipped with a revision door",null,null,null,"Odlew aluminiowy malowany proszkowo.",null,"Klosz- tworzywo sztuczne PMMA optyczne, przeźroczyste.",null,null,"Komplet ze słupem",null,"Sterowanie światłem w systemie: DALI outdoor pełny program. Zasilacz zaprogramowany na max prąd. Programowanie pozostałych parametrów po uzgodnieniu z Działem Handlowym firmy Norlys.","Moduł LED","Philips Fortimo FastFlex LED 2x6 DP G4+ 3K","Philips Xi FP 22W 0,2-0,7A SNLDAE 230V S175 sXt",100000,"DALI2 / NightDim (XI FP NLD)",null,70,null,"111GA0009, 405ZX0009, 406ZX0009","Złącze podłączeniowe: na przewód max 5x4mm². Przewód w oponie okrągłej o średnicy max ø12,5mm.","1824XX0309.jpg","1824XX0309.ldt",3,null,1,47]
["1825","1825XX0009","KOSTER PRO POLE-TOP LED 2776LM VSM 3000K DALI2","Koster","Post,Head","Aluminium",null,null,"PRO","LED zintegrowane","AC","DALI2","16,9W","19,4W","2776lm","2747lm",null,null,"65",null,"Class I",3000,"szerokie dół",0,0,0,"CE",null,"DALI",">120 000h",2,"Oprawa słupowa (nasadzana).","Soczewka firmy Ledil typu VSM (IESNA typ V).","VSM","Luminaire on a straight arm, intended for mounting on a pole with a Ø60mm mounting shaft","Luminaire on a straight arm, intended for mounting on a pole with a Ø60mm mounting shaft, Wide and even light distribution",null,null,"Odlew aluminiowy malowany proszkowo.",null,"Soczewka hermetyczna zewnętrzna- tworzywo sztuczne PMMA przeźroczyste.",null,null,"Ø60",null,"Sterowanie światłem w systemie: DALI outdoor pełny program. Zasilacz zaprogramowany na max prąd. Programowanie pozostałych parametrów po uzgodnieniu z Działem Handlowym firmy Norlys.","Moduł LED","Philips Fortimo FastFlex LED 2x6 DP G4+ 3K","Philips Xi FP 22W 0,2-0,7A SNLDAE 230V S175 sXt",100000,"DALI2 / NightDim (XI FP NLD)",null,70,"D","3004XX0009, 7660XX0009, 7663ZX0009","Przewód H05VV-F 5G1 o długości 3,7m do podłączenia wewnątrz słupa oświetleniowego (w odpowiednio dobranej puszce elektroinstalacyjnej).","1825XX0009.jpg","1825XX0009.ldt",3,null,1,47]
["1834","1834XX0010","KOSTER PRO WALL-ARM 2XLED 2801LM VSM 4000K DIM.","Koster","Wall","Aluminium",null,null,"PRO","LED zintegrowane","AC","DIM.","15,4W","16,9W","2801lm","2090lm",null,null,"45",null,"Class I",4000,"szerokie dół",0.44,0.24,0.24,"CE",null,null,"> 100 000h",21,"Oprawa ścienna na ramieniu.","Soczewka firmy Ledil typu VSM (IESNA typ V).","VSM","Wall lamp luminaire with a modern design Can be mounted on the corners of architectural structures","A wall luminaire on a straight arm with a modern design, Can be mounted on the corners of architectural structures, Wide and even light distribution The luminaire is also adapted to DC voltage: DC 176 ÷ 280 V",null,null,"Odlew aluminiowy malowany proszkowo.",null,"Klosz- poliwęglan przeźroczysty ze strukturą, stabilizowany UV.",null,null,null,"Ramię proste","Oprawa ściemnialna fazowo TRAILING EDGE (TE) - LEADING EDGE (LE)","2 Moduły LED","Philips Fortimo FastFlex LED 2x4 G5 4K","TCI Mini JOLLY 20W code 127556 Triac",0,null,null,70,"D","158XX0009","Zaciski podłączeniowe: max 3x2,5mm², możliwość podłączenia oprawy w pętle max 3x1,5mm². Przewód w oponie okrągłej o średnicy ø7...10,5mm.","1834XX0010.jpg","1834XX0010.ldt",1,null,1,47]
["1835","1835XX0009","KOSTER PRO POLE-TOP LED 2145LM VSM 4000K ON/OFF","Koster","Post","Aluminium",null,null,"PRO","LED zintegrowane","AC","ON/OFF","11W","14,4W","2145lm","2031lm",null,null,"65",null,"Class I",4000,"szerokie dół",0,0,0,"CE",null,null,">120 000h",2,"Oprawa słupowa (nasadzana).","Soczewka firmy Ledil typu VSM (IESNA typ V).","VSM","Classic design luminaire on a straight top arm. Intended for mounting on a pole with a Ø50mm mounting shaft","Luminaire on a straight top arm, intended for mounting on a pole with a Ø50mm mounting shaft, Wide and even light distribution",null,null,"Odlew aluminiowy malowany proszkowo.",null,"Soczewka hermetyczna zewnętrzna- tworzywo sztuczne PMMA przeźroczyste.",null,null,"Ø50",null,"Oprawa nieściemnialna","Moduł LED","Philips Fortimo FastFlex LED 2x6 DP G4+ 4K","Philips Xi BP 12 W 0,1-0,5AS 230 V C100",100000,null,null,70,null,"1270XX0010, 405ZX0009, 406ZX0009","Przewód H05VV-F 3G1 o długości 3,7m do podłączenia wewnątrz słupa oświetleniowego (w odpowiednio dobranej puszce elektroinstalacyjnej).","1835XX0009.jpg","1835XX0009.ldt",4,null,1,47]
["1836","1836XX0309","KOSTER PRO LIGHT LUMINAIRES POLE LED 2145LM VSM 4000K ON/OFF","Koster","Post","Aluminium",null,null,"PRO","LED zintegrowane","AC","ON/OFF","11W","14,4W","2145lm","2031lm",null,null,"65",null,"Class I",4000,"szerokie dół",0,0,0,"CE",null,null,">120 000h",20,"Oprawa słupowa (lekka konstrukcja).","Soczewka firmy Ledil typu VSM (IESNA typ V).","VSM","Luminaire with a classic design mounted on a telescopic pole with adjustable height 2360..3360mm, Pole equipped with a revision door",null,null,null,"Odlew aluminiowy malowany proszkowo.",null,"Klosz- tworzywo sztuczne PMMA optyczne, przeźroczyste.",null,null,"Komplet ze słupem",null,"Oprawa nieściemnialna","Moduł LED","Philips Fortimo FastFlex LED 2x6 DP G4+ 4K","Philips Xi BP 12 W 0,1-0,5AS 230 V C100",100000,null,null,70,null,"111GA0009, 405ZX0009, 406ZX0009","Złącze podłączeniowe: na przewód max 3x4mm², Przewód w oponie okrągłej o średnicy max ø12,5mm.","1836XX0309.jpg","1836XX0309.ldt",4,null,1,47]
["1837","1837XX0009","KOSTER PRO POLE-TOP LED 2145LM VSM 4000K ON/OFF","Koster","Post","Aluminium",null,null,"PRO","LED zintegrowane","AC","ON/OFF","11W","14,4W","2145lm","2031lm",null,null,"65",null,"Class I",4000,"szerokie dół",0,0,0,"CE",null,null,">120 000h",2,"Oprawa słupowa (nasadzana).","Soczewka firmy Ledil typu VSM (IESNA typ V).","VSM","Luminaire on a straight top arm, intended for mounting on a pole with a Ø60mm mounting shaft","Luminaire on a straight top arm, intended for mounting on a pole with a Ø60mm mounting shaft, Wide and even light distribution",null,null,"Odlew aluminiowy malowany proszkowo.",null,"Soczewka hermetyczna zewnętrzna- tworzywo sztuczne PMMA przeźroczyste.",null,null,"Ø60",null,"Oprawa nieściemnialna","Moduł LED","Philips Fortimo FastFlex LED 2x6 DP G4+ 4K","Philips Xi BP 12 W 0,1-0,5AS 230 V C100",100000,null,null,70,null,"3004XX0009, 7660XX0009, 7663ZX0009","Przewód H05VV-F 3G1 o długości 3,7m do podłączenia wewnątrz słupa oświetleniowego (w odpowiednio dobranej puszce elektroinstalacyjnej).","1837XX0009.jpg","1837XX0009.ldt",4,null,1,47]
["1842","1842XX0009","KOSTER PRO WALL-ARM LED 2927LM VSM 4000K DALI2","Koster","Wall","Aluminium",null,null,"PRO","LED zintegrowane","AC","DALI2","16,9W","19,4W","2927lm","2718lm",null,null,"45",null,"Class I",4000,"szerokie dół",0,0,0,"CE",null,"DALI","> 120 000h",21,"Oprawa ścienna na ramieniu.","Soczewka firmy Ledil typu VSM (IESNA typ V).","VSM","Wall lamp luminaire with a modern design, Can be mounted on the corners of architectural structures","A wall luminaire on a straight arm with a modern design, Can be mounted on the corners of architectural structures, Wide and even light distribution",null,null,"Odlew aluminiowy malowany proszkowo.",null,"Soczewka hermetyczna zewnętrzna- tworzywo sztuczne PMMA przeźroczyste.",null,null,null,"Ramię proste","Sterowanie światłem w systemie: DALI outdoor pełny program. Zasilacz zaprogramowany na max prąd. Programowanie pozostałych parametrów po uzgodnieniu z Działem Handlowym firmy Norlys.","Moduł LED","Philips Fortimo FastFlex LED 2x6 DP G4+ 3K","Philips Xi FP 22W 0,2-0,7A SNLDAE 230V S175 sXt",100000,"DALI2 / NightDim (XI FP NLD)",null,70,"D","158XX0009","Zaciski podłączeniowe: max 5x2,5mm², możliwość podłączenia oprawy w pętle max 5x2,5mm². Przewód w oponie okrągłej o średnicy ø7...10,5mm.","1842XX0009.jpg","1842XX0009.ldt",3,null,1,47]
["1843","1843XX0009","KOSTER PRO POLE-TOP LED 2927LM VSM 4000K DALI2","Koster","Post","Aluminium",null,null,"PRO","LED zintegrowane","AC","DALI2","16,9W","19,4W","2927lm","2718lm",null,null,"65",null,"Class I",4000,"szerokie dół",0,0,0,"CE",null,"DALI",">120 000h",2,"Oprawa słupowa (nasadzana).","Soczewka firmy Ledil typu VSM (IESNA typ V).","VSM","Luminaire on a straight arm with classic design. Mounted, intended for mounting on a lighting pole with a Ø50mm mounting base.","Luminaire on a straight arm, mounted, intended for installation on a lighting pole with a Ø50mm mounting base. Wide, even light distribution.",null,null,"Odlew aluminiowy malowany proszkowo.",null,"Soczewka hermetyczna zewnętrzna- tworzywo sztuczne PMMA przeźroczyste.",null,null,"Ø50",null,"Sterowanie światłem w systemie: DALI outdoor pełny program. Zasilacz zaprogramowany na max prąd. Programowanie pozostałych parametrów po uzgodnieniu z Działem Handlowym firmy Norlys.","Moduł LED","Philips Fortimo FastFlex LED 2x6 DP G4+ 3K","Philips Xi FP 22W 0,2-0,7A SNLDAE 230V S175 sXt",100000,"DALI2 / NightDim (XI FP NLD)",null,70,"D","1270XX0010, 405ZX0009, 406ZX0009","Przewód H05VV-F 5G1 o długości 3,7m do podłączenia wewnątrz słupa oświetleniowego (w odpowiednio dobranej puszce elektroinstalacyjnej).","1843XX0009.jpg","1843XX0009.ldt",3,null,1,47]
["1844","1844XX0309","KOSTER PRO LIGHT LUMINAIRES POLE LED 2927LM VSM 4000K DALI2","Koster","Post","Aluminium",null,null,"PRO","LED zintegrowane","AC","DALI2","16,9W","19,4W","2927lm","2718lm",null,null,"65",null,"Class I",4000,"szerokie dół",0.45,0.24,0.24,"CE",null,"DALI",">120 000h",20,"Oprawa słupowa (lekka konstrukcja).","Soczewka firmy Ledil typu VSM (IESNA typ V).","VSM","Luminaire with a classic design mounted on a telescopic pole with adjustable height 2360..3360mm, Pole equipped with a revision door",null,null,null,"Odlew aluminiowy malowany proszkowo.",null,"Klosz- tworzywo sztuczne PMMA optyczne, przeźroczyste.",null,null,"Komplet ze słupem",null,"Sterowanie światłem w systemie: DALI outdoor pełny program. Zasilacz zaprogramowany na max prąd. Programowanie pozostałych parametrów po uzgodnieniu z Działem Handlowym firmy Norlys.","Moduł LED","Philips Fortimo FastFlex LED 2x6 DP G4+ 3K","Philips Xi FP 22W 0,2-0,7A SNLDAE 230V S175 sXt",100000,"DALI2 / NightDim (XI FP NLD)",null,70,null,"111GA0009, 405ZX0009, 406ZX0009","Złącze podłączeniowe: na przewód max 5x4mm². Przewód w oponie okrągłej o średnicy max ø12,5mm.","1844XX0309.jpg","1844XX0309.ldt",3,null,1,47]
["1845","1845XX0009","KOSTER PRO POLE-TOP LED 2927LM VSM 4000K DALI2","Koster","Post","Aluminium",null,null,"PRO","LED zintegrowane","AC","DALI2","16,9W","19,4W","2927lm","2718lm",null,null,"65",null,"Class I",4000,"szerokie dół",0,0,0,"CE",null,"DALI",">120 000h",2,"Oprawa słupowa (nasadzana).","Soczewka firmy Ledil typu VSM (IESNA typ V).","VSM","Luminaire on a straight arm, intended for mounting on a pole with a Ø60mm mounting shaft","Luminaire on a straight arm, intended for mounting on a pole with a Ø60mm mounting shaft, Wide and even light distribution",null,null,"Odlew aluminiowy malowany proszkowo.",null,"Soczewka hermetyczna zewnętrzna- tworzywo sztuczne PMMA przeźroczyste.",null,null,"Ø60",null,"Sterowanie światłem w systemie: DALI outdoor pełny program. Zasilacz zaprogramowany na max prąd. Programowanie pozostałych parametrów po uzgodnieniu z Działem Handlowym firmy Norlys.","Moduł LED","Philips Fortimo FastFlex LED 2x6 DP G4+ 3K","Philips Xi FP 22W 0,2-0,7A SNLDAE 230V S175 sXt",100000,"DALI2 / NightDim (XI FP NLD)",null,70,"D","3004XX0009, 7660XX0009, 7663ZX0009","Przewód H05VV-F 5G1 o długości 3,7m do podłączenia wewnątrz słupa oświetleniowego (w odpowiednio dobranej puszce elektroinstalacyjnej).","1845XX0009.jpg","1845XX0009.ldt",3,null,1,47]
["1850","1850XX0010","NARVIK II BOLLARD LED 3017LM 3000K ON/OFF","Narvik","Bollard","Aluminium",null,null,null,"LED zintegrowane","AC","ON/OFF","18,1W","22,2W","3017lm","1122lm",null,null,"65","IK10","Class II",3000,null,0.24,0.24,0.95,"CE",null,null,"> 72 000h",1,"Oprawa słupkowa.","Czterostronny wylot światła przysłonięty od góry.",null,"A bollard luminaire with a stable and durable structure. For lighting private and public areas",null,null,null,"Odlew aluminiowy malowany proszkowo.",null,"Klosz- tworzywo sztuczne PMMA satynowane.","Uszczelka silikonowa.",null,null,"satynowany","Oprawa nieściemnialna","Moduł LED","Cree DK210704 V2 JB2835 3V 3K","TCI Pro Flat 40 code 127574 on-off switch KL II",0,null,null,80,"C","110GA0009, 505ZX0009, 7667ZX0009","Zaciski podłączeniowe: max 2x4mm², możliwość podłączenia oprawy w pętle max 2x4mm². Przewód w oponie okrągłej o średnicy: ø8...12mm lub ø10...14mm. Oprawa wyposażona w drzwiczki rewizyjne","1850XX0010.png","1850XX0010.ldt",4,null,1,16]
["1851","1851XX0010","NARVIK II BOLLARD LED 3200LM 4000K ON/OFF","Narvik","Bollard","Aluminium",null,null,"PRO","LED zintegrowane","AC","ON/OFF","18,1W","22,2W","3200lm","1162lm",null,null,"65","IK10","Class II",4000,null,0.24,0.24,0.95,"CE",null,null,"> 72 000h",1,"Oprawa słupkowa.","Czterostronny wylot światła przysłonięty od góry.",null,"A bollard luminaire with a stable and durable structure. For lighting private and public areas",null,null,null,"Odlew aluminiowy malowany proszkowo.",null,"Klosz- tworzywo sztuczne PMMA satynowane.","Uszczelka silikonowa.",null,null,"satynowany","Oprawa nieściemnialna","Moduł LED","Cree DK210704 V2 JB2835 3V 4K","TCI Pro Flat 40 code 127574 on-off switch KL II",0,null,null,80,"C","110GA0009, 505ZX0009, 7667ZX0009","Zaciski podłączeniowe: max 2x4mm², możliwość podłączenia oprawy w pętle max 2x4mm². Przewód w oponie okrągłej o średnicy: ø8...12mm lub ø10...14mm. Oprawa wyposażona w drzwiczki rewizyjne","1851XX0010.png","1851XX0010.ldt",4,null,1,16]
["1852","1852XX0010","NARVIK II BOLLARD LED 3017LM 3000K ON/OFF","Narvik","Bollard","Aluminium",null,null,null,"LED zintegrowane","AC","ON/OFF","18,1W","22,2W","3017lm","1416lm",null,null,"65","IK10","Class II",3000,null,0.24,0.24,0.95,"CE",null,null,"> 72 000h",1,"Oprawa słupkowa.","Czterostronny wylot światła przysłonięty od góry.",null,"A bollard luminaire with a stable and durable structure. For lighting private and public areas",null,null,null,"Odlew aluminiowy malowany proszkowo.",null,"Klosz- tworzywo sztuczne PMMA przeźroczyste.","Uszczelka silikonowa.",null,null,"przeźroczysty","Oprawa nieściemnialna","Moduł LED","Cree DK210704 V2 JB2835 3V 3K","TCI Pro Flat 40 code 127574 on-off switch KL II",0,null,null,80,"C","110GA0009, 505ZX0009, 7667ZX0009","Zaciski podłączeniowe: max 2x4mm², możliwość podłączenia oprawy w pętle max 2x4mm². Przewód w oponie okrągłej o średnicy: ø8...12mm lub ø10...14mm. Oprawa wyposażona w drzwiczki rewizyjne","1852XX0010.png","1852XX0010.ldt",4,null,1,16]
["1853","1853XX0010","NARVIK II BOLLARD LED 3200LM 4000K ON/OFF","Narvik","Bollard","Aluminium",null,null,null,"LED zintegrowane","AC","ON/OFF","18,1W","22,2W","3200lm","1475lm",null,null,"65","IK10","Class II",4000,null,0.24,0.24,0.95,"CE",null,null,"> 72 000h",1,"Oprawa słupkowa.","Czterostronny wylot światła przysłonięty od góry.",null,"A bollard luminaire with a stable and durable structure. For lighting private and public areas",null,null,null,"Odlew aluminiowy malowany proszkowo.",null,"Klosz- tworzywo sztuczne PMMA przeźroczyste.","Uszczelka silikonowa.",null,null,"przeźroczysty","Oprawa nieściemnialna","Moduł LED","Cree DK210704 V2 JB2835 3V 4K","TCI Pro Flat 40 code 127574 on-off switch KL II",0,null,null,80,"C","110GA0009, 505ZX0009, 7667ZX0009","Zaciski podłączeniowe: max 2x4mm², możliwość podłączenia oprawy w pętle max 2x4mm². Przewód w oponie okrągłej o średnicy: ø8...12mm lub ø10...14mm. Oprawa wyposażona w drzwiczki rewizyjne","1853XX0010.png","1853XX0010.ldt",4,null,1,16]
["1874","1874XX0009","GENEVE WALL E27 UP-DOWN","Geneva","Wall","Aluminium",null,null,null,"Wymienne","E27",null,"LED max 9W","LED max 9W",null,null,null,null,"65","IK08","Class I",null,null,0.31,0.21,0.95,"CE",null,null,null,12,"Oprawa ścienna.","Światło dwustronne: ukierunkowane do góry i w dół.","Up-Down","A luminaire with a wide range of applications, including lighting: wall surfaces, facades, and other architectural concepts.",null,null,null,"Odlew aluminiowy malowany proszkowo.",null,"Klosz- poliwęglan przeźroczysty ze strukturą, stabilizowany UV.","Uszczelka silikonowa.","Dławnica EPDM.","góra/dół",null,null,"Lampa E27","LED A55...67",null,0,null,null,80,null,null,"Zaciski podłączeniowe: max 3x2,5mm², możliwość podłączenia oprawy w pętle max 3x1,5mm². Przewód w oponie okrągłej o średnicy ø7...10,5mm.","1874XX0009.jpg","1874XX0009.ldt",4,"E27",1,4]
["1879","1879XX0009","GENEVE WALL 2XLED 1128LM UP-DOWN 3000K DIM.","Geneva","Wall","Aluminium",null,null,null,"LED zintegrowane","AC","DIM.","6,6W","8,3W","1128lm","609lm",null,null,"65","IK08","Class I",3000,"szerokie góra / szerokie dół",0.21,0.1,0.31,"CE",null,null,"> 72 000h",12,"Oprawa ścienna.","Światło dwustronne: ukierunkowane do góry i w dół.","Up-Down","A luminaire with a wide range of applications, including lighting: wall surfaces, facades, and other architectural concepts.",null,null,null,"Odlew aluminiowy malowany proszkowo.",null,"Klosz- poliwęglan satynowany, stabilizowany UV.","Uszczelka silikonowa.","Dławnica EPDM.","góra/dół",null,"Oprawa ściemnialna fazowo TRAILING EDGE (TE)","2 Moduły LED","Philips Fortimo Strip 0,5ft MF FC LV6 3K","Philips Xitanium 8W 0,2A 40V TE SC 230V",0,"Philips Xitanium TE",null,80,"D",null,"Zaciski podłączeniowe: max 3x2,5mm², możliwość podłączenia oprawy w pętle max 3x1,5mm². Przewód w oponie okrągłej o średnicy ø7...10,5mm.","1879XX0009.jpg","1879XX0009.ldt",1,null,1,4]
["1880","1880XX0009","GENEVE WALL 2XLED 1196LM UP-DOWN 4000K DIM.","Geneva","Wall","Aluminium",null,null,null,"LED zintegrowane","AC","DIM.","6,6","8,4","1196lm","656lm",null,null,"65","IK08","Class I",4000,"szerokie góra / szerokie dół",null,null,null,"CE",null,null,"> 70 000h",12,"Oprawa ścienna.","Światło dwustronne: ukierunkowane do góry i w dół.","Up-Down","A luminaire with a wide range of applications, including lighting: wall surfaces, facades, and other architectural concepts.",null,null,null,"Odlew aluminiowy malowany proszkowo.",null,"Klosz- poliwęglan satynowany, stabilizowany UV.","Uszczelka silikonowa.","Dławnica EPDM.","góra/dół",null,"Oprawa ściemnialna fazowo TRAILING EDGE (TE) - LEADING EDGE (LE)","2 Moduły LED","Philips Fortimo Strip 0,5ft MF FC LV6 4K","Philips Xitanium 8W 0,2A 40V TE SC 230V",0,"Philips Xitanium TE",null,80,"C",null,"Zaciski podłączeniowe: max 3x2,5mm², możliwość podłączenia oprawy w pętle max 3x1,5mm². Przewód w oponie okrągłej o średnicy ø7...10,5mm.","1880XX0009.jpg","1880XX0009.ldt",1,null,1,4]
["1901","1901XX0013","MOLDE BOLLARD 80CM LED 743LM 3000K DIM.","Molde","Bollard","Aluminium",null,null,null,"LED zintegrowane","AC","DIM.","8W","8W","743lm","386lm",null,null,"54","IK07","Class I",3000,null,0.8,0.16,0.11,"CE",null,null,"50000",1,"Oprawa słupkowa.","Światło rozproszone przysłonięte od góry.",null,"Luminaire with contemporary design. For lighting private areas, parks, and other concepts architectural",null,null,null,"Odlew aluminiowy malowany proszkowo.",null,"Klosz- poliwęglan przeźroczysty ze strukturą, stabilizowany UV.",null,null,"80cm",null,"Oprawa ściemnialna fazowo TRAILING EDGE (TE) - LEADING EDGE (LE)","Moduł LED","Lumens EDC 57C 8W xxx 230V F201 3K",null,0,"Ściemnianie fazowe Lumens LED AC",0.02,80,"F","1907ZX0009, 1908GA0009, 3081XX0009","Zaciski podłączeniowe: max 3x2,5mm², możliwość podłączenia oprawy w pętle max 3x1,5mm². Przewód w oponie okrągłej o średnicy max ø6...10mm.","1901XX0013.jpg","1901XX0013.ldt",1,null,1,25]
["1903","1903XX0009","MOLDE BOLLARD 50CM LED 743LM 3000K DIM.","Molde","Bollard","Aluminium",null,null,null,"LED zintegrowane","AC","DIM.","8W","8W","743lm","386lm",null,null,"54",null,"Class I",3000,null,0.5,0.16,0.11,"CE",null,null,"50 000h",1,"Oprawa słupkowa.","Światło rozproszone przysłonięte od góry.",null,"Luminaire with contemporary design. For lighting private areas, parks and other concepts architectural",null,null,null,"Odlew aluminiowy malowany proszkowo.",null,"Klosz- poliwęglan przeźroczysty ze strukturą, stabilizowany UV.",null,null,"50cm",null,"Oprawa ściemnialna fazowo TRAILING EDGE (TE) - LEADING EDGE (LE)","Moduł LED","Lumens EDC 57C 8W xxx 230V F201 3K",null,0,"Ściemnianie fazowe Lumens LED AC",0.02,80,"F","1907ZX0009, 1908GA0009","Zaciski podłączeniowe: max 3x2,5mm², możliwość podłączenia oprawy w pętle max 3x1,5mm². Przewód w oponie okrągłej o średnicy max ø6...10,5mm.","1903XX0009.jpg","1903XX0009.ldt",1,null,1,25]
["1904","1904XX0009","MOLDE BOLLARD 50CM LED 772LM 4000K DIM.","Molde","Bollard","Aluminium",null,null,null,"LED zintegrowane","AC","DIM.","8W","8W","772lm","438lm",null,null,"54",null,"Class I",4000,null,0.5,0.16,0.11,"CE",null,null,"50 000h",1,"Oprawa słupkowa.","Światło rozproszone przysłonięte od góry.",null,"Luminaire with contemporary design. For lighting private areas, parks and other concepts architectural",null,null,null,"Odlew aluminiowy malowany proszkowo.",null,"Klosz- poliwęglan przeźroczysty ze strukturą, stabilizowany UV.",null,null,"50cm",null,"Oprawa ściemnialna fazowo TRAILING EDGE (TE) - LEADING EDGE (LE)","Moduł LED","Lumens EDC 57C 8W xxx 230V F201 4K",null,0,"Ściemnianie fazowe Lumens LED AC",null,80,"F","1907ZX0009, 1908GA0009","Zaciski podłączeniowe: max 3x2,5mm², możliwość podłączenia oprawy w pętle max 3x1,5mm². Przewód w oponie okrągłej o średnicy max ø10,5mm.","1904XX0009.jpg","1904XX0009.ldt",1,null,1,25]
["1912","1912XX0012","KOSTER WALL-ARM LED 1950LM 3000K ON/OFF","Koster","Wall","Aluminium",null,null,null,"LED zintegrowane","AC","ON/OFF","17,5W","17,5W","1950lm","1568lm",null,null,"54","IK10","Class I",3000,null,0,0,0,"CE",null,null,"50000",21,"Oprawa ścienna na ramieniu.","Światło jednostronne: symetryczne, ukierunkowane w dół.",null,"Classic type wall-mounted luminaire. Possibility to install on corners of architectural objects.",null,null,"Oprawa wyposażona w wymienne źródło światła typu moduł LED, który zapewnia trwałość i optymalny rozsył światła, przy zachowaniu stosunkowo niskiego zużycia energii.","Odlew aluminiowy malowany proszkowo.",null,"Klosz- poliwęglan przeźroczysty ze strukturą, stabilizowany UV.",null,null,null,"Ramię proste","Oprawa nieściemnialna","Moduł LED","Philips Fortimo DLM ES 2000/8xx G2 3K",null,null,null,0,80,"E","158XX0009","Zaciski podłączeniowe: max 3x2,5mm², możliwość podłączenia oprawy w pętle max 3x1,5mm². Przewód w oponie okrągłej o średnicy ø7...10,5mm.","1912XX0012.jpg","1912XX0012.ldt",4,null,1,27]
["1913","1913XX0011","KOSTER POLE-TOP LED 1950LM 3000K","Koster","Post,Head","Aluminium",null,null,null,"LED zintegrowane","AC",null,"17,5W","17,5W","1950lm","1568lm",null,null,"54","IK10","Class I",3000,null,0,0,0,"CE",null,null,"50000",2,"Oprawa słupowa (nasadzana).","Światło jednostronne: symetryczne, ukierunkowane w dół.",null,"Classic design luminaire for mounting on a telescopic lighting pole with cap diameter Ø60mm.",null,null,null,"Odlew aluminiowy malowany proszkowo.",null,"Klosz- poliwęglan przeźroczysty ze strukturą, stabilizowany UV.",null,null,"Ø60",null,"Oprawa nieściemnialna","Moduł LED","Philips LED Fortimo DLM ES 2000/830 G2",null,null,null,0,80,"E","3004XX0009, 7660XX0009, 7662ZX0009, MONTAŻ DO PODŁOŻA","Przewód H05VV-F 3G1 o długości 4,3m do podłączenia wewnątrz słupa oświetleniowego (w odpowiednio dobranej puszce elektroinstalacyjnej).","1913XX0011.jpg","1913XX0011.ldt",4,null,1,27]
["1914","1914XX0309","KOSTER POLE-TOP LED 1950LM 3000K","Koster","Post,Post complete","Aluminium",null,null,null,"LED zintegrowane","AC",null,"17,5W","17,5W","1950lm","1568lm",null,null,"54","IK10","Class I",3000,null,null,null,null,"CE",null,null,"50000",2,"Oprawa słupowa (nasadzana).","Światło jednostronne: symetryczne, ukierunkowane w dół.",null,"Classic design luminaire, mounted on a telescopic lighting pole. Adjustable height 2360..3360mm.",null,null,"Oprawa wyposażona w wymienne źródło światła typu moduł LED, który zapewnia trwałość i optymalny rozsył światła, przy zachowaniu stosunkowo niskiego zużycia energii.","Odlew aluminiowy malowany proszkowo.",null,"Klosz- poliwęglan przeźroczysty ze strukturą, stabilizowany UV.",null,null,"Komplet ze słupem",null,"Oprawa nieściemnialna","Moduł LED","Philips LED Fortimo DLM ES 2000/830 G2",null,0,null,0,80,null,"111GA0009, 405ZX0009, 406ZX0009","Złącze podłączeniowe: na przewód max 3x2,5mm², wyposażone w bezpiecznik topikowy 1A 5x20. Przewód w oponie okrągłej o średnicy max ø12,5mm.","1914XX0309.jpg","1914XX0309.ldt",4,null,1,27]
["1915","1915XX0011","KOSTER POLE-TOP LED 1950LM 3000K","Koster","Post,Head","Aluminium",null,null,null,"LED zintegrowane","AC",null,"17,5W","17,5W","1950lm","1568lm",null,null,"54","IK10","Class I",3000,null,0,0,0,"CE",null,null,"50000",2,"Oprawa słupowa (nasadzana).","Światło jednostronne: symetryczne, ukierunkowane w dół.",null,"Classic design luminaire for mounting on a telescopic lighting pole with cap diameter Ø50mm.",null,null,"Oprawa wyposażona w wymienne źródło światła typu moduł LED, która zapewnia trwałość i optymalny rozsył światła, przy zachowaniu stosunkowo niskiego zużycia energii.","Odlew aluminiowy malowany proszkowo.",null,"Klosz- poliwęglan przeźroczysty ze strukturą, stabilizowany UV.",null,null,"Ø50",null,"Oprawa nieściemnialna","Moduł LED","Philips LED Fortimo DLM ES 2000/830 G2",null,null,null,0,80,"E","111GA0009, 1270XX0009, 405ZX0009, 406ZX0009","Przewód H05VV-F 3G1 o długości 3,7m do podłączenia wewnątrz słupa oświetleniowego (w odpowiednio dobranej puszce elektroinstalacyjnej).","1915XX0011.jpg","1915XX0011.ldt",4,null,1,27]
["1920","1920XX0010","VANSBRO WALL E27","Vansbro","Wall","Stal",null,null,null,"Wymienne","E27",null,"LED max 9W",null,null,null,null,null,"55",null,"Class II",null,null,0,0,0,"CE",null,null,null,12,"Oprawa ścienna.","Światło odkryte, częściowo przysłonięte od góry.",null,"Scandinavian design wall-mounted luminaire. Possibility to install on corners of architectural objects.",null,null,"Oprawa na wymienne źródło światła typu: lampa LED, świetlówka TC-SE, tradycyjna żarówka (halogenowa) o trzonku E27. Źródło światła należy dokupić oddzielnie.","Stal cynkowana ogniowo. Miedź naturalna.","Stal malowana proszkowo.","Klosz- poliwęglan przeźroczysty, stabilizowany UV.",null,"Dławnica EPDM.",null,null,null,"Lampa E27","LED A55..60",null,null,null,null,80,null,"153XX0009, 159XX0009","Zaciski podłączeniowe: max 2x2,5mm², możliwość podłączenia oprawy w pętle max 2x1,5mm². Przewód w oponie okrągłej o średnicy ø7...10,5mm.","1920XX0010.jpg","1920XX0010.ldt",4,"E27",1,23]
["1921","1921XX0009","NAMSOS BOLLARD 95CM LED 1891LM 3000K DIM.","Namsos","Bollard","Aluminium",null,null,null,"LED zintegrowane","AC","DIM.","11W","13,6W","1891lm","843lm",null,null,"65","IK08","Class I",3000,null,0.24,0.12,0.95,"CE",null,null,"> 102 000h",1,"Oprawa słupkowa.","Światło rozproszone półsferyczne ukierunkowane w dół",null,"Luminaire with a modern design. For lighting gardens and other private and public areas",null,null,null,"Odlew aluminiowy malowany proszkowo.",null,"Klosz- szkło bezpieczne, satynowane.","Uszczelka silikonowa.","Dławnica EPDM.","95cm",null,"Oprawa ściemnialna fazowo TRAILING EDGE (TE) - LEADING EDGE (LE)","Moduł LED","Cree DK200305 V3 JB2835 3V 3K","TCI Mini MD 20W 500mA BI code 127033 Triak",0,null,null,80,"C","112ZX0009, 113GA0009, 114GA0009","Zaciski podłączeniowe: max 3x4mm², możliwość podłączenia oprawy w pętle max 3x4mm². Przewód w oponie okrągłej o średnicy: ø8...12mm lub ø10...14mm.","1921XX0009.jpg","1921XX0009.ldt",1,null,1,76]
["1922","1922XX0009","NAMSOS BOLLARD 95CM LED 2006LM 4000K DIM.","Namsos","Bollard","Aluminium",null,null,null,"LED zintegrowane","AC","DIM.","11W","14W","2006lm","907lm",null,null,"65","IK08","Class I",4000,null,0.24,0.12,0.95,"CE",null,null,"> 102 000h",1,"Oprawa słupkowa.","Światło rozproszone półsferyczne ukierunkowane w dół",null,"Luminaire with a modern design. For lighting gardens and other private and public areas",null,null,null,"Odlew aluminiowy malowany proszkowo.",null,"Klosz- szkło bezpieczne, satynowane.","Uszczelka silikonowa.","Dławnica EPDM.","95cm",null,"Oprawa ściemnialna fazowo TRAILING EDGE (TE) - LEADING EDGE (LE)","Moduł LED","Cree DK200305 V3 JB2835 3V 4K","TCI Mini MD 20W 500mA BI code 127033 Triak",0,null,null,80,"C","112ZX0009, 113GA0009, 114GA0009","Zaciski podłączeniowe: max 3x4mm², możliwość podłączenia oprawy w pętle max 3x4mm². Przewód w oponie okrągłej o średnicy: ø8...12mm lub ø10...14mm.","1922XX0009.jpg","1922XX0009.ldt",1,null,1,76]
["1923","1923XX0009","NAMSOS BOLLARD 65CM LED 1891LM 3000K DIM.","Namsos","Bollard","Aluminium",null,null,null,"LED zintegrowane","AC","DIM.","11W","13,6W","1891lm","843lm",null,null,"65","IK08","Class I",3000,null,0.24,0.12,0.65,"CE",null,null,"> 102 000h",1,"Oprawa słupkowa.","Światło rozproszone półsferyczne ukierunkowane w dół",null,"Luminaire with a modern design. For lighting gardens and other private and public areas",null,null,null,"Odlew aluminiowy malowany proszkowo.",null,"Klosz- szkło bezpieczne, satynowane.","Uszczelka silikonowa.","Dławnica EPDM.","65cm",null,"Oprawa ściemnialna fazowo TRAILING EDGE (TE) - LEADING EDGE (LE)","Moduł LED","Cree DK200305 V3 JB2835 3V 3K","TCI Mini MD 20W 500mA BI code 127033 Triak",0,null,null,80,"C","112ZX0009, 113GA0009, 114GA0009","Zaciski podłączeniowe: max 3x4mm², możliwość podłączenia oprawy w pętle max 3x4mm². Przewód w oponie okrągłej o średnicy max ø12,5mm.","1923XX0009.jpg","1923XX0009.ldt",1,null,1,76]
["1924","1924XX0009","NAMSOS BOLLARD 65CM LED 2006LM 4000K DIM.","Namsos","Bollard","Aluminium",null,null,null,"LED zintegrowane","AC","DIM.","11W","14W","2006lm","907lm",null,null,"65","IK08","Class I",4000,null,0.24,0.12,0.65,"CE",null,null,"> 102 000h",1,"Oprawa słupkowa.","Światło rozproszone półsferyczne ukierunkowane w dół",null,"Luminaire with a modern design. For lighting gardens and other private and public areas",null,null,null,"Odlew aluminiowy malowany proszkowo.",null,"Klosz- szkło bezpieczne, satynowane.","Uszczelka silikonowa.","Dławnica EPDM.","65cm",null,"Oprawa ściemnialna fazowo TRAILING EDGE (TE) - LEADING EDGE (LE)","Moduł LED","Cree DK200305 V3 JB2835 3V 4K","TCI Mini MD 20W 500mA BI code 127033 Triak",0,null,null,80,"C","112ZX0009, 113GA0009, 114GA0009","Zaciski podłączeniowe: max 3x4mm², możliwość podłączenia oprawy w pętle max 3x4mm². Przewód w oponie okrągłej o średnicy: ø8...12mm lub ø10...14mm.","1924XX0009.jpg","1924XX0009.ldt",1,null,1,76]
["1929","1929XX0010","NAMSOS WALL-RECESSED LED 1891LM 3000K DIM. TRIAC","Namsos","Bollard","Aluminium",null,null,null,"LED zintegrowane","AC","DIM. TRIAC","11W","13,6W","1891lm","843lm",null,null,"65","IK08","Class I",3000,null,0.22,0.22,0.12,"CE",null,null,"> 102 000h",11,"Oprawa wbudowana ścienna.","Światło rozproszone półsferyczne ukierunkowane w dół",null,"The luminaire is adapted to illuminate stairs, steps, staircases, pathways, ceiling illumination and the implementation of other architectural concepts",null,null,null,"Odlew aluminiowy malowany proszkowo.",null,"Klosz- szkło bezpieczne, satynowane.","Uszczelka silikonowa.","Dławnica EPDM.",null,null,"Oprawa ściemnialna fazowo TRAILING EDGE (TE) - LEADING EDGE (LE)","Moduł LED","Cree DK200305 V3 JB2835 3V 3K","TCI Mini MD 20W 500mA BI code 127033 Triak",0,null,null,80,"C",null,"Zaciski podłączeniowe: max 3x2,5mm², możliwość podłączenia oprawy w pętle max 3x1,5mm². Przewód w oponie okrągłej o średnicy ø7...10,5mm.","1929XX0010.jpg","1929XX0010.ldt",1,null,1,76]
["1930","1930XX0016","NAMSOS WALL-RECESSED LED 1176LM 3000K DIM.","Namsos","Recessed","Aluminium",null,null,null,"LED zintegrowane","AC","DIM.","6,5W","8,4W","1176lm","566lm",null,null,"65","IK08","Class I",3000,null,0.22,0.22,0.12,"CE",null,null,"> 102 000h",11,"Oprawa wbudowana ścienna.","Światło rozproszone półsferyczne ukierunkowane w dół",null,"The luminaire is adapted to illuminate stairs, steps, staircases, pathways, ceiling lighting and implementation of other architectural concepts",null,null,null,"Odlew aluminiowy malowany proszkowo.",null,"Klosz- szkło bezpieczne, satynowane.","Uszczelka silikonowa.","Dławnica EPDM.",null,null,"Oprawa ściemnialna fazowo TRAILING EDGE (TE) - LEADING EDGE (LE)","Moduł LED","Cree DK200305 V3 JB2835 3V 3K","KGP CC10W200-350CG",50000,"Dim. TRIAC (KGP)",null,80,"C",null,"Zaciski podłączeniowe: max 3x2,5mm², możliwość podłączenia oprawy w pętle max 3x1,5mm². Przewód w oponie okrągłej o średnicy ø7...10,5mm.","1930XX0016.jpg","1930XX0016.ldt",1,null,1,76]
["1931","1931XX0015","NAMSOS BOLLARD 95CM LED 1176LM 3000K DIM.","Namsos","Bollard","Aluminium",null,null,null,"LED zintegrowane","AC","DIM.","6,5W","8,4W","1176lm","566lm","Szkło",null,"65","IK08","Class I",3000,null,0.24,0.12,0.95,"CE",null,null,"> 102 000h",1,"Oprawa słupkowa.","Światło rozproszone półsferyczne ukierunkowane w dół",null,"Luminaire with a modern design. For lighting gardens and other private and public areas",null,null,null,"Odlew aluminiowy malowany proszkowo.",null,"Klosz- szkło bezpieczne, satynowane.","Uszczelka silikonowa.","Dławnica EPDM.","95cm",null,"Oprawa ściemnialna fazowo TRAILING EDGE (TE) - LEADING EDGE (LE)","Moduł LED","Cree DK200305 V3 JB2835 3V 3K","KGP CC10W200-350CG",50000,"Dim. TRIAC (KGP)",null,80,"C","112ZX0009, 113GA0009, 114GA0009","Zaciski podłączeniowe: max 3x4mm², możliwość podłączenia oprawy w pętle max 3x4mm². Przewód w oponie okrągłej o średnicy: ø8...12mm lub ø10...14mm.","1931XX0015.jpg","1931XX0015.ldt",1,null,1,76]
["1932","1932XX0014","NAMSOS BOLLARD 65CM LED 1176LM 3000K DIM.","Namsos","Bollard","Aluminium",null,null,null,"LED zintegrowane","AC","DIM.","6,5W","8,6W","1176lm","566lm","Tworzywo sztuczne","Satynowany","65","IK08","Class I",3000,null,0.24,0.12,0.65,"CE",null,null,"> 102 000h",1,"Oprawa słupkowa.","Światło rozproszone półsferyczne ukierunkowane w dół",null,"Luminaire with a modern design. For lighting gardens and other private and public areas",null,null,null,"Odlew aluminiowy malowany proszkowo.",null,"Klosz- szkło bezpieczne, satynowane.","Uszczelka silikonowa.","Dławnica EPDM.","65cm",null,"Oprawa ściemnialna fazowo TRAILING EDGE (TE) - LEADING EDGE (LE)","Moduł LED","Cree DK200305 V3 JB2835 3V 3K","KGP CC10W200-350CG",50000,"Dim. TRIAC (KGP)",null,80,"C","112ZX0009, 113GA0009, 114GA0009","Zaciski podłączeniowe: max 3x4mm², możliwość podłączenia oprawy w pętle max 3x4mm². Przewód w oponie okrągłej o średnicy: ø8...12mm lub ø10...14mm.","1932XX0014.jpg","1932XX0014.ldt",1,null,1,76]
["1933","1933XX0011","NAMSOS WALL-RECESSED LED 653LM 3000K DIM.","Namsos,Galvanized","Recessed","Stal",null,null,null,"LED zintegrowane","AC","DIM.","3,9W","5,2W","653lm","295lm",null,null,"44","IK10","Class I",3000,null,null,null,null,"CE",null,null,"> 70000",11,"Oprawa wbudowana ścienna.","Światło rozproszone półsferyczne ukierunkowane w dół",null,"The luminaire is adapted to illuminate stairs, steps, staircases, communication pathways and other applications",null,null,null,"Front- stal cynkowana ogniowo.","Korpus- odlew aluminiowy malowany proszkowo.","Klosz- szkło bezpieczne, satynowane.","Uszczelka silikonowa.","Dławnica EPDM.",null,null,"Oprawa ściemnialna fazowo TRAILING EDGE (TE)","Moduł LED","Philips Fortimo_LED_Strip_0.5ft_MF_8xx_HV6 3K","Philips Xitanium 7W 0,35A 20V TE SC 230V [2017]",50000,null,null,80,"C",null,"Zaciski podłączeniowe: max 3x2,5mm², możliwość podłączenia oprawy w pętle max 3x1,5mm². Przewód w oponie okrągłej o średnicy ø7...10,5mm.","1933XX0011.jpg","1933XX0011.ldt",1,null,1,76]
["1950","1950XX0B11","VOSS WALL 3XLED 2166LM 3000K ON/OFF","Voss","Wall","Aluminium",null,null,null,"LED zintegrowane","AC","ON/OFF","12,5W","15,4W","2166lm","705lm",null,null,"54","IK06","Class I",3000,"wąskie góra / szerokie dół",0.18,0.16,0.27,"CE",null,null,"> 102 000h",12,"Oprawa ścienna.","Światło dwustronne: o kącie 4º do góry i kącie 62º w dół.",null,"A luminaire with a wide range of applications, for lighting: wall and facade surfaces and other architectural concepts",null,null,null,"Odlew aluminiowy malowany proszkowo.",null,"Klosz- szkło bezpieczne, przeźroczyste.","Uszczelka silikonowa.","Dławnica EPDM.","góra/dół","wąskie/szerokie","Oprawa nieściemnialna","3 Moduły LED","Cree DK180501 V8 JB2835 3V 3K","Philips Xitanium 20W/m 0.15-0,5A 54V 230V",0,null,null,80,"C",null,"Zaciski podłączeniowe: max 3x2,5mm², możliwość podłączenia oprawy w pętle max 3x1,5mm². Przewód w oponie okrągłej o średnicy ø7...10,5mm.","1950XX0B11.jpg","1950XX0B11.ldt",4,null,1,31]
["1954","1954XX0D09","VOSS WALL LED 629LM DOWN 4º 3000K ON/OFF","Voss","Wall","Aluminium",null,null,null,"LED zintegrowane","AC","ON/OFF","4,5W","6,4W","629lm","55lm",null,null,"54","IK06","Class I",3000,"wąskie dół",0.18,0.16,0.27,"CE",null,null,"> 50 000",12,"Oprawa ścienna.","Światło jednostronne: o kącie 4º w dół.","Down 4º","A luminaire with a wide range of applications, including lighting: wall and facade surfaces as well as other architectural concepts",null,null,null,"Odlew aluminiowy malowany proszkowo.",null,"Klosz- szkło bezpieczne, przeźroczyste.","Uszczelka silikonowa.","Dławnica EPDM.","dół","wąskie jednostronne","Oprawa nieściemnialna","Moduł LED","Cree DK180501 V3 JK3030 3V 3K","Philips Xitanium 10W 0,5A 20V TE SC 230V",0,null,0,80,"E",null,"Zaciski podłączeniowe: max 3x2,5mm², możliwość podłączenia oprawy w pętle max 3x1,5mm². Przewód w oponie okrągłej o średnicy ø7...10,5mm.","1954XX0D09.jpg","1954XX0D09.ldt",4,null,1,40]
["1955","1955XX0H10","VOSS WALL 2XLED 1444LM UP62º 3000K DIM.","Voss","Wall","Aluminium",null,null,null,"LED zintegrowane","AC","DIM.","8,3W","16,8W","1444lm","557lm",null,null,"54",null,"Class I",3000,"szerokie góra",0.18,0.16,0.27,"CE",null,null,"> 102 000h",12,"Oprawa ścienna.","Światło jednostronne: o kącie 62º w górę.","Up62º","A luminaire with a wide range of applications, for lighting: wall and facade surfaces and other architectural concepts",null,null,null,"Odlew aluminiowy malowany proszkowo.",null,"Klosz- szkło bezpieczne, przeźroczyste.","Uszczelka silikonowa.","Dławnica EPDM.","jednostronne skierowane w dół","szerokie","Oprawa ściemnialna fazowo TRAILING EDGE (TE)","2 Moduły LED","Cree DK180501 V8 JB2835 3V 3K","Philips Xitanium 10W 0,5A 20V TE SC 230V",0,"Philips Xitanium TE",null,80,"C",null,"Zaciski podłączeniowe: max 3x2,5mm², możliwość podłączenia oprawy w pętle max 3x1,5mm². Przewód w oponie okrągłej o średnicy ø7...10,5mm.","1955XX0H10.jpg","1955XX0H10.ldt",1,null,1,56]
["1960","1960XX0009","LOFOTEN WALL E27","Lofoten","Wall","Stal",null,null,null,"Wymienne","E27",null,"LED max 11W","LED max 11W",null,null,null,null,"44",null,"Class II",null,null,null,null,null,"CE",null,null,null,12,"Oprawa ścienna.","Światło odkryte.",null,"A luminaire with a classic and simple design for general use, Perfect for lighting terraces, entrances, gazebos, and other architectural concepts",null,null,null,null,"Stal malowana proszkowo.","Klosz- tworzywo sztuczne PMMA w kolorze mlecznym.","Uszczelka silikonowa.","Dławnica EPDM.",null,null,null,"Lampa E27","LED A55...67",null,0,null,null,80,null,"46999021","Zaciski podłączeniowe: max 2x2,5mm², możliwość podłączenia oprawy w pętle max 2x1,5mm². Przewód w oponie okrągłej o średnicy ø7...10,5mm.","1960XX0009.jpg","1960XX0009.ldt",4,"E27",1,9]
["1963","1963XX0009","LOFOTEN UP WALL-ARM E27","Lofoten","Wall","Stal",null,null,null,"Wymienne","E27",null,"LED max 11W","LED max 11W",null,null,null,null,"44",null,"Class II",null,null,null,null,null,"CE",null,null,null,21,"Oprawa ścienna na ramieniu.","Światło odkryte.",null,"Luminaire with a classic and simple design for general use. Perfect for lighting terraces, entrances, gazebos and other architectural concepts. Possibility to mount the luminaire as a wall lamp directed upwards Possibility of mounting the luminaire on the corners",null,null,null,"Stal cynkowana galwanicznie i malowana proszkowo.",null,"Klosz- tworzywo sztuczne PMMA w kolorze mlecznym.",null,null,"góra","mleczny",null,"Lampa E27","LED A55...67",null,0,null,null,80,null,"155XX0009, 46999021","Zaciski podłączeniowe: max 2x2,5mm², możliwość podłączenia oprawy w pętle max 2x1,5mm². Przewód w oponie okrągłej o średnicy ø7...10,5mm.","1963XX0009.png","1963XX0009.ldt",4,"E27",1,9]
["1970","1970XX0009","MOLDE BOLLARD 80CM LED 743LM 3000K ON/OFF MD","Molde","Bollard","Aluminium",null,null,null,"LED zintegrowane","AC","ON/OFF","8W","8,2W","743lm","386lm",null,null,"54",null,"Class I",3000,null,0.8,0.16,0.11,"CE","Daylight sensor,Motion sensor",null,"> 55 000h",1,"Oprawa słupkowa.","Światło rozproszone przysłonięte od góry.",null,"Luminaire with a contemporary design For lighting private areas, parks and other architectural concepts",null,null,null,"Odlew aluminiowy malowany proszkowo.",null,"Klosz- poliwęglan przeźroczysty ze strukturą, stabilizowany UV.",null,null,"80cm","PIR","Oprawa wyposażona w czujnik ruchu typu PIR, z wyłącznikiem zmierzchowym i podtrzymaniem ruchu. Zaprogramowany na: maksymalny zasięg działania, czas świecenia 1 minuta, zmierzch 10lux.","Moduł LED","Lumens EDC 57C 8W xxx 230V F201 3K",null,0,"Czujnik ruchu PIR ESYLUX MD-C 360I/6 mini",null,80,"F","1907ZX0009, 1908GA0009, 4699990003","Zaciski podłączeniowe: max 3x4mm², możliwość podłączenia oprawy w pętle max 3x4mm². Przewód w oponie okrągłej o średnicy: ø4…8mm, ø8...12mm lub ø10...13,6mm","1970XX0009.jpg","1970XX0009.ldt",3,null,1,25]
["1971","1971XX0009","MOLDE BOLLARD 50CM LED 743LM 3000K ON/OFF MD","Molde","Bollard","Aluminium",null,null,null,"LED zintegrowane","AC","ON/OFF","8W","8,2W","743lm","386lm",null,null,"54",null,"Class I",3000,null,0.16,0.11,0.5,"CE","Daylight sensor,Motion sensor",null,"> 55 000h",1,"Oprawa słupkowa.","Światło rozproszone przysłonięte od góry.",null,"Luminaire with a contemporary design For lighting private areas, parks and other architectural concepts",null,null,null,"Odlew aluminiowy malowany proszkowo.",null,"Klosz- poliwęglan przeźroczysty ze strukturą, stabilizowany UV.",null,null,"50cm","PIR","Oprawa wyposażona w czujnik ruchu typu PIR, z wyłącznikiem zmierzchowym i podtrzymaniem ruchu. Zaprogramowany na: maksymalny zasięg działania, czas świecenia 1 minuta, zmierzch 10lux.","Moduł LED","Lumens EDC 57C 8W xxx 230V F201 3K",null,0,"Czujnik ruchu PIR ESYLUX MD-C 360I/6 mini",0.02,80,"F","1907ZX0009, 1908GA0009, 4699990003","Zaciski podłączeniowe: max 3x4mm², możliwość podłączenia oprawy w pętle max 3x4mm². Przewód w oponie okrągłej o średnicy: ø4…8mm, ø8...12mm lub ø10...13,6mm","1971XX0009.jpg","1971XX0009.ldt",3,null,1,25]
["1972","1972XX0009","MOLDE BOLLARD 80CM LED 772LM 4000K ON/OFF MD","Molde","Bollard","Aluminium",null,null,null,"LED zintegrowane","AC","ON/OFF","8W","8,2W","772lm","438lm",null,null,"54",null,"Class I",4000,null,0.8,0.16,0.11,"CE","Daylight sensor,Motion sensor",null,"> 55 000h",1,"Oprawa słupkowa.","Światło rozproszone przysłonięte od góry.",null,"Luminaire with a contemporary design For lighting private areas, parks and other architectural concepts",null,null,null,"Odlew aluminiowy malowany proszkowo.",null,"Klosz- poliwęglan przeźroczysty ze strukturą, stabilizowany UV.",null,null,"80cm","PIR","Oprawa wyposażona w czujnik ruchu typu PIR, z wyłącznikiem zmierzchowym i podtrzymaniem ruchu. Zaprogramowany na: maksymalny zasięg działania, czas świecenia 1 minuta, zmierzch 10lux.","Moduł LED","Lumens EDC 57C 8W xxx 230V F201 4K",null,0,"Czujnik ruchu PIR ESYLUX MD-C 360I/6 mini",null,80,"F","1907ZX0009, 1908GA0009, 4699990003","Zaciski podłączeniowe: max 3x4mm², możliwość podłączenia oprawy w pętle max 3x4mm². Przewód w oponie okrągłej o średnicy: ø4…8mm, ø8...12mm lub ø10...13,6mm","1972XX0009.jpg","1972XX0009.ldt",3,null,1,25]
["1973","1973XX0009","MOLDE BOLLARD 50CM LED 772LM 4000K ON/OFF MD","Molde","Bollard","Aluminium",null,null,null,"LED zintegrowane","AC","ON/OFF","8W","8,2W","772lm","438lm",null,null,"54",null,"Class I",4000,null,0.16,0.11,0.5,"CE","Daylight sensor,Motion sensor",null,"> 55 000h",1,"Oprawa słupkowa.","Światło rozproszone przysłonięte od góry.",null,"Luminaire with a contemporary design For lighting private areas, parks and other architectural concepts",null,null,null,"Odlew aluminiowy malowany proszkowo.",null,"Klosz- poliwęglan przeźroczysty ze strukturą, stabilizowany UV.",null,null,"50cm","PIR","Oprawa wyposażona w czujnik ruchu typu PIR, z wyłącznikiem zmierzchowym i podtrzymaniem ruchu. Zaprogramowany na: maksymalny zasięg działania, czas świecenia 1 minuta, zmierzch 10lux.","Moduł LED","Lumens EDC 57C 8W xxx 230V F201 4K",null,0,"Czujnik ruchu PIR ESYLUX MD-C 360I/6 mini",0.02,80,"F","1907ZX0009, 1908GA0009, 4699990003","Zaciski podłączeniowe: max 3x4mm², możliwość podłączenia oprawy w pętle max 3x4mm². Przewód w oponie okrągłej o średnicy: ø4…8mm, ø8...12mm lub ø10...13,6mm","1973XX0009.jpg","1973XX0009.ldt",3,null,1,25]
["2018","2018XX0010","STOCKHOLM POLE-TOP E27","Stockholm","Pole","Stal",null,null,null,"Wymienne","E27",null,"LED max 2x 9W","LED max 2x 9W",null,null,null,null,"54",null,"Class II",null,null,0.92,0.35,0.45,"CE",null,null,null,29,"Oprawa słupowa (do montażu na słupie).","Światło odkryte, częściowo przysłonięte od góry.",null,"Luminaire with Scandinavian design, mounted on a telescopic lighting pole with a diameter of ø50 mm. For lighting gardens, parks and other architectural concepts.",null,null,null,"Stal cynkowana ogniowo.","Stal malowana proszkowo.","Klosz- tworzywo sztuczne PMMA przeźroczyste.",null,null,"Podwójny",null,null,"Lampa E27","LED A55..60",null,0,null,null,80,null,null,"Zaciski podłączeniowe, max 2x2,5mm²","2018XX0010.jpg","2018XX0010.ldt",4,"E27",1,23]
["2026","2026XX0009","MOLDE WALL LED 743LM 3000K DIM.","Molde","Wall","Aluminium",null,null,null,"LED zintegrowane","AC","DIM.","8W","8W","743lm","386lm",null,null,"54","IK07","Class I",3000,null,0.3,0.23,0.11,"CE",null,null,"50000",12,"Oprawa ścienna.","Światło rozproszone przysłonięte od góry.",null,"A luminaire with a contemporary design. For lighting private areas, parks and other concepts architectural",null,null,null,"Odlew aluminiowy malowany proszkowo.",null,"Klosz- poliwęglan przeźroczysty ze strukturą, stabilizowany UV.",null,null,null,null,"Oprawa ściemnialna fazowo TRAILING EDGE (TE) - LEADING EDGE (LE)","Moduł LED","Lumens EDC 57C 8W xxx 230V F201 3K",null,0,"Ściemnianie fazowe Lumens LED AC",0.02,80,"F",null,"Zaciski podłączeniowe: max 3x2,5mm², możliwość podłączenia oprawy w pętle max 3x1,5mm². Przewód w oponie okrągłej o średnicy max ø6...10mm.","2026XX0009.png","2026XX0009.ldt",1,null,1,25]
["2027","2027XX0009","MOLDE WALL LED 772LM 4000K DIM.","Molde","Wall","Aluminium",null,null,null,"LED zintegrowane","AC","DIM.","8W","8W","772lm","438lm",null,null,"54","IK07","Class I",4000,null,0.23,0.11,0.3,"CE",null,null,"50 000h",12,"Oprawa ścienna.","Światło rozproszone przysłonięte od góry.",null,"A luminaire with a contemporary design. For lighting private areas, parks and other concepts architectural",null,null,null,"Odlew aluminiowy malowany proszkowo.",null,"Klosz- poliwęglan przeźroczysty ze strukturą, stabilizowany UV.",null,null,null,null,"Oprawa ściemnialna fazowo TRAILING EDGE (TE) - LEADING EDGE (LE)","Moduł LED","Lumens EDC 57C 8W xxx 230V F201 4K",null,0,"Ściemnianie fazowe Lumens LED AC",null,80,"F",null,"Zaciski podłączeniowe: max 3x2,5mm², możliwość podłączenia oprawy w pętle max 3x1,5mm². Przewód w oponie okrągłej o średnicy max ø12,5mm.","2027XX0009.png","2027XX0009.ldt",1,null,1,25]
["2028","2028XX0009","MOLDE WALL LED 743LM 3000K ON/OFF MD","Molde","Wall","Aluminium",null,null,null,"LED zintegrowane","AC","ON/OFF","8W","8W","743lm","386lm",null,null,"54","IK07","Class I",3000,null,0.3,0.23,0.11,"CE","Daylight sensor,Motion sensor",null,"50000",12,"Oprawa ścienna.","Światło rozproszone przysłonięte od góry.",null,"A luminaire with a contemporary design. For lighting private areas, parks and other concepts architectural",null,null,null,"Odlew aluminiowy malowany proszkowo.",null,"Klosz- poliwęglan przeźroczysty ze strukturą, stabilizowany UV.",null,null,null,"PIR","Oprawa wyposażona w czujnik ruchu typu PIR, z wyłącznikiem zmierzchowym i podtrzymaniem ruchu. Zaprogramowany na: maksymalny zasięg działania, czas świecenia 1 minuta, zmierzch 10lux.","Moduł LED","Lumens EDC 57C 8W xxx 230V F201 3K",null,0,"Czujnik ruchu PIR ESYLUX MD-C 360I/6 mini",0.02,80,"F",null,"Zaciski podłączeniowe: max 3x2,5mm², możliwość podłączenia oprawy w pętle max 3x1,5mm². Przewód w oponie okrągłej o średnicy max ø6...10mm.","2028XX0009.png","2028XX0009.ldt",3,null,1,25]
["2029","2029XX0009","MOLDE WALL LED 772LM 4000K ON/OFF MD","Molde","Wall","Aluminium",null,null,null,"LED zintegrowane","AC","ON/OFF","8W","8W","772lm","438lm",null,null,"54","IK07","Class I",4000,null,0.23,0.11,0.3,"CE","Daylight sensor,Motion sensor",null,"50 000h",12,"Oprawa ścienna.","Światło rozproszone przysłonięte od góry.",null,"A luminaire with a contemporary design. For lighting private areas, parks and other concepts architectural",null,null,null,"Odlew aluminiowy malowany proszkowo.",null,"Klosz- poliwęglan przeźroczysty ze strukturą, stabilizowany UV.",null,null,null,"PIR","Oprawa wyposażona w czujnik ruchu typu PIR, z wyłącznikiem zmierzchowym i podtrzymaniem ruchu. Zaprogramowany na: maksymalny zasięg działania, czas świecenia 1 minuta, zmierzch 10lux.","Moduł LED","Lumens EDC 57C 8W xxx 230V F201 4K",null,0,"Czujnik ruchu PIR ESYLUX MD-C 360I/6 mini",null,80,"F",null,"Zaciski podłączeniowe: max 3x2,5mm², możliwość podłączenia oprawy w pętle max 3x1,5mm². Przewód w oponie okrągłej o średnicy max ø12,5mm.","2029XX0009.png","2029XX0009.ldt",3,null,1,25]
["210","210XX0010","HALMSTAD BOLLARD 26CM E27","Halmstad","Bollard","Stal",null,null,null,"Wymienne","E27",null,"LED max 9W","LED max 9W",null,null,null,null,"65","IK10","Class II",null,null,0.26,0.12,0.12,"CE",null,null,null,1,"Oprawa słupkowa.","Światło odkryte, częściowo przysłonięte od góry.",null,"Bollard luminaire of stable and durable construction For lighting private areas and public spaces","Bollard luminaire of stable and durable construction For lighting private and public areas Functions: control, color change 2700K…6500K (TW), WiZ, WiZ Pro - Available after mounting in the luminaire, Signify WiZ Pro A60 E27 TW 8W 230V - Full control of the luminaire after installing the free application https://pro.wizconnected.com/ - Technical support: Information Sales Department of Norlys",null,null,"Stal cynkowana ogniowo.",null,"Klosz- tworzywo sztuczne PMMA w kolorze mlecznym.","Uszczelka silikonowa.",null,"26cm",null,null,"Lampa E27","LED A55..60",null,0,null,null,80,null,"205ZX0010, 206GA0010, 206GA0S10, 46999021","Zaciski podłączeniowe max 3x2,5mm². Przewód w oponie okrągłej o średnicy max ø12,5mm.","210XX0010.jpg","210XX0010.ldt",4,"E27",1,23]
["211","211XX0011","HALMSTAD BOLLARD 26CM LED 1098LM 3000K DIM. TRIAC","Halmstad","Bollard","Stal",null,null,null,"LED zintegrowane","AC","DIM. TRIAC",null,"10,5W","1098lm","295lm",null,null,"65","IK10","Class I",3000,null,0,0,0,"CE",null,null,"> 50 000h",1,"Oprawa słupkowa.","Światło odkryte, częściowo przysłonięte od góry.",null,"Bollard luminaire of stable and durable construction. For lighting private areas and public spaces.",null,null,null,"Stal cynkowana ogniowo.","Stal cynkowana ogniowo i malowana proszkowo.","Klosz- tworzywo sztuczne PMMA w kolorze mlecznym.","Uszczelka silikonowa.",null,"26cm","Triac","Oprawa ściemnialna fazowo TRAILING EDGE (TE) - LEADING EDGE (LE)","Moduł LED","Lumens EDC 47C 10W xxx 230V A101 3K",null,null,"Ściemnianie fazowe Lumens LED AC",0.44,80,"E","205ZX0010, 206GA0010","Zaciski podłączeniowe max 3x2,5mm². Przewód w oponie okrągłej o średnicy max ø12,5mm.","211XX0011.jpg","211XX0011.ldt",1,null,1,23]
["2120","2120XX0010","NIDAROS CEILING 9CM LED 1051LM DOWN 24º 3000K DIM.","Nidaros","Ceiling","Aluminium",null,null,null,"LED zintegrowane","AC","DIM.","10W","10,7W","1051lm","631lm",null,null,"65",null,"Class I",3000,"szerokie dół, montaż sufitowy",0.09,0.12,0.12,"CE",null,null,"50 000h",6,"Oprawa sufitowa.","Światło jednostronne: o kącie 24º w dół.","Down 24º","A luminaire with a wide range of applications mounted on horizontal surfaces, including lighting: wall and facade surfaces, and other architectural concepts",null,null,"Moduł LED, Wymienne (tylko LED) źródło światła przez profesjonalny serwis.","Odlew aluminiowy malowany proszkowo.",null,"Klosz- szkło bezpieczne, przeźroczyste.","Uszczelka silikonowa.",null,"9cm",null,"Oprawa ściemnialna fazowo TRAILING EDGE (TE) - LEADING EDGE (LE)","Moduł LED","Lumens EDC 57C 10W xxx 230V F201 3K",null,0,"Ściemnianie fazowe Lumens LED AC",0,80,"F",null,"Zaciski podłączeniowe: max 3x2,5mm², możliwość podłączenia oprawy w pętle max 1,5 mm². Przewód w oponie okrągłej o średnicy ø7...10,5mm.","2120XX0010.png","2120XX0010.ldt",1,null,1,54]
["2121","2121XX0010","NIDAROS CEILING 18CM LED 1051LM DOWN 24º 3000K DIM.","Nidaros","Ceiling","Aluminium",null,null,null,"LED zintegrowane","AC","DIM.","6,7W","7,8W","1051lm","765lm",null,null,"65",null,"Class I",3000,"szerokie dół",0.18,0.12,0.12,"CE",null,null,">110 000h",6,"Oprawa sufitowa.","Światło jednostronne: o kącie 24º w dół.","Down 24º","A luminaire with a wide range of applications mounted on horizontal surfaces, including lighting: walls, facade surfaces and other architectural concepts.",null,null,"Moduł LED, zasilacz elektroniczny Wymienne (tylko LED) źródło światła przez profesjonalny serwis. Wymienny osprzęt sterujący za pomocą profesjonalnego serwisu.","Odlew aluminiowy malowany proszkowo.",null,"Klosz- szkło bezpieczne, przeźroczyste.",null,null,"18cm",null,"Oprawa ściemnialna fazowo TRAILING EDGE (TE) - LEADING EDGE (LE)","Moduł LED","Philips Fortimo SLM C 1203 L09 1619 G7 3K","KGP CC10W180-270CG",50000,"Dim. TRIAC (KGP)",null,80,"D",null,"Zaciski podłączeniowe: max 3x2,5mm², możliwość podłączenia oprawy w pętle max 1,5mm². Przewód w oponie okrągłej o średnicy ø7...10,5mm.","2121XX0010.png","2121XX0010.ldt",1,null,1,54]
["2122","2122XX0010","NIDAROS CEILING 23CM LED 1051LM DOWN 24º 3000K DIM.","Nidaros","Ceiling","Aluminium",null,null,null,"LED zintegrowane","AC","DIM.","6,7W","8,3W","1051lm","765lm",null,null,"65",null,"Class I",3000,"szerokie dół",0.23,0.12,0.12,"CE",null,null,">50 000h",6,"Oprawa sufitowa.","Światło jednostronne: o kącie 24º w dół.","Down 24º","A luminaire with a wide range of applications can be mounted on horizontal surfaces, including wall, facade surfaces, and other architectural concepts",null,null,"Moduł LED, zasilacz elektroniczny Wymienne (tylko LED) źródło światła przez profesjonalny serwis. Wymienny osprzęt sterujący za pomocą profesjonalnego serwisu.","Odlew aluminiowy malowany proszkowo.",null,"Klosz- szkło bezpieczne, przeźroczyste.",null,null,"23cm",null,"Oprawa ściemnialna fazowo TRAILING EDGE (TE) - LEADING EDGE (LE)","Moduł LED","Philips Fortimo SLM C 1203 L09 1619 G7 3K","KGP CC10W180-270CG",50000,"Dim. TRIAC (KGP)",null,80,"D",null,"Zaciski podłączeniowe: max 3x2,5mm², możliwość podłączenia oprawy w pętle max 1,5mm². Przewód w oponie okrągłej o średnicy ø7...10,5mm.","2122XX0010.png","2122XX0010.ldt",1,null,1,54]
["2123","2123XX0010","NIDAROS CEILING 9CM LED 1051LM DOWN 24º 4000K DIM.","Nidaros","Ceiling","Aluminium",null,null,null,"LED zintegrowane","AC","DIM.","10W","10,7W","1051lm","631lm",null,null,"65",null,"Class I",4000,"szerokie dół, montaż sufitowy",0.09,0.12,0.12,"CE",null,null,"50 000h",6,"Oprawa sufitowa.","Światło jednostronne: o kącie 24º w dół.","Down 24º","A luminaire with a wide range of applications mounted on horizontal surfaces, including lighting: walls, facade surfaces and other architectural concepts.",null,null,"Moduł LED, Wymienne (tylko LED) źródło światła przez profesjonalny serwis.","Odlew aluminiowy malowany proszkowo.",null,"Klosz- szkło bezpieczne, przeźroczyste.","Uszczelka silikonowa.",null,"9cm",null,"Oprawa ściemnialna fazowo TRAILING EDGE (TE) - LEADING EDGE (LE)","Moduł LED","Lumens EDC 57C 10W xxx 230V F201 3K",null,0,"Ściemnianie fazowe Lumens LED AC",0,80,"F",null,"Zaciski podłączeniowe: max 3x2,5mm², możliwość podłączenia oprawy w pętle max 1,5 mm². Przewód w oponie okrągłej o średnicy ø7...10,5mm.","2123XX0010.png","2123XX0010.ldt",1,null,1,54]
["2124","2124XX0010","NIDAROS CEILING 18CM LED 1051LM DOWN 24º 4000K DIM.","Nidaros","Ceiling","Aluminium",null,null,null,"LED zintegrowane","AC","DIM.","6,7W","8,5W","1051lm","765lm",null,null,"65",null,"Class I",4000,"szerokie dół",0.18,0.12,0.12,"CE",null,null,"50 000h",6,"Oprawa sufitowa.","Światło jednostronne: o kącie 24º w dół.","Down 24º","A luminaire with a wide range of applications mounted on horizontal surfaces, including lighting: walls, facade surfaces and other architectural concepts.",null,null,"Moduł LED, zasilacz elektroniczny Wymienne (tylko LED) źródło światła przez profesjonalny serwis. Wymienny osprzęt sterujący za pomocą profesjonalnego serwisu.","Odlew aluminiowy malowany proszkowo.",null,"Klosz- szkło bezpieczne, przeźroczyste.",null,null,"18cm",null,"Oprawa ściemnialna fazowo TRAILING EDGE (TE) - LEADING EDGE (LE)","Moduł LED","Philips Fortimo SLM C 1203 L09 1619 G7 4K","KGP CC10W180-270CG",50000,"Dim. TRIAC (KGP)",null,80,"D",null,"Zaciski podłączeniowe: max 3x2,5mm², możliwość podłączenia oprawy w pętle max 1,5mm². Przewód w oponie okrągłej o średnicy ø7...10,5mm.","2124XX0010.png","2124XX0010.ldt",1,null,1,54]
["2125","2125XX0010","NIDAROS CEILING 23CM LED 1051LM DOWN 24º 4000K DIM.","Nidaros","Ceiling","Aluminium",null,null,null,"LED zintegrowane","AC","DIM.","6,7W","8,5W","1051lm","765lm",null,null,"65",null,"Class I",4000,"szerokie dół",0.23,0.12,0.12,"CE",null,null,"50 000h",6,"Oprawa sufitowa.","Światło jednostronne: o kącie 24º w dół.","Down 24º","A luminaire with a wide range of applications mounted on horizontal surfaces, including lighting: walls, facade surfaces and other architectural concepts.",null,null,"Moduł LED, zasilacz elektroniczny Wymienne (tylko LED) źródło światła przez profesjonalny serwis. Wymienny osprzęt sterujący za pomocą profesjonalnego serwisu.","Odlew aluminiowy malowany proszkowo.",null,"Klosz- szkło bezpieczne, przeźroczyste.",null,null,"23cm",null,"Oprawa ściemnialna fazowo TRAILING EDGE (TE) - LEADING EDGE (LE)","Moduł LED","Philips Fortimo SLM C 1203 L09 1619 G7 4K","KGP CC10W180-270CG",50000,"Dim. TRIAC (KGP)",null,80,"D",null,"Zaciski podłączeniowe: max 3x2,5mm², możliwość podłączenia oprawy w pętle max 1,5mm². Przewód w oponie okrągłej o średnicy ø7...10,5mm.","2125XX0010.png","2125XX0010.ldt",1,null,1,54]
["212","212XX0010","HALMSTAD BOLLARD 26CM E27 806LM 2700K DIM.","Halmstad","Bollard","Stal",null,null,null,"Wymienne","E27",null,"5,9W","5,9W","806lm",null,null,null,"65","IK10","Class II",2700,null,null,null,null,"CE",null,null,"25000",1,"Oprawa słupkowa.","Światło odkryte, częściowo przysłonięte od góry.",null,"Bollard luminaire of stable and durable construction. For lighting private areas and public spaces.",null,null,null,"Stal cynkowana ogniowo.",null,"Klosz- tworzywo sztuczne PMMA w kolorze mlecznym.","Uszczelka silikonowa.",null,"26cm",null,"Oprawa ściemnialna fazowo TRAILING EDGE (TE) - LEADING EDGE (LE)","Lampa E27","Philips MAS LEDBulb DT5.9-60W E27 927 A60 FR G",null,0,"Ściemnianie fazowe LED GU10 E27",null,80,"F","205ZX0010, 206GA0010, 206GA0S10","Zaciski podłączeniowe max 3x2,5mm². Przewód w oponie okrągłej o średnicy max ø12,5mm.","212XX0010.jpg","212XX0010.ldt",1,"E27",1,23]
["2240","2240XX0009","STAVANGER BOLLARD 95CM LED 1940LM 3000K DIM.","Stavanger","Bollard","Aluminium",null,null,null,"LED zintegrowane","AC","DIM.","10,9W","13,6W","1940lm","483lm",null,null,"65","IK08","Class II",3000,null,0.2,0.2,0.95,"CE",null,null,"> 72 000h",1,"Oprawa słupkowa.","Światło rozproszone.",null,"Luminaire with a modern design For lighting gardens and other private land and public areas",null,null,null,"Odlew aluminiowy malowany proszkowo.",null,"Klosz- tworzywo sztuczne PMMA satynowane.","Uszczelka silikonowa.","Dławnica nylon6.","95cm","satyna PMMA","Oprawa ściemnialna fazowo TRAILING EDGE (TE) - LEADING EDGE (LE)","Moduł LED","Cree DK210704 V2 JB2835 3V 3K","TCI Mini MD 20W 500mA code 127032 Triak",0,null,null,80,"C","1230ZX0009, 1231GA0009, 1232GA0009, 6139ZX0009, 7662ZX0009","Zaciski podłączeniowe: max 2x4mm², możliwość podłączenia oprawy w pętle max 2x4mm². Przewód w oponie okrągłej o średnicy ø8...17mm.","2240XX0009.jpg","2240XX0009.ldt",1,null,1,7]
["2241","2241XX0009","STAVANGER BOLLARD 95CM LED 2058LM 4000K DIM.","Stavanger","Bollard","Aluminium",null,null,null,"LED zintegrowane","AC","DIM.","10,9W","13,6W","2058lm","565lm",null,null,"65","IK08","Class II",4000,null,0.2,0.2,0.95,"CE",null,null,"> 72 000h",1,"Oprawa słupkowa.","Światło rozproszone.",null,"Luminaire with a modern design For lighting gardens and other private land and public areas",null,null,null,"Odlew aluminiowy malowany proszkowo.",null,"Klosz- tworzywo sztuczne PMMA satynowane.","Uszczelka silikonowa.","Dławnica nylon6.","95cm","satyna PMMA","Oprawa ściemnialna fazowo TRAILING EDGE (TE) - LEADING EDGE (LE)","Moduł LED","Cree DK210704 V2 JB2835 3V 4K","TCI Mini MD 20W 500mA code 127032 Triak",0,null,null,80,"C","1230ZX0009, 1231GA0009, 1232GA0009, 6139ZX0009, 7662ZX0009","Zaciski podłączeniowe: max 2x4mm², możliwość podłączenia oprawy w pętle max 2x4mm². Przewód w oponie okrągłej o średnicy ø8...17mm.","2241XX0009.jpg","2241XX0009.ldt",1,null,1,7]
["2244","2244XX0009","STAVANGER BOLLARD 50CM LED 1940LM 3000K DIM.","Stavanger","Bollard","Aluminium",null,null,null,"LED zintegrowane","AC","DIM.","10,9W","13,6W","1940lm","483lm",null,null,"65","IK08","Class II",3000,null,0.2,0.2,0.5,"CE",null,null,"> 72 000h",1,"Oprawa słupkowa.","Światło rozproszone.",null,"A bollard luminaire with a stable and durable structure For lighting gardens, private areas and other architectural applications",null,null,null,"Odlew aluminiowy malowany proszkowo.",null,"Klosz- tworzywo sztuczne PMMA satynowane.","Uszczelka silikonowa.","Dławnica nylon6.","50cm","satyna PMMA",null,"Moduł LED","Cree DK210704 V2 JB2835 3V 3K","TCI Mini MD 20W 500mA code 127032 Triak",0,null,null,80,"C","1230ZX0009, 1231GA0009, 1232GA0009","Zaciski podłączeniowe: max 2x4mm², możliwość podłączenia oprawy w pętle max 2x4mm². Przewód w oponie okrągłej o średnicy ø8...17mm.","2244XX0009.jpg","2244XX0009.ldt",1,null,1,7]
["2245","2245XX0009","STAVANGER BOLLARD 50CM LED 2058LM 4000K DIM.","Stavanger","Bollard","Aluminium",null,null,null,"LED zintegrowane","AC","DIM.","10,9W","13,6W","2058lm","565lm",null,null,"65","IK08","Class II",4000,null,0.2,0.2,0.5,"CE",null,null,"> 72 000h",1,"Oprawa słupkowa.","Światło rozproszone.",null,"A bollard luminaire with a stable and durable structure For lighting gardens, private areas and other architectural applications",null,null,null,"Odlew aluminiowy malowany proszkowo.",null,"Klosz- tworzywo sztuczne PMMA satynowane.","Uszczelka silikonowa.","Dławnica nylon6.","50cm","satyna PMMA","Oprawa ściemnialna fazowo TRAILING EDGE (TE) - LEADING EDGE (LE)","Moduł LED","Cree DK210704 V2 JB2835 3V 4K","TCI Mini MD 20W 500mA code 127032 Triak",0,null,null,80,"C","1230ZX0009, 1231GA0009, 1232GA0009","Zaciski podłączeniowe: max 2x4mm², możliwość podłączenia oprawy w pętle max 2x4mm². Przewód w oponie okrągłej o średnicy ø8...17mm.","2245XX0009.jpg","2245XX0009.ldt",1,null,1,7]
["2248","2248XX0009","STAVANGER BOLLARD 28CM LED 1386LM 3000K DIM.","Stavanger","Bollard","Aluminium",null,null,null,"LED zintegrowane","AC","DIM.","7,5W","8,9W","1386lm","337lm",null,null,"65","IK08","Class II",3000,null,0.2,0.2,0.28000000000000003,"CE",null,null,"> 72 000h",1,"Oprawa słupkowa.","Światło rozproszone.",null,"A bollard luminaire with a stable and durable structure. For lighting gardens, private areas and other architectural applications",null,null,null,"Odlew aluminiowy malowany proszkowo.",null,"Klosz- tworzywo sztuczne PMMA satynowane.","Uszczelka silikonowa.","Dławnica nylon6.","28cm","satyna PMMA","Oprawa ściemnialna fazowo TRAILING EDGE (TE) - LEADING EDGE (LE)","Moduł LED","Cree DK210704 V2 JB2835 3V 3K","TCI MICRO MD 10W 350mA 127040 Triac",0,null,null,80,"C","1230ZX0009, 1231GA0009, 1232GA0009","Zaciski podłączeniowe: max 2x4mm², możliwość podłączenia oprawy w pętle max 2x4mm². Przewód w oponie okrągłej o średnicy ø8...17mm.","2248XX0009.jpg","2248XX0009.ldt",1,null,1,7]
["2249","2249XX0009","STAVANGER BOLLARD 28CM LED 1470LM 4000K DIM.","Stavanger","Bollard","Aluminium",null,null,null,"LED zintegrowane","AC","DIM.","7,5W","8,9W","1470lm","403lm",null,null,"65","IK08","Class II",4000,null,0.2,0.2,0.28000000000000003,"CE",null,null,"> 72 000h",1,"Oprawa słupkowa.","Światło rozproszone.",null,"A bollard luminaire with a stable and durable structure For lighting gardens, private areas and other architectural applications",null,null,null,"Odlew aluminiowy malowany proszkowo.",null,"Klosz- tworzywo sztuczne PMMA satynowane.","Uszczelka silikonowa.","Dławnica nylon6.","28cm","satyna PMMA","Oprawa ściemnialna fazowo TRAILING EDGE (TE) - LEADING EDGE (LE)","Moduł LED","Cree DK210704 V2 JB2835 3V 4K","TCI MICRO MD 10W 350mA 127040 Triac",0,null,null,80,"C","1230ZX0009, 1231GA0009, 1232GA0009","Zaciski podłączeniowe: max 2x4mm², możliwość podłączenia oprawy w pętle max 2x4mm². Przewód w oponie okrągłej o średnicy ø8...17mm.","2249XX0009.jpg","2249XX0009.ldt",1,null,1,7]
["2304","2304XX0009","EGERSUND WOOD BOLLARD 85CM LED 1370LM 3000K DIM.","Egersund Mini,Wood","Bollard","Drewno","Malowane",null,null,"LED zintegrowane","AC","DIM.","7,4W","9,1W","1370lm","864lm",null,null,"65",null,"Class II",3000,null,0.12,0.12,0.85,"CE",null,null,"72 000h",1,"Oprawa słupkowa.","Światło obrotowo-symetryczne.",null,"Luminaire with contemporary design. For lighting gardens, private areas, and other architectural applications",null,null,null,"Odlew aluminiowy malowany proszkowo.","Drewno- sosna skandynawska malowana","Klosz- tworzywo sztuczne PMMA przeźroczyste.","Uszczelka silikonowa.",null,"85cm","Drewno malowane","Oprawa ściemnialna fazowo TRAILING EDGE (TE) - LEADING EDGE (LE)","Moduł LED","Cree DK210704 V2 JB2835 3V 3K","TCI MICRO MD 10W 350mA 127040 Triac",0,null,null,80,"C","205ZX0010, 206GA0010, 206GA0S10","Zaciski podłączeniowe: max 2x4mm², możliwość podłączenia oprawy w pętle max 2x4mm². Przewód w oponie okrągłej o średnicy ø8...12,5mm.","2304XX0009.png","2304XX0009.ldt",1,null,1,17]
["2305","2305XX0009","EGERSUND WOOD BOLLARD 85CM LED 1462LM 4000K DIM.","Egersund Mini,Wood","Bollard","Drewno","Malowane",null,null,"LED zintegrowane","AC","DIM.","7,4W","9,1W","1462lm","873lm",null,null,"65",null,"Class II",4000,null,0.12,0.12,0.85,"CE",null,null,"72 000h",1,"Oprawa słupkowa.","Światło obrotowo-symetryczne.",null,"Luminaire with contemporary design. For lighting gardens, private areas, and other architectural applications",null,null,null,"Odlew aluminiowy malowany proszkowo.","Drewno- sosna skandynawska malowana","Klosz- tworzywo sztuczne PMMA przeźroczyste.","Uszczelka silikonowa.",null,"85cm","Drewno malowane","Oprawa ściemnialna fazowo TRAILING EDGE (TE) - LEADING EDGE (LE)","Moduł LED","Cree DK210704 V2 JB2835 3V 4K","TCI MICRO MD 10W 350mA 127040 Triac",0,null,null,80,"C","205ZX0010, 206GA0010, 206GA0S10","Zaciski podłączeniowe: max 2x4mm², możliwość podłączenia oprawy w pętle max 2x4mm². Przewód w oponie okrągłej o średnicy ø8...12,5mm.","2305XX0009.png","2305XX0009.ldt",1,null,1,17]
["2308","2308XX0009","EGERSUND WOOD BOLLARD 85CM LED 1370LM 3000K DIM.","Egersund Mini,Wood","Bollard","Drewno","Impregnowane",null,null,"LED zintegrowane","AC","DIM.","7,4W","9,1W","1370lm","864lm",null,null,"65",null,"Class II",3000,null,0.12,0.12,0.85,"CE",null,null,"72 000h",1,"Oprawa słupkowa.","Światło obrotowo-symetryczne.",null,"Luminaire with contemporary design. For lighting gardens, private areas, and other architectural applications",null,null,null,"Odlew aluminiowy malowany proszkowo.","Drewno- sosna skandynawska impregnowana","Klosz- tworzywo sztuczne PMMA przeźroczyste.","Uszczelka silikonowa.",null,"85cm","Drewno impregnowane","Oprawa ściemnialna fazowo TRAILING EDGE (TE) - LEADING EDGE (LE)","Moduł LED","Cree DK210704 V2 JB2835 3V 3K","TCI MICRO MD 10W 350mA 127040 Triac",0,null,null,80,"C","205ZX0010, 206GA0010, 206GA0S10","Zaciski podłączeniowe: max 2x4mm², możliwość podłączenia oprawy w pętle max 2x4mm². Przewód w oponie okrągłej o średnicy ø8...12,5mm.","2308XX0009.png","2308XX0009.ldt",1,null,1,17]
["2309","2309XX0009","EGERSUND WOOD BOLLARD 85CM LED 1462LM 4000K DIM.","Egersund Mini,Wood","Bollard","Drewno","Impregnowane",null,null,"LED zintegrowane","AC","DIM.","7,4W","9,1W","1462lm","873lm",null,null,"65",null,"Class II",4000,null,0.12,0.12,0.85,"CE",null,null,"72 000h",1,"Oprawa słupkowa.","Światło obrotowo-symetryczne.",null,"Luminaire with contemporary design. For lighting gardens, private areas, and other architectural applications",null,null,null,"Odlew aluminiowy malowany proszkowo.","Drewno- sosna skandynawska impregnowana","Klosz- tworzywo sztuczne PMMA przeźroczyste.","Uszczelka silikonowa.",null,"85cm","Drewno impregnowane","Oprawa ściemnialna fazowo TRAILING EDGE (TE) - LEADING EDGE (LE)","Moduł LED","Cree DK210704 V2 JB2835 3V 4K","TCI MICRO MD 10W 350mA 127040 Triac",0,null,null,80,"C","205ZX0010, 206GA0010, 206GA0S10","Zaciski podłączeniowe: max 2x4mm², możliwość podłączenia oprawy w pętle max 2x4mm². Przewód w oponie okrągłej o średnicy ø8...12,5mm.","2309XX0009.png","2309XX0009.ldt",1,null,1,17]
["2317","2317XX0009","EGERSUND WOOD BOLLARD 49CM LED 1462LM 4000K DIM.","Egersund Mini,Wood","Bollard","Drewno","Malowane",null,null,"LED zintegrowane","AC","DIM.","7,4W","9,1W","1462lm","873lm",null,null,"65",null,"Class II",4000,null,0.12,0.12,0.49,"CE",null,null,"72 000h",1,"Oprawa słupkowa.","Światło obrotowo-symetryczne.",null,"Luminaire with contemporary design. For lighting gardens, private areas, and other architectural applications",null,null,null,"Odlew aluminiowy malowany proszkowo.","Drewno- sosna skandynawska malowana","Klosz- tworzywo sztuczne PMMA przeźroczyste.","Uszczelka silikonowa.",null,"49cm","Drewno malowane","Oprawa ściemnialna fazowo TRAILING EDGE (TE) - LEADING EDGE (LE)","Moduł LED","Cree DK210704 V2 JB2835 3V 4K","TCI MICRO MD 10W 350mA 127040 Triac",0,null,null,80,"C","205ZX0010, 206GA0010, 206GA0S10","Zaciski podłączeniowe: max 2x4mm², możliwość podłączenia oprawy w pętle max 2x4mm². Przewód w oponie okrągłej o średnicy ø8...12,5mm.","2317XX0009.png","2317XX0009.ldt",1,null,1,17]
["2320","2320XX0009","EGERSUND WOOD BOLLARD 49CM LED 1370LM 3000K DIM.","Egersund Mini,Wood","Bollard","Drewno","Impregnowane",null,null,"LED zintegrowane","AC","DIM.","7,4W","9,1W","1370lm","864lm",null,null,"65",null,"Class II",3000,null,0.12,0.12,0.49,"CE",null,null,"72 000h",1,"Oprawa słupkowa.","Światło obrotowo-symetryczne.",null,"Luminaire with contemporary design. For lighting gardens, private areas, and other architectural applications",null,null,null,"Odlew aluminiowy malowany proszkowo.","Drewno- sosna skandynawska impregnowana","Klosz- tworzywo sztuczne PMMA przeźroczyste.","Uszczelka silikonowa.",null,"49cm","Drewno impregnowane","Oprawa ściemnialna fazowo TRAILING EDGE (TE) - LEADING EDGE (LE)","Moduł LED","Cree DK210704 V2 JB2835 3V 3K","TCI MICRO MD 10W 350mA 127040 Triac",0,null,null,80,"C","205ZX0010, 206GA0010, 206GA0S10","Zaciski podłączeniowe: max 2x4mm², możliwość podłączenia oprawy w pętle max 2x4mm². Przewód w oponie okrągłej o średnicy ø8...12,5mm.","2320XX0009.png","2320XX0009.ldt",1,null,1,17]
["2321","2321XX0009","EGERSUND WOOD BOLLARD 49CM LED 1462LM 4000K DIM.","Egersund Mini,Wood","Bollard","Drewno","Impregnowane",null,null,"LED zintegrowane","AC","DIM.","7,4W","9,1W","1462lm","873lm",null,null,"65",null,"Class II",4000,null,0.12,0.12,0.49,"CE",null,null,"72 000h",1,"Oprawa słupkowa.","Światło obrotowo-symetryczne.",null,"Luminaire with contemporary design. For lighting gardens, private areas, and other architectural applications",null,null,null,"Odlew aluminiowy malowany proszkowo.","Drewno- sosna skandynawska impregnowana","Klosz- tworzywo sztuczne PMMA przeźroczyste.","Uszczelka silikonowa.",null,"49cm","Drewno impregnowane","Oprawa ściemnialna fazowo TRAILING EDGE (TE) - LEADING EDGE (LE)","Moduł LED","Cree DK210704 V2 JB2835 3V 4K","TCI MICRO MD 10W 350mA 127040 Triac",0,null,null,80,"C","205ZX0010, 206GA0010, 206GA0S10","Zaciski podłączeniowe: max 2x4mm², możliwość podłączenia oprawy w pętle max 2x4mm². Przewód w oponie okrągłej o średnicy ø8...12,5mm.","2321XX0009.png","2321XX0009.ldt",1,null,1,17]
["2330","2330XX0009","LILLESAND BOLLARD 85CM LED 1370LM 3000K DIM.","Lillesand","Bollard","Aluminium",null,null,null,"LED zintegrowane","AC","DIM.","7,4W","9,2W","1370lm","897lm",null,null,"65","IK08","Class II",3000,null,null,null,null,"CE",null,null,"> 72 000h",1,"Oprawa słupkowa.","Światło obrotowo-symetryczne.",null,"Luminaire with contemporary design. For lighting gardens, private areas, and other architectural structures",null,null,null,"Odlew aluminiowy malowany proszkowo.",null,"Klosz- tworzywo sztuczne PMMA satynowane.","Uszczelka silikonowa.","Dławnica nylon6.","85cm",null,"Oprawa ściemnialna fazowo TRAILING EDGE (TE) - LEADING EDGE (LE)","Moduł LED","Cree DK210704 V2 JB2835 3V 3K","TCI MICRO MD 10W 350mA 127040 Triac",0,null,null,80,"C","205ZX0010, 206GA0010, 206GA0S10, 2951ZX0009, 6138ZX0009","Zaciski podłączeniowe: max 2x4mm², możliwość podłączenia oprawy w pętle max 2x2,5mm². Przewód w oponie okrągłej o średnicy ø8...12,5mm.","2330XX0009.png","2330XX0009.ldt",1,null,1,17]
["2331","2331XX0009","LILLESAND BOLLARD 85CM LED 1462LM 4000K DIM.","Lillesand","Bollard","Aluminium",null,null,null,"LED zintegrowane","AC","DIM.","7,4W","9,2W","1462lm","956lm",null,null,"65","IK08","Class II",4000,null,null,null,null,"CE",null,null,"> 72 000h",1,"Oprawa słupkowa.","Światło obrotowo-symetryczne.",null,"Luminaire with contemporary design. For lighting gardens, private areas, and other architectural structures",null,null,null,"Odlew aluminiowy malowany proszkowo.",null,"Klosz- tworzywo sztuczne PMMA satynowane.","Uszczelka silikonowa.","Dławnica nylon6.","85cm",null,"Oprawa ściemnialna fazowo TRAILING EDGE (TE) - LEADING EDGE (LE)","Moduł LED","Cree DK210704 V2 JB2835 3V 4K","TCI MICRO MD 10W 350mA 127040 Triac",0,null,null,80,"C","205ZX0010, 206GA0010, 206GA0S10, 2951ZX0009, 6138ZX0009","Zaciski podłączeniowe: max 2x4mm², możliwość podłączenia oprawy w pętle max 2x2,5mm². Przewód w oponie okrągłej o średnicy ø8...12,5mm.","2331XX0009.png","2331XX0009.ldt",1,null,1,17]
["2334","2334XX0009","LILLESAND WOOD BOLLARD 85CM LED 1370LM 3000K DIM.","Lillesand,Wood","Bollard","Drewno","Malowane",null,null,"LED zintegrowane","AC","DIM.","7,4W","9,2W","1370lm","897lm",null,null,"65",null,"Class II",3000,null,0,0,0,"CE",null,null,"72 000h",1,"Oprawa słupkowa.","Światło obrotowo-symetryczne.",null,"A luminaire with a contemporary design. For lighting gardens, private areas and other architectural concepts.",null,null,null,"Odlew aluminiowy malowany proszkowo.","Drewno- sosna skandynawska malowana","Klosz- tworzywo sztuczne PMMA satynowane.","Uszczelka silikonowa.",null,"85cm",null,"Oprawa ściemnialna fazowo TRAILING EDGE (TE) - LEADING EDGE (LE)","Moduł LED","Cree DK210704 V2 JB2835 3V 3K","TCI MICRO MD 10W 350mA 127040 Triac",0,null,null,80,"C","205ZX0010, 206GA0010, 206GA0S10","Zaciski podłączeniowe: max 2x4mm², możliwość podłączenia oprawy w pętle max 2x4mm². Przewód w oponie okrągłej o średnicy ø8...12,5mm.","2334XX0009.png","2334XX0009.ldt",1,null,1,17]
["2335","2335XX0009","LILLESAND WOOD BOLLARD 85CM LED 1462LM 4000K DIM.","Lillesand,Wood","Bollard","Drewno","Malowane",null,null,"LED zintegrowane","AC","DIM.","7,4W","9,2W","1462lm","956lm",null,null,"65",null,"Class II",4000,null,0,0,0,"CE",null,null,"72 000h",1,"Oprawa słupkowa.","Światło obrotowo-symetryczne.",null,"A luminaire with a contemporary design. For lighting gardens, private areas and other architectural concepts.",null,null,null,"Odlew aluminiowy malowany proszkowo.","Drewno- sosna skandynawska malowana","Klosz- tworzywo sztuczne PMMA satynowane.","Uszczelka silikonowa.",null,"85cm",null,"Oprawa ściemnialna fazowo TRAILING EDGE (TE) - LEADING EDGE (LE)","Moduł LED","Cree DK210704 V2 JB2835 3V 4K","TCI MICRO MD 10W 350mA 127040 Triac",0,null,null,80,"C","205ZX0010, 206GA0010, 206GA0S10","Zaciski podłączeniowe: max 2x4mm², możliwość podłączenia oprawy w pętle max 2x4mm². Przewód w oponie okrągłej o średnicy ø8...12,5mm.","2335XX0009.png","2335XX0009.ldt",1,null,1,17]
["2338","2338XX0009","LILLESAND WOOD BOLLARD 85CM LED 1370LM 3000K DIM.","Lillesand,Wood","Bollard","Drewno","Impregnowane",null,null,"LED zintegrowane","AC","DIM.","7,4W","9,2W","1370lm","897lm",null,null,"65",null,"Class II",3000,null,0,0,0,"CE",null,null,"72 000h",1,"Oprawa słupkowa.","Światło obrotowo-symetryczne.",null,"A luminaire with a contemporary design. For lighting gardens, private areas and other architectural concepts.",null,null,null,"Odlew aluminiowy malowany proszkowo.","Drewno- sosna skandynawska impregnowana","Klosz- tworzywo sztuczne PMMA satynowane.","Uszczelka silikonowa.",null,"85cm",null,"Oprawa ściemnialna fazowo TRAILING EDGE (TE) - LEADING EDGE (LE)","Moduł LED","Cree DK210704 V2 JB2835 3V 3K","TCI MICRO MD 10W 350mA 127040 Triac",0,null,null,80,"C","205ZX0010, 206GA0010, 206GA0S10","Zaciski podłączeniowe: max 2x4mm², możliwość podłączenia oprawy w pętle max 2x4mm². Przewód w oponie okrągłej o średnicy ø8...12,5mm.","2338XX0009.png","2338XX0009.ldt",1,null,1,17]
["2339","2339XX0009","LILLESAND WOOD BOLLARD 85CM LED 1462LM 4000K DIM.","Lillesand,Wood","Bollard","Drewno","Impregnowane",null,null,"LED zintegrowane","AC","DIM.","7,4W","9,2W","1462lm","956lm",null,null,"65",null,"Class II",4000,null,0,0,0,"CE",null,null,"72 000h",1,"Oprawa słupkowa.","Światło obrotowo-symetryczne.",null,"A luminaire with a contemporary design. For lighting gardens, private areas and other architectural concepts.",null,null,null,"Odlew aluminiowy malowany proszkowo.","Drewno- sosna skandynawska impregnowana","Klosz- tworzywo sztuczne PMMA satynowane.","Uszczelka silikonowa.",null,"85cm",null,"Oprawa ściemnialna fazowo TRAILING EDGE (TE) - LEADING EDGE (LE)","Moduł LED","Cree DK210704 V2 JB2835 3V 4K","TCI MICRO MD 10W 350mA 127040 Triac",0,null,null,80,"C","205ZX0010, 206GA0010, 206GA0S10","Zaciski podłączeniowe: max 2x4mm², możliwość podłączenia oprawy w pętle max 2x4mm². Przewód w oponie okrągłej o średnicy ø8...12,5mm.","2339XX0009.png","2339XX0009.ldt",1,null,1,17]
["2342","2342XX0009","LILLESAND BOLLARD 49CM LED 1370LM 3000K DIM.","Lillesand","Bollard","Aluminium",null,null,null,"LED zintegrowane","AC","DIM.","7,4W","9,2W","1370lm","897lm",null,null,"65","IK08","Class II",3000,null,null,null,null,"CE",null,null,"> 72 000h",1,"Oprawa słupkowa.","Światło obrotowo-symetryczne.",null,"Luminaire with contemporary design. For lighting gardens, private areas, and other architectural structures",null,null,null,"Odlew aluminiowy malowany proszkowo.",null,"Klosz- tworzywo sztuczne PMMA satynowane.","Uszczelka silikonowa.","Dławnica nylon6.","49cm",null,"Oprawa ściemnialna fazowo TRAILING EDGE (TE) - LEADING EDGE (LE)","Moduł LED","Cree DK210704 V2 JB2835 3V 3K","TCI MICRO MD 10W 350mA 127040 Triac",0,null,null,80,"C","205ZX0010, 206GA0010, 206GA0S10, 2951ZX0009, 6138ZX0009","Zaciski podłączeniowe: max 2x4mm², możliwość podłączenia oprawy w pętle max 2x2,5mm². Przewód w oponie okrągłej o średnicy ø8...12,5mm.","2342XX0009.png","2342XX0009.ldt",1,null,1,17]
["2343","2343XX0009","LILLESAND BOLLARD 49CM LED 1462LM 4000K DIM.","Lillesand","Bollard","Aluminium",null,null,null,"LED zintegrowane","AC","DIM.","7,4W","9,2W","1462lm","956lm",null,null,"65","IK08","Class II",4000,null,null,null,null,"CE",null,null,"> 72 000h",1,"Oprawa słupkowa.","Światło obrotowo-symetryczne.",null,"Luminaire with contemporary design. For lighting gardens, private areas, and other architectural structures",null,null,null,"Odlew aluminiowy malowany proszkowo.",null,"Klosz- tworzywo sztuczne PMMA satynowane.","Uszczelka silikonowa.","Dławnica nylon6.","49cm",null,"Oprawa ściemnialna fazowo TRAILING EDGE (TE) - LEADING EDGE (LE)","Moduł LED","Cree DK210704 V2 JB2835 3V 4K","TCI MICRO MD 10W 350mA 127040 Triac",0,null,null,80,"C","205ZX0010, 206GA0010, 206GA0S10, 2951ZX0009, 6138ZX0009","Zaciski podłączeniowe: max 2x4mm², możliwość podłączenia oprawy w pętle max 2x2,5mm². Przewód w oponie okrągłej o średnicy ø8...12,5mm.","2343XX0009.png","2343XX0009.ldt",1,null,1,17]
["2346","2346XX0009","LILLESAND WOOD BOLLARD 49CM LED 1370LM 3000K DIM.","Lillesand,Wood","Bollard","Drewno","Malowane",null,null,"LED zintegrowane","AC","DIM.","7,4W","9,2W","1370lm","897lm",null,null,"65",null,"Class II",3000,null,0,0,0,"CE",null,null,"72 000h",1,"Oprawa słupkowa.","Światło obrotowo-symetryczne.",null,"A luminaire with a contemporary design. For lighting gardens, private areas and other architectural concepts.",null,null,null,"Odlew aluminiowy malowany proszkowo.","Drewno- sosna skandynawska malowana","Klosz- tworzywo sztuczne PMMA satynowane.","Uszczelka silikonowa.",null,"49cm",null,"Oprawa ściemnialna fazowo TRAILING EDGE (TE) - LEADING EDGE (LE)","Moduł LED","Cree DK210704 V2 JB2835 3V 3K","TCI MICRO MD 10W 350mA 127040 Triac",0,null,null,80,"C","205ZX0010, 206GA0010, 206GA0S10","Zaciski podłączeniowe: max 2x4mm², możliwość podłączenia oprawy w pętle max 2x4mm². Przewód w oponie okrągłej o średnicy ø8...12,5mm.","2346XX0009.png","2346XX0009.ldt",1,null,1,17]
["2347","2347XX0009","LILLESAND WOOD BOLLARD 49CM LED 1462LM 4000K DIM.","Lillesand,Wood","Bollard","Drewno","Malowane",null,null,"LED zintegrowane","AC","DIM.","7,4W","9,2W","1462lm","956lm",null,null,"65",null,"Class II",4000,null,0,0,0,"CE",null,null,"72 000h",1,"Oprawa słupkowa.","Światło obrotowo-symetryczne.",null,"A luminaire with a contemporary design. For lighting gardens, private areas and other architectural concepts.",null,null,null,"Odlew aluminiowy malowany proszkowo.","Drewno- sosna skandynawska malowana","Klosz- tworzywo sztuczne PMMA satynowane.","Uszczelka silikonowa.",null,"49cm",null,"Oprawa ściemnialna fazowo TRAILING EDGE (TE) - LEADING EDGE (LE)","Moduł LED","Cree DK210704 V2 JB2835 3V 4K","TCI MICRO MD 10W 350mA 127040 Triac",0,null,null,80,"C","205ZX0010, 206GA0010, 206GA0S10","Zaciski podłączeniowe: max 2x4mm², możliwość podłączenia oprawy w pętle max 2x4mm². Przewód w oponie okrągłej o średnicy ø8...12,5mm.","2347XX0009.png","2347XX0009.ldt",1,null,1,17]
["2350","2350XX0009","LILLESAND WOOD BOLLARD 49CM LED 1370LM 3000K DIM.","Lillesand,Wood","Bollard","Drewno","Impregnowane",null,null,"LED zintegrowane","AC","DIM.","7,4W","9,2W","1370lm","897lm",null,null,"65",null,"Class II",3000,null,0,0,0,"CE",null,null,"72 000h",1,"Oprawa słupkowa.","Światło obrotowo-symetryczne.",null,"A luminaire with a contemporary design. For lighting gardens, private areas and other architectural concepts.",null,null,null,"Odlew aluminiowy malowany proszkowo.","Drewno- sosna skandynawska impregnowana","Klosz- tworzywo sztuczne PMMA satynowane.","Uszczelka silikonowa.",null,"49cm",null,"Oprawa ściemnialna fazowo TRAILING EDGE (TE) - LEADING EDGE (LE)","Moduł LED","Cree DK210704 V2 JB2835 3V 3K","TCI MICRO MD 10W 350mA 127040 Triac",0,null,null,80,"C","205ZX0010, 206GA0010, 206GA0S10","Zaciski podłączeniowe: max 2x4mm², możliwość podłączenia oprawy w pętle max 2x4mm². Przewód w oponie okrągłej o średnicy ø8...12,5mm.","2350XX0009.png","2350XX0009.ldt",1,null,1,17]
["2351","2351XX0009","LILLESAND WOOD BOLLARD 49CM LED 1462LM 4000K DIM.","Lillesand,Wood","Bollard","Drewno","Impregnowane",null,null,"LED zintegrowane","AC","DIM.","7,4W","9,2W","1462lm","956lm",null,null,"65",null,"Class II",4000,null,0,0,0,"CE",null,null,"72 000h",1,"Oprawa słupkowa.","Światło obrotowo-symetryczne.",null,"A luminaire with a contemporary design. For lighting gardens, private areas and other architectural concepts.",null,null,null,"Odlew aluminiowy malowany proszkowo.","Drewno- sosna skandynawska impregnowana","Klosz- tworzywo sztuczne PMMA satynowane.","Uszczelka silikonowa.",null,"49cm",null,"Oprawa ściemnialna fazowo TRAILING EDGE (TE) - LEADING EDGE (LE)","Moduł LED","Cree DK210704 V2 JB2835 3V 4K","TCI MICRO MD 10W 350mA 127040 Triac",0,null,null,80,"C","205ZX0010, 206GA0010, 206GA0S10","Zaciski podłączeniowe: max 2x4mm², możliwość podłączenia oprawy w pętle max 2x4mm². Przewód w oponie okrągłej o średnicy ø8...12,5mm.","2351XX0009.png","2351XX0009.ldt",1,null,1,17]
["2360","2360XX0009","OPPLAND WOOD BOLLARD 85CM LED 1294LM 3000K DIM.","Oppland,Wood","Bollard","Drewno","Malowane",null,null,"LED zintegrowane","AC","DIM.","8,5W","10W","1294lm","301lm",null,null,"65","IK09","Class II",3000,"szerokie dół",0.12,0.12,0.85,"CE",null,null,"> 50 000h",1,"Oprawa słupkowa.","Światło rozproszone półsferyczne ukierunkowane w dół",null,"A bollard luminaire with a stable and durable structure. For lighting private areas and other architectural concepts",null,null,null,"Odlew aluminiowy malowany proszkowo.","Drewno- sosna skandynawska malowana, stal cynkowana ogniowo i malowana proszkowo.","Klosz- poliwęglan przeźroczysty ze strukturą, stabilizowany UV.","Uszczelka silikonowa.",null,"85cm","Drewno malowane","Oprawa ściemnialna fazowo TRAILING EDGE (TE)","Moduł LED","Philips Fortimo SLM C 1203 L09 1619 G7 3K","Philips Xitanium 10W 0,25A 40V TE SC 230V",0,"Philips Xitanium TE",null,80,"D","205ZX0010, 206GA0010, 206GA0S10","Zaciski podłączeniowe: max 2x4mm², możliwość podłączenia oprawy w pętle max 2x4mm². Przewód w oponie okrągłej o średnicy max ø12,5mm.","2360XX0009.png","2360XX0009.ldt",1,null,1,76]
["2361","2361XX0009","OPPLAND WOOD BOLLARD 85CM LED 1371LM 4000K DIM.","Oppland,Wood","Bollard","Drewno","Malowane",null,null,"LED zintegrowane","AC","DIM.","8,5W","10,1W","1371lm","312lm",null,null,"65","IK09","Class II",4000,"szerokie dół",0.12,0.12,0.85,"CE",null,null,"> 50 000h",1,"Oprawa słupkowa.","Światło rozproszone półsferyczne ukierunkowane w dół",null,"A bollard luminaire with a stable and durable structure. For lighting private areas and other architectural concepts",null,null,null,"Odlew aluminiowy malowany proszkowo.","Drewno- sosna skandynawska malowana, stal cynkowana ogniowo i malowana proszkowo.","Klosz- poliwęglan przeźroczysty ze strukturą, stabilizowany UV.","Uszczelka silikonowa.",null,"85cm","Drewno malowane","Oprawa ściemnialna fazowo TRAILING EDGE (TE)","Moduł LED","Philips Fortimo SLM C 1203 L09 1619 G7 4K","Philips Xitanium 10W 0,25A 40V TE SC 230V",0,"Philips Xitanium TE",null,80,"D","205ZX0010, 206GA0010, 206GA0S10","Zaciski podłączeniowe: max 2x4mm², możliwość podłączenia oprawy w pętle max 2x4mm². Przewód w oponie okrągłej o średnicy max ø12,5mm.","2361XX0009.png","2361XX0009.ldt",1,null,1,76]
["2364","2364XX0009","OPPLAND WOOD BOLLARD 85CM LED 1294LM 3000K DIM.","Oppland,Wood","Bollard","Drewno","Malowane",null,null,"LED zintegrowane","AC","DIM.","8,5W","10W","1294lm","301lm",null,null,"65","IK09","Class II",3000,"szerokie dół",0.12,0.12,0.85,"CE",null,null,"> 50 000h",1,"Oprawa słupkowa.","Światło rozproszone półsferyczne ukierunkowane w dół",null,"A bollard luminaire with a stable and durable structure. For lighting private areas and other architectural concepts",null,null,"Oprawa wyposażona w wymienne źródło światła typu moduł LED, który zapewnia trwałość i optymalny rozsył światła, przy zachowaniu stosunkowo niskiego zużycia energii.","Odlew aluminiowy malowany proszkowo.","Drewno- sosna skandynawska malowana, stal cynkowana ogniowo i malowana proszkowo.","Klosz- poliwęglan przeźroczysty ze strukturą, stabilizowany UV.","Uszczelka silikonowa.",null,"85cm","Drewno impregnowane","Oprawa ściemnialna fazowo TRAILING EDGE (TE)","Moduł LED","Philips Fortimo SLM C 1203 L09 1619 G7 3K","Philips Xitanium 10W 0,25A 40V TE SC 230V",0,"Philips Xitanium TE",null,80,"D","205ZX0010, 206GA0010, 206GA0S10","Zaciski podłączeniowe: max 2x4mm², możliwość podłączenia oprawy w pętle max 2x4mm². Przewód w oponie okrągłej o średnicy max ø12,5mm.","2364XX0009.png","2364XX0009.ldt",1,null,1,76]
["2365","2365XX0009","OPPLAND WOOD BOLLARD 85CM LED 1371LM 4000K DIM.","Oppland,Wood","Bollard","Drewno","Malowane",null,null,"LED zintegrowane","AC","DIM.","8,5W","10,1W","1371lm","312lm",null,null,"65","IK09","Class II",4000,"szerokie dół",0.12,0.12,0.85,"CE",null,null,"> 50 000h",1,"Oprawa słupkowa.","Światło rozproszone półsferyczne ukierunkowane w dół",null,"A bollard luminaire with a stable and durable structure. For lighting private areas and other architectural concepts",null,null,"Oprawa wyposażona w wymienne źródło światła typu moduł LED, który zapewnia trwałość i optymalny rozsył światła, przy zachowaniu stosunkowo niskiego zużycia energii.","Odlew aluminiowy malowany proszkowo.","Drewno- sosna skandynawska malowana, stal cynkowana ogniowo i malowana proszkowo.","Klosz- poliwęglan przeźroczysty ze strukturą, stabilizowany UV.","Uszczelka silikonowa.",null,"85cm","Drewno impregnowane","Oprawa ściemnialna fazowo TRAILING EDGE (TE)","Moduł LED","Philips Fortimo SLM C 1203 L09 1619 G7 4K","Philips Xitanium 10W 0,25A 40V TE SC 230V",0,"Philips Xitanium TE",null,80,"D","205ZX0010, 206GA0010, 206GA0S10","Zaciski podłączeniowe: max 2x4mm², możliwość podłączenia oprawy w pętle max 2x4mm². Przewód w oponie okrągłej o średnicy max ø12,5mm.","2365XX0009.png","2365XX0009.ldt",1,null,1,76]
["2400","2400XX0010","HELLVIK BOLLARD 55CM LED 978LM 3000K DIM.","Hellvik","Bollard","Aluminium",null,null,null,"LED zintegrowane","AC","DIM.","5,2W","6,9W","978lm","531lm",null,null,"65",null,"Class II",3000,"szerokie dół",0.42,0.11,0.55000000000000004,"CE",null,null,"> 72 000h",1,"Oprawa słupkowa.","Światło rozproszone przysłonięte od góry.",null,"A luminaire with a contemporary design. For lighting gardens, private areas and other architectural concepts.",null,null,null,"Odlew aluminiowy malowany proszkowo.",null,"Klosz- poliwęglan przeźroczysty ze strukturą, stabilizowany UV.","Uszczelka silikonowa.",null,"55cm",null,"Oprawa ściemnialna fazowo TRAILING EDGE (TE) - LEADING EDGE (LE)","Moduł LED","Cree DK200305 V3 JB2835 3V 3K","TCI Micro MD 7W 250mA code 127048 Triac",0,null,null,80,"C","209GA0S09","Zaciski podłączeniowe: max 2x4mm², możliwość podłączenia oprawy w pętle max 2x4mm². Przewód w oponie okrągłej o średnicy max ø12,5mm.","2400XX0010.png","2400XX0010.ldt",1,null,1,25]
["2401","2401XX0010","HELLVIK BOLLARD 55CM LED 978LM 4000K DIM.","Hellvik","Bollard","Aluminium",null,null,null,"LED zintegrowane","AC","DIM.","5,2W","6,9W","978lm","575lm",null,null,"65","IK08","Class II",4000,"szerokie dół",0.42,0.11,0.55000000000000004,"CE",null,null,"> 72 000h",1,"Oprawa słupkowa.","Światło rozproszone przysłonięte od góry.",null,"A luminaire with a contemporary design. For lighting gardens, private areas and other architectural concepts.",null,null,null,"Odlew aluminiowy malowany proszkowo.",null,"Klosz- poliwęglan przeźroczysty ze strukturą, stabilizowany UV.","Uszczelka silikonowa.",null,"55cm",null,"Oprawa ściemnialna fazowo TRAILING EDGE (TE) - LEADING EDGE (LE)","Moduł LED","Cree DK200305 V3 JB2835 3V 4K","TCI Micro MD 7W 250mA code 127048 Triac",0,null,null,80,"C","209GA0S09","Zaciski podłączeniowe: max 2x4mm², możliwość podłączenia oprawy w pętle max 2x4mm². Przewód w oponie okrągłej o średnicy max ø12,5mm.","2401XX0010.png","2401XX0010.ldt",1,null,1,25]
["2402","2402XX0009","HELLVIK BOLLARD 55CM LED 1344LM 3000K DALI","Hellvik","Bollard","Aluminium",null,null,null,"LED zintegrowane","AC","DALI","7,5W","10,1 W","1344lm","670lm",null,null,"65",null,"Class I",3000,"szerokie dół",0.42,0.11,0.55000000000000004,"CE",null,"DALI","> 72 000h",1,"Oprawa słupkowa.","Światło rozproszone przysłonięte od góry.",null,"A luminaire with a contemporary design. For lighting gardens, private areas and other architectural concepts",null,null,null,"Odlew aluminiowy malowany proszkowo.",null,"Klosz- poliwęglan przeźroczysty ze strukturą, stabilizowany UV.","Uszczelka silikonowa.",null,"55cm",null,"Sterowanie światłem w systemie: DALI2","Moduł LED","Cree DK200305 V3 JB2835 3V 3K","TCI Mini JOLLY 20W code 151403 DALI",0,null,null,80,"C","209GA0S09, 2409GA0009","Zaciski podłączeniowe: max 4x 4 mm², możliwość podłączenia oprawy w pętle max 4x2,5 mm². Przewód w oponie okrągłej o średnicy max ø12,5mm.","2402XX0009.png","2402XX0009.ldt",3,null,1,25]
["2403","2403XX0009","HELLVIK BOLLARD 55CM LED 1426LM 4000K DALI","Hellvik","Bollard","Aluminium",null,null,null,"LED zintegrowane","AC","DALI","7,5W","10,1 W","1426lm","808lm",null,null,"65","IK08","Class I",4000,"szerokie dół",0.42,0.11,0.55000000000000004,"CE",null,"DALI","> 72 000h",1,"Oprawa słupkowa.","Światło rozproszone przysłonięte od góry.",null,"A luminaire with a contemporary design. For lighting gardens, private areas and other architectural concepts",null,null,null,"Odlew aluminiowy malowany proszkowo.",null,"Klosz- poliwęglan przeźroczysty ze strukturą, stabilizowany UV.","Uszczelka silikonowa.",null,"55cm",null,"Sterowanie światłem w systemie: DALI2","Moduł LED","Cree DK200305 V3 JB2835 3V 4K","TCI Mini JOLLY 20W code 151403 DALI",0,null,null,80,"C","209GA0S09, 2409GA0009","Zaciski podłączeniowe: max 4x 4 mm², możliwość podłączenia oprawy w pętle max 2x2,5 mm². Przewód w oponie okrągłej o średnicy max ø12,5mm.","2403XX0009.png","2403XX0009.ldt",3,null,1,25]
["2404","2404XX0009","HELLVIK BOLLARD 55CM LED 1159LM 3000K DIM.","Hellvik","Bollard","Aluminium",null,null,null,"LED zintegrowane","AC","DIM.","6,5W","8W","1159lm","1038lm",null,null,"65","IK08","Class II",3000,"szerokie dół",0.42,0.11,0.55000000000000004,"CE",null,null,"> 100 000h",1,"Oprawa słupkowa.","Światło rozproszone przysłonięte od góry.",null,"A luminaire with a contemporary design. For lighting gardens, private areas and other architectural concepts.",null,null,null,"Odlew aluminiowy malowany proszkowo.",null,"Soczewka hermetyczna zewnętrzna- tworzywo sztuczne PMMA przeźroczyste.","Uszczelka silikonowa.",null,"55cm",null,"Oprawa ściemnialna fazowo TRAILING EDGE (TE)","Moduł LED","Philips Fortimo FastFlex LED 2x6 DP G5 3K","Philips Xitanium 8W 0,2A 40V TE SC 230V",0,"Philips Xitanium TE",null,70,"D","209GA0S09, 2409GA0009","Zaciski podłączeniowe: max 2x4mm², możliwość podłączenia oprawy w pętle max 2x4mm². Przewód w oponie okrągłej o średnicy max ø12,5mm.","2404XX0009.png","2404XX0009.ldt",1,null,1,25]
["2405","2405XX0009","HELLVIK BOLLARD 55CM LED 1254LM 4000K DIM.","Hellvik","Bollard","Aluminium",null,null,null,"LED zintegrowane","AC","DIM.","6,5W","8,1W","1254lm","1007lm",null,null,"65","IK08","Class II",4000,"szerokie dół",0.42,0.11,0.55000000000000004,"CE",null,null,"> 100 000h",1,"Oprawa słupkowa.","Światło rozproszone przysłonięte od góry.",null,"A luminaire with a contemporary design. For lighting gardens, private areas and other architectural concepts.",null,null,null,"Odlew aluminiowy malowany proszkowo.",null,"Soczewka hermetyczna zewnętrzna- tworzywo sztuczne PMMA przeźroczyste.","Uszczelka silikonowa.",null,"55cm",null,"Oprawa ściemnialna fazowo TRAILING EDGE (TE)","Moduł LED","Philips Fortimo FastFlex LED 2x6 DP G5 4K","Philips Xitanium 8W 0,2A 40V TE SC 230V",0,"Philips Xitanium TE",null,70,"D","209GA0S09, 2409GA0009","Zaciski podłączeniowe: max 2x4mm², możliwość podłączenia oprawy w pętle max 2x4mm². Przewód w oponie okrągłej o średnicy max ø12,5mm.","2405XX0009.png","2405XX0009.ldt",1,null,1,25]
["2406","2406XX0009","HELLVIK BOLLARD 55CM LED 1691LM 3000K DALI2","Hellvik","Bollard","Aluminium",null,null,null,"LED zintegrowane","AC","DALI2","9,9W","11,9W","1691lm","1537lm",null,null,"65","IK08","Class I",3000,"szerokie dół",0.42,0.11,0.55000000000000004,"CE",null,"DALI","> 100 000h",1,"Oprawa słupkowa.","Światło rozproszone przysłonięte od góry.",null,"A luminaire with a contemporary design. For lighting gardens, private areas and other architectural concepts.","A luminaire with a contemporary design. For lighting gardens, private areas and other architectural concepts. Suitable for emergency installations with direct voltage: DC 176 ÷ 276V",null,null,"Odlew aluminiowy malowany proszkowo.",null,"Klosz- poliwęglan przeźroczysty ze strukturą, stabilizowany UV.","Uszczelka silikonowa.",null,"55cm",null,"Sterowanie światłem w systemie: DALI2","Moduł LED","Philips Fortimo FastFlex LED 2x6 DP G5 3K","Osram OTi DALI 20/220…240/500 NFC S",0,null,null,70,"D","209GA0S09, 2409GA0009","Zaciski podłączeniowe: max 5x2,5mm², możliwość podłączenia oprawy w pętle max 5x2,5mm². Przewód w oponie okrągłej o średnicy max ø12,5mm.","2406XX0009.png","2406XX0009.ldt",3,null,1,25]
["2407","2407XX0009","HELLVIK BOLLARD 55CM LED 1831LM 4000K DALI2","Hellvik","Bollard","Aluminium",null,null,null,"LED zintegrowane","AC","DALI2","9,9W","11,9","1831lm","1549lm",null,null,"65","IK08","Class I",4000,"szerokie dół",0.42,0.11,0.55000000000000004,"CE",null,"DALI","> 100 000h",1,"Oprawa słupkowa.","Światło rozproszone przysłonięte od góry.",null,"A luminaire with a contemporary design. For lighting gardens, private areas and other architectural concepts.","A uminaire with a contemporary design. For lighting gardens, private areas and other architectural concepts. Suitable for emergency installations with direct voltage: DC 176 ÷ 276V",null,null,"Odlew aluminiowy malowany proszkowo.",null,"Klosz- poliwęglan przeźroczysty ze strukturą, stabilizowany UV.","Uszczelka silikonowa.",null,"55cm",null,"Sterowanie światłem w systemie: DALI2","Moduł LED","Philips Fortimo FastFlex LED 2x6 DP G5 4K","Osram OTi DALI 20/220…240/500 NFC S",0,null,null,70,"D","209GA0S09, 2409GA0009","Zaciski podłączeniowe: max 5x2,5mm², możliwość podłączenia oprawy w pętle max 5x2,5mm². Przewód w oponie okrągłej o średnicy max ø12,5mm.","2407XX0009.png","2407XX0009.ldt",3,null,1,25]
["240A","240XX0111","OSLO CEILING-CHAIN E27","Oslo","Ceiling","Stal",null,null,null,"Wymienne","E27",null,"LED max 9W","LED max 9W",null,null,null,null,"55","IK07","Class II",null,null,0.28000000000000003,0.28000000000000003,0.86,"CE",null,null,null,16,"Oprawa wisząca.","Światło odkryte.",null,"Scandinavian design luminaire with chain suspension. For lighting gardens, terraces and other architectural concepts.",null,null,"Oprawa na wymienne źródło światła typu: lampa LED, świetlówka TC-SE, tradycyjna żarówka (halogenowa) o trzonku E27. Źródło światła należy dokupić oddzielnie.","Stal cynkowana ogniowo.","Stal malowana proszkowo.","Klosz- poliwęglan przeźroczysty, stabilizowany UV.",null,null,null,null,null,"Lampa E27","LED A55..60",null,0,null,null,80,null,null,"Zaciski podłączeniowe: max 2x2,5mm². Przewód w oponie okrągłej o średnicy ø7...10,5mm.","240XX0111.jpg","240XX0111.ldt",4,"E27",1,9]
["2410","2410XX0010","HELLVIK BOLLARD 85CM LED 1956LM 3000K DIM. TRIAC","Hellvik","Bollard","Aluminium",null,null,null,"LED zintegrowane","AC","DIM. TRIAC","10,5W","11,8W","1956lm","1014lm",null,null,"65","IK08","Class II",3000,"szerokie dół",0.42,0.11,0.85,"CE",null,null,"> 72 000h",1,"Oprawa słupkowa.","Światło rozproszone przysłonięte od góry.",null,"A luminaire with a contemporary design. For lighting gardens, private areas and other architectural concepts.",null,null,null,"Odlew aluminiowy malowany proszkowo.",null,"Klosz- poliwęglan przeźroczysty ze strukturą, stabilizowany UV.","Uszczelka silikonowa.",null,"85cm",null,"Oprawa ściemnialna fazowo TRAILING EDGE (TE) - LEADING EDGE (LE)","Moduł LED","Cree DK200305 V3 JB2835 3V 3K","TCI Mini MD 12,5W 250mA code 127036 Triac",0,null,null,80,"C","209GA0S09","Zaciski podłączeniowe: max 2x4mm², możliwość podłączenia oprawy w pętle max 2x2,5mm². Przewód w oponie okrągłej o średnicy max ø12,5mm.","2410XX0010.jpg","2410XX0010.ldt",1,null,1,25]
["2411","2411XX0010","HELLVIK BOLLARD 85CM LED 1956LM 4000K DIM. TRIAC","Hellvik","Bollard","Aluminium",null,null,null,"LED zintegrowane","AC","DIM. TRIAC","10,5W","11,8W","1956lm","1072lm",null,null,"65","IK08","Class II",4000,"szerokie dół",0.42,0.11,0.85,"CE",null,null,"> 72 000h",1,"Oprawa słupkowa.","Światło rozproszone przysłonięte od góry.",null,"A luminaire with a contemporary design. For lighting gardens, private areas and other architectural concepts.",null,null,null,"Odlew aluminiowy malowany proszkowo.",null,"Klosz- poliwęglan przeźroczysty ze strukturą, stabilizowany UV.","Uszczelka silikonowa.",null,"85cm",null,"Oprawa ściemnialna fazowo TRAILING EDGE (TE) - LEADING EDGE (LE)","Moduł LED","Cree DK200305 V3 JB2835 3V 4K","TCI Mini MD 12,5W 250mA code 127036 Triac",0,null,null,80,"C","209GA0S09","Zaciski podłączeniowe: max 2x4mm², możliwość podłączenia oprawy w pętle max 2x2,5mm². Przewód w oponie okrągłej o średnicy max ø12,5mm.","2411XX0010.jpg","2411XX0010.ldt",1,null,1,25]
["2412","2412XX0009","HELLVIK BOLLARD 85CM 2XLED 3075LM 3000K DALI","Hellvik","Bollard","Aluminium",null,null,null,"LED zintegrowane","AC","DALI","17,4W","20,2W","3075lm","1747lm",null,null,"65","IK08","Class I",3000,"szerokie dół",0.42,0.11,0.85,"CE",null,"DALI","> 72 000h",1,"Oprawa słupkowa.","Światło rozproszone przysłonięte od góry.",null,"A luminaire with a contemporary design. For lighting gardens, private areas and other architectural concepts",null,null,null,"Odlew aluminiowy malowany proszkowo.",null,"Klosz- poliwęglan przeźroczysty ze strukturą, stabilizowany UV.","Uszczelka silikonowa.",null,"85cm",null,"Sterowanie światłem w systemie: DALI2","2 Moduły LED","Cree DK200305 V3 JB2835 3V 3K","TCI Mini JOLLY 20W code 151403 DALI",0,null,null,80,"C","209GA0S09, 2409GA0009","Zaciski podłączeniowe: max 2x4mm², możliwość podłączenia oprawy w pętle max 2x2,5mm². Przewód w oponie okrągłej o średnicy max ø12,5mm.","2412XX0009.jpg","2412XX0009.ldt",3,null,1,25]
["2413","2413XX0009","HELLVIK BOLLARD 85CM 2XLED 3075LM 4000K DALI","Hellvik","Bollard","Aluminium",null,null,null,"LED zintegrowane","AC","DALI","17,4W","20,2W","3075lm","1803lm",null,null,"65","IK08","Class I",4000,"szerokie dół",0.42,0.11,0.85,"CE",null,"DALI","> 72 000h",1,"Oprawa słupkowa.","Światło rozproszone przysłonięte od góry.",null,"A luminaire with a contemporary design. For lighting gardens, private areas and other architectural concepts",null,null,null,"Odlew aluminiowy malowany proszkowo.",null,"Klosz- poliwęglan przeźroczysty ze strukturą, stabilizowany UV.","Uszczelka silikonowa.",null,"85cm",null,"Sterowanie światłem w systemie: DALI2","2 Moduły LED","Cree DK200305 V3 JB2835 3V 4K","TCI Mini JOLLY 20W code 151403 DALI",0,null,null,80,"C","209GA0S09, 2409GA0009","Zaciski podłączeniowe: max 2x4mm², możliwość podłączenia oprawy w pętle max 2x2,5mm². Przewód w oponie okrągłej o średnicy max ø12,5mm.","2413XX0009.jpg","2413XX0009.ldt",3,null,1,25]
["2414","2414XX0009","HELLVIK BOLLARD 85CM LED 1159LM 3000K DIM.","Hellvik","Bollard","Aluminium",null,null,null,"LED zintegrowane","AC","DIM.","6,5W","8W","1159lm","1038lm",null,null,"65","IK08","Class II",3000,"szerokie dół",0.42,0.11,0.85,"CE",null,null,"> 100 000h",1,"Oprawa słupkowa.","Światło rozproszone przysłonięte od góry.",null,"A luminaire with a contemporary design. For lighting gardens, private areas and other architectural concepts.",null,null,null,"Odlew aluminiowy malowany proszkowo.",null,"Soczewka hermetyczna zewnętrzna- tworzywo sztuczne PMMA przeźroczyste.","Uszczelka silikonowa.",null,"85cm",null,"Oprawa ściemnialna fazowo TRAILING EDGE (TE)","Moduł LED","Philips Fortimo FastFlex LED 2x6 DP G5 3K","Philips Xitanium 8W 0,2A 40V TE SC 230V",0,"Philips Xitanium TE",null,70,"D","209GA0S09, 2409GA0009","Zaciski podłączeniowe: max 2x4mm², możliwość podłączenia oprawy w pętle max 2x2,5mm². Przewód w oponie okrągłej o średnicy max ø12,5mm.","2414XX0009.jpg","2414XX0009.ldt",1,null,1,25]
["2415","2415XX0009","HELLVIK BOLLARD 85CM LED 1254LM 4000K DIM.","Hellvik","Bollard","Aluminium",null,null,null,"LED zintegrowane","AC","DIM.","6,5W","8,1W","1254lm","1007lm",null,null,"65","IK08","Class II",4000,"szerokie dół",0.42,0.11,0.85,"CE",null,null,"> 100 000h",1,"Oprawa słupkowa.","Światło rozproszone przysłonięte od góry.",null,"A luminaire with a contemporary design. For lighting gardens, private areas and other architectural concepts.",null,null,null,"Odlew aluminiowy malowany proszkowo.",null,"Soczewka hermetyczna zewnętrzna- tworzywo sztuczne PMMA przeźroczyste.","Uszczelka silikonowa.",null,"85cm",null,"Oprawa ściemnialna fazowo TRAILING EDGE (TE)","Moduł LED","Philips Fortimo FastFlex LED 2x6 DP G5 4K","Philips Xitanium 8W 0,2A 40V TE SC 230V",0,"Philips Xitanium TE",null,70,"D","209GA0S09, 2409GA0009","Zaciski podłączeniowe: max 2x4mm², możliwość podłączenia oprawy w pętle max 2x4mm². Przewód w oponie okrągłej o średnicy max ø12,5mm.","2415XX0009.jpg","2415XX0009.ldt",1,null,1,25]
["2416","2416XX0009","HELLVIK BOLLARD 85CM LED 1691LM 3000K DALI2","Hellvik","Bollard","Aluminium",null,null,null,"LED zintegrowane","AC","DALI2","9,9W","11,9","1691lm","1537lm",null,null,"65",null,"Class I",3000,"szerokie dół",0.42,0.11,0.85,"CE",null,"DALI",">100 000h",1,"Oprawa słupkowa.","Światło rozproszone przysłonięte od góry.",null,"A luminaire with a contemporary design. For lighting gardens, private areas and other architectural concepts.","A luminaire with a contemporary design. For lighting gardens, private areas and other architectural concepts. Suitable for emergency installations with direct voltage: DC 176 ÷ 276V",null,null,"Odlew aluminiowy malowany proszkowo.",null,"Klosz- poliwęglan przeźroczysty ze strukturą, stabilizowany UV.","Uszczelka silikonowa.",null,"85cm",null,"Sterowanie światłem w systemie: DALI2","Moduł LED","Philips Fortimo FastFlex LED 2x6 DP G5 3K","Osram OTi DALI 20/220…240/500 NFC S",0,null,null,70,"D","209GA0S09, 2409GA0009","Zaciski podłączeniowe: max 5x2,5mm², możliwość podłączenia oprawy w pętle max 5x2,5mm². Przewód w oponie okrągłej o średnicy max ø12,5mm.","2416XX0009.jpg","2416XX0009.ldt",3,null,1,25]
["2417","2417XX0009","HELLVIK BOLLARD 85CM LED 1831LM 4000K DALI2","Hellvik","Bollard","Aluminium",null,null,null,"LED zintegrowane","AC","DALI2","9,9W","11,9W","1831lm","1466lm",null,null,"65",null,"Class I",4000,"szerokie dół",0.42,0.11,0.85,"CE",null,"DALI","> 100 000h",1,"Oprawa słupkowa.","Światło rozproszone przysłonięte od góry.",null,"A luminaire with a contemporary design. For lighting gardens, private areas and other architectural concepts.","A luminaire with a contemporary design. For lighting gardens, private areas and other architectural concepts. Suitable for emergency installations with direct voltage: DC 176 ÷ 276V",null,null,"Odlew aluminiowy malowany proszkowo.",null,"Klosz- poliwęglan przeźroczysty ze strukturą, stabilizowany UV.","Uszczelka silikonowa.",null,"85cm",null,"Sterowanie światłem w systemie: DALI2","Moduł LED","Philips Fortimo FastFlex LED 2x6 DP G5 4K","Osram OTi DALI 20/220…240/500 NFC S",0,null,null,70,"D","209GA0S09, 2409GA0009","Zaciski podłączeniowe: max 5x2,5mm², możliwość podłączenia oprawy w pętle max 5x2,5mm². Przewód w oponie okrągłej o średnicy max ø12,5mm.","2417XX0009.jpg","2417XX0009.ldt",3,null,1,25]
["242","242XX0309","OSLO POLE-TOP E27","Oslo","Post,Post complete","Stal",null,null,null,"Wymienne","E27",null,"LED max 2 x 9W","LED max 2 x 9W",null,null,null,null,"55",null,"Class II",null,null,0.78,0.28000000000000003,2.38,"CE",null,null,null,2,"Oprawa słupowa (nasadzana).","Światło jednostronne: symetryczne, ukierunkowane w dół.",null,"Classic design luminaire, mounted on a telescopic lighting pole. Adjustable height 1700..2300mm. For lighting gardens, terraces and other architectural concepts.",null,null,"Oprawa na wymienne źródło światła typu: lampa LED, świetlówka TC-SE, tradycyjna żarówka (halogenowa) o trzonku E27. Źródło światła należy dokupić oddzielnie.","Stal cynkowana ogniowo.","Stal malowana proszkowo.","Klosz- poliwęglan przeźroczysty, stabilizowany UV.",null,null,null,null,null,"Lampa E27","LED A55..60",null,0,null,null,80,null,"111GA0012, 405ZX0009, 406ZX0009",null,"242XX0309.jpg","242XX0309.ldt",4,"E27",1,27]
["245","245XX0011","OSLO BOLLARD E27","Oslo","Bollard,Flower","Stal",null,null,null,"Wymienne","E27",null,"LED max 9W","LED max 9W",null,null,null,null,"55",null,"Class II",null,null,0.28000000000000003,0.48,1.18,"CE",null,null,null,1,"Oprawa słupkowa.","Światło odkryte.",null,"Scandinavian design luminaire. For lighting private areas and public spaces.",null,null,null,"Stal cynkowana ogniowo.","Stal malowana proszkowo.","Klosz- poliwęglan przeźroczysty, stabilizowany UV.",null,null,null,null,null,"Lampa E27","LDE A55..60",null,0,null,null,80,null,null,"Zaciski podłączeniowe: max 2x2,5mm², możliwość podłączenia oprawy w pętle max 2x1,5mm². Przewód w oponie okrągłej o średnicy max 12mm.","245XX0011.jpg","245XX0011.ldt",4,"E27",1,9]
["280","280XX0010","STOCKHOLM WALL E27","Stockholm","Wall","Stal",null,null,null,"Wymienne","E27",null,"LED max 9W","LED max 9W",null,null,null,null,"54",null,"Class II",null,null,0.28999999999999998,0.28999999999999998,0.31,"CE",null,null,null,12,"Oprawa ścienna.","Światło odkryte.",null,"Classic type, wall-mounted luminaire in scandinavian design for general use. Possibility to install on corners of architectural objects.",null,null,"Oprawa na wymienne źródło światła typu: lampa LED, świetlówka TC-SE, tradycyjna żarówka (halogenowa) o trzonku E27. Źródło światła należy dokupić oddzielnie.","Stal cynkowana ogniowo i malowana proszkowo.",null,"Klosz- tworzywo sztuczne PMMA przeźroczyste.","Uszczelka silikonowa.","Dławnica EPDM.",null,null,null,"Lampa E27","LED A55..60",null,0,null,null,80,null,"153XX0009, 159XX0009, 46999021","Zaciski podłączeniowe: max 2x2,5mm², możliwość podłączenia oprawy w pętle max 2x1,5mm². Przewód w oponie okrągłej o średnicy ø7...10,5mm.","280XX0010.jpg","280XX0010.ldt",4,"E27",1,9]
["281","281XX0309","STOCKHOLM POLE LUMINAIRE. E27","Stockholm","Post,Post complete","Stal",null,null,null,"Wymienne","E27",null,"LED max 9W","LED max 9W",null,null,null,null,"54",null,"Class II",null,null,0.35,0.35,2.48,"CE",null,null,null,23,"Oprawa słupowa.","Światło odkryte.",null,"Pole top luminaire in scandinavian design. For installation on a lighting pole with adjustable height 1510...2480mm. For lighting gardens, parks, and any other architectural concepts.",null,null,null,"Stal cynkowana ogniowo.","Stal malowana proszkowo.","Klosz- tworzywo sztuczne PMMA przeźroczyste.",null,null,"Pojedynczy",null,null,"Lampa E27","LED A55..60",null,0,null,null,80,null,"111GA0012, 405ZX0009, 406ZX0009","Zaciski podłączeniowe: max 4x2,5mm², możliwość podłączenia oprawy w pętle max 4x2,5mm². Przewód w oponie okrągłej o średnicy ø6...12,5mm.","281XX0309.jpg","281XX0309.ldt",4,"E27",1,9]
["283","283XX0309","STOCKHOLM POLE-TOP E27","Stockholm","Post,Post complete","Stal",null,null,null,"Wymienne","E27",null,"LED max 2x 9W","LED max 2x 9W",null,null,null,null,"54",null,"Class II",null,null,0.35,0.92,2.52,"CE",null,null,null,2,"Oprawa słupowa (nasadzana).","Światło odkryte.",null,"Pole top luminaire in scandinavian design. For installation on a lighting pole with adjustable height 1740...2520mm. For lighting gardens, parks, and any other architectural concepts.",null,null,null,"Stal cynkowana ogniowo.","Stal malowana proszkowo.","Klosz- tworzywo sztuczne PMMA przeźroczyste.",null,null,"Podwójny",null,null,"Lampa E27","LED A55..60",null,0,null,null,80,null,"111GA0012, 405ZX0009, 406ZX0009","Zaciski podłączeniowe: max 4x2,5mm². Przewód w oponie okrągłej o średnicy max ø12 mm.","283XX0309.jpg","283XX0309.ldt",4,"E27",1,9]
["284","284XX0010","STOCKHOLM BOLLARD 345CM E27","Stockholm","Bollard,Pedestal","Stal",null,null,null,"Wymienne","E27",null,"LED max 9W","LED max 9W",null,null,null,null,"54",null,"Class II",null,null,0.27,0.27,0.34,"CE",null,null,null,13,"Oprawa słupkowa.","Światło odkryte.",null,"Scandinavian design luminaire. For lighting gardens, terraces and any others architectural concepts.",null,null,"Oprawa na wymienne źródło światła typu: lampa LED, tradycyjna żarówka (halogenowa) o trzonku E27. Źródło światła należy dokupić oddzielnie.","Stal cynkowana ogniowo i malowana proszkowo.",null,"Klosz- tworzywo sztuczne PMMA przeźroczyste.",null,"Dławnica EPDM.","34,5cm",null,null,"Lampa E27","LED A55..60",null,0,null,null,80,null,null,"Zaciski podłączeniowe: max 2x2,5mm². Przewód w oponie okrągłej o średnicy max ø12 mm.","284XX0010.jpg","284XX0010.ldt",4,"E27",1,9]
["285","285XX0010","STOCKHOLM BOLLARD 118CM E27","Stockholm","Bollard,Flower","Stal",null,null,null,"Wymienne","E27",null,"LED max 9W","LED max 9W",null,null,null,null,"54",null,"Class II",null,null,0.27,0.27,1.18,"CE",null,null,null,1,"Oprawa słupkowa.","Światło odkryte.",null,"Scandinavian design luminaire for general use. For lighting gardens, terraces and any other architectural concepts.",null,null,"Oprawa na wymienne źródło światła typu: lampa LED, świetlówka TC-SE, tradycyjna żarówka (halogenowa) o trzonku E27. Źródło światła należy dokupić oddzielnie.","Stal cynkowana ogniowo i malowana proszkowo.",null,"Klosz- tworzywo sztuczne PMMA przeźroczyste.",null,null,"118cm",null,null,"Lampa E27","LED A55..60",null,0,null,null,80,null,null,"Zaciski podłączeniowe: max 2x2,5mm². Przewód w oponie okrągłej o średnicy max 12mm.","285XX0010.jpg","285XX0010.ldt",4,"E27",1,9]
["286","286XX0010","STOCKHOLM WALL E27","Stockholm,Big","Wall","Stal",null,null,null,"Wymienne","E27",null,"LED max 9W","LED max 9W",null,null,null,null,"54",null,"Class II",null,null,0.39,0.39,0.38,"CE",null,null,null,12,"Oprawa ścienna.","Światło odkryte.",null,"Scandinavian design, wall-mounted luminaire for general use. Possibility to install on corners of architectural objects.",null,null,"Oprawa na wymienne źródło światła typu: lampa LED, świetlówka TC-SE, tradycyjna żarówka (halogenowa) o trzonku E27. Źródło światła należy dokupić oddzielnie.","Stal cynkowana ogniowo.","Stal malowana proszkowo.","Klosz- tworzywo sztuczne PMMA przeźroczyste.","Uszczelka silikonowa.","Dławnica EPDM.",null,null,null,"Lampa E27","LED A55..60",null,0,null,null,80,null,"153XX0009, 159XX0009, 46999021","Zaciski podłączeniowe: max 2x2,5mm². Przewód w oponie okrągłej o średnicy ø7...10,5mm.","286XX0010.jpg","286XX0010.ldt",4,"E27",1,9]
["287","287XX0010","STOCKHOLM BOLLARD E27","Stockholm,Big","Bollard,Pedestal","Stal",null,null,null,"Wymienne","E27",null,"LED max 9W","LED max 9W",null,null,null,null,"54",null,"Class II",null,null,0.35,0.35,0.48,"CE",null,null,null,1,"Oprawa słupkowa.","Światło odkryte.",null,"Scandinavian design luminaire. For lighting gardens, terraces and any other architectural concepts.",null,null,"Oprawa na wymienne źródło światła typu: lampa LED, tradycyjna żarówka (halogenowa) o trzonku E27. Źródło światła należy dokupić oddzielnie.","Stal cynkowana ogniowo.",null,"Klosz- tworzywo sztuczne PMMA przeźroczyste.",null,null,null,null,null,"Lampa E27","LED A55..60",null,0,null,null,80,null,null,"Zaciski podłączeniowe: max 2x2,5mm². Przewód w oponie okrągłej o średnicy max ø12mm.","287XX0010.jpg","287XX0010.ldt",4,"E27",1,9]
["288","288XX0011","STOCKHOLM BOLLARD 85CM E27","Stockholm","Bollard","Stal",null,null,null,"Wymienne","E27",null,"LED max 9W","LED max 9W",null,null,null,null,"65",null,"Class II",null,null,0.17,0.17,0.85,"CE",null,null,null,1,"Oprawa słupkowa.","Światło odkryte, rozproszone z obrotowo- symetrycznym rozsyłem światła.",null,"Bollard luminaire of stable and durable construction. For lighting private areas and public spaces.",null,null,"Oprawa na wymienne źródło światła typu: lampa LED, świetlówka TC-SE, tradycyjna żarówka (halogenowa) o trzonku E27. Źródło światła należy dokupić oddzielnie.","Stal cynkowana ogniowo.",null,"Klosz- tworzywo sztuczne PMMA w kolorze mlecznym.","Uszczelka silikonowa.",null,"85cm","mleczny",null,"Lampa E27","LED A55..60",null,0,null,null,80,null,"205ZX0010, 206GA0010, 206GA0S10","Zaciski podłączeniowe: max 3x2,5mm², możliwość podłączenia oprawy w pętle max 3x2,5mm². Przewód w oponie okrągłej o średnicy max ø12,5mm.","288XX0011.jpg","288XX0011.ldt",4,"E27",1,24]
["289","289XX0011","STOCKHOLM BOLLARD 49CM E27","Stockholm","Bollard","Stal",null,null,null,"Wymienne","E27",null,"LED max 9W","LED max 9W",null,null,null,null,"65",null,"Class II",null,null,0.17,0.17,0.49,"CE",null,null,null,1,"Oprawa słupkowa.","Światło odkryte, rozproszone z obrotowo- symetrycznym rozsyłem światła.",null,"Bollard luminaire of stable and durable construction. For lighting private areas and public spaces.",null,null,"Oprawa na wymienne źródło światła typu: lampa LED, świetlówka TC-SE, tradycyjna żarówka (halogenowa) o trzonku E27. Źródło światła należy dokupić oddzielnie.","Stal cynkowana ogniowo.",null,"Klosz- tworzywo sztuczne PMMA w kolorze mlecznym.","Uszczelka silikonowa.",null,"49cm","mleczny",null,"Lampa E27","LED A55..60",null,0,null,null,80,null,"205ZX0010, 206GA0010, 206GA0S10","Zaciski podłączeniowe: max 3x2,5mm², możliwość podłączenia oprawy w pętle max 3x2,5mm². Przewód w oponie okrągłej o średnicy max ø12,5mm.","289XX0011.jpg","289XX0011.ldt",4,"E27",1,24]
["291","291XX0011","ALTA BOLLARD 85CM E27","Alta","Bollard","Stal",null,null,null,"Wymienne","E27",null,"LED max 9W","LED max 9W",null,null,null,null,"65","IK10","Class II",null,null,0.15,0.15,0.85,"CE",null,null,null,1,"Oprawa słupkowa.","Światło obrotowo symetryczne przysłonięte od góry.",null,"Bollard luminaire of stable and durable construction. For lighting private areas and public spaces.",null,null,null,"Stal cynkowana ogniowo.",null,"Klosz- tworzywo sztuczne PMMA w kolorze mlecznym.","Uszczelka silikonowa.",null,"85cm",null,null,"Lampa E27","LED A55..60",null,0,null,null,80,null,"205ZX0010, 206GA0010, 206GA0S10","Zaciski podłączeniowe: max 3x2,5mm², możliwość podłączenia oprawy w pętle max 3x2,5mm². Przewód w oponie okrągłej o średnicy max ø12,5mm.","291XX0011.jpg","291XX0011.ldt",4,"E27",1,1]
["2935","2935XX0009","SKARA BOLLARD LED 828LM SCL 3000K DIM.","Skara","Bollard","Aluminium",null,null,"PRO","LED zintegrowane","AC","DIM.","5,8W","7,7W","828lm","699lm",null,null,"65","IK08","Class II",3000,"szerokie dół",null,null,null,"CE",null,null,"> 268 210h",13,"Oprawa słupkowa.","Soczewka firmy Ledil typu SCL (IESNA typ II / III).","SCL","A luminaire with a contemporary design. For lighting private areas and other architectural concepts.","A luminaire with a contemporary design. For lighting private areas and other architectural concepts.",null,null,"Profil aluminiowy wyciskany, malowany proszkowo.",null,"Soczewka hermetyczna zewnętrzna- tworzywo sztuczne PMMA przeźroczyste.",null,"Dławnica EPDM.",null,null,"Oprawa ściemnialna fazowo TRAILING EDGE (TE)","Moduł LED","Cree DK200402 V1 XTE-HE 3K","Philips Xitanium 10W 0,5A 20V TE SC 230V",0,"Philips Xitanium TE",null,80,"E","2934ZX0009","Zaciski podłączeniowe: max 3x4mm², możliwość podłączenia oprawy w pętle max 3x4mm². Przewód w oponie okrągłej o średnicy max ø12,5mm.","2935XX0009.png","2935XX0009.ldt",1,null,1,46]
["2937","2937XX0009","SKARA BOLLARD LED 856LM SCL 4000K DIM.","Skara","Bollard","Aluminium",null,null,"PRO","LED zintegrowane","AC","DIM.","5,8W","7,7W","856lm","730lm",null,null,"65","IK08","Class II",4000,"szerokie dół",null,null,null,"CE",null,null,"> 268 210h",13,"Oprawa słupkowa.","Soczewka firmy Ledil typu SCL (IESNA typ II / III).","SCL","A luminaire with a contemporary design. For lighting private areas and other architectural concepts.","A luminaire with a contemporary design. For lighting private areas and other architectural concepts.",null,null,"Profil aluminiowy wyciskany, malowany proszkowo.",null,"Soczewka hermetyczna zewnętrzna- tworzywo sztuczne PMMA przeźroczyste.",null,"Dławnica EPDM.",null,null,"Oprawa ściemnialna fazowo TRAILING EDGE (TE)","Moduł LED","Cree DK200402 V1 XTE-HE 3V 4K.","Philips Xitanium 10W 0,5A 20V TE SC 230V",0,"Philips Xitanium TE",null,80,"E","2934ZX0009","Zaciski podłączeniowe: max 3x4mm², możliwość podłączenia oprawy w pętle max 3x4mm². Przewód w oponie okrągłej o średnicy max ø12,5mm.","2937XX0009.png","2937XX0009.ldt",1,null,1,46]
["2939","2939XX0009","SKARA BOLLARD LED 828LM VSM 3000K DIM.","Skara","Bollard","Aluminium",null,null,"PRO","LED zintegrowane","AC","DIM.","5,8W","7,7W","828lm","604lm",null,null,"65","IK08","Class II",3000,"szerokie dół",null,null,null,"CE",null,null,"> 268 210h",13,"Oprawa słupkowa.","Soczewka firmy Ledil typu VSM (IESNA typ V).","VSM","A luminaire with a contemporary design. For lighting private areas and other architectural concepts.","A luminaire with a contemporary design. For lighting private areas and other architectural concepts.",null,null,"Profil aluminiowy wyciskany, malowany proszkowo.",null,"Soczewka hermetyczna zewnętrzna- tworzywo sztuczne PMMA przeźroczyste.",null,"Dławnica EPDM.",null,null,"Oprawa ściemnialna fazowo TRAILING EDGE (TE)","Moduł LED","Cree DK200402 V1 XTE-HE 3K","Philips Xitanium 10W 0,5A 20V TE SC 230V",0,"Philips Xitanium TE",null,80,"E","2934ZX0009","Zaciski podłączeniowe: max 3x4mm², możliwość podłączenia oprawy w pętle max 3x4mm². Przewód w oponie okrągłej o średnicy max ø12,5mm.","2939XX0009.png","2939XX0009.ldt",1,null,1,47]
["293","293XX0011","ALTA BOLLARD 49CM E27","Alta","Bollard","Stal",null,null,null,"Wymienne","E27",null,"LED max 9W","LED max 9W",null,null,null,null,"65","IK10","Class II",null,null,0.15,0.15,0.49,"CE",null,null,null,1,"Oprawa słupkowa.","Światło obrotowo symetryczne przysłonięte od góry.",null,"Bollard luminaire of stable and durable construction. For lighting private areas and public spaces.",null,null,null,"Stal cynkowana ogniowo.",null,"Klosz- tworzywo sztuczne PMMA w kolorze mlecznym.","Uszczelka silikonowa.",null,"49cm",null,null,"Lampa E27","LED A55..60",null,0,null,null,80,null,"205ZX0010, 206GA0010, 206GA0S10, 46999021","Zaciski podłączeniowe: max 3x4mm², możliwość podłączenia oprawy w pętle max 3x2,5mm². Przewód w oponie okrągłej o średnicy max ø12,5mm.","293XX0011.jpg","293XX0011.ldt",4,"E27",1,1]
["2941","2941XX0009","SKARA BOLLARD LED 856LM VSM 4000K DIM.","Skara","Bollard","Aluminium",null,null,"PRO","LED zintegrowane","AC","DIM.","5,8W","7,7W","856lm","616lm",null,null,"65","IK08","Class II",4000,"szerokie dół",null,null,null,"CE",null,null,"> 268 210h",13,"Oprawa słupkowa.","Soczewka firmy Ledil typu VSM (IESNA typ V).","VSM","A luminaire with a contemporary design. For lighting private areas and other architectural concepts.","A luminaire with a contemporary design. For lighting private areas and other architectural concepts.",null,null,"Profil aluminiowy wyciskany, malowany proszkowo.",null,"Soczewka hermetyczna zewnętrzna- tworzywo sztuczne PMMA przeźroczyste.",null,"Dławnica EPDM.",null,null,"Oprawa ściemnialna fazowo TRAILING EDGE (TE)","Moduł LED","Cree DK200402 V1 XTE-HE 3V 4K.","Philips Xitanium 10W 0,5A 20V TE SC 230V",0,"Philips Xitanium TE",null,80,"E","2934ZX0009","Zaciski podłączeniowe: max 3x4mm², możliwość podłączenia oprawy w pętle max 3x4mm². Przewód w oponie okrągłej o średnicy max ø12,5mm.","2941XX0009.png","2941XX0009.ldt",1,null,1,47]
["2943","2943XX0009","SKARA BOLLARD - CONNECTORS E [UNI] LED 828LM SCL 3000K DIM.","Skara","Bollard","Aluminium",null,null,"PRO","LED zintegrowane","AC","DIM.","5,8W","7,7W","828lm","699lm",null,null,"65","IK08","Class II",3000,"szerokie dół",null,null,null,"CE",null,null,"> 268 210h",41,"Oprawa słupkowa - dystrybutor energii E [Uni].","Soczewka firmy Ledil typu SCL (IESNA typ II / III).","SCL","A luminaire with a contemporary design. For lighting private areas and other architectural concepts.","A luminaire with a contemporary design. For lighting private areas and other architectural concepts. Lighting luminaire equipped with: - Two E-type sockets (Uni)",null,null,"Profil aluminiowy wyciskany, malowany proszkowo.",null,"Soczewka hermetyczna zewnętrzna- tworzywo sztuczne PMMA przeźroczyste.",null,null,null,null,"Oprawa ściemnialna fazowo TRAILING EDGE (TE)","Moduł LED","Cree DK200402 V1 XTE-HE 3K","Philips Xitanium 10W 0,5A 20V TE SC 230V",0,"Philips Xitanium TE",null,80,"E","2934ZX0009","Zaciski podłączeniowe: max 3x4mm², możliwość podłączenia oprawy w pętle max 3x4mm². Przewód w oponie okrągłej o średnicy max ø12,5mm.","2943XX0009.png","2943XX0009.ldt",1,null,1,46]
["2945","2945XX0009","SKARA BOLLARD - CONNECTORS E [UNI] LED 828LM SCL 4000K DIM.","Skara","Bollard","Aluminium",null,null,"PRO","LED zintegrowane","AC","DIM.","5,8W","7,7W","828lm","730lm",null,null,"65","IK08","Class II",4000,"szerokie dół",null,null,null,"CE",null,null,"> 268 210h",41,"Oprawa słupkowa - dystrybutor energii E [Uni].","Soczewka firmy Ledil typu SCL (IESNA typ II / III).","SCL","A luminaire with a contemporary design. For lighting private areas and other architectural concepts.","A luminaire with a contemporary design. For lighting private areas and other architectural concepts. Lighting luminaire equipped with: - Two E-type sockets (Uni)",null,null,"Profil aluminiowy wyciskany, malowany proszkowo.",null,"Soczewka hermetyczna zewnętrzna- tworzywo sztuczne PMMA przeźroczyste.",null,null,null,null,"Oprawa ściemnialna fazowo TRAILING EDGE (TE)","Moduł LED","Cree DK200402 V1 XTE-HE 3V 4K.","Philips Xitanium 10W 0,5A 20V TE SC 230V",0,"Philips Xitanium TE",null,80,"E","2934ZX0009","Zaciski podłączeniowe: max 3x4mm², możliwość podłączenia oprawy w pętle max 3x4mm². Przewód w oponie okrągłej o średnicy max ø12,5mm.","2945XX0009.png","2945XX0009.ldt",1,null,1,46]
["2947","2947XX0009","SKARA BOLLARD - CONNECTORS E [UNI] LED 828LM VSM 3000K DIM.","Skara","Bollard","Aluminium",null,null,"PRO","LED zintegrowane","AC","DIM.","5,8W","7,7W","828lm","604lm",null,null,"65","IK08","Class II",3000,"szerokie dół",null,null,null,"CE",null,null,"> 268 210h",41,"Oprawa słupkowa - dystrybutor energii E [Uni].","Soczewka firmy Ledil typu VSM (IESNA typ V).","VSM","A luminaire with a contemporary design. For lighting private areas and other architectural concepts.","A luminaire with a contemporary design. For lighting private areas and other architectural concepts. Lighting luminaire equipped with: - Two E-type sockets (Uni)",null,null,"Profil aluminiowy wyciskany, malowany proszkowo.",null,"Soczewka hermetyczna zewnętrzna- tworzywo sztuczne PMMA przeźroczyste.",null,"Dławnica EPDM.",null,null,"Oprawa ściemnialna fazowo TRAILING EDGE (TE)","Moduł LED","Cree DK200402 V1 XTE-HE 3K","Philips Xitanium 10W 0,5A 20V TE SC 230V",0,"Philips Xitanium TE",null,80,"E","2934ZX0009","Zaciski podłączeniowe: max 3x4mm², możliwość podłączenia oprawy w pętle max 3x4mm². Przewód w oponie okrągłej o średnicy max ø12,5mm.","2947XX0009.png","2947XX0009.ldt",1,null,1,47]
["2949","2949XX0009","SKARA BOLLARD - CONNECTORS E [UNI] LED 856LM VSM 4000K DIM.","Skara","Bollard","Aluminium",null,null,"PRO","LED zintegrowane","AC","DIM.","5,8W","7,7W","856lm","616lm",null,null,"65","IK08","Class II",4000,"szerokie dół",null,null,null,"CE",null,null,"> 268 210h",41,"Oprawa słupkowa - dystrybutor energii E [Uni].","Soczewka firmy Ledil typu VSM (IESNA typ V).","VSM","A luminaire with a contemporary design. For lighting private areas and other architectural concepts.","A luminaire with a contemporary design. For lighting private areas and other architectural concepts. Lighting luminaire equipped with: - Two E-type sockets (Uni)",null,null,"Profil aluminiowy wyciskany, malowany proszkowo.",null,"Soczewka hermetyczna zewnętrzna- tworzywo sztuczne PMMA przeźroczyste.",null,"Dławnica EPDM.",null,null,"Oprawa ściemnialna fazowo TRAILING EDGE (TE)","Moduł LED","Cree DK200402 V1 XTE-HE 3V 4K.","Philips Xitanium 10W 0,5A 20V TE SC 230V",0,"Philips Xitanium TE",null,80,"E","2934ZX0009","Zaciski podłączeniowe: max 3x4mm², możliwość podłączenia oprawy w pętle max 3x4mm². Przewód w oponie okrągłej o średnicy max ø12,5mm.","2949XX0009.png","2949XX0009.ldt",1,null,1,47]
["295","295XX0011","HALMSTAD BOLLARD 49CM LED E27 DIM.","Halmstad","Bollard","Stal",null,null,null,"Wymienne","E27",null,"LED max 9W","LED max 9W",null,null,null,null,"65","IK10","Class II",null,null,0.12,0.12,0.49,"CE",null,null,null,1,"Oprawa słupkowa.","Światło odkryte, częściowo przysłonięte od góry.",null,"Bollard luminaire of stable and durable construction For lighting private and public areas","Bollard luminaire of stable and durable construction For lighting private and public areas Functions: control, color change 2700K…6500K (TW), WiZ, WiZ Pro - Available after mounting in the luminaire, Signify WiZ Pro A60 E27 TW 8W 230V - Full control of the luminaire after installing the free application https://pro.wizconnected.com/ - Technical support: Information Sales Department of Norlys",null,null,"Stal cynkowana ogniowo.",null,"Klosz- tworzywo sztuczne PMMA w kolorze mlecznym.","Uszczelka silikonowa.",null,"49cm",null,null,"Lampa LED E27","LED A55..60",null,0,null,null,80,null,"205ZX0010, 206GA0010, 206GA0S10, 46999021, 4699990100, 4699990101","Zaciski podłączeniowe: max 3 x 4mm², możliwość podłączenia oprawy w pętle max 3x1,5mm². Przewód w oponie okrągłej o średnicy max ø12,5mm. Zgodnie z dołączoną instrukcją montażu. Pozostałe akcesoria należy dokupić oddzielnie. Pełne sterowanie oprawy z lampą WiZ, za pomocą sygnałów Bluetooth i WiFi - należy sprawdzić zasięg sieci WiFi w miejscu montażu oprawy.","295XX0011.jpg","295XX0011.ldt",1,"E27",1,23]
["296","296XX0011","HALMSTAD BOLLARD 85CM E27","Halmstad","Bollard","Stal",null,null,null,"Wymienne","E27",null,"LED max 9W","LED max 9W",null,null,null,null,"65","IK10","Class II",null,null,0.12,0.12,0.85,"CE",null,null,null,1,"Oprawa słupkowa.","Światło odkryte, częściowo przysłonięte od góry.",null,"Bollard luminaire of stable and durable construction For lighting private areas and public spaces","Bollard luminaire of stable and durable construction For lighting private and public areas Functions: control, color change 2700K…6500K (TW), WiZ, WiZ Pro - Available after mounting in the luminaire, Signify WiZ Pro A60 E27 TW 8W 230V - Full control of the luminaire after installing the free application https://pro.wizconnected.com/ - Technical support: Information Sales Department of Norlys",null,null,"Stal cynkowana ogniowo.",null,"Klosz- tworzywo sztuczne PMMA w kolorze mlecznym.","Uszczelka silikonowa.",null,"85cm",null,null,"Lampa E27","LED A55..60",null,0,null,null,80,null,"205ZX0010, 206GA0010, 206GA0S10, 46999021","Zaciski podłączeniowe: max 3 x 2,5mm², możliwość podłączenia oprawy w pętle max 3x2,5mm². Przewód w oponie okrągłej o średnicy max ø12,5mm.","296XX0011.jpg","296XX0011.ldt",4,"E27",1,23]
["297","297XX0010","STOCKHOLM BOLLARD 85CM E27","Stockholm","Bollard","Stal",null,null,null,"Wymienne","E27",null,"LED max 9W","LED max 9W",null,null,null,null,"65","IK10","Class II",null,null,0.17,0.17,0.85,"CE",null,null,null,1,"Oprawa słupkowa.","Światło odkryte, rozproszone z obrotowo- symetrycznym rozsyłem światła.",null,"Bollard luminaire of stable and durable construction. For lighting private areas and public spaces.",null,null,"Oprawa na wymienne źródło światła typu: lampa LED, świetlówka TC-SE, tradycyjna żarówka (halogenowa) o trzonku E27. Źródło światła należy dokupić oddzielnie.","Stal cynkowana ogniowo.",null,"Klosz- tworzywo sztuczne PMMA przeźroczyste.","Uszczelka silikonowa.",null,"85cm","przeźroczysty",null,"Lampa E27","LED A55..60",null,0,null,null,80,null,"205ZX0010, 206GA0010, 206GA0S10","Zaciski podłączeniowe: max 3x4mm², możliwość podłączenia oprawy w pętle max 3x2,5mm². Przewód w oponie okrągłej o średnicy max ø12,5mm.","297XX0010.jpg","297XX0010.ldt",4,"E27",1,24]
["298","298XX0012","STOCKHOLM BOLLARD 49CM E27","Stockholm","Bollard","Stal",null,null,null,"Wymienne","E27",null,"LED max 9W","LED max 9W",null,null,null,null,"65",null,"Class II",null,null,0.17,0.17,0.49,"CE",null,null,null,1,"Oprawa słupkowa.","Światło odkryte, rozproszone z obrotowo- symetrycznym rozsyłem światła.",null,"Bollard luminaire of stable and durable construction. For lighting private areas and public spaces.",null,null,"Oprawa na wymienne źródło światła typu: lampa LED, świetlówka TC-SE, tradycyjna żarówka (halogenowa) o trzonku E27. Źródło światła należy dokupić oddzielnie.","Stal cynkowana ogniowo.",null,"Klosz- tworzywo sztuczne PMMA przeźroczyste.","Uszczelka silikonowa.",null,"49cm","przeźroczysty",null,"Lampa E27","LED A55..60",null,0,null,null,80,null,"205ZX0010, 206GA0010, 206GA0S10","Zaciski podłączeniowe: max 3x4mm², możliwość podłączenia oprawy w pętle max 3x2,5mm². Przewód w oponie okrągłej o średnicy max ø12,5mm.","298XX0012.jpg","298XX0012.ldt",4,"E27",1,24]
["299","299XX0010","STOCKHOLM BOLLARD 28CM E27","Stockholm","Bollard","Stal",null,null,null,"Wymienne","E27",null,"LED max 9W","LED max 9W",null,null,null,null,"65","IK10","Class II",null,null,0.16,0.16,0.28000000000000003,"CE",null,null,null,1,"Oprawa słupkowa.","Światło odkryte, rozproszone z obrotowo- symetrycznym rozsyłem światła.",null,"Bollard luminaire of stable and durable construction. For lighting private areas and public spaces.",null,null,"Oprawa na wymienne źródło światła typu: lampa LED, świetlówka TC-SE, tradycyjna żarówka (halogenowa) o trzonku E27. Źródło światła należy dokupić oddzielnie.","Stal cynkowana ogniowo.",null,"Klosz- tworzywo sztuczne PMMA w kolorze mlecznym.","Uszczelka silikonowa.",null,"28cm","mleczny",null,"Lampa E27","LED A55..60",null,0,null,null,80,null,"205ZX0010, 206GA0010, 206GA0S10","Zaciski podłączeniowe: max 2x2,5mm², Przewód w oponie okrągłej o średnicy max ø12mm.","299XX0010.jpg","299XX0010.ldt",4,"E27",1,24]
["370","370XX0010","COMO WALL E27","Como","Wall","Aluminium",null,null,null,"Wymienne","E27",null,"LED max 9W","LED max 9W",null,null,null,null,"54",null,"Class II",null,null,0,0,0,"CE",null,null,null,12,"Oprawa ścienna.","Światło odkryte.",null,"Classic type wall-mounted luminaire. Possibility to install on corners of architectural objects.",null,null,null,"Odlew aluminiowy malowany proszkowo.",null,"Klosz- poliwęglan przeźroczysty, stabilizowany UV.",null,"Dławnica EPDM.",null,null,null,"Lampa E27","LED A55..60",null,0,null,null,80,null,"152XX0009, 46999021","Zaciski podłączeniowe, max 2x2,5mm². Przewód w oponie okrągłej o średnicy ø7...10,5mm.","370XX0010.jpg","370XX0010.ldt",4,"E27",1,9]
["371","371XX0309","COMO POLE LUMINAIRE. E27","Como","Post,Post complete","Aluminium",null,null,null,"Wymienne","E27",null,"LED max 9W","LED max 9W",null,null,null,null,"54",null,"Class II",null,null,null,null,null,"CE",null,null,null,23,"Oprawa słupowa.","Światło odkryte.",null,"Classic design luminaire, mounted on a telescopic lighting pole. Adjustable height 1820..2490mm. For lighting gardens, terraces and other architectural concepts.",null,null,"Oprawa na wymienne źródło światła typu: lampa LED, świetlówka TC-SE, tradycyjna żarówka (halogenowa) o trzonku E27. Źródło światła należy dokupić oddzielnie.","Odlew aluminiowy malowany proszkowo.",null,"Klosz- poliwęglan przeźroczysty, stabilizowany UV.","Uszczelka silikonowa.",null,"Pojedyncze",null,null,"Lampa E27","LED A55..60",null,0,null,null,80,null,"108GA0009, 305ZX0009, 306ZX0009, 46999021","Zaciski podłączeniowe: max 4x2,5mm², możliwość podłączenia oprawy w pętle max 4x2,5mm². Przewód w oponie okrągłej o średnicy ø6...12,5mm.","371XX0309.jpg","371XX0309.ldt",4,"E27",1,9]
["372","372XX0309","COMO POLE LUMINAIRE. E27","Como","Post,Post complete","Aluminium",null,null,null,"Wymienne","E27",null,"LED max 2x 9W","LED max 2x 9W",null,null,null,null,"54",null,"Class II",null,null,null,null,null,"CE",null,null,null,23,"Oprawa słupowa.","Światło odkryte.",null,"Classic design luminaire, mounted on a telescopic lighting pole. Adjustable height 1820..2490mm. For lighting gardens, terraces and other architectural concepts.",null,null,"Oprawa na wymienne źródło światła typu: lampa LED, świetlówka TC-SE, tradycyjna żarówka (halogenowa) o trzonku E27. Źródło światła należy dokupić oddzielnie.","Odlew aluminiowy malowany proszkowo.",null,"Klosz- poliwęglan przeźroczysty, stabilizowany UV.","Uszczelka silikonowa.",null,"Podwójne",null,null,"Lampa E27","LED A55..60",null,0,null,null,80,null,"108GA0009, 305ZX0009, 306ZX0009, 46999021","Zaciski podłączeniowe: max 4x2,5mm², możliwość podłączenia oprawy w pętle max 4x2,5mm². Przewód w oponie okrągłej o średnicy ø6...12,5mm.","372XX0309.jpg","372XX0309.ldt",4,"E27",1,9]
["373","373XX0309","COMO POLE LUMINAIRE. E27","Como","Post,Post complete","Aluminium",null,null,null,"Wymienne","E27",null,"LED max 3x 9W","LED max 3x 9W",null,null,null,null,"54",null,"Class II",null,null,null,null,null,"CE",null,null,null,23,"Oprawa słupowa.","Światło odkryte.",null,"Classic design luminaire, mounted on a telescopic lighting pole. Adjustable height 1820..2490mm. For lighting gardens, terraces and other architectural concepts.",null,null,null,"Odlew aluminiowy malowany proszkowo.",null,"Klosz- poliwęglan przeźroczysty, stabilizowany UV.","Uszczelka silikonowa.",null,"Potrójne",null,null,"Lampa E27","LED A55..60",null,0,null,null,80,null,"108GA0009, 305ZX0009, 306ZX0009, 46999021","Zaciski podłączeniowe: max 4x2,5mm², możliwość podłączenia oprawy w pętle max 4x2,5mm². Przewód w oponie okrągłej o średnicy ø6...12,5mm.","373XX0309.jpg","373XX0309.ldt",4,"E27",1,9]
["375","375XX0010","COMO BOLLARD E27","Como","Bollard,Flower","Aluminium",null,null,null,"Wymienne","E27",null,"LED max 9W","LED max 9W",null,null,null,null,"54",null,"Class II",null,null,0,0,0,"CE",null,null,null,1,"Oprawa słupkowa.","Światło odkryte z obrotowo-symetrycznym rozsyłem światła.",null,"Classic design luminaire. For lighting private areas and public spaces.",null,null,"Oprawa na wymienne źródło światła typu: lampa LED, tradycyjna żarówka (halogenowa) o trzonku E27. Źródło światła należy dokupić oddzielnie.","Odlew aluminiowy malowany proszkowo.",null,"Klosz- poliwęglan przeźroczysty, stabilizowany UV.",null,"Dławnica EPDM.",null,null,null,"Lampa E27","LED A55..60",null,0,null,null,80,null,"307ZX0009, 46999021","Zaciski podłączeniowe: max 2x2,5mm², możliwość podłączenia oprawy w pętle max 2x1,5mm². Przewód w oponie okrągłej o średnicy ø7...10,5mm.","375XX0010.jpg","375XX0010.ldt",4,"E27",1,26]
["4043","4043XX0009","SOL CEILING LED 2200LM 3000K DIM.","Sol","Ceiling","Aluminium",null,null,null,"LED zintegrowane","AC","DIM.","16,8W","19,3W","2200lm","1938lm","Szkło","Transparentny","65","IK06","Class I",3000,"szerokie dół",0.2,0.2,0.11,"CE",null,null,"> 100 000h",6,"Oprawa sufitowa.","Światło symetryczne ukierunkowane w dół.",null,"A luminaire with a contemporary design. For lighting gardens, private areas and other architectural concepts",null,null,null,"Profil aluminiowy wyciskany, malowany proszkowo.","Stop aluminiowy malowany proszkowo.","Klosz- szkło bezpieczne, przeźroczyste.","Uszczelka silikonowa.","Dławnica EPDM.",null,null,"Oprawa ściemnialna fazowo TRAILING EDGE (TE) - LEADING EDGE (LE)","Moduł LED","Philips Fortimo DLM Flex 5000/830 Gen2 3K","TCI Mini MD 20W 500mA BI code 127033 Triak",0,null,null,80,"E","3095XX0009","Zaciski podłączeniowe: max 3x2,5mm², możliwość podłączenia oprawy w pętle max 1,5 mm². Przewód w oponie okrągłej o średnicy ø7...10,5mm.","4043XX0009.png","4043XX0009.ldt",1,null,1,34]
["4044","4044XX0009","SOL CEILING LED 2399LM 4000K DIM.","Sol","Ceiling","Aluminium",null,null,null,"LED zintegrowane","AC","DIM.","16,8W","19,3W","2399lm","2221lm","Szkło","Transparentny","65","IK06","Class I",4000,"szerokie dół",0.2,0.2,0.11,"CE",null,null,"> 100 000h",6,"Oprawa sufitowa.","Światło symetryczne ukierunkowane w dół.",null,"A fixture with a contemporary design. For lighting gardens, private areas and other architectural concepts",null,null,null,"Profil aluminiowy wyciskany, malowany proszkowo.","Stop aluminiowy malowany proszkowo.","Klosz- szkło bezpieczne, przeźroczyste.","Uszczelka silikonowa.","Dławnica EPDM.",null,null,"Oprawa ściemnialna fazowo TRAILING EDGE (TE) - LEADING EDGE (LE)","Moduł LED","Philips Fortimo DLM Flex 5000/840 Gen2 4K","TCI Mini MD 20W 500mA BI code 127033 Triak",0,null,null,80,"D","3095XX0009","Zaciski podłączeniowe: max 3x2,5mm², możliwość podłączenia oprawy w pętle max 1,5 mm². Przewód w oponie okrągłej o średnicy ø7...10,5mm.","4044XX0009.png","4044XX0009.ldt",1,null,1,34]
["4045","4045XX0009","SOL CEILING LED 2200LM 3000K DIM.","Sol","Ceiling","Aluminium",null,null,null,"LED zintegrowane","AC","DIM.","16,8W","19,3W","2200lm","1633lm","Szkło","Satynowany","65","IK06","Class I",3000,"szerokie dół",0.2,0.2,0.11,"CE",null,null,"> 100 000h",6,"Oprawa sufitowa.","Światło symetryczne ukierunkowane w dół.",null,"A luminaire with a contemporary design. For lighting gardens, private areas and other architectural concepts",null,null,null,"Profil aluminiowy wyciskany, malowany proszkowo.","Stop aluminiowy malowany proszkowo.","Klosz- szkło bezpieczne, satynowane.","Uszczelka silikonowa.","Dławnica EPDM.",null,null,"Oprawa ściemnialna fazowo TRAILING EDGE (TE) - LEADING EDGE (LE)","Moduł LED","Philips Fortimo DLM Flex 5000/830 Gen2 3K","TCI Mini MD 20W 500mA BI code 127033 Triak",0,null,null,80,"E","3095XX0009","Zaciski podłączeniowe: max 3x2,5mm², możliwość podłączenia oprawy w pętle max 1,5 mm². Przewód w oponie okrągłej o średnicy ø7...10,5mm.","4045XX0009.png","4045XX0009.ldt",1,null,1,34]
["4046","4046XX0009","SOL CEILING LED 2399LM 4000K DIM.","Sol","Ceiling","Aluminium",null,null,null,"LED zintegrowane","AC","DIM.","16,8W","19,1W","2399lm","1890lm","Szkło","Satynowany","65","IK06","Class I",4000,"szerokie dół",0.2,0.2,0.11,"CE",null,null,"> 100 000h",6,"Oprawa sufitowa.","Światło symetryczne ukierunkowane w dół.",null,"A luminaire with a contemporary design. For lighting gardens, private areas and other architectural concepts",null,null,null,"Profil aluminiowy wyciskany, malowany proszkowo.","Stop aluminiowy malowany proszkowo.","Klosz- szkło bezpieczne, satynowane.","Uszczelka silikonowa.","Dławnica EPDM.",null,null,"Oprawa ściemnialna fazowo TRAILING EDGE (TE) - LEADING EDGE (LE)","Moduł LED","Philips Fortimo DLM Flex 5000/840 Gen2 4K","TCI Mini MD 20W 500mA BI code 127033 Triak",0,null,null,80,"D","3095","Zaciski podłączeniowe: max 3x2,5mm², możliwość podłączenia oprawy w pętle max 1,5 mm². Przewód w oponie okrągłej o średnicy ø7...10,5mm.","4046XX0009.png","4046XX0009.ldt",1,null,1,34]
["4047","4047XX0009","SOL CEILING LED 2200LM 3000K DALI2","Sol","Ceiling","Aluminium",null,null,null,"LED zintegrowane","AC","DALI2","16,8W","19,3W","2200lm","1924lm","Szkło","Transparentny","65","IK06","Class I",3000,"szerokie dół",0.2,0.2,0.11,"CE",null,"DALI","> 100 000h",6,"Oprawa sufitowa.","Światło symetryczne ukierunkowane w dół.",null,"A luminaire with a contemporary design. For lighting gardens, private areas and other architectural concepts","A luminaire with a contemporary design. For lighting gardens, private areas and other architectural concepts The luminaire is also suitable for direct voltage: DC 176 ÷ 280 V","DC",null,"Profil aluminiowy wyciskany, malowany proszkowo.","Stop aluminiowy malowany proszkowo.","Klosz- szkło bezpieczne, przeźroczyste.","Uszczelka silikonowa.","Dławnica EPDM.",null,null,"Sterowanie światłem w systemie: DALI2","Moduł LED","Philips Fortimo DLM Flex 5000/830 Gen2 3K","TCI Mini JOLLY 20W code 151403 BI DALI",0,null,null,80,"E","3095XX0009","Zaciski podłączeniowe: max 5x2,5mm², możliwość podłączenia oprawy w pętle max 1,5 mm². Przewód w oponie okrągłej o średnicy ø7...10,5mm.","4047XX0009.png","4047XX0009.ldt",3,null,1,34]
["4048","4048XX0009","SOL CEILING LED 2400LM 4000K DALI2","Sol","Ceiling","Aluminium",null,null,null,"LED zintegrowane","AC","DALI2","16,8W","19,1W","2400lm","2227lm","Szkło","Transparentny","65","IK06","Class I",4000,"szerokie dół",0.2,0.2,0.11,"CE",null,"DALI","> 100 000h",6,"Oprawa sufitowa.","Światło symetryczne ukierunkowane w dół.",null,"A luminaire with a contemporary design. For lighting gardens, private areas and other architectural concepts","A luminaire with a contemporary design. For lighting gardens, private areas and other architectural concepts The luminaire is also suitable for direct voltage: DC 176 ÷ 280 V","DC",null,"Profil aluminiowy wyciskany, malowany proszkowo.","Stop aluminiowy malowany proszkowo.","Klosz- szkło bezpieczne, przeźroczyste.","Uszczelka silikonowa.","Dławnica EPDM.",null,null,"Sterowanie światłem w systemie: DALI2","Moduł LED","Philips Fortimo DLM Flex 5000/840 Gen2 4K","TCI Mini JOLLY 20W code 151403 BI DALI",0,null,null,80,"D","3095XX0009","Zaciski podłączeniowe: max 5x2,5mm², możliwość podłączenia oprawy w pętle max 1,5 mm². Przewód w oponie okrągłej o średnicy ø7...10,5mm.","4048XX0009.png","4048XX0009.ldt",3,null,1,34]
["4049","4049XX0009","SOL CEILING LED 2200LM 3000K DALI2","Sol","Ceiling","Aluminium",null,null,null,"LED zintegrowane","AC","DALI2","16,8W","19,3W","2200lm","1618lm","Szkło","Satynowany","65","IK06","Class I",3000,"szerokie dół",0.2,0.2,0.11,"CE",null,"DALI","> 100 000h",6,"Oprawa sufitowa.","Światło symetryczne ukierunkowane w dół.",null,"A luminaire with a contemporary design. For lighting gardens, private areas and other architectural concepts","A luminaire with a contemporary design. For lighting gardens, private areas and other architectural concepts The luminaire is also suitable for direct voltage: DC 176 ÷ 280 V","DC",null,"Profil aluminiowy wyciskany, malowany proszkowo.","Stop aluminiowy malowany proszkowo.","Klosz- szkło bezpieczne, satynowane.","Uszczelka silikonowa.","Dławnica EPDM.",null,null,"Sterowanie światłem w systemie: DALI2","Moduł LED","Philips Fortimo DLM Flex 5000/830 Gen2 3K","TCI Mini JOLLY 20W code 151403 BI DALI",0,null,null,80,"E","3095","Zaciski podłączeniowe: max 5x2,5mm², możliwość podłączenia oprawy w pętle max 1,5 mm². Przewód w oponie okrągłej o średnicy ø7...10,5mm.","4049XX0009.png","4049XX0009.ldt",3,null,1,34]
["4050","4050XX0009","SOL CEILING LED 2400LM 4000K DALI2","Sol","Ceiling","Aluminium",null,null,null,"LED zintegrowane","AC","DALI2","16,8W","19,1W","2400lm","1866lm","Szkło","Satynowany","65","IK06","Class I",4000,"szerokie dół",0.2,0.2,0.11,"CE",null,"DALI","> 100 000h",6,"Oprawa sufitowa.","Światło symetryczne ukierunkowane w dół.",null,"A luminaire with a contemporary design. For lighting gardens, private areas and other architectural concepts","A luminaire with a contemporary design. For lighting gardens, private areas and other architectural concepts The luminaire is also suitable for direct voltage: DC 176 ÷ 280 V","DC",null,"Profil aluminiowy wyciskany, malowany proszkowo.","Stop aluminiowy malowany proszkowo.","Klosz- szkło bezpieczne, satynowane.","Uszczelka silikonowa.","Dławnica EPDM.",null,null,"Sterowanie światłem w systemie: DALI2","Moduł LED","Philips Fortimo DLM Flex 5000/840 Gen2 4K","TCI Mini JOLLY 20W code 151403 BI DALI",0,null,null,80,"D","3095XX0009","Zaciski podłączeniowe: max 5x2,5mm², możliwość podłączenia oprawy w pętle max 1,5 mm². Przewód w oponie okrągłej o średnicy ø7...10,5mm.","4050XX0009.png","4050XX0009.ldt",3,null,1,34]
["4051","4051XX0009","SOL CEILING LED 2200LM 3000K DIM.","Sol","Ceiling","Aluminium",null,null,null,"LED zintegrowane","AC","DIM.","16,8W","19,1W","2200lm","2101lm","Tworzywo sztuczne","Transparentny","65","IK10","Class I",3000,"szerokie dół",0.2,0.2,0.11,"CE",null,null,"> 100 000h",6,"Oprawa sufitowa.","Światło symetryczne ukierunkowane w dół.",null,"A luminaire with a contemporary design. For lighting gardens, private areas and other architectural concepts",null,null,null,"Profil aluminiowy wyciskany, malowany proszkowo.","Stop aluminiowy malowany proszkowo.","Klosz- poliwęglan przeźroczysty, stabilizowany UV.","Uszczelka silikonowa.","Dławnica EPDM.",null,"przeźroczysty PC","Oprawa ściemnialna fazowo TRAILING EDGE (TE) - LEADING EDGE (LE)","Moduł LED","Philips Fortimo DLM Flex 5000/830 Gen2 3K","TCI Mini MD 20W 500mA BI code 127033 Triak",0,null,null,80,"E","3095XX0009","Zaciski podłączeniowe: max 3x2,5mm², możliwość podłączenia oprawy w pętle max 1,5 mm². Przewód w oponie okrągłej o średnicy ø7...10,5mm.","4051XX0009.png","4051XX0009.ldt",1,null,1,34]
["4052","4052XX0009","SOL CEILING LED 2499LM 4000K DIM.","Sol","Ceiling","Aluminium",null,null,null,"LED zintegrowane","AC","DIM.","16,8W","19,1W","2499lm","2421lm","Tworzywo sztuczne","Transparentny","65","IK10","Class I",4000,"szerokie dół",0.2,0.2,0.11,"CE",null,null,"> 100 000h",6,"Oprawa sufitowa.","Światło symetryczne ukierunkowane w dół.",null,"A luminaire with a contemporary design. For lighting gardens, private areas and other architectural concepts",null,null,null,"Profil aluminiowy wyciskany, malowany proszkowo.","Stop aluminiowy malowany proszkowo.","Klosz- poliwęglan przeźroczysty, stabilizowany UV.","Uszczelka silikonowa.","Dławnica EPDM.",null,"przeźroczysty PC","Oprawa ściemnialna fazowo TRAILING EDGE (TE) - LEADING EDGE (LE)","Moduł LED","Philips Fortimo DLM Flex 5000/840 Gen2 4K","TCI Mini MD 20W 500mA BI code 127033 Triak",0,null,null,80,"D","3095XX0009","Zaciski podłączeniowe: max 3x2,5mm², możliwość podłączenia oprawy w pętle max 1,5 mm². Przewód w oponie okrągłej o średnicy ø7...10,5mm.","4052XX0009.png","4052XX0009.ldt",1,null,1,34]
["4053","4053XX0009","SOL CEILING LED 2200LM 3000K DIM.","Sol","Ceiling","Aluminium",null,null,null,"LED zintegrowane","AC","DIM.","16,8W","19,3W","2200lm","1655lm","Tworzywo sztuczne","Satynowany","65","IK10","Class I",3000,"szerokie dół",0.2,0.2,0.11,"CE",null,null,"> 100 000h",6,"Oprawa sufitowa.","Światło symetryczne ukierunkowane w dół.",null,"A luminaire with a contemporary design. For lighting gardens, private areas and other architectural concepts",null,null,null,"Profil aluminiowy wyciskany, malowany proszkowo.","Stop aluminiowy malowany proszkowo.","Klosz- poliwęglan satynowany, stabilizowany UV.","Uszczelka silikonowa.","Dławnica EPDM.",null,"satyna PC","Oprawa ściemnialna fazowo TRAILING EDGE (TE) - LEADING EDGE (LE)","Moduł LED","Philips Fortimo DLM Flex 5000/830 Gen2 3K","TCI Mini MD 20W 500mA BI code 127033 Triak",0,null,null,80,"E","3095","Zaciski podłączeniowe: max 3x2,5mm², możliwość podłączenia oprawy w pętle max 1,5 mm². Przewód w oponie okrągłej o średnicy ø7...10,5mm.","4053XX0009.png","4053XX0009.ldt",1,null,1,34]
["4054","4054XX0009","SOL CEILING LED 2400LM 4000K DIM.","Sol","Ceiling","Aluminium",null,null,null,"LED zintegrowane","AC","DIM.","16,8W","19,3W","2400lm","1905lm","Tworzywo sztuczne","Satynowany","65","IK10","Class I",4000,"szerokie dół",0.2,0.2,0.11,"CE",null,null,"> 100 000h",6,"Oprawa sufitowa.","Światło symetryczne ukierunkowane w dół.",null,"A luminaire with a contemporary design. For lighting gardens, private areas and other architectural concepts",null,null,null,"Profil aluminiowy wyciskany, malowany proszkowo.","Stop aluminiowy malowany proszkowo.","Klosz- poliwęglan satynowany, stabilizowany UV.","Uszczelka silikonowa.","Dławnica EPDM.",null,"satyna PC","Oprawa ściemnialna fazowo TRAILING EDGE (TE) - LEADING EDGE (LE)","Moduł LED","Philips Fortimo DLM Flex 5000/840 Gen2 4K","TCI Mini MD 20W 500mA BI code 127033 Triak",0,null,null,80,"D","3095XX0009","Zaciski podłączeniowe: max 3x2,5mm², możliwość podłączenia oprawy w pętle max 1,5 mm². Przewód w oponie okrągłej o średnicy ø7...10,5mm.","4054XX0009.png","4054XX0009.ldt",1,null,1,34]
["4055","4055XX0009","SOL CEILING LED 2200LM 3000K DALI2","Sol","Ceiling","Aluminium",null,null,null,"LED zintegrowane","AC","DALI2","16,8W","19,1W","2200lm","2101lm","Tworzywo sztuczne","Transparentny","65","IK10","Class I",3000,"szerokie dół",0.2,0.2,0.11,"CE",null,"DALI","> 100 000h",6,"Oprawa sufitowa.","Światło symetryczne ukierunkowane w dół.",null,"A luminaire with a contemporary design. For lighting gardens, private areas and other architectural concepts","A luminaire with a contemporary design. For lighting gardens, private areas and other architectural concepts The luminaire is also suitable for direct voltage: DC 176 ÷ 280 V","DC",null,"Profil aluminiowy wyciskany, malowany proszkowo.","Stop aluminiowy malowany proszkowo.","Klosz- poliwęglan przeźroczysty, stabilizowany UV.","Uszczelka silikonowa.","Dławnica EPDM.",null,"przeźroczysty PC","Sterowanie światłem w systemie: DALI2","Moduł LED","Philips Fortimo DLM Flex 5000/830 Gen2 3K","TCI Mini JOLLY 20W code 151403 BI DALI",0,null,null,80,"E","3095XX0009","Zaciski podłączeniowe: max 5x2,5mm², możliwość podłączenia oprawy w pętle max 1,5 mm². Przewód w oponie okrągłej o średnicy ø7...10,5mm.","4055XX0009.png","4055XX0009.ldt",3,null,1,34]
["4056","4056XX0009","SOL CEILING LED 2499LM 4000K DALI2","Sol","Ceiling","Aluminium",null,null,null,"LED zintegrowane","AC","DALI2","16,8W","19,1W","2499lm","2421lm","Tworzywo sztuczne","Transparentny","65","IK10","Class I",4000,"szerokie dół",0.2,0.2,0.11,"CE",null,"DALI","> 100 000h",6,"Oprawa sufitowa.","Światło symetryczne ukierunkowane w dół.",null,"A luminaire with a contemporary design. For lighting gardens, private areas and other architectural concepts","A luminaire with a contemporary design. For lighting gardens, private areas and other architectural concepts The luminaire is also suitable for direct voltage: DC 176 ÷ 280 V","DC",null,"Profil aluminiowy wyciskany, malowany proszkowo.","Stop aluminiowy malowany proszkowo.","Klosz- poliwęglan przeźroczysty, stabilizowany UV.","Uszczelka silikonowa.","Dławnica EPDM.",null,"przeźroczysty PC","Sterowanie światłem w systemie: DALI2","Moduł LED","Philips Fortimo DLM Flex 5000/840 Gen2 4K","TCI Mini JOLLY 20W code 151403 BI DALI",0,null,null,80,"D","3095XX0009","Zaciski podłączeniowe: max 5x2,5mm², możliwość podłączenia oprawy w pętle max 1,5 mm². Przewód w oponie okrągłej o średnicy ø7...10,5mm.","4056XX0009.png","4056XX0009.ldt",3,null,1,34]
["4057","4057XX0009","SOL CEILING LED 2200LM 3000K DALI2","Sol","Ceiling","Aluminium",null,null,null,"LED zintegrowane","AC","DALI2","16,8W","19,3W","2200lm","1663lm","Tworzywo sztuczne","Satynowany","65","IK10","Class I",3000,"szerokie dół",0.2,0.2,0.11,"CE",null,"DALI","> 100 000h",6,"Oprawa sufitowa.","Światło symetryczne ukierunkowane w dół.",null,"A luminaire with a contemporary design. For lighting gardens, private areas and other architectural concepts","A luminaire with a contemporary design. For lighting gardens, private areas and other architectural concepts The luminaire is also suitable for direct voltage: DC 176 ÷ 280 V","DC",null,"Profil aluminiowy wyciskany, malowany proszkowo.","Stop aluminiowy malowany proszkowo.","Klosz- poliwęglan satynowany, stabilizowany UV.","Uszczelka silikonowa.","Dławnica EPDM.",null,"satyna PC","Sterowanie światłem w systemie: DALI2","Moduł LED","Philips Fortimo DLM Flex 5000/830 Gen2 3K","TCI Mini JOLLY 20W code 151403 BI DALI",0,null,null,80,"E","3095XX0009","Zaciski podłączeniowe: max 5x2,5mm², możliwość podłączenia oprawy w pętle max 1,5 mm². Przewód w oponie okrągłej o średnicy ø7...10,5mm.","4057XX0009.png","4057XX0009.ldt",3,null,1,34]
["4058","4058XX0009","SOL CEILING LED 2400LM 4000K DALI2","Sol","Ceiling","Aluminium",null,null,null,"LED zintegrowane","AC","DALI2","16,8W","19,3W","2400lm","1912lm","Tworzywo sztuczne","Satynowany","65","IK10","Class I",4000,"szerokie dół",0.2,0.2,0.11,"CE",null,"DALI","> 100 000h",6,"Oprawa sufitowa.","Światło symetryczne ukierunkowane w dół.",null,"A luminaire with a contemporary design. For lighting gardens, private areas and other architectural concepts","A luminaire with a contemporary design. For lighting gardens, private areas and other architectural concepts The luminaire is also suitable for direct voltage: DC 176 ÷ 280 V","DC",null,"Profil aluminiowy wyciskany, malowany proszkowo.","Stop aluminiowy malowany proszkowo.","Klosz- poliwęglan satynowany, stabilizowany UV.","Uszczelka silikonowa.","Dławnica EPDM.",null,"satyna PC","Sterowanie światłem w systemie: DALI2","Moduł LED","Philips Fortimo DLM Flex 5000/840 Gen2 4K","TCI Mini JOLLY 20W code 151403 BI DALI",0,null,null,80,"D","3095XX0009","Zaciski podłączeniowe: max 5x2,5mm², możliwość podłączenia oprawy w pętle max 1,5 mm². Przewód w oponie okrągłej o średnicy ø7...10,5mm.","4058XX0009.png","4058XX0009.ldt",3,null,1,34]
["4113","4113XX0009","LONDON POLE-TOP LED 1950LM 4000K","London,Big","Post,Head","Aluminium",null,null,null,"LED zintegrowane","AC",null,"17,5W","17,5W","1950lm","1392lm",null,null,"54",null,"Class II",4000,null,null,null,null,"CE",null,null,"50000",2,"Oprawa słupowa (nasadzana).","Światło odkryte.",null,"A luminaire with a classic design, mounted on a lighting pole, with a mounting base of Ø50mm For lighting gardens, parks and other architectural concepts.",null,null,null,"Odlew aluminiowy malowany proszkowo.",null,null,null,null,"Pojedyncze",null,null,"Moduł LED","Philips Fortimo DLM ES 2000/8xx G2 4K",null,null,null,null,80,"E","1273XX0010, 305ZX0009, 3061XX0010, 306ZX0009","PRZEWÓD H05RN-F 2x1 CZARNY o długości 4m do podłączenia wewnątrz słupa oświetleniowego (w odpowiednio dobranej puszce elektroinstalacyjnej).","4113XX0009.png","4113XX0009.ldt",4,null,1,9]
["4114","4114XX0009","LONDON POLE-TOP LED 2000LM 3000K ON/OFF","London,Big","Post,Head","Aluminium",null,null,null,"LED zintegrowane","AC","ON/OFF","19,6","14,6","2000lm","1716lm",null,null,"65",null,"Class II",3000,null,0,0,0,"CE",null,null,"> 120 000h",2,"Oprawa słupowa (nasadzana).","Światło odkryte.",null,"A luminaire with a classic design, mounted on a lighting pole, with a mounting base of Ø50mm For lighting gardens, parks and other architectural concepts.",null,null,null,"Odlew aluminiowy malowany proszkowo.",null,null,null,null,"Pojedyncze",null,"Oprawa nieściemnialna","Moduł LED","Philips Fortimo FastFlex LED 2x6 DP G4+ 3K","Philips Xi BP 12 W 0,1-0,5AS 230 V C100",100000,null,null,70,"D","3010XX0010, 305ZX0009, 3061XX0010, 306ZX0009","Przewód H05RN-F 2x1 L=5m do podłączenia wewnątrz słupa oświetleniowego (w odpowiednio dobranej puszce elektroinstalacyjnej).","4114XX0009.png","4114XX0009.ldt",4,null,1,9]
["4116","4116XX0009","LONDON WALL-ARM LED 1100LM 3000K","London","Wall","Aluminium",null,null,null,"LED zintegrowane","AC",null,"9,5W","9,5W","1100lm","757lm",null,null,"54",null,"Class II",3000,null,0,0,0,"CE",null,null,"50000",21,"Oprawa ścienna na ramieniu.","Światło odkryte.",null,"Wall lamp luminaire with a classic design for general use, Can be mounted on the corners of architectural structures",null,null,null,"Odlew aluminiowy malowany proszkowo.",null,null,null,null,"na ramieniu w górę big",null,null,"Moduł LED","Philips Fortimo DLM ES 1100/8xx G2 3K",null,null,null,null,80,"E","152XX0009","PRZEWÓD H03VV-F 2x0,5 zaciski podłączeniowe, max 2x2,5mm². Przewód w oponie okrągłej o średnicy ø7...10,5mm.","4116XX0009.png","4116XX0009.ldt",4,null,1,9]
["4117","4117XX0009","LONDON WALL-ARM LED 1100LM 4000K","London","Wall","Aluminium",null,null,null,"LED zintegrowane","AC",null,"9,5W","9,5W","1100lm","805lm",null,null,"54",null,"Class II",4000,null,0,0,0,"CE",null,null,"50000",21,"Oprawa ścienna na ramieniu.","Światło odkryte.",null,"A wall lamp luminaire with a classic design for general use. Can be mounted on the corners of architectural structures.",null,null,null,"Odlew aluminiowy malowany proszkowo.",null,null,null,null,"na ramieniu w górę",null,null,"Moduł LED","Philips Fortimo DLM ES 1100/8xx G2 4K",null,null,null,null,80,"E","152XX0009","PRZEWÓD H03VV-F 2x0,5 zaciski podłączeniowe, max 2x2,5mm². Przewód w oponie okrągłej o średnicy ø7...10,5mm.","4117XX0009.png","4117XX0009.ldt",4,null,1,9]
["4118","4118XX0009","LONDON WALL-ARM LED 2000LM 3000K","London,Big","Wall","Aluminium",null,null,null,"LED zintegrowane","AC",null,"19,6W","14,6W","2000lm","1716lm",null,null,"54",null,"Class II",3000,null,0,0,0,"CE",null,null,"50000",21,"Oprawa ścienna na ramieniu.","Światło odkryte.",null,"A wall lamp luminaire with a classic design for general use. Can be mounted on the corners of architectural structures.",null,null,"Zestaw optyczny o IP67 (moduł LED i soczewka) ; zasilacz elektroniczny Wymienne (tylko LED) źródło światła przez profesjonalny serwis. Wymienny osprzęt sterujący za pomocą profesjonalnego serwisu.","Odlew aluminiowy malowany proszkowo.",null,null,null,null,"na ramieniu w górę big",null,null,"Moduł LED","Philips Fortimo FastFlex LED 2x6 DP G4+ 3K","Philips Xi BP 12 W 0,1-0,5AS 230 V C100",100000,null,null,80,"E","152XX0009","PRZEWÓD H03VV-F 2x0,5 zaciski podłączeniowe, max 2x2,5mm². Przewód w oponie okrągłej o średnicy ø7...10,5mm.","4118XX0009.png","4118XX0009.ldt",4,null,1,9]
["4119","4119XX0009","LONDON WALL-ARM LED 2000LM 4000K ON/OFF","London","Wall","Aluminium",null,null,null,"LED zintegrowane","AC","ON/OFF","19,6W","14,6W","2000lm","1767lm",null,null,"54",null,"Class II",4000,"szerokie dół",null,null,null,"CE",null,null,"50000",21,"Oprawa ścienna na ramieniu.","Światło odkryte.",null,"A wall luminaire with a classic design for general use. Can be mounted on the corners of architectural structures.",null,null,"Zestaw optyczny o IP67 (moduł LED i soczewka) ; zasilacz elektroniczny Wymienne (tylko LED) źródło światła przez profesjonalny serwis. Wymienny osprzęt sterujący za pomocą profesjonalnego serwisu.","Odlew aluminiowy malowany proszkowo.",null,null,null,null,"na ramieniu w górę big",null,"Oprawa nieściemnialna","Moduł LED","Philips Fortimo FastFlex LED 2x6 DP G4+ 4K","Philips Xi BP 12 W 0,1-0,5AS 230 V C100",100000,null,null,80,"E","152XX0009","PRZEWÓD H03VV-F 2x0,5 zaciski podłączeniowe, max 2x2,5mm². Przewód w oponie okrągłej o średnicy ø7...10,5mm.","4119XX0009.png","4119XX0009.ldt",4,null,1,9]
["4120","4120XX0009","LONDON POLE-TOP LED 1100LM 3000K","London,Big","Post,Head","Aluminium",null,null,null,"LED zintegrowane","AC",null,"9,5W","9,5W","1100lm","757lm",null,null,"54",null,"Class II",3000,null,0,0,0,"CE",null,null,"50000",29,"Oprawa słupowa (do montażu na słupie).","Światło odkryte.",null,"Pole luminaire with a classic design for general use. With appropriate accessories, it can be mounted on the corners of architectural structures as a wall lamp.",null,null,null,"Odlew aluminiowy malowany proszkowo.",null,null,null,null,"na ramieniu w górę","Ramię proste",null,"Moduł LED","Philips Fortimo DLM ES 1100/8xx G2 3K",null,null,null,null,80,"E","3010XX0010, 3040XX0009","PRZEWÓD H03VV-F 2x0,5 zaciski podłączeniowe, max 2x2,5mm². Przewód w oponie okrągłej o średnicy ø7...10,5mm.","4120XX0009.png","4120XX0009.ldt",4,null,1,9]
["4121","4121XX0009","LONDON POLE-TOP LED 1100LM 4000K ON/OFF","London,Big","Post,Head","Aluminium",null,null,null,"LED zintegrowane","AC","ON/OFF","9,5W","9,5W","1100lm","757lm",null,null,"54",null,"Class II",4000,"szerokie dół",0,0,0,"CE",null,null,"50000",29,"Oprawa słupowa (do montażu na słupie).","Światło odkryte.",null,"Pole luminaire with a classic design for general use. With appropriate accessories, it can be mounted on the corners of architectural structures as a wall lamp.",null,null,null,"Odlew aluminiowy malowany proszkowo.",null,null,null,null,"na ramieniu w górę","Ramię proste","Oprawa nieściemnialna","Moduł LED","Philips Fortimo DLM ES 1100/8xx G2 4K",null,null,null,null,80,"E","3010XX0010, 3040XX0009","PRZEWÓD H03VV-F 2x0,5 zaciski podłączeniowe, max 2x2,5mm². Przewód w oponie okrągłej o średnicy ø7...10,5mm.","4121XX0009.png","4121XX0009.ldt",4,null,1,9]
["4122","4122XX0009","LONDON LIGHT LUMINAIRES POLE LED 2000LM 3000K ON/OFF","London,Big","Post/Wall,Head","Aluminium",null,null,null,"LED zintegrowane","AC","ON/OFF","16,9W","14,6W","2000lm","1716lm",null,null,"65",null,"Class II",3000,null,0,0,0,"CE",null,null,"50000",20,"Oprawa słupowa (lekka konstrukcja).","Światło odkryte.",null,"A luminaire with a classic design for general use. Designed to be mounted on poles equipped with a terminal.",null,null,"Zestaw optyczny o IP67 (moduł LED i soczewka) ; zasilacz elektroniczny Wymienne (tylko LED) źródło światła przez profesjonalny serwis. Wymienny osprzęt sterujący za pomocą profesjonalnego serwisu.","Odlew aluminiowy malowany proszkowo.",null,null,null,null,"na ramieniu w górę big",null,"Oprawa nieściemnialna","Moduł LED","Philips Fortimo FastFlex LED 2x6 DP G4+ 3K","Philips Xi BP 12 W 0,1-0,5AS 230 V C100",100000,null,null,80,"E",null,"PRZEWÓD H03VV-F 2x0,5 zaciski podłączeniowe, max 2x2,5mm². Przewód w oponie okrągłej o średnicy ø7...10,5mm.","4122XX0009.png","4122XX0009.ldt",4,null,1,9]
["4126","4126XX0309","LONDON POLE LUMINAIRE. LED 2000LM 3000K ON/OFF","London,Big","Post,Post complete","Aluminium",null,null,null,"LED zintegrowane","AC","ON/OFF","19,6W","14,6W","2000lm","1716lm",null,null,"65",null,"Class II",3000,null,null,null,null,"CE",null,null,">120 000h",23,"Oprawa słupowa.","Światło odkryte.",null,"A luminaire with a classic design, mounted on a telescopic lighting pole with adjustable height of 1910...2790 mm For lighting gardens, parks and other architectural concepts.",null,null,"Moduł LED, zasilacz elektroniczny Zestaw optyczny o IP67 (moduł LED i soczewka) ; zasilacz elektroniczny","Odlew aluminiowy malowany proszkowo.",null,null,null,null,"Pojedyncze",null,"Oprawa nieściemnialna","Moduł LED","Philips Fortimo FastFlex LED 2x6 DP G4+ 3K","Philips Xi BP 12 W 0,1-0,5AS 230 V C100",100000,null,null,70,"D","305ZX0009, 306ZX0009","Zaciski podłączeniowe: max 4x2,5mm², możliwość podłączenia oprawy w pętle max 4x2,5mm². Przewód w oponie okrągłej o średnicy ø7...12,5mm.","4126XX0309.jpg","4126XX0309.ldt",4,null,1,9]
["4136","4136XX0009","LONDON WALL LED 1100LM 3000K","London,Big","Wall","Aluminium",null,null,null,"LED zintegrowane","AC",null,"9,5W","9,5W","1100lm","757lm",null,null,"54",null,"Class II",3000,null,0,0,0,"CE",null,null,"50000",12,"Oprawa ścienna.","Światło odkryte.",null,"A wall lamp luminaire with a classic design for general use. Can be mounted on the corners of architectural structures.",null,null,"Oprawa na wymienne źródło światła typu: lampa LED, tradycyjna żarówka (halogenowa) o trzonku E27. Źródło światła należy dokupić oddzielnie.","Odlew aluminiowy malowany proszkowo.",null,"Klosz- poliwęglan przeźroczysty, stabilizowany UV.",null,"Dławnica EPDM.","na ramieniu w dół big",null,null,"Moduł LED","Philips Fortimo DLM ES 1100/8xx G2 3K",null,0,null,null,80,"E","152XX0009","PRZEWÓD H03VV-F 2x0,5 zaciski podłączeniowe, zaciski podłączeniowe, max 2x2,5mm². Przewód w oponie okrągłej o średnicy ø7...10,5mm.","4136XX0009.jpg","4136XX0009.ldt",4,null,1,9]
["4140","4140XX0009","LONDON CEILING-CHAIN 110CM LED 1950LM 3000K ON/OFF","London,Big","Ceiling","Aluminium",null,null,null,"LED zintegrowane","AC","ON/OFF","17,5W","17,5W","1950lm","1392lm",null,null,"65",null,"Class II",3000,null,null,null,null,"CE",null,null,"50000",16,"Oprawa wisząca.","Światło odkryte.",null,"A luminaire on a chain with a classic design. For lighting gardens, terraces and other architectural concepts",null,null,"Moduł LED, zasilacz elektroniczny Wymienne źródło światła przez profesjonalny serwis. Wymienny osprzęt sterujący za pomocą profesjonalnego serwisu.","Odlew aluminiowy malowany proszkowo.",null,null,null,null,"110cm","big",null,"Moduł LED","Philips Fortimo DLM ES 2000/8xx G2 3K",null,null,null,null,80,"E",null,"Zaciski podłączeniowe, max 2x2,5mm². Przewód w oponie okrągłej o średnicy ø5...12mm.","4140XX0009.jpg","4140XX0009.ldt",4,null,1,9]
["4300","4300XX0009","ASKER POLE-TOP LED 2904LM SCL 3000K DALI2","Asker","Pole","Aluminium",null,null,"PRO","LED zintegrowane","AC","DALI2","16,8W","19,5W","2904lm","2624lm",null,null,"65",null,"Class I",3000,"szerokie dół",0.47,0.11,7.0000000000000007E-2,"CE",null,"DALI",">100 000h",2,"Oprawa słupowa (nasadzana).","Soczewka firmy Ledil typu SCL (IESNA typ II / III).","SCL","Pole luminaire with a modern design. Mounted, intended for mounting on a lighting pole with a mounting base of Ø50, Ø60, Ø76 using an appropriate head (accessory)","Mounted luminaire, intended for mounting on a lighting pole with a mounting base of Ø50mm; Ø60mm; Ø76mm Wide, even light distribution. The luminaire is also suitable for direct voltage: DC 168 ÷ 275 V","DC",null,"Profil aluminiowy wyciskany, malowany proszkowo.",null,"Soczewka hermetyczna zewnętrzna- tworzywo sztuczne PC przeźroczyste.",null,null,null,null,"Sterowanie światłem w systemie: DALI outdoor pełny program. Zasilacz zaprogramowany na max prąd. Programowanie pozostałych parametrów po uzgodnieniu z Działem Handlowym firmy Norlys.","Moduł LED","Philips Fortimo FastFlex LED 2x6 DP G5 3K","Philips Xi FP 22W 0,2-0,7A SNLDAE 230V S175 sXt",100000,"DALI2 / NightDim (XI FP NLD)",null,70,"D",null,"Podłączenie wewnątrz oprawy - zalecany przewód H05BQ-F 5G1 o długości odpowiedniej dla zastosowanego słupa - nie dołączony.","4300XX0009.jpg","4300XX0009.ldt",3,null,1,46]
["4301","4301XX0009","ASKER POLE-TOP LED 3036LM SCL 4000K DALI2","Asker","Pole","Aluminium",null,null,"PRO","LED zintegrowane","AC","DALI2","16,8W","19,5W","3036lm","2742lm",null,null,"65",null,"Class I",4000,"szerokie dół",0.47,0.11,7.0000000000000007E-2,"CE",null,"DALI",">100 000h",2,"Oprawa słupowa (nasadzana).","Soczewka firmy Ledil typu SCL (IESNA typ II / III).","SCL","Pole luminaire with a modern design. Mounted, intended for mounting on a lighting pole with a mounting base of Ø 50, Ø 60, Ø 76 using an appropriate head (accessory)","Mounted luminaire, intended for mounting on a lighting pole with a mounting base of Ø50mm; Ø60mm; Ø76mm Wide, even light distribution. The luminaire is also suitable for direct voltage: DC 168 ÷ 275 V","DC",null,"Profil aluminiowy wyciskany, malowany proszkowo.",null,"Soczewka hermetyczna zewnętrzna- tworzywo sztuczne PC przeźroczyste.",null,null,null,null,"Sterowanie światłem w systemie: DALI outdoor pełny program. Zasilacz zaprogramowany na max prąd. Programowanie pozostałych parametrów po uzgodnieniu z Działem Handlowym firmy Norlys.","Moduł LED","Philips Fortimo FastFlex LED 2x6 DP G5 4K","Philips Xi FP 22W 0,2-0,7A SNLDAE 230V S175 sXt",100000,"DALI2 / NightDim (XI FP NLD)",null,70,"D",null,"Podłączenie wewnątrz oprawy - zalecany przewód H05BQ-F 5G1 o długości odpowiedniej dla zastosowanego słupa - nie dołączony","4301XX0009.jpg","4301XX0009.ldt",3,null,1,46]
["4302","4302XX0009","ASKER POLE-TOP LED 2904LM VSM 3000K DALI2","Asker","Pole","Aluminium",null,null,"PRO","LED zintegrowane","AC","DALI2","16,8W","19,6W","2904lm","2711lm",null,null,"65",null,"Class I",3000,"szerokie dół",0.47,0.11,7.0000000000000007E-2,"CE",null,"DALI",">100 000h",2,"Oprawa słupowa (nasadzana).","Soczewka firmy Ledil typu VSM (IESNA typ V).","VSM","Pole luminaire with a modern design. Mounted, intended for mounting on a lighting pole with a mounting base of Ø 50, Ø 60, Ø 76 using an appropriate head (accessory)","Mounted luminaire, intended for mounting on a lighting pole with a mounting base of Ø50mm; Ø60mm; Ø76mm Wide, even light distribution. The luminaire is also suitable for direct voltage: DC 168 ÷ 275 V","DC",null,"Profil aluminiowy wyciskany, malowany proszkowo.",null,"Soczewka hermetyczna zewnętrzna- tworzywo sztuczne PC przeźroczyste.",null,null,null,null,"Sterowanie światłem w systemie: DALI outdoor pełny program. Zasilacz zaprogramowany na max prąd. Programowanie pozostałych parametrów po uzgodnieniu z Działem Handlowym firmy Norlys.","Moduł LED","Philips Fortimo FastFlex LED 2x6 DP G5 3K","Philips Xi FP 22W 0,2-0,7A SNLDAE 230V S175 sXt",100000,"DALI2 / NightDim (XI FP NLD)",null,70,"D",null,"Podłączenie wewnątrz oprawy - zalecany przewód H05BQ-F 5G1 o długości odpowiedniej dla zastosowanego słupa - nie dołączony.","4302XX0009.jpg","4302XX0009.ldt",3,null,1,47]
["4303","4303XX0009","ASKER POLE-TOP LED 3036LM VSM 4000K DALI2","Asker","Pole","Aluminium",null,null,"PRO","LED zintegrowane","AC","DALI2","16,8W","19,5W","3036lm","2832lm",null,null,"65",null,"Class I",4000,"szerokie dół",0.47,0.11,7.0000000000000007E-2,"CE",null,"DALI",">120 000h",2,"Oprawa słupowa (nasadzana).","Soczewka firmy Ledil typu VSM (IESNA typ V).","VSM","Pole luminaire with a modern design. Mounted, intended for mounting on a lighting pole with a mounting base of Ø 50, Ø 60, Ø 76 using an appropriate head (accessory)","Mounted luminaire, intended for mounting on a lighting pole with a mounting base of Ø50mm; Ø60mm; Ø76mm Wide, even light distribution. The luminaire is also suitable for direct voltage: DC 168 ÷ 275 V","DC",null,"Profil aluminiowy wyciskany, malowany proszkowo.",null,"Soczewka hermetyczna zewnętrzna- tworzywo sztuczne PC przeźroczyste.",null,null,null,null,"Sterowanie światłem w systemie: DALI outdoor pełny program. Zasilacz zaprogramowany na max prąd. Programowanie pozostałych parametrów po uzgodnieniu z Działem Handlowym firmy Norlys.","Moduł LED","Philips Fortimo FastFlex LED 2x6 DP G5 4K","Philips Xi FP 22W 0,2-0,7A SNLDAE 230V S175 sXt",100000,"DALI2 / NightDim (XI FP NLD)",null,70,"D",null,"Podłączenie wewnątrz oprawy - zalecany przewód H05BQ-F 5G1 o długości odpowiedniej dla zastosowanego słupa - nie dołączony","4303XX0009.jpg","4303XX0009.ldt",3,null,1,47]
["4310","4310XX0009","ASKER POLE-TOP LED 6051LM SCL 3000K DALI2","Asker","Pole","Aluminium",null,null,"PRO","LED zintegrowane","AC","DALI2","35,6W","39,8W","6051lm","5457lm",null,null,"65",null,"Class I",3000,"szerokie dół",0.47,0.11,7.0000000000000007E-2,"CE",null,"DALI",">100 000h",2,"Oprawa słupowa (nasadzana).","Soczewka firmy Ledil typu SCL (IESNA typ II / III).","SCL","Pole luminaire with a modern design. Mounted, intended for mounting on a lighting pole with a mounting base of Ø50, Ø60, Ø76 using an appropriate head (accessory)","Mounted luminaire, intended for mounting on a lighting pole with a mounting base of Ø50mm; Ø60mm; Ø76mm Wide, even light distribution. The luminaire is also suitable for direct voltage: DC 168 ÷ 275 V","DC",null,"Profil aluminiowy wyciskany, malowany proszkowo.",null,"Klosz- poliwęglan przeźroczysty, stabilizowany UV.",null,null,null,null,"Sterowanie światłem w systemie: DALI outdoor pełny program. Zasilacz zaprogramowany na max prąd. Programowanie pozostałych parametrów po uzgodnieniu z Działem Handlowym firmy Norlys.","Moduł LED","Philips Fortimo FastFlex LED 2x6 DP G5 3K","Philips Xi FP 40W 0.2-0.7A SNLDAE 230V S175 929000989206",100000,"DALI2 / NightDim (XI FP NLD)",null,70,"D",null,"Podłączenie wewnątrz oprawy - zalecany przewód H05BQ-F 5G1 o długości odpowiedniej dla zastosowanego słupa - nie dołączony.","4310XX0009.jpg","4310XX0009.ldt",3,null,1,46]
["4311","4311XX0009","ASKER POLE-TOP LED 6342LM SCL 4000K DALI2","Asker","Pole","Aluminium",null,null,"PRO","LED zintegrowane","AC","DALI2","35,6W","39,8W","6342lm","5723lm",null,null,"65",null,"Class I",4000,"szerokie dół",0.47,0.11,7.0000000000000007E-2,"CE",null,"DALI",">120 000h",2,"Oprawa słupowa (nasadzana).","Soczewka firmy Ledil typu SCL (IESNA typ II / III).","SCL","Pole luminaire with a modern design. Mounted, intended for mounting on a lighting pole with a mounting base of Ø50, Ø60, Ø76 using an appropriate head (accessory)","Mounted luminaire, intended for mounting on a lighting pole with a mounting base of Ø50mm; Ø60mm; Ø76mm Wide, even light distribution. The luminaire is also suitable for direct voltage: DC 168 ÷ 275 V","DC",null,"Profil aluminiowy wyciskany, malowany proszkowo.",null,"Soczewka hermetyczna zewnętrzna- tworzywo sztuczne PC przeźroczyste.",null,null,null,null,"Sterowanie światłem w systemie: DALI outdoor pełny program. Zasilacz zaprogramowany na max prąd. Programowanie pozostałych parametrów po uzgodnieniu z Działem Handlowym firmy Norlys.","Moduł LED","Philips Fortimo FastFlex LED 2x6 DP G5 4K","Philips Xi FP 40W 0.2-0.7A SNLDAE 230V S175 929000989206",100000,"DALI2 / NightDim (XI FP NLD)",null,70,"D",null,"Podłączenie wewnątrz oprawy - zalecany przewód H05BQ-F 5G1 o długości odpowiedniej dla zastosowanego słupa - nie dołączony","4311XX0009.jpg","4311XX0009.ldt",3,null,1,46]
["4312","4312XX0009","ASKER POLE-TOP LED 6051LM VSM 3000K DALI2","Asker","Pole","Aluminium",null,null,"PRO","LED zintegrowane","AC","DALI2","35,6W","39,8W","6051lm","5732lm",null,null,"65",null,"Class I",3000,"szerokie dół",0.47,0.11,7.0000000000000007E-2,"CE",null,"DALI",">100 000h",2,"Oprawa słupowa (nasadzana).","Soczewka firmy Ledil typu VSM (IESNA typ V).","VSM","Pole luminaire with a modern design. Mounted, intended for mounting on a lighting pole with a mounting base of Ø50, Ø60, Ø76 using an appropriate head (accessory)","Mounted luminaire, intended for mounting on a lighting pole with a mounting base of Ø50mm; Ø60mm; Ø76mm Wide, even light distribution. The luminaire is also suitable for direct voltage: DC 168 ÷ 275 V","DC",null,"Profil aluminiowy wyciskany, malowany proszkowo.",null,"Soczewka hermetyczna zewnętrzna- tworzywo sztuczne PC przeźroczyste.",null,null,null,null,"Sterowanie światłem w systemie: DALI outdoor pełny program. Zasilacz zaprogramowany na max prąd. Programowanie pozostałych parametrów po uzgodnieniu z Działem Handlowym firmy Norlys.","Moduł LED","Philips Fortimo FastFlex LED 2x6 DP G5 3K","Philips Xi FP 40W 0.2-0.7A SNLDAE 230V S175 929000989206",100000,"DALI2 / NightDim (XI FP NLD)",null,70,"D",null,"Podłączenie wewnątrz oprawy - zalecany przewód H05BQ-F 5G1 o długości odpowiedniej dla zastosowanego słupa - nie dołączony.","4312XX0009.jpg","4312XX0009.ldt",3,null,1,47]
["4313","4313XX0009","ASKER POLE-TOP LED 6342LM VSM 4000K DALI2","Asker","Pole","Aluminium",null,null,"PRO","LED zintegrowane","AC","DALI2","35,6W","39,8W","6342lm","6015lm",null,null,"65",null,"Class I",4000,"szerokie dół",0.47,0.11,7.0000000000000007E-2,"CE",null,"DALI",">120 000h",2,"Oprawa słupowa (nasadzana).","Soczewka firmy Ledil typu VSM (IESNA typ V).","VSM","Pole luminaire with a modern design. Mounted, intended for mounting on a lighting pole with a mounting base of Ø50, Ø60, Ø76 using an appropriate head (accessory)","Mounted luminaire, intended for mounting on a lighting pole with a mounting base of Ø50mm; Ø60mm; Ø76mm Wide, even light distribution. The luminaire is also suitable for direct voltage: DC 168 ÷ 275 V","DC",null,"Profil aluminiowy wyciskany, malowany proszkowo.",null,"Soczewka hermetyczna zewnętrzna- tworzywo sztuczne PC przeźroczyste.",null,null,null,null,"Sterowanie światłem w systemie: DALI outdoor pełny program. Zasilacz zaprogramowany na max prąd. Programowanie pozostałych parametrów po uzgodnieniu z Działem Handlowym firmy Norlys.","Moduł LED","Philips Fortimo FastFlex LED 2x6 DP G5 4K","Philips Xi FP 40W 0.2-0.7A SNLDAE 230V S175 929000989206",100000,"DALI2 / NightDim (XI FP NLD)",null,70,"D",null,"Podłączenie wewnątrz oprawy - zalecany przewód H05BQ-F 5G1 o długości odpowiedniej dla zastosowanego słupa - nie dołączony","4313XX0009.jpg","4313XX0009.ldt",3,null,1,47]
["4322","4322XX0309","ASKER HEAD POLE-TOP LED 2904LM SCL 3000K DALI2","Asker","Pole","Aluminium",null,null,"PRO","LED zintegrowane","AC","DALI2","16,8W","19,5W","2904lm","2624lm",null,null,"65",null,"Class I",3000,"szerokie dół",0.47,0.11,7.0000000000000007E-2,"CE",null,"DALI",">100 000h",2,"Oprawa słupowa (nasadzana).","Soczewka firmy Ledil typu SCL (IESNA typ II / III).","SCL","Pole luminaire with a modern design. Intended for mounting on a lighting pole with a Ø 60 mounting shaft","Mounted luminaire, intended for mounting on a lighting pole with a Ø60mm mounting shaft. Wide and even light distribution. The luminaire is also suitable for direct voltage: DC 168 ÷ 275 V","DC",null,"Profil aluminiowy wyciskany, malowany proszkowo.",null,"Soczewka hermetyczna zewnętrzna- tworzywo sztuczne PC przeźroczyste.",null,null,"Ø60",null,"Sterowanie światłem w systemie: DALI outdoor pełny program. Zasilacz zaprogramowany na max prąd. Programowanie pozostałych parametrów po uzgodnieniu z Działem Handlowym firmy Norlys.","Moduł LED","Philips Fortimo FastFlex LED 2x6 DP G5 3K","Philips Xi FP 22W 0,2-0,7A SNLDAE 230V S175 sXt",100000,"DALI2 / NightDim (XI FP NLD)",null,70,"D",null,"Podłączenie wewnątrz oprawy - zalecany przewód H05BQ-F 5G1 o długości odpowiedniej dla zastosowanego słupa - nie dołączony.","4322XX0309.jpg","4322XX0309.ldt",3,null,1,46]
["4323","4323XX0309","ASKER HEAD POLE-TOP LED 3036LM SCL 4000K DALI2","Asker","Pole","Aluminium",null,null,"PRO","LED zintegrowane","AC","DALI2","16,8W","19,5W","3036lm","2742lm",null,null,"65",null,"Class I",4000,"szerokie dół",0.47,0.11,7.0000000000000007E-2,"CE",null,"DALI",">100 000h",2,"Oprawa słupowa (nasadzana).","Soczewka firmy Ledil typu SCL (IESNA typ II / III).","SCL","Pole luminaire with a modern design. Intended for mounting on a lighting pole with a Ø 60 mounting shaft","Mounted luminaire, intended for mounting on a lighting pole with a Ø60mm mounting shaft. Wide and even light distribution. The luminaire is also suitable for direct voltage: DC 168 ÷ 275 V","DC",null,"Profil aluminiowy wyciskany, malowany proszkowo.",null,"Soczewka hermetyczna zewnętrzna- tworzywo sztuczne PC przeźroczyste.",null,null,"Ø60",null,"Sterowanie światłem w systemie: DALI outdoor pełny program. Zasilacz zaprogramowany na max prąd. Programowanie pozostałych parametrów po uzgodnieniu z Działem Handlowym firmy Norlys.","Moduł LED","Philips Fortimo FastFlex LED 2x6 DP G5 4K","Philips Xi FP 22W 0,2-0,7A SNLDAE 230V S175 sXt",100000,"DALI2 / NightDim (XI FP NLD)",null,70,"D",null,"Podłączenie wewnątrz oprawy - zalecany przewód H05BQ-F 5G1 o długości odpowiedniej dla zastosowanego słupa - nie dołączony","4323XX0309.jpg","4323XX0309.ldt",3,null,1,46]
["4332","4332XX0309","ASKER HEAD POLE-TOP LED 6051LM SCL 3000K DALI2","Asker","Pole","Aluminium",null,null,"PRO","LED zintegrowane","AC","DALI2","35,6W","39,8W","6051lm","5457lm",null,null,"65",null,"Class I",3000,"szerokie dół",0.47,0.11,7.0000000000000007E-2,"CE",null,"DALI",">100 000h",2,"Oprawa słupowa (nasadzana).","Soczewka firmy Ledil typu SCL (IESNA typ II / III).","SCL","Pole luminaire with a modern design. Intended for mounting on a lighting pole with a Ø 60 mounting shaft","Mounted luminaire, intended for mounting on a lighting pole with a Ø60mm mounting shaft. Wide and even light distribution. The luminaire is also suitable for direct voltage: DC 168 ÷ 275 V","DC",null,"Profil aluminiowy wyciskany, malowany proszkowo.",null,"Klosz- poliwęglan przeźroczysty, stabilizowany UV.",null,null,"Ø60",null,"Sterowanie światłem w systemie: DALI outdoor pełny program. Zasilacz zaprogramowany na max prąd. Programowanie pozostałych parametrów po uzgodnieniu z Działem Handlowym firmy Norlys.","Moduł LED","Philips Fortimo FastFlex LED 2x6 DP G5 3K","Philips Xi FP 40W 0.2-0.7A SNLDAE 230V S175 929000989206",100000,"DALI2 / NightDim (XI FP NLD)",null,70,"D",null,"Podłączenie wewnątrz oprawy - zalecany przewód H05BQ-F 5G1 o długości odpowiedniej dla zastosowanego słupa - nie dołączony.","4332XX0309.jpg","4332XX0309.ldt",3,null,1,46]
["4333","4333XX0309","ASKER HEAD POLE-TOP LED 6342LM SCL 4000K DALI2","Asker","Pole","Aluminium",null,null,"PRO","LED zintegrowane","AC","DALI2","35,6W","39,8W","6342lm","5723lm",null,null,"65",null,"Class I",4000,"szerokie dół",0.47,0.11,7.0000000000000007E-2,"CE",null,"DALI",">120 000h",2,"Oprawa słupowa (nasadzana).","Soczewka firmy Ledil typu SCL (IESNA typ II / III).","SCL","Pole luminaire with a modern design. Intended for mounting on a lighting pole with a Ø 60 mounting shaft","Mounted luminaire, intended for mounting on a lighting pole with a Ø60mm mounting shaft. Wide and even light distribution. The luminaire is also suitable for direct voltage: DC 168 ÷ 275 V","DC",null,"Profil aluminiowy wyciskany, malowany proszkowo.",null,"Soczewka hermetyczna zewnętrzna- tworzywo sztuczne PC przeźroczyste.",null,null,"Ø60",null,"Sterowanie światłem w systemie: DALI outdoor pełny program. Zasilacz zaprogramowany na max prąd. Programowanie pozostałych parametrów po uzgodnieniu z Działem Handlowym firmy Norlys.","Moduł LED","Philips Fortimo FastFlex LED 2x6 DP G5 4K","Philips Xi FP 40W 0.2-0.7A SNLDAE 230V S175 929000989206",100000,"DALI2 / NightDim (XI FP NLD)",null,70,"D",null,"Podłączenie wewnątrz oprawy - zalecany przewód H05BQ-F 5G1 o długości odpowiedniej dla zastosowanego słupa - nie dołączony","4333XX0309.jpg","4333XX0309.ldt",3,null,1,46]
["4362","4362XX0309","ASKER HEAD POLE-TOP LED 2904LM VSM 3000K DALI2","Asker","Pole","Aluminium",null,null,"PRO","LED zintegrowane","AC","DALI2","16,8W","19,6W","2904lm","2711lm",null,null,"65",null,"Class I",3000,"szerokie dół",0.47,0.11,7.0000000000000007E-2,"CE",null,"DALI",">100 000h",2,"Oprawa słupowa (nasadzana).","Soczewka firmy Ledil typu VSM (IESNA typ V).","VSM","Pole luminaire with a modern design. Intended for mounting on a lighting pole with a Ø 60 mounting shaft","Mounted luminaire, intended for mounting on a lighting pole with a Ø60mm mounting shaft. Wide and even light distribution. The luminaire is also suitable for direct voltage: DC 168 ÷ 275 V","DC",null,"Profil aluminiowy wyciskany, malowany proszkowo.",null,"Soczewka hermetyczna zewnętrzna- tworzywo sztuczne PC przeźroczyste.",null,null,"Ø60",null,"Sterowanie światłem w systemie: DALI outdoor pełny program. Zasilacz zaprogramowany na max prąd. Programowanie pozostałych parametrów po uzgodnieniu z Działem Handlowym firmy Norlys.","Moduł LED","Philips Fortimo FastFlex LED 2x6 DP G5 3K","Philips Xi FP 22W 0,2-0,7A SNLDAE 230V S175 sXt",100000,"DALI2 / NightDim (XI FP NLD)",null,70,"D",null,"Podłączenie wewnątrz oprawy - zalecany przewód H05BQ-F 5G1 o długości odpowiedniej dla zastosowanego słupa - nie dołączony.","4362XX0309.jpg","4362XX0309.ldt",3,null,1,47]
["4363","4363XX0309","ASKER HEAD POLE-TOP LED 3036LM VSM 4000K DALI2","Asker","Pole","Aluminium",null,null,"PRO","LED zintegrowane","AC","DALI2","16,8W","19,5W","3036lm","2832lm",null,null,"65",null,"Class I",4000,"szerokie dół",0.47,0.11,7.0000000000000007E-2,"CE",null,"DALI",">120 000h",2,"Oprawa słupowa (nasadzana).","Soczewka firmy Ledil typu VSM (IESNA typ V).","VSM","Pole luminaire with a modern design. Intended for mounting on a lighting pole with a Ø 60 mounting shaft","Mounted luminaire, intended for mounting on a lighting pole with a Ø60mm mounting shaft. Wide and even light distribution. The luminaire is also suitable for direct voltage: DC 168 ÷ 275 V","DC",null,"Profil aluminiowy wyciskany, malowany proszkowo.",null,"Soczewka hermetyczna zewnętrzna- tworzywo sztuczne PC przeźroczyste.",null,null,"Ø60",null,"Sterowanie światłem w systemie: DALI outdoor pełny program. Zasilacz zaprogramowany na max prąd. Programowanie pozostałych parametrów po uzgodnieniu z Działem Handlowym firmy Norlys.","Moduł LED","Philips Fortimo FastFlex LED 2x6 DP G5 4K","Philips Xi FP 22W 0,2-0,7A SNLDAE 230V S175 sXt",100000,"DALI2 / NightDim (XI FP NLD)",null,70,"D",null,"Podłączenie wewnątrz oprawy - zalecany przewód H05BQ-F 5G1 o długości odpowiedniej dla zastosowanego słupa - nie dołączony","4363XX0309.jpg","4363XX0309.ldt",3,null,1,47]
["4372","4372XX0309","ASKER HEAD POLE-TOP LED 6051LM VSM 3000K DALI2","Asker","Pole","Aluminium",null,null,"PRO","LED zintegrowane","AC","DALI2","35,6W","39,8W","6051lm","5732lm",null,null,"65",null,"Class I",3000,"szerokie dół",0.47,0.11,7.0000000000000007E-2,"CE",null,"DALI",">100 000h",2,"Oprawa słupowa (nasadzana).","Soczewka firmy Ledil typu VSM (IESNA typ V).","VSM","Pole luminaire with a modern design. Intended for mounting on a lighting pole with a Ø 60 mounting shaft","Mounted luminaire, intended for mounting on a lighting pole with a Ø60mm mounting shaft. Wide and even light distribution. The luminaire is also suitable for direct voltage: DC 168 ÷ 275 V","DC",null,"Profil aluminiowy wyciskany, malowany proszkowo.",null,"Soczewka hermetyczna zewnętrzna- tworzywo sztuczne PC przeźroczyste.",null,null,"Ø60",null,"Sterowanie światłem w systemie: DALI outdoor pełny program. Zasilacz zaprogramowany na max prąd. Programowanie pozostałych parametrów po uzgodnieniu z Działem Handlowym firmy Norlys.","Moduł LED","Philips Fortimo FastFlex LED 2x6 DP G5 3K","Philips Xi FP 40W 0.2-0.7A SNLDAE 230V S175 929000989206",100000,"DALI2 / NightDim (XI FP NLD)",null,70,"D",null,"Podłączenie wewnątrz oprawy - zalecany przewód H05BQ-F 5G1 o długości odpowiedniej dla zastosowanego słupa - nie dołączony.","4372XX0309.jpg","4372XX0309.ldt",3,null,1,47]
["4373","4373XX0309","ASKER HEAD POLE-TOP LED 6342LM VSM 4000K DALI2","Asker","Pole","Aluminium",null,null,"PRO","LED zintegrowane","AC","DALI2","35,6W","39,8W","6342lm","6015lm",null,null,"65",null,"Class I",4000,"szerokie dół",0.47,0.11,7.0000000000000007E-2,"CE",null,"DALI",">120 000h",2,"Oprawa słupowa (nasadzana).","Soczewka firmy Ledil typu VSM (IESNA typ V).","VSM","Pole luminaire with a modern design. Intended for mounting on a lighting pole with a Ø 60 mounting shaft","Mounted luminaire, intended for mounting on a lighting pole with a Ø60mm mounting shaft. Wide and even light distribution. The luminaire is also suitable for direct voltage: DC 168 ÷ 275 V","DC",null,"Profil aluminiowy wyciskany, malowany proszkowo.",null,"Soczewka hermetyczna zewnętrzna- tworzywo sztuczne PC przeźroczyste.",null,null,"Ø60",null,"Sterowanie światłem w systemie: DALI outdoor pełny program. Zasilacz zaprogramowany na max prąd. Programowanie pozostałych parametrów po uzgodnieniu z Działem Handlowym firmy Norlys.","Moduł LED","Philips Fortimo FastFlex LED 2x6 DP G5 4K","Philips Xi FP 40W 0.2-0.7A SNLDAE 230V S175 929000989206",100000,"DALI2 / NightDim (XI FP NLD)",null,70,"D",null,"Podłączenie wewnątrz oprawy - zalecany przewód H05BQ-F 5G1 o długości odpowiedniej dla zastosowanego słupa - nie dołączony","4373XX0309.jpg","4373XX0309.ldt",3,null,1,47]
["450","450XX0009","VASA WALL LED 799LM DOWN 3000K DIM.","Vasa","Wall","Aluminium",null,null,null,"LED zintegrowane","AC","DIM.","4,2W","6W","799lm","440lm",null,null,"65","IK08","Class I",3000,"szerokie dół",0.31,0.12,0.16,"CE",null,null,"> 102 000h",12,"Oprawa ścienna.","Światło rozproszone półsferyczne ukierunkowane w dół",null,"A luminaire with a wide range of applications, including lighting: wall surfaces and other architectural concepts",null,null,null,"Odlew aluminiowy malowany proszkowo.",null,"Klosz- poliwęglan przeźroczysty ze strukturą, stabilizowany UV.","Uszczelka silikonowa.","Dławnica EPDM.",null,null,"Oprawa ściemnialna fazowo TRAILING EDGE (TE) - LEADING EDGE (LE)","Moduł LED","Cree DK200305 V3 JB2835 3V 3K","KGP CC10W200-350CG",50000,"Dim. TRIAC (KGP)",null,80,"C",null,"Zaciski podłączeniowe: max 3x2,5mm², możliwość podłączenia oprawy w pętle max 3x1,5mm². Przewód w oponie okrągłej o średnicy ø7...10,5mm.","450XX0009.png","450XX0009.ldt",1,null,1,76]
["454","454XX0009","VASA WALL LED 799LM UP 3000K DIM.","Vasa","Wall","Aluminium",null,null,null,"LED zintegrowane","AC","DIM.","4,2W","6W","799lm","440lm",null,null,"65","IK08","Class I",3000,"szerokie góra",0.31,0.12,0.16,"CE",null,null,"> 102 000h",12,"Oprawa ścienna.","Światło rozproszone półsferyczne ukierunkowane w górę",null,"A luminaire with a wide range of applications, including lighting: wall surfaces and other architectural concepts",null,null,null,"Odlew aluminiowy malowany proszkowo.",null,"Klosz- poliwęglan przeźroczysty ze strukturą, stabilizowany UV.","Uszczelka silikonowa.","Dławnica EPDM.",null,null,"Oprawa ściemnialna fazowo TRAILING EDGE (TE) - LEADING EDGE (LE)","Moduł LED","Cree DK200305 V3 JB2835 3V 3K","KGP CC10W200-350CG",50000,"Dim. TRIAC (KGP)",null,80,"C",null,"Zaciski podłączeniowe: max 3x2,5mm², możliwość podłączenia oprawy w pętle max 3x1,5mm². Przewód w oponie okrągłej o średnicy ø7...10,5mm.","454XX0009.jpg","454XX0009.ldt",1,null,1,78]
["5001","5001XX0016","NICE POLE-TOP LED 3092LM 4000K ON/OFF","Nice","Post,Head","Aluminium",null,null,null,"LED zintegrowane","AC","ON/OFF","33,9W","38W","3092lm","3092lm",null,null,"65",null,"Class I",4000,null,0.7,0.55000000000000004,0.55000000000000004,"CE",null,null,"> 110 000h",2,"Oprawa słupowa (nasadzana).","Światło symetryczne pośrednie.",null,"Top-mounted luminaire designed for mounting on a lighting pole with a Ø60mm mounting shaft",null,null,null,"Odlew aluminiowy malowany proszkowo.",null,"Klosz- szkło bezpieczne, przeźroczyste.","Uszczelka silikonowa.",null,null,null,"Oprawa nieściemnialna","Moduł LED","Philips Fortimo SLM C 1211 L19 2828 G7 4K","Philips Xitanium 36W/m 929001486006",0,null,6.8400000000000002E-2,80,"D","154XX0009, 3005XX0009, 7662ZX0009, 7664ZX0009, 7665XX0009","Przewód H05VV-F 3G1 o długości 4,5m do podłączenia wewnątrz słupa oświetleniowego (w odpowiednio dobranej puszce elektroinstalacyjnej).","5001XX0016.jpg","5001XX0016.ldt",4,null,1,21]
["5002","5002XX0309","VISBY POLE-TOP 2XLED 5200LM 4000K","Visby","Post,Head","Aluminium",null,null,null,"LED zintegrowane","AC",null,"44,5W","43,6W","5200lm","2624lm",null,null,"65",null,"Class I",4000,null,0,0,0,"CE",null,null,"50000",2,"Oprawa słupowa (nasadzana).","Światło obrotowo- symetryczne (kombinacja pośrednie/bezpośrednie).",null,"Pole top luminaire for installation on a lighting pole with Ø60mm mounting shaft.",null,null,"Oprawa wyposażona jest w wymienne źródło światła typu moduł LED, który zapewnia trwałość i optymalny rozsył światła, przy zachowaniu stosunkowo niskiego zużycia energii.","Odlew aluminiowy malowany proszkowo.",null,"Klosz- tworzywo sztuczne PMMA przeźroczyste.","Uszczelka silikonowa.",null,null,null,"Oprawa nieściemnialna","2 Moduły LED","Philips LED Fortimo DLM ES 2000/840 G2 / 3000/840 G2",null,0,null,null,80,null,"3005XX0009, 7660XX0009, 7662ZX0009, 7664ZX0009","Przewód H05VV-F 3G1 o długości 4,5m do podłączenia wewnątrz słupa oświetleniowego (w odpowiednio dobranej puszce elektroinstalacyjnej). Możliwość sterowania modułami LED (zał./wył.): świecenie modułu górnego i dolnego lub tylko modułu górnego (światło pośrednie, 3000lm/27W), lub tylko modułu dolnego (światło bezpośrednie, 2000lm/17,5W).","5002XX0309.jpg","5002XX0309.ldt",4,null,1,30]
["5003","5003XX0309","VISBY POLE-TOP LED 3150LM 4000K","Visby","Post,Head","Aluminium",null,null,null,"LED zintegrowane","AC",null,"27W","26,5W","3150lm","1553lm",null,null,"65",null,"Class I",4000,null,0,0,0,"CE",null,null,"50000",2,"Oprawa słupowa (nasadzana).","Światło obrotowo-symetryczne pośrednie.",null,"Pole top luminaire for installation on a lighting pole with Ø60mm mounting shaft.",null,null,"Oprawa wyposażona w wymienne źródło światła typu moduł LED, która zapewnia trwałość i optymalny rozsył światła, przy zachowaniu stosunkowo niskiego zużycia energii.","Odlew aluminiowy malowany proszkowo.",null,"Klosz- tworzywo sztuczne PMMA przeźroczyste.","Uszczelka silikonowa.",null,null,null,"Oprawa nieściemnialna","Moduł LED","Philips Fortimo LED DLM ES 3000/840 G2",null,0,null,3.15E-2,80,null,"3005XX0009, 7660XX0009, 7662ZX0009, 7664ZX0009","Przewód H05VV-F 3G1 o długości 4,5m do podłączenia wewnątrz słupa oświetleniowego (w odpowiednio dobranej puszcze elektroinstalacyjnej).","5003XX0309.jpg","5003XX0309.ldt",4,null,1,2]
["5004","5004XX0012","KOSTER WALL-ARM LED 2050LM 4000K ON/OFF","Koster","Wall","Aluminium",null,null,null,"LED zintegrowane","AC","ON/OFF","17,5W","17,5W","2050lm","1625lm",null,null,"54","IK10","Class I",4000,null,0,0,0,"CE",null,null,"50000",21,"Oprawa ścienna na ramieniu.","Światło jednostronne: symetryczne, ukierunkowane w dół.",null,"Classic type wall-mounted luminaire. Possibility to install on corners of architectural objects.",null,null,"Oprawa wyposażona w wymienne źródło światła typu moduł LED, która zapewnia trwałość i optymalny rozsył światła, przy zachowaniu stosunkowo niskiego zużycia energii.","Odlew aluminiowy malowany proszkowo.",null,"Klosz- poliwęglan przeźroczysty ze strukturą, stabilizowany UV.",null,null,null,null,"Oprawa nieściemnialna","Moduł LED","Philips Fortimo DLM ES 2000/8xx G2 4K",null,null,null,0,80,"D","158XX0009","Zaciski podłączeniowe: max 3x2,5mm², możliwość podłączenia oprawy w pętle max 3x1,5mm². Przewód w oponie okrągłej o średnicy ø7...10,5mm.","5004XX0012.jpg","5004XX0012.ldt",4,null,1,27]
["5006","5006XX0011","KOSTER POLE-TOP LED 2050LM 4000K","Koster","Post,Head","Aluminium",null,null,null,"LED zintegrowane","AC",null,"17,5W","17,5W","2050lm","1625lm",null,null,"54","IK10","Class I",4000,null,0.45,0.24,0.24,"CE",null,null,"50000",2,"Oprawa słupowa (nasadzana).","Światło jednostronne: symetryczne, ukierunkowane w dół.",null,"Luminaire mounted on a straight arm, for assembly on a telescopic lighting pole with a diameter of Ø60mm.",null,null,null,"Odlew aluminiowy malowany proszkowo.",null,"Klosz- poliwęglan przeźroczysty ze strukturą, stabilizowany UV.",null,null,"Ø60",null,"Oprawa nieściemnialna","Moduł LED","Philips Fortimo DLM ES 2000/8xx G2 4K",null,0,null,0,80,"D","3005XX0009, 7660XX0009, 7662ZX0009, 7664ZX0009","Przewód H05VV-F 3G1 o długości 3,7m do podłączenia wewnątrz słupa oświetleniowego (w odpowiednio dobranej puszce elektroinstalacyjnej).","5006XX0011.jpg","5006XX0011.ldt",4,null,1,27]
["5007","5007XX0309","KOSTER POLE-TOP LED 2050LM 4000K","Koster","Post,Post complete","Aluminium",null,null,null,"LED zintegrowane","AC",null,"17,5W","17,5W","2050lm","1625lm",null,null,"54","IK10","Class I",4000,null,0.45,0.24,0.24,"CE",null,null,"50000",2,"Oprawa słupowa (nasadzana).","Światło jednostronne: symetryczne, ukierunkowane w dół.",null,"Classic design luminaire, mounted on a telescopic lighting pole. Adjustable height 2360..3360mm.",null,null,"Oprawa wyposażona w wymienne źródło światła typu moduł LED, która zapewnia trwałość i optymalny rozsył światła, przy zachowaniu stosunkowo niskiego zużycia energii.","Odlew aluminiowy malowany proszkowo.",null,"Klosz- poliwęglan przeźroczysty ze strukturą, stabilizowany UV.",null,null,"Komplet ze słupem",null,"Oprawa nieściemnialna","Moduł LED","Philips Fortimo DLM ES 2000/8xx G2 4K",null,0,null,0,80,"D","111GA0009, 405ZX0009, 406ZX0009","Złącze podłączeniowe: na przewód max 3x2,5mm², wyposażone w bezpiecznik topikowy 1A 5x20. Przewód w oponie okrągłej o średnicy max ø12,5mm.","5007XX0309.jpg","5007XX0309.ldt",4,null,1,27]
["5008","5008XX0011","STAVANGER BOLLARD 95CM LED 1171LM 4000K DIM.","Stavanger","Bollard","Aluminium",null,null,null,"LED zintegrowane","AC","DIM.","9,6W","12,2W","1171lm","493lm",null,null,"65","IK10","Class I",4000,null,0.2,0.2,0.95,"CE",null,null,"50 000h",1,"Oprawa słupkowa.","Światło pośrednie, obrotowo- symetryczne, ukierunkowane w dół.",null,"Bollard luminaire of stable and durable construction For lighting private areas and public spaces",null,null,null,"Odlew aluminiowy malowany proszkowo.",null,"Klosz- poliwęglan przeźroczysty, stabilizowany UV.","Uszczelka silikonowa.","Dławnica nylon6.","95cm","przeźroczysty PC","Oprawa ściemnialna fazowo TRAILING EDGE (TE)","Moduł LED","Cree DK1305003 V2 XD16 4K","Philips Xitanium 10W 0,5A 20V TE SC",0,"Philips Xitanium TE",null,80,"E","1230ZX0009, 1231GA0009, 1232GA0009, 6139ZX0009, 7662ZX0009","Zaciski podłączeniowe: max 3x4mm², możliwość podłączenia oprawy w pętle max 3x2,5mm². Przewód w oponie okrągłej o średnicy ø8...17mm.","5008XX0011.jpg","5008XX0011.ldt",1,null,1,33]
["5009","5009XX0010","STAVANGER BOLLARD 50CM LED 1171LM 4000K DIM.","Stavanger","Bollard","Aluminium",null,null,null,"LED zintegrowane","AC","DIM.","9,6W","11,9W","1171lm","530lm",null,null,"65","IK10","Class I",4000,null,0.2,0.2,0.5,"CE",null,null,"50 000h",1,"Oprawa słupkowa.","Światło pośrednie, obrotowo- symetryczne, ukierunkowane w dół.",null,"Bollard luminaire of stable and durable construction. For lighting private areas and public spaces.",null,null,null,"Odlew aluminiowy malowany proszkowo.",null,"Klosz- poliwęglan przeźroczysty, stabilizowany UV.","Uszczelka silikonowa.","Dławnica nylon6.","50cm","przeźroczysty PC","Oprawa ściemnialna fazowo TRAILING EDGE (TE)","Moduł LED","Cree DK1305003 V2 XD16 4K","Philips Xitanium 10W 0,5A 20V TE SC 230V",0,"Philips Xitanium TE",null,80,"E","1230ZX0009, 1231GA0009, 1232GA0009","Zaciski podłączeniowe: max 5x4mm², możliwość podłączenia oprawy w pętle max 5x2,5mm². Przewód w oponie okrągłej o średnicy ø8...17mm. Oprawa wyposażona w otwory do zamontowania szyny montażowej TH-35, o długości 10cm.","5009XX0010.jpg","5009XX0010.ldt",1,null,1,33]
["5010","5010XX0011","STAVANGER BOLLARD 28CM LED 854LM 4000K DIM.","Stavanger","Bollard","Aluminium",null,null,null,"LED zintegrowane","AC","DIM.","6,6W","8,4W","854lm","351lm",null,null,"65","IK10","Class I",4000,null,0.2,0.2,0.28000000000000003,"CE",null,null,"50000",1,"Oprawa słupkowa.","Światło pośrednie, obrotowo- symetryczne, ukierunkowane w dół.",null,"Bollard luminaire of stable and durable construction. For lighting private areas and public spaces.",null,null,null,"Odlew aluminiowy malowany proszkowo.",null,"Klosz- poliwęglan przeźroczysty, stabilizowany UV.","Uszczelka silikonowa.","Dławnica nylon6.","28cm","przeźroczysty PC","Oprawa ściemnialna fazowo TRAILING EDGE (TE)","Moduł LED","Cree DK1305003 V2 XD16 4K","Philips Xitanium 7W 0.35A 20V TE SC 230V 12NC",0,"Philips Xitanium TE",2.5999999999999999E-2,80,"E","1230ZX0009, 1231GA0009, 1232GA0009","Zaciski podłączeniowe: max 3x2,5mm², możliwość podłączenia oprawy w pętle max 3x1,5mm². Przewód w oponie okrągłej o średnicy ø8...17mm.","5010XX0011.jpg","5010XX0011.ldt",1,null,1,33]
["5011","5011XX0016","NAMSOS WALL-RECESSED LED 1247LM 4000K DIM.","Namsos","Recessed","Aluminium",null,null,null,"LED zintegrowane","AC","DIM.","6,5W","8,6W","1247lm","612lm",null,null,"65","IK08","Class I",4000,null,0.22,0.22,0.12,"CE",null,null,"> 102 000h",11,"Oprawa wbudowana ścienna.","Światło rozproszone półsferyczne ukierunkowane w dół",null,"The luminaire is adapted to illuminate stairs, steps, staircases, pathways, ceiling lighting and implementation of other architectural concepts",null,null,null,"Odlew aluminiowy malowany proszkowo.",null,"Klosz- szkło bezpieczne, satynowane.","Uszczelka silikonowa.","Dławnica EPDM.",null,null,"Oprawa ściemnialna fazowo TRAILING EDGE (TE) - LEADING EDGE (LE)","Moduł LED","Cree DK200305 V3 JB2835 3V 4K","KGP CC10W200-350CG",50000,"Dim. TRIAC (KGP)",null,80,"C",null,"Zaciski podłączeniowe: max 3x2,5mm², możliwość podłączenia oprawy w pętle max 3x1,5mm². Przewód w oponie okrągłej o średnicy ø7...10,5mm.","5011XX0016.jpg","5011XX0016.ldt",1,null,1,76]
["5012","5012XX0014","NAMSOS BOLLARD 95CM LED 1247LM 4000K DIM.","Namsos","Bollard","Aluminium",null,null,null,"LED zintegrowane","AC","DIM.","6,5W","8,6W","1247lm","612lm","Szkło",null,"65","IK08","Class I",4000,null,0.24,0.12,0.95,"CE",null,null,"> 102 000h",1,"Oprawa słupkowa.","Światło rozproszone półsferyczne ukierunkowane w dół",null,"Luminaire with a modern design. For lighting gardens and other private and public areas",null,null,null,"Odlew aluminiowy malowany proszkowo.",null,"Klosz- szkło bezpieczne, satynowane.","Uszczelka silikonowa.","Dławnica EPDM.","95cm",null,"Oprawa ściemnialna fazowo TRAILING EDGE (TE) - LEADING EDGE (LE)","Moduł LED","Cree DK200305 V3 JB2835 3V 4K","KGP CC10W200-350CG",50000,"Dim. TRIAC (KGP)",null,80,"C","112ZX0009, 113GA0009, 114GA0009","Zaciski podłączeniowe: max 3x4mm², możliwość podłączenia oprawy w pętle max 3x4mm². Przewód w oponie okrągłej o średnicy: ø8...12mm lub ø10...14mm.","5012XX0014.jpg","5012XX0014.ldt",1,null,1,76]
["5013","5013XX0013","NAMSOS BOLLARD 65CM LED 1247LM 4000K DIM.","Namsos","Bollard","Aluminium",null,null,null,"LED zintegrowane","AC","DIM.","6,5W","8,6W","1247lm","612lm","Tworzywo sztuczne","Satynowany","65","IK08","Class I",4000,null,0.24,0.12,0.65,"CE",null,null,"> 102 000h",1,"Oprawa słupkowa.","Światło rozproszone półsferyczne ukierunkowane w dół",null,"Luminaire with a modern design. For lighting gardens and other private and public areas",null,null,null,"Odlew aluminiowy malowany proszkowo.",null,"Klosz- szkło bezpieczne, satynowane.","Uszczelka silikonowa.","Dławnica EPDM.","65cm",null,"Oprawa ściemnialna fazowo TRAILING EDGE (TE) - LEADING EDGE (LE)","Moduł LED","Cree DK200305 V3 JB2835 3V 4K","KGP CC10W200-350CG",50000,"Dim. TRIAC (KGP)",null,80,"C","112ZX0009, 113GA0009, 114GA0009","Zaciski podłączeniowe: max 3x4mm², możliwość podłączenia oprawy w pętle max 3x4mm². Przewód w oponie okrągłej o średnicy: ø8...12mm lub ø10...14mm.","5013XX0013.jpg","5013XX0013.ldt",1,null,1,76]
["5014","5014XX0013","EGERSUND BOLLARD 108CM LED 2655LM 4000K DIM.","Egersund","Bollard","Aluminium",null,null,null,"LED zintegrowane","AC","DIM.","18W","20,3W","2655lm","1782lm",null,null,"65","IK08","Class II",4000,null,0.2,0.2,1.08,"CE",null,null,"> 162 000h",1,"Oprawa słupkowa.","Światło obrotowo-symetryczne.",null,"Contemporary design luminaire. For lighting gardens and other private and public spaces",null,null,null,"Odlew aluminiowy malowany proszkowo.",null,"Klosz- tworzywo sztuczne PMMA przeźroczyste.","Uszczelka silikonowa.","Dławnica nylon6.","108cm",null,"Oprawa ściemnialna fazowo TRAILING EDGE (TE) - LEADING EDGE (LE)","Moduł LED","Cree DK201002 V1 JK3030 6V 4K","TCI Mini JOLLY 20W code 127556 Triac",0,null,null,80,"E","1230ZX0009, 1231GA0009, 1232GA0010","Zaciski podłączeniowe: max 2x4mm², możliwość podłączenia oprawy w pętle max 2x4mm². Przewód w oponie okrągłej o średnicy ø8...17mm.","5014XX0013.jpg","5014XX0013.ldt",1,null,1,17]
["5015","5015XX0012","EGERSUND BOLLARD 63CM LED 2655LM 4000K DIM.","Egersund","Bollard","Aluminium",null,null,null,"LED zintegrowane","AC","DIM.","18W","20W","2655lm","1782lm",null,null,"65","IK08","Class II",4000,null,0.2,0.2,0.63,"CE",null,null,"> 162 000h",1,"Oprawa słupkowa.","Światło obrotowo-symetryczne.",null,"Luminaire with a contemporary design. For lighting gardens and other private and public areas",null,null,null,"Odlew aluminiowy malowany proszkowo.",null,"Klosz- tworzywo sztuczne PMMA przeźroczyste.","Uszczelka silikonowa.","Dławnica nylon6.","63cm",null,"Oprawa ściemnialna fazowo TRAILING EDGE (TE) - LEADING EDGE (LE)","Moduł LED","Cree DK201002 V1 JK3030 6V 4K","TCI Mini JOLLY 20W code 127556 Triac",0,null,null,80,"D","1230ZX0009, 1231GA0009, 1232GA0010","Zaciski podłączeniowe: max 2x4mm², możliwość podłączenia oprawy w pętle max 2x4mm². Przewód w oponie okrągłej o średnicy ø8...17mm.","5015XX0012.jpg","5015XX0012.ldt",1,null,1,17]
["5016","5016XX0015","NORDLAND CEILING/WALL LED 594LM 4000K DIM.","Nordland","Wall,Ceiling","Aluminium",null,null,null,"LED zintegrowane","AC","DIM.","10W","9,6W","594lm","594lm",null,null,"65","IK10","Class I",4000,null,0.28000000000000003,0.28000000000000003,0.1,"CE",null,null,"50 000h",7,"Oprawa sufitowo-ścienna.","Światło rozproszone.",null,"A ceiling-type luminaire with a modern design For lighting private areas and other architectural concepts",null,null,null,"Odlew aluminiowy malowany proszkowo.",null,"Klosz- poliwęglan mleczny, stabilizowany UV.","Uszczelka silikonowa.","Dławnica EPDM.","NIE",null,"Oprawa ściemnialna fazowo TRAILING EDGE (TE) - LEADING EDGE (LE)","Moduł LED","Lumens DLM 100C 10W 840 230V F201 V0,5 4K",null,0,"Ściemnianie fazowe Lumens LED AC",null,80,"F",null,"Zaciski podłączeniowe: max 3x2,5mm², możliwość podłączenia oprawy w pętle max 3x1,5mm². Przewód w oponie okrągłej o średnicy ø7...10,5mm.","5016XX0015.jpg","5016XX0015.ldt",1,null,1,7]
["5018","5018XX0013","ASKER BIG WALL 2XLED 1188LM UP-DOWN 4000K DIM.","Asker,Big","Wall","Aluminium",null,null,null,"LED zintegrowane","AC","DIM.","6,6W","8,5W","1188lm","550lm",null,null,"65","IK08","Class I",4000,"szerokie góra / szerokie dół",0.3,0.12,0.12,"CE",null,null,"> 70 000h",12,"Oprawa ścienna.","Światło dwustronne: ukierunkowane do góry i w dół.","Up-Down","A luminaire with a wide range of applications, for illuminating wall surfaces, facades and other architectural concepts",null,null,null,"Odlew aluminiowy malowany proszkowo.",null,"Klosz- poliwęglan przeźroczysty ze strukturą, stabilizowany UV.","Uszczelka silikonowa.","Dławnica EPDM.","góra/dół",null,"Oprawa ściemnialna fazowo TRAILING EDGE (TE)","2 Moduły LED","Philips Fortimo Strip 0,5ft MF FC LV6 4K","Philips Xitanium 8W 0,2A 40V TE SC 230V",0,null,null,80,null,null,"Zaciski podłączeniowe: max 3x2,5mm², możliwość podłączenia oprawy w pętle max 3x1,5mm². Przewód w oponie okrągłej o średnicy ø7...10,5mm.","5018XX0013.jpg","5018XX0013.ldt",1,null,1,4]
["5019","5019XX0013","VASA WALL 2XLED 1188LM UP-DOWN 4000K DIM.","Vasa","Wall","Aluminium",null,null,null,"LED zintegrowane","AC","DIM.","6,6W","8,3W","1188lm","668lm",null,null,"65","IK08","Class I",4000,"szerokie góra / szerokie dół",null,null,null,"CE",null,null,"> 70 000",12,"Oprawa ścienna.","Światło dwustronne: ukierunkowane do góry i w dół.","Up-Down","A luminaire with a wide range of applications, for lighting: wall and facade surfaces and other architectural concepts",null,null,null,"Odlew aluminiowy malowany proszkowo.",null,"Klosz- poliwęglan przeźroczysty ze strukturą, stabilizowany UV.","Uszczelka silikonowa.","Dławnica EPDM.",null,null,"Oprawa ściemnialna fazowo TRAILING EDGE (TE)","2 Moduły LED","Philips Fortimo Strip 0,5ft MF FC LV6 4K","Philips Xitanium 8W 0,2A 40V TE SC 230V",0,null,null,80,"C",null,"Zaciski podłączeniowe: max 3x2,5mm², możliwość podłączenia oprawy w pętle max 3x1,5mm². Przewód w oponie okrągłej o średnicy ø7...10,5mm.","5019XX0013.jpg","5019XX0013.ldt",1,null,1,4]
["5020","5020XX0013","HALDEN WALL LED 1121LM DOWN 4000K DIM.","Halden","Wall","Aluminium",null,null,null,"LED zintegrowane","AC","DIM.","6,7W","8,5W","1121lm","690lm",null,null,"65","IK10","Class I",4000,null,3.1,1.55,1.5,"CE",null,null,">110 000",12,"Oprawa ścienna.","Światło rozproszone półsferyczne ukierunkowane w dół",null,"Luminaire with a wide range of applications for example for illumination of walls and facade surfaces or any other architectural concepts.",null,null,null,"Odlew aluminiowy malowany proszkowo.",null,"Klosz- poliwęglan przeźroczysty ze strukturą, stabilizowany UV.","Uszczelka silikonowa.","Dławnica EPDM.",null,null,"Oprawa ściemnialna fazowo TRAILING EDGE (TE)","Moduł LED","Philips Fortimo SLM C 1203 L09 1619 G7 4K","Philips Xitanium 8W 0,2A 40V TE SC 230V",0,null,0,80,"D",null,"Zaciski podłączeniowe: max 3x2,5mm², możliwość podłączenia oprawy w pętle max 3x1,5mm². Przewód w oponie okrągłej o średnicy ø7...10,5mm.","5020XX0013.jpg","5020XX0013.ldt",1,null,1,76]
["5021","5021XX0012","ALTA BOLLARD 85CM LED 1164LM 4000K DIM.","Alta","Bollard","Stal",null,null,null,"LED zintegrowane","AC","DIM.","10W","10,8W","1164lm","114lm",null,null,"65",null,"Class I",4000,null,0,0,0,"CE",null,null,"> 50 000h",1,"Oprawa słupkowa.","Światło obrotowo symetryczne przysłonięte od góry.",null,"A bollard luminaire with a stable and durable structure. For lighting private areas and public areas",null,null,null,"Stal cynkowana ogniowo.","Stal cynkowana ogniowo i malowana proszkowo.","Klosz- tworzywo sztuczne PMMA w kolorze mlecznym.","Uszczelka silikonowa.",null,"85cm",null,"Oprawa ściemnialna fazowo TRAILING EDGE (TE) - LEADING EDGE (LE)","Moduł LED","Lumens EDC 47C 10W xxx 230V A101 3K",null,null,"Ściemnianie fazowe Lumens LED AC",null,80,"E","205ZX0010, 206GA0010","Zaciski podłączeniowe: max 3x4mm², możliwość podłączenia oprawy w pętle max 3x2,5mm². Przewód w oponie okrągłej o średnicy max ø12,5mm.","5021XX0012.jpg","5021XX0012.ldt",1,null,1,1]
["5022","5022XX0013","HALMSTAD BOLLARD 85CM LED 1121LM 4000K DIM.","Halmstad","Bollard","Stal",null,null,null,"LED zintegrowane","AC","DIM.","6,7W","8,5W","1121lm","310lm",null,null,"65","IK10","Class II",4000,null,0,0,0,"CE",null,null,"> 50 000h",1,"Oprawa słupkowa.","Światło odkryte, częściowo przysłonięte od góry.",null,"A bollard luminaire with a stable and durable structure For lighting private areas and other architectural concepts",null,null,null,"Stal cynkowana ogniowo.",null,"Klosz- tworzywo sztuczne PMMA w kolorze mlecznym.","Uszczelka silikonowa.",null,"85cm",null,"Oprawa ściemnialna fazowo TRAILING EDGE (TE) - LEADING EDGE (LE)","Moduł LED","Philips Fortimo SLM C 1203 L09 1619 G7 4K","KGP CC10W180-270CG",50000,"Dim. TRIAC (KGP)",null,80,"D","205ZX0010, 206GA0010, 206GA0S10, 2951ZX0009, 6138ZX0009","Zaciski podłączeniowe: max 2x4mm², możliwość podłączenia oprawy w pętle max 2x2,5mm². Przewód w oponie okrągłej o średnicy max ø12,5mm.","5022XX0013.jpg","5022XX0013.ldt",1,null,1,23]
["5023","5023XX0012","STOCKHOLM BOLLARD 85CM LED 1164LM 4000K DIM.","Stockholm","Bollard","Stal",null,null,null,"LED zintegrowane","AC","DIM.","10W","10W","1164lm","337lm",null,null,"65","IK10","Class I",4000,null,0,0,0,"CE",null,null,"> 50 000h",1,"Oprawa słupkowa.","Światło odkryte, rozproszone z obrotowo- symetrycznym rozsyłem światła.",null,"Bollard luminaire of stable and durable construction. For lighting private areas and public spaces.",null,null,"Oprawa wyposażona w wymienne źródło światła typu moduł LED, który zapewnia trwałość i optymalny rozsył światła, przy zachowaniu stosunkowo niskiego zużycia energii.","Stal cynkowana ogniowo.","Stal cynkowana ogniowo i malowana proszkowo.","Klosz- tworzywo sztuczne PMMA w kolorze mlecznym.","Uszczelka silikonowa.",null,"85cm","mleczny","Oprawa ściemnialna fazowo TRAILING EDGE (TE) - LEADING EDGE (LE)","Moduł LED","Lumens EDC 47C 10W xxx 230V A101 4K",null,null,"Ściemnianie fazowe Lumens LED AC",null,80,"E","205ZX0010, 206GA0010, 206GA0S10","Zaciski podłączeniowe: max 3x2,5mm², możliwość podłączenia oprawy w pętle max 3x1,5mm². Przewód w oponie okrągłej o średnicy ø7...10,5mm.","5023XX0012.jpg","5023XX0012.ldt",1,null,1,24]
["5024","5024XX0016","NARVIK BOLLARD LED 3264LM 4000K ON/OFF","Narvik","Bollard","Aluminium",null,null,null,"LED zintegrowane","AC","ON/OFF","19,2W","21,8W","3264lm","564lm",null,null,"65","IK10","Class I",4000,"szerokie dół",0.24,0.24,0.95,"CE",null,null,"> 110 000h",1,"Oprawa słupkowa.","Czterostronny wylot światła przysłonięty od góry.",null,"A bollard luminaire with a stable and durable structure. For lighting private and public areas",null,null,null,"Odlew aluminiowy malowany proszkowo.",null,"Klosz- poliwęglan przeźroczysty, stabilizowany UV.","Uszczelka silikonowa.",null,null,null,"Oprawa nieściemnialna","Moduł LED","Philips Fortimo SLM C 1208 L15 2024 G7 3K","Philips Xitanium 36W/m 929001486006",0,null,0,80,"D","110GA0009, 505ZX0009, 7667ZX0009","Zaciski podłączeniowe: max 3x4mm², możliwość podłączenia oprawy w pętle max 3x2,5mm². Przewód w oponie okrągłej o średnicy max ø12,5mm. Oprawa wyposażona w drzwiczki rewizyjne","5024XX0016.jpg","5024XX0016.ldt",4,null,1,16]
["5028","5028XX0016","LILLEHAMMER WALL 2XLED 1069LM UP60º & DOWN60º 4000K DIM.","Lillehammer","Wall","Aluminium",null,null,null,"LED zintegrowane","AC","DIM.","5,6W","7,3W","1069lm","231lm",null,null,"65","IK08","Class I",4000,"szerokie góra / szerokie dół",0.18,0.11,0.08,"CE",null,null,">102 000h",12,"Oprawa ścienna.","Światło dwustronne: o kącie 60º do góry i w dół.","Up60º & Down60º","A luminaire with a wide range of applications, including for lighting: wall surfaces and facades as well as other architectural concepts",null,null,null,"Odlew aluminiowy malowany proszkowo.",null,"Klosz- szkło bezpieczne, optyczne.","Uszczelka silikonowa.","Dławnica EPDM.","góra/dół","szerokie/szerokie","Oprawa ściemnialna fazowo TRAILING EDGE (TE)","2 Moduły LED","Cree DK180501 V8 JB2835 3V 4K","Philips Xitanium 7W 0,35A 20V TE SC 230V [2019]",50000,"Philips Xitanium TE",null,80,"C",null,"Zaciski podłączeniowe: max 3x2,5mm², możliwość podłączenia oprawy w pętle max 3x1,5mm². Przewód w oponie okrągłej o średnicy w zakresie ø7...10,5 mm.","5028XX0016.jpg","5028XX0016.ldt",1,null,1,13]
["5029","5029XX0016","LILLEHAMMER WALL LED 534LM DOWN60º 4000K DIM.","Lillehammer","Wall","Aluminium",null,null,null,"LED zintegrowane","AC","DIM.","2,8W","4W","534lm","112lm",null,null,"65","IK08","Class I",4000,"szerokie dół",0.18,0.11,0.08,"CE",null,null,"> 102 000h",12,"Oprawa ścienna.","Światło jednostronne: o kącie 60º w dół.","Down60º","A luminaire with a wide range of applications, including lighting wall surfaces, facades and other architectural concepts",null,null,null,"Odlew aluminiowy malowany proszkowo.",null,"Klosz- szkło bezpieczne, przeźroczyste.","Uszczelka silikonowa.","Dławnica EPDM.","dół","szerokie","Oprawa ściemnialna fazowo TRAILING EDGE (TE)","Moduł LED","Cree DK180501 V8 JB2835 3V 4K","Philips Xitanium 7W 0,35A 20V TE SC 230V [2019]",50000,"Philips Xitanium TE",null,80,"C",null,"Zaciski podłączeniowe: max 3x2,5mm², możliwość podłączenia oprawy w pętle max 3x1,5mm². Przewód w oponie okrągłej o średnicy w zakresie ø7...10,5 mm.","5029XX0016.jpg","5029XX0016.ldt",1,null,1,38]
["5030","5030XX0017","LILLEHAMMER WALL 2XLED 1069LM UP4º & DOWN4º 4000K DIM.","Lillehammer","Wall","Aluminium",null,null,null,"LED zintegrowane","AC","DIM.","5,6W","7,3W","1069lm","38lm",null,null,"65","IK08","Class I",4000,"wąskie góra / wąskie dół",0.18,0.11,0.08,"CE",null,null,"> 102 000h",12,"Oprawa ścienna.","Światło dwustronne: o kącie 4º do góry i w dół.","Up4º & Down4º","A luminaire with a wide range of applications, including lighting: wall surfaces, facades and other architectural concepts",null,null,null,"Odlew aluminiowy malowany proszkowo.",null,"Klosz- szkło bezpieczne, optyczne.","Uszczelka silikonowa.","Dławnica EPDM.","góra/dół","wąskie/wąskie","Oprawa ściemnialna fazowo TRAILING EDGE (TE)","2 Moduły LED","Cree DK180501 V8 JB2835 3V 4K","Philips Xitanium 7W 0,35A 20V TE SC 230V [2019]",50000,"Philips Xitanium TE",null,80,"C",null,"Zaciski podłączeniowe: max 3x2,5mm², możliwość podłączenia oprawy w pętle max 3x1,5mm². Przewód w oponie okrągłej o średnicy w zakresie ø7...10,5 mm.","5030XX0017.jpg","5030XX0017.ldt",1,null,1,14]
["5031","5031XX0017","LILLEHAMMER WALL LED 534LM DOWN 4º 4000K DIM.","Lillehammer","Wall","Aluminium",null,null,null,"LED zintegrowane","AC","DIM.","2,8W","4W","534lm","18lm",null,null,"65","IK08","Class I",4000,"wąskie dół",0.18,0.11,0.08,"CE",null,null,"> 102 000h",12,"Oprawa ścienna.","Światło jednostronne: o kącie 4º w dół.","Down 4º","A luminaire with a wide range of applications, including lighting wall surfaces, facades and other architectural concepts",null,null,null,"Odlew aluminiowy malowany proszkowo.",null,"Klosz- szkło bezpieczne, optyczne.","Uszczelka silikonowa.","Dławnica EPDM.","dół","wąskie","Oprawa ściemnialna fazowo TRAILING EDGE (TE)","Moduł LED","Cree DK180501 V8 JB2835 3V 4K","Philips Xitanium 7W 0,35A 20V TE SC 230V [2019]",50000,"Philips Xitanium TE",null,80,"C",null,"Zaciski podłączeniowe: max 3x2,5mm², możliwość podłączenia oprawy w pętle max 3x1,5mm². Przewód w oponie okrągłej o średnicy w zakresie ø7...10,5 mm.","5031XX0017.jpg","5031XX0017.ldt",1,null,1,40]
["5032","5032XX0B10","VOSS WALL 3XLED 2301LM 4000K ON/OFF","Voss","Wall","Aluminium",null,null,null,"LED zintegrowane","AC","ON/OFF","12,5W","16,9W","2301lm","655lm",null,null,"54","IK06","Class I",4000,"wąskie góra / szerokie dół",0.18,0.16,0.27,"CE",null,null,"> 102 000h",12,"Oprawa ścienna.","Światło dwustronne: o kącie 4º do góry i kącie 62º w dół.",null,"A luminaire with a wide range of applications, for lighting: wall and facade surfaces and other architectural concepts",null,null,null,"Odlew aluminiowy malowany proszkowo.",null,"Klosz- szkło bezpieczne, przeźroczyste.","Uszczelka silikonowa.","Dławnica EPDM.","góra/dół","wąskie/szerokie","Oprawa nieściemnialna","3 Moduły LED","Cree DK180501 V8 JB2835 3V 4K","Philips Xitanium 20W/m 0.15-0,5A 54V 230V",0,null,null,80,"C",null,"Zaciski podłączeniowe: max 3x2,5mm², możliwość podłączenia oprawy w pętle max 3x1,5mm². Przewód w oponie okrągłej o średnicy ø7...10,5mm.","5032XX0B10.jpg","5032XX0B10.ldt",4,null,1,31]
["5033","5033XX0F10","VOSS WALL 4XLED 3068LM 4000K ON/OFF","Voss","Wall","Aluminium",null,null,null,"LED zintegrowane","AC","ON/OFF","16,6W","21W","3068lm","1077lm",null,null,"54","IK06","Class I",4000,"szerokie góra / szerokie dół",0.18,0.16,0.27,"CE",null,null,"> 102 000h",12,"Oprawa ścienna.","Światło dwustronne: o kącie 62º do góry i w dół.",null,"A luminaire with a wide range of applications, for lighting: walls, facades surfaces, and other architectural concepts",null,null,null,"Odlew aluminiowy malowany proszkowo.",null,"Klosz- szkło bezpieczne, przeźroczyste.","Uszczelka silikonowa.","Dławnica EPDM.","góra/dół","szerokie/szerokie","Oprawa nieściemnialna","4 Moduły LED","Cree DK180501 V8 JB2835 3V 4K","Philips Xitanium 20W/m 0.15-0,5A 54V 230V",0,null,null,80,"C",null,"Zaciski podłączeniowe: max 3x2,5mm², możliwość podłączenia oprawy w pętle max 3x1,5mm². Przewód w oponie okrągłej o średnicy ø7...10,5mm.","5033XX0F10.jpg","5033XX0F10.ldt",4,null,1,36]
["5038","5038XX0013","PARIS SMALL WALL LED 681LM DOWN 4000K DIM.","Paris","Wall","Stal",null,null,null,"LED zintegrowane","AC","DIM.","4W","5,4W","681lm","476lm",null,null,"43",null,"Class I",4000,null,0.23,0.12,0.14000000000000001,"CE",null,null,"> 70 000h",12,"Oprawa ścienna.","Światło rozproszone półsferyczne ukierunkowane w dół",null,"Classic and simple design luminaire with a wide range of applications",null,null,null,"Stal cynkowana ogniowo.","Stal malowana proszkowo.","Klosz- poliwęglan satynowany, stabilizowany UV.",null,"Dławnica EPDM.",null,null,"Oprawa ściemnialna fazowo TRAILING EDGE (TE)","Moduł LED","Philips Strip OC 0.5ft 550lm 8xx FC HV5 4K","Philips Xitanium 7W 0,35A 20V TE SC 230V [2019]",50000,"Philips Xitanium TE",0,80,"C",null,"Zaciski podłączeniowe: max 3x2,5mm², możliwość podłączenia oprawy w pętle max 3x1,5mm². Przewód w oponie okrągłej o średnicy ø7...10,5mm.","5038XX0013.jpg","5038XX0013.ldt",1,null,1,76]
["5039","5039XX0013","PARIS WALL LED 683LM DOWN 4000K DIM.","Paris,Big","Wall","Stal",null,null,null,"LED zintegrowane","AC","DIM.","4W","5,2W","683lm","438lm",null,null,"43",null,"Class I",4000,null,0,0,0,"CE",null,null,"> 70000",12,"Oprawa ścienna.","Światło rozproszone półsferyczne ukierunkowane w dół",null,"Classic design luminaire with a wide range of applications for example for illumination of walls and facade surfaces or any other architectural concepts.",null,null,null,"Stal cynkowana ogniowo.","Stal malowana proszkowo.","Klosz- poliwęglan satynowany, stabilizowany UV.",null,"Dławnica EPDM.",null,null,"Oprawa ściemnialna fazowo TRAILING EDGE (TE)","Moduł LED","Philips Strip 0.5ft 550lm 8xx FC HV4","Philips Xitanium 7W 0,35A 20V TE SC 230V [2017]",50000,null,0,80,null,null,"Zaciski podłączeniowe: max 3x2,5mm², możliwość podłączenia oprawy w pętle max 3x1,5mm². Przewód w oponie okrągłej o średnicy ø7...10,5mm.","5039XX0013.jpg","5039XX0013.ldt",1,null,1,76]
["5045","5045XX0010","NORDLAND CEILING/WALL LED 2050LM 4000K MD","Nordland","Wall","Aluminium",null,null,null,"LED zintegrowane","AC","MD","17,5W","17,5W","2050lm","763lm",null,null,"65","IK10","Class I",4000,null,0.28000000000000003,0.28000000000000003,0.1,"CE","Daylight sensor,Motion sensor",null,"50 000h",7,"Oprawa sufitowo-ścienna.","Światło rozproszone.",null,"Luminaire with modern design. Equipped with a motion sensor with a twilight switch and movement sustain sensor",null,null,null,"Odlew aluminiowy malowany proszkowo.",null,"Klosz- poliwęglan mleczny, stabilizowany UV.","Uszczelka silikonowa.","Dławnica EPDM.","TAK",null,"Oprawa wyposażona w mikrofalowy czujnik ruchu, z wyłącznikiem zmierzchowym i podtrzymaniem ruchu","Moduł LED","Philips Fortimo DLM ES 2000/8xx G2 4K",null,0,"Mikrofalowy czujnik ruchu MD (PD-MV1005)",null,80,"D",null,"Zaciski podłączeniowe: max 3x2,5mm², możliwość podłączenia oprawy w pętle max 5x1,5mm². Przewód w oponie okrągłej o średnicy ø7...10,5mm.","5045XX0010.jpg","5045XX0010.ldt",3,null,1,7]
["5046","5046XX0009","NORDLAND CEILING/WALL LED 1419LM 3000K DIM.","Nordland","Wall,Ceiling","Aluminium",null,null,null,"LED zintegrowane","AC","DIM.","16W","16W","1419lm","934lm",null,null,"65","IK10","Class I",3000,null,2.8,2.8,0.95,"CE",null,null,"50 000h",7,"Oprawa sufitowo-ścienna.","Światło rozproszone.",null,"A ceiling-type luminaire with a modern design For lighting private areas and other architectural concepts",null,null,null,"Odlew aluminiowy malowany proszkowo.",null,"Klosz- poliwęglan mleczny, stabilizowany UV.","Uszczelka silikonowa.","Dławnica EPDM.","NIE",null,"Oprawa ściemnialna fazowo TRAILING EDGE (TE) - LEADING EDGE (LE)","Moduł LED","Lumens DLM 100C 16W 830 230V F201 V0,5 3K",null,0,"Ściemnianie fazowe Lumens LED AC",null,80,"F",null,"Zaciski podłączeniowe: max 3x2,5mm², możliwość podłączenia oprawy w pętle max 3x2,5mm². Przewód w oponie okrągłej o średnicy ø7...10,5mm.","5046XX0009.jpg","5046XX0009.ldt",1,null,1,7]
["5047","5047XX0009","NORDLAND CEILING/WALL LED 1467LM 4000K DIM.","Nordland","Wall,Ceiling","Aluminium",null,null,null,"LED zintegrowane","AC","DIM.","16W","15,4W","1467lm","933lm",null,null,"65","IK10","Class I",4000,null,2.8,2.8,0.95,"CE",null,null,"50 000h",7,"Oprawa sufitowo-ścienna.","Światło rozproszone.",null,"A ceiling-type luminaire with a modern design For lighting private areas and other architectural concepts",null,null,null,"Odlew aluminiowy malowany proszkowo.",null,"Klosz- poliwęglan mleczny, stabilizowany UV.","Uszczelka silikonowa.","Dławnica EPDM.","NIE",null,"Oprawa ściemnialna fazowo TRAILING EDGE (TE) - LEADING EDGE (LE)","Moduł LED","Lumens DLM 100C 16W 840 230V F201 V0,5 4K",null,0,"Ściemnianie fazowe Lumens LED AC",null,80,"F",null,"Zaciski podłączeniowe: max 3x2,5mm², możliwość podłączenia oprawy w pętle max 3x1,5mm². Przewód w oponie okrągłej o średnicy ø7...10,5mm.","5047XX0009.jpg","5047XX0009.ldt",1,null,1,7]
["5060","5060XX0010","STAVANGER BOLLARD 95CM LED 1171LM 4000K DALI2","Stavanger","Bollard","Aluminium",null,null,null,"LED zintegrowane","AC","DALI2","9,6W","12,2W","1171lm","493lm",null,null,"65","IK10","Class I",4000,"szerokie dół",0.2,0.2,0.95,"CE",null,"DALI","50 000h",1,"Oprawa słupkowa.","Światło pośrednie, obrotowo- symetryczne, ukierunkowane w dół.",null,"A bollard luminaire with a stable and durable structure For lighting private and public areas",null,null,null,"Odlew aluminiowy malowany proszkowo.",null,"Klosz- poliwęglan przeźroczysty, stabilizowany UV.","Uszczelka silikonowa.","Dławnica nylon6.","95cm","przeźroczysty PC","Sterowanie światłem w systemie: DALI outdoor pełny program. Zasilacz zaprogramowany na max prąd. Programowanie pozostałych parametrów po uzgodnieniu z Działem Handlowym firmy Norlys.","Moduł LED","Cree DK1305003 V2 XD16 4K","Philips Xi FP 22W 0,2-0,7A SNLDAE 230V S175 sXt",100000,"DALI2 / NightDim (XI FP NLD)",null,80,"E","1230ZX0009, 1231GA0009, 1232GA0009, 6139ZX0009, 7662ZX0009","Zaciski podłączeniowe: max 5x4mm², możliwość podłączenia oprawy w pętle max 5x2,5mm². Przewód w oponie okrągłej o średnicy ø8...17mm.","5060XX0010.jpg","5060XX0010.ldt",3,null,1,33]
["5061","5061XX0010","STAVANGER BOLLARD 50CM LED 1171LM 4000K DALI2","Stavanger","Bollard","Aluminium",null,null,null,"LED zintegrowane","AC","DALI2","9,6W","12,2W","1171lm","493lm",null,null,"65","IK08","Class I",4000,"szerokie dół",0.2,0.2,0.5,"CE",null,"DALI","50 000h",1,"Oprawa słupkowa.","Światło pośrednie, obrotowo- symetryczne, ukierunkowane w dół.",null,"A bollard luminaire with a stable and durable structure. For lighting private and public areas",null,null,null,"Odlew aluminiowy malowany proszkowo.",null,"Klosz- poliwęglan przeźroczysty, stabilizowany UV.","Uszczelka silikonowa.","Dławnica nylon6.","50cm","przeźroczysty PC","Sterowanie światłem w systemie: DALI outdoor pełny program. Zasilacz zaprogramowany na max prąd. Programowanie pozostałych parametrów po uzgodnieniu z Działem Handlowym firmy Norlys.","Moduł LED","Cree DK1305003 V2 XD16 4K","Philips Xi FP 22W 0,2-0,7A SNLDAE 230V C123 sXt 12NC: 929002165006",100000,"DALI2 / NightDim (XI FP NLD)",null,80,"E","1230ZX0009, 1231GA0009, 1232GA0009","Zaciski podłączeniowe: max 5x4mm², możliwość podłączenia oprawy w pętle max 5x1,5mm². Przewód w oponie okrągłej o średnicy ø8...17mm.","5061XX0010.jpg","5061XX0010.ldt",3,null,1,33]
["5062","5062XX0009","STAVANGER BOLLARD 28CM LED 1092LM 4000K DALI","Stavanger","Bollard","Aluminium",null,null,null,"LED zintegrowane","AC","DALI","6,6W","8,5W","1092lm","351lm",null,null,"65","IK08","Class I",4000,"szerokie dół",0.2,0.2,0.28000000000000003,"CE",null,"DALI","50 000h",1,"Oprawa słupkowa.","Światło pośrednie, obrotowo- symetryczne, ukierunkowane w dół.",null,"A bollard luminaire with a stable and durable structure. For lighting gardens, private areas and other architectural applications",null,null,null,"Odlew aluminiowy malowany proszkowo.",null,"Klosz- poliwęglan przeźroczysty, stabilizowany UV.","Uszczelka silikonowa.","Dławnica nylon6.","28cm","przeźroczysty PC",null,"Moduł LED","Cree DK1305003 V2 XD16 4K","Osram OTI DALI 10/220-240/700 NFC",0,null,null,80,"E","1230ZX0009, 1231GA0009","Zaciski podłączeniowe: max 5x2,5mm², możliwość podłączenia oprawy w pętle max 5x2,5mm². Przewód w oponie okrągłej o średnicy ø8...17mm.","5062XX0009.jpg","5062XX0009.ldt",3,null,1,33]
["5063","5063XX0010","STAVANGER BOLLARD 95CM LED 1179LM 3000K DALI2","Stavanger","Bollard","Aluminium",null,null,null,"LED zintegrowane","AC","DALI2","9,6W","12,2W","1179lm","428lm",null,null,"65","IK08","Class I",3000,"szerokie dół",0.2,0.2,0.95,"CE",null,"DALI","> 145 000h",1,"Oprawa słupkowa.","Światło pośrednie, obrotowo- symetryczne, ukierunkowane w dół.",null,"Bollard luminaire of stable and durable construction For lighting private areas and public spaces",null,null,null,"Odlew aluminiowy malowany proszkowo.",null,"Klosz- poliwęglan przeźroczysty, stabilizowany UV.","Uszczelka silikonowa.","Dławnica nylon6.","95cm","przeźroczysty PC","Sterowanie światłem w systemie: DALI outdoor pełny program. Zasilacz zaprogramowany na max prąd. Programowanie pozostałych parametrów po uzgodnieniu z Działem Handlowym firmy Norlys.","Moduł LED","Cree DK1305003 V2 XPG3 3K","Philips Xi FP 22W 0,2-0,7A SNLDAE 230V C123 sXt 12NC: 929002165006",100000,"DALI2 / NightDim (XI FP NLD)",null,80,null,"1230ZX0009, 1231GA0009, 1232GA0009, 6139ZX0009, 7662ZX0009","Zaciski podłączeniowe: max 5x4mm², możliwość podłączenia oprawy w pętle max 5x2,5mm². Przewód w oponie okrągłej o średnicy ø8...17mm.","5063XX0010.jpg","5063XX0010.ldt",3,null,1,33]
["5065","5065XX0009","STAVANGER BOLLARD 28CM LED 854LM 3000K DALI","Stavanger","Bollard","Aluminium",null,null,null,"LED zintegrowane","AC","DALI","6,6W","8,4W","854lm","400lm",null,null,"65",null,"Class I",3000,"szerokie dół",0.2,0.2,0.28000000000000003,"CE",null,"DALI","> 145 000h",1,"Oprawa słupkowa.","Światło pośrednie, obrotowo- symetryczne, ukierunkowane w dół.",null,"A bollard luminaire with a stable and durable structure, For lighting private areas and public areas",null,null,null,"Odlew aluminiowy malowany proszkowo.",null,"Klosz- poliwęglan przeźroczysty, stabilizowany UV.","Uszczelka silikonowa.","Dławnica nylon6.","28cm","przeźroczysty PC",null,"Moduł LED","Cree DK1305003 V2 XPG3 3K","Osram OTI DALI 10/220-240/700 NFC",0,null,null,80,"D","1230ZX0009, 1231GA0009","Zaciski podłączeniowe: max 5x2,5mm², możliwość podłączenia oprawy w pętle max 5x2,5mm². Przewód w oponie okrągłej o średnicy ø8...17mm.","5065XX0009.jpg","5065XX0009.ldt",3,null,1,33]
["5066","5066XX0011","EGERSUND BOLLARD 108CM LED 2655LM 4000K DALI2","Egersund","Bollard","Aluminium",null,null,null,"LED zintegrowane","AC","DALI2","18W","21,9W","2655lm","1782lm",null,null,"65","IK08","Class I",4000,null,0.2,0.2,1.08,"CE",null,"DALI","> 162 000h",1,"Oprawa słupkowa.","Światło obrotowo-symetryczne.",null,"Luminaire with a contemporary design. For lighting gardens and other private and public areas",null,null,null,"Odlew aluminiowy malowany proszkowo.",null,"Klosz- tworzywo sztuczne PMMA przeźroczyste.","Uszczelka silikonowa.",null,"108cm",null,"Sterowanie światłem w systemie: DALI outdoor pełny program. Zasilacz zaprogramowany na max prąd. Programowanie pozostałych parametrów po uzgodnieniu z Działem Handlowym firmy Norlys.","Moduł LED","Cree DK201002 V1 JK3030 6V 3K","Osram OT 40/170-240/1A0 4DIMLT2 NFC E",100000,"DALI2 / NightDim (4DIM)",0.1,80,"E","1230ZX0009, 1231GA0009, 6036ZX0009, 6037ZX0009","Zaciski podłączeniowe: max 5x4mm², możliwość podłączenia oprawy w pętle max 5x4mm². Przewód w oponie okrągłej o średnicy ø8...17mm.","5066XX0011.jpg","5066XX0011.ldt",3,null,1,17]
["5068","5068XX0011","EGERSUND BOLLARD 108CM LED 2617LM 3000K DALI2","Egersund","Bollard","Aluminium",null,null,null,"LED zintegrowane","AC","DALI2","18W","21,9W","2617lm","1681lm",null,null,"65","IK08","Class I",3000,null,0.2,0.2,1.08,"CE",null,"DALI","> 162 000h",1,"Oprawa słupkowa.","Światło obrotowo-symetryczne.",null,"Luminaire with a contemporary design. For lighting gardens and other private and public areas",null,null,null,"Odlew aluminiowy malowany proszkowo.",null,"Klosz- tworzywo sztuczne PMMA przeźroczyste.","Uszczelka silikonowa.",null,"108cm",null,"Sterowanie światłem w systemie: DALI outdoor pełny program. Zasilacz zaprogramowany na max prąd. Programowanie pozostałych parametrów po uzgodnieniu z Działem Handlowym firmy Norlys.","Moduł LED","Cree DK201002 V1 JK3030 6V 3K","Osram OT 40/170-240/1A0 4DIMLT2 NFC E",100000,"DALI2 / NightDim (4DIM)",0.1,80,"E","1230ZX0009, 1231GA0009, 6036ZX0009, 6037ZX0009","Zaciski podłączeniowe: max 5x4mm², możliwość podłączenia oprawy w pętle max 5x4mm². Przewód w oponie okrągłej o średnicy ø8...17mm.","5068XX0011.jpg","5068XX0011.ldt",3,null,1,17]
["5069","5069XX0010","EGERSUND BOLLARD 63CM 5XLED 2434LM 3000K DALI2","Egersund","Bollard","Aluminium",null,null,null,"LED zintegrowane","AC","DALI2",null,"23W","2434lm","1586lm",null,null,"65","IK08","Class I",3000,null,0.2,0.2,0.63,"CE",null,"DALI","> 50 000h",1,"Oprawa słupkowa.","Światło obrotowo-symetryczne.",null,"Luminaire with contemporary design. For lighting gardens and other private and public areas",null,null,"Oprawa wyposażona w wymienne źródło światła typu moduł LED. Możliwość sterowania i programowania pracy źródła światła w ramach systemu DALI2, co gwarantuje optymalnie niskie zużycie energii.","Odlew aluminiowy malowany proszkowo.",null,"Klosz- tworzywo sztuczne PMMA przeźroczyste.","Uszczelka silikonowa.","Dławnica nylon6.","63cm",null,"Sterowanie światłem w systemie: DALI outdoor pełny program. Zasilacz zaprogramowany na max prąd. Programowanie pozostałych parametrów po uzgodnieniu z Działem Handlowym firmy Norlys.","5 Modułów LED","Cree DK180501 V3 JK3030 3V 3K","Osram OT 40/170-240/1A0 4DIMLT2 NFC E",100000,"DALI2 / NightDim (4DIM)",null,80,"E","1230ZX0009, 1231GA0009, 1232GA0009","Zaciski podłączeniowe: max 5x4mm², możliwość podłączenia oprawy w pętle max 5x4mm². Przewód w oponie okrągłej o średnicy ø8...17mm.","5069XX0010.jpg","5069XX0010.ldt",3,null,1,17]
["5070","5070XX0011","KOSTER POLE-TOP LED 2050LM 4000K","Koster","Post,Head","Aluminium",null,null,null,"LED zintegrowane","AC",null,"17,5W","17,5W","2050lm","1625lm",null,null,"54","IK10","Class I",4000,null,0,0,0,"CE",null,null,"50000",2,"Oprawa słupowa (nasadzana).","Światło jednostronne: symetryczne, ukierunkowane w dół.",null,"Classic design luminaire for mounting on a telescopic lighting pole with cap diameter Ø50mm.",null,null,"Oprawa wyposażona w wymienne źródło światła typu moduł LED, która zapewnia trwałość i optymalny rozsył światła, przy zachowaniu stosunkowo niskiego zużycia energii.","Odlew aluminiowy malowany proszkowo.",null,"Klosz- poliwęglan przeźroczysty ze strukturą, stabilizowany UV.",null,null,"Ø50",null,"Oprawa nieściemnialna","Moduł LED","Philips LED Fortimo DLM ES 2000/840 G2",null,null,null,0,80,"D","111GA0009, 1270XX0009, 405ZX0009, 406ZX0009","Przewód H05VV-F 3G1 o długości 3,7m do podłączenia wewnątrz słupa oświetleniowego (w odpowiednio dobranej puszce elektroinstalacyjnej).","5070XX0011.jpg","5070XX0011.ldt",4,null,1,27]
["5080","5080XX0010","ASKER BIG PRO WALL 4XLED 2587LM UP-DOWN 3000K DALI2","Asker,Big","Wall","Aluminium",null,null,"PRO","LED zintegrowane","AC","DALI2","17W","19,4W","2587lm","1669lm",null,null,"65","IK08","Class I",3000,"szerokie góra / szerokie dół",0.3,0.12,0.12,"CE",null,"DALI","> 70 000h",12,"Oprawa ścienna.","Światło dwustronne: ukierunkowane do góry i w dół.","Up-Down","A luminaire with a wide range of applications, for illuminating wall and facade surfaces as well as other architectural concepts",null,null,null,"Odlew aluminiowy malowany proszkowo.",null,"Klosz- poliwęglan przeźroczysty ze strukturą, stabilizowany UV.","Uszczelka silikonowa.","Dławnica EPDM.","góra/dół",null,null,"4 Moduły LED","Philips Fortimo Strip 0,5ft MF FC LV6 3K","Osram OTi DALI 20/220…240/500 NFC S",0,null,null,80,"C",null,"Zaciski podłączeniowe: max 3x2,5mm², możliwość podłączenia oprawy w pętle max 3x1,5mm². Przewód w oponie okrągłej o średnicy ø7...10,5mm.","5080XX0010.jpg","5080XX0010.ldt",3,null,1,4]
["5085","5085XX0010","ASKER BIG PRO WALL 2XLED 1231LM DOWN 3000K DALI2","Asker,Big","Wall","Aluminium",null,null,"PRO","LED zintegrowane","AC","DALI2","8W","10,2W","1231lm","843lm",null,null,"65",null,"Class I",3000,"szerokie dół",0.3,0.12,0.12,"CE",null,"DALI","> 72 000h",12,"Oprawa ścienna.","Światło rozproszone półsferyczne ukierunkowane w dół",null,"A luminaire with a wide range of applications, including lighting of wall surfaces, facades and other architectural concepts","A luminaire with a wide range of applications, for illuminating wall surfaces, facades, and other architectural concepts. Suitable for emergency installations with direct voltage: DC 176 ÷ 276V",null,null,"Odlew aluminiowy malowany proszkowo.",null,"Klosz- poliwęglan przeźroczysty ze strukturą, stabilizowany UV.","Uszczelka silikonowa.","Dławnica EPDM.","dół",null,"Sterowanie światłem w systemie: DALI2","2 Moduły LED","Philips Fortimo_LED_Strip_0.5ft_MF_8xx_HV6 3K","Osram OTi DALI 20/220…240/500 NFC S",0,null,null,80,"D",null,"Zaciski podłączeniowe: max 5x2,5mm², możliwość podłączenia oprawy w pętle max 5x1,5mm². Przewód w oponie okrągłej o średnicy ø7...10,5mm.","5085XX0010.jpg","5085XX0010.ldt",3,null,1,76]
["5086","5086XX0010","ASKER BIG PRO WALL 4XLED 2740LM UP-DOWN 4000K DALI2","Asker,Big","Wall","Aluminium",null,null,"PRO","LED zintegrowane","AC","DALI2","17W","19,3W","2740lm","1942lm",null,null,"65","IK08","Class I",4000,"szerokie góra / szerokie dół",0.3,0.12,0.12,"CE",null,"DALI","> 70 000h",12,"Oprawa ścienna.","Światło dwustronne: ukierunkowane do góry i w dół.","Up-Down","A luminaire with a wide range of applications, for illuminating wall and facade surfaces and other architectural concepts.",null,null,null,"Odlew aluminiowy malowany proszkowo.",null,"Klosz- poliwęglan przeźroczysty ze strukturą, stabilizowany UV.","Uszczelka silikonowa.","Dławnica EPDM.","góra/dół",null,null,"4 Moduły LED","Philips Fortimo Strip 0,5ft MF FC LV6 4K","Osram OTi DALI 20/220…240/500 NFC S",0,null,null,80,"C",null,"Zaciski podłączeniowe: max 3x2,5mm², możliwość podłączenia oprawy w pętle max 3x1,5mm². Przewód w oponie okrągłej o średnicy ø7...10,5mm.","5086XX0010.jpg","5086XX0010.ldt",3,null,1,4]
["5087","5087XX0010","ASKER BIG PRO WALL 2XLED 1303LM DOWN 4000K DALI2","Asker,Big","Wall","Aluminium",null,null,"PRO","LED zintegrowane","AC","DALI2","8W","10,2W","1303lm","960lm",null,null,"65",null,"Class I",4000,"szerokie dół",0.3,0.12,0.12,"CE",null,"DALI","> 70 000h",12,"Oprawa ścienna.","Światło rozproszone półsferyczne ukierunkowane w dół",null,"A luminaire with a wide range of applications, for illuminating wall and facade surfaces as well as other architectural concepts",null,null,null,"Odlew aluminiowy malowany proszkowo.",null,"Klosz- poliwęglan przeźroczysty ze strukturą, stabilizowany UV.","Uszczelka silikonowa.","Dławnica EPDM.","dół",null,null,"2 Moduły LED","Philips Fortimo Strip 0,5ft MF FC LV6 4K","Osram OTi DALI 20/220…240/500 NFC S",0,null,null,80,"C",null,"Zaciski podłączeniowe: max 5x2,5mm², możliwość podłączenia oprawy w pętle max 5x1,5mm². Przewód w oponie okrągłej o średnicy ø7...10,5mm.","5087XX0010.jpg","5087XX0010.ldt",3,null,1,76]
["5088","5088XX0009","NICE POLE-TOP LED 4000K DALI2","Nice","Post,Head","Aluminium",null,null,null,"LED zintegrowane","AC","DALI2","32,2W","36,3W",null,"3092lm",null,null,"65",null,"Class I",4000,null,0.7,0.55000000000000004,0.55000000000000004,"CE",null,"DALI","> 50 000h",2,"Oprawa słupowa (nasadzana).","Światło symetryczne pośrednie.",null,"A mounted luminaire designed to be mounted on a lighting pole with a Ø60mm mounting shaft",null,null,null,"Odlew aluminiowy malowany proszkowo.",null,"Klosz- szkło bezpieczne, przeźroczyste.","Uszczelka silikonowa.",null,null,null,"Sterowanie światłem w systemie: DALI outdoor pełny program. Zasilacz zaprogramowany na max prąd. Programowanie pozostałych parametrów po uzgodnieniu z Działem Handlowym firmy Norlys.","Moduł LED","Philips Fortimo SLM C 1211 L19 2828 G7 4K","Philips Xi FP 40W 0,3-1,0A SNLDAE 230V C123 sXt 929002165306",0,"DALI2 / NightDim (XI FP NLD)",null,80,"D","3005XX0009, 7662ZX0009, 7664ZX0009, 7665XX0009","Przewód OLFLEX 540 P 5G1 o długości 4,5m do podłączenia wewnątrz słupa oświetleniowego (w odpowiednio dobranej puszcze elektroinstalacyjnej).","5088XX0009.jpg","5088XX0009.ldt",3,null,1,21]
["5089","5089XX0010","NICE POLE-TOP LED 3029LM 3000K DALI2","Nice","Post,Head","Aluminium",null,null,null,"LED zintegrowane","AC","DALI2","32,2W","36,5W","3029lm","2964lm",null,null,"65",null,"Class I",3000,null,0.55000000000000004,0.55000000000000004,0.7,"CE",null,"DALI","> 50 000h",2,"Oprawa słupowa (nasadzana).","Światło symetryczne pośrednie.",null,"Top-mounted luminaire designed for mounting on a lighting pole with a Ø60mm mounting shaft",null,null,null,"Odlew aluminiowy malowany proszkowo.",null,"Klosz- szkło bezpieczne, przeźroczyste.","Uszczelka silikonowa.",null,null,null,"Sterowanie światłem w systemie: DALI outdoor pełny program. Zasilacz zaprogramowany na max prąd. Programowanie pozostałych parametrów po uzgodnieniu z Działem Handlowym firmy Norlys.","Moduł LED","Philips Fortimo SLM C 1211 L19 2828 G7 3K","Philips Xi FP 40W 0,3-1,0A SNLDAE 230V C123 sXt 929002165306",0,"DALI2 / NightDim (XI FP NLD)",null,80,"D","3005XX0009, 7662ZX0009, 7664ZX0009, 7665XX0009","Przewód OLFLEX 540 P 5G1 o długości 4,5m do podłączenia wewnątrz słupa oświetleniowego (w odpowiednio dobranej puszce elektroinstalacyjnej).","5089XX0010.jpg","5089XX0010.ldt",3,null,1,21]
["5090","5090XX0011","NARVIK BOLLARD LED 3264LM 4000K DALI2","Narvik","Bollard","Aluminium",null,null,null,"LED zintegrowane","AC","DALI2","19W","21,8W","3264lm","582lm",null,null,"65","IK10","Class I",4000,"szerokie dół",0.24,0.24,0.95,"CE",null,"DALI","> 50 000h",1,"Oprawa słupkowa.","Czterostronny wylot światła przysłonięty od góry.",null,"A bollard luminaire with a stable and durable structure. For lighting private and public areas",null,null,null,"Odlew aluminiowy malowany proszkowo.",null,"Klosz- poliwęglan przeźroczysty, stabilizowany UV.","Uszczelka silikonowa.",null,null,null,"Sterowanie światłem w systemie: DALI outdoor pełny program. Zasilacz zaprogramowany na max prąd. Programowanie pozostałych parametrów po uzgodnieniu z Działem Handlowym firmy Norlys.","Moduł LED","Philips Fortimo SLM C 1208 L15 2024 G7 3K","Osram OT 40/170-240/1A0 4DIMLT2 NFC E",100000,"DALI2 / NightDim (4DIM)",0,80,"D","110GA0009, 505ZX0009, 7667ZX0009","Zaciski podłączeniowe: max 5x4mm², możliwość podłączenia oprawy w pętle max 5x2,5mm². Przewód w oponie okrągłej o średnicy max ø12,5mm. Oprawa wyposażona w drzwiczki rewizyjne.","5090XX0011.jpg","5090XX0011.ldt",3,null,1,16]
["5091","5091XX0010","NARVIK BOLLARD LED 3137LM 3000K DALI2","Narvik","Bollard","Aluminium",null,null,null,"LED zintegrowane","AC","DALI2","19W","22,5W","3137lm","597lm",null,null,"65","IK10","Class I",3000,"szerokie dół",0,0,0,"CE",null,"DALI",">110 000h",1,"Oprawa słupkowa.","Czterostronny wylot światła przysłonięty od góry.",null,"A post luminaire with a stable and durable construction For lighting private and public areas",null,null,null,"Odlew aluminiowy malowany proszkowo.",null,"Klosz- poliwęglan przeźroczysty, stabilizowany UV.","Uszczelka silikonowa.",null,null,null,"Sterowanie światłem w systemie: DALI outdoor pełny program. Zasilacz zaprogramowany na max prąd. Programowanie pozostałych parametrów po uzgodnieniu z Działem Handlowym firmy Norlys.","Moduł LED","Philips Fortimo SLM C 1208 L15 2024 G7 3K","Osram OT 40/170-240/1A0 4DIMLT2 NFC E",100000,"DALI2 / NightDim (4DIM)",0,80,"D","110GA0009, 505ZX0009","Zaciski podłączeniowe: max 5x4mm², możliwość podłączenia oprawy w pętle max 5x2,5mm². Przewód w oponie okrągłej o średnicy max ø12,5mm. Oprawa wyposażona w drzwiczki rewizyjne.","5091XX0010.jpg","5091XX0010.ldt",3,null,1,16]
["5092","5092XX0010","VASA WALL 2XLED 1303LM UP-DOWN 4000K DALI2","Vasa","Wall","Aluminium",null,null,null,"LED zintegrowane","AC","DALI2","8W","14,1W","1303lm","1039lm",null,null,"65","IK08","Class I",4000,"szerokie góra / szerokie dół",0.31,0.12,0.16,"CE",null,"DALI","> 70 000h",12,"Oprawa ścienna.","Światło dwustronne: ukierunkowane do góry i w dół.","Up-Down","A luminaire with a wide range of applications, for lighting: wall surfaces, facade and other architectural concepts",null,null,null,"Odlew aluminiowy malowany proszkowo.",null,"Klosz- poliwęglan przeźroczysty ze strukturą, stabilizowany UV.","Uszczelka silikonowa.","Dławnica EPDM.",null,null,null,"2 Moduły LED","Philips Fortimo Strip 0,5ft MF FC LV6 4K","Osram OTi DALI 20/220…240/500 NFC S",0,null,null,80,"C",null,"Zaciski podłączeniowe: max 5x2,5mm², możliwość podłączenia oprawy w pętle max 5x1,5mm². Przewód w oponie okrągłej o średnicy ø7...10,5mm.","5092XX0010.jpg","5092XX0010.ldt",3,null,1,4]
["5093","5093XX0010","VASA WALL 2XLED 1231LM UP-DOWN 3000K DALI2","Vasa","Wall","Aluminium",null,null,null,"LED zintegrowane","AC","DALI2","8W","9,7W","1231lm","670lm",null,null,"65","IK08","Class I",3000,"szerokie góra / szerokie dół",0.31,0.12,0.16,"CE",null,"DALI","> 70 000h",12,"Oprawa ścienna.","Światło dwustronne: ukierunkowane do góry i w dół.","Up-Down","A luminaire with a wide range of applications, for lighting: wall surfaces, facades and other architectural concepts",null,null,null,"Odlew aluminiowy malowany proszkowo.",null,"Klosz- poliwęglan przeźroczysty ze strukturą, stabilizowany UV.","Uszczelka silikonowa.","Dławnica EPDM.",null,null,null,"2 Moduły LED","Philips Fortimo Strip 0,5ft MF FC LV6 3K","Osram OTi DALI 20/220…240/500 NFC S",0,null,null,80,"C",null,"Zaciski podłączeniowe: max 5x2,5mm², możliwość podłączenia oprawy w pętle max 5x1,5mm². Przewód w oponie okrągłej o średnicy ø7...10,5mm.","5093XX0010.jpg","5093XX0010.ldt",3,null,1,4]
["5096","5096XX0010","HALDEN WALL LED 1059LM DOWN 3000K DALI2","Halden","Wall","Aluminium",null,null,null,"LED zintegrowane","AC","DALI2","6,7W","8,4W","1059lm","662lm",null,null,"65","IK10","Class I",3000,"szerokie dół",0.31,0.16,0.15,"CE",null,"DALI",">110 000",12,"Oprawa ścienna.","Światło rozproszone półsferyczne ukierunkowane w dół",null,"A luminaire with a wide range of applications, among others for lighting: wall surfaces, facade, and other architectural concepts",null,null,null,"Odlew aluminiowy malowany proszkowo.",null,"Klosz- poliwęglan przeźroczysty ze strukturą, stabilizowany UV.","Uszczelka silikonowa.","Dławnica EPDM.",null,null,null,"Moduł LED","Philips Fortimo SLM C 1203 L09 1619 G7 3K","Osram OTi DALI 15/220…240/NFC index 4699210300",100000,null,null,80,"D",null,"Zaciski podłączeniowe: max 3x2,5mm², możliwość podłączenia oprawy w pętle max 3x1,5mm². Przewód w oponie okrągłej o średnicy ø7...10,5mm.","5096XX0010.jpg","5096XX0010.ldt",3,null,1,76]
["5097","5097XX0009","HALDEN WALL LED 1121LM 4000K DALI2","Halden","Wall","Aluminium",null,null,null,"LED zintegrowane","AC","DALI2","6,7W","8,8W","1121lm","696lm",null,null,"65","IK10","Class I",4000,null,0.31,0.16,0.15,"CE",null,"DALI",">110 000h",12,"Oprawa ścienna.","Światło rozproszone półsferyczne ukierunkowane w dół",null,"Luminaire with a wide range of applications for example for illumination of walls and facade surfaces or any other architectural concepts.",null,null,null,"Odlew aluminiowy malowany proszkowo.",null,"Klosz- poliwęglan przeźroczysty ze strukturą, stabilizowany UV.","Uszczelka silikonowa.","Dławnica EPDM.",null,null,"Sterowanie światłem w systemie: DALI/TD.","Moduł LED","Philips Fortimo SLM C 1203 L09 1619 G7 4K","Osram OTi DALI 15/220…240/NFC index 4699210300",100000,null,null,80,"D",null,"Zaciski podłączeniowe: max 5x2,5mm², możliwość podłączenia oprawy w pętle max 5x1,5mm². Przewód w oponie okrągłej o średnicy ø7...10,5mm.","5097XX0009.jpg","5097XX0009.ldt",3,null,1,76]
["5100","5100XX0010","ASKER WALL LED 961LM UP-DOWN 4000K DIM.","Asker","Wall","Stal","Ocynkowane",null,null,"LED zintegrowane","AC","DIM.","8W","8W","961lm","367lm",null,null,"44","IK08","Class I",4000,"szerokie góra / szerokie dół",null,null,null,"CE",null,null,"50000",12,"Oprawa ścienna.","Światło dwustronne: ukierunkowane do góry i w dół.","Up-Down","Luminaire with a wide range of applications for example for illumination of walls and facade surfaces or any other architectural concepts.",null,null,"Oprawa wyposażona w wymienne źródło światła typu moduł LED, który zapewnia trwałość i optymalny rozsył światła, przy zachowaniu stosunkowo niskiego zużycia energii.",null,"Korpus- stal cynkowana ogniowo.","Klosz- poliwęglan przeźroczysty ze strukturą, stabilizowany UV.","Uszczelka silikonowa.","Podstawa- odlew aluminiowy malowany proszkowo.","góra/dół",null,"Oprawa ściemnialna fazowo TRAILING EDGE (TE) - LEADING EDGE (LE)","Moduł LED","Lumens EDC 57C 8W xxx 230V A FF Ver.1.0",null,0,null,null,80,null,null,"Zaciski podłączeniowe: max 3x2,5mm², możliwość podłączenia oprawy w pętle max 3x1,5mm². Przewód w oponie okrągłej o średnicy ø7...10,5mm.","5100XX0010.jpg","5100XX0010.ldt",1,null,1,4]
["5101","5101XX0010","ASKER WALL LED 961LM DOWN 4000K DIM.","Asker","Wall","Stal","Ocynkowane",null,null,"LED zintegrowane","AC","DIM.","8W","8W","961lm","183lm",null,null,"44",null,"Class I",4000,"szerokie dół",0,0,0,"CE",null,null,"50000",12,"Oprawa ścienna.","Światło rozproszone półsferyczne ukierunkowane w dół",null,"Luminaire with a wide range of applications for example for illumination of walls and facade surfaces or any other architectural concepts.",null,null,"Oprawa wyposażona w wymienne źródło światła typu moduł LED, który zapewnia trwałość i optymalny rozsył światła, przy zachowaniu stosunkowo niskiego zużycia energii.",null,"Korpus- stal cynkowana ogniowo.","Klosz- poliwęglan przeźroczysty ze strukturą, stabilizowany UV.","Uszczelka silikonowa.","Podstawa- odlew aluminiowy malowany proszkowo.",null,null,"Oprawa ściemnialna fazowo TRAILING EDGE (TE) - LEADING EDGE (LE)","Moduł LED","Lumens EDC 57C 8W xxx 230V A FF Ver.1.0",null,null,null,null,80,null,null,"Zaciski podłączeniowe: max 3x2,5mm², możliwość podłączenia oprawy w pętle max 3x1,5mm². Przewód w oponie okrągłej o średnicy ø7...10,5mm.","5101XX0010.jpg","5101XX0010.ldt",1,null,1,76]
["5102","5102XX0010","ASKER WALL LED UP-DOWN 4000K DIM.","Asker","Wall","Aluminium",null,null,null,"LED zintegrowane","AC","DIM.","8W","8,8W",null,"329lm",null,null,"65","IK08","Class I",4000,"szerokie góra / szerokie dół",0.22,0.08,0.11,"CE",null,null,"50000",12,"Oprawa ścienna.","Światło dwustronne: ukierunkowane do góry i w dół.","Up-Down","A luminaire with a wide range of applications, including lighting wall surfaces, facades and other architectural concepts",null,null,null,"Odlew aluminiowy malowany proszkowo.",null,"Klosz- poliwęglan przeźroczysty ze strukturą, stabilizowany UV.","Uszczelka silikonowa.","Dławnica EPDM.",null,null,"Oprawa ściemnialna fazowo TRAILING EDGE (TE) - LEADING EDGE (LE)","Moduł LED","Lumens EDC 57C 8W xxx 230V F201 4K",null,0,"Ściemnianie fazowe Lumens LED AC",null,80,"E",null,"Zaciski podłączeniowe: max 3x2,5mm², możliwość podłączenia oprawy w pętle max 3x1,5mm². Przewód w oponie okrągłej o średnicy ø7...10,5mm.","5102XX0010.jpg","5102XX0010.ldt",1,null,1,4]
["5103","5103XX0010","ASKER WALL LED DOWN 4000K DIM.","Asker","Wall","Aluminium",null,null,null,"LED zintegrowane","AC","DIM.","8W","8,8W",null,"164lm",null,null,"65","IK08","Class I",4000,"szerokie dół",0.22,0.08,0.11,"CE",null,null,"50 000h",12,"Oprawa ścienna.","Światło rozproszone półsferyczne ukierunkowane w dół",null,"A luminaire with a wide range of applications, including lighting wall surfaces, facades and other architectural concepts",null,null,null,"Odlew aluminiowy malowany proszkowo.",null,"Klosz- poliwęglan przeźroczysty ze strukturą, stabilizowany UV.","Uszczelka silikonowa.","Dławnica EPDM.","dół",null,"Oprawa ściemnialna fazowo TRAILING EDGE (TE) - LEADING EDGE (LE)","Moduł LED","Lumens EDC 57C 8W xxx 230V F201 4K",null,0,"Ściemnianie fazowe Lumens LED AC",null,80,"E",null,"Zaciski podłączeniowe: max 3x2,5mm², możliwość podłączenia oprawy w pętle max 3x1,5mm². Przewód w oponie okrągłej o średnicy ø7...10,5mm.","5103XX0010.jpg","5103XX0010.ldt",1,null,1,76]
["5104","5104XX0010","ASKER BIG WALL LED 681LM DOWN 4000K DIM.","Asker,Big","Wall","Aluminium",null,null,null,"LED zintegrowane","AC","DIM.","4W","5,2W","681lm","362lm",null,null,"65","IK08","Class I",4000,"szerokie dół",0,0,0,"CE",null,null,"> 70 000",12,"Oprawa ścienna.","Światło rozproszone półsferyczne ukierunkowane w dół",null,"A luminaire with a wide range of applications, for lighting wall and facade surfaces as well as other architectural concepts.",null,null,null,"Odlew aluminiowy malowany proszkowo.",null,"Klosz- poliwęglan przeźroczysty ze strukturą, stabilizowany UV.","Uszczelka silikonowa.","Dławnica EPDM.","dół",null,"Oprawa ściemnialna fazowo TRAILING EDGE (TE)","Moduł LED","Philips Strip 0.5ft 490lm 8xx FC HV5","Philips Xitanium 7W 0,35A 20V TE SC 230V [2017]",50000,null,null,80,"C",null,"Zaciski podłączeniowe: max 3x2,5mm², możliwość podłączenia oprawy w pętle max 3x1,5mm². Przewód w oponie okrągłej o średnicy ø7...10,5mm.","5104XX0010.jpg","5104XX0010.ies",1,null,1,76]
["5105","5105XX0010","ASKER BIG PRO WALL 4XLED 2108LM UP-DOWN 4000K DIM.","Asker,Big","Wall","Aluminium",null,null,"PRO","LED zintegrowane","AC","DIM.","11,6W","13,7W","2108lm","1313lm",null,null,"65","IK08","Class I",4000,"szerokie góra / szerokie dół",0.3,0.12,0.12,"CE",null,null,"> 70 000h",12,"Oprawa ścienna.","Światło dwustronne: ukierunkowane do góry i w dół.","Up-Down","A luminaire with a wide range of applications, for illuminating wall and facade surfaces as well as other architectural concepts",null,null,null,"Odlew aluminiowy malowany proszkowo.",null,"Klosz- poliwęglan przeźroczysty ze strukturą, stabilizowany UV.","Uszczelka silikonowa.","Dławnica EPDM.","góra/dół",null,"Oprawa ściemnialna fazowo TRAILING EDGE (TE)","4 Moduły LED","Philips Fortimo Strip 0,5ft MF FC LV6 4K","Philips Xitanium 14W 0,35A 40V TE SC 230V",0,"Philips Xitanium TE",null,80,"C",null,"Zaciski podłączeniowe: max 3x2,5mm², możliwość podłączenia oprawy w pętle max 3x1,5mm². Przewód w oponie okrągłej o średnicy ø7...10,5mm.","5105XX0010.jpg","5105XX0010.ldt",1,null,1,4]
["5106","5106XX0010","ASKER BIG PRO WALL 2XLED 1196LM DOWN 4000K DIM.","Asker,Big","Wall","Aluminium",null,null,"PRO","LED zintegrowane","AC","DIM.","6,6W","8,5W","1196lm","782lm",null,null,"65","IK08","Class I",4000,"szerokie dół",0.3,0.12,0.12,"CE",null,null,"> 70 000h",12,"Oprawa ścienna.","Światło rozproszone półsferyczne ukierunkowane w dół",null,"A luminaire with a wide range of applications, for illuminating wall and facade surfaces as well as other architectural concepts",null,null,null,"Odlew aluminiowy malowany proszkowo.",null,"Klosz- poliwęglan przeźroczysty ze strukturą, stabilizowany UV.","Uszczelka silikonowa.","Dławnica EPDM.","dół",null,"Oprawa ściemnialna fazowo TRAILING EDGE (TE)","2 Moduły LED","Philips Fortimo Strip 0,5ft MF FC LV6 4K","Philips Xitanium 8W 0,2A 40V TE SC 230V",0,"Philips Xitanium TE",null,80,"C",null,"Zaciski podłączeniowe: max 3x2,5mm², możliwość podłączenia oprawy w pętle max 3x1,5mm². Przewód w oponie okrągłej o średnicy ø7...10,5mm.","5106XX0010.jpg","5106XX0010.ldt",1,null,1,76]
["5107","5107XX0012","MOLDE BOLLARD 80CM LED 772LM 4000K DIM.","Molde","Bollard","Aluminium",null,null,null,"LED zintegrowane","AC","DIM.","8W","8W","772lm","438lm",null,null,"54","IK07","Class I",4000,null,0.8,0.16,0.11,"CE",null,null,"50 000h",1,"Oprawa słupkowa.","Światło rozproszone przysłonięte od góry.",null,"Luminaire with contemporary design. For lighting private areas, parks and other architectural concepts",null,null,null,"Odlew aluminiowy malowany proszkowo.",null,"Klosz- poliwęglan przeźroczysty ze strukturą, stabilizowany UV.",null,null,"80cm",null,"Oprawa ściemnialna fazowo TRAILING EDGE (TE) - LEADING EDGE (LE)","Moduł LED","Lumens EDC 57C 8W xxx 230V F201 4K",null,0,"Ściemnianie fazowe Lumens LED AC",null,80,"F","1907ZX0009, 1908GA0009","Zaciski podłączeniowe: max 3x2,5mm², możliwość podłączenia oprawy w pętle max 3x1,5mm². Przewód w oponie okrągłej o średnicy max ø12,5mm.","5107XX0012.jpg","5107XX0012.ldt",1,null,1,25]
["510","510XX0009","HALDEN WALL E27 DOWN","Halden","Wall","Aluminium",null,null,null,"Wymienne","E27",null,"LED max 9W","LED max 9W",null,null,null,null,"65",null,"Class I",null,"szerokie dół",0.31,0.15,null,"CE",null,null,null,12,"Oprawa ścienna.","Światło rozproszone półsferyczne ukierunkowane w dół",null,"Luminaire with a wide range of applications for example for illumination of walls and facade surfaces or any other architectural concepts.",null,null,"Oprawa na wymienne źródło światła typu: lampa LED, świetlówka TC-SE, tradycyjna żarówka (halogenowa) o trzonku E27. Źródło światła należy dokupić oddzielnie.","Odlew aluminiowy malowany proszkowo.",null,"Klosz- poliwęglan przeźroczysty ze strukturą, stabilizowany UV.","Uszczelka silikonowa.","Dławnica EPDM.",null,null,null,"Lampa E27","LED A55..60",null,0,null,null,80,null,null,"Zaciski podłączeniowe: max 3x2,5mm², możliwość podłączenia oprawy w pętle max 3x1,5mm². Przewód w oponie okrągłej o średnicy ø7...10,5mm.","510XX0009.jpg","510XX0009.ldt",4,"E27",1,76]
["5110","5110XX0009","STOCKHOLM WALL LED 961LM 4000K DIM.","Stockholm,Połówka","Wall,Ceiling","Stal",null,null,null,"LED zintegrowane","AC","DIM.","8W","8W","961lm","362lm",null,null,"54","IK10","Class I",4000,null,null,null,null,"CE",null,null,"50000",12,"Oprawa ścienna.","Światło rozproszone.",null,"Scandinavian design luminaire. For lighting gardens, private areas and public spaces.",null,null,"Oprawa wyposażona w wymienne źródło światła typu moduł LED, który zapewnia trwałość i optymalny rozsył światła, przy zachowaniu stosunkowo niskiego zużycia energii.",null,"Front- stal cynkowana ogniowo, stal malowana proszkowo.","Klosz- poliwęglan mleczny, stabilizowany UV.","Uszczelka silikonowa.","Podstawa- odlew aluminiowy malowany proszkowo.",null,"mleczny","Oprawa ściemnialna fazowo TRAILING EDGE (TE) - LEADING EDGE (LE)","Moduł LED","Lumens EDC 57C 8W xxx 230V A FF Ver.1.0",null,0,null,null,80,null,null,"Zaciski podłączeniowe: max 3x2,5mm², możliwość podłączenia oprawy w pętle max 3x1,5mm². Przewód w oponie okrągłej o średnicy ø7...10,5mm.","5110XX0009.jpg","5110XX0009.ldt",1,null,1,7]
["5113","5113XX0009","SKI WALL LED 681LM DOWN 4000K DIM.","Ski","Wall","Stal",null,null,null,"LED zintegrowane","AC","DIM.","4W","5,4W","681lm","432lm",null,null,"44","IK09","Class I",4000,"szerokie dół",0.2,0.14000000000000001,0.13,"CE",null,null,"> 70 000h",12,"Oprawa ścienna.","Światło rozproszone półsferyczne ukierunkowane w dół",null,"Luminaire with a wide range of applications for example for illumination of walls and facade surfaces or any other architectural concepts",null,null,null,null,"Front- stal cynkowana ogniowo lub stal malowana proszkowo.","Klosz- poliwęglan przeźroczysty ze strukturą, stabilizowany UV.","Uszczelka silikonowa.","Podstawa- stal cynkowana ogniowo.",null,null,"Oprawa ściemnialna fazowo TRAILING EDGE (TE)","Moduł LED","Philips Strip OC 0.5ft 550lm 8xx FC HV5 4K","Philips Xitanium 7W 0,35A 20V TE SC 230V [2019]",50000,"Philips Xitanium TE",null,80,"C",null,"Zaciski podłączeniowe: max 3x2,5mm², możliwość podłączenia oprawy w pętle max 3x1,5mm². Przewód w oponie okrągłej o średnicy ø7...10,5mm.","5113XX0009.jpg","5113XX0009.ldt",1,null,1,76]
["5114","5114XX0009","HITRA WALL LED 1150LM 4000K ON/OFF","Hitra","Wall","Aluminium",null,null,null,"LED zintegrowane","AC","ON/OFF","9,5W","9,5W","1150lm","979lm",null,null,"65","IK06","Class I",4000,"szerokie dół",0.2,0.15,0.06,"CE",null,null,"50000",12,"Oprawa ścienna.","Światło rozproszone półsferyczne ukierunkowane w dół",null,"Modern design luminaire. For lighting private areas and public spaces.",null,null,null,"Odlew aluminiowy malowany proszkowo.",null,"Klosz- szkło bezpieczne, przeźroczyste.","Uszczelka silikonowa.","Dławnica EPDM.",null,null,"Oprawa nieściemnialna","Moduł LED","Philips Fortimo DLM ES 1100/8xx G2 4K",null,0,null,0,80,"D","151XX0009","Zaciski podłączeniowe: max 3x2,5mm², możliwość podłączenia oprawy w pętle max 3x1,5mm². Przewód w oponie okrągłej o średnicy ø7...10,5mm.","5114XX0009.jpg","5114XX0009.ldt",4,null,1,76]
["5115","5115XX0009","HITRA WALL LED 2050LM 4000K ON/OFF","Hitra","Wall","Aluminium",null,null,null,"LED zintegrowane","AC","ON/OFF","17,5W","17,5W","2050lm","1717lm",null,null,"65","IK06","Class I",4000,"szerokie dół",0.2,0.15,0.06,"CE",null,null,"50000",12,"Oprawa ścienna.","Światło rozproszone półsferyczne ukierunkowane w dół",null,"Luminaire with contemporary design. For lighting private areas and other architectural concepts",null,null,null,"Odlew aluminiowy malowany proszkowo.",null,"Klosz- szkło bezpieczne, przeźroczyste.","Uszczelka silikonowa.","Dławnica EPDM.",null,null,"Oprawa nieściemnialna","Moduł LED","Philips Fortimo DLM ES 2000/8xx G2 4K",null,0,null,0,80,"D","151XX009","Zaciski podłączeniowe: max 3x2,5mm², możliwość podłączenia oprawy w pętle max 3x1,5mm². Przewód w oponie okrągłej o średnicy ø7...10,5mm.","5115XX0009.jpg","5115XX0009.ldt",4,null,1,76]
["5116","5116XX0009","NAMSOS WALL-RECESSED LED 4000K DIM.","Namsos","Recessed","Stal",null,null,null,"LED zintegrowane","AC","DIM.","4W","5,2W",null,"689lm",null,null,"44","IK10","Class I",4000,null,0,0,0,"CE",null,null,"> 70000",11,"Oprawa wbudowana ścienna.","Światło rozproszone półsferyczne ukierunkowane w dół",null,"Luminaire designed to illuminate stairs, steps, staircases, communication lines, ceiling illumination and many other architectural applications.",null,null,"Oprawa wyposażona w wymienne źródło światła typu moduł LED, który zapewnia trwałość i optymalny rozsył światła, przy zachowaniu stosunkowo niskiego zużycia energii.","Front- stal cynkowana ogniowo.","Korpus- odlew aluminiowy malowany proszkowo.","Klosz- szkło bezpieczne, satynowane.","Uszczelka silikonowa.","Dławnica EPDM.",null,null,"Oprawa ściemnialna fazowo TRAILING EDGE (TE)","Moduł LED","Philips Strip 0.5ft 550lm 840 FC HV4","Philips Xitanium 7W 0.35A 20V TE SC 230V",0,null,null,80,null,null,"Zaciski podłączeniowe: max 3x2,5mm², możliwość podłączenia oprawy w pętle max 3x1,5mm². Przewód w oponie okrągłej o średnicy ø7...10,5mm.","5116XX0009.jpg","5116XX0009.ldt",1,null,1,76]
["5117","5117XX0010","EGERSUND MINI BOLLARD 85CM LED 1462LM 4000K DIM.","Egersund Mini","Bollard","Aluminium",null,null,null,"LED zintegrowane","AC","DIM.","7,4W","9,1W","1462lm","917lm",null,null,"65","IK08","Class II",4000,null,0,0,0,"CE",null,null,"> 72 000h",1,"Oprawa słupkowa.","Światło obrotowo-symetryczne.",null,"Luminaire with contemporary design For lighting gardens and other private and public areas",null,null,null,"Odlew aluminiowy malowany proszkowo.",null,"Klosz- tworzywo sztuczne PMMA przeźroczyste.","Uszczelka silikonowa.","Dławnica nylon6.","85cm",null,"Oprawa ściemnialna fazowo TRAILING EDGE (TE) - LEADING EDGE (LE)","Moduł LED","Cree DK210704 V2 JB2835 3V 4K","TCI MICRO MD 10W 350mA 127040 Triac",0,null,null,80,"C","205ZX0010, 206GA0010, 206GA0S10, 2951ZX0009, 6138ZX0009","Zaciski podłączeniowe: max 2x4mm², możliwość podłączenia oprawy w pętle max 2x2,5mm². Przewód w oponie okrągłej o średnicy ø8...12,5mm","5117XX0010.jpg","5117XX0010.ldt",1,null,1,17]
["5118","5118XX0010","EGERSUND MINI BOLLARD 49CM LED 1462LM 4000K DIM.","Egersund Mini","Bollard","Aluminium",null,null,null,"LED zintegrowane","AC","DIM.","7,4W","9,1W","1462lm","917lm",null,null,"65","IK08","Class II",4000,null,0,0,0,"CE",null,null,"> 72 000h",1,"Oprawa słupkowa.","Światło obrotowo-symetryczne.",null,"Luminaire with contemporary design For lighting gardens, private areas, parks, and other architectural concepts",null,null,null,"Odlew aluminiowy malowany proszkowo.",null,"Klosz- tworzywo sztuczne PMMA przeźroczyste.","Uszczelka silikonowa.","Dławnica nylon6.","49cm",null,"Oprawa ściemnialna fazowo TRAILING EDGE (TE) - LEADING EDGE (LE)","Moduł LED","Cree DK210704 V2 JB2835 3V 4K","TCI MICRO MD 10W 350mA 127040 Triac",0,null,null,80,"C","205ZX0010, 206GA0010, 206GA0S10, 2951ZX0009, 6138ZX0009","Zaciski podłączeniowe: max 2x4mm², możliwość podłączenia oprawy w pętle max 2x2,5mm². Przewód w oponie okrągłej o średnicy ø8...12,5mm.","5118XX0010.jpg","5118XX0010.ldt",1,null,1,17]
["5120","5120XX0009","ASKER BOLLARD 55CM LED 1100LM 4000K ON/OFF","Asker","Bollard","Aluminium",null,null,null,"LED zintegrowane","AC","ON/OFF","9,5W","9,5W","1100lm","636lm",null,null,"65","IK09","Class I",4000,"szerokie dół",null,null,null,"CE",null,null,"50 000h",1,"Oprawa słupkowa.","Światło rozproszone półsferyczne ukierunkowane w dół",null,"Luminaire with contemporary design. For lighting private areas and other architectural concepts",null,null,null,"Odlew aluminiowy malowany proszkowo.",null,"Klosz- poliwęglan przeźroczysty ze strukturą, stabilizowany UV.","Uszczelka silikonowa.","Dławnica EPDM.","55cm",null,"Oprawa nieściemnialna","Moduł LED","Philips Fortimo DLM ES 1100/8xx G2 4K",null,0,null,0,80,"D","1907ZX0009, 1908GA0009, 3081XX0009","Zaciski podłączeniowe: max 3x2,5mm², możliwość podłączenia oprawy w pętle max 3x1,5mm². Przewód w oponie okrągłej o średnicy max ø12,5mm.","5120XX0009.jpg","5120XX0009.ldt",4,null,1,76]
["5121","5121XX0011","BORNHOLM CEILING/WALL LED 1121LM 4000K DIM.","Bornholm","Wall,Ceiling","Aluminium",null,null,null,"LED zintegrowane","AC","DIM.","6,7W","7,8W","1121lm","443lm",null,null,"65","IK10","Class I",4000,null,0,0,0,"CE",null,null,"> 50 000h",7,"Oprawa sufitowo-ścienna.","Światło rozproszone.",null,"A ceiling-type luminaire with a modern design",null,null,null,"Odlew aluminiowy malowany proszkowo.",null,"Klosz- poliwęglan mleczny, stabilizowany UV.","Uszczelka silikonowa.","Dławnica EPDM.",null,null,"Oprawa ściemnialna fazowo TRAILING EDGE (TE) - LEADING EDGE (LE)","Moduł LED","Philips Fortimo SLM C 1203 L09 1619 G7 4K","KGP CC15W200-350CG",50000,"Dim. TRIAC (KGP)",null,80,"D",null,"Zaciski podłączeniowe: max 3x2,5mm², możliwość podłączenia oprawy w pętle max 3x1,5mm². Przewód w oponie okrągłej o średnicy ø7...10,5mm.","5121XX0011.jpg","5121XX0011.ldt",1,null,1,7]
["5122","5122XX0010","BORNHOLM CEILING/WALL LED 2050LM 4000K ON/OFF","Bornholm","Wall,Ceiling","Aluminium",null,null,null,"LED zintegrowane","AC","ON/OFF","17,5W","17,5W","2050lm","836lm",null,null,"65","IK10","Class I",4000,null,0,0,0,"CE",null,null,"50 000h",7,"Oprawa sufitowo-ścienna.","Światło rozproszone.",null,"A ceiling lamp with a modern design",null,null,null,"Odlew aluminiowy malowany proszkowo.",null,"Klosz- poliwęglan mleczny, stabilizowany UV.","Uszczelka silikonowa.","Dławnica EPDM.",null,null,"Oprawa nieściemnialna","Moduł LED","Philips Fortimo DLM ES 2000/8xx G2 4K",null,null,null,null,80,"D",null,"Zaciski podłączeniowe: max 3x2,5mm², możliwość podłączenia oprawy w pętle max 3x1,5mm². Przewód w oponie okrągłej o średnicy ø7...10,5mm.","5122XX0010.jpg","5122XX0010.ldt",4,null,1,7]
["5123","5123XX0009","OPPLAND BOLLARD LED 1371LM 4000K DIM.","Oppland","Bollard","Aluminium",null,null,null,"LED zintegrowane","AC","DIM.","8,5W","9,3W","1371lm","322lm",null,null,"65","IK09","Class I",4000,null,0,0,0,"CE",null,null,"> 50000h",1,"Oprawa słupkowa.","Światło rozproszone półsferyczne ukierunkowane w dół",null,"Bollard luminaire of stable and durable construction. For lighting private areas and public spaces. IP of lighting chamber - 65.",null,null,"Oprawa wyposażona w wymienne źródło światła typu moduł LED, który zapewnia trwałość i optymalny rozsył światła, przy zachowaniu stosunkowo niskiego zużycia energii.","Odlew aluminiowy malowany proszkowo.",null,"Klosz- poliwęglan przeźroczysty ze strukturą, stabilizowany UV.","Uszczelka silikonowa.","Dławnica nylon6.",null,null,"Oprawa ściemnialna fazowo TRAILING EDGE (TE)","Moduł LED","Philips SLM C 840 1203 L09 1619 G7","Philips Xitanium 10W 0.25A 40V TE SC 230V",0,null,0,80,"D","205ZX0010, 206GA0010, 206GA0S10","Zaciski podłączeniowe: max 3x2,5mm², możliwość podłączenia oprawy w pętle max 3x1,5mm². Przewód w oponie okrągłej o średnicy max ø12,5mm.","5123XX0009.jpg","5123XX0009.ldt",1,null,1,76]
["5123","5123XX0011","OPPLAND BOLLARD LED 1090LM 4000K DIM.","Oppland","Bollard","Aluminium",null,null,null,"LED zintegrowane","AC","DIM.","6,1W","8,2W","1090lm","313lm",null,null,"65","IK09","Class II",4000,"szerokie dół",0.85,0.12,0.12,"CE",null,null,"> 102 000h",1,"Oprawa słupkowa.","Światło rozproszone półsferyczne ukierunkowane w dół",null,"A bollard luminaire with a stable and durable construction. For lighting private areas and other architectural concepts",null,null,null,"Odlew aluminiowy malowany proszkowo.",null,"Klosz- poliwęglan przeźroczysty ze strukturą, stabilizowany UV.","Uszczelka silikonowa.","Dławnica nylon6.",null,null,"Oprawa ściemnialna fazowo TRAILING EDGE (TE) - LEADING EDGE (LE)","Moduł LED","Cree DK180501 V8 JB2835 3V 4K","TCI Micro MD 10W 700mA code 127046 Triac",0,null,0,80,"C","205ZX0010, 206GA0010, 206GA0S10","Zaciski podłączeniowe: max 2x4mm², możliwość podłączenia oprawy w pętle max 2x4mm². Przewód w oponie okrągłej o średnicy: ø4…8mm; ø8...12mm lub ø10...13,6mm.","5123XX0011.jpg","5123XX0011.ldt",1,null,1,76]
["5124","5124XX0010","ASKER BOLLARD LED 1150LM 4000K","Asker","Bollard","Aluminium",null,null,null,"LED zintegrowane","AC",null,"9,5W","9,5W","1150lm","640lm",null,null,"65","IK09","Class I",4000,null,0,0,0,"CE",null,null,"50000",1,"Oprawa słupkowa.","Światło rozproszone półsferyczne ukierunkowane w dół",null,"Luminaire with contemporary design. For lighting gardens and other private land and public areas",null,null,"Oprawa wyposażona w wymienne źródło światła typu moduł LED, który zapewnia trwałość i optymalny rozsył światła, przy zachowaniu stosunkowo niskiego zużycia energii.","Odlew aluminiowy malowany proszkowo.",null,"Klosz- poliwęglan przeźroczysty ze strukturą, stabilizowany UV.","Uszczelka silikonowa.",null,null,null,"Oprawa nieściemnialna","Moduł LED","Philips Fortimo LED DLM ES 1100 lm G2",null,null,null,0,80,"D","1907ZX0009, 1908GA0009, 3081XX0009","Zaciski podłączeniowe: max 3x2,5mm², możliwość podłączenia oprawy w pętle max 3x1,5mm². Przewód w oponie okrągłej o średnicy max ø12,5mm.","5124XX0010.jpg","5124XX0010.ldt",4,null,1,76]
["5126","5126XX0009","ASKER POLE LIGHT LUMINAIRES POLE 216CM 2XLED 1778LM 4000K DIM.","Asker","Post,Post complete","Aluminium",null,null,null,"LED zintegrowane","AC","DIM.","18W","18W","1778lm","1100lm",null,null,"65","IK09","Class I",4000,"szerokie dół",0,0,0,"CE",null,null,"50 000h",20,"Oprawa słupowa (lekka konstrukcja).","Światło ukierunkowane w dół.",null,"Luminaire for lighting private areas, and other architectural concepts. The tightness of the lighting and connection chamber is IP65.",null,null,null,"Profil aluminiowy wyciskany, malowany proszkowo.",null,"Klosz- poliwęglan przeźroczysty ze strukturą, stabilizowany UV.","Uszczelka silikonowa.",null,"216cm","dwu-segmentowy","Oprawa ściemnialna fazowo TRAILING EDGE (TE) - LEADING EDGE (LE)","2 Moduły LED","Lumens LNM/280X30/9W/830/230V",null,null,"Ściemnianie fazowe Lumens LED AC",0,80,null,"116ZX0009, 117GA0009, 118GA0009, 119ZX0009, 7666ZX0009","Zaciski podłączeniowe: max 3x2,5mm², możliwość podłączenia oprawy w pętle max 3x2,5mm². Przewód w oponie okrągłej o średnicy max ø12,5mm.","5126XX0009.jpg","5126XX0009.ldt",1,null,1,45]
["5127","5127XX0010","ASKER POLE LIGHT LUMINAIRES POLE 2XLED 1778LM 4000K DIM.","Asker","Post,Post complete","Aluminium",null,null,null,"LED zintegrowane","AC","DIM.","18W","18W","1778lm","1100lm",null,null,"65","IK09","Class I",4000,"szerokie dół",0.11,2.36,0.39,"CE",null,null,"50000",20,"Oprawa słupowa (lekka konstrukcja).","Światło jednostronne: symetryczne, ukierunkowane w dół.",null,"For lighting private areas and other concepts architectural",null,null,null,"Profil aluminiowy wyciskany, malowany proszkowo.",null,"Klosz- poliwęglan przeźroczysty ze strukturą, stabilizowany UV.","Uszczelka silikonowa.",null,null,"jedno-segmentowy","Oprawa ściemnialna fazowo TRAILING EDGE (TE) - LEADING EDGE (LE)","2 Moduły LED","Lumens LNM/280X30/9W/840/230V",null,0,"Ściemnianie fazowe Lumens LED AC",0,80,null,"116ZX0009, 117GA0009, 118GA0009, 119ZX0009, 7666ZX0009","Zaciski podłączeniowe: max 3x2,5mm², możliwość podłączenia oprawy w pętle max 3x2,5mm². Przewód w oponie okrągłej o średnicy max ø12,5mm.","5127XX0010.jpg","5127XX0010.ldt",1,null,1,27]
["5128","5128XX0C10","VOSS WALL LED 767LM UP 4º 4000K DIM.","Voss","Wall","Aluminium",null,null,null,"LED zintegrowane","AC","DIM.","4,5W","6,4W","767lm","55lm",null,null,"54","IK06","Class I",4000,"wąskie góra",0.18,0.16,0.27,"CE",null,null,"> 102 000h",12,"Oprawa ścienna.","Światło jednostronne: o kącie 4º do góry.","Up 4º","A luminaire with a wide range of applications, for lighting: walls and facade surfaces and other architectural concepts",null,null,null,"Odlew aluminiowy malowany proszkowo.",null,"Klosz- szkło bezpieczne, przeźroczyste.","Uszczelka silikonowa.","Dławnica EPDM.","góra","wąskie jednostronne","Oprawa ściemnialna fazowo TRAILING EDGE (TE)","Moduł LED","Cree DK180501 V8 JB2835 3V 4K","Philips Xitanium 10W 0,5A 20V TE SC 230V",0,"Philips Xitanium TE",null,80,"C",null,"Zaciski podłączeniowe: max 3x2,5mm², możliwość podłączenia oprawy w pętle max 3x1,5mm². Przewód w oponie okrągłej o średnicy ø7...10,5mm.","5128XX0C10.jpg","5128XX0C10.ldt",1,null,1,39]
["5130","5130XX0010","HAMMERFEST POLE-TOP LED 4503LM 4000K ON/OFF","Hammerfest","Post,Head","Aluminium",null,null,null,"LED zintegrowane","AC","ON/OFF","28,9W","32W","4503lm","3933lm",null,null,"65","IK07","Class I",4000,"szerokie dół",0.55000000000000004,0.76,0.55000000000000004,"CE",null,null,"> 72 000h",2,"Oprawa słupowa (nasadzana).","Światło rozproszone przysłonięte od góry.",null,"A mounted luminaire designed to be mounted on a lighting pole with Ø60mm mounting shaft",null,null,null,"Odlew aluminiowy malowany proszkowo.",null,"Klosz- tworzywo sztuczne PMMA satynowane.","Uszczelka silikonowa.",null,null,"satynowany","Oprawa nieściemnialna","Moduł LED","Cree DK190707 V2 JK3030 4K","Philips Xi BP 40W 0.3-1.0A S 230V C123_sXt",100000,null,0.02,80,"E","3004XX0009, 3005XX0009, 7661ZX0009, 7663ZX0009, 7664ZX0009, 7665XX0009","Przewód H05RN-F 3G1 o długości 6m do podłączenia w odpowiednio dobranej puszce elektroinstalacyjnej.","5130XX0010.jpg","5130XX0010.ldt",4,null,1,25]
["5131","5131XX0009","HAMMERFEST POLE-TOP LED 4311LM 3000K DALI2","Hammerfest","Post,Head","Aluminium",null,null,null,"LED zintegrowane","AC","DALI2","28,8W","32,5W","4311lm","3974lm",null,null,"65","IK07","Class I",3000,"szerokie dół",0.76,0.55000000000000004,0.55000000000000004,"CE",null,"DALI","> 72 000h",2,"Oprawa słupowa (nasadzana).","Światło ukierunkowane w dół.",null,"Luminaire mounted on a telescopic lighting pole with a diameter Ø60mm. Other components need to be ordered separately",null,null,null,"Odlew aluminiowy malowany proszkowo.",null,"Klosz- tworzywo sztuczne PMMA satynowane.","Uszczelka silikonowa.",null,null,"satynowany","Sterowanie światłem w systemie: DALI outdoor pełny program. Zasilacz zaprogramowany na max prąd. Programowanie pozostałych parametrów po uzgodnieniu z Działem Handlowym firmy Norlys.","Moduł LED","Cree DK190707 V2 JK3030 3K","Osram OT 40/170-240/1A0 4DIMLT2 NFC E",100000,"DALI2 / NightDim (4DIM)",0.02,80,"E","3004XX0009, 3005XX0009, 7661ZX0009, 7663ZX0009, 7664ZX0009, 7665XX0009","Przewód H05RN-F 6G1 o długości 6m do podłączenia w słupie, w odpowiednio dobranej puszce elektroinstalacyjnej.","5131XX0009.jpg","5131XX0009.ldt",3,null,1,45]
["5132","5132XX0009","HAMMERFEST POLE-TOP LED 4503LM 4000K DALI2","Hammerfest","Post,Head","Aluminium",null,null,null,"LED zintegrowane","AC","DALI2","28,8W","32,5W","4503lm","3721lm",null,null,"65","IK07","Class I",4000,"szerokie dół",0.76,0.55000000000000004,0.55000000000000004,"CE",null,"DALI","> 72 000h",2,"Oprawa słupowa (nasadzana).","Światło ukierunkowane w dół.",null,"Luminaire mounted on a telescopic lighting pole with a diameter Ø60mm. Other components need to be ordered separately",null,null,null,"Odlew aluminiowy malowany proszkowo.",null,"Klosz- tworzywo sztuczne PMMA satynowane.","Uszczelka silikonowa.",null,null,"satynowany","Sterowanie światłem w systemie: DALI outdoor pełny program. Zasilacz zaprogramowany na max prąd. Programowanie pozostałych parametrów po uzgodnieniu z Działem Handlowym firmy Norlys.","Moduł LED","Cree DK190707 V2 JK3030 3K","Osram OT 40/170-240/1A0 4DIMLT2 NFC E",100000,"DALI2 / NightDim (4DIM)",0.02,80,"E","3004XX0009, 3005XX0009, 7661ZX0009, 7663ZX0009, 7664ZX0009, 7665XX0009","Przewód H05RN-F 6G1 o długości 6m do podłączenia w słupie, w odpowiednio dobranej puszce elektroinstalacyjnej.","5132XX0009.jpg","5132XX0009.ldt",3,null,1,45]
["5135","5135XX0010","HAMMERFEST POLE-TOP LED 4503LM 4000K ON/OFF","Hammerfest","Post,Head","Aluminium",null,null,null,"LED zintegrowane","AC","ON/OFF","28,9W","32,3W","4503lm","3320lm",null,null,"65","IK07","Class I",4000,"szerokie dół",0.55000000000000004,0.55000000000000004,0.76,"CE",null,null,"> 72 000h",2,"Oprawa słupowa (nasadzana).","Światło rozproszone przysłonięte od góry.",null,"Modern design luminaire mounted on a lighting pole with a cap diameter Ø60mm",null,null,"Oprawa wyposażona w źródło światła typu moduł LED.","Odlew aluminiowy malowany proszkowo.",null,"Klosz- tworzywo sztuczne PMMA w kolorze mlecznym.","Uszczelka silikonowa.",null,null,"mleczny","Oprawa nieściemnialna","Moduł LED","Cree DK190707 V2 JK3030 4K","Philips Xi BP 40W 0.3-1.0A S 230V C123_sXt",100000,null,0.02,80,"E","3004XX0009, 3005XX0009, 7661ZX0009, 7663ZX0009, 7664ZX0009, 7665XX0009","Przewód H05RN-F 3G1 o długości 6m do podłączenia w odpowiednio dobranej puszce elektroinstalacyjnej.","5135XX0010.jpg","5135XX0010.ldt",4,null,1,25]
["5136","5136XX0009","HAMMERFEST POLE-TOP LED 4311LM 3000K DALI2","Hammerfest","Post,Head","Aluminium",null,null,null,"LED zintegrowane","AC","DALI2","28,8W","32,5W","4311lm","3117lm",null,null,"65","IK07","Class I",3000,"szerokie dół",0.76,0.55000000000000004,0.55000000000000004,"CE",null,"DALI","> 72 000h",2,"Oprawa słupowa (nasadzana).","Światło ukierunkowane w dół.",null,"Luminaire mounted on a telescopic lighting pole with a diameter Ø60mm. Other components need to be ordered separately",null,null,null,"Odlew aluminiowy malowany proszkowo.",null,"Klosz- tworzywo sztuczne PMMA w kolorze mlecznym.","Uszczelka silikonowa.",null,null,"mleczny","Sterowanie światłem w systemie: DALI outdoor pełny program. Zasilacz zaprogramowany na max prąd. Programowanie pozostałych parametrów po uzgodnieniu z Działem Handlowym firmy Norlys.","Moduł LED","Cree DK190707 V2 JK3030 3K","Osram OT 40/170-240/1A0 4DIMLT2 NFC E",100000,"DALI2 / NightDim (4DIM)",0.02,80,"E","3004XX0009, 3005XX0009, 7661ZX0009, 7663ZX0009, 7664ZX0009, 7665XX0009","Przewód H05RN-F 6G1 o długości 6m do podłączenia w słupie, w odpowiednio dobranej puszce elektroinstalacyjnej.","5136XX0009.jpg","5136XX0009.ldt",3,null,1,45]
["5137","5137XX0009","HAMMERFEST POLE-TOP LED 4503LM 4000K DALI2","Hammerfest","Post,Head","Aluminium",null,null,null,"LED zintegrowane","AC","DALI2","28,8W","32,5W","4503lm","3310lm",null,null,"65","IK07","Class I",4000,"szerokie dół",0.76,0.55000000000000004,0.55000000000000004,"CE",null,"DALI","> 72 000h",2,"Oprawa słupowa (nasadzana).","Światło ukierunkowane w dół.",null,"Luminaire mounted on a telescopic lighting pole with a diameter Ø60mm. Other components need to be ordered separately",null,null,null,"Odlew aluminiowy malowany proszkowo.",null,"Klosz- tworzywo sztuczne PMMA w kolorze mlecznym.","Uszczelka silikonowa.",null,null,"mleczny","Sterowanie światłem w systemie: DALI outdoor pełny program. Zasilacz zaprogramowany na max prąd. Programowanie pozostałych parametrów po uzgodnieniu z Działem Handlowym firmy Norlys.","Moduł LED","Cree DK190707 V2 JK3030 3K","Osram OT 40/170-240/1A0 4DIMLT2 NFC E",100000,"DALI2 / NightDim (4DIM)",0.02,80,"E","3004XX0009, 3005XX0009, 7661ZX0009, 7663ZX0009, 7664ZX0009, 7665XX0009","Przewód H05RN-F 6G1 o długości 6m do podłączenia w słupie, w odpowiednio dobranej puszce elektroinstalacyjnej.","5137XX0009.jpg","5137XX0009.ldt",3,null,1,45]
["5140","5140XX0009","BORG POLE-TOP LED 4380LM 4000K ON/OFF","Borg","Post,Head","Aluminium",null,null,null,"LED zintegrowane","AC","ON/OFF","27,2W","32W","4380lm","3928lm",null,null,"65","IK08","Class I",4000,"szerokie dół",0,0,0,"CE",null,null,"> 72 000h",2,"Oprawa słupowa (nasadzana).","Światło ukierunkowane w dół.",null,"Mounted on a telescopic lighting pole with a cap diameter Ø60mm. Other accessories have to be ordered separately.",null,null,null,"Odlew aluminiowy malowany proszkowo.",null,"Klosz- tworzywo sztuczne PMMA satynowane.","Uszczelka silikonowa.",null,"on/off","satynowany","Oprawa nieściemnialna","Moduł LED","Cree DK190804 V2 JK3030 3V 4K","Philips Xi BP 40W 0.3-1.0A S 230V C123_sXt",100000,null,0,80,"D","3004XX0009, 3005XX0009, 7661ZX0009, 7663ZX0009, 7664ZX0009, 7665XX0009","Przewód H05RN-F 3G1 o długości 6m do podłączenia w odpowiednio dobranej puszce elektroinstalacyjnej.","5140XX0009.jpg","5140XX0009.ldt",4,null,1,45]
["5142","5142XX0009","BORG POLE-TOP LED 4380LM 4000K DALI2","Borg","Post,Head","Aluminium",null,null,null,"LED zintegrowane","AC","DALI2","27,2W","32,6W","4380lm","3970lm",null,null,"65","IK08","Class I",4000,"szerokie dół",0,0,0,"CE",null,"DALI","> 72 000h",2,"Oprawa słupowa (nasadzana).","Światło ukierunkowane w dół.",null,"Luminaire mounted on a telescopic lighting pole with a shaft diameter of Ø60mm",null,null,null,"Odlew aluminiowy malowany proszkowo.",null,"Klosz- tworzywo sztuczne PMMA satynowane.","Uszczelka silikonowa.",null,null,null,"Sterowanie światłem w systemie: DALI outdoor pełny program. Zasilacz zaprogramowany na max prąd. Programowanie pozostałych parametrów po uzgodnieniu z Działem Handlowym firmy Norlys.","Moduł LED","Cree DK190804 V2 JK3030 3V 3K","Philips Xi FP 40W 0.3-1.0A SNLDAE 230V C123 sXt",100000,"DALI2 / NightDim (XI FP NLD)",0,80,"D","3004XX0009, 3005XX0009, 7661ZX0009, 7663ZX0009, 7664ZX0009, 7665XX0009","Przewód H05RN-F 6G1 o długości 6m do podłączenia w odpowiednio dobranej puszce elektroinstalacyjnej.","5142XX0009.jpg","5142XX0009.ldt",3,null,1,45]
["5145","5145XX0009","BORG POLE-TOP LED 4380LM 4000K ON/OFF","Borg","Post,Head","Aluminium",null,null,null,"LED zintegrowane","AC","ON/OFF","27,2W","32W","4380lm","3069lm",null,null,"65","IK08","Class I",4000,"szerokie dół",0,0,0,"CE",null,null,"> 72 000",2,"Oprawa słupowa (nasadzana).","Światło ukierunkowane w dół.",null,"Modern design luminaire mounted on a telescopic lighting pole with a cap diameter Ø60mm. Other accessories need to be purchased separately.",null,null,null,"Odlew aluminiowy malowany proszkowo.",null,"Klosz- tworzywo sztuczne PMMA w kolorze mlecznym.","Uszczelka silikonowa.",null,"on/off","mleczny","Oprawa nieściemnialna","Moduł LED","Cree DK190804 V2 JK3030 3V 4K","Philips Xi BP 40W 0.3-1.0A S 230V C123_sXt",100000,null,0,80,"D","3004XX0009, 3005XX0009, 7661ZX0009, 7663ZX0009, 7664ZX0009, 7665XX0009","Przewód H05RN-F 3G1 o długości 6m do podłączenia w odpowiednio dobranej puszce elektroinstalacyjnej.","5145XX0009.jpg","5145XX0009.ldt",4,null,1,45]
["5147","5147XX0009","BORG POLE-TOP LED 4380LM 4000K DALI2","Borg","Post,Head","Aluminium",null,null,null,"LED zintegrowane","AC","DALI2","27,2W","32,6","4380lm","3194lm",null,null,"65","IK08","Class I",4000,"szerokie dół",0,0,0,"CE",null,"DALI","> 72 000h",2,"Oprawa słupowa (nasadzana).","Światło ukierunkowane w dół.",null,"Luminaire mounted on a telescopic lighting pole with a shaft diameter of Ø60mm",null,null,null,"Odlew aluminiowy malowany proszkowo.",null,"Klosz- tworzywo sztuczne PMMA w kolorze mlecznym.","Uszczelka silikonowa.",null,null,null,"Sterowanie światłem w systemie: DALI outdoor pełny program. Zasilacz zaprogramowany na max prąd. Programowanie pozostałych parametrów po uzgodnieniu z Działem Handlowym firmy Norlys.","Moduł LED","Cree DK190804 V2 JK3030 3V 3K","Philips Xi FP 40W 0.3-1.0A SNLDAE 230V C123 sXt",100000,"DALI2 / NightDim (XI FP NLD)",0,80,"D","3004XX0009, 3005XX0009, 7661ZX0009, 7663ZX0009, 7664ZX0009, 7665XX0009","Przewód H05RN-F 6G1 o długości 6m do podłączenia w odpowiednio dobranej puszce elektroinstalacyjnej.","5147XX0009.jpg","5147XX0009.ldt",3,null,1,45]
["5147","5147XX0010","BORG POLE-TOP LED 4380LM 4000K DALI2","Borg","Post,Head","Aluminium",null,null,null,"LED zintegrowane","AC","DALI2","27,2W","32W","4380lm","3183lm",null,null,"65",null,"Class I",4000,"szerokie dół",0.15,0.51,0.51,"CE",null,"DALI","> 72 000h",2,"Oprawa słupowa (nasadzana).","Światło ukierunkowane w dół.",null,"A mounted luminaire designed to be mounted on a lighting pole with Ø60mm mounting shaft",null,null,null,"Odlew aluminiowy malowany proszkowo.",null,"Klosz- poliwęglan mleczny, stabilizowany UV.","Uszczelka silikonowa.",null,null,null,"Sterowanie światłem w systemie: DALI outdoor pełny program. Zasilacz zaprogramowany na max prąd. Programowanie pozostałych parametrów po uzgodnieniu z Działem Handlowym firmy Norlys.","Moduł LED","Cree DK190804 V2 JK3030 3V 4K","Osram OT 40/170-240/1A0 4DIMLT2 NFC E",100000,"DALI2 / NightDim (4DIM)",0,80,"D","3004XX0009, 3005XX0009, 7661ZX0009, 7663ZX0009, 7664ZX0009, 7665XX0009","Przewód H05RN-F 6G1 o długości 6m do podłączenia w odpowiednio dobranej puszce elektroinstalacyjnej.","5147XX0010.jpg","5147XX0010.ldt",3,null,1,45]
["5150","5150XX0010","ASKER SMALL PRO WALL 2XLED 1188LM UP-DOWN 4000K DIM.","Asker","Wall","Aluminium",null,null,"PRO","LED zintegrowane","AC","DIM.","6,6W","8,3W","1188lm","901lm",null,null,"65","IK08","Class I",4000,"szerokie góra / szerokie dół",null,null,null,"CE",null,null,"> 70 000h",12,"Oprawa ścienna.","Światło dwustronne: ukierunkowane do góry i w dół.","Up-Down","A luminaire with a wide range of applications, including lighting wall surfaces, facades, and other architectural concepts",null,null,null,"Odlew aluminiowy malowany proszkowo.",null,"Klosz- poliwęglan przeźroczysty ze strukturą, stabilizowany UV.","Uszczelka silikonowa.","Dławnica EPDM.","góra/dół",null,"Oprawa ściemnialna fazowo TRAILING EDGE (TE)","2 Moduły LED","Philips Fortimo Strip 0,5ft MF FC LV6 4K","Philips Xitanium 8W 0,2A 40V TE SC 230V",0,null,null,80,"C",null,"Zaciski podłączeniowe: max 3x2,5mm², możliwość podłączenia oprawy w pętle max 3x1,5mm². Przewód w oponie okrągłej o średnicy ø7...10,5mm.","5150XX0010.jpg","5150XX0010.ldt",1,null,1,4]
["5151","5151XX0009","ASKER SMALL PRO WALL LED 681LM DOWN 4000K DIM.","Asker","Wall","Aluminium",null,null,"PRO","LED zintegrowane","AC","DIM.","4W","5,4W","681lm","444lm",null,null,"65","IK08","Class I",4000,"szerokie dół",0.22,0.11,0.08,"CE",null,null,"> 70 000h",12,"Oprawa ścienna.","Światło rozproszone półsferyczne ukierunkowane w dół",null,"Luminaire with a wide range of applications for example for illumination of walls and facade surfaces or any other architectural concepts",null,null,null,"Odlew aluminiowy malowany proszkowo.",null,"Klosz- poliwęglan przeźroczysty ze strukturą, stabilizowany UV.","Uszczelka silikonowa.","Dławnica EPDM.","dół",null,"Oprawa ściemnialna fazowo TRAILING EDGE (TE)","Moduł LED","Philips Strip OC 0.5ft 550lm 8xx FC HV5 4K","Philips Xitanium 7W 0,35A 20V TE SC 230V [2019]",50000,"Philips Xitanium TE",0,80,"C",null,"Zaciski podłączeniowe: max 3x2,5mm², możliwość podłączenia oprawy w pętle max 3x1,5mm². Przewód w oponie okrągłej o średnicy ø7...10,5mm.","5151XX0009.jpg","5151XX0009.ldt",1,null,1,76]
["5152","5152XX0009","SANDVIK WALL 2XLED 1604LM UP36D&DOWN36D 4000K DIM.","Sandvik","Wall","Aluminium",null,null,null,"LED zintegrowane","AC","DIM.","2 x 8W","16W","1604lm","1350lm",null,null,"65","IK08","Class I",4000,"szerokie góra / szerokie dół",0,0,0,"CE",null,null,"> 50 000h",12,"Oprawa ścienna.","Światło dwustronne: o kącie 36D do góry i w dół.","Up36D&Down36D","Classic design ceiling luminaire. For lighting private areas and public spaces.",null,null,null,"Odlew aluminiowy malowany proszkowo.",null,"Klosz- szkło bezpieczne, przeźroczyste.","Uszczelka silikonowa.","Dławnica EPDM.",null,null,"Oprawa ściemnialna fazowo TRAILING EDGE (TE) - LEADING EDGE (LE)","2 Moduły LED","Lumens EDC 38C 8W xxx 230V A101 4K",null,0,"Ściemnianie fazowe Lumens LED AC",null,80,"E",null,"Zaciski podłączeniowe: max 3x2,5mm², możliwość podłączenia oprawy w pętle max 3x1,5mm². Przewód w oponie okrągłej o średnicy ø7...10,5mm.","5152XX0009.jpg","5152XX0009.ldt",1,null,1,70]
["5153","5153XX0009","SANDVIK DOWN WALL LED 802LM DOWN 36D 4000K DIM.","Sandvik","Wall","Aluminium",null,null,null,"LED zintegrowane","AC","DIM.","8W","8W","802lm","675lm",null,null,"65","IK08","Class I",4000,"szerokie dół",0,0,0,"CE",null,null,"> 50 000h",12,"Oprawa ścienna.","Światło jednostronne: ukierunkowane w dół o kącie 36D.","Down 36D","Classic design wall luminaire. For lighting private areas and public spaces",null,null,null,"Odlew aluminiowy malowany proszkowo.",null,"Klosz- szkło bezpieczne, przeźroczyste.","Uszczelka silikonowa.","Dławnica EPDM.",null,null,"Oprawa ściemnialna fazowo TRAILING EDGE (TE) - LEADING EDGE (LE)","Moduł LED","Lumens EDC 38C 8W xxx 230V A101 4K",null,0,"Ściemnianie fazowe Lumens LED AC",0,80,"E",null,"Zaciski podłączeniowe: max 3x2,5mm², możliwość podłączenia oprawy w pętle max 3x1,5mm². Przewód w oponie okrągłej o średnicy ø7...10,5mm.","5153XX0009.jpg","5153XX0009.ldt",1,null,1,71]
["5157","5157XX0009","ASKER SMALL PRO WALL LED 688LM DOWN 4000K DALI2","Asker","Wall","Aluminium",null,null,"PRO","LED zintegrowane","AC","DALI2","3,9W","5,5W","688lm","465lm",null,null,"65",null,"Class I",4000,"szerokie dół",0,0,0,"CE",null,"DALI","> 70000",12,"Oprawa ścienna.","Światło rozproszone półsferyczne ukierunkowane w dół",null,"A luminaire with a wide range of applications, including lighting wall surfaces, facades, and other architectural concepts",null,null,null,"Odlew aluminiowy malowany proszkowo.",null,"Klosz- poliwęglan przeźroczysty ze strukturą, stabilizowany UV.","Uszczelka silikonowa.","Dławnica EPDM.","dół",null,null,"Moduł LED","Philips Strip OC 0.5ft 550lm 8xx FC HV5 3K","Osram OTI DALI 10/220-240/700 NFC",0,null,0,80,"D",null,"Zaciski podłączeniowe: max 3x2,5mm², możliwość podłączenia oprawy w pętle max 3x1,5mm². Przewód w oponie okrągłej o średnicy ø7...10,5mm.","5157XX0009.jpg","5157XX0009.ldt",3,null,1,76]
["515","515XX0009","HALDEN WALL LED E27 806LM DOWN 2700K DIM.","Halden","Wall","Aluminium",null,null,null,"Wymienne","E27",null,"5,9W","5,9W","806lm","175lm",null,null,"65","IK10","Class I",2700,null,0.31,null,0.15,"CE",null,null,"25000",12,"Oprawa ścienna.","Światło rozproszone półsferyczne ukierunkowane w dół",null,"Luminaire with a wide range of applications for example for illumination of walls and facade surfaces or any other architectural concepts.",null,null,"Oprawa wyposażona w wymienne źródło światła typu lampa LED o trzonku E27, która zapewnia trwałość i optymalny rozsył światła, przy zachowaniu stosunkowo małego zużycia energii.","Odlew aluminiowy malowany proszkowo.",null,"Klosz- poliwęglan przeźroczysty ze strukturą, stabilizowany UV.","Uszczelka silikonowa.","Dławnica EPDM.",null,null,"Oprawa ściemnialna fazowo TRAILING EDGE (TE) - LEADING EDGE (LE)","Lampa LED E27","Philips MAS LEDBulb DT5.9-60W E27 927 A60 FR G",null,0,"Ściemnianie fazowe LED GU10 E27",0,80,"F",null,"Zaciski podłączeniowe: max 3x2,5mm², możliwość podłączenia oprawy w pętle max 3x1,5mm². Przewód w oponie okrągłej o średnicy ø7...10,5mm.","515XX0009.jpg","515XX0009.ldt",1,"E27",1,76]
["5160","5160XX0009","ASKER SMALL PRO WALL LED 1376LM UP-DOWN 4000K DALI2","Asker","Wall","Aluminium",null,null,"PRO","LED zintegrowane","AC","DALI2","7,8W","9,9W","1376lm","901lm",null,null,"65",null,"Class I",4000,"szerokie góra / szerokie dół",0,0,0,"CE",null,"DALI","> 70 000h",12,"Oprawa ścienna.","Światło dwustronne: ukierunkowane do góry i w dół.","Up-Down","A luminaire with a wide range of applications, including lighting wall surfaces, facades, and other architectural concepts",null,null,null,"Odlew aluminiowy malowany proszkowo.",null,"Klosz- poliwęglan przeźroczysty ze strukturą, stabilizowany UV.","Uszczelka silikonowa.","Dławnica EPDM.","dół",null,null,"Moduł LED","Philips Strip OC 0.5ft 550lm 8xx FC HV5 3K","Osram OTI DALI 10/220-240/700 NFC",0,null,null,80,"D",null,"Zaciski podłączeniowe: max 5x2,5mm², możliwość podłączenia oprawy w pętle max 5x1,5mm². Przewód w oponie okrągłej o średnicy ø7...10,5mm.","5160XX0009.jpg","5160XX0009.ldt",3,null,1,4]
["5164","5164XX0009","ASKER POLE PRO LIGHT LUMINAIRES POLE 236CM LED 1169LM VSM 4000K ON/OFF","Asker","Post,Post complete","Aluminium",null,null,"PRO","LED zintegrowane","AC","ON/OFF","6,1W","8,5W","1169lm","1097lm",null,null,"65","IK08","Class I",4000,"szerokie dół",0.24,2.36,0.39,"CE",null,null,"> 100 000h",20,"Oprawa słupowa (lekka konstrukcja).","Soczewka firmy Ledil typu VSM (IESNA typ V).","VSM","Luminaire for lighting private areas, public spaces, and other architectural concepts",null,null,null,"Profil aluminiowy wyciskany, malowany proszkowo.",null,"Soczewka hermetyczna zewnętrzna- tworzywo sztuczne PMMA przeźroczyste.","Uszczelka silikonowa.",null,"236cm","jedno-segmentowy","Oprawa nieściemnialna","Moduł LED","Philips Fortimo FastFlex LED 2x6 DP G5 4K","Philips Xi BP 12 W 0,1-0,5AS 230 V C100",100000,null,0.01,70,"D","116ZX0009, 117GA0009, 118GA0009, 119ZX0009, 7666ZX0009","Zaciski podłączeniowe: max 3x4mm², możliwość podłączenia oprawy w pętle max 3x4mm². Przewód w oponie okrągłej o średnicy: ø4…8mm, ø8...12mm lub ø10...13,6mm","5164XX0009.jpg","5164XX0009.ldt",4,null,1,47]
["5165","5165XX0009","ASKER POLE PRO LIGHT LUMINAIRES POLE 236CM LED 1221LM VSM 4000K DALI2","Asker","Post,Post complete","Aluminium",null,null,"PRO","LED zintegrowane","AC","DALI2","6,4W","8,5W","1221lm","1140lm",null,null,"65","IK08","Class I",4000,"szerokie dół",0.39,0.11,2.36,"CE",null,"DALI","> 100 000h",20,"Oprawa słupowa (lekka konstrukcja).","Soczewka firmy Ledil typu VSM (IESNA typ V).","VSM","Luminaire for lighting private areas, public spaces, and other architectural concepts","For lighting private areas, parks, and other architectural concepts The wide and even luminous flux.",null,null,"Profil aluminiowy wyciskany, malowany proszkowo.",null,"Soczewka hermetyczna zewnętrzna- tworzywo sztuczne PMMA przeźroczyste.","Uszczelka silikonowa.",null,"236cm","jedno-segmentowy","Sterowanie światłem w systemie: DALI outdoor pełny program. Zasilacz zaprogramowany na max prąd. Programowanie pozostałych parametrów po uzgodnieniu z Działem Handlowym firmy Norlys.","Moduł LED","Philips Fortimo FastFlex LED 2x6 DP G5 4K","Philips Xi FP 22W 0,2-0,7A SNLDAE 230V S175 sXt",100000,"DALI2 / NightDim (XI FP NLD)",0.01,70,"D","116ZX0009, 117GA0009, 118GA0009, 119ZX0009, 7666ZX0009","Zaciski podłączeniowe: max 5x4mm², możliwość podłączenia oprawy w pętle max 5x2,5mm². Przewód w oponie okrągłej o średnicy: ø4…8mm, ø8...12mm lub ø10...13,6mm","5165XX0009.jpg","5165XX0009.ldt",3,null,1,47]
["5167","5167XX0009","ASKER POLE PRO LIGHT LUMINAIRES POLE 236CM LED 1169LM T2-L 4000K ON/OFF","Asker","Post,Post complete","Aluminium",null,null,"PRO","LED zintegrowane","AC","ON/OFF","6,1W","8,5W","1169lm","1076lm",null,null,"65","IK08","Class I",4000,"szerokie dół",2.36,0.11,0.39,"CE",null,null,"> 100 000h",20,"Oprawa słupowa (lekka konstrukcja).","Soczewka firmy Ledil typu T2-L (IESNA typ III).","T2-L","Luminaire for lighting private areas, public spaces, and other architectural concepts",null,null,null,"Profil aluminiowy wyciskany, malowany proszkowo.",null,"Soczewka hermetyczna zewnętrzna- tworzywo sztuczne PMMA przeźroczyste.","Uszczelka silikonowa.",null,"236cm","jedno-segmentowy","Oprawa nieściemnialna","Moduł LED","Philips Fortimo FastFlex LED 2x6 DP G5 4K","Philips Xi BP 12 W 0,1-0,5AS 230 V C100",100000,null,0.01,70,"D","116ZX0009, 117GA0009, 118GA0009, 119ZX0009, 7666ZX0009","Zaciski podłączeniowe: max 3x4mm², możliwość podłączenia oprawy w pętle max 3x4mm². Przewód w oponie okrągłej o średnicy: ø4…8mm, ø8...12mm lub ø10...13,6mm.","5167XX0009.jpg","5167XX0009.ldt",4,null,1,48]
["5169","5169XX0009","ASKER POLE PRO LIGHT LUMINAIRES POLE 236CM LED 1221LM T2-L 4000K DALI2","Asker","Post,Post complete","Aluminium",null,null,"PRO","LED zintegrowane","AC","DALI2","6,4W","8,7W","1221lm","1118lm",null,null,"65","IK08","Class I",4000,"szerokie dół",null,null,null,"CE",null,"DALI","> 120 000h",20,"Oprawa słupowa (lekka konstrukcja).","Soczewka firmy Ledil typu T2-L (IESNA typ III).","T2-L","Luminaire for lighting private areas, public spaces, and other architectural concepts",null,null,null,"Profil aluminiowy wyciskany, malowany proszkowo.",null,"Soczewka hermetyczna zewnętrzna- tworzywo sztuczne PMMA przeźroczyste.","Uszczelka silikonowa.",null,"236cm","jedno-segmentowy","Sterowanie światłem w systemie: DALI outdoor pełny program. Zasilacz zaprogramowany na max prąd. Programowanie pozostałych parametrów po uzgodnieniu z Działem Handlowym firmy Norlys.","Moduł LED","Philips Fortimo FastFlex LED 2x6 DP G4+ 3K","Philips Xi FP 22W 0,2-0,7A SNLDAE 230V S175 sXt",100000,"DALI2 / NightDim (XI FP NLD)",0.01,70,"D","116ZX0009, 117GA0009, 118GA0009, 119ZX0009, 7666ZX0009","Zaciski podłączeniowe: max 5x4mm², możliwość podłączenia oprawy w pętle max 5x4mm². Przewód w oponie okrągłej o średnicy max ø12,5mm.","5169XX0009.jpg","5169XX0009.ldt",3,null,1,48]
["5170","5170XX0009","KISA HEAD POLE-TOP 90CM 3XLED 1175LM 180D 3000K DIM.","Kisa","Other,Head","Aluminium",null,null,null,"LED zintegrowane","AC","DIM.","6,5W","8,8W","1175lm","706lm",null,null,"65","IK08","Class I",3000,null,0.14000000000000001,0.14000000000000001,0.9,"CE",null,null,null,2,"Oprawa słupowa (nasadzana).","Światło jednostronne rozproszone.","180D","Luminaire with a contemporary design. For lighting gardens and other private and public areas",null,null,null,"Profil aluminiowy wyciskany, malowany proszkowo.",null,"Klosz- tworzywo sztuczne PMMA satynowane.",null,null,"90cm","jednostronna","Oprawa ściemnialna fazowo TRAILING EDGE (TE) - LEADING EDGE (LE)","3 Moduły LED","Philips Strip OC 0.5ft 550lm 8xx FC LV5 3K","Philips Xitanium 8W 0,2A 40V TE SC 230V",0,"Philips Xitanium TE",null,80,"D","5188XX0009","Puszka hermetyczna IP68, zaciski podłączeniowe: max 3x4mm², możliwość podłączenia oprawy w pętle max 3x4mm². Przewód w oponie okrągłej o średnicy ø4...14mm.","5170XX0009.jpg","5170XX0009.ldt",1,null,1,50]
["517","517XX0013","HALDEN WALL LED 1059LM DOWN 3000K DIM.","Halden","Wall","Aluminium",null,null,null,"LED zintegrowane","AC","DIM.","6,7W","8,5W","1059lm","682lm",null,null,"65","IK10","Class I",3000,"szerokie dół",0.31,0.16,0.15,"CE",null,null,"> 110 000h",12,"Oprawa ścienna.","Światło rozproszone półsferyczne ukierunkowane w dół",null,"Luminaire with a wide range of applications for example for illumination of walls and facade surfaces or any other architectural concepts",null,null,null,"Odlew aluminiowy malowany proszkowo.",null,"Klosz- poliwęglan przeźroczysty ze strukturą, stabilizowany UV.","Uszczelka silikonowa.","Dławnica EPDM.",null,null,"Oprawa ściemnialna fazowo TRAILING EDGE (TE)","Moduł LED","Philips Fortimo SLM C 1203 L09 1619 G7 3K","Philips Xitanium 8W 0,2A 40V TE SC 230V",0,"Philips Xitanium TE",0,80,"D",null,"Zaciski podłączeniowe: max 3x2,5mm², możliwość podłączenia oprawy w pętle max 3x1,5mm². Przewód w oponie okrągłej o średnicy ø7...10,5mm.","517XX0013.jpg","517XX0013.ldt",1,null,1,76]
["5180","5180XX0010","KISA BOLLARD 85CM 3XLED 1175LM 180D 3000K DIM.","Kisa","Bollard","Aluminium",null,null,null,"LED zintegrowane","AC","DIM.","6,5W","8,8W","1175lm","706lm",null,null,"55","IK08","Class I",3000,null,0.12,0.12,0.85,"CE",null,null,"> 70 000h",1,"Oprawa słupkowa.","Światło jednostronne rozproszone.","180D","Luminaire with contemporary design For lighting gardens and other private and public areas",null,null,null,"Odlew aluminiowy malowany proszkowo.",null,"Klosz- tworzywo sztuczne PMMA satynowane.",null,null,"85cm","jednostronna","Oprawa ściemnialna fazowo TRAILING EDGE (TE) - LEADING EDGE (LE)","3 Moduły LED","Philips Fortimo Strip 0,5ft MF FC LV6 3K","Philips Xitanium 8W 0,2A 40V TE SC 230V",0,"Philips Xitanium TE",null,80,"C","205ZX0010, 206GA0010","Zaciski podłączeniowe: max 3x4mm², możliwość podłączenia oprawy w pętle max 3x2,5mm². Przewód w oponie okrągłej o średnicy ø8...12,5mm.","5180XX0010.png","5180XX0010.ldt",1,null,1,50]
["5181","5181XX0010","KISA BOLLARD 85CM 3XLED 1246LM 180D 4000K DIM. TRIAC","Kisa","Bollard","Aluminium",null,null,null,"LED zintegrowane","AC","DIM. TRIAC","6,5W","8,8W","1246lm","766lm",null,null,"55","IK08","Class I",4000,null,0.12,0.12,0.85,"CE",null,null,"> 70 000h",1,"Oprawa słupkowa.","Światło jednostronne rozproszone.","180D","Luminaire with contemporary design For lighting gardens and other private and public areas",null,null,null,"Odlew aluminiowy malowany proszkowo.",null,"Klosz- tworzywo sztuczne PMMA satynowane.",null,null,"85cm","jednostronna","Oprawa ściemnialna fazowo TRAILING EDGE (TE) - LEADING EDGE (LE)","3 Moduły LED","Philips Fortimo Strip 0,5ft MF FC LV6 4K","Philips Xitanium 8W 0,2A 40V TE SC 230V",0,"Philips Xitanium TE",null,80,"C","205ZX0010, 206GA0010","Zaciski podłączeniowe: max 3x4mm², możliwość podłączenia oprawy w pętle max 3x2,5mm². Przewód w oponie okrągłej o średnicy ø8...12,5mm.","5181XX0010.png","5181XX0010.ldt",1,null,1,50]
["5182","5182XX0009","KISA BOLLARD 85CM 3XLED 2002LM 180D 3000K DALI2","Kisa","Bollard","Aluminium",null,null,null,"LED zintegrowane","AC","DALI2","11,8W","14,1W","2002lm","1185lm",null,null,"55","IK08","Class I",3000,null,0.85,0.12,0.12,"CE",null,"DALI","> 70 000h",1,"Oprawa słupkowa.","Światło jednostronne rozproszone.","180D","Luminaire with contemporary design, For lighting gardens and other private and public areas",null,null,null,"Odlew aluminiowy malowany proszkowo.",null,"Klosz- tworzywo sztuczne PMMA satynowane.",null,null,"85cm","jednostronna","Sterowanie światłem w systemie: DALI outdoor pełny program. Zasilacz zaprogramowany na max prąd. Programowanie pozostałych parametrów po uzgodnieniu z Działem Handlowym firmy Norlys.","3 Moduły LED","Philips Fortimo Strip 0,5ft MF FC LV6 3K","Philips Xi FP 22W 0,2-0,7A SNLDAE 230V S175 sXt",100000,"DALI2 / NightDim (XI FP NLD)",null,80,"C","205ZX0010, 206GA0010","Zaciski podłączeniowe: max 5x4mm², możliwość podłączenia oprawy w pętle max 5x2,5mm². Przewód w oponie okrągłej o średnicy ø8...12,5mm.","5182XX0009.png","5182XX0009.ldt",3,null,1,50]
["5183","5183XX0009","KISA BOLLARD 85CM 3XLED 2122LM 180D 4000K DALI2","Kisa","Bollard","Aluminium",null,null,null,"LED zintegrowane","AC","DALI2","11,8W","14,1W","2122lm","1222lm",null,null,"55","IK08","Class I",4000,null,0.85,0.12,0.12,"CE",null,"DALI","> 70 000h",1,"Oprawa słupkowa.","Światło jednostronne rozproszone.","180D","Luminaire with contemporary design, For lighting gardens and other private and public areas",null,null,null,"Odlew aluminiowy malowany proszkowo.",null,"Klosz- tworzywo sztuczne PMMA satynowane.",null,null,"85cm","jednostronna","Sterowanie światłem w systemie: DALI outdoor pełny program. Zasilacz zaprogramowany na max prąd. Programowanie pozostałych parametrów po uzgodnieniu z Działem Handlowym firmy Norlys.","3 Moduły LED","Philips Fortimo Strip 0,5ft MF FC LV6 4K","Philips Xi FP 22W 0,2-0,7A SNLDAE 230V S175 sXt",100000,"DALI2 / NightDim (XI FP NLD)",null,80,"C","205ZX0010, 206GA0010","Zaciski podłączeniowe: max 5x4mm², możliwość podłączenia oprawy w pętle max 5x2,5mm². Przewód w oponie okrągłej o średnicy ø8...12,5mm.","5183XX0009.png","5183XX0009.ldt",3,null,1,50]
["5184","5184XX0010","KISA BOLLARD 85CM 6XLED 2009LM 3000K DIM.","Kisa","Bollard","Aluminium",null,null,null,"LED zintegrowane","AC","DIM.","11,3W","13,4W","2009lm","1274lm",null,null,"55","IK08","Class I",3000,null,0.12,0.12,0.85,"CE",null,null,"> 70 000",1,"Oprawa słupkowa.","Światło dwustronne rozproszone.",null,"Luminaire with contemporary design For lighting gardens and other private and public areas",null,null,null,"Odlew aluminiowy malowany proszkowo.",null,"Klosz- tworzywo sztuczne PMMA satynowane.",null,null,"85cm","dwustronna","Oprawa ściemnialna fazowo TRAILING EDGE (TE) - LEADING EDGE (LE)","6 Modułów LED","Philips Fortimo Strip 0,5ft MF FC LV6 3K","Philips Xitanium 14W 0,35A 40V TE SC 230V",0,"Philips Xitanium TE",null,80,"C","205ZX0010, 206GA0010","Zaciski podłączeniowe: max 3x4mm², możliwość podłączenia oprawy w pętle max 3x2,5mm². Przewód w oponie okrągłej o średnicy ø8...12,5mm.","5184XX0010.png","5184XX0010.ldt",1,null,1,51]
["5185","5185XX0010","KISA BOLLARD 85CM 6XLED 2131LM 4000K DIM.","Kisa","Bollard","Aluminium",null,null,null,"LED zintegrowane","AC","DIM.","11,3W","13,4W","2131lm","1357lm",null,null,"55","IK08","Class I",4000,null,0.12,0.12,0.85,"CE",null,null,"> 70 000",1,"Oprawa słupkowa.","Światło dwustronne rozproszone.",null,"Luminaire with contemporary design For lighting gardens and other private and public areas",null,null,null,"Odlew aluminiowy malowany proszkowo.",null,"Klosz- tworzywo sztuczne PMMA satynowane.",null,null,"85cm","dwustronna","Oprawa ściemnialna fazowo TRAILING EDGE (TE) - LEADING EDGE (LE)","6 Modułów LED","Philips Fortimo Strip 0,5ft MF FC LV6 4K","Philips Xitanium 14W 0,35A 40V TE SC 230V",0,"Philips Xitanium TE",null,80,"C","205ZX0010, 206GA0010","Zaciski podłączeniowe: max 3x4mm², możliwość podłączenia oprawy w pętle max 3x2,5mm². Przewód w oponie okrągłej o średnicy ø8...12,5mm.","5185XX0010.png","5185XX0010.ldt",1,null,1,51]
["5187","5187XX0009","KISA BOLLARD 85CM 6XLED 4126LM 4000K DALI2","Kisa","Bollard","Aluminium",null,null,null,"LED zintegrowane","AC","DALI2","23,5W","27W","4126lm","2637lm",null,null,"55","IK08","Class I",4000,null,0.85,0.12,0.12,"CE",null,"DALI","> 70 000h",1,"Oprawa słupkowa.","Światło dwustronne rozproszone.",null,"Luminaire with contemporary design For lighting gardens and other private and public areas",null,null,null,"Odlew aluminiowy malowany proszkowo.",null,"Klosz- tworzywo sztuczne PMMA satynowane.",null,null,"85cm","dwustronna","Sterowanie światłem w systemie: DALI outdoor pełny program. Zasilacz zaprogramowany na max prąd. Programowanie pozostałych parametrów po uzgodnieniu z Działem Handlowym firmy Norlys.","6 Modułów LED","Philips Fortimo Strip 0,5ft MF FC LV6 4K","Philips Xi FP 40W 0.2-0.7A SNLDAE 230V S175 929000989206",100000,"DALI2 / NightDim (XI FP NLD)",null,80,"C","205ZX0010, 206GA0010","Zaciski podłączeniowe: max 5x4mm², możliwość podłączenia oprawy w pętle max 5x2,5mm². Przewód w oponie okrągłej o średnicy ø8...12,5mm.","5187XX0009.png","5187XX0009.ldt",3,null,1,51]
["5190","5190XX0309","KISA LIGHT LUMINAIRES POLE 3XLED 1175LM 180D 3000K DIM.","Kisa","Post,Post complete","Aluminium",null,null,null,"LED zintegrowane","AC","DIM.","6,5W","8,8W","1175lm","706lm",null,null,"65","IK08","Class I",3000,null,0.12,0.12,2.5,"CE",null,null,"> 70 000h",20,"Oprawa słupowa (lekka konstrukcja).","Światło jednostronne rozproszone.","180D","Pole luminaire, mounting ø120mm","Top-mounted pole luminaire ø120mm, equipped with: - Lighting pole art. 5188xx0009 equipped with an revision door - Luminaire art. 5170xx0009 equipped with LED module and hermetic electric box Other accessories must be ordered separately",null,null,"Profil aluminiowy wyciskany, malowany proszkowo.",null,"Klosz- tworzywo sztuczne PMMA satynowane.","Uszczelka silikonowa.",null,"jednostronna","Drzwiczki rewizyjne","Oprawa ściemnialna fazowo TRAILING EDGE (TE) - LEADING EDGE (LE)","3 Moduły LED","Philips Strip OC 0.5ft 550lm 8xx FC LV5 3K","Philips Xitanium 8W 0,2A 40V TE SC 230V",0,"Philips Xitanium TE",null,80,"C","6130ZX0009, 6132GA0009, 6133GA0009, ZS6135XX0009","Puszka hermetyczna IP68: Zaciski podłączeniowe: max 3x4mm², możliwość podłączenia oprawy w pętle max 3x4mm². Przewód w oponie okrągłej o średnicy: ø4...14mm. Oprawa oświetleniowa wyposażona w drzwiczki rewizyjne.","5190XX0309.jpg","5190XX0309.ldt",1,null,1,50]
["5191","5191XX0309","KISA LIGHT LUMINAIRES POLE 3XLED 1246LM 180D 4000K DIM.","Kisa","Post,Post complete","Aluminium",null,null,null,"LED zintegrowane","AC","DIM.","6,5W","8,8W","1246lm","766lm",null,null,"65","IK08","Class I",4000,null,0.12,0.12,2.5,"CE",null,null,"> 70 000h",20,"Oprawa słupowa (lekka konstrukcja).","Światło jednostronne rozproszone.","180D","Pole luminaire, mounted ø120mm","Luminaire with a contemporary design For lighting gardens and other private and public areas Top-mounted pole luminaire ø120mm, equipped with: - Pole art. 5188xx0009 equipped with an revision door - Head art. 5171xx0009 equipped with LED module and hermetic electric box Other accessories must be ordered separately",null,null,"Profil aluminiowy wyciskany, malowany proszkowo.",null,"Klosz- tworzywo sztuczne PMMA satynowane.","Uszczelka silikonowa.",null,"jednostronna","Drzwiczki rewizyjne","Oprawa ściemnialna fazowo TRAILING EDGE (TE) - LEADING EDGE (LE)","3 Moduły LED","Philips Strip OC 0.5ft 550lm 8xx FC LV5 4K","Philips Xitanium 8W 0,2A 40V TE SC 230V",0,"Philips Xitanium TE",null,80,"C","6130ZX0009, 6132GA0009, 6133GA0009, ZS6135XX0009","Puszka hermetyczna IP68: Zaciski podłączeniowe: max 3x4mm², możliwość podłączenia oprawy w pętle max 3x4mm². Przewód w oponie okrągłej o średnicy: ø8...14mm. Oprawa oświetleniowa wyposażona w drzwiczki rewizyjne.","5191XX0309.jpg","5191XX0309.ldt",1,null,1,50]
["5192","5192XX0309","KISA LIGHT LUMINAIRES POLE 3XLED 2002LM 180D 3000K DALI2","Kisa","Pole","Aluminium",null,null,null,"LED zintegrowane","AC","DALI2","11,8W","14,1W","2002lm","1185lm",null,null,"65","IK08","Class I",3000,null,0.12,0.12,2.5,"CE",null,"DALI","> 70 000h",20,"Oprawa słupowa (lekka konstrukcja).","Światło jednostronne rozproszone.","180D","Luminaire with a contemporary design For lighting gardens and other private and public areas Top-mounted pole luminaire ø120mm, equipped with: - Pole art. 5188xx0009 equipped with an revision door - Head art. 5172xx0009 equipped with LED module and hermetic electric box Other accessories must be ordered separately",null,null,null,"Odlew aluminiowy malowany proszkowo.",null,"Klosz- tworzywo sztuczne PMMA satynowane.",null,null,"jednostronna","Drzwiczki rewizyjne","Sterowanie światłem w systemie: DALI outdoor pełny program. Zasilacz zaprogramowany na max prąd. Programowanie pozostałych parametrów po uzgodnieniu z Działem Handlowym firmy Norlys.","3 Moduły LED","Philips Strip OC 0.5ft 550lm 8xx FC LV5 3K","Philips Xi FP 22W 0,2-0,7A SNLDAE 230V S175 sXt",100000,"DALI2 / NightDim (XI FP NLD)",null,80,"C","6130ZX0009, 6132GA0009, 6133GA0009, ZS6135XX0009","Puszka hermetyczna IP 68: Zaciski podłączeniowe: max 5x4mm², możliwość podłączenia oprawy w pętle max 5x2,5mm². Przewód w oponie okrągłej o średnicy ø8...14mm.","5192XX0309.jpg","5192XX0309.ldt",3,null,1,50]
["5193","5193XX0309","KISA LIGHT LUMINAIRES POLE 3XLED 2122LM 180D 4000K DALI2","Kisa,Pole","Pole","Aluminium",null,null,null,"LED zintegrowane","AC","DALI2","11,8W","14,1W","2122lm","1222lm",null,null,"65","IK08","Class I",4000,null,0.12,0.12,2.5,"CE",null,"DALI","> 70 000h",20,"Oprawa słupowa (lekka konstrukcja).","Światło jednostronne rozproszone.","180D","Luminaire with a contemporary design For lighting gardens and other private and public areas Top-mounted pole luminaire ø120mm, equipped with: - Pole art. 5188xx0009 equipped with an revision door - Head art. 5173xx0009 equipped with LED module and hermetic electric box Other accessories must be ordered separately",null,null,null,"Odlew aluminiowy malowany proszkowo.",null,"Klosz- tworzywo sztuczne PMMA satynowane.",null,null,"jednostronna","Drzwiczki rewizyjne","Sterowanie światłem w systemie: DALI outdoor pełny program. Zasilacz zaprogramowany na max prąd. Programowanie pozostałych parametrów po uzgodnieniu z Działem Handlowym firmy Norlys.","3 Moduły LED","Philips Strip OC 0.5ft 550lm 8xx FC LV5 3K","Philips Xi FP 22W 0,2-0,7A SNLDAE 230V S175 sXt",100000,"DALI2 / NightDim (XI FP NLD)",null,80,"C","6130ZX0009, 6132GA0009, 6133GA0009, ZS6135XX0009","Zaciski podłączeniowe: max 5x4mm², możliwość podłączenia oprawy w pętle max 5x2,5mm². Przewód w oponie okrągłej o średnicy ø8...14mm.","5193XX0309.jpg","5193XX0309.ldt",3,null,1,50]
["5194","5194XX0309","KISA LIGHT LUMINAIRES POLE 6XLED 2009LM 3000K DIM.","Kisa","Pole","Aluminium",null,null,null,"LED zintegrowane","AC","DIM.","11,3W","13,4W","2009lm","1274lm",null,null,"65","IK08","Class I",3000,null,0.12,0.12,1.2,"CE",null,null,"> 70 000",20,"Oprawa słupowa (lekka konstrukcja).","Światło dwustronne rozproszone.",null,"Luminaire with a contemporary design For lighting gardens and other private and public areas Top-mounted pole luminaire ø120mm, equipped with: - Pole art. 5188xx0009 equipped with an revision door - Head art. 5174xx0009 equipped with LED module and hermetic electric box Other accessories must be ordered separately",null,null,null,"Odlew aluminiowy malowany proszkowo.",null,"Klosz- tworzywo sztuczne PMMA satynowane.",null,null,"dwustronna","Drzwiczki rewizyjne","Oprawa ściemnialna fazowo TRAILING EDGE (TE) - LEADING EDGE (LE)","6 Modułów LED","Philips Strip OC 0.5ft 550lm 8xx FC LV5 3K","Philips Xitanium 14W 0,35A 40V TE SC 230V",0,"Philips Xitanium TE",null,80,"C","6130ZX0009, 6132GA0009, 6133GA0009, ZS6135XX0009","Zaciski podłączeniowe: max 3x4mm², możliwość podłączenia oprawy w pętle max 3x2,5mm². Przewód w oponie okrągłej o średnicy ø8...12,5mm.","5194XX0309.png","5194XX0309.ldt",1,null,1,51]
["5195","5195XX0309","KISA LIGHT LUMINAIRES POLE 6XLED 2131LM 4000K DIM.","Kisa","Pole","Aluminium",null,null,null,"LED zintegrowane","AC","DIM.","11,3W","13,4W","2131lm","1357lm",null,null,"65","IK08","Class I",4000,null,0.12,0.12,2.5,"CE",null,null,"> 70 000",20,"Oprawa słupowa (lekka konstrukcja).","Światło dwustronne rozproszone.",null,"Luminaire with a contemporary design For lighting gardens and other private and public areas Top-mounted pole luminaire ø120mm, equipped with: - Pole art. 5188xx0009 equipped with an revision door - Head art. 5175xx0009 equipped with LED module and hermetic electric box Other accessories must be ordered separately",null,null,null,"Odlew aluminiowy malowany proszkowo.",null,"Klosz- tworzywo sztuczne PMMA satynowane.",null,null,"dwustronna","Drzwiczki rewizyjne","Oprawa ściemnialna fazowo TRAILING EDGE (TE) - LEADING EDGE (LE)","6 Modułów LED","Philips Strip OC 0.5ft 550lm 8xx FC LV5 4K","Philips Xitanium 14W 0,35A 40V TE SC 230V",0,"Philips Xitanium TE",null,80,"C","6130ZX0009, 6132GA0009, 6133GA0009, ZS6135XX0009","Zaciski podłączeniowe: max 3x4mm², możliwość podłączenia oprawy w pętle max 3x2,5mm². Przewód w oponie okrągłej o średnicy ø8...14mm.","5195XX0309.png","5195XX0309.ldt",1,null,1,51]
["5196","5196XX0309","KISA LIGHT LUMINAIRES POLE 6XLED 3891LM 3000K DALI2","Kisa","Pole,Post complete","Aluminium",null,null,null,"LED zintegrowane","AC","DALI2","23,5W","27W","3891lm","2432lm",null,null,"65","IK08","Class I",3000,null,0.12,0.12,2.5,"CE",null,"DALI","> 70 000h",20,"Oprawa słupowa (lekka konstrukcja).","Światło dwustronne rozproszone.",null,"Pole luminaire, mounted ø120mm","Luminaire with a contemporary design For lighting gardens and other private and public areas Top-mounted pole luminaire ø120mm, equipped with: - Pole art. 5188xx0009 equipped with an revision door - Head art. 5176xx0009 equipped with LED module and hermetic electric box Other accessories must be ordered separately",null,null,"Odlew aluminiowy malowany proszkowo.",null,"Klosz- tworzywo sztuczne PMMA satynowane.","Uszczelka silikonowa.","Dławnica nylon6.","dwustronna","Drzwiczki rewizyjne",null,"6 Modułów LED","Philips Strip OC 0.5ft 550lm 8xx FC LV5 3K","Philips Xi FP 40W 0.2-0.7A SNLDAE 230V S175 929000989206",100000,"DALI2 / NightDim (XI FP NLD)",null,80,"C","6130ZX0009, 6132GA0009, 6133GA0009, ZS6135XX0009","Puszka hermetyczna IP68: Zaciski podłączeniowe: max 5x2,5mm², możliwość podłączenia oprawy w pętle max 5x1,5mm². Przewód w oponie okrągłej o średnicy: ø8...17mm. Oprawa oświetleniowa wyposażona w drzwiczki rewizyjne.","5196XX0309.png","5196XX0309.ldt",3,null,1,51]
["5197","5197XX0309","KISA LIGHT LUMINAIRES POLE 6XLED 4126LM 4000K DALI2","Kisa","Pole,Post complete","Aluminium",null,null,null,"LED zintegrowane","AC","DALI2","23,5W","27W","4126lm","2637lm",null,null,"65","IK08","Class I",4000,null,0.12,0.12,2.5,"CE",null,"DALI","> 70 000h",20,"Oprawa słupowa (lekka konstrukcja).","Światło dwustronne rozproszone.",null,"Luminaire with a contemporary design For lighting gardens and other private and public areas Top-mounted pole luminaire ø120mm, equipped with: - Pole art. 5188xx0009 equipped with an revision door - Head art. 5177xx0009 equipped with LED module and hermetic electric box Other accessories must be ordered separately",null,null,null,"Odlew aluminiowy malowany proszkowo.",null,"Klosz- tworzywo sztuczne PMMA satynowane.",null,null,"dwustronna","Drzwiczki rewizyjne","Sterowanie światłem w systemie: DALI outdoor pełny program. Zasilacz zaprogramowany na max prąd. Programowanie pozostałych parametrów po uzgodnieniu z Działem Handlowym firmy Norlys.","6 Modułów LED","Philips Strip OC 0.5ft 550lm 8xx FC LV5 4K","Philips Xi FP 40W 0.2-0.7A SNLDAE 230V S175 929000989206",100000,"DALI2 / NightDim (XI FP NLD)",null,80,"C","6130ZX0009, 6132GA0009, 6133GA0009, ZS6135XX0009","Zaciski podłączeniowe: max 5x4mm², możliwość podłączenia oprawy w pętle max 5x2,5mm². Przewód w oponie okrągłej o średnicy ø8...14mm.","5197XX0309.png","5197XX0309.ldt",3,null,1,51]
["5200","5200XX0010","ASKER POLE PRO 350CM LED 2628LM VSM 3000K DALI2","Asker","Post","Aluminium",null,null,"PRO","LED zintegrowane","AC","DALI2","16,6W","19,9W","2628lm","2620lm",null,null,"65","IK08","Class I",3000,"szerokie dół",null,null,null,"CE",null,"DALI","> 120 000h",23,"Oprawa słupowa.","Soczewka firmy Ledil typu VSM (IESNA typ V).","VSM","For lighting private areas, parks and other architectural concepts","For lighting private areas, parks and other architectural concepts Wide uniform luminous flux Lighting chamber tightness IP65",null,null,"Profil aluminiowy wyciskany, malowany proszkowo.",null,"Soczewka hermetyczna zewnętrzna- tworzywo sztuczne PMMA przeźroczyste.","Uszczelka silikonowa.",null,"350cm","dwu-segmentowy","Sterowanie światłem w systemie: DALI outdoor pełny program. Zasilacz zaprogramowany na max prąd. Programowanie pozostałych parametrów po uzgodnieniu z Działem Handlowym firmy Norlys.","Moduł LED","Philips Fortimo FastFlex LED 2x6 DP G4+ 3K","Philips Xi FP 22W 0,2-0,7A SNLDAE 230V S175 sXt",100000,"DALI2 / NightDim (XI FP NLD)",null,70,"D","7666ZX0009, B-50","Zaciski podłączeniowe: max 3x4mm², możliwość podłączenia oprawy w pętle max 3x2,5mm². Przewód w oponie okrągłej o średnicy: ø8...12mm lub ø10...14mm.","5200XX0010.jpg","5200XX0010.ldt",3,null,1,47]
["5201","5201XX0010","ASKER POLE PRO 350CM LED 2772LM VSM 4000K DALI2","Asker","Post","Aluminium",null,null,"PRO","LED zintegrowane","AC","DALI2","16,6W","19,9W","2772lm","2681lm",null,null,"65","IK08","Class I",4000,"szerokie dół",null,null,null,"CE",null,"DALI","> 120 000h",23,"Oprawa słupowa.","Soczewka firmy Ledil typu VSM (IESNA typ V).","VSM","For lighting private areas, parks and other architectural concepts","For lighting private areas, parks and other architectural concepts. Wide uniform luminous flux. Lighting chamber tightness IP65",null,null,"Profil aluminiowy wyciskany, malowany proszkowo.",null,"Soczewka hermetyczna zewnętrzna- tworzywo sztuczne PMMA przeźroczyste.","Uszczelka silikonowa.",null,"350cm","dwu-segmentowy","Sterowanie światłem w systemie: DALI outdoor pełny program. Zasilacz zaprogramowany na max prąd. Programowanie pozostałych parametrów po uzgodnieniu z Działem Handlowym firmy Norlys.","Moduł LED","Philips Fortimo FastFlex LED 2x6 DP G4+ 4K","Philips Xi FP 22W 0,2-0,7A SNLDAE 230V S175 sXt",100000,"DALI2 / NightDim (XI FP NLD)",null,70,"D","7666ZX0009, B-50","Zaciski podłączeniowe: max 3x4mm², możliwość podłączenia oprawy w pętle max 3x2,5mm². Przewód w oponie okrągłej o średnicy: ø8...12mm lub ø10...14mm.","5201XX0010.jpg","5201XX0010.ldt",3,null,1,47]
["5202","5202XX0011","ASKER POLE PRO 350CM LED 2667LM VSM 3000K DIM.","Asker,Pole","Post,Post complete","Aluminium",null,null,"PRO","LED zintegrowane","AC","DIM.","16,8W","19,5W","2667lm","2660lm",null,null,"65","IK08","Class I",3000,"szerokie dół",0.24,0.48,3.5,"CE",null,null,"> 100 000h",23,"Oprawa słupowa.","Soczewka firmy Ledil typu VSM (IESNA typ V).","VSM","For lighting private areas, parks and other architectural concepts","For lighting private areas, parks and other architectural concepts. Wide, even light flux.",null,null,"Profil aluminiowy wyciskany, malowany proszkowo.",null,"Soczewka hermetyczna zewnętrzna- tworzywo sztuczne PMMA przeźroczyste.","Uszczelka silikonowa.",null,"350cm","dwu-segmentowy","Oprawa ściemnialna fazowo TRAILING EDGE (TE) - LEADING EDGE (LE)","Moduł LED","Philips Fortimo FastFlex LED 2x6 DP G5 3K","TCI Mini MD 20W 500mA BI code 127033 Triak",0,null,null,70,"D","7666ZX0009, B-50","Zaciski podłączeniowe: max 3x4mm², możliwość podłączenia oprawy w pętle max 3x4mm². Przewód w oponie okrągłej o średnicy: ø8...12mm lub ø10...13,6mm","5202XX0011.jpg","5202XX0011.ldt",1,null,1,47]
["5203","5203XX0010","ASKER POLE PRO 350CM LED 2772LM VSM 4000K ON/OFF","Asker,Pole","Post,Post complete","Aluminium",null,null,"PRO","LED zintegrowane","AC","ON/OFF","16,6W","19,6W","2772lm","2681lm",null,null,"65","IK08","Class I",4000,"szerokie dół",null,null,null,"CE",null,null,"> 120 000h",23,"Oprawa słupowa.","Soczewka firmy Ledil typu VSM (IESNA typ V).","VSM","For lighting private areas, parks and other architectural concepts","For lighting private areas, parks and other architectural concepts Wide uniform luminous flux Lighting chamber tightness IP65",null,null,"Profil aluminiowy wyciskany, malowany proszkowo.",null,"Soczewka hermetyczna zewnętrzna- tworzywo sztuczne PMMA przeźroczyste.","Uszczelka silikonowa.",null,"350cm","dwu-segmentowy","Oprawa nieściemnialna","Moduł LED","Philips Fortimo FastFlex LED 2x6 DP G4+ 4K","Philips Xitanium 36W/m 929001486006",0,null,null,70,"D","7666ZX0009, B-50","Zaciski podłączeniowe: max 3x4mm², możliwość podłączenia oprawy w pętle max 3x2,5mm². Przewód w oponie okrągłej o średnicy: ø8...12mm lub ø10...14mm.","5203XX0010.jpg","5203XX0010.ldt",4,null,1,47]
["5204","5204XX0010","ASKER POLE PRO 350CM LED 2628LM T2-L 3000K DALI2","Asker","Post","Aluminium",null,null,"PRO","LED zintegrowane","AC","DALI2","16,6W","19,9W","2628lm","2620lm",null,null,"65","IK08","Class I",3000,"szerokie dół",3.5,0.39,0.11,"CE",null,"DALI","> 120 000h",23,"Oprawa słupowa.","Soczewka firmy Ledil typu T2-L (IESNA typ III).","T2-L","For lighting private areas, parks and other architectural concepts","For lighting private areas, parks and other architectural concepts Wide uniform luminous flux Lighting chamber tightness IP65",null,null,"Profil aluminiowy wyciskany, malowany proszkowo.",null,"Soczewka hermetyczna zewnętrzna- tworzywo sztuczne PMMA przeźroczyste.","Uszczelka silikonowa.",null,"350cm","dwu-segmentowy","Sterowanie światłem w systemie: DALI outdoor pełny program. Zasilacz zaprogramowany na max prąd. Programowanie pozostałych parametrów po uzgodnieniu z Działem Handlowym firmy Norlys.","Moduł LED","Philips Fortimo FastFlex LED 2x6 DP G4+ 3K","Philips Xi FP 22W 0,2-0,7A SNLDAE 230V S175 sXt",100000,"DALI2 / NightDim (XI FP NLD)",null,70,"D","7666ZX0009, B-50","Zaciski podłączeniowe: max 3x4mm², możliwość podłączenia oprawy w pętle max 3x2,5mm². Przewód w oponie okrągłej o średnicy: ø8...12mm lub ø10...14mm.","5204XX0010.jpg","5204XX0010.ldt",3,null,1,48]
["5205","5205XX0010","ASKER POLE PRO 350CM LED 2772LM T2-L 4000K DALI2","Asker","Post","Aluminium",null,null,"PRO","LED zintegrowane","AC","DALI2","16,6W","19,9W","2772lm","2634lm",null,null,"65","IK08","Class I",4000,"szerokie dół",null,null,null,"CE",null,"DALI","> 120 000h",23,"Oprawa słupowa.","Soczewka firmy Ledil typu T2-L (IESNA typ III).","T2-L","For lighting private areas, parks and other architectural concepts","For lighting private areas, parks and other architectural concepts Wide uniform luminous flux Lighting chamber tightness IP65",null,null,"Profil aluminiowy wyciskany, malowany proszkowo.",null,"Soczewka hermetyczna zewnętrzna- tworzywo sztuczne PMMA przeźroczyste.","Uszczelka silikonowa.",null,"350cm","dwu-segmentowy","Sterowanie światłem w systemie: DALI outdoor pełny program. Zasilacz zaprogramowany na max prąd. Programowanie pozostałych parametrów po uzgodnieniu z Działem Handlowym firmy Norlys.","Moduł LED","Philips Fortimo FastFlex LED 2x6 DP G4+ 4K","Philips Xi FP 22W 0,2-0,7A SNLDAE 230V S175 sXt",100000,"DALI2 / NightDim (XI FP NLD)",null,70,"D","7666ZX0009, B-50","Zaciski podłączeniowe: max 3x4mm², możliwość podłączenia oprawy w pętle max 3x2,5mm². Przewód w oponie okrągłej o średnicy: ø8...12mm lub ø10...14mm.","5205XX0010.jpg","5205XX0010.ldt",3,null,1,48]
["5206","5206XX0011","ASKER POLE PRO 350CM LED 2687LM T2-L 3000K DIM.","Asker,Pole","Post,Post complete","Aluminium",null,null,"PRO","LED zintegrowane","AC","DIM.","16,8W","19,6W","2687lm","2666lm",null,null,"65","IK08","Class I",3000,"szerokie dół",3.5,0.39,0.24,"CE",null,null,"> 100 000h",23,"Oprawa słupowa.","Soczewka firmy Ledil typu T2-L (IESNA typ III).","T2-L","For lighting private areas, parks and other architectural concepts","For lighting private areas, parks and other architectural concepts Wide uniform luminous flux Lighting chamber tightness IP65",null,null,"Profil aluminiowy wyciskany, malowany proszkowo.",null,"Soczewka hermetyczna zewnętrzna- tworzywo sztuczne PMMA przeźroczyste.","Uszczelka silikonowa.",null,"350cm","dwu-segmentowy","Oprawa ściemnialna fazowo TRAILING EDGE (TE) - LEADING EDGE (LE)","Moduł LED","Philips Fortimo FastFlex LED 2x6 DP G5 3K","TCI Mini MD 20W 500mA BI code 127033 Triak",0,null,null,70,"D","7666ZX0009, B-50","Zaciski podłączeniowe: max 3x4mm², możliwość podłączenia oprawy w pętle max 3x4mm². Przewód w oponie okrągłej o średnicy: ø8...12mm lub ø10...13,6mm.","5206XX0011.jpg","5206XX0011.ldt",1,null,1,48]
["5207","5207XX0011","ASKER POLE PRO 350CM LED 2910LM T2-L 4000K DIM.","Asker,Pole","Post,Post complete","Aluminium",null,null,"PRO","LED zintegrowane","AC","DIM.","16,8W","19,4W","2910lm","2774lm",null,null,"65","IK08","Class I",4000,"szerokie dół",3.5,0.39,0.24,"CE",null,null,"> 100 000h",23,"Oprawa słupowa.","Soczewka firmy Ledil typu T2-L (IESNA typ III).","T2-L","For lighting private areas, parks and other architectural concepts","For lighting private areas, parks and other architectural concepts. Wide uniform luminous flux. Lighting chamber tightness IP65",null,null,"Profil aluminiowy wyciskany, malowany proszkowo.",null,"Soczewka hermetyczna zewnętrzna- tworzywo sztuczne PMMA przeźroczyste.","Uszczelka silikonowa.",null,"350cm","dwu-segmentowy","Oprawa ściemnialna fazowo TRAILING EDGE (TE) - LEADING EDGE (LE)","Moduł LED","Philips Fortimo FastFlex LED 2x6 DP G5 4K","TCI Mini MD 20W 500mA BI code 127033 Triak",0,null,null,70,"D","7666ZX0009, B-50","Zaciski podłączeniowe: max 3x4mm², możliwość podłączenia oprawy w pętle max 3x4mm². Przewód w oponie okrągłej o średnicy: ø8...12mm lub ø10...13,6mm.","5207XX0011.jpg","5207XX0011.ldt",1,null,1,48]
["5210","5210XX0009","ASKER BOLLARD 85CM LED 929LM 3000K DIM.","Asker","Bollard","Aluminium",null,null,null,"LED zintegrowane","AC","DIM.","10W","10W","929lm","394lm",null,null,"65","IK10","Class I",3000,"szerokie dół",0.85,0.2,0.11,"CE",null,null,"> 55 000",1,"Oprawa słupkowa.","Światło rozproszone półsferyczne ukierunkowane w dół",null,"Luminaire with a contemporary design. For lighting private areas and other architectural concepts",null,null,null,"Odlew aluminiowy malowany proszkowo.",null,"Klosz- poliwęglan przeźroczysty ze strukturą, stabilizowany UV.","Uszczelka silikonowa.",null,"85cm",null,"Oprawa ściemnialna fazowo TRAILING EDGE (TE) - LEADING EDGE (LE)","Moduł LED","Lumens EDC 57C 10W xxx 230V F201 3K",null,0,"Ściemnianie fazowe Lumens LED AC",0,80,"F","1907ZX0009, 1908GA0009, 3081XX0009","Zaciski podłączeniowe: max 3x2,5mm², możliwość podłączenia oprawy w pętle max 3x1,5mm². Przewód w oponie okrągłej o średnicy max ø12,5mm.","5210XX0009.jpg","5210XX0009.ldt",1,null,1,76]
["5211","5211XX0009","ASKER BOLLARD 85CM LED 966LM 4000K DIM.","Asker","Bollard","Aluminium",null,null,null,"LED zintegrowane","AC","DIM.","10W","10W","966lm","457lm",null,null,"65","IK10","Class I",4000,"szerokie dół",0.85,0.2,0.11,"CE",null,null,"> 55 000",1,"Oprawa słupkowa.","Światło rozproszone półsferyczne ukierunkowane w dół",null,"Luminaire with a contemporary design. For lighting private areas and other architectural concepts",null,null,null,"Odlew aluminiowy malowany proszkowo.",null,"Klosz- poliwęglan przeźroczysty ze strukturą, stabilizowany UV.","Uszczelka silikonowa.",null,"85cm",null,"Oprawa ściemnialna fazowo TRAILING EDGE (TE) - LEADING EDGE (LE)","Moduł LED","Lumens EDC 57C 10W xxx 230V F201 4K",null,0,"Ściemnianie fazowe Lumens LED AC",0,80,"E","1907ZX0009, 1908GA0009, 3081XX0009","Zaciski podłączeniowe: max 3x2,5mm², możliwość podłączenia oprawy w pętle max 3x1,5mm². Przewód w oponie okrągłej o średnicy max ø12,5mm.","5211XX0009.jpg","5211XX0009.ldt",1,null,1,76]
["5212","5212XX0009","ASKER BOLLARD 55CM LED 929LM 3000K DIM.","Asker","Bollard","Aluminium",null,null,null,"LED zintegrowane","AC","DIM.","10W","10W","929lm","394lm",null,null,"65","IK10","Class I",3000,"szerokie dół",0.55000000000000004,0.2,0.11,"CE",null,null,"> 55 000h",1,"Oprawa słupkowa.","Światło rozproszone półsferyczne ukierunkowane w dół",null,"Luminaire with a contemporary design. For lighting private areas and other architectural concepts",null,null,null,"Odlew aluminiowy malowany proszkowo.",null,"Klosz- poliwęglan przeźroczysty ze strukturą, stabilizowany UV.","Uszczelka silikonowa.","Dławnica EPDM.","55cm",null,"Oprawa ściemnialna fazowo TRAILING EDGE (TE) - LEADING EDGE (LE)","Moduł LED","Lumens EDC 57C 10W xxx 230V F201 3K",null,0,"Ściemnianie fazowe Lumens LED AC",0,80,"F","1907ZX0009, 1908GA0009, 3081XX0009","Zaciski podłączeniowe: max 3x2,5mm², możliwość podłączenia oprawy w pętle max 3x1,5mm². Przewód w oponie okrągłej o średnicy max ø12,5mm.","5212XX0009.jpg","5212XX0009.ldt",1,null,1,76]
["5213","5213XX0009","ASKER BOLLARD 55CM LED 966LM 4000K DIM.","Asker","Bollard","Aluminium",null,null,null,"LED zintegrowane","AC","DIM.","10W","10W","966lm","458lm",null,null,"65","IK10","Class I",4000,"szerokie dół",0.55000000000000004,0.2,0.11,"CE",null,null,"> 55 000h",1,"Oprawa słupkowa.","Światło rozproszone półsferyczne ukierunkowane w dół",null,"Luminaire with a contemporary design. For lighting private areas and other architectural concepts",null,null,null,"Odlew aluminiowy malowany proszkowo.",null,"Klosz- poliwęglan przeźroczysty ze strukturą, stabilizowany UV.","Uszczelka silikonowa.","Dławnica EPDM.","55cm",null,"Oprawa ściemnialna fazowo TRAILING EDGE (TE) - LEADING EDGE (LE)","Moduł LED","Lumens EDC 57C 10W xxx 230V F201 4K",null,0,"Ściemnianie fazowe Lumens LED AC",0,80,"E","1907ZX0009, 1908GA0009, 3081XX0009","Zaciski podłączeniowe: max 3x2,5mm², możliwość podłączenia oprawy w pętle max 3x1,5mm². Przewód w oponie okrągłej o średnicy max ø12,5mm.","5213XX0009.jpg","5213XX0009.ldt",1,null,1,76]
["5214","5214XX0009","ASKER PRO BOLLARD 55CM LED 828LM SCL 3000K DIM.","Asker","Bollard","Aluminium",null,null,"PRO","LED zintegrowane","AC","DIM.","5,8W","7,7W","828lm","682lm",null,null,"65","IK08","Class I",3000,"szerokie dół",0.55000000000000004,0.2,0.11,"CE",null,null,"> 109 000h",1,"Oprawa słupkowa.","Soczewka firmy Ledil typu SCL (IESNA typ II / III).","SCL","Luminaire with a contemporary design For lighting gardens, private areas and other architectural concepts",null,null,null,"Odlew aluminiowy malowany proszkowo.",null,"Soczewka hermetyczna zewnętrzna- tworzywo sztuczne PMMA przeźroczyste.","Uszczelka silikonowa.","Dławnica EPDM.","55cm",null,"Oprawa ściemnialna fazowo TRAILING EDGE (TE)","Moduł LED","Cree DK200402 V1 XTE-HE 3K","Philips Xitanium 10W 0,5A 20V TE SC 230V",0,"Philips Xitanium TE",0.01,80,"E","1907ZX0009, 1908GA0009, 3081XX0009","Zaciski podłączeniowe: max 3x2,5mm², możliwość podłączenia oprawy w pętle max 3x1,5mm². Przewód w oponie okrągłej o średnicy max ø12,5mm.","5214XX0009.jpg","5214XX0009.ldt",1,null,1,46]
["5215","5215XX0009","ASKER PRO BOLLARD 55CM LED 828LM SCL 4000K DIM.","Asker","Bollard","Aluminium",null,null,"PRO","LED zintegrowane","AC","DIM.","5,8W","7,7W","828lm","654lm",null,null,"65","IK08","Class I",4000,"szerokie dół",0.55000000000000004,0.2,0.11,"CE",null,null,"> 109 000h",1,"Oprawa słupkowa.","Soczewka firmy Ledil typu SCL (IESNA typ II / III).","SCL","Luminaire with a contemporary design For lighting gardens, private areas and other architectural concepts",null,null,null,"Odlew aluminiowy malowany proszkowo.",null,"Soczewka hermetyczna zewnętrzna- tworzywo sztuczne PMMA przeźroczyste.","Uszczelka silikonowa.","Dławnica EPDM.","55cm",null,"Oprawa ściemnialna fazowo TRAILING EDGE (TE)","Moduł LED","Cree DK200402 V1 XTE-HE 3V 4K.","Philips Xitanium 10W 0,5A 20V TE SC 230V",0,"Philips Xitanium TE",0.01,80,"E","1907ZX0009, 1908GA0009, 3081XX0009","Zaciski podłączeniowe: max 3x2,5mm², możliwość podłączenia oprawy w pętle max 3x1,5mm². Przewód w oponie okrągłej o średnicy max ø12,5mm.","5215XX0009.jpg","5215XX0009.ldt",1,null,1,46]
["5216","5216XX0009","ASKER PRO BOLLARD 55CM LED 828LM VSM 3000K DIM.","Asker","Bollard","Aluminium",null,null,"PRO","LED zintegrowane","AC","DIM.","5,8W","7,7W","828lm","604lm",null,null,"65","IK08","Class I",3000,"szerokie dół",0.55000000000000004,0.2,0.11,"CE",null,null,"> 109 000h",1,"Oprawa słupkowa.","Soczewka firmy Ledil typu VSM (IESNA typ V).","VSM","Luminaire with a contemporary design For lighting gardens, private areas and other architectural concepts",null,null,null,"Odlew aluminiowy malowany proszkowo.",null,"Soczewka hermetyczna zewnętrzna- tworzywo sztuczne PMMA przeźroczyste.","Uszczelka silikonowa.","Dławnica EPDM.","55cm",null,"Oprawa ściemnialna fazowo TRAILING EDGE (TE)","Moduł LED","Cree DK200402 V1 XTE-HE 3K","Philips Xitanium 10W 0,5A 20V TE SC 230V",0,"Philips Xitanium TE",0.01,80,"E","1907ZX0009, 1908GA0009, 3081XX0009","Zaciski podłączeniowe: max 3x2,5mm², możliwość podłączenia oprawy w pętle max 3x1,5mm². Przewód w oponie okrągłej o średnicy max ø12,5mm.","5216XX0009.jpg","5216XX0009.ldt",1,null,1,47]
["5217","5217XX0009","ASKER PRO BOLLARD 55CM LED 828LM VSM 4000K DIM.","Asker","Bollard","Aluminium",null,null,"PRO","LED zintegrowane","AC","DIM.","5,8W","7,7W","828lm","654lm",null,null,"65","IK08","Class I",4000,"szerokie dół",0.55000000000000004,0.2,0.11,"CE",null,null,"> 109 000h",1,"Oprawa słupkowa.","Soczewka firmy Ledil typu VSM (IESNA typ V).","VSM","A luminaire with a contemporary design. For lighting gardens, private areas and other architectural concepts.",null,null,null,"Odlew aluminiowy malowany proszkowo.",null,"Soczewka hermetyczna zewnętrzna- tworzywo sztuczne PMMA przeźroczyste.","Uszczelka silikonowa.","Dławnica EPDM.","55cm",null,"Oprawa ściemnialna fazowo TRAILING EDGE (TE)","Moduł LED","Cree DK200402 V1 XTE-HE 3V 4K.","Philips Xitanium 10W 0,5A 20V TE SC 230V",0,"Philips Xitanium TE",0.01,80,"E","1907ZX0009, 1908GA0009, 3081XX0009","Zaciski podłączeniowe: max 3x2,5mm², możliwość podłączenia oprawy w pętle max 3x1,5mm². Przewód w oponie okrągłej o średnicy max ø12,5mm.","5217XX0009.jpg","5217XX0009.ldt",1,null,1,47]
["5218","5218XX0009","ASKER PRO BOLLARD 55CM LED 828LM SCL 3000K DALI","Asker","Bollard","Aluminium",null,null,"PRO","LED zintegrowane","AC","DALI","5,8W","7,8W","828lm","682lm",null,null,"65","IK08","Class I",3000,"szerokie dół",0,0,0,"CE",null,"DALI","> 109 000h",1,"Oprawa słupkowa.","Soczewka firmy Ledil typu SCL (IESNA typ II / III).","SCL","A luminaire with a contemporary design. For lighting gardens, private areas and other architectural concepts.",null,null,null,"Odlew aluminiowy malowany proszkowo.",null,"Soczewka hermetyczna zewnętrzna- tworzywo sztuczne PMMA przeźroczyste.","Uszczelka silikonowa.","Dławnica EPDM.","55cm",null,null,"Moduł LED","Cree DK200402 V1 XTE-HE 3K","Osram OTi DALI 15W 220-240V 1A0 NFC EAN 4062172061766",0,null,0.01,80,"E","1907ZX0009, 1908GA0009, 3081XX0009","Zaciski podłączeniowe: max 5x2,5mm², możliwość podłączenia oprawy w pętle max 5x1,5mm². Przewód w oponie okrągłej o średnicy max ø12,5mm.","5218XX0009.jpg","5218XX0009.ldt",3,null,1,46]
["5222","5222XX0009","ASKER POLE PRO 300CM LED 2667LM VSM 3000K DALI2","Asker,Pole","Post,Post complete","Aluminium",null,null,"PRO","LED zintegrowane","AC","DALI2","16,8W","19,5W","2667lm","2667lm",null,null,"65","IK08","Class I",3000,"szerokie dół",0.24,0.48,3,"CE",null,"DALI","> 120 000h",23,"Oprawa słupowa.","Soczewka firmy Ledil typu VSM (IESNA typ V).","VSM","For lighting private areas, parks and other architectural concepts","For lighting private areas, parks and other architectural concepts. Wide and even light flux",null,null,"Profil aluminiowy wyciskany, malowany proszkowo.",null,"Soczewka hermetyczna zewnętrzna- tworzywo sztuczne PMMA przeźroczyste.","Uszczelka silikonowa.",null,"300cm","dwu-segmentowy","Sterowanie światłem w systemie: DALI outdoor pełny program. Zasilacz zaprogramowany na max prąd. Programowanie pozostałych parametrów po uzgodnieniu z Działem Handlowym firmy Norlys.","Moduł LED","Philips Fortimo FastFlex LED 2x6 DP G5 3K","Philips Xi FP 22W 0,2-0,7A SNLDAE 230V S175 sXt",100000,"DALI2 / NightDim (XI FP NLD)",null,70,"D","7666ZX0009","Zaciski podłączeniowe: max 5x2,5mm², możliwość podłączenia oprawy w pętle max 5x2,5mm². Przewód w oponie okrągłej o średnicy: ø8...12mm lub ø10...13,6mm","5222XX0009.jpg","5222XX0009.ldt",3,null,1,47]
["5223","5223XX0009","ASKER POLE PRO 300CM LED VSM 4000K DALI2","Asker","Post","Aluminium",null,null,"PRO","LED zintegrowane","AC","DALI2","16,8W","19,7W",null,"2681lm",null,null,"65","IK08","Class I",4000,"szerokie dół",0.24,0.48,3,"CE",null,"DALI",">100 000h",23,"Oprawa słupowa.","Soczewka firmy Ledil typu VSM (IESNA typ V).","VSM","For lighting private areas, parks and other architectural concepts","For lighting private areas, parks and other architectural concepts. Wide and even light flux",null,null,"Profil aluminiowy wyciskany, malowany proszkowo.",null,"Soczewka hermetyczna zewnętrzna- tworzywo sztuczne PMMA przeźroczyste.","Uszczelka silikonowa.",null,"300cm","dwu-segmentowy","Sterowanie światłem w systemie: DALI outdoor pełny program. Zasilacz zaprogramowany na max prąd. Programowanie pozostałych parametrów po uzgodnieniu z Działem Handlowym firmy Norlys.","Moduł LED","Philips Fortimo FastFlex LED 2x6 DP G5 4K","Philips Xi FP 22W 0,2-0,7A SNLDAE 230V S175 sXt",100000,"DALI2 / NightDim (XI FP NLD)",null,70,"D","7666ZX0009, B-50","Zaciski podłączeniowe: max 3x4mm², możliwość podłączenia oprawy w pętle max 3x2,5mm². Przewód w oponie okrągłej o średnicy: ø4…8mm; ø8...12mm lub ø10...13,6mm","5223XX0009.jpg","5223XX0009.ldt",3,null,1,47]
["5224","5224XX0009","ASKER POLE PRO 300CM LED 2667LM VSM 3000K DIM.","Asker,Pole","Post,Post complete","Aluminium",null,null,"PRO","LED zintegrowane","AC","DIM.","16,8W","19,5W","2667lm","2660lm",null,null,"65","IK08","Class I",3000,"szerokie dół",0.24,0.48,3,"CE",null,null,"> 100 000h",23,"Oprawa słupowa.","Soczewka firmy Ledil typu VSM (IESNA typ V).","VSM","For lighting outdoor areas, parks and other architectural concepts","For lighting private areas, parks and other architectural concepts. Wide, even light flux",null,null,"Profil aluminiowy wyciskany, malowany proszkowo.",null,"Soczewka hermetyczna zewnętrzna- tworzywo sztuczne PMMA przeźroczyste.","Uszczelka silikonowa.",null,"300cm","dwu-segmentowy","Oprawa ściemnialna fazowo TRAILING EDGE (TE) - LEADING EDGE (LE)","Moduł LED","Philips Fortimo FastFlex LED 2x6 DP G5 3K","TCI Mini MD 20W 500mA BI code 127033 Triak",0,null,null,70,"D","7666ZX0009","Zaciski podłączeniowe: max 5x2,5mm², możliwość podłączenia oprawy w pętle max 5x2,5mm². Przewód w oponie okrągłej o średnicy: ø8...12mm lub ø10...13,6mm","5224XX0009.jpg","5224XX0009.ldt",1,null,1,47]
["5225","5225XX0009","ASKER POLE PRO 300CM LED 2772LM VSM 4000K DIM.","Asker,Pole","Post,Post complete","Aluminium",null,null,"PRO","LED zintegrowane","AC","DIM.","16,8W","19,7W","2772lm","2790lm",null,null,"65","IK08","Class I",4000,"szerokie dół",0.24,0.48,3,"CE",null,null,"> 100 000h",23,"Oprawa słupowa.","Soczewka firmy Ledil typu VSM (IESNA typ V).","VSM","For lighting outdoor areas, parks and other architectural concepts","For lighting private areas, parks and other architectural concepts. Wide, even light flux",null,null,"Profil aluminiowy wyciskany, malowany proszkowo.",null,"Soczewka hermetyczna zewnętrzna- tworzywo sztuczne PMMA przeźroczyste.","Uszczelka silikonowa.",null,"300cm","dwu-segmentowy","Sterowanie światłem w systemie: DALI outdoor pełny program. Zasilacz zaprogramowany na max prąd. Programowanie pozostałych parametrów po uzgodnieniu z Działem Handlowym firmy Norlys.","Moduł LED","Philips Fortimo FastFlex LED 2x6 DP G5 4K","TCI Mini MD 20W 500mA BI code 127033 Triak",0,null,null,70,"D","7666ZX0009","Zaciski podłączeniowe: max 5x2,5mm², możliwość podłączenia oprawy w pętle max 5x2,5mm². Przewód w oponie okrągłej o średnicy: ø8...12mm lub ø10...13,6mm","5225XX0009.jpg","5225XX0009.ldt",1,null,1,47]
["5226","5226XX0009","ASKER POLE PRO 300CM LED 2628LM T2-L 3000K DALI2","Asker,Pole","Post,Post complete","Aluminium",null,null,"PRO","LED zintegrowane","AC","DALI2","16,8W","19,5W","2628lm","2646lm",null,null,"65","IK08","Class I",3000,"szerokie dół",0.24,0.48,3,"CE",null,"DALI","> 100 000h",23,"Oprawa słupowa.","Soczewka firmy Ledil typu T2-L (IESNA typ III).","T2-L","For lighting outdoor areas, parks and other architectural concepts","For lighting private areas, parks and other architectural concepts. Wide, even light flux",null,null,"Profil aluminiowy wyciskany, malowany proszkowo.",null,"Soczewka hermetyczna zewnętrzna- tworzywo sztuczne PMMA przeźroczyste.","Uszczelka silikonowa.",null,"300cm","dwu-segmentowy","Sterowanie światłem w systemie: DALI outdoor pełny program. Zasilacz zaprogramowany na max prąd. Programowanie pozostałych parametrów po uzgodnieniu z Działem Handlowym firmy Norlys.","Moduł LED","Philips Fortimo FastFlex LED 2x6 DP G5 3K","Philips Xi FP 22W 0,2-0,7A SNLDAE 230V S175 sXt",100000,"DALI2 / NightDim (XI FP NLD)",null,70,"D","7666ZX0009","Zaciski podłączeniowe: max 5x2,5mm², możliwość podłączenia oprawy w pętle max 5x2,5mm². Przewód w oponie okrągłej o średnicy: ø8...12mm lub ø10...13,6mm","5226XX0009.jpg","5226XX0009.ldt",3,null,1,48]
["5227","5227XX0009","ASKER POLE PRO 300CM LED 2910LM T2-L 4000K DALI2","Asker,Pole","Post,Post complete","Aluminium",null,null,"PRO","LED zintegrowane","AC","DALI2","16,8W","19,4W","2910lm","2782lm",null,null,"65","IK08","Class I",4000,"szerokie dół",0.24,0.48,3,"CE",null,"DALI","> 100 000h",23,"Oprawa słupowa.","Soczewka firmy Ledil typu T2-L (IESNA typ III).","T2-L","For lighting outdoor areas, parks and other architectural concepts","For lighting private areas, parks and other architectural concepts. Wide, even light flux",null,null,"Profil aluminiowy wyciskany, malowany proszkowo.",null,"Soczewka hermetyczna zewnętrzna- tworzywo sztuczne PMMA przeźroczyste.","Uszczelka silikonowa.",null,"300cm","dwu-segmentowy","Sterowanie światłem w systemie: DALI outdoor pełny program. Zasilacz zaprogramowany na max prąd. Programowanie pozostałych parametrów po uzgodnieniu z Działem Handlowym firmy Norlys.","Moduł LED","Philips Fortimo FastFlex LED 2x6 DP G5 4K","Philips Xi FP 22W 0,2-0,7A SNLDAE 230V S175 sXt",100000,null,null,70,"D","7666ZX0009","Zaciski podłączeniowe: max 5x2,5mm², możliwość podłączenia oprawy w pętle max 5x2,5mm². Przewód w oponie okrągłej o średnicy: ø8...12mm lub ø10...13,6mm","5227XX0009.jpg","5227XX0009.ldt",3,null,1,48]
["5228","5228XX0009","ASKER POLE PRO 300CM LED 2687LM T2-L 3000K DIM.","Asker,Pole","Post,Post complete","Aluminium",null,null,"PRO","LED zintegrowane","AC","DIM.","16,8W","19,6W","2687lm","2666lm",null,null,"65","IK08","Class I",3000,"szerokie dół",0.24,0.48,3,"CE",null,null,"> 100 000h",23,"Oprawa słupowa.","Soczewka firmy Ledil typu T2-L (IESNA typ III).","T2-L","For lighting outdoor areas, parks and other architectural concepts","For lighting private areas, parks and other architectural concepts. Wide, even light flux",null,null,"Profil aluminiowy wyciskany, malowany proszkowo.",null,"Soczewka hermetyczna zewnętrzna- tworzywo sztuczne PMMA przeźroczyste.","Uszczelka silikonowa.",null,"300cm","dwu-segmentowy","Oprawa ściemnialna fazowo TRAILING EDGE (TE) - LEADING EDGE (LE)","Moduł LED","Philips Fortimo FastFlex LED 2x6 DP G5 3K","TCI Mini MD 20W 500mA BI code 127033 Triak",0,null,null,70,"D","7666ZX0009","Zaciski podłączeniowe: max 5x2,5mm², możliwość podłączenia oprawy w pętle max 5x2,5mm². Przewód w oponie okrągłej o średnicy: ø8...12mm lub ø10...13,6mm","5228XX0009.jpg","5228XX0009.ldt",1,null,1,48]
["5229","5229XX0009","ASKER POLE PRO 300CM LED 2910LM T2-L 4000K DIM.","Asker,Pole","Post,Post complete","Aluminium",null,null,"PRO","LED zintegrowane","AC","DIM.","16,8W","19,4W","2910lm","2774lm",null,null,"65","IK08","Class I",4000,"szerokie dół",0.24,0.48,3,"CE",null,null,"> 100 000h",23,"Oprawa słupowa.","Soczewka firmy Ledil typu T2-L (IESNA typ III).","T2-L","For lighting outdoor areas, parks and other architectural concepts","For lighting private areas, parks and other architectural concepts. Wide, even light flux",null,null,"Profil aluminiowy wyciskany, malowany proszkowo.",null,"Soczewka hermetyczna zewnętrzna- tworzywo sztuczne PMMA przeźroczyste.","Uszczelka silikonowa.",null,"300cm","dwu-segmentowy","Oprawa ściemnialna fazowo TRAILING EDGE (TE) - LEADING EDGE (LE)","Moduł LED","Philips Fortimo FastFlex LED 2x6 DP G5 4K","TCI Mini MD 20W 500mA BI code 127033 Triak",0,null,null,70,"D","7666ZX0009","Zaciski podłączeniowe: max 5x2,5mm², możliwość podłączenia oprawy w pętle max 5x2,5mm². Przewód w oponie okrągłej o średnicy: ø8...12mm lub ø10...13,6mm","5229XX0009.jpg","5229XX0009.ldt",1,null,1,48]
["5253","5253XX0009","NORDLAND CEILING/WALL LED 3796LM 3000K DALI2","Nordland","Wall,Ceiling","Aluminium",null,null,null,"LED zintegrowane","AC","DALI2","24,8W","28,9W","3796lm","2183lm",null,null,"65","IK10","Class I",3000,null,0.28000000000000003,0.28000000000000003,0.1,"CE",null,"DALI","> 80 000h",7,"Oprawa sufitowo-ścienna.","Światło rozproszone.",null,"A ceiling type luminaire with a modern design For lighting private areas and other architectural concepts",null,null,null,"Odlew aluminiowy malowany proszkowo.",null,"Klosz- poliwęglan mleczny, stabilizowany UV.","Uszczelka silikonowa.","Dławnica EPDM.","NIE",null,"Sterowanie światłem w systemie: DALI/TD.","Moduł LED","TCI RM160E78 128964/830H 3K","TCI ATON 38 DALI NFC BI 151376",0,null,null,80,"D",null,"Zaciski podłączeniowe: max 5x1,5mm², możliwość podłączenia oprawy w pętle max 5x1,5mm². Przewód w oponie okrągłej o średnicy ø7...10,5mm.","5253XX0009.jpg","5253XX0009.ldt",3,null,1,7]
["5255","5255XX0009","NORDLAND CEILING/WALL LED 3996LM 4000K DALI2","Nordland","Wall,Ceiling","Aluminium",null,null,null,"LED zintegrowane","AC","DALI2","24,8W","28,9W","3996lm","2308lm",null,null,"65","IK10","Class I",4000,null,0.28000000000000003,0.28000000000000003,0.1,"CE",null,"DALI","> 80 000h",7,"Oprawa sufitowo-ścienna.","Światło rozproszone.",null,"A ceiling type luminaire with a modern design For lighting private areas and other architectural concepts",null,null,null,"Odlew aluminiowy malowany proszkowo.",null,"Klosz- poliwęglan mleczny, stabilizowany UV.","Uszczelka silikonowa.","Dławnica EPDM.","NIE",null,"Sterowanie światłem w systemie: DALI/TD.","Moduł LED","TCI RM160E78 128964/840H 4K","TCI ATON 38 DALI NFC BI 151376",0,null,null,80,"D",null,"Zaciski podłączeniowe: max 5x1,5mm², możliwość podłączenia oprawy w pętle max 5x1,5mm². Przewód w oponie okrągłej o średnicy ø7...10,5mm.","5255XX0009.jpg","5255XX0009.ldt",3,null,1,7]
["537","537XX0014","RONDANE CEILING/WALL LED 1059LM 3000K DIM.","Rondane","Wall,Ceiling","Aluminium",null,null,null,"LED zintegrowane","AC","DIM.","6,7W","8,5W","1059lm","305lm",null,null,"65","IK10","Class I",3000,null,0,0,0,"CE",null,null,"> 110 000",7,"Oprawa sufitowo-ścienna.","Światło rozproszone.",null,"A ceiling-type luminaire with a modern design",null,null,null,"Odlew aluminiowy malowany proszkowo.",null,"Klosz- poliwęglan mleczny, stabilizowany UV.","Uszczelka silikonowa.","Dławnica EPDM.",null,null,"Oprawa ściemnialna fazowo TRAILING EDGE (TE) - LEADING EDGE (LE)","Moduł LED","Philips Fortimo SLM C 1203 L09 1619 G7 3K","KGP CC15W200-350CG",50000,"Dim. TRIAC (KGP)",null,80,"D",null,"Zaciski podłączeniowe: max 3x2,5mm², możliwość podłączenia oprawy w pętle max 3x1,5mm². Przewód w oponie okrągłej o średnicy ø7...10,5mm.","537XX0014.jpg","537XX0014.ldt",1,null,1,7]
["539","539XX0011","RONDANE CEILING/WALL LED 1950LM 3000K ON/OFF","Rondane","Wall,Ceiling","Aluminium",null,null,null,"LED zintegrowane","AC","ON/OFF","17,5W","17,5W","1950lm","732lm",null,null,"65","IK10","Class I",3000,null,0,0,0,"CE",null,null,"50 000h",7,"Oprawa sufitowo-ścienna.","Światło rozproszone.",null,"A ceiling-type luminaire with a modern design",null,null,null,"Odlew aluminiowy malowany proszkowo.",null,"Klosz- poliwęglan mleczny, stabilizowany UV.","Uszczelka silikonowa.","Dławnica EPDM.",null,null,"Oprawa nieściemnialna","Moduł LED","Philips Fortimo DLM ES 2000/8xx G2 3K",null,0,null,null,80,"E",null,"Zaciski podłączeniowe: max 3x2,5mm², możliwość podłączenia oprawy w pętle max 3x1,5mm². Przewód w oponie okrągłej o średnicy ø7...10,5mm.","539XX0011.jpg","539XX0011.ldt",4,null,1,7]
["541","541XX0014","BORNHOLM CEILING/WALL LED 1059LM 3000K DIM.","Bornholm","Wall,Ceiling","Aluminium",null,null,null,"LED zintegrowane","AC","DIM.","6,7W","7,8W","1059lm","428lm",null,null,"65","IK10","Class I",3000,null,0,0,0,"CE",null,null,"> 50 000h",7,"Oprawa sufitowo-ścienna.","Światło rozproszone.",null,"A ceiling-type luminaire with a modern design",null,null,null,"Odlew aluminiowy malowany proszkowo.",null,"Klosz- poliwęglan mleczny, stabilizowany UV.","Uszczelka silikonowa.","Dławnica EPDM.",null,null,"Oprawa ściemnialna fazowo TRAILING EDGE (TE) - LEADING EDGE (LE)","Moduł LED","Philips Fortimo SLM C 1203 L09 1619 G7 3K","KGP CC15W200-350CG",50000,"Dim. TRIAC (KGP)",null,80,"D",null,"Zaciski podłączeniowe: max 3x2,5mm², możliwość podłączenia oprawy w pętle max 3x1,5mm². Przewód w oponie okrągłej o średnicy ø7...10,5mm.","541XX0014.jpg","541XX0014.ldt",1,null,1,7]
["542","542XX0011","BORNHOLM CEILING/WALL LED 1950LM 3000K ON/OFF","Bornholm","Wall,Ceiling","Aluminium",null,null,null,"LED zintegrowane","AC","ON/OFF","17,5W","17,5W","1950lm","794lm",null,null,"65","IK10","Class I",3000,null,0,0,0,"CE",null,null,"50 000h",7,"Oprawa sufitowo-ścienna.","Światło rozproszone.",null,"A ceiling lauminaire with a modern design",null,null,null,"Odlew aluminiowy malowany proszkowo.",null,"Klosz- poliwęglan mleczny, stabilizowany UV.","Uszczelka silikonowa.","Dławnica EPDM.",null,null,"Oprawa nieściemnialna","Moduł LED","Philips Fortimo DLM ES 2000/8xx G2 3K",null,0,null,null,80,"E",null,"Zaciski podłączeniowe: max 3x2,5mm², możliwość podłączenia oprawy w pętle max 3x1,5mm². Przewód w oponie okrągłej o średnicy ø7...10,5mm.","542XX0011.jpg","542XX0011.ldt",4,null,1,7]
["544","544XX0009","BORNHOLM CEILING/WALL LED 1080LM 3000K MD","Bornholm","Wall","Aluminium",null,null,null,"Wymienne",null,null,"9,5W","10W","1080lm","417lm",null,null,"65",null,"Class I",3000,null,0.28999999999999998,0.28999999999999998,0.09,"CE","Daylight sensor,Motion sensor",null,"50 000h",7,"Oprawa sufitowo-ścienna.","Światło rozproszone.",null,"A ceiling type luminaire with a modern design",null,null,null,"Odlew aluminiowy malowany proszkowo.",null,"Klosz- poliwęglan mleczny, stabilizowany UV.","Uszczelka silikonowa.","Dławnica EPDM.",null,"PIR","Oprawa wyposażona w mikrofalowy czujnik ruchu, z wyłącznikiem zmierzchowym i podtrzymaniem ruchu","Moduł LED","Philips Fortimo DLM ES 1100/8xx G2 3K",null,0,"Mikrofalowy czujnik ruchu MD (PD-MV1005)",null,80,"E",null,"Zaciski podłączeniowe: max 3x2,5mm², możliwość podłączenia oprawy w pętle max 3x1,5mm². Przewód w oponie okrągłej o średnicy ø7...10,5mm.","544XX0009.jpg","544XX0009.ldt",3,null,1,7]
["545","545XX0009","BORNHOLM CEILING/WALL LED 1150LM 4000K MD","Bornholm","Wall","Aluminium",null,null,null,"Wymienne",null,null,"9,5W","10,5W","1150lm","464lm",null,null,"65",null,"Class I",4000,null,0.28999999999999998,0.28999999999999998,0.09,"CE","Daylight sensor,Motion sensor",null,"> 55 000h",7,"Oprawa sufitowo-ścienna.","Światło rozproszone.",null,"A ceiling type luminaire with a modern design",null,null,null,"Odlew aluminiowy malowany proszkowo.",null,"Klosz- poliwęglan mleczny, stabilizowany UV.","Uszczelka silikonowa.","Dławnica EPDM.",null,"PIR","Oprawa wyposażona w mikrofalowy czujnik ruchu, z wyłącznikiem zmierzchowym i podtrzymaniem ruchu","Moduł LED","Philips Fortimo DLM ES 1100/8xx G2 4K",null,0,"Mikrofalowy czujnik ruchu MD (PD-MV1005)",null,80,"E",null,"Zaciski podłączeniowe: max 3x2,5mm², możliwość podłączenia oprawy w pętle max 3x1,5mm². Przewód w oponie okrągłej o średnicy ø7...10,5mm.","545XX0009.jpg","545XX0009.ldt",3,null,1,7]
["548","548XX0009","RONDANE CEILING/WALL LED 1080LM 3000K MD","Rondane","Wall,Ceiling","Aluminium",null,null,null,"LED zintegrowane","AC","MD","9,5W","9,5W","1080lm","345lm",null,null,"65","IK10","Class I",3000,null,0.26,0.26,0.1,"CE","Daylight sensor,Motion sensor",null,"50 000h",7,"Oprawa sufitowo-ścienna.","Światło rozproszone.",null,"A ceiling type luminaire with a modern design",null,null,null,"Odlew aluminiowy malowany proszkowo.",null,"Klosz- poliwęglan mleczny, stabilizowany UV.","Uszczelka silikonowa.","Dławnica EPDM.","TAK",null,"Oprawa wyposażona w mikrofalowy czujnik ruchu, z wyłącznikiem zmierzchowym i podtrzymaniem ruchu","Moduł LED","Philips Fortimo DLM ES 1100/8xx G2 3K",null,0,"Mikrofalowy czujnik ruchu MD (PD-MV1005)",null,80,"E",null,"Zaciski podłączeniowe: max 3x2,5mm², możliwość podłączenia oprawy w pętle max 3x1,5mm². Przewód w oponie okrągłej o średnicy ø7...10,5mm.","548XX0009.jpg","548XX0009.ldt",3,null,1,7]
["549","549XX0009","RONDANE CEILING/WALL LED 1150LM 4000K MD","Rondane","Wall,Ceiling","Aluminium",null,null,null,"LED zintegrowane","AC","MD","9,5W","9,5W","1150lm","366lm",null,null,"65","IK10","Class I",4000,null,0.26,0.26,0.1,"CE","Daylight sensor,Motion sensor",null,"50 000h",7,"Oprawa sufitowo-ścienna.","Światło rozproszone.",null,"A ceiling type luminaire with a modern design",null,null,null,"Odlew aluminiowy malowany proszkowo.",null,"Klosz- poliwęglan mleczny, stabilizowany UV.","Uszczelka silikonowa.","Dławnica EPDM.","TAK",null,"Oprawa wyposażona w mikrofalowy czujnik ruchu, z wyłącznikiem zmierzchowym i podtrzymaniem ruchu","Moduł LED","Philips Fortimo DLM ES 1100/8xx G2 4K",null,0,"Mikrofalowy czujnik ruchu MD (PD-MV1005)",null,80,"D",null,"Zaciski podłączeniowe: max 3x2,5mm², możliwość podłączenia oprawy w pętle max 3x1,5mm². Przewód w oponie okrągłej o średnicy ø7...10,5mm.","549XX0009.jpg","549XX0009.ldt",3,null,1,7]
["553","553XX0010","NARVIK II BOLLARD LED 1940LM 3000K DIM.","Narvik","Bollard","Aluminium",null,null,null,"LED zintegrowane","AC","DIM.","10,9W","13,6W","1940lm","853lm",null,null,"65","IK10","Class II",3000,null,0.24,0.24,0.95,"CE",null,null,"> 72 000h",1,"Oprawa słupkowa.","Czterostronny wylot światła przysłonięty od góry.",null,"A bollard luminaire with a stable and durable structure. For lighting private and public areas",null,null,null,"Odlew aluminiowy malowany proszkowo.",null,"Klosz- tworzywo sztuczne PMMA przeźroczyste.","Uszczelka silikonowa.",null,null,"przeźroczysty","Oprawa ściemnialna fazowo TRAILING EDGE (TE) - LEADING EDGE (LE)","Moduł LED","Cree DK210704 V2 JB2835 3V 3K","TCI Mini MD 20W 500mA code 127032 Triak",0,null,null,80,"C","110GA0009, 505ZX0009, 7667ZX0009","Zaciski podłączeniowe: max 2x4mm², możliwość podłączenia oprawy w pętle max 2x4mm². Przewód w oponie okrągłej o średnicy: ø8...12mm lub ø10...14mm. Oprawa wyposażona w drzwiczki rewizyjne","553XX0010.png","553XX0010.LDT",1,null,1,16]
["557","557XX0017","NARVIK BOLLARD LED 3137LM 3000K ON/OFF","Narvik","Bollard","Aluminium",null,null,null,"LED zintegrowane","AC","ON/OFF","19W","21,8W","3137lm","556lm",null,null,"65","IK10","Class I",3000,"szerokie dół",0.24,0.24,0.95,"CE",null,null,">110 000h",1,"Oprawa słupkowa.","Czterostronny wylot światła przysłonięty od góry.",null,"A bollard luminaire with a stable and durable structure. For lighting private and public areas",null,null,null,"Odlew aluminiowy malowany proszkowo.",null,"Klosz- poliwęglan przeźroczysty, stabilizowany UV.","Uszczelka silikonowa.",null,null,null,"Oprawa nieściemnialna","Moduł LED","Philips Fortimo SLM C 1208 L15 2024 G7 3K","Philips Xitanium 36W/m 929001486006",0,null,0,80,"D","110GA0009, 505ZX0009, 7667ZX0009","Zaciski podłączeniowe: max 3x4mm², możliwość podłączenia oprawy w pętle max 3x2,5mm². Przewód w oponie okrągłej o średnicy max ø12,5mm. Oprawa wyposażona w drzwiczki rewizyjne","557XX0017.jpg","557XX0017.ldt",4,null,1,16]
["559","559XX0010","NARVIK II BOLLARD LED 1940LM 3000K DIM.","Narvik","Bollard","Aluminium",null,null,null,"LED zintegrowane","AC","DIM.","10,9W","13,4W","1940lm","666lm",null,null,"65","IK10","Class II",3000,null,0.24,0.24,0.95,"CE",null,null,"> 72 000h",1,"Oprawa słupkowa.","Czterostronny wylot światła przysłonięty od góry.",null,"A bollard luminaire with a stable and durable structure. For lighting private and public areas.",null,null,null,"Odlew aluminiowy malowany proszkowo.",null,"Klosz- tworzywo sztuczne PMMA satynowane.","Uszczelka silikonowa.",null,null,"satynowany","Oprawa ściemnialna fazowo TRAILING EDGE (TE) - LEADING EDGE (LE)","Moduł LED","Cree DK210704 V2 JB2835 3V 3K","TCI Mini MD 20W 500mA code 127032 Triak",0,null,null,80,"C","110GA0009, 505ZX0009, 7667ZX0009.","Zaciski podłączeniowe: max 2x4mm², możliwość podłączenia oprawy w pętle max 2x4mm². Przewód w oponie okrągłej o średnicy: ø8...12mm lub ø10...14mm. Oprawa wyposażona w drzwiczki rewizyjne","559XX0010.png","559XX0010.ldt",1,null,1,16]
["576","576XX0309","VISBY POLE-TOP 2XLED 4900LM 3000K","Visby","Post,Head","Aluminium",null,null,null,"LED zintegrowane","AC",null,"44,5W","44,5W","4900lm","2465lm",null,null,"65","IK05","Class I",3000,null,0,0,0,"CE",null,null,"50000",2,"Oprawa słupowa (nasadzana).","Światło obrotowo- symetryczne (kombinacja pośrednie/bezpośrednie).",null,"A mounted luminaire designed to be mounted on a lighting pole with a Ø60mm mounting shaft",null,null,"Oprawa wyposażona w wymienne źródło światła typu moduł LED, który zapewnia trwałość i optymalny rozsył światła, przy zachowaniu stosunkowo niskiego zużycia energii.","Odlew aluminiowy malowany proszkowo.",null,"Klosz- tworzywo sztuczne PMMA przeźroczyste.","Uszczelka silikonowa.",null,null,null,"Oprawa nieściemnialna","2 Moduły LED","Philips Fortimo LED DLM ES 3000lm/2000lm G2",null,null,null,0.02,80,"E","3005XX0009, 7660XX0009, 7662ZX0009, 7664ZX0009","Przewód H05VV-F 3G1 o długości 4,5m do podłączenia wewnątrz słupa oświetleniowego (w odpowiednio dobranej puszce elektroinstalacyjnej). Możliwość sterowania modułami LED (zał./wył.): świecenie modułu górnego i dolnego, lub tylko modułu górnego (światło pośrednie, 3000lm/27W), lub tylko modułu dolnego (światło bezpośrednie, 2000lm/17,5W).","576XX0309.jpg","576XX0309.ldt",4,null,1,30]
["577","577XX0309","VISBY POLE-TOP LED 2950LM 3000K","Visby","Post,Head","Aluminium",null,null,null,"LED zintegrowane","AC",null,"27W","27W","2950lm","1388lm",null,null,"65",null,"Class I",3000,null,0,0,0,"CE",null,null,"50000",2,"Oprawa słupowa (nasadzana).","Światło obrotowo-symetryczne pośrednie.",null,"Pole top luminaire for installation on a lighting pole with Ø60mm mounting cap.",null,null,"Oprawa wyposażona w wymienne źródło światła typu moduł LED, który zapewnia trwałość i optymalny rozsył światła, przy zachowaniu stosunkowo niskiego zużycia energii.","Odlew aluminiowy malowany proszkowo.",null,"Klosz- tworzywo sztuczne PMMA przeźroczyste.","Uszczelka silikonowa.",null,null,null,"Oprawa nieściemnialna","Moduł LED","Philips Fortimo LED DLM ES 3000lm G2",null,null,null,0.03,80,"E","3005XX0009, 7660XX0009, 7662ZX0009, 7664ZX0009","Przewód H05VV-F 3G1 o długości 4,5m do podłączenia wewnątrz słupa oświetleniowego (w odpowiednio dobranej puszce elektroinstalacyjnej).","577XX0309.jpg","577XX0309.ldt",4,null,1,2]
["596","596XX0011","KIRUNA WALL LED 1950LM 3000K","Kiruna","Wall,Ceiling","Aluminium",null,null,null,"LED zintegrowane","AC",null,"17,5W","17,5W","1950lm","604lm",null,null,"65","IK10","Class I",3000,null,0,0,0,"CE",null,null,"50000",12,"Oprawa ścienna.","Światło rozproszone przysłonięte od góry.",null,"Luminaire with stable and durable construction. For use in private and public areas requiring high resistance to external mechanical damage.",null,null,"Oprawa wyposażona w wymienne źródło światła typu moduł LED, który zapewnia trwałość i optymalny rozsył światła, przy zachowaniu stosunkowo niskiego zużycia energii.","Odlew aluminiowy malowany proszkowo.",null,"Klosz- poliwęglan mleczny, stabilizowany UV.","Uszczelka silikonowa.","Dławnica EPDM.",null,"mleczny","Oprawa nieściemnialna","Moduł LED","Philips LED Fortimo DLM ES 2000/830 G2",null,null,null,null,80,"E",null,"Zaciski podłączeniowe: 3x2,5mm², możliwość podłączenia oprawy w pętle max 3x2,5mm². Przewód w oponie okrągłej o średnicy ø7...10,5mm.","596XX0011.jpg","596XX0011.ldt",4,null,1,25]
["6031","6031XX0010","NAMSOS WALL-RECESSED LED 2006LM 4000K DALI2","Namsos","Recessed","Aluminium",null,null,null,"LED zintegrowane","AC","DALI2","11W","13,8W","2006lm","877lm",null,null,"65","IK08","Class I",4000,null,0.22,0.22,0.12,"CE",null,"DALI","> 102 000h",11,"Oprawa wbudowana ścienna.","Światło rozproszone półsferyczne ukierunkowane w dół",null,"The luminaire is adapted to illuminate stairs, steps, staircases, pathways for ceiling lighting and implementation of other architectural concepts",null,null,null,"Odlew aluminiowy malowany proszkowo.",null,"Klosz- szkło bezpieczne, satynowane.","Uszczelka silikonowa.","Dławnica EPDM.",null,null,"Sterowanie światłem w systemie: DALI/TD.","Moduł LED","Cree DK200305 V3 JB2835 3V 4K","Osram IT DALI 30-220…240-700 CS Switch 4062172306232",50000,null,null,80,"C",null,"Zaciski podłączeniowe: max 5x1,5mm², możliwość podłączenia oprawy w pętle max 5x1,5mm². Przewód w oponie okrągłej o średnicy ø7...10,5mm.","6031XX0010.jpg","6031XX0010.ldt",3,null,1,76]
["6032","6032XX0010","NAMSOS WALL-RECESSED LED 1891LM 3000K DALI2","Namsos","Recessed","Aluminium",null,null,null,"LED zintegrowane","AC","DALI2","11W","13,8W","1891lm","904lm",null,null,"65","IK08","Class I",3000,null,0.22,0.22,0.12,"CE",null,"DALI","> 102 000h",11,"Oprawa wbudowana ścienna.","Światło rozproszone półsferyczne ukierunkowane w dół",null,"The luminaire is adapted to illuminate stairs, steps, staircases, pathways for ceiling lighting and implementation of other architectural concepts",null,null,null,"Odlew aluminiowy malowany proszkowo.",null,"Klosz- szkło bezpieczne, satynowane.","Uszczelka silikonowa.","Dławnica EPDM.",null,null,"Sterowanie światłem w systemie: DALI/TD.","Moduł LED","Cree DK200305 V3 JB2835 3V 3K","Osram IT DALI 30-220…240-700 CS Switch 4062172306232",50000,null,null,80,"C",null,"Zaciski podłączeniowe: max 5x1,5mm², możliwość podłączenia oprawy w pętle max 5x1,5mm². Przewód w oponie okrągłej o średnicy ø7...10,5mm.","6032XX0010.jpg","6032XX0010.ldt",3,null,1,76]
["6033","6033XX0009","NAMSOS BOLLARD 95CM LED 1891LM 3000K DALI2","Namsos","Bollard","Aluminium",null,null,null,"LED zintegrowane","AC","DALI2","11W","13,8W","1891lm","904lm",null,null,"65","IK07","Class I",3000,null,0.24,0.12,0.95,"CE",null,"DALI","> 102 000h",1,"Oprawa słupkowa.","Światło rozproszone półsferyczne ukierunkowane w dół",null,"Luminaire with a modern design. For lighting gardens and other private and public areas",null,null,null,"Odlew aluminiowy malowany proszkowo.",null,"Klosz- szkło bezpieczne, satynowane.","Uszczelka silikonowa.","Dławnica EPDM.","95cm",null,"Sterowanie światłem w systemie: DALI/TD.","Moduł LED","Cree DK200305 V3 JB2835 3V 3K","Osram IT DALI 30-220…240-700 CS Switch 4062172306232",50000,null,null,80,"C","112ZX0009, 113GA0009, 114GA0009","Zaciski podłączeniowe: max 5x2,5mm², możliwość podłączenia oprawy w pętle max 5x2,5mm². Przewód w oponie okrągłej o średnicy: ø8...12mm lub ø10...14mm.","6033XX0009.jpg","6033XX0009.ldt",3,null,1,76]
["6034","6034XX0009","NAMSOS BOLLARD 65CM LED 1891LM 3000K DALI2","Namsos","Bollard","Aluminium",null,null,null,"LED zintegrowane","AC","DALI2","11W","13,8W","1891lm","904lm","Tworzywo sztuczne","Satynowany","65","IK08","Class I",3000,null,0.24,0.12,0.65,"CE",null,"DALI","> 102 000h",1,"Oprawa słupkowa.","Światło rozproszone półsferyczne ukierunkowane w dół",null,"Luminaire with a modern design. For lighting gardens and other private and public areas",null,null,null,"Odlew aluminiowy malowany proszkowo.",null,"Klosz- szkło bezpieczne, satynowane.","Uszczelka silikonowa.","Dławnica EPDM.","65cm",null,"Sterowanie światłem w systemie: DALI/TD.","Moduł LED","Cree DK200305 V3 JB2835 3V 3K","Osram IT DALI 30-220…240-700 CS Switch 4062172306232",50000,null,null,80,"C","112ZX0009, 113GA0009, 114GA0009","Zaciski podłączeniowe: max 5x2,5mm², możliwość podłączenia oprawy w pętle max 5x2,5mm². Przewód w oponie okrągłej o średnicy: ø8...12mm lub ø10...14mm.","6034XX0009.jpg","6034XX0009.ldt",3,null,1,76]
["6035","6035XX0009","NAMSOS BOLLARD 95CM LED 2006LM 4000K DALI2","Namsos","Bollard","Aluminium",null,null,null,"LED zintegrowane","AC","DALI2","11W","13,8W","2006lm","877lm",null,null,"65",null,"Class I",4000,null,0.24,0.12,0.95,"CE",null,"DALI","> 102 000h",1,"Oprawa słupkowa.","Światło rozproszone półsferyczne ukierunkowane w dół",null,"Luminaire with a modern design. For lighting gardens and other private and public areas",null,null,null,"Odlew aluminiowy malowany proszkowo.",null,"Klosz- szkło bezpieczne, satynowane.","Uszczelka silikonowa.","Dławnica EPDM.","95cm",null,"Sterowanie światłem w systemie: DALI/TD.","Moduł LED","Cree DK200305 V3 JB2835 3V 3K","Osram IT DALI 30-220…240-700 CS Switch 4062172306232",50000,null,null,80,"C","112ZX0009, 113GA0009, 114GA0009","Zaciski podłączeniowe: max 5x2,5mm², możliwość podłączenia oprawy w pętle max 5x2,5mm². Przewód w oponie okrągłej o średnicy: ø8...12mm lub ø10...14mm.","6035XX0009.jpg","6035XX0009.ldt",3,null,1,76]
["6036","6036XX0009","NAMSOS BOLLARD 65CM LED 2006LM 4000K DALI2","Namsos","Bollard","Aluminium",null,null,null,"LED zintegrowane","AC","DALI2","11W","13,8W","2006lm","877lm","Tworzywo sztuczne","Satynowany","65","IK08","Class I",4000,null,0.24,0.12,0.65,"CE",null,"DALI","> 102 000h",1,"Oprawa słupkowa.","Światło rozproszone półsferyczne ukierunkowane w dół",null,"Luminaire with a modern design. For lighting gardens and other private and public areas",null,null,null,"Odlew aluminiowy malowany proszkowo.",null,"Klosz- szkło bezpieczne, satynowane.","Uszczelka silikonowa.","Dławnica EPDM.","65cm",null,"Sterowanie światłem w systemie: DALI/TD.","Moduł LED","Cree DK200305 V3 JB2835 3V 3K","Osram IT DALI 30-220…240-700 CS Switch 4062172306232",50000,null,null,80,"C","112ZX0009, 113GA0009, 114GA0009","Zaciski podłączeniowe: max 5x2,5mm², możliwość podłączenia oprawy w pętle max 5x2,5mm². Przewód w oponie okrągłej o średnicy: ø8...12mm lub ø10...14mm.","6036XX0009.jpg","6036XX0009.ldt",3,null,1,76]
["6081","6081XX0009","EGERSUND PARK BOLLARD 105CM LED 1462LM 4000K DIM.","Egersund,Park","Bollard","Aluminium",null,null,null,"LED zintegrowane","AC","DIM.","7,4W","9,1W","1462lm","935lm",null,null,"65","IK08","Class II",4000,null,1.05,0.12,0.12,"CE",null,null,"> 102 000h",1,"Oprawa słupkowa.","Światło symetryczne ukierunkowane w dół.",null,"Luminaire with a contemporary design. For garden illumination and other private and public areas",null,null,null,"Odlew aluminiowy malowany proszkowo.",null,"Klosz- tworzywo sztuczne PMMA przeźroczyste.","Uszczelka silikonowa.",null,"105cm",null,"Oprawa ściemnialna fazowo TRAILING EDGE (TE) - LEADING EDGE (LE)","Moduł LED","Cree DK210704 V2 JB2835 3V 4K","TCI MICRO MD 10W 350mA 127040 Triac",0,null,null,80,"C","205ZX0010, 206GA0010, 206GA0S10, 6138ZX0009","Zaciski podłączeniowe: max 2x4mm², możliwość podłączenia oprawy w pętle max 2x4mm². Przewód w oponie okrągłej o średnicy: ø8...12mm lub ø10...14mm Pozostałe systemy podłączeniowe jako akcesoria, należy dokupić oddzielnie.","6081XX0009.png","6081XX0009.ldt",1,null,1,34]
["6082","6082XX0009","EGERSUND PARK BOLLARD 105CM LED 3363LM 3000K DALI2","Egersund,Park","Bollard","Aluminium",null,null,null,"LED zintegrowane","AC","DALI2","20,5W","23,9W","3363lm","2258lm",null,null,"65","IK08","Class I",3000,null,1.05,0.12,0.12,"CE",null,"DALI","> 102 000h",1,"Oprawa słupkowa.","Światło symetryczne ukierunkowane w dół.",null,"Luminaire with a contemporary design For lighting gardens and other private and public areas",null,null,null,"Odlew aluminiowy malowany proszkowo.",null,"Klosz- tworzywo sztuczne PMMA przeźroczyste.","Uszczelka silikonowa.",null,"105cm",null,"Sterowanie światłem w systemie: DALI outdoor pełny program. Zasilacz zaprogramowany na max prąd. Programowanie pozostałych parametrów po uzgodnieniu z Działem Handlowym firmy Norlys.","Moduł LED","Cree DK210704 V2 JB2835 3V 3K","Philips Xi FP 22W 0,3-1,0A SNLDAE 230V S175 sXt",100000,"DALI2 / NightDim (XI FP NLD)",null,80,"C","205ZX0010, 206GA0010, 206GA0S10, 6138ZX0009","Zaciski podłączeniowe: max 5x4mm², możliwość podłączenia oprawy w pętle max 5x2,5mm². Przewód w oponie okrągłej o średnicy: ø8...12mm lub ø10...14mm Pozostałe systemy podłączeniowe jako akcesoria, należy dokupić oddzielnie.","6082XX0009.png","6082XX0009.ldt",3,null,1,34]
["6083","6083XX0009","EGERSUND PARK BOLLARD 105CM LED 3566LM 4000K DALI2","Egersund,Park","Bollard","Aluminium",null,null,null,"LED zintegrowane","AC","DALI2","20,5W","23,9W","3566lm","2319lm",null,null,"65","IK08","Class I",4000,null,1.05,0.12,0.12,"CE",null,"DALI","> 102 000h",1,"Oprawa słupkowa.","Światło symetryczne ukierunkowane w dół.",null,"Luminaire with a contemporary design For lighting gardens and other private and public areas",null,null,null,"Odlew aluminiowy malowany proszkowo.",null,"Klosz- tworzywo sztuczne PMMA przeźroczyste.","Uszczelka silikonowa.",null,"105cm",null,"Sterowanie światłem w systemie: DALI outdoor pełny program. Zasilacz zaprogramowany na max prąd. Programowanie pozostałych parametrów po uzgodnieniu z Działem Handlowym firmy Norlys.","Moduł LED","Cree DK210704 V2 JB2835 3V 4K","Philips Xi FP 22W 0,3-1,0A SNLDAE 230V S175 sXt",100000,"DALI2 / NightDim (XI FP NLD)",null,80,"C","205ZX0010, 206GA0010, 206GA0S10, 6138ZX0009","Zaciski podłączeniowe: max 5x4mm², możliwość podłączenia oprawy w pętle max 5x2,5mm². Przewód w oponie okrągłej o średnicy: ø8...12mm lub ø10...14mm Pozostałe systemy podłączeniowe jako akcesoria, należy dokupić oddzielnie.","6083XX0009.png","6083XX0009.ldt",3,null,1,34]
["6090","6090XX0009","EGERSUND PARK BOLLARD 85CM LED 1370LM 3000K DIM.","Egersund,Park","Bollard","Aluminium",null,null,null,"LED zintegrowane","AC","DIM.","7,4W","9,1W","1370lm","907lm",null,null,"65","IK08","Class II",3000,null,0.85,0.12,0.12,"CE",null,null,"> 102 000h",1,"Oprawa słupkowa.","Światło symetryczne ukierunkowane w dół.",null,"Luminaire with a contemporary design. For garden illumination and other private and public areas",null,null,null,"Odlew aluminiowy malowany proszkowo.",null,"Klosz- tworzywo sztuczne PMMA przeźroczyste.","Uszczelka silikonowa.",null,"85cm",null,"Oprawa ściemnialna fazowo TRAILING EDGE (TE) - LEADING EDGE (LE)","Moduł LED","Cree DK210704 V2 JB2835 3V 3K","TCI MICRO MD 10W 350mA 127040 Triac",0,null,null,80,"C","205ZX0010, 206GA0010, 206GA0S10, 6138ZX0009","Zaciski podłączeniowe: max 2x4mm², możliwość podłączenia oprawy w pętle max 2x4mm². Przewód w oponie okrągłej o średnicy: ø8...12mm lub ø10...14mm Pozostałe systemy podłączeniowe jako akcesoria, należy dokupić oddzielnie.","6090XX0009.png","6090XX0009.ldt",1,null,1,34]
["6091","6091XX0009","EGERSUND PARK BOLLARD 85CM LED 1462LM 4000K DIM.","Egersund,Park","Bollard","Aluminium",null,null,null,"LED zintegrowane","AC","DIM.","7,4W","9,1W","1462lm","935lm",null,null,"65","IK08","Class II",4000,null,0.85,0.12,0.12,"CE",null,null,"> 102 000h",1,"Oprawa słupkowa.","Światło symetryczne ukierunkowane w dół.",null,"Luminaire with a contemporary design. For garden illumination and other private and public areas",null,null,null,"Odlew aluminiowy malowany proszkowo.",null,"Klosz- tworzywo sztuczne PMMA przeźroczyste.","Uszczelka silikonowa.",null,"85cm",null,"Oprawa ściemnialna fazowo TRAILING EDGE (TE) - LEADING EDGE (LE)","Moduł LED","Cree DK210704 V2 JB2835 3V 4K","TCI MICRO MD 10W 350mA 127040 Triac",0,null,null,80,"C","205ZX0010, 206GA0010, 206GA0S10, 6138ZX0009","Zaciski podłączeniowe: max 2x4mm², możliwość podłączenia oprawy w pętle max 2x4mm². Przewód w oponie okrągłej o średnicy: ø8...12mm lub ø10...14mm Pozostałe systemy podłączeniowe jako akcesoria, należy dokupić oddzielnie.","6091XX0009.png","6091XX0009.ldt",1,null,1,34]
["6092","6092XX0009","EGERSUND PARK BOLLARD 85CM LED 3363LM 3000K DALI2","Egersund,Park","Bollard","Aluminium",null,null,"PRO","LED zintegrowane","AC","DALI2","20,5W","23,9W","3363lm","2258lm",null,null,"65","IK08","Class I",3000,null,0.85,0.12,0.12,"CE",null,"DALI","> 102 000h",1,"Oprawa słupkowa.","Światło symetryczne ukierunkowane w dół.",null,"Luminaire with a contemporary design For lighting gardens and other private and public areas",null,null,null,"Odlew aluminiowy malowany proszkowo.",null,"Klosz- tworzywo sztuczne PMMA przeźroczyste.","Uszczelka silikonowa.",null,"85cm",null,"Sterowanie światłem w systemie: DALI outdoor pełny program. Zasilacz zaprogramowany na max prąd. Programowanie pozostałych parametrów po uzgodnieniu z Działem Handlowym firmy Norlys.","Moduł LED","Cree DK210704 V2 JB2835 3V 3K","Philips Xi FP 22W 0,3-1,0A SNLDAE 230V S175 sXt",100000,"DALI2 / NightDim (XI FP NLD)",null,80,"C","205ZX0010, 206GA0010, 206GA0S10","Zaciski podłączeniowe: max 5x4mm², możliwość podłączenia oprawy w pętle max 5x2,5mm². Przewód w oponie okrągłej o średnicy: ø8...12mm lub ø10...14mm","6092XX0009.png","6092XX0009.ldt",3,null,1,34]
["6093","6093XX0009","EGERSUND PARK BOLLARD 85CM LED 3566LM 4000K DALI2","Egersund,Park","Bollard","Aluminium",null,null,"PRO","LED zintegrowane","AC","DALI2","20,5W","23,9W","3566lm","2319lm",null,null,"65","IK08","Class I",4000,null,0.85,0.12,0.12,"CE",null,"DALI","> 102 000h",1,"Oprawa słupkowa.","Światło symetryczne ukierunkowane w dół.",null,"Luminaire with a contemporary design For lighting gardens and other private and public areas",null,null,null,"Odlew aluminiowy malowany proszkowo.",null,"Klosz- tworzywo sztuczne PMMA przeźroczyste.","Uszczelka silikonowa.",null,"85cm",null,"Sterowanie światłem w systemie: DALI outdoor pełny program. Zasilacz zaprogramowany na max prąd. Programowanie pozostałych parametrów po uzgodnieniu z Działem Handlowym firmy Norlys.","Moduł LED","Cree DK210704 V2 JB2835 3V 4K","Philips Xi FP 22W 0,3-1,0A SNLDAE 230V S175 sXt",100000,"DALI2 / NightDim (XI FP NLD)",null,80,"C","205ZX0010, 206GA0010, 206GA0S10","Zaciski podłączeniowe: max 5x4mm², możliwość podłączenia oprawy w pętle max 5x2,5mm². Przewód w oponie okrągłej o średnicy: ø8...12mm lub ø10...14mm.","6093XX0009.png","6093XX0009.ldt",3,null,1,34]
["6105","6105XX0311","EGERSUND PARK LIGHT LUMINAIRES POLE 250CM LED 1370LM 3000K DIM.","Egersund,Park","Post,Post complete","Aluminium",null,null,null,"LED zintegrowane","AC","DIM.","7,4W","9,1W","1370lm","907lm",null,null,"65",null,"Class II",3000,null,0,0,0,"CE",null,null,"> 72 000h",20,"Oprawa słupowa (lekka konstrukcja).","Światło symetryczne ukierunkowane w dół.",null,"Pole mounted luminaire ø120mm","Pole mounted luminaire fitting ø120mm, equipped with: - Lighting pole art. 6101xx0010 with revision door - Lighting fixture (head) art. 6116xx0009 - Hermetic connection box",null,null,"Odlew aluminiowy malowany proszkowo.",null,"Klosz- tworzywo sztuczne PMMA przeźroczyste.","Uszczelka silikonowa.",null,"250cm","Drzwiczki rewizyjne","Oprawa ściemnialna fazowo TRAILING EDGE (TE) - LEADING EDGE (LE)","Moduł LED","Cree DK210704 V2 JB2835 3V 3K","TCI MICRO MD 10W 350mA 127040 Triac",0,null,0.01,80,"C","6130ZX0009, 6132GA0010, 6135ZX0009","Puszka hermetyczna IP68: Zaciski podłączeniowe: max 2x4mm², możliwość podłączenia oprawy w pętle max 2x2,5mm². Przewód w oponie okrągłej o średnicy: ø8...12mm lub ø10...14mm. Oprawa oświetleniowa wyposażona w drzwiczki rewizyjne.","6105XX0311.jpg","6105XX0311.ldt",1,null,1,34]
["6106","6106XX0011","EGERSUND PARK POLE-TOP LED 1370LM 3000K DIM.","Egersund,Park","Post,Head","Aluminium",null,null,null,"LED zintegrowane","AC","DIM.","7,4W","9,1W","1370lm","907lm",null,null,"65","IK05","Class II",3000,"szerokie dół",0.12,0.12,0.52,"CE",null,null,"> 171 460h",2,"Oprawa słupowa (nasadzana).","Światło symetryczne ukierunkowane w dół.",null,"Pole mounted luminaire ø120mm","Pole mounted luminaire ø120mm, equipped with: - Hermetic electric box Other accessories must be ordered separately",null,null,"Odlew aluminiowy malowany proszkowo.",null,"Klosz- tworzywo sztuczne PMMA przeźroczyste.","Uszczelka silikonowa.","Dławnica nylon6.",null,"Oprawa nasadzana","Oprawa ściemnialna fazowo TRAILING EDGE (TE) - LEADING EDGE (LE)","Moduł LED","Cree DK210704 V2 JB2835 3V 3K","TCI MICRO MD 10W 350mA 127040 Triac",0,null,0.01,80,"C",null,"Przewód H05VV-F 2x1 o długości 2,7m zakończony puszką podłączeniową hermetyczną IP68 do podłączenia wewnątrz oprawy oświetleniowej. Zaciski podłączeniowe: max 2x4mm², możliwość podłączenia oprawy w pętle max 2x4mm². Przewód w oponie okrągłej o średnicy: ø8...12mm lub ø10...14mm","6106XX0011.png","6106XX0011.ldt",1,null,1,34]
["6108","6108XX0011","EGERSUND PARK POLE-TOP LED 1462LM 4000K DIM.","Egersund,Park","Post,Head","Aluminium",null,null,null,"LED zintegrowane","AC","DIM.","7,4W","9,1W","1462lm","962lm",null,null,"65",null,"Class II",4000,null,0,0,0,"CE",null,null,"> 72 000h",2,"Oprawa słupowa (nasadzana).","Światło symetryczne ukierunkowane w dół.",null,"Pole mounted luminaire ø120mm","Pole mounted luminaire ø120mm, equipped with: - Hermetic electric box",null,null,"Odlew aluminiowy malowany proszkowo.",null,"Klosz- tworzywo sztuczne PMMA przeźroczyste.","Uszczelka silikonowa.","Dławnica nylon6.",null,"Oprawa nasadzana","Oprawa ściemnialna fazowo TRAILING EDGE (TE) - LEADING EDGE (LE)","Moduł LED","Cree DK210704 V2 JB2835 3V 4K","TCI MICRO MD 10W 350mA 127040 Triac",0,null,0.01,80,"C",null,"Przewód H05RN-F 2x1 o długości 2,5m zakończony puszką podłączeniową hermetyczną IP68. Zaciski podłączeniowe: max 2x4mm², możliwość podłączenia oprawy w pętle max 2x2,5mm². Przewód w oponie okrągłej o średnicy: ø8...12mm lub ø10...14mm","6108XX0011.png","6108XX0011.ldt",1,null,1,34]
["610","610XX0011","BERLIN WALL E27","Berlin","Wall","Aluminium",null,null,null,"Wymienne","E27",null,"LED max 9W","LED max 9W",null,"468lm",null,null,"54","IK10","Class I",null,null,0.27,0.27,0.14000000000000001,"CE",null,null,null,12,"Oprawa ścienna.","Światło odkryte, częściowo przysłonięte od góry.",null,"Classic design plafon type luminaire.",null,null,"Oprawa na wymienne źródło światła typu: lampa LED, świetlówka TC-SE, tradycyjna żarówka (halogenowa) o trzonku E27. Źródło światła należy dokupić oddzielnie.","Odlew aluminiowy malowany proszkowo.",null,"Klosz- poliwęglan przeźroczysty, stabilizowany UV.","Uszczelka silikonowa.","Dławnica EPDM.",null,"przeźroczysty",null,"Lampa E27","LED A55..60",null,0,null,null,80,null,"46999021","Zaciski podłączeniowe: max 3x2,5mm², możliwość podłączenia oprawy w pętle max 3x1,5mm². Przewód w oponie okrągłej o średnicy ø7...10,5mm.","610XX0011.jpg","610XX0011.ldt",4,"E27",1,23]
["6111","6111XX0309","EGERSUND PARK PRO LIGHT LUMINAIRES POLE 250CM LED 3363LM 3000K DALI2","Egersund,Park","Post,Post complete","Aluminium",null,null,"PRO","LED zintegrowane","AC","DALI2","20,5W","23,7W","3363lm","2239lm",null,null,"65",null,"Class I",3000,"szerokie dół",0.12,0.12,2.5,"CE",null,"DALI","> 72 000h",20,"Oprawa słupowa (lekka konstrukcja).","Światło symetryczne ukierunkowane w dół.",null,"Pole mounted luminaire, mounted on a ø120mm base","Pole mounted luminaire, mounted on a ø120mm base, equipped with: - Pole art. 6100xx0010 - Top head art. 6114xx0009 - Hermetic connection box",null,null,"Odlew aluminiowy malowany proszkowo.",null,"Klosz- tworzywo sztuczne PMMA przeźroczyste.","Uszczelka silikonowa.",null,"250cm","Drzwiczki rewizyjne","Sterowanie światłem w systemie: DALI outdoor pełny program. Zasilacz zaprogramowany na max prąd. Programowanie pozostałych parametrów po uzgodnieniu z Działem Handlowym firmy Norlys.","Moduł LED","Cree DK210704 V2 JB2835 3V 3K","Philips Xi FP 22W 0,3-1,0A SNLDAE 230V S175 sXt",100000,"DALI2 / NightDim (XI FP NLD)",0.01,80,"C","6130ZX0009, 6132GA0009, 6133GA0009, 6135ZX0009","Puszka hermetyczna IP68: Zaciski podłączeniowe: max 5x2,5mm², możliwość podłączenia oprawy w pętle max 5x1,5mm². Przewód w oponie okrągłej o średnicy: ø8...17mm.","6111XX0309.png","6111XX0309.ldt",3,null,1,34]
["6112","6112XX0309","EGERSUND PARK PRO LIGHT LUMINAIRES POLE 250CM LED 3566LM 4000K DALI2","Egersund,Park","Post,Post complete","Aluminium",null,null,"PRO","LED zintegrowane","AC","DALI2","20,5W","23,9W","3566lm","2314lm",null,null,"65",null,"Class I",4000,"szerokie dół",0.12,0.12,2.5,"CE",null,"DALI","> 72 000h",20,"Oprawa słupowa (lekka konstrukcja).","Światło symetryczne ukierunkowane w dół.",null,"Pole mounted luminaire, mounted on a ø120mm base","Pole mounted luminaire, mounted on a ø120mm base, equipped with: - Pole art. 6100xx0010 - Top head art. 6116xx0009 - Hermetic connection box",null,null,"Odlew aluminiowy malowany proszkowo.",null,"Klosz- tworzywo sztuczne PMMA przeźroczyste.","Uszczelka silikonowa.",null,"250cm","Drzwiczki rewizyjne","Sterowanie światłem w systemie: DALI outdoor pełny program. Zasilacz zaprogramowany na max prąd. Programowanie pozostałych parametrów po uzgodnieniu z Działem Handlowym firmy Norlys.","Moduł LED","Cree DK210704 V2 JB2835 3V 4K","Philips Xi FP 22W 0,3-1,0A SNLDAE 230V S175 sXt",100000,"DALI2 / NightDim (XI FP NLD)",0.01,80,"C","6130ZX0009, 6132GA0009, 6133GA0009, 6135ZX0009","Puszka hermetyczna IP68: Zaciski podłączeniowe: max 5x2,5mm², możliwość podłączenia oprawy w pętle max 5x1,5mm². Przewód w oponie okrągłej o średnicy: ø8...17mm.","6112XX0309.png","6112XX0309.ldt",3,null,1,34]
["6113","6113XX0309","EGERSUND PARK PRO LIGHT LUMINAIRES POLE 250CM LED 3363LM 3000K DALI2","Egersund,Park","Post,Post complete","Aluminium",null,null,"PRO","LED zintegrowane","AC","DALI2","20,5W","23,7W","3363lm","2239lm",null,null,"65",null,"Class I",3000,"szerokie dół",0.12,0.12,2.5,"CE",null,"DALI","> 72 000h",20,"Oprawa słupowa (lekka konstrukcja).","Światło symetryczne ukierunkowane w dół.",null,"Pole mounted luminaire, mounted on a ø120mm base","Pole mounted luminaire, mounted on a ø120mm base, equipped with: - Pole art. 6101xx0010 - Top head art. 6114xx0009 - Hermetic connection box",null,null,"Odlew aluminiowy malowany proszkowo.",null,"Klosz- tworzywo sztuczne PMMA przeźroczyste.","Uszczelka silikonowa.",null,"250cm","Drzwiczki rewizyjne","Sterowanie światłem w systemie: DALI outdoor pełny program. Zasilacz zaprogramowany na max prąd. Programowanie pozostałych parametrów po uzgodnieniu z Działem Handlowym firmy Norlys.","Moduł LED","Cree DK210704 V2 JB2835 3V 3K","Philips Xi FP 22W 0,3-1,0A SNLDAE 230V S175 sXt",100000,"DALI2 / NightDim (XI FP NLD)",0.01,80,"C","6130ZX0009, 6132GA0009, 6133GA0009, 6135ZX0009","Puszka hermetyczna IP68: Zaciski podłączeniowe: max 5x2,5mm², możliwość podłączenia oprawy w pętle max 5x1,5mm². Przewód w oponie okrągłej o średnicy: ø8...17mm. Oprawa oświetleniowa wyposażona w drzwiczki rewizyjne.","6113XX0309.png","6113XX0309.ldt",3,null,1,34]
["6114","6114XX0009","EGERSUND PARK PRO POLE-TOP LED 3363LM 3000K DALI2","Egersund,Park","Post,Head","Aluminium",null,null,"PRO","LED zintegrowane","AC","DALI2","20,5W","23,7W","3363lm","2239lm",null,null,"65",null,"Class I",3000,"szerokie dół",0.12,0.12,0.66,"CE",null,"DALI","> 171 460hrs",29,"Oprawa słupowa (do montażu na słupie).","Światło symetryczne ukierunkowane w dół.",null,"Pole mounted luminaire ø120mm","Pole mounted lighting fitting ø120mm, equipped with: - lighting pole, art. 6101xx0011 equipped with an inspection door - hermetic electric box",null,null,"Odlew aluminiowy malowany proszkowo.",null,"Klosz- tworzywo sztuczne PMMA przeźroczyste.","Uszczelka silikonowa.",null,null,"Oprawa nasadzana","Sterowanie światłem w systemie: DALI outdoor pełny program. Zasilacz zaprogramowany na max prąd. Programowanie pozostałych parametrów po uzgodnieniu z Działem Handlowym firmy Norlys.","Moduł LED","Cree DK210704 V2 JB2835 3V 3K","Philips Xi FP 22W 0,3-1,0A SNLDAE 230V S175 sXt",100000,"DALI2 / NightDim (XI FP NLD)",0.01,80,"C","6130ZX0009, 6132GA0009, 6133GA0009, 6135ZX0009","Puszka hermetyczna IP68: Zaciski podłączeniowe: max 5x2,5mm², możliwość podłączenia oprawy w pętle max 5x1,5mm². Przewód w oponie okrągłej o średnicy: ø8...17mm. Oprawa oświetleniowa wyposażona w drzwiczki rewizyjne.","6114XX0009.png","6114XX0009.ldt",3,null,1,34]
["6115","6115XX0309","EGERSUND PARK PRO LIGHT LUMINAIRES POLE 250CM LED 3566LM 4000K DALI2","Egersund,Park","Post,Post complete","Aluminium",null,null,"PRO","LED zintegrowane","AC","DALI2","20,5W","23,9W","3566lm","2314lm",null,null,"65",null,"Class I",4000,"szerokie dół",0.12,0.12,2.5,"CE",null,"DALI","> 72 000h",20,"Oprawa słupowa (lekka konstrukcja).","Światło symetryczne ukierunkowane w dół.",null,"Pole mounted luminaire, mounted on a ø120mm base","Pole mounted luminaire, mounted on a ø120mm base, equipped with: - Pole art. 6101xx0010 - Top head art. 6116xx0009 - Hermetic connection box",null,null,"Odlew aluminiowy malowany proszkowo.",null,"Klosz- tworzywo sztuczne PMMA przeźroczyste.","Uszczelka silikonowa.",null,"250cm","Drzwiczki rewizyjne","Sterowanie światłem w systemie: DALI outdoor pełny program. Zasilacz zaprogramowany na max prąd. Programowanie pozostałych parametrów po uzgodnieniu z Działem Handlowym firmy Norlys.","Moduł LED","Cree DK210704 V2 JB2835 3V 4K","Philips Xi FP 22W 0,3-1,0A SNLDAE 230V S175 sXt",100000,"DALI2 / NightDim (XI FP NLD)",0.01,80,"C","6130ZX0009, 6132GA0009, 6133GA0009, 6135ZX0009","Puszka hermetyczna IP68: Zaciski podłączeniowe: max 5x2,5mm², możliwość podłączenia oprawy w pętle max 5x1,5mm². Przewód w oponie okrągłej o średnicy: ø8...17mm. Oprawa oświetleniowa wyposażona w drzwiczki rewizyjne.","6115XX0309.png","6115XX0309.ldt",3,null,1,34]
["6116","6116XX0009","EGERSUND PARK PRO POLE-TOP 250CM LED 3566LM 4000K DALI2","Egersund,Park","Post,Head","Aluminium",null,null,"PRO","LED zintegrowane","AC","DALI2","20,5W","23,9W","3566lm","2314lm",null,null,"65",null,"Class I",4000,"szerokie dół",0.12,0.12,0.66,"CE",null,"DALI","> 171 460hrs",29,"Oprawa słupowa (do montażu na słupie).","Światło symetryczne ukierunkowane w dół.",null,"Pole mounted luminaire ø120mm","Pole mounted lighting fitting ø120mm, equipped with: - lighting pole, art. 6101xx0011 equipped with a revision door - hermetic electric box",null,null,"Odlew aluminiowy malowany proszkowo.",null,"Klosz- tworzywo sztuczne PMMA przeźroczyste.","Uszczelka silikonowa.",null,"250cm","Drzwiczki rewizyjne","Sterowanie światłem w systemie: DALI outdoor pełny program. Zasilacz zaprogramowany na max prąd. Programowanie pozostałych parametrów po uzgodnieniu z Działem Handlowym firmy Norlys.","Moduł LED","Cree DK210704 V2 JB2835 3V 4K","Philips Xi FP 22W 0,3-1,0A SNLDAE 230V S175 sXt",100000,"DALI2 / NightDim (XI FP NLD)",0.01,80,"C","6130ZX0009, 6132GA0009, 6133GA0009, 6135ZX0009","Puszka hermetyczna IP68: Zaciski podłączeniowe: max 5x2,5mm², możliwość podłączenia oprawy w pętle max 5x1,5mm². Przewód w oponie okrągłej o średnicy: ø8...17mm. Oprawa oświetleniowa wyposażona w drzwiczki rewizyjne.","6116XX0009.png","6116XX0009.ldt",3,null,1,34]
["6118","6118XX0309","EGERSUND PARK BOLLARD 250CM LED 1170LM 4000K DIM.","Egersund,Park","Post,Post complete","Aluminium",null,null,null,"LED zintegrowane","AC","DIM.","10W","10W","1170lm","1064lm",null,null,"65",null,"Class I",4000,null,0,0,0,"CE",null,null,"> 50 000h",1,"Oprawa słupkowa.","Światło ukierunkowane w dół.",null,"Pole luminaire, mounted ø120mm.",null,null,null,"Odlew aluminiowy malowany proszkowo.",null,"Klosz- tworzywo sztuczne PMMA przeźroczyste.","Uszczelka silikonowa.","Dławnica nylon6.","250cm",null,"Oprawa ściemnialna fazowo TRAILING EDGE (TE) - LEADING EDGE (LE)","Moduł LED","Lumens DLM 90C 10W xxx 230V /A V0.1",null,0,"Ściemnianie fazowe Lumens LED AC",0.02,80,null,"6130ZX0009, 6132GA0009, 6133GA0009, 6135ZX0009","Puszka hermetyczna IP68: Zaciski podłączeniowe: max 4x4mm², możliwość podłączenia oprawy w pętle max 4x2,5mm². Przewód w oponie okrągłej o średnicy: ø8...12mm lub ø10...14mm.","6118XX0309.jpg","6118XX0309.ldt",1,null,1,45]
["611","611XX0010","BERLIN WALL E27","Berlin","Wall","Aluminium",null,null,null,"Wymienne","E27",null,"LED max 9W","LED max 9W",null,null,null,null,"54","IK10","Class I",null,null,0.27,0.27,0.14000000000000001,"CE",null,null,null,12,"Oprawa ścienna.","Światło rozproszone półsferyczne ukierunkowane w dół",null,"Classic design plafon type luminaire for normal use.",null,null,"Oprawa na wymienne źródło światła typu: lampa LED, świetlówka TC-SE, tradycyjna żarówka (halogenowa) o trzonku E27. Źródło światła należy dokupić oddzielnie.","Odlew aluminiowy malowany proszkowo.",null,"Klosz- poliwęglan mleczny, stabilizowany UV.","Uszczelka silikonowa.","Dławnica EPDM.",null,"mleczny",null,"Lampa E27","LED A55..60",null,0,null,null,80,null,"46999021","Zaciski podłączeniowe: max 3x2,5mm², możliwość podłączenia oprawy w pętle max 3x1,5mm². Przewód w oponie okrągłej o średnicy ø7...10,5mm.","611XX0010.jpg","611XX0010.ldt",4,"E27",1,76]
["6120","6120XX0010","BORG BOLLARD BOLLARD 35CM LED 2093LM 3000K DIM.","Borg","Bollard","Aluminium",null,null,null,"LED zintegrowane","AC","DIM.","13,7W","16,1W","2093lm","1358lm",null,null,"65","IK08","Class I",3000,"szerokie dół",0.2,0.2,0.35,"CE",null,null,"> 72 000h",1,"Oprawa słupkowa.","Światło obrotowo-symetryczne.",null,"Luminaire with contemporary design. For lighting gardens and other private and public areas",null,null,null,"Odlew aluminiowy malowany proszkowo.",null,"Klosz- tworzywo sztuczne PMMA satynowane.","Uszczelka silikonowa.",null,"35cm",null,"Oprawa ściemnialna fazowo TRAILING EDGE (TE) - LEADING EDGE (LE)","Moduł LED","Cree DK201002 V1 JK3030 6V 3K","TCI Mini MD 18W 350mA code 127030 Triac",0,null,0,80,"E","202GA0009, 203ZX0009","Zaciski podłączeniowe: max 3x2,5mm², możliwość podłączenia oprawy w pętle max 3x1,5mm². Przewód w oponie okrągłej o średnicy ø8...12,5mm.","6120XX0010.png","6120XX0010.ldt",1,null,1,17]
["6121","6121XX0010","BORG BOLLARD BOLLARD 35CM LED 2214LM 4000K DIM.","Borg","Bollard","Aluminium",null,null,null,"LED zintegrowane","AC","DIM.","13,7W","16W","2214lm","1396lm",null,null,"65","IK08","Class I",4000,"szerokie dół",0.2,0.2,0.35,"CE",null,null,"> 72 000h",1,"Oprawa słupkowa.","Światło obrotowo-symetryczne.",null,"Luminaire with contemporary design. For lighting gardens and other private and public areas",null,null,null,"Odlew aluminiowy malowany proszkowo.",null,"Klosz- tworzywo sztuczne PMMA satynowane.","Uszczelka silikonowa.",null,"35cm",null,"Oprawa ściemnialna fazowo TRAILING EDGE (TE) - LEADING EDGE (LE)","Moduł LED","Cree DK201002 V1 JK3030 6V 4K","TCI Mini MD 18W 350mA code 127030 Triac",0,null,0,80,"E","202GA0009, 203ZX0009","Zaciski podłączeniowe: max 3x4mm², możliwość podłączenia oprawy w pętle max 3x4mm². Przewód w oponie okrągłej o średnicy ø8...12,5mm.","6121XX0010.png","6121XX0010.ldt",1,null,1,17]
["6122","6122XX0009","BORG BOLLARD BOLLARD 35CM LED 2093LM 3000K DALI2","Borg","Bollard","Aluminium",null,null,null,"LED zintegrowane","AC","DALI2","13,7W","17,2W","2093lm","1358lm",null,null,"65","IK08","Class I",3000,"szerokie dół",0.2,0.2,0.35,"CE",null,"DALI","> 72 000h",1,"Oprawa słupkowa.","Światło obrotowo-symetryczne.",null,"Luminaire with contemporary design. For lighting gardens, other private areas and architectural concepts",null,null,null,"Odlew aluminiowy malowany proszkowo.",null,"Klosz- tworzywo sztuczne PMMA satynowane.","Uszczelka silikonowa.",null,"35cm",null,"Sterowanie światłem w systemie: DALI2","Moduł LED","Cree DK201002 V1 JK3030 6V 3K","TCI Mini JOLLY 20W code 151403 DALI",0,null,0,80,"E","202GA0009, 203ZX0009","Zaciski podłączeniowe: max 5x2,5mm², możliwość podłączenia oprawy w pętle max 5x1,5mm². Przewód w oponie okrągłej o średnicy do ø12,5mm.","6122XX0009.png","6122XX0009.ldt",3,null,1,17]
["6123","6123XX0009","BORG BOLLARD BOLLARD 35CM LED 2216LM 4000K DALI2","Borg","Bollard","Aluminium",null,null,null,"LED zintegrowane","AC","DALI2","13,7W","17,2W","2216lm","1396lm",null,null,"65","IK08","Class I",4000,"szerokie dół",0.2,0.2,0.35,"CE",null,"DALI","> 72 000h",1,"Oprawa słupkowa.","Światło obrotowo-symetryczne.",null,"Luminaire with a contemporary design. For garden lighting and other private areas and architectural concepts",null,null,null,"Odlew aluminiowy malowany proszkowo.",null,"Klosz- tworzywo sztuczne PMMA satynowane.","Uszczelka silikonowa.",null,"35cm",null,"Sterowanie światłem w systemie: DALI2","Moduł LED","Cree DK201002 V1 JK3030 6V 4K","TCI Mini JOLLY 20W code 151403 DALI",0,null,0,80,"E","202GA0009, 203ZX0009","Zaciski podłączeniowe: max 5x2,5mm², możliwość podłączenia oprawy w pętle max 5x1,5mm². Przewód w oponie okrągłej o średnicy do ø12,5mm.","6123XX0009.png","6123XX0009.ldt",3,null,1,17]
["6140","6140XX0009","HAMMERFEST POLE-TOP LED 4246LM 3000K ON/OFF","Hammerfest","Post,Head","Aluminium",null,null,null,"LED zintegrowane","AC","ON/OFF","24,2W","26,4W","4246lm","3321lm",null,null,"65","IK07","Class I",3000,null,0.55000000000000004,0.55000000000000004,0.76,"CE",null,null,"> 54 000",2,"Oprawa słupowa (nasadzana).","Światło ukierunkowane w dół.",null,"Mounted on a telescopic lighting pole with a cap diameter Ø60mm. Other accessories have to be ordered separately.",null,null,null,"Odlew aluminiowy malowany proszkowo.",null,"Klosz- tworzywo sztuczne PMMA satynowane.","Uszczelka silikonowa.",null,null,"satynowany","Oprawa nieściemnialna","Moduł LED","R0-000440 OSRAM S5 - GW.","Philips Xitanium 36Wm 0.3-1.05A 54V 230V",0,null,0.01,70,null,"3004XX0009, 3005XX0009, 7661ZX0009, 7663ZX0009, 7664ZX0009, 7665XX0009","Przewód H05RN-F 3G1 o długości 6m do podłączenia w odpowiednio dobranej puszce elektroinstalacyjnej.","6140XX0009.jpg","6140XX0009.ldt",4,null,1,45]
["6141","6141XX0010","HAMMERFEST POLE-TOP LED 4311LM 3000K ON/OFF","Hammerfest","Post,Head","Aluminium",null,null,null,"LED zintegrowane","AC","ON/OFF","28,9W","32,7W","4311lm","3227lm",null,null,"65","IK07","Class I",3000,null,0.55000000000000004,0.55000000000000004,0.76,"CE",null,null,"> 50000",2,"Oprawa słupowa (nasadzana).","Światło rozproszone półsferyczne ukierunkowane w dół",null,"A mounted luminaire designed to be mounted on a lighting pole with a Ø60mm shaft",null,null,null,"Odlew aluminiowy malowany proszkowo.",null,"Klosz- tworzywo sztuczne PMMA w kolorze mlecznym.","Uszczelka silikonowa.",null,null,"mleczny","Oprawa nieściemnialna","Moduł LED","Cree DK190707 V2 JK3030 3K","Philips Xi BP 40W 0.3-1.0A S 230V C123_sXt",100000,null,0.01,80,"E","3004XX0009, 3005XX0009, 7661ZX0009, 7663ZX0009, 7664ZX0009, 7665XX0009","Przewód H05RN-F 3G1 o długości 6m do podłączenia w odpowiednio dobranej puszce elektroinstalacyjnej.","6141XX0010.jpg","6141XX0010.ldt",4,null,1,76]
["6146","6146XX0009","HAMMERFEST POLE-TOP 3XLED VSM 3000K DALI2","Hammerfest","Post,Head","Aluminium",null,null,null,"LED zintegrowane","AC","DALI2","47W","53W",null,"6519lm",null,null,"65","IK07","Class I",3000,"szerokie dół",0.76,0.55000000000000004,0.55000000000000004,"CE",null,"DALI","> 100 000h",2,"Oprawa słupowa (nasadzana).","Soczewka firmy Ledil typu VSM (IESNA typ V).","VSM","Mounted luminaire designed to be mounted on a lighting pole with a mounting shaft Ø60mm",null,null,null,"Odlew aluminiowy malowany proszkowo.",null,"Klosz- tworzywo sztuczne PMMA przeźroczyste.","Uszczelka silikonowa.",null,"DALI2","przeźroczysty","Sterowanie światłem w systemie: DALI outdoor pełny program. Zasilacz zaprogramowany na max prąd. Programowanie pozostałych parametrów po uzgodnieniu z Działem Handlowym firmy Norlys.","3 Moduły LED","Philips Fortimo FastFlex LED 2x4 G4+ 3K","Philips Xi FP 75W 0,2-0,7A SNLDAE 230V C133 sXt kod. 929002101406",100000,"DALI2 / NightDim (XI FP NLD)",0.01,70,"D","3004XX0009, 3005XX0009, 7661ZX0009, 7663ZX0009, 7664ZX0009, 7665XX0009","Przewód H05RN-F 5G1 o długości 6m do podłączenia w słupie, w odpowiednio dobranej puszce elektroinstalacyjnej.","6146XX0009.jpg","6146XX0009.ldt",3,null,1,47]
["6148","6148XX0009","HAMMERFEST POLE-TOP 3XLED VSM 4000K DALI2","Hammerfest","Post,Head","Aluminium",null,null,null,"LED zintegrowane","AC","DALI2","47W","53W",null,"6802lm",null,null,"65","IK07","Class I",4000,"szerokie dół",0.76,0.55000000000000004,0.55000000000000004,"CE",null,"DALI","> 100 000h",2,"Oprawa słupowa (nasadzana).","Soczewka firmy Ledil typu VSM (IESNA typ V).","VSM","Mounted luminaire designed to be mounted on a lighting pole with a mounting shaft Ø60mm",null,null,null,"Odlew aluminiowy malowany proszkowo.",null,"Klosz- tworzywo sztuczne PMMA przeźroczyste.","Uszczelka silikonowa.",null,"DALI2","przeźroczysty","Sterowanie światłem w systemie: DALI outdoor pełny program. Zasilacz zaprogramowany na max prąd. Programowanie pozostałych parametrów po uzgodnieniu z Działem Handlowym firmy Norlys.","3 Moduły LED","Philips Fortimo FastFlex LED 2x4 G4+ 4K","Philips Xi FP 75W 0,2-0,7A SNLDAE 230V C133 sXt kod. 929002101406",100000,"DALI2 / NightDim (4DIM)",0.01,70,"D","3004XX0009, 3005XX0009, 7661ZX0009, 7663ZX0009, 7664ZX0009, 7665XX0009","Przewód H05RN-F 5G1 o długości 6m do podłączenia w słupie, w odpowiednio dobranej puszce elektroinstalacyjnej.","6148XX0009.jpg","6148XX0009.ldt",3,null,1,47]
["6150","6150XX0009","BORG POLE-TOP LED 4180LM 3000K ON/OFF","Borg","Post,Head","Aluminium",null,null,null,"LED zintegrowane","AC","ON/OFF","27,2W","32W","4180lm","3735lm",null,null,"65","IK08","Class I",3000,"szerokie dół",0.51,0.51,0.15,"CE",null,null,"> 72 000h",2,"Oprawa słupowa (nasadzana).","Światło ukierunkowane w dół.",null,"Mounted on a telescopic lighting pole with a cap diameter Ø60mm. Other accessories have to be ordered separately.",null,null,null,"Odlew aluminiowy malowany proszkowo.",null,"Klosz- tworzywo sztuczne PMMA satynowane.","Uszczelka silikonowa.",null,"on/off","satynowany","Oprawa nieściemnialna","Moduł LED","Cree DK190804 V2 JK3030 3V 3K","Philips Xi BP 40W 0.3-1.0A S 230V C123_sXt",100000,null,0,80,"D","3004XX0009, 3005XX0009, 7661ZX0009, 7663ZX0009, 7664ZX0009, 7665XX0009","Przewód H05RN-F 3G1 o długości 6m do podłączenia w odpowiednio dobranej puszce elektroinstalacyjnej.","6150XX0009.jpg","6150XX0009.ldt",4,null,1,45]
["6151","6151XX0009","BORG POLE-TOP LED 4180LM 3000K ON/OFF","Borg","Post,Head","Aluminium",null,null,null,"LED zintegrowane","AC","ON/OFF","27,2W","32W","4180lm","2996lm",null,null,"65","IK08","Class I",3000,"szerokie dół",0,0,0,"CE",null,null,"> 72 000h",2,"Oprawa słupowa (nasadzana).","Światło ukierunkowane w dół.",null,"Modern design luminaire mounted on a telescopic lighting pole with a cap diameter Ø60mm. Other accessories have to be ordered separately.",null,null,null,"Odlew aluminiowy malowany proszkowo.",null,"Klosz- tworzywo sztuczne PMMA w kolorze mlecznym.","Uszczelka silikonowa.",null,"on/off","mleczny","Oprawa nieściemnialna","Moduł LED","Cree DK190804 V2 JK3030 3V 3K","Philips Xi BP 40W 0.3-1.0A S 230V C123_sXt",100000,null,0,80,"D","3004XX0009, 3005XX0009, 7661ZX0009, 7663ZX0009, 7664ZX0009, 7665XX0009","Przewód H05RN-F 3G1 o długości 6m do podłączenia w odpowiednio dobranej puszce elektroinstalacyjnej.","6151XX0009.jpg","6151XX0009.ldt",4,null,1,45]
["6153","6153XX0010","BORG PRO POLE-TOP LED 7218LM VSM 3000K DALI2","Borg","Post,Head","Aluminium",null,null,"PRO","LED zintegrowane","AC","DALI2","47,7W","52,6W","7218lm","7000lm",null,null,"65","IK08","Class I",3000,"szerokie dół",0.15,0.51,0.51,"CE",null,"DALI","> 72 000h",2,"Oprawa słupowa (nasadzana).","Soczewka firmy Ledil typu VSM (IESNA typ V).","VSM","Luminaire designed to be mounted on a lighting pole with a mounting shaft Ø60mm",null,null,null,"Odlew aluminiowy malowany proszkowo.",null,"Klosz- tworzywo sztuczne PMMA przeźroczyste.","Uszczelka silikonowa.",null,null,"przeźroczysty","Sterowanie światłem w systemie: DALI outdoor pełny program. Zasilacz zaprogramowany na max prąd. Programowanie pozostałych parametrów po uzgodnieniu z Działem Handlowym firmy Norlys.","Moduł LED","Philips Fortimo FastFlex LED 2x4 G5 3K","Philips Xi FP 75W 0,2-0,7A SNLDAE 230V C133 sXt kod. 929002101406",100000,"DALI2 / NightDim (4DIM)",0,80,"D","3004XX0009, 3005XX0009, 7661ZX0009, 7663ZX0009, 7664ZX0009, 7665XX0009","Przewód H05RN-F 6G1 o długości 6m do podłączenia w odpowiednio dobranej puszce elektroinstalacyjnej.","6153XX0010.png","6153XX0010.ldt",3,null,1,47]
["6154","6154XX0010","BORG PRO POLE-TOP 3XLED 7218LM VSM 3000K D4I","Borg","Post,Head","Aluminium",null,null,"PRO","LED zintegrowane","AC","D4i","47,7W","52,6W","7218lm","6730lm",null,null,"65","IK08","Class I",3000,"szerokie dół",0,0,0,"CE",null,null,"> 72 000h",2,"Oprawa słupowa (nasadzana).","Soczewka firmy Ledil typu VSM (IESNA typ V).","VSM","Mounted luminaire designed to be mounted on a lighting pole with mounting shaft Ø60mm",null,null,null,"Odlew aluminiowy malowany proszkowo.",null,"Klosz- tworzywo sztuczne PMMA przeźroczyste.","Uszczelka silikonowa.",null,null,"przeźroczysty","Sterowanie światłem w systemie D4i. Zasilacz zaprogramowany na max dopuszczalny prąd. Programowanie pozostałych parametrów po uzgodnieniu z Działem Handlowym firmy Norlys.","3 Moduły LED","Philips Fortimo FastFlex LED 2x4 G5 3K","Philips Xi SR 75W 0.2-0.7A SNEMP 230V C150 sXt 12NC:929002808406",0,"D4i",0,80,"D","3005XX0009, 7661ZX0009, 7663ZX0009, 7664ZX0009, 7665XX0009, SENSOR POD ZłĄCZE ZHAGA BOOK 18","Przewód H05RN-F 6G1 o długości 6m do podłączenia w odpowiednio dobranej puszce elektroinstalacyjnej.","6154XX0010.png","6154XX0010.ldt",3,null,1,47]
["6155","6155XX0009","BORG POLE-TOP LED 7426LM VSM 4000K DALI2","Borg","Post,Head","Aluminium",null,null,null,"LED zintegrowane","AC","DALI2","47,4W","53W","7426lm","7200lm",null,null,"65","IK08","Class I",4000,"szerokie dół",0,0,0,"CE",null,"DALI","> 100 000h",2,"Oprawa słupowa (nasadzana).","Soczewka firmy Ledil typu VSM (IESNA typ V).","VSM","A mounted luminaire designed to be mounted on a lighting pole with a Ø60mm mounting shaft",null,null,null,"Odlew aluminiowy malowany proszkowo.",null,"Klosz- tworzywo sztuczne PMMA przeźroczyste.","Uszczelka silikonowa.",null,null,"przeźroczysty","Sterowanie światłem w systemie: DALI outdoor pełny program. Zasilacz zaprogramowany na max prąd. Programowanie pozostałych parametrów po uzgodnieniu z Działem Handlowym firmy Norlys.","Moduł LED","Philips Fortimo FastFlex LED 2x4 G4+ 4K","Philips Xi FP 75W 0,2-0,7A SNLDAE 230V C133 sXt kod. 929002101406",100000,"DALI2 / NightDim (4DIM)",0,80,"D","3004XX0009, 3005XX0009, 7661ZX0009, 7663ZX0009, 7664ZX0009, 7665XX0009","Przewód H05RN-F 6G1 o długości 6m do podłączenia w odpowiednio dobranej puszce elektroinstalacyjnej.","6155XX0009.png","6155XX0009.ldt",3,null,1,47]
["6156","6156XX0009","BORG POLE-TOP LED 7426LM VSM 4000K D4I","Borg","Post,Head","Aluminium",null,null,null,"LED zintegrowane","AC","D4i","47,4W","53W","7426lm","7200lm",null,null,"65","IK08","Class I",4000,"szerokie dół",0.51,0.51,0.15,"CE",null,null,"> 72 000h",2,"Oprawa słupowa (nasadzana).","Soczewka firmy Ledil typu VSM (IESNA typ V).","VSM","Mounted luminaire designed to be mounted on a lighting pole with a mounting shaft Ø60mm",null,null,null,"Odlew aluminiowy malowany proszkowo.",null,"Klosz- tworzywo sztuczne PMMA przeźroczyste.","Uszczelka silikonowa.",null,null,"przeźroczysty","Sterowanie światłem w systemie D4i. Zasilacz zaprogramowany na max dopuszczalny prąd. Programowanie pozostałych parametrów po uzgodnieniu z Działem Handlowym firmy Norlys.","Moduł LED","Philips Fortimo FastFlex LED 2x4 G4+ 4K","Philips Xi SR 75W 0.2-0.7A SNEMP 230V C150 sXt 12NC:929002808406",100000,"D4i",0,80,"D","3004XX0009, 3005XX0009, 7661ZX0009, 7663ZX0009, 7664ZX0009, 7665XX0009","Przewód H05RN-F 6G1 o długości 6m do podłączenia w odpowiednio dobranej puszce elektroinstalacyjnej.","6156XX0009.png","6156XX0009.ldt",3,null,1,47]
["615","615XX0012","BERLIN WALL LED E27 DIM.","Berlin","Wall","Aluminium",null,null,null,"Wymienne","E27",null,"LED max 9W","8,3W",null,"240lm",null,null,"54","IK10","Class I",null,null,0.27,0.27,0.14000000000000001,"CE",null,null,"25000",12,"Oprawa ścienna.","Światło rozproszone półsferyczne ukierunkowane w dół",null,"Plafond type luminaire with modern design.",null,null,"Oprawa na wymienne źródło światła typu: lampa LED, Źródło światła dołączone do oprawy.","Odlew aluminiowy malowany proszkowo.",null,"Klosz- poliwęglan mleczny, stabilizowany UV.","Uszczelka silikonowa.","Dławnica EPDM.",null,"mleczny","Oprawa ściemnialna fazowo TRAILING EDGE (TE) - LEADING EDGE (LE)","Lampa LED E27","Philips Master LEDbulb DT 8-60W E27 A60 CL 806lm/827",null,0,"Ściemnianie fazowe LED GU10 E27",null,80,"F",null,"Zaciski podłączeniowe: max 3x2,5mm², możliwość podłączenia oprawy w pętle max 3x1,5mm². Przewód w oponie okrągłej o średnicy ø7...10,5mm.","615XX0012.jpg","615XX0012.ldt",1,"E27",1,76]
["6161","6161XX0009","MOSS CEILING/WALL LED 439LM 36D 3000K DIM.","Moss","Spot,Wall","Aluminium",null,null,null,"LED zintegrowane","AC","DIM.","4W","4W","439lm","389lm",null,null,"65",null,"Class I",3000,null,0.08,0.08,0.13,"CE",null,null,"> 50 000h",7,"Oprawa sufitowo-ścienna.","Światło symetryczne o kącie 36D","36D","For lighting gardens, private areas, and other architectural concepts. The light direction can also be adjusted vertically",null,null,null,"Odlew aluminiowy malowany proszkowo.",null,"Klosz- szkło bezpieczne, przeźroczyste.",null,null,"Triac",null,"Oprawa ściemnialna fazowo TRAILING EDGE (TE) - LEADING EDGE (LE)","Moduł LED","Lumens EDC 38C 4W xxx 230V A101 3K",null,0,"Ściemnianie fazowe Lumens LED AC",null,80,"E",null,"Elektryczne złącze zaciskowe 316IR 3M ™ Scotchlok ™ do łączenia dwóch lub trzech przewodów o przekroju 0,5 - 1,5mm2 bez zdejmowania izolacji z przewodów.","6161XX0009.jpg","6161XX0009.ldt",1,null,4,68]
["6163","6163XX0009","MOSS CEILING/WALL LED 840LM 36D 3000K DIM.","Moss","Spot,Wall","Aluminium",null,null,null,"LED zintegrowane","AC","DIM.","8W","8W","840lm","686lm",null,null,"65",null,"Class I",3000,null,0,0,0,"CE",null,null,"> 50 000h",7,"Oprawa sufitowo-ścienna.","Światło symetryczne o kącie 36D","36D","For lighting gardens, private areas, and other architectural concepts, The light direction can also be adjusted vertically",null,null,null,"Odlew aluminiowy malowany proszkowo.",null,"Klosz- szkło bezpieczne, przeźroczyste.",null,null,"Triac",null,"Oprawa ściemnialna fazowo TRAILING EDGE (TE) - LEADING EDGE (LE)","Moduł LED","Lumens EDC 38C 8W xxx 230V A101 3K",null,0,"Ściemnianie fazowe Lumens LED AC",null,80,"E",null,"Elektryczne złącze zaciskowe 316IR 3M ™ Scotchlok ™ do łączenia dwóch lub trzech przewodów o przekroju 0,5 - 1,5mm2 bez zdejmowania izolacji z przewodów.","6163XX0009.jpg","6163XX0009.ldt",1,null,4,68]
["6164","6164XX0009","MOSS CEILING/WALL LED 891LM 36D 4000K DIM.","Moss","Spot,Wall","Aluminium",null,null,null,"LED zintegrowane","AC","DIM.","8W","8W","891lm","749lm",null,null,"65",null,"Class I",4000,null,0.08,0.08,0.13,"CE",null,null,"> 50 000h",7,"Oprawa sufitowo-ścienna.","Światło symetryczne o kącie 36D","36D","For lighting gardens, private areas, and other architectural concepts, The light direction can also be adjusted vertically",null,null,null,"Odlew aluminiowy malowany proszkowo.",null,"Klosz- szkło bezpieczne, przeźroczyste.",null,null,"Triac",null,"Oprawa ściemnialna fazowo TRAILING EDGE (TE) - LEADING EDGE (LE)","Moduł LED","Lumens EDC 38C 8W xxx 230V A101 4K",null,0,"Ściemnianie fazowe Lumens LED AC",null,80,"E",null,"Elektryczne złącze zaciskowe 316IR 3M ™ Scotchlok ™ do łączenia dwóch lub trzech przewodów o przekroju 0,5 - 1,5mm2 bez zdejmowania izolacji z przewodów.","6164XX0009.jpg","6164XX0009.ldt",1,null,4,68]
["6165","6165XX0009","MOSS FLOODLIGHT-EARTHSPIKE LED 439LM 36D 3000K DIM.","Moss","Ground","Aluminium",null,null,null,"LED zintegrowane","AC","DIM.","4W","4W","439lm","389lm",null,null,"65",null,"Class I",3000,null,0,0,0,"CE",null,null,"> 50 000h",17,"Oprawa typu reflektor, przenośna gruntowa.","Światło symetryczne o kącie 36D","36D","For lighting gardens, private areas, and other architectural concepts, The light direction can also be adjusted vertically",null,null,null,"Odlew aluminiowy malowany proszkowo.",null,"Klosz- szkło bezpieczne, przeźroczyste.",null,null,"Triac",null,"Oprawa ściemnialna fazowo TRAILING EDGE (TE) - LEADING EDGE (LE)","Moduł LED","Lumens EDC 38C 4W xxx 230V A101 3K",null,0,"Ściemnianie fazowe Lumens LED AC",null,80,"E","145ZX0009, 146ZX0009","Oprawa wyposażona w przewód typu H05RN-F 3G1 o długości 3 m. Do podłączenia w odpowiednio dobranej puszce elektroinstalacyjnej.","6165XX0009.jpg","6165XX0009.ldt",1,null,4,68]
["6166","6166XX0010","MOSS FLOODLIGHT-EARTHSPIKE LED 466LM 36D 4000K DIM.","Moss","Ground","Aluminium",null,null,null,"LED zintegrowane","AC","DIM.","4W","4W","466lm","414lm",null,null,"65",null,"Class I",4000,null,0,0,0,"CE",null,null,">50000",17,"Oprawa typu reflektor, przenośna gruntowa.","Światło symetryczne o kącie 36D","36D","For illuminating gardens, private areas and other architectural concepts. Possibility to adjust the direction of light also in the vertical plane.",null,null,null,"Odlew aluminiowy malowany proszkowo.",null,"Klosz- szkło bezpieczne, przeźroczyste.",null,null,"Triac",null,"Oprawa ściemnialna fazowo TRAILING EDGE (TE) - LEADING EDGE (LE)","Moduł LED","Lumens EDC 38C 4W xxx 230V A101 4K",null,0,"Ściemnianie fazowe Lumens LED AC",null,80,"E","145ZX0009, 146ZX0009","Oprawa wyposażona w przewód typu H05RN-F 3G1 o długości 3 m. Do podłączenia w odpowiednio dobranej puszce elektroinstalacyjnej.","6166XX0010.jpg","6166XX0010.ldt",1,null,4,68]
["6167.01","6167.01XX0009","MOSS FLOODLIGHT-EARTHSPIKE LED 840LM 36º 3000K DIM.","Moss","Ground","Aluminium",null,null,null,"LED zintegrowane","AC","DIM.","8W","8W","840lm","686lm",null,null,"65",null,"Class I",3000,null,null,null,null,"CE",null,null,"> 50 000h",17,"Oprawa typu reflektor, przenośna gruntowa.","Światło symetryczne o kącie 36 stopni.","36º",null,null,null,null,"Odlew aluminiowy malowany proszkowo.",null,"Klosz- szkło bezpieczne, przeźroczyste.",null,null,"Triac",null,"Oprawa ściemnialna fazowo TRAILING EDGE (TE) - LEADING EDGE (LE)","Moduł LED","Lumens EDC 38C 8W xxx 230V A101 3K",null,null,"Ściemnianie fazowe Lumens LED AC",null,80,"F","145ZX0009, 146ZX0009","Oprawa wyposażona w przewód typu H05RN-F 3G1 o długości 10 m. Do podłączenia w odpowiednio dobranej puszce elektroinstalacyjnej.","6167.01XX0009.jpg","6167.01XX0009.ldt",1,null,4,35]
["6167","6167XX0009","MOSS FLOODLIGHT-EARTHSPIKE LED 840LM 36D 3000K DIM.","Moss","Ground","Aluminium",null,null,null,"LED zintegrowane","AC","DIM.","8W","8W","840lm","686lm",null,null,"65",null,"Class I",3000,null,0,0,0,"CE",null,null,"> 50 000h",17,"Oprawa typu reflektor, przenośna gruntowa.","Światło symetryczne o kącie 36D","36D","For lighting gardens, private areas, and other architectural concepts, The light direction can also be adjusted vertically",null,null,null,"Odlew aluminiowy malowany proszkowo.",null,"Klosz- szkło bezpieczne, przeźroczyste.",null,null,"Triac",null,"Oprawa ściemnialna fazowo TRAILING EDGE (TE) - LEADING EDGE (LE)","Moduł LED","Lumens EDC 38C 8W xxx 230V A101 3K",null,0,"Ściemnianie fazowe Lumens LED AC",null,80,"E","145ZX0009, 146ZX0009","Oprawa wyposażona w przewód typu H05RN-F 3G1 o długości 3 m. Do podłączenia w odpowiednio dobranej puszce elektroinstalacyjnej.","6167XX0009.jpg","6167XX0009.ldt",1,null,4,68]
["6168","6168XX0009","MOSS FLOODLIGHT-EARTHSPIKE LED 891LM 36D 4000K DIM.","Moss","Ground","Aluminium",null,null,null,"LED zintegrowane","AC","DIM.","8W","8W","891lm","749lm",null,null,"65",null,"Class I",4000,null,0,0,0,"CE",null,null,">50000",17,"Oprawa typu reflektor, przenośna gruntowa.","Światło symetryczne o kącie 36D","36D","For lighting gardens, private areas, and other concepts architectural. The light direction can also be adjusted vertically",null,null,null,"Odlew aluminiowy malowany proszkowo.",null,"Klosz- szkło bezpieczne, przeźroczyste.",null,null,"Triac",null,"Oprawa ściemnialna fazowo TRAILING EDGE (TE) - LEADING EDGE (LE)","Moduł LED","Lumens EDC 38C 8W xxx 230V A101 4K",null,0,"Ściemnianie fazowe Lumens LED AC",null,80,"E","145ZX0009, 146ZX0009","Oprawa wyposażona w przewód typu H05RN-F 3G1 o długości 3 m. Do podłączenia w odpowiednio dobranej puszce elektroinstalacyjnej.","6168XX0009.jpg","6168XX0009.ldt",1,null,4,68]
["6170","6170XX0010","BORG BOLLARD BOLLARD 55CM LED 2093LM 3000K DIM.","Borg","Bollard","Aluminium",null,null,null,"LED zintegrowane","AC","DIM.","13,7W","16W","2093lm","1358lm",null,null,"65","IK08","Class I",3000,"szerokie dół",0.2,0.2,0.55000000000000004,"CE",null,null,"> 72 000h",1,"Oprawa słupkowa.","Światło obrotowo-symetryczne.",null,"Luminaire with contemporary design. For lighting gardens and other private and public areas",null,null,null,"Odlew aluminiowy malowany proszkowo.",null,"Klosz- tworzywo sztuczne PMMA satynowane.","Uszczelka silikonowa.",null,"55cm",null,"Oprawa ściemnialna fazowo TRAILING EDGE (TE) - LEADING EDGE (LE)","Moduł LED","Cree DK201002 V1 JK3030 6V 3K","TCI Mini MD 18W 350mA code 127030 Triac",0,null,0,80,"E","202GA0009, 203ZX0009","Zaciski podłączeniowe: max 3x4mm², możliwość podłączenia oprawy w pętle max 3x4mm². Przewód w oponie okrągłej o średnicy ø8...12,5mm.","6170XX0010.jpg","6170XX0010.ldt",1,null,1,17]
["6171","6171XX0010","BORG BOLLARD BOLLARD 55CM LED 2214LM 4000K DIM.","Borg","Bollard","Aluminium",null,null,null,"LED zintegrowane","AC","DIM.","13,7W","16W","2214lm","1396lm",null,null,"65","IK08","Class I",4000,"szerokie dół",0.2,0.2,0.55000000000000004,"CE",null,null,"> 72 000h",1,"Oprawa słupkowa.","Światło obrotowo-symetryczne.",null,"Luminaire with contemporary design. For lighting gardens and other private and public areas",null,null,null,"Odlew aluminiowy malowany proszkowo.",null,"Klosz- tworzywo sztuczne PMMA satynowane.","Uszczelka silikonowa.",null,"55cm",null,"Oprawa ściemnialna fazowo TRAILING EDGE (TE) - LEADING EDGE (LE)","Moduł LED","Cree DK201002 V1 JK3030 6V 4K","TCI Mini MD 18W 350mA code 127030 Triac",0,null,0,80,"E","202GA0009, 203ZX0009","Zaciski podłączeniowe: max 3x4mm², możliwość podłączenia oprawy w pętle max 3x4mm². Przewód w oponie okrągłej o średnicy ø8...12,5mm.","6171XX0010.jpg","6171XX0010.ldt",1,null,1,17]
["6172","6172XX0009","BORG BOLLARD BOLLARD 55CM LED 2093LM 3000K DALI2","Borg","Bollard","Aluminium",null,null,null,"LED zintegrowane","AC","DALI2","13,7W","17,6W","2093lm","1358lm",null,null,"65","IK08","Class I",3000,"szerokie dół",0.2,0.2,0.55000000000000004,"CE",null,"DALI","> 72 000h",1,"Oprawa słupkowa.","Światło obrotowo-symetryczne.",null,"Luminaire with a contemporary design. For lighting gardens and other private and public areas",null,null,null,"Odlew aluminiowy malowany proszkowo.",null,"Klosz- tworzywo sztuczne PMMA satynowane.","Uszczelka silikonowa.",null,"55cm",null,"Sterowanie światłem w systemie: DALI outdoor pełny program. Zasilacz zaprogramowany na max prąd. Programowanie pozostałych parametrów po uzgodnieniu z Działem Handlowym firmy Norlys.","Moduł LED","Cree DK201002 V1 JK3030 6V 3K","Philips Xi FP 22W 0,2-0,7A SNLDAE 230V S175 sXt 929002172306",100000,"DALI2 / NightDim (XI FP NLD)",0,80,"E","202GA0009, 203ZX0009","Zaciski podłączeniowe: max 5x2,5mm², możliwość podłączenia oprawy w pętle max 5x2,5mm². Przewód w oponie okrągłej o średnicy ø7...13,5mm.","6172XX0009.jpg","6172XX0009.ldt",3,null,1,17]
["6173","6173XX0009","BORG BOLLARD BOLLARD 55CM LED 2216LM 4000K DALI2","Borg","Bollard","Aluminium",null,null,null,"LED zintegrowane","AC","DALI2","13,7W","17,6W","2216lm","1396lm",null,null,"65","IK08","Class I",4000,"szerokie dół",0.2,0.2,0.55000000000000004,"CE",null,"DALI","> 72 000h",1,"Oprawa słupkowa.","Światło obrotowo-symetryczne.",null,"Luminaire with a contemporary design. For lighting gardens and other private and public areas",null,null,null,"Odlew aluminiowy malowany proszkowo.",null,"Klosz- tworzywo sztuczne PMMA satynowane.","Uszczelka silikonowa.",null,"55cm",null,"Sterowanie światłem w systemie: DALI outdoor pełny program. Zasilacz zaprogramowany na max prąd. Programowanie pozostałych parametrów po uzgodnieniu z Działem Handlowym firmy Norlys.","Moduł LED","Cree DK201002 V1 JK3030 6V 4K","Philips Xi FP 22W 0,2-0,7A SNLDAE 230V S175 sXt 929002172306",100000,"DALI2 / NightDim (XI FP NLD)",0,80,"E","202GA0009, 203ZX0009","Zaciski podłączeniowe: max 5x2,5mm², możliwość podłączenia oprawy w pętle max 5x2,5mm². Przewód w oponie okrągłej o średnicy ø7...13,5mm.","6173XX0009.jpg","6173XX0009.ldt",3,null,1,17]
["617","617XX0013","BERLIN WALL LED 880LM 3000K DIM.","Berlin","Wall","Aluminium",null,null,null,"LED zintegrowane","AC","DIM.","8W","8W","880lm","185lm",null,null,"54","IK10","Class I",3000,null,0.27,0.27,0.14000000000000001,"CE",null,null,"50 000h",12,"Oprawa ścienna.","Światło rozproszone półsferyczne ukierunkowane w dół",null,"A ceiling-type luminaire with a contemporary design for general use",null,null,null,"Odlew aluminiowy malowany proszkowo.",null,"Klosz- poliwęglan mleczny, stabilizowany UV.","Uszczelka silikonowa.","Dławnica EPDM.",null,"mleczny","Oprawa ściemnialna fazowo TRAILING EDGE (TE) - LEADING EDGE (LE)","Moduł LED","Lumens EDC 38C 8W xxx 230V A101 3K",null,0,"Ściemnianie fazowe Lumens LED AC",null,80,"E",null,"Zaciski podłączeniowe: max 3x2,5mm², możliwość podłączenia oprawy w pętle max 3x1,5mm². Przewód w oponie okrągłej o średnicy ø7...10,5mm.","617XX0013.jpg","617XX0013.ldt",1,null,1,76]
["6180","6180XX0010","BORG BOLLARD BOLLARD 85CM LED 2093LM 3000K DIM.","Borg","Bollard","Aluminium",null,null,null,"LED zintegrowane","AC","DIM.","13,7W","16W","2093lm","1358lm",null,null,"65","IK08","Class I",3000,"szerokie dół",0.2,0.2,0.85,"CE",null,null,"> 72 000h",1,"Oprawa słupkowa.","Światło obrotowo-symetryczne.",null,"Luminaire with contemporary design. For lighting gardens and other private and public areas",null,null,null,"Odlew aluminiowy malowany proszkowo.",null,"Klosz- tworzywo sztuczne PMMA satynowane.","Uszczelka silikonowa.",null,"85cm",null,"Oprawa ściemnialna fazowo TRAILING EDGE (TE) - LEADING EDGE (LE)","Moduł LED","Cree DK201002 V1 JK3030 6V 3K","TCI Mini MD 18W 350mA code 127030 Triac",0,null,0,80,"E","202GA0009, 203ZX0009","Zaciski podłączeniowe: max 3x4mm², możliwość podłączenia oprawy w pętle max 3x4mm². Przewód w oponie okrągłej o średnicy ø8...12,5mm.","6180XX0010.jpg","6180XX0010.ldt",1,null,1,17]
["6181","6181XX0010","BORG BOLLARD BOLLARD 85CM LED 2241LM 4000K DIM.","Borg","Bollard","Aluminium",null,null,null,"LED zintegrowane","AC","DIM.","13,7W","16W","2241lm","1396lm",null,null,"65","IK08","Class I",4000,"szerokie dół",0.2,0.2,0.85,"CE",null,null,"> 72 000h",1,"Oprawa słupkowa.","Światło obrotowo-symetryczne.",null,"Luminaire with contemporary design. For lighting gardens and other private and public areas",null,null,null,"Odlew aluminiowy malowany proszkowo.",null,"Klosz- tworzywo sztuczne PMMA satynowane.","Uszczelka silikonowa.",null,"85cm",null,"Oprawa ściemnialna fazowo TRAILING EDGE (TE) - LEADING EDGE (LE)","Moduł LED","Cree DK201002 V1 JK3030 6V 4K","TCI Mini MD 18W 350mA code 127030 Triac",0,null,0,80,"E","202GA0009, 203ZX0009","Zaciski podłączeniowe: max 3x4mm², możliwość podłączenia oprawy w pętle max 3x4mm². Przewód w oponie okrągłej o średnicy ø8...12,5mm.","6181XX0010.jpg","6181XX0010.ldt",1,null,1,17]
["6182","6182XX0009","BORG BOLLARD BOLLARD 85CM LED 2093LM 3000K DALI2","Borg","Bollard","Aluminium",null,null,null,"LED zintegrowane","AC","DALI2","13,7W","17,6W","2093lm","1358lm",null,null,"65","IK08","Class I",3000,"szerokie dół",0.2,0.2,0.85,"CE",null,"DALI","> 72 000h",1,"Oprawa słupkowa.","Światło obrotowo-symetryczne.",null,"Luminaire with a contemporary design For lighting gardens, other private and public areas",null,null,null,"Odlew aluminiowy malowany proszkowo.",null,"Klosz- tworzywo sztuczne PMMA satynowane.","Uszczelka silikonowa.",null,"85cm",null,"Sterowanie światłem w systemie: DALI outdoor pełny program. Zasilacz zaprogramowany na max prąd. Programowanie pozostałych parametrów po uzgodnieniu z Działem Handlowym firmy Norlys.","Moduł LED","Cree DK201002 V1 JK3030 6V 3K","Philips Xi FP 22W 0,2-0,7A SNLDAE 230V S175 sXt 929002172306",100000,"DALI2 / NightDim (XI FP NLD)",0,80,"E","202GA0009, 203ZX0009","Zaciski podłączeniowe: max 5x2,5mm², możliwość podłączenia oprawy w pętle max 5x2,5mm². Przewód w oponie okrągłej o średnicy ø7...13,5mm.","6182XX0009.jpg","6182XX0009.ldt",3,null,1,17]
["6183","6183XX0009","BORG BOLLARD BOLLARD 85CM LED 2216LM 4000K DALI2","Borg","Bollard","Aluminium",null,null,null,"LED zintegrowane","AC","DALI2","13,7W","15,9W","2216lm","1396lm",null,null,"65","IK08","Class I",4000,"szerokie dół",0.2,0.2,0.85,"CE",null,"DALI","> 72 000h",1,"Oprawa słupkowa.","Światło obrotowo-symetryczne.",null,"Luminaire with a contemporary design. For lighting gardens and other private and public areas",null,null,null,"Odlew aluminiowy malowany proszkowo.",null,"Klosz- tworzywo sztuczne PMMA satynowane.","Uszczelka silikonowa.",null,"85cm",null,"Sterowanie światłem w systemie: DALI outdoor pełny program. Zasilacz zaprogramowany na max prąd. Programowanie pozostałych parametrów po uzgodnieniu z Działem Handlowym firmy Norlys.","Moduł LED","Cree DK201002 V1 JK3030 6V 4K","Philips Xi FP 22W 0,2-0,7A SNLDAE 230V S175 sXt 929002172306",100000,"DALI2 / NightDim (XI FP NLD)",0,80,"E","202GA0009, 203ZX0009","Zaciski podłączeniowe: max 5x2,5mm², możliwość podłączenia oprawy w pętle max 5x2,5mm². Przewód w oponie okrągłej o średnicy ø7...13,5mm.","6183XX0009.jpg","6183XX0009.ldt",3,null,1,17]
["6190","6190XX0010","BORG BOLLARD BOLLARD 110CM LED 2093LM 3000K DIM.","Borg","Bollard","Aluminium",null,null,null,"LED zintegrowane","AC","DIM.","13,7W","16W","2093lm","1358lm",null,null,"65","IK08","Class I",3000,"szerokie dół",0.2,0.2,1.05,"CE",null,null,"> 72 000h",1,"Oprawa słupkowa.","Światło obrotowo-symetryczne.",null,"Luminaire with contemporary design. For lighting gardens and other private and public areas",null,null,null,"Odlew aluminiowy malowany proszkowo.",null,"Klosz- tworzywo sztuczne PMMA satynowane.","Uszczelka silikonowa.",null,"110cm",null,"Oprawa ściemnialna fazowo TRAILING EDGE (TE) - LEADING EDGE (LE)","Moduł LED","Cree DK201002 V1 JK3030 6V 3K","TCI Mini MD 18W 350mA code 127030 Triac",0,null,0,80,"E","202GA0009, 203ZX0009","Zaciski podłączeniowe: max 3x4mm², możliwość podłączenia oprawy w pętle max 3x4mm². Przewód w oponie okrągłej o średnicy ø8...12,5mm.","6190XX0010.png","6190XX0010.ldt",1,null,1,17]
["6191","6191XX0010","BORG BOLLARD BOLLARD 110CM LED 2241LM 4000K DIM.","Borg","Bollard","Aluminium",null,null,null,"LED zintegrowane","AC","DIM.","13,7W","16W","2241lm","1396lm",null,null,"65","IK08","Class I",4000,"szerokie dół",0.2,0.2,1.05,"CE",null,null,"> 72 000h",1,"Oprawa słupkowa.","Światło obrotowo-symetryczne.",null,"Luminaire with contemporary design. For lighting gardens and other private and public areas",null,null,null,"Odlew aluminiowy malowany proszkowo.",null,"Klosz- tworzywo sztuczne PMMA satynowane.","Uszczelka silikonowa.",null,"110cm",null,"Oprawa ściemnialna fazowo TRAILING EDGE (TE) - LEADING EDGE (LE)","Moduł LED","Cree DK201002 V1 JK3030 6V 4K","TCI Mini MD 18W 350mA code 127030 Triac",0,null,0,80,"E","202GA0009, 203ZX0009","Zaciski podłączeniowe: max 3x4mm², możliwość podłączenia oprawy w pętle max 3x4mm². Przewód w oponie okrągłej o średnicy ø8...12,5mm.","6191XX0010.png","6191XX0010.ldt",1,null,1,17]
["6192","6192XX0009","BORG BOLLARD BOLLARD 110CM LED 2093LM 3000K DALI2","Borg","Bollard","Aluminium",null,null,null,"LED zintegrowane","AC","DALI2","13,7W","17,6W","2093lm","1358lm",null,null,"65","IK08","Class I",3000,"szerokie dół",0.2,0.2,1.05,"CE",null,"DALI","> 72 000h",1,"Oprawa słupkowa.","Światło obrotowo-symetryczne.",null,"Luminaire with a contemporary design. For garden lighting and other private and public areas.",null,null,null,"Odlew aluminiowy malowany proszkowo.",null,"Klosz- tworzywo sztuczne PMMA satynowane.","Uszczelka silikonowa.",null,"110cm",null,"Sterowanie światłem w systemie: DALI outdoor pełny program. Zasilacz zaprogramowany na max prąd. Programowanie pozostałych parametrów po uzgodnieniu z Działem Handlowym firmy Norlys.","Moduł LED","Cree DK201002 V1 JK3030 6V 3K","Philips Xi FP 22W 0,2-0,7A SNLDAE 230V S175 sXt 929002172306",100000,"DALI2 / NightDim (XI FP NLD)",0,80,"E","202GA0009, 203ZX0009","Zaciski podłączeniowe: max 5x2,5mm², możliwość podłączenia oprawy w pętle max 5x2,5mm². Przewód w oponie okrągłej o średnicy ø7...13,5mm.","6192XX0009.png","6192XX0009.ldt",3,null,1,17]
["6193","6193XX0009","BORG BOLLARD BOLLARD 110CM LED 2216LM 4000K DALI2","Borg","Bollard","Aluminium",null,null,null,"LED zintegrowane","AC","DALI2","13,7W","17,6W","2216lm","1396lm",null,null,"65","IK08","Class I",4000,"szerokie dół",1.05,0.2,0.2,"CE",null,"DALI","> 72 000h",1,"Oprawa słupkowa.","Światło obrotowo-symetryczne.",null,"Luminaire with a contemporary design. For lighting gardens and other private and public areas",null,null,null,"Odlew aluminiowy malowany proszkowo.",null,"Klosz- tworzywo sztuczne PMMA satynowane.","Uszczelka silikonowa.",null,"110cm",null,"Sterowanie światłem w systemie: DALI outdoor pełny program. Zasilacz zaprogramowany na max prąd. Programowanie pozostałych parametrów po uzgodnieniu z Działem Handlowym firmy Norlys.","Moduł LED","Cree DK201002 V1 JK3030 6V 4K","Philips Xi FP 22W 0,2-0,7A SNLDAE 230V S175 sXt 929002172306",100000,"DALI2 / NightDim (XI FP NLD)",0,80,"E","202GA0009, 203ZX0009","Zaciski podłączeniowe: max 5x2,5mm², możliwość podłączenia oprawy w pętle max 5x2,5mm². Przewód w oponie okrągłej o średnicy ø7...13,5mm.","6193XX0009.png","6193XX0009.ldt",3,null,1,17]
["630","630XX0011","BREMEN WALL E27","Bremen","Wall","Stal",null,null,null,"Wymienne","E27",null,"LED max 9W","LED max 9W",null,null,null,null,"54","IK10","Class I",null,null,0.28000000000000003,0.28000000000000003,0.14000000000000001,"CE",null,null,null,12,"Oprawa ścienna.","Światło odkryte.",null,"Classic design plafond type luminaire.",null,null,"Oprawa na wymienne źródło światła typu: lampa LED, świetlówka TC-SE, tradycyjna żarówka (halogenowa) o trzonku E27. Źródło światła należy dokupić oddzielnie.","Odlew aluminiowy malowany proszkowo.","Front- stal cynkowana ogniowo, stal malowana proszkowo.","Klosz- poliwęglan przeźroczysty, stabilizowany UV.","Uszczelka silikonowa.","Dławnica EPDM.",null,"przeźroczysty",null,"Lampa E27","LED A55..60",null,0,null,null,80,null,"46999021","Zaciski podłączeniowe: max 3x2,5mm², możliwość podłączenia oprawy w pętle max 3x1,5mm². Przewód w oponie okrągłej o średnicy ø7...10,5mm.","630XX0011.jpg","630XX0011.ldt",4,"E27",1,9]
["631","631XX0010","BREMEN WALL E27","Bremen","Wall","Stal",null,null,null,"Wymienne","E27",null,"LED max 9W","LED max 9W",null,null,null,null,"54","IK10","Class I",null,null,0.28000000000000003,0.28000000000000003,0.14000000000000001,"CE",null,null,null,12,"Oprawa ścienna.","Światło rozproszone.",null,"Classic design plafond type luminaire","A ceiling-type luminaire with a classic design. Functions: control, color change 2700K…6500K (TW), WiZ, WiZ Pro. - Available after mounting in the luminaire, Signify WiZ Pro A60 E27 TW 8W 230V lamps - Full control of the luminaire after installing the free application https://pro.wizconnected.com/ - Technical support: Information Sales Department of Norlys",null,null,"Odlew aluminiowy malowany proszkowo.","Front- stal cynkowana ogniowo, stal malowana proszkowo.","Klosz- poliwęglan mleczny, stabilizowany UV.","Uszczelka silikonowa.","Dławnica EPDM.",null,"mleczny",null,"Lampa E27","LED A55..60",null,0,null,null,80,null,"46999021","Zaciski podłączeniowe: max 3x2,5mm², możliwość podłączenia oprawy w pętle max 3x1,5mm². Przewód w oponie okrągłej o średnicy ø7...10,5mm.","631XX0010.jpg","631XX0010.ldt",4,"E27",1,7]
["6346","6346XX0009","MOSS LED 439LM 36D 3000K DIM.","Moss","Recessed","Stal",null,null,null,"LED zintegrowane","AC","DIM.","4W","4W","439lm","389lm",null,null,"65",null,"Class I",3000,null,0.12,0.12,7.0000000000000007E-2,"CE",null,null,"> 50 000h",3,"Oprawa wbudowana.","Światło symetryczne o kącie 36D","36D","For illuminating gardens, private areas and other architectural concepts. Possibility to adjust the direction of light",null,null,null,"Odlew aluminiowy malowany proszkowo.",null,"Klosz- szkło bezpieczne, przeźroczyste.",null,null,"Ø120","Mocowanie śrubowe","Oprawa ściemnialna fazowo TRAILING EDGE (TE) - LEADING EDGE (LE)","Moduł LED","Lumens EDC 38C 4W xxx 230V A101 3K",null,0,"Ściemnianie fazowe Lumens LED AC",null,80,"E","145ZX0009, 4701420002","Przewód H05RN-F 3G1 o długości 0,3m do podłączenia w odpowiednio dobranej puszce elektroinstalacyjnej.","6346XX0009.png","6346XX0009.ldt",1,null,4,68]
["6352","6352XX0009","MOSS LED 466LM 36D 4000K DIM.","Moss","Recessed","Stal",null,null,null,"LED zintegrowane","AC","DIM.","4W","4W","466lm","414lm",null,null,"65",null,"Class I",4000,null,0.12,0.12,7.0000000000000007E-2,"CE",null,null,"> 50 000h",3,"Oprawa wbudowana.","Światło symetryczne o kącie 36D","36D","For illuminating gardens, private areas and other concepts architectural. Possibility to adjust the direction of light.",null,null,null,"Odlew aluminiowy malowany proszkowo.",null,"Klosz- szkło bezpieczne, przeźroczyste.",null,null,"Ø120","Mocowanie śrubowe","Oprawa ściemnialna fazowo TRAILING EDGE (TE) - LEADING EDGE (LE)","Moduł LED","Lumens EDC 38C 4W xxx 230V A101 4K",null,0,"Ściemnianie fazowe Lumens LED AC",null,80,"E","145ZX0009, 4701420002","Przewód H05RN-F 3G1 o długości 0,3m do podłączenia w odpowiednio dobranej puszce elektroinstalacyjnej.","6352XX0009.png","6352XX0009.ldt",1,null,4,68]
["6355","6355XX0009","MOSS LED 439LM 36D 3000K DIM.","Moss","Recessed","Stal",null,null,null,"LED zintegrowane","AC","DIM.","4W","4W","439lm","389lm",null,null,"65",null,"Class I",3000,null,0.13,0.13,0.06,"CE",null,null,"> 50 000h",3,"Oprawa wbudowana.","Światło symetryczne o kącie 36D","36D","For illuminating gardens, private areas and other concepts architectural. Possibility to adjust the direction of light also in the vertical plane",null,null,null,"Odlew aluminiowy malowany proszkowo.",null,"Klosz- szkło bezpieczne, przeźroczyste.",null,null,"Ø130","Mocowanie sprężynowe","Oprawa ściemnialna fazowo TRAILING EDGE (TE) - LEADING EDGE (LE)","Moduł LED","Lumens EDC 38C 4W xxx 230V A101 3K",null,0,"Ściemnianie fazowe Lumens LED AC",null,80,"E","145ZX0009, 4701420002","Przewód H05RN-F 3G1 o długości 0,3m do podłączenia w odpowiednio dobranej puszce elektroinstalacyjnej.","6355XX0009.png","6355XX0009.ldt",1,null,4,68]
["6361","6361XX0009","MOSS LED 466LM 36D 4000K DIM.","Moss","Recessed","Stal",null,null,null,"LED zintegrowane","AC","DIM.","4W","4W","466lm","414lm",null,null,"65",null,"Class I",4000,null,0.13,0.13,0.06,"CE",null,null,"> 50 000h",3,"Oprawa wbudowana.","Światło symetryczne o kącie 36D","36D","For illuminating gardens, private areas and other concepts architectural. Possibility to adjust the direction of light.",null,null,null,"Odlew aluminiowy malowany proszkowo.",null,"Klosz- szkło bezpieczne, przeźroczyste.",null,null,"Ø130","Mocowanie sprężynowe","Oprawa ściemnialna fazowo TRAILING EDGE (TE) - LEADING EDGE (LE)","Moduł LED","Lumens EDC 38C 4W xxx 230V A101 4K",null,0,"Ściemnianie fazowe Lumens LED AC",null,80,"E","145ZX0009, 4701420002","Przewód H05RN-F 3G1 o długości 0,3m do podłączenia w odpowiednio dobranej puszce elektroinstalacyjnej.","6361XX0009.png","6361XX0009.ldt",1,null,4,68]
["6370","6370XX0009","MOSS LED 840LM 36D 3000K DIM.","Moss","Recessed","Stal",null,null,null,"LED zintegrowane","AC","DIM.","8W","8W","840lm","686lm",null,null,"65",null,"Class I",3000,null,0.12,0.12,7.0000000000000007E-2,"CE",null,null,"> 50 000h",3,"Oprawa wbudowana.","Światło symetryczne o kącie 36D","36D","For illuminating gardens, private areas and other concepts architectural. Possibility to adjust the direction of light.",null,null,null,"Odlew aluminiowy malowany proszkowo.",null,"Klosz- szkło bezpieczne, przeźroczyste.",null,null,"Ø120","Mocowanie śrubowe","Oprawa ściemnialna fazowo TRAILING EDGE (TE) - LEADING EDGE (LE)","Moduł LED","Lumens EDC 38C 8W xxx 230V A101 3K",null,0,"Ściemnianie fazowe Lumens LED AC",null,80,"E","145ZX0009, 4701420002","Przewód H05RN-F 3G1 o długości 0,3m do podłączenia w odpowiednio dobranej puszce elektroinstalacyjnej.","6370XX0009.png","6370XX0009.ldt",1,null,4,68]
["6376","6376XX0009","MOSS LED 891LM 36D 4000K DIM.","Moss","Recessed","Stal",null,null,null,"LED zintegrowane","AC","DIM.","8W","8W","891lm","749lm",null,null,"65",null,"Class I",4000,null,0.12,0.12,7.0000000000000007E-2,"CE",null,null,"> 50 000h",3,"Oprawa wbudowana.","Światło symetryczne o kącie 36D","36D","For illuminating gardens, private areas and other concepts architectural. Possibility to adjust the direction of light.",null,null,null,"Odlew aluminiowy malowany proszkowo.",null,"Klosz- szkło bezpieczne, przeźroczyste.",null,null,"Ø120","Mocowanie śrubowe","Oprawa ściemnialna fazowo TRAILING EDGE (TE) - LEADING EDGE (LE)","Moduł LED","Lumens EDC 38C 8W xxx 230V A101 4K",null,0,"Ściemnianie fazowe Lumens LED AC",null,80,"E","145ZX0009, 4701420002","Przewód H05RN-F 3G1 o długości 0,3m do podłączenia w odpowiednio dobranej puszce elektroinstalacyjnej.","6376XX0009.png","6376XX0009.ldt",1,null,4,68]
["6379","6379XX0009","MOSS LED 840LM 36D 3000K DIM.","Moss","Recessed","Stal",null,null,null,"LED zintegrowane","AC","DIM.","8W","8W","840lm","686lm",null,null,"65",null,"Class I",3000,null,0.13,0.13,0.06,"CE",null,null,"> 50 000h",3,"Oprawa wbudowana.","Światło symetryczne o kącie 36D","36D","For illuminating gardens, private areas and other concepts architectural. Possibility to adjust the direction of light also in the vertical plane",null,null,null,"Odlew aluminiowy malowany proszkowo.",null,"Klosz- szkło bezpieczne, przeźroczyste.",null,null,"Ø130","Mocowanie sprężynowe","Oprawa ściemnialna fazowo TRAILING EDGE (TE) - LEADING EDGE (LE)","Moduł LED","Lumens EDC 38C 8W xxx 230V A101 3K",null,0,"Ściemnianie fazowe Lumens LED AC",null,80,"E","145ZX0009, 4701420002","Przewód H05RN-F 3G1 o długości 0,3m do podłączenia w odpowiednio dobranej puszce elektroinstalacyjnej.","6379XX0009.png","6379XX0009.ldt",1,null,4,68]
["637","637XX0013","BREMEN WALL LED 880LM 3000K DIM.","Bremen","Wall","Stal",null,null,null,"LED zintegrowane","AC","DIM.","8W","8W","880lm","364lm",null,null,"54","IK10","Class I",3000,null,0,0,0,"CE",null,null,"50 000h",12,"Oprawa ścienna.","Światło rozproszone.",null,"A ceiling-type luminaire with a contemporary design for general use",null,null,null,"Odlew aluminiowy malowany proszkowo.",null,"Klosz- poliwęglan mleczny, stabilizowany UV.","Uszczelka silikonowa.","Dławnica EPDM.",null,"mleczny","Oprawa ściemnialna fazowo TRAILING EDGE (TE) - LEADING EDGE (LE)","Moduł LED","Lumens EDC 38C 8W xxx 230V A101 3K",null,0,"Ściemnianie fazowe Lumens LED AC",null,80,"E",null,"Zaciski podłączeniowe: max 3x2,5mm², możliwość podłączenia oprawy w pętle max 3x1,5mm². Przewód w oponie okrągłej o średnicy ø7...10,5mm.","637XX0013.jpg","637XX0013.ldt",1,null,1,7]
["6385","6385XX0009","MOSS LED 891LM 36D 4000K DIM.","Moss","Recessed","Aluminium",null,null,null,"LED zintegrowane","AC","DIM.","8W","8W","891lm","749lm",null,null,"65",null,"Class I",4000,null,0.13,0.13,0.06,"CE",null,null,"> 50 000h",3,"Oprawa wbudowana.","Światło symetryczne o kącie 36D","36D","For illuminating gardens, private areas and other concepts architectural. Possibility to adjust the direction of light.",null,null,null,"Odlew aluminiowy malowany proszkowo.",null,"Klosz- szkło bezpieczne, przeźroczyste.",null,null,"Ø130","Mocowanie sprężynowe","Oprawa ściemnialna fazowo TRAILING EDGE (TE) - LEADING EDGE (LE)","Moduł LED","Lumens EDC 38C 8W xxx 230V A101 4K",null,0,"Ściemnianie fazowe Lumens LED AC",null,80,"E","145ZX0009, 4701420002","Przewód H05RN-F 3G1 o długości 0,3m do podłączenia w odpowiednio dobranej puszce elektroinstalacyjnej.","6385XX0009.png","6385XX0009.ldt",1,null,4,68]
["638","638XX0009","BREMEN WALL LED 1080LM 3000K MD","Bremen","Wall","Stal",null,null,null,"LED zintegrowane","AC","MD","9,5W","10W","1080lm","532lm",null,null,"54",null,"Class I",3000,null,null,null,null,"CE","Daylight sensor,Motion sensor",null,"50 000h",12,"Oprawa ścienna.","Światło rozproszone.",null,"A ceiling-type luminaire with a contemporary design for general use. Equipped with a wave motion sensor, a twilight switch, and motion support",null,null,null,"Odlew aluminiowy malowany proszkowo.",null,"Klosz- poliwęglan mleczny, stabilizowany UV.","Uszczelka silikonowa.","Dławnica EPDM.",null,"mleczny","Oprawa wyposażona w mikrofalowy czujnik ruchu, z wyłącznikiem zmierzchowym i podtrzymaniem ruchu","Moduł LED","Philips Fortimo DLM ES 1100/8xx G2 3K",null,0,"Mikrofalowy czujnik ruchu MD (PD-MV1005)",null,80,"E",null,"Zaciski podłączeniowe: max 3x2,5mm², możliwość podłączenia oprawy w pętle max 3x1,5mm². Przewód w oponie okrągłej o średnicy ø7...10,5mm.","638XX0009.jpg","638XX0009.ldt",3,null,1,7]
["6401","6401XX0009","LYSFJORD WALL 2XLED 4144LM UP4º & DOWN60º 3000K DALI2","Lysfjord","Wall","Aluminium",null,null,null,"LED zintegrowane","AC","DALI2","22,5W","26,5W","4144lm","946lm",null,null,"65","IK08","Class I",3000,"wąskie góra / szerokie dół",0.43,0.15,0.2,"CE",null,"DALI","> 70 000h",12,"Oprawa ścienna.","Światło dwustronne: o kącie 4º do góry i kącie 60º w dół.","Up4º & Down60º","A luminaire with a wide range of applications, including lighting: wall surfaces, facades and other architectural concepts.",null,null,null,"Odlew aluminiowy malowany proszkowo.",null,"Klosz- szkło bezpieczne, optyczne.","Uszczelka silikonowa.","Dławnica EPDM.","góra/dół","wąskie/szerokie","Sterowanie światłem w systemie: DALI outdoor pełny program. Zasilacz zaprogramowany na max prąd. Programowanie pozostałych parametrów po uzgodnieniu z Działem Handlowym firmy Norlys.","2 Moduły LED","Cree DK200305 V3 JB2835 3V 3K","Osram OT 40/170-240/1A0 4DIMLT2 NFC E",100000,"DALI2 / NightDim (4DIM)",null,80,"C",null,"Zaciski podłączeniowe: max 5x2,5mm², możliwość podłączenia oprawy w pętle max 5x1,5mm². Przewód w oponie okrągłej o średnicy ø7...10,5mm.","6401XX0009.png","6401XX0009.ldt",3,null,1,42]
["6402","6402XX0009","LYSFJORD WALL 2XLED 4144LM UP60º & DOWN4º 3000K DALI2","Lysfjord","Wall","Aluminium",null,null,null,"LED zintegrowane","AC","DALI2","22,5W","26,5W","4144lm","946lm",null,null,"65","IK08","Class I",3000,"szerokie góra / wąskie dół",0.43,0.15,0.2,"CE",null,"DALI","> 70 000h",12,"Oprawa ścienna.","Światło dwustronne: o kącie 60º do góry i kącie 4º w dół.","Up60º & Down4º","A luminaire with a wide range of applications, including lighting: wall surfaces, facades and other architectural concepts.",null,null,null,"Odlew aluminiowy malowany proszkowo.",null,"Klosz- szkło bezpieczne, optyczne.","Uszczelka silikonowa.","Dławnica EPDM.","góra/dół","szerokie/wąskie","Sterowanie światłem w systemie: DALI outdoor pełny program. Zasilacz zaprogramowany na max prąd. Programowanie pozostałych parametrów po uzgodnieniu z Działem Handlowym firmy Norlys.","2 Moduły LED","Cree DK200305 V3 JB2835 3V 3K","Osram OT 40/170-240/1A0 4DIMLT2 NFC E",100000,"DALI2 / NightDim (4DIM)",null,80,"C",null,"Zaciski podłączeniowe: max 5x2,5mm², możliwość podłączenia oprawy w pętle max 5x1,5mm². Przewód w oponie okrągłej o średnicy ø7...10,5mm.","6402XX0009.png","6402XX0009.ldt",3,null,1,59]
["6403","6403XX0009","LYSFJORD WALL 2XLED 4144LM UP60º & DOWN60º 3000K DALI2","Lysfjord","Wall","Aluminium",null,null,null,"LED zintegrowane","AC","DALI2","22,5W","26,5W","4144lm","1814lm",null,null,"65","IK08","Class I",3000,"szerokie góra / szerokie dół",0.43,0.15,0.12,"CE",null,"DALI","> 70 000h",12,"Oprawa ścienna.","Światło dwustronne: o kącie 60º do góry i w dół.","Up60º & Down60º","A luminaire with a wide range of applications, including lighting: wall surfaces, facades and other architectural concepts.",null,null,null,"Odlew aluminiowy malowany proszkowo.",null,"Klosz- szkło bezpieczne, optyczne.","Uszczelka silikonowa.","Dławnica EPDM.","góra/dół","szerokie/szerokie","Sterowanie światłem w systemie: DALI outdoor pełny program. Zasilacz zaprogramowany na max prąd. Programowanie pozostałych parametrów po uzgodnieniu z Działem Handlowym firmy Norlys.","2 Moduły LED","Cree DK200305 V3 JB2835 3V 3K","Osram OT 40/170-240/1A0 4DIMLT2 NFC E",100000,"DALI2 / NightDim (4DIM)",null,80,"C",null,"Zaciski podłączeniowe: max 5x2,5mm², możliwość podłączenia oprawy w pętle max 5x1,5mm². Przewód w oponie okrągłej o średnicy ø7...10,5mm.","6403XX0009.png","6403XX0009.ldt",3,null,1,13]
["6404","6404XX0009","LYSFJORD WALL 2XLED 4144LM UP4º & DOWN4º 3000K DALI2","Lysfjord","Wall","Aluminium",null,null,null,"LED zintegrowane","AC","DALI2","22,5W","26,5W","4144lm","78lm",null,null,"65","IK08","Class I",3000,"wąskie góra / wąskie dół",0.43,0.15,0.2,"CE",null,"DALI","> 70 000h",12,"Oprawa ścienna.","Światło dwustronne: o kącie 4º do góry i w dół.","Up4º & Down4º","A luminaire with a wide range of applications, including lighting: wall surfaces, facades and other architectural concepts.",null,null,null,"Odlew aluminiowy malowany proszkowo.",null,"Klosz- szkło bezpieczne, optyczne.","Uszczelka silikonowa.","Dławnica EPDM.","góra/dół","wąskie/wąskie","Sterowanie światłem w systemie: DALI outdoor pełny program. Zasilacz zaprogramowany na max prąd. Programowanie pozostałych parametrów po uzgodnieniu z Działem Handlowym firmy Norlys.","2 Moduły LED","Cree DK200305 V3 JB2835 3V 3K","Osram OT 40/170-240/1A0 4DIMLT2 NFC E",100000,"DALI2 / NightDim (4DIM)",null,80,"C",null,"Zaciski podłączeniowe: max 5x2,5mm², możliwość podłączenia oprawy w pętle max 5x1,5mm². Przewód w oponie okrągłej o średnicy ø7...10,5mm.","6404XX0009.png","6404XX0009.ldt",3,null,1,14]
["6405","6405XX0009","LYSFJORD WALL LED 2072LM UP 4º 3000K DALI2","Lysfjord","Wall","Aluminium",null,null,null,"LED zintegrowane","AC","DALI2","11,8W","14,6W","2072lm","39lm",null,null,"65","IK08","Class I",3000,"wąskie góra",0.34,0.15,0.2,"CE",null,"DALI","> 70 000h",12,"Oprawa ścienna.","Światło jednostronne: o kącie 4º do góry.","Up 4º","A luminaire with a wide range of applications, including lighting: wall surfaces, facades and other architectural concepts.",null,null,null,"Odlew aluminiowy malowany proszkowo.",null,"Klosz- szkło bezpieczne, optyczne.","Uszczelka silikonowa.","Dławnica EPDM.","góra","wąskie jednostronne","Sterowanie światłem w systemie: DALI outdoor pełny program. Zasilacz zaprogramowany na max prąd. Programowanie pozostałych parametrów po uzgodnieniu z Działem Handlowym firmy Norlys.","Moduł LED","Cree DK200305 V3 JB2835 3V 3K","Osram OT 40/170-240/1A0 4DIMLT2 NFC E",100000,"DALI2 / NightDim (4DIM)",null,80,"C",null,"Zaciski podłączeniowe: max 5x2,5mm², możliwość podłączenia oprawy w pętle max 5x1,5mm². Przewód w oponie okrągłej o średnicy ø7...10,5mm.","6405XX0009.png","6405XX0009.ldt",3,null,1,39]
["6406","6406XX0009","LYSFJORD WALL LED 2072LM DOWN 4º 3000K DALI2","Lysfjord","Wall","Aluminium",null,null,null,"LED zintegrowane","AC","DALI2","11,8W","14,6W","2072lm","39lm",null,null,"65","IK08","Class I",3000,"wąskie dół",0.34,0.15,0.2,"CE",null,"DALI","> 70 000h",12,"Oprawa ścienna.","Światło jednostronne: o kącie 4º w dół.","Down 4º","A luminaire with a wide range of applications, including lighting: wall surfaces, facades and other architectural concepts.",null,null,null,"Odlew aluminiowy malowany proszkowo.",null,"Klosz- szkło bezpieczne, optyczne.","Uszczelka silikonowa.","Dławnica EPDM.","dół","wąskie jednostronne","Sterowanie światłem w systemie: DALI outdoor pełny program. Zasilacz zaprogramowany na max prąd. Programowanie pozostałych parametrów po uzgodnieniu z Działem Handlowym firmy Norlys.","Moduł LED","Cree DK200305 V3 JB2835 3V 3K","Osram OT 40/170-240/1A0 4DIMLT2 NFC E",100000,"DALI2 / NightDim (4DIM)",null,80,"C",null,"Zaciski podłączeniowe: max 5x2,5mm², możliwość podłączenia oprawy w pętle max 5x1,5mm². Przewód w oponie okrągłej o średnicy ø7...10,5mm.","6406XX0009.png","6406XX0009.ldt",3,null,1,40]
["6407","6407XX0009","LYSFJORD WALL LED 2072LM UP60º 3000K DALI2","Lysfjord","Wall","Aluminium",null,null,null,"LED zintegrowane","AC","DALI2","11,8W","14,6W","2072lm","998lm",null,null,"65","IK08","Class I",3000,"szerokie góra",0.34,0.15,0.2,"CE",null,"DALI","> 70 000h",12,"Oprawa ścienna.","Światło jednostronne: o kącie 60º w górę.","Up60º","A luminaire with a wide range of applications, including lighting: wall surfaces, facades and other architectural concepts.",null,null,null,"Odlew aluminiowy malowany proszkowo.",null,"Klosz- szkło bezpieczne, optyczne.","Uszczelka silikonowa.","Dławnica EPDM.","góra","szerokie jednostronne","Sterowanie światłem w systemie: DALI outdoor pełny program. Zasilacz zaprogramowany na max prąd. Programowanie pozostałych parametrów po uzgodnieniu z Działem Handlowym firmy Norlys.","Moduł LED","Cree DK200305 V3 JB2835 3V 3K","Osram OT 40/170-240/1A0 4DIMLT2 NFC E",100000,"DALI2 / NightDim (4DIM)",null,80,"C",null,"Zaciski podłączeniowe: max 5x2,5mm², możliwość podłączenia oprawy w pętle max 5x1,5mm². Przewód w oponie okrągłej o średnicy ø7...10,5mm.","6407XX0009.png","6407XX0009.ldt",3,null,1,65]
["6408","6408XX0009","LYSFJORD WALL LED 2072LM DOWN60º 3000K DALI2","Lysfjord","Wall","Aluminium",null,null,null,"LED zintegrowane","AC","DALI2","11,8W","14,6W","2072lm","998lm",null,null,"65","IK08","Class I",3000,"szerokie dół",0.34,0.15,0.2,"CE",null,"DALI","> 70 000h",12,"Oprawa ścienna.","Światło jednostronne: o kącie 60º w dół.","Down60º","A luminaire with a wide range of applications, including lighting: wall surfaces, facades and other architectural concepts.",null,null,null,"Odlew aluminiowy malowany proszkowo.",null,"Klosz- szkło bezpieczne, optyczne.","Uszczelka silikonowa.","Dławnica EPDM.","dół","szerokie jednostronne","Sterowanie światłem w systemie: DALI outdoor pełny program. Zasilacz zaprogramowany na max prąd. Programowanie pozostałych parametrów po uzgodnieniu z Działem Handlowym firmy Norlys.","Moduł LED","Cree DK200305 V3 JB2835 3V 3K","Osram OT 40/170-240/1A0 4DIMLT2 NFC E",100000,"DALI2 / NightDim (4DIM)",null,80,"C",null,"Zaciski podłączeniowe: max 5x2,5mm², możliwość podłączenia oprawy w pętle max 5x1,5mm². Przewód w oponie okrągłej o średnicy ø7...10,5mm.","6408XX0009.png","6408XX0009.ldt",3,null,1,38]
["6421","6421XX0009","LYSFJORD WALL 2XLED 4144LM UP4º & DOWN60º 4000K DALI2","Lysfjord","Wall","Aluminium",null,null,null,"LED zintegrowane","AC","DALI2","22,5W","26,5W","4144lm","946lm",null,null,"65","IK08","Class I",4000,"wąskie góra / szerokie dół",0.43,0.15,0.2,"CE",null,"DALI","> 70 000h",12,"Oprawa ścienna.","Światło dwustronne: o kącie 4º do góry i kącie 60º w dół.","Up4º & Down60º","A luminaire with a wide range of applications, including lighting: wall surfaces, facades and other architectural concepts.",null,null,null,"Odlew aluminiowy malowany proszkowo.",null,"Klosz- szkło bezpieczne, optyczne.","Uszczelka silikonowa.","Dławnica EPDM.","góra/dół","wąskie/szerokie","Sterowanie światłem w systemie: DALI outdoor pełny program. Zasilacz zaprogramowany na max prąd. Programowanie pozostałych parametrów po uzgodnieniu z Działem Handlowym firmy Norlys.","2 Moduły LED","Cree DK200305 V3 JB2835 3V 4K","Osram OT 40/170-240/1A0 4DIMLT2 NFC E",100000,"DALI2 / NightDim (4DIM)",null,80,"C",null,"Zaciski podłączeniowe: max 5x2,5mm², możliwość podłączenia oprawy w pętle max 5x1,5mm². Przewód w oponie okrągłej o średnicy ø7...10,5mm.","6421XX0009.png","6421XX0009.ldt",3,null,1,42]
["6422","6422XX0009","LYSFJORD WALL 2XLED 4144LM UP60º & DOWN4º 4000K DALI2","Lysfjord","Wall","Aluminium",null,null,null,"LED zintegrowane","AC","DALI2","22,5W","26,5W","4144lm","946lm",null,null,"65","IK08","Class I",4000,"szerokie góra / wąskie dół",0.43,0.15,0.2,"CE",null,"DALI","> 70 000h",12,"Oprawa ścienna.","Światło dwustronne: o kącie 60º do góry i kącie 4º w dół.","Up60º & Down4º","A luminaire with a wide range of applications, including lighting: wall surfaces, facades and other architectural concepts.",null,null,null,"Odlew aluminiowy malowany proszkowo.",null,"Klosz- szkło bezpieczne, optyczne.","Uszczelka silikonowa.","Dławnica EPDM.","góra/dół","szerokie/wąskie","Sterowanie światłem w systemie: DALI outdoor pełny program. Zasilacz zaprogramowany na max prąd. Programowanie pozostałych parametrów po uzgodnieniu z Działem Handlowym firmy Norlys.","2 Moduły LED","Cree DK200305 V3 JB2835 3V 4K","Osram OT 40/170-240/1A0 4DIMLT2 NFC E",100000,"DALI2 / NightDim (4DIM)",null,80,"C",null,"Zaciski podłączeniowe: max 5x2,5mm², możliwość podłączenia oprawy w pętle max 5x1,5mm². Przewód w oponie okrągłej o średnicy ø7...10,5mm.","6422XX0009.png","6422XX0009.ldt",3,null,1,59]
["6423","6423XX0009","LYSFJORD WALL 2XLED 4144LM UP60º & DOWN60º 4000K DALI2","Lysfjord","Wall","Aluminium",null,null,null,"LED zintegrowane","AC","DALI2","22,5W","26,5W","4144lm","1814lm",null,null,"65","IK08","Class I",4000,"szerokie góra / szerokie dół",0.43,0.15,0.2,"CE",null,"DALI","> 70 000h",12,"Oprawa ścienna.","Światło dwustronne: o kącie 60º do góry i w dół.","Up60º & Down60º","A luminaire with a wide range of applications, including lighting: wall surfaces, facades and other architectural concepts.",null,null,null,"Odlew aluminiowy malowany proszkowo.",null,"Klosz- szkło bezpieczne, optyczne.","Uszczelka silikonowa.","Dławnica EPDM.","góra/dół","szerokie/szerokie","Sterowanie światłem w systemie: DALI outdoor pełny program. Zasilacz zaprogramowany na max prąd. Programowanie pozostałych parametrów po uzgodnieniu z Działem Handlowym firmy Norlys.","2 Moduły LED","Cree DK200305 V3 JB2835 3V 4K","Osram OT 40/170-240/1A0 4DIMLT2 NFC E",100000,"DALI2 / NightDim (4DIM)",null,80,"C",null,"Zaciski podłączeniowe: max 5x2,5mm², możliwość podłączenia oprawy w pętle max 5x1,5mm². Przewód w oponie okrągłej o średnicy ø7...10,5mm.","6423XX0009.png","6423XX0009.ldt",3,null,1,13]
["6424","6424XX0009","LYSFJORD WALL 2XLED 4144LM UP4º & DOWN4º 4000K DALI2","Lysfjord","Wall","Aluminium",null,null,null,"LED zintegrowane","AC","DALI2","22,5W","26,5W","4144lm","78lm",null,null,"65","IK08","Class I",4000,"wąskie góra / wąskie dół",0.43,0.15,0.2,"CE",null,"DALI","> 70 000h",12,"Oprawa ścienna.","Światło dwustronne: o kącie 4º do góry i w dół.","Up4º & Down4º","A luminaire with a wide range of applications, including lighting: wall surfaces, facades and other architectural concepts.",null,null,null,"Odlew aluminiowy malowany proszkowo.",null,"Klosz- szkło bezpieczne, optyczne.","Uszczelka silikonowa.","Dławnica EPDM.","góra/dół","wąskie/wąskie","Sterowanie światłem w systemie: DALI outdoor pełny program. Zasilacz zaprogramowany na max prąd. Programowanie pozostałych parametrów po uzgodnieniu z Działem Handlowym firmy Norlys.","2 Moduły LED","Cree DK200305 V3 JB2835 3V 4K","Osram OT 40/170-240/1A0 4DIMLT2 NFC E",100000,"DALI2 / NightDim (4DIM)",null,80,"C",null,"Zaciski podłączeniowe: max 5x2,5mm², możliwość podłączenia oprawy w pętle max 5x1,5mm². Przewód w oponie okrągłej o średnicy ø7...10,5mm.","6424XX0009.png","6424XX0009.ldt",3,null,1,14]
["6425","6425XX0009","LYSFJORD WALL LED 2072LM UP 4º 4000K DALI2","Lysfjord","Wall","Aluminium",null,null,null,"LED zintegrowane","AC","DALI2","11,8W","14,6W","2072lm","37lm",null,null,"65","IK08","Class I",4000,"wąskie góra",0.34,0.15,0.2,"CE",null,"DALI","> 70 000h",12,"Oprawa ścienna.","Światło jednostronne: o kącie 4º do góry.","Up 4º","A luminaire with a wide range of applications, including lighting: wall surfaces, facades and other architectural concepts.",null,null,null,"Odlew aluminiowy malowany proszkowo.",null,"Klosz- szkło bezpieczne, optyczne.","Uszczelka silikonowa.","Dławnica EPDM.","góra","wąskie jednostronne","Sterowanie światłem w systemie: DALI outdoor pełny program. Zasilacz zaprogramowany na max prąd. Programowanie pozostałych parametrów po uzgodnieniu z Działem Handlowym firmy Norlys.","Moduł LED","Cree DK200305 V3 JB2835 3V 4K","Osram OT 40/170-240/1A0 4DIMLT2 NFC E",100000,"DALI2 / NightDim (4DIM)",null,80,"C",null,"Zaciski podłączeniowe: max 5x2,5mm², możliwość podłączenia oprawy w pętle max 5x1,5mm². Przewód w oponie okrągłej o średnicy ø7...10,5mm.","6425XX0009.png","6425XX0009.ldt",3,null,1,39]
["6426","6426XX0009","LYSFJORD WALL LED 2072LM DOWN 4º 4000K DALI2","Lysfjord","Wall","Aluminium",null,null,null,"LED zintegrowane","AC","DALI2","11,8W","14,6W","2072lm","37lm",null,null,"65","IK08","Class I",4000,"wąskie dół",0.34,0.15,0.2,"CE",null,"DALI","> 70 000h",12,"Oprawa ścienna.","Światło jednostronne: o kącie 4º w dół.","Down 4º","A luminaire with a wide range of applications, including lighting: wall surfaces, facades and other architectural concepts.",null,null,null,"Odlew aluminiowy malowany proszkowo.",null,"Klosz- szkło bezpieczne, optyczne.","Uszczelka silikonowa.","Dławnica EPDM.","dół","wąskie jednostronne","Sterowanie światłem w systemie: DALI outdoor pełny program. Zasilacz zaprogramowany na max prąd. Programowanie pozostałych parametrów po uzgodnieniu z Działem Handlowym firmy Norlys.","Moduł LED","Cree DK200305 V3 JB2835 3V 4K","Osram OT 40/170-240/1A0 4DIMLT2 NFC E",100000,"DALI2 / NightDim (4DIM)",null,80,"C",null,"Zaciski podłączeniowe: max 5x2,5mm², możliwość podłączenia oprawy w pętle max 5x1,5mm². Przewód w oponie okrągłej o średnicy ø7...10,5mm.","6426XX0009.png","6426XX0009.ldt",3,null,1,40]
["6427","6427XX0009","LYSFJORD WALL LED 2072LM UP60º 4000K DALI2","Lysfjord","Wall","Aluminium",null,null,null,"LED zintegrowane","AC","DALI2","11,8W","14,6W","2072lm","1016lm",null,null,"65","IK08","Class I",4000,"szerokie góra",0.34,0.15,0.2,"CE",null,"DALI","> 70 000h",12,"Oprawa ścienna.","Światło jednostronne: o kącie 60º w górę.","Up60º","A luminaire with a wide range of applications, including lighting: wall surfaces, facades and other architectural concepts.",null,null,null,"Odlew aluminiowy malowany proszkowo.",null,"Klosz- szkło bezpieczne, optyczne.","Uszczelka silikonowa.","Dławnica EPDM.","góra","szerokie jednostronne","Sterowanie światłem w systemie: DALI outdoor pełny program. Zasilacz zaprogramowany na max prąd. Programowanie pozostałych parametrów po uzgodnieniu z Działem Handlowym firmy Norlys.","Moduł LED","Cree DK200305 V3 JB2835 3V 4K","Osram OT 40/170-240/1A0 4DIMLT2 NFC E",100000,"DALI2 / NightDim (4DIM)",null,80,"C",null,"Zaciski podłączeniowe: max 5x2,5mm², możliwość podłączenia oprawy w pętle max 5x1,5mm². Przewód w oponie okrągłej o średnicy ø7...10,5mm.","6427XX0009.png","6427XX0009.ldt",3,null,1,65]
["6428","6428XX0009","LYSFJORD WALL LED 2072LM DOWN60º 4000K DALI2","Lysfjord","Wall","Aluminium",null,null,null,"LED zintegrowane","AC","DALI2","11,8W","14,6W","2072lm","1016lm",null,null,"65","IK08","Class I",4000,"szerokie dół",0.34,0.15,0.2,"CE",null,"DALI","> 70 000h",12,"Oprawa ścienna.","Światło jednostronne: o kącie 60º w dół.","Down60º","A luminaire with a wide range of applications, including lighting: wall surfaces, facades and other architectural concepts.",null,null,null,"Odlew aluminiowy malowany proszkowo.",null,"Klosz- szkło bezpieczne, optyczne.","Uszczelka silikonowa.","Dławnica EPDM.","dół","wąskie jednostronne","Sterowanie światłem w systemie: DALI outdoor pełny program. Zasilacz zaprogramowany na max prąd. Programowanie pozostałych parametrów po uzgodnieniu z Działem Handlowym firmy Norlys.","Moduł LED","Cree DK200305 V3 JB2835 3V 4K","Osram OT 40/170-240/1A0 4DIMLT2 NFC E",100000,"DALI2 / NightDim (4DIM)",null,80,"C",null,"Zaciski podłączeniowe: max 5x2,5mm², możliwość podłączenia oprawy w pętle max 5x1,5mm². Przewód w oponie okrągłej o średnicy ø7...10,5mm.","6428XX0009.png","6428XX0009.ldt",3,null,1,38]
["6460","6460XX0009","MORA POLE-TOP LED 2501LM 30D 3000K DALI2","Mora","Pole","Aluminium",null,null,null,"LED zintegrowane","AC","DALI2","14,7W","17,6W","2501lm","1626lm",null,null,"65","IK08","Class I",3000,"szerokie dół",0.46,0.15,0.27,"CE",null,"DALI",">110 000h",2,"Oprawa słupowa (nasadzana).","Światło symetryczne o kącie 30D","30D","A mounting luminaire with a contemporary design, for mounting on a lighting pole with a base of Ø60mm",null,null,null,"Profil aluminiowy wyciskany, malowany proszkowo.",null,"Klosz- szkło bezpieczne, przeźroczyste.","Uszczelka silikonowa.","Dławnica EPDM.","Pojedyncza","szerokie jednostronne","Sterowanie światłem w systemie: DALI outdoor pełny program. Zasilacz zaprogramowany na max prąd. Programowanie pozostałych parametrów po uzgodnieniu z Działem Handlowym firmy Norlys.","Moduł LED","Philips Fortimo SLM C 1208 L15 2024 G7 3K","Philips Xi FP 22W 0,2-0,7A SNLDAE 230V C123 sXt 12NC: 929002165006",100000,"DALI2 / NightDim (4DIM)",null,80,"D","7661ZX0010, 7662ZX0009","Przewód H05VV-F 5G1 o długości 6,5m do podłączenia wewnątrz słupa oświetleniowego (w odpowiednio dobranej puszcze elektroinstalacyjnej).","6460XX0009.png","6460XX0009.ldt",3,null,1,77]
["6461","6461XX0009","MORA POLE-TOP LED 2601LM DOWN 4000K DALI2","Mora","Pole","Aluminium",null,null,null,"LED zintegrowane","AC","DALI2","14,7W","17,6W","2601lm","1735lm",null,null,"65","IK08","Class I",4000,"szerokie dół",0.46,0.15,0.27,"CE",null,"DALI",">110 000h",2,"Oprawa słupowa (nasadzana).","Światło symetryczne o kącie 30D","30D","A mounting luminaire with a contemporary design, for mounting on a lighting pole with a base of Ø60mm",null,null,null,"Profil aluminiowy wyciskany, malowany proszkowo.",null,"Klosz- szkło bezpieczne, przeźroczyste.","Uszczelka silikonowa.","Dławnica EPDM.","Pojedyncza","szerokie jednostronne","Sterowanie światłem w systemie: DALI outdoor pełny program. Zasilacz zaprogramowany na max prąd. Programowanie pozostałych parametrów po uzgodnieniu z Działem Handlowym firmy Norlys.","Moduł LED","Philips Fortimo SLM C 1208 L15 2024 G7 4K","Philips Xi FP 22W 0,2-0,7A SNLDAE 230V C123 sXt 12NC: 929002165006",100000,"DALI2 / NightDim (4DIM)",null,80,"D","7661ZX0010, 7662ZX0009","Przewód H05VV-F 5G1 o długości 6,5m do podłączenia wewnątrz słupa oświetleniowego (w odpowiednio dobranej puszcze elektroinstalacyjnej).","6461XX0009.png","6461XX0009.ldt",3,null,1,77]
["6466","6466XX0009","MORA POLE-TOP LED 5002LM DOWN 3000K DALI2","Mora","Pole","Aluminium",null,null,null,"LED zintegrowane","AC","DALI2","29,4W","33,9W","5002lm","3229lm",null,null,"65","IK08","Class I",3000,"szerokie dół",0.85,0.15,0.27,"CE",null,"DALI",">110 000h",2,"Oprawa słupowa (nasadzana).","Światło symetryczne o kącie 30D","30D","A mounting luminaire with a contemporary design, for mounting on a lighting pole with a base of Ø60mm",null,null,null,"Profil aluminiowy wyciskany, malowany proszkowo.",null,"Klosz- szkło bezpieczne, przeźroczyste.","Uszczelka silikonowa.","Dławnica EPDM.","Podwójna","szerokie jednostronne","Sterowanie światłem w systemie: DALI outdoor pełny program. Zasilacz zaprogramowany na max prąd. Programowanie pozostałych parametrów po uzgodnieniu z Działem Handlowym firmy Norlys.","Moduł LED","Philips Fortimo SLM C 1208 L15 2024 G7 3K","Philips Xi FP 75W 0,2-0,7A SNLDAE 230V C133 sXt kod. 929002101406",100000,"DALI2 / NightDim (4DIM)",null,80,"D","7661ZX0010, 7662ZX0009","Przewód H05VV-F 5G1 o długości 6,5m do podłączenia wewnątrz słupa oświetleniowego (w odpowiednio dobranej puszcze elektroinstalacyjnej).","6466XX0009.png","6466XX0009.ldt",3,null,1,77]
["6467","6467XX0009","MORA POLE-TOP LED 5202LM DOWN 4000K DALI2","Mora","Pole","Aluminium",null,null,null,"LED zintegrowane","AC","DALI2","29,4W","33,5W","5202lm","3437lm",null,null,"65","IK08","Class I",4000,"szerokie dół",0.85,0.15,0.27,"CE",null,"DALI",">110 000h",2,"Oprawa słupowa (nasadzana).","Światło symetryczne o kącie 30D","30D","A mounting luminaire with a contemporary design, for mounting on a lighting pole with a base of Ø60mm",null,null,null,"Profil aluminiowy wyciskany, malowany proszkowo.",null,"Klosz- szkło bezpieczne, przeźroczyste.","Uszczelka silikonowa.","Dławnica EPDM.","Podwójna","szerokie jednostronne","Sterowanie światłem w systemie: DALI outdoor pełny program. Zasilacz zaprogramowany na max prąd. Programowanie pozostałych parametrów po uzgodnieniu z Działem Handlowym firmy Norlys.","Moduł LED","Philips Fortimo SLM C 1208 L15 2024 G7 4K","Philips Xi FP 75W 0,2-0,7A SNLDAE 230V C133 sXt kod. 929002101406",100000,"DALI2 / NightDim (4DIM)",null,80,"D","7661ZX0010, 7662ZX0009","Przewód H05VV-F 5G1 o długości 6,5m do podłączenia wewnątrz słupa oświetleniowego (w odpowiednio dobranej puszcze elektroinstalacyjnej).","6467XX0009.png","6467XX0009.ldt",3,null,1,77]
["6471","6471XX0009","MOSS LED 840LM 36D 3000K DIM.","Moss,Move","Spot,Ground","Aluminium",null,null,null,"LED zintegrowane","AC","DIM.","8W","8W","840lm","686lm",null,null,"65",null,"Class I",3000,null,0,0,0,"CE",null,null,"> 50 000h",40,"Oprawa typu reflektor, przenośna.","Światło symetryczne o kącie 36D","36D","For illuminating gardens, private areas and other concepts architectural. Possibility to adjust the direction of light also in the vertical plane",null,null,null,"Odlew aluminiowy malowany proszkowo.",null,"Klosz- szkło bezpieczne, przeźroczyste.",null,null,"Triac",null,"Oprawa ściemnialna fazowo TRAILING EDGE (TE) - LEADING EDGE (LE)","Moduł LED","Lumens EDC 38C 8W xxx 230V A101 3K",null,0,"Ściemnianie fazowe Lumens LED AC",null,80,"E","145ZX0009, 4701420002","Oprawa wyposażona w przewód typu H05RN-F 3G1 o długości 5 m. zakończony wtyczką 16A 250V 2P+Z IP65","6471XX0009.png","6471XX0009.ldt",1,null,4,68]
["6473","6473XX0009","MOSS LED 439LM 36D 3000K DIM.","Moss,Move","Spot,Ground","Aluminium",null,null,null,"LED zintegrowane","AC","DIM.","4W","4W","439lm","389Mlm",null,null,"65",null,"Class I",3000,null,null,null,null,"CE",null,null,"> 50 000h",40,"Oprawa typu reflektor, przenośna.","Światło symetryczne o kącie 36D","36D","For illuminating gardens, private areas and other architectural concepts. Possibility to adjust the direction of light also in the vertical plane.",null,null,null,"Odlew aluminiowy malowany proszkowo.",null,"Klosz- szkło bezpieczne, przeźroczyste.",null,null,"Triac",null,"Oprawa ściemnialna fazowo TRAILING EDGE (TE) - LEADING EDGE (LE)","Moduł LED","Lumens EDC 38C 8W xxx 230V A101 3K",null,0,"Ściemnianie fazowe Lumens LED AC",null,80,"E",null,"Oprawa wyposażona w przewód typu H05RN-F 3G1 o długości 5 m. zakończony wtyczką 16A 250V 2P+Z IP65","6473XX0009.png","6473XX0009.ldt",1,null,4,68]
["6483","6483XX0009","MOSS LED 840LM 36D 3000K DIM.","Moss,Move","Spot,Ground","Aluminium",null,null,null,"LED zintegrowane","AC","DIM.","8W","8W","840lm","686lm",null,null,"65",null,"Class I",3000,null,0.22,0.2,1.19,"CE",null,null,"> 50 000h",40,"Oprawa typu reflektor, przenośna.","Światło symetryczne o kącie 36D","36D","For illuminating gardens, private areas and other concepts architectural. Possibility to adjust the direction of light also in the vertical plane",null,null,null,"Odlew aluminiowy malowany proszkowo.",null,"Klosz- szkło bezpieczne, przeźroczyste.",null,"Stal nierdzewna.","Triac","Stal nierdzewna","Oprawa ściemnialna fazowo TRAILING EDGE (TE) - LEADING EDGE (LE)","Moduł LED","Lumens EDC 38C 8W xxx 230V A101 3K",null,0,"Ściemnianie fazowe Lumens LED AC",null,80,"E","145ZX0009, 4701420002","Oprawa wyposażona w przewód typu H05RN-F 3G1 o długości 5 m. zakończony wtyczką 16A 250V 2P+Z IP65","6483XX0009.png","6483XX0009.ldt",1,null,4,68]
["6485","6485XX0009","MOSS LED 439LM 36D 3000K DIM.","Moss,Move","Spot,Ground","Aluminium",null,null,null,"LED zintegrowane","AC","DIM.","4W","4W","439lm","389Mlm",null,null,"65",null,"Class I",3000,null,0.22,0.2,1.19,"CE",null,null,"> 50 000h",40,"Oprawa typu reflektor, przenośna.","Światło symetryczne o kącie 36D","36D","For illuminating gardens, private areas and other concepts architectural. Possibility to adjust the direction of light also in the vertical plane",null,null,null,"Odlew aluminiowy malowany proszkowo.",null,"Klosz- szkło bezpieczne, przeźroczyste.",null,"Stal nierdzewna.","Triac","Stal nierdzewna","Oprawa ściemnialna fazowo TRAILING EDGE (TE) - LEADING EDGE (LE)","Moduł LED","Lumens EDC 38C 4W xxx 230V A101 3K",null,0,"Ściemnianie fazowe Lumens LED AC",null,80,"E",null,"Oprawa wyposażona w przewód typu H05RN-F 3G1 o długości 5 m. zakończony wtyczką 16A 250V 2P+Z IP65","6485XX0009.png","6485XX0009.ldt",1,null,4,68]
["655","655XX0013","BERN WALL LED 667LM 3000K DIM.","Bern","Wall","Stal",null,null,null,"LED zintegrowane","AC","DIM.","3,9W","5,2W","667lm","477lm",null,null,"54","IK07","Class I",3000,null,0.24,0.24,0.12,"CE",null,null,"> 72 000h",12,"Oprawa ścienna.","Światło rozproszone.",null,"A ceiling-type luminaire with a contemporary design",null,null,null,null,"Front- stal nierdzewna, stal cynkowana ogniowo, stal malowana proszkowo.","Klosz- szkło bezpieczne, satynowane.","Uszczelka silikonowa.","Podstawa- odlew aluminiowy malowany proszkowo.",null,"satynowany","Oprawa ściemnialna fazowo TRAILING EDGE (TE)","Moduł LED","Philips Fortimo_LED_Strip_0.5ft_MF_8xx_HV6 3K","Philips Xitanium 7W 0,35A 20V TE SC 230V [2017]",50000,"Philips Xitanium TE",null,80,"D",null,"Zaciski podłączeniowe: max 3x2,5mm², możliwość podłączenia oprawy w pętle max 3x1,5mm². Przewód w oponie okrągłej o średnicy ø7...10,5mm.","655XX0013.jpg","655XX0013.ldt",1,null,1,7]
["6600","6600XX0009","MOSS FLOODLIGHT-EARTHSPIKE LED 840LM 36D 3000K DIM.","Moss,Move","Spot,Ground","Aluminium",null,null,null,"LED zintegrowane","AC","DIM.","8W","8W","840lm","686lm",null,null,"65",null,"Class I",3000,null,0,0,0,"CE",null,null,"> 50 000h",17,"Oprawa typu reflektor, przenośna gruntowa.","Światło symetryczne o kącie 36D","36D","For illuminating gardens, private areas and other concepts architectural. Possibility to adjust the direction of light also in the vertical plane",null,null,null,"Odlew aluminiowy malowany proszkowo.",null,"Klosz- szkło bezpieczne, przeźroczyste.",null,"Stal nierdzewna.","Triac",null,"Oprawa ściemnialna fazowo TRAILING EDGE (TE) - LEADING EDGE (LE)","Moduł LED","Lumens EDC 38C 8W xxx 230V A101 3K",null,0,"Ściemnianie fazowe Lumens LED AC",null,80,"E","145ZX0009, 4701420002","Oprawa wyposażona w przewód typu H05RN-F 3G1 o długości 3 m. Do podłączenia w odpowiednio dobranej puszce elektroinstalacyjnej.","6600XX0009.png","6600XX0009.ldt",1,null,4,68]
["6601","6601XX0009","MOSS FLOODLIGHT-EARTHSPIKE LED 891LM 36D 4000K DIM.","Moss,Move","Spot,Ground","Aluminium",null,null,null,"LED zintegrowane","AC","DIM.","8W","8W","891lm","749lm",null,null,"65",null,"Class I",4000,null,0,0,0,"CE",null,null,"> 50 000h",17,"Oprawa typu reflektor, przenośna gruntowa.","Światło symetryczne o kącie 36D","36D","For illuminating gardens, private areas and other concepts architectural. Possibility to adjust the direction of light also in the vertical plane",null,null,null,"Odlew aluminiowy malowany proszkowo.",null,"Klosz- szkło bezpieczne, przeźroczyste.",null,"Stal nierdzewna.","Triac",null,"Oprawa ściemnialna fazowo TRAILING EDGE (TE) - LEADING EDGE (LE)","Moduł LED","Lumens EDC 38C 8W xxx 230V A101 4K",null,0,"Ściemnianie fazowe Lumens LED AC",null,80,"E","145ZX0009, 4701420002","Oprawa wyposażona w przewód typu H05RN-F 3G1 o długości 3 m. Do podłączenia w odpowiednio dobranej puszce elektroinstalacyjnej.","6601XX0009.png","6601XX0009.ldt",1,null,4,68]
["6602","6602XX0009","MOSS FLOODLIGHT-EARTHSPIKE LED 439LM 36D 3000K DIM.","Moss,Move","Spot,Ground","Aluminium",null,null,null,"LED zintegrowane","AC","DIM.","4W","4W","439lm","389lm",null,null,"65",null,"Class I",3000,null,0,0,0,"CE",null,null,"> 50 000h",17,"Oprawa typu reflektor, przenośna gruntowa.","Światło symetryczne o kącie 36D","36D","For lighting gardens, private areas and other architectural concepts. The light direction can also be adjusted in the vertical plane",null,null,null,"Odlew aluminiowy malowany proszkowo.",null,"Klosz- szkło bezpieczne, przeźroczyste.",null,null,"Triac",null,"Oprawa ściemnialna fazowo TRAILING EDGE (TE) - LEADING EDGE (LE)","Moduł LED","Lumens EDC 38C 4W xxx 230V A101 3K",null,0,"Ściemnianie fazowe Lumens LED AC",null,80,"E","145ZX0009, 146ZX0009","Oprawa wyposażona w przewód typu H05RN-F 3G1 o długości 3 m. Do podłączenia w odpowiednio dobranej puszce elektroinstalacyjnej.","6602XX0009.png","6602XX0009.ldt",1,null,4,68]
["6603","6603XX0009","MOSS FLOODLIGHT-EARTHSPIKE LED 466LM 36D 4000K DIM.","Moss,Move","Spot,Ground","Aluminium",null,null,null,"LED zintegrowane","AC","DIM.","4W","4W","466lm","414lm",null,null,"65",null,"Class I",4000,null,0,0,0,"CE",null,null,"> 50 000h",17,"Oprawa typu reflektor, przenośna gruntowa.","Światło symetryczne o kącie 36D","36D","For illuminating gardens, private areas and other architectural concepts. Possibility to adjust the direction of light also in the vertical plane.",null,null,null,"Odlew aluminiowy malowany proszkowo.",null,"Klosz- szkło bezpieczne, przeźroczyste.",null,null,"Triac",null,"Oprawa ściemnialna fazowo TRAILING EDGE (TE) - LEADING EDGE (LE)","Moduł LED","Lumens EDC 38C 4W xxx 230V A101 4K",null,0,"Ściemnianie fazowe Lumens LED AC",null,80,"E","145ZX0009, 146ZX0009","Oprawa wyposażona w przewód typu H05RN-F 3G1 o długości 3 m. Do podłączenia w odpowiednio dobranej puszce elektroinstalacyjnej.","6603XX0009.png","6603XX0009.ldt",1,null,4,68]
["660","660XX0009","BASEL WALL E27","Basel","Wall","Stal",null,null,null,"Wymienne","E27",null,"LED max 9W","LED max 9W",null,null,null,null,"54","IK07","Class I",null,null,0.21,0.13,0.31,"CE",null,null,null,12,"Oprawa ścienna.","Światło odkryte.",null,"Modern design plafon type luminaire.",null,null,"Oprawa na wymienne źródło światła typu: lampa LED, świetlówka TC-SE, tradycyjna żarówka (halogenowa) o trzonku E27. Źródło światła należy dokupić oddzielnie.",null,"Front- stal nierdzewna, stal cynkowana ogniowo, stal malowana proszkowo.","Klosz- szkło bezpieczne, przeźroczyste.","Uszczelka silikonowa.","Podstawa- odlew aluminiowy malowany proszkowo.","NIE","przeźroczysty",null,"Lampa E27","LED A55..60",null,0,null,null,80,null,"46999021","Zaciski podłączeniowe: max 3x2,5mm², możliwość podłączenia oprawy w pętle max 3x1,5mm². Przewód w oponie okrągłej o średnicy ø7...10,5mm.","660XX0009.jpg","660XX0009.ldt",4,"E27",1,9]
["661","661XX0009","BASEL WALL E27","Basel","Wall","Stal",null,null,null,"Wymienne","E27",null,"LED max 9W","LED max 9W",null,null,null,null,"54","IK07","Class I",null,null,0.21,0.13,0.31,"CE",null,null,null,12,"Oprawa ścienna.","Światło rozproszone.",null,"Modern design plafon type luminaire","A ceiling-type luminaire with a classic design Functions: control, color change 2700K…6500K (TW), WiZ, WiZ Pro - Available after mounting in the luminaire, Signify WiZ Pro A60 E27 TW 8W 230V - Full control of the luminaire after installing the free application https://pro.wizconnected.com/ - Technical support: Information Sales Department of Norlys",null,null,null,"Front- stal nierdzewna, stal cynkowana ogniowo, stal malowana proszkowo.","Klosz- szkło bezpieczne, satynowane.","Uszczelka silikonowa.","Podstawa- odlew aluminiowy malowany proszkowo.","NIE","satynowany",null,"Lampa E27","LED A55..60",null,0,null,null,80,null,null,"Zaciski podłączeniowe: max 3x2,5mm², możliwość podłączenia oprawy w pętle max 3x1,5mm². Przewód w oponie okrągłej o średnicy ø7...10,5mm.","661XX0009.jpg","661XX0009.ldt",4,"E27",1,7]
["668","668XX0013","BASEL WALL LED 667LM 3000K DIM. TE","Basel","Wall","Stal",null,null,null,"LED zintegrowane","AC","DIM. TE","3,9W","5,2W","667lm","483lm",null,null,"54","IK07","Class I",3000,null,null,null,null,"CE",null,null,"> 70 000",12,"Oprawa ścienna.","Światło rozproszone.",null,"Modern design plafon type luminaire",null,null,null,null,"Front- stal nierdzewna, stal cynkowana ogniowo, stal malowana proszkowo.","Klosz- szkło bezpieczne, satynowane.","Uszczelka silikonowa.","Podstawa- odlew aluminiowy malowany proszkowo.","NIE","satynowany","Oprawa ściemnialna fazowo TRAILING EDGE (TE)","Moduł LED","Philips Fortimo_LED_Strip_0.5ft_MF_8xx_HV6 3K","Philips Xitanium 7W 0,35A 20V TE SC 230V [2017]",50000,null,null,80,"C",null,"Zaciski podłączeniowe: max 3x2,5mm², możliwość podłączenia oprawy w pętle max 3x1,5mm². Przewód w oponie okrągłej o średnicy ø7...10,5mm.","668XX0013.jpg","668XX0013.ldt",1,null,1,7]
["6702","6702XX0309","MOSS FLOODLIGHT-BOX LED 840LM 36º 3000K DIM.","Moss,Arm","Spot,Wall","Aluminium",null,null,null,"LED zintegrowane","AC","DIM.","8W","8W","840lm","686lm",null,null,"65",null,"Class I",3000,null,0,0,0,"CE",null,null,">50 000h",4,"Oprawa typu reflektor.","Światło symetryczne o kącie 36 stopni.","36º","For lighting gardens, private areas and other architectural concepts. Possibility to adjust the lighting direction also in the vertical plane.",null,null,null,"Odlew aluminiowy malowany proszkowo.",null,"Klosz- szkło bezpieczne, przeźroczyste.",null,null,"ramię długie",null,"Oprawa ściemnialna fazowo TRAILING EDGE (TE) - LEADING EDGE (LE)","Moduł LED","Lumens EDC 38C 8W xxx 230V A101 3K",null,0,"Ściemnianie fazowe Lumens LED AC",null,80,"E","145ZX0009, 4701420002, 6729XX0009","Oprawa wyposażona w przewód typu H05RN-F 3G1 o długości 3 m. Do podłączenia w odpowiednio dobranej puszce elektroinstalacyjnej.","6702XX0309.png","6702XX0309.ldt",1,null,4,35]
["6706","6706XX0309","MOSS FLOODLIGHT-BOX LED 438LM 36D 3000K DIM.","Moss,Arm","Spot,Wall","Aluminium",null,null,null,"LED zintegrowane","AC","DIM.","4W","4W","438lm","389lm",null,null,"65",null,"Class I",3000,null,0,0,0,"CE",null,null,">50 000h",4,"Oprawa typu reflektor.","Światło symetryczne o kącie 36D","36D","For lighting gardens, private areas and other architectural concepts. Possibility to adjust the lighting direction also in the vertical plane.",null,null,null,"Odlew aluminiowy malowany proszkowo.",null,"Klosz- szkło bezpieczne, przeźroczyste.",null,null,"ramię długie",null,"Oprawa ściemnialna fazowo TRAILING EDGE (TE) - LEADING EDGE (LE)","Moduł LED","Lumens EDC 38C 4W xxx 230V A101 3K",null,0,"Ściemnianie fazowe Lumens LED AC",null,80,"E","145ZX0009, 4701420002, 6729XX0009","Oprawa wyposażona w przewód typu H05RN-F 3G1 o długości 3 m. Do podłączenia w odpowiednio dobranej puszce elektroinstalacyjnej.","6706XX0309.png","6706XX0309.ldt",1,null,4,68]
["6732","6732XX0309","MOSS FLOODLIGHT-BOX LED 439LM 36D 3000K DIM.","Moss","Spot,Ø50 pipe","Aluminium",null,null,null,"LED zintegrowane","AC","DIM.","4W","4W","439lm","389lm",null,null,"65",null,"Class I",3000,null,0,0,0,"CE",null,null,"> 50 000h",4,"Oprawa typu reflektor.","Światło symetryczne o kącie 36D","36D","For illuminating gardens, private areas and other architectural concepts. Possibility to adjust the direction of light also in the vertical plane.",null,null,null,"Odlew aluminiowy malowany proszkowo.",null,"Klosz- szkło bezpieczne, przeźroczyste.",null,null,"Ø50",null,"Oprawa ściemnialna fazowo TRAILING EDGE (TE) - LEADING EDGE (LE)","Moduł LED","Lumens EDC 38C 4W xxx 230V A101 3K",null,0,"Ściemnianie fazowe Lumens LED AC",null,80,"E","145ZX0009, 4701420002","Przewód H05RN-F 3G1 o długości 3m do podłączenia w odpowiednio dobranej puszce elektroinstalacyjnej.","6732XX0309.png","6732XX0309.ldt",1,null,4,68]
["6735","6735XX0309","MOSS FLOODLIGHT-BOX LED 439LM 36D 3000K DIM.","Moss","Spot,Ø60 pipe","Aluminium",null,null,null,"LED zintegrowane","AC","DIM.","4W","4W","439lm","389lm",null,null,"65",null,"Class I",3000,null,0,0,0,"CE",null,null,"> 50 000h",4,"Oprawa typu reflektor.","Światło symetryczne o kącie 36D","36D","For illuminating gardens, private areas and other architectural concepts. Possibility to adjust the direction of light also in the vertical plane.",null,null,null,"Odlew aluminiowy malowany proszkowo.",null,"Klosz- szkło bezpieczne, przeźroczyste.",null,null,"Ø60",null,"Oprawa ściemnialna fazowo TRAILING EDGE (TE) - LEADING EDGE (LE)","Moduł LED","Lumens EDC 38C 4W xxx 230V A101 3K",null,0,"Ściemnianie fazowe Lumens LED AC",null,80,"E","145ZX0009, 4701420002","Przewód H05RN-F 3G1 o długości 3m do podłączenia w odpowiednio dobranej puszce elektroinstalacyjnej.","6735XX0309.png","6735XX0309.ldt",1,null,4,68]
["6738","6738XX0309","MOSS FLOODLIGHT-BOX LED 439LM 36D 3000K DIM.","Moss","Spot,Ø76 pipe","Aluminium",null,null,null,"LED zintegrowane","AC","DIM.","4W","4W","439lm","389lm",null,null,"65",null,"Class I",3000,null,0,0,0,"CE",null,null,"> 50 000h",4,"Oprawa typu reflektor.","Światło symetryczne o kącie 36D","36D","For illuminating gardens, private areas and other architectural concepts. Possibility to adjust the direction of light also in the vertical plane.",null,null,null,"Odlew aluminiowy malowany proszkowo.",null,"Klosz- szkło bezpieczne, przeźroczyste.",null,null,"Ø76",null,"Oprawa ściemnialna fazowo TRAILING EDGE (TE) - LEADING EDGE (LE)","Moduł LED","Lumens EDC 38C 4W xxx 230V A101 3K",null,0,"Ściemnianie fazowe Lumens LED AC",null,80,"E","145ZX0009, 4701420002","Przewód H05RN-F 3G1 o długości 3m do podłączenia w odpowiednio dobranej puszce elektroinstalacyjnej.","6738XX0309.png","6738XX0309.ldt",1,null,4,68]
["6750","6750XX0309","MOSS FLOODLIGHT-BOX LED 840LM 36D 3000K DIM.","Moss","Spot,Ø50 pipe","Aluminium",null,null,null,"LED zintegrowane","AC","DIM.","8W","8W","840lm","686lm",null,null,"65",null,"Class I",3000,null,0,0,0,"CE",null,null,"> 50 000h",4,"Oprawa typu reflektor.","Światło symetryczne o kącie 36D","36D","For illuminating gardens, private areas and other architectural concepts. Possibility to adjust the direction of light also in the vertical plane.",null,null,null,"Odlew aluminiowy malowany proszkowo.",null,"Klosz- szkło bezpieczne, przeźroczyste.",null,null,"Ø50",null,"Oprawa ściemnialna fazowo TRAILING EDGE (TE) - LEADING EDGE (LE)","Moduł LED","Lumens EDC 38C 8W xxx 230V A101 3K",null,0,"Ściemnianie fazowe Lumens LED AC",null,80,"E","145ZX0009, 4701420002","Przewód H05RN-F 3G1 o długości 3m do podłączenia w odpowiednio dobranej puszce elektroinstalacyjnej.","6750XX0309.png","6750XX0309.ldt",1,null,4,68]
["6753","6753XX0309","MOSS FLOODLIGHT-BOX LED 840LM 36D 3000K DIM.","Moss","Spot,Ø60 pipe","Aluminium",null,null,null,"LED zintegrowane","AC","DIM.","8W","8W","840lm","686lm",null,null,"65",null,"Class I",3000,null,0,0,0,"CE",null,null,"> 50 000h",4,"Oprawa typu reflektor.","Światło symetryczne o kącie 36D","36D","For illuminating gardens, private areas and other architectural concepts. Possibility to adjust the direction of light also in the vertical plane.",null,null,null,"Odlew aluminiowy malowany proszkowo.",null,"Klosz- szkło bezpieczne, przeźroczyste.",null,null,"Ø60",null,"Oprawa ściemnialna fazowo TRAILING EDGE (TE) - LEADING EDGE (LE)","Moduł LED","Lumens EDC 38C 8W xxx 230V A101 3K",null,0,"Ściemnianie fazowe Lumens LED AC",null,80,"E","145ZX0009, 4701420002","Przewód H05RN-F 3G1 o długości 3m do podłączenia w odpowiednio dobranej puszce elektroinstalacyjnej.","6753XX0309.png","6753XX0309.ldt",1,null,4,68]
["6756","6756XX0309","MOSS FLOODLIGHT-BOX LED 840LM 36D 3000K DIM.","Moss","Spot,Ø76 pipe","Aluminium",null,null,null,"LED zintegrowane","AC","DIM.","8W","8W","840lm","686lm",null,null,"65",null,"Class I",3000,null,0,0,0,"CE",null,null,"> 50 000h",4,"Oprawa typu reflektor.","Światło symetryczne o kącie 36D","36D","For illuminating gardens, private areas and other architectural concepts. Possibility to adjust the direction of light also in the vertical plane.",null,null,null,"Odlew aluminiowy malowany proszkowo.",null,"Klosz- szkło bezpieczne, przeźroczyste.",null,null,"Ø76",null,"Oprawa ściemnialna fazowo TRAILING EDGE (TE) - LEADING EDGE (LE)","Moduł LED","Lumens EDC 38C 8W xxx 230V A101 3K",null,0,"Ściemnianie fazowe Lumens LED AC",null,80,"E","145ZX0009, 4701420002","Przewód H05RN-F 3G1 o długości 3m do podłączenia w odpowiednio dobranej puszce elektroinstalacyjnej.","6756XX0309.png","6756XX0309.ldt",1,null,4,68]
["675","675XX0009","BERN WALL LED 1080LM 3000K MD","Bern","Wall,Ceiling","Stal",null,null,null,"LED zintegrowane","AC","MD","9,5W","11,2W","1080lm","819lm",null,null,"54","IK07","Class I",3000,null,0.24,0.12,0.24,"CE","Daylight sensor,Motion sensor",null,"50 000h",12,"Oprawa ścienna.","Światło rozproszone.",null,"A ceiling-type luminaire with a contemporary design",null,null,null,null,"Front- stal nierdzewna, stal cynkowana ogniowo, stal malowana proszkowo.","Klosz- szkło bezpieczne, satynowane.","Uszczelka silikonowa.","Podstawa- odlew aluminiowy malowany proszkowo.",null,"satynowany","Oprawa wyposażona w mikrofalowy czujnik ruchu, z wyłącznikiem zmierzchowym i podtrzymaniem ruchu","Moduł LED","Philips Fortimo DLM ES 1100/8xx G2 3K",null,0,"Mikrofalowy czujnik ruchu MD (PD-MV1005)",null,80,"E",null,"Zaciski podłączeniowe: max 3x2,5mm², możliwość podłączenia oprawy w pętle max 3x1,5mm². Przewód w oponie okrągłej o średnicy ø7...10,5mm.","675XX0009.jpg","675XX0009.ldt",3,null,1,7]
["676","676XX0009","BERN WALL LED 1150LM 4000K MD","Bern","Wall","Stal",null,null,null,"LED zintegrowane","AC","MD","9,5W","11,2W","1150lm","878lm",null,null,"54","IK07","Class I",4000,null,0.24,0.12,0.24,"CE","Daylight sensor,Motion sensor",null,"50 000h",12,"Oprawa ścienna.","Światło rozproszone.",null,"A ceiling-type luminaire with a contemporary design",null,null,null,null,"Front- stal nierdzewna, stal cynkowana ogniowo, stal malowana proszkowo.","Klosz- szkło bezpieczne, satynowane.","Uszczelka silikonowa.","Podstawa- odlew aluminiowy malowany proszkowo.",null,"satynowany","Oprawa wyposażona w mikrofalowy czujnik ruchu, z wyłącznikiem zmierzchowym i podtrzymaniem ruchu","Moduł LED","Philips Fortimo DLM ES 1100/8xx G2 4K",null,0,"Mikrofalowy czujnik ruchu MD (PD-MV1005)",null,80,"D",null,"Zaciski podłączeniowe: max 3x2,5mm², możliwość podłączenia oprawy w pętle max 3x1,5mm². Przewód w oponie okrągłej o średnicy ø7...10,5mm.","676XX0009.jpg","676XX0009.ldt",3,null,1,7]
["6772","6772XX0309","MOSS FLOODLIGHT-BOX LED 840LM 36D 3000K DIM.","Moss","Spot,Wall","Aluminium",null,null,null,"LED zintegrowane","AC","DIM.","8W","8W","840lm","686lm",null,null,"65",null,"Class I",3000,null,0,0,0,"CE",null,null,"59 000h",4,"Oprawa typu reflektor.","Światło symetryczne o kącie 36D","36D","For illuminating gardens, private areas and other architectural concepts. Possibility to adjust the direction of light also in the vertical plane.",null,null,null,"Odlew aluminiowy malowany proszkowo.",null,"Klosz- szkło bezpieczne, przeźroczyste.",null,null,"ramię krótkie",null,"Oprawa ściemnialna fazowo TRAILING EDGE (TE) - LEADING EDGE (LE)","Moduł LED","Lumens EDC 38C 8W xxx 230V A101 [2022] 3K",null,0,"Ściemnianie fazowe Lumens LED AC",null,80,"E","145ZX0009, 4701420002","Oprawa wyposażona w przewód typu H05RN-F 3G1 o długości 3 m. Do podłączenia w odpowiednio dobranej puszce elektroinstalacyjnej.","6772XX0309.png","6772XX0309.ldt",1,null,4,68]
["6778","6778XX0309","MOSS FLOODLIGHT-BOX LED 438LM 36D 3000K DIM.","Moss","Spot,Wall","Aluminium",null,null,null,"LED zintegrowane","AC","DIM.","4W","4W","438lm","389lm",null,null,"65",null,"Class I",3000,null,0,0,0,"CE",null,null,"59 000h",4,"Oprawa typu reflektor.","Światło symetryczne o kącie 36D","36D","For illuminating gardens, private areas and other architectural concepts. Possibility to adjust the direction of light also in the vertical plane.",null,null,null,"Odlew aluminiowy malowany proszkowo.",null,"Klosz- szkło bezpieczne, przeźroczyste.",null,null,"ramię krótkie",null,"Oprawa ściemnialna fazowo TRAILING EDGE (TE) - LEADING EDGE (LE)","Moduł LED","Lumens EDC 38C 4W xxx 230V A101 [2022] 3K",null,0,"Ściemnianie fazowe Lumens LED AC",null,80,"E","145ZX0009, 4701420002","Oprawa wyposażona w przewód typu H05RN-F 3G1 o długości 3 m. Do podłączenia w odpowiednio dobranej puszce elektroinstalacyjnej.","6778XX0309.png","6778XX0309.ldt",1,null,4,68]
["7120","7120XX0011","NORDLAND CEILING/WALL 2XLED E27","Nordland","Wall,Ceiling","Aluminium",null,null,null,"Wymienne","E27",null,"LED 2 x max 9W","LED 2 x max 9W",null,null,null,null,"65","IK10","Class I",null,null,0.28000000000000003,0.28000000000000003,0.1,"CE",null,null,null,7,"Oprawa sufitowo-ścienna.","Światło rozproszone.",null,"A ceiling luminaire with a modern design For lighting private areas and other architectural concepts",null,null,null,"Odlew aluminiowy malowany proszkowo.",null,"Klosz- poliwęglan mleczny, stabilizowany UV.","Uszczelka silikonowa.","Dławnica EPDM.","NIE",null,null,"2 Lampy LED E27","LED A55..60",null,0,null,null,80,null,"46999021","Zaciski podłączeniowe: max 3x2,5mm², możliwość podłączenia oprawy w pętle max 3x1,5mm². Przewód w oponie okrągłej o średnicy ø7...10,5mm.","7120XX0011.jpg","7120XX0011.ldt",4,"E27",1,7]
["7150","7150XX0009","VARBERG LED T4-B 3000K DALI2","Varberg","Ground,Ground/Wall","Aluminium","Malowane",null,"PRO","LED zintegrowane","AC","DALI2","26,9W","30W",null,"3621lm",null,null,"65","IK10","Class I",3000,"szerokie góra",null,null,null,"CE",null,"DALI","> 100 000h",50,"Oprawa typu naświetlacz","Soczewka firmy Ledil typu T4-B (IESNA typ IV).","T4-B","For illuminating building facades, gardens, private areas and other architectural concepts. Possibility to adjust the direction of light also in the vertical plane. The luminaire is also suitable for direct voltage: DC 168 ÷ 275 V",null,"DC",null,"Profil aluminiowy wyciskany, malowany proszkowo.",null,"Soczewka hermetyczna zewnętrzna- tworzywo sztuczne PC przeźroczyste.",null,"Dławnica mosiężna niklowana.",null,"DALI2 / NightDim","Sterowanie światłem w systemie: DALI outdoor pełny program. Zasilacz zaprogramowany na max prąd. Programowanie pozostałych parametrów po uzgodnieniu z Działem Handlowym firmy Norlys.","Moduł LED","Philips Fortimo FastFlex LED 2x6 DP G5 3K","Philips Xi FP 40W 0,3-1,0A SNLDAE 230V C123 sXt 929002165306",0,"DALI2 / NightDim (XI FP NLD)",null,70,"D",null,"Oprawa wyposażona w przewód typu H07RN-F 5G1 Do podłączenia w odpowiednio dobranej puszce elektroinstalacyjnej.","7150XX0009.png","7150XX0009.ldt",3,null,1,64]
["7151","7151XX0009","VARBERG LED T4-B 4000K DALI2","Varberg","Ground,Ground/Wall","Aluminium","Malowane",null,"PRO","LED zintegrowane","AC","DALI2","26,9W","30W",null,"3843lm",null,null,"65","IK10","Class I",4000,"szerokie góra",null,null,null,"CE",null,"DALI","> 100 000h",50,"Oprawa typu naświetlacz","Soczewka firmy Ledil typu T4-B (IESNA typ IV).","T4-B","Luminaire for illuminating facades, gardens, private areas and other architectural concepts. Possibility to adjust the direction of light also in the vertical plane. The luminaire is also suitable for direct voltage: DC 168 ÷ 275 V",null,"DC",null,"Profil aluminiowy wyciskany, malowany proszkowo.",null,"Soczewka hermetyczna zewnętrzna- tworzywo sztuczne PC przeźroczyste.",null,"Dławnica mosiężna niklowana.",null,"DALI2 / NightDim","Sterowanie światłem w systemie: DALI outdoor pełny program. Zasilacz zaprogramowany na max prąd. Programowanie pozostałych parametrów po uzgodnieniu z Działem Handlowym firmy Norlys.","Moduł LED","Philips Fortimo FastFlex LED 2x6 DP G5 4K","Philips Xi FP 40W 0,3-1,0A SNLDAE 230V C123 sXt 929002165306",0,"DALI2 / NightDim (XI FP NLD)",null,70,"D",null,"Oprawa wyposażona w przewód typu H07RN-F 5G1 Do podłączenia w odpowiednio dobranej puszce elektroinstalacyjnej.","7151XX0009.png","7151XX0009.ldt",3,null,1,64]
["7152","7152XX0009","VARBERG LED T4-B 3000K DIM. TRIAC","Varberg","Ground,Ground/Wall","Aluminium","Malowane",null,"PRO","LED zintegrowane","AC","DIM. TRIAC",null,"7,7W",null,"741lm",null,null,"65","IK08","Class I",3000,"szerokie góra",null,null,null,"CE",null,null,"> 109 000h",50,"Oprawa typu naświetlacz","Soczewka firmy Ledil typu T4-B (IESNA typ IV).","T4-B","Luminaire for illuminating facades, gardens, private areas and other architectural concepts. Possibility to adjust the direction of light also in the vertical plane.",null,null,null,"Profil aluminiowy wyciskany, malowany proszkowo.",null,"Soczewka hermetyczna zewnętrzna- tworzywo sztuczne PC przeźroczyste.",null,"Dławnica mosiężna niklowana.",null,null,"Oprawa ściemnialna fazowo TRAILING EDGE (TE)","Moduł LED","Cree DK200402 V1 XTE-HE 3K","Philips Xitanium 10W 0,5A 20V TE SC 230V",0,null,null,80,"E",null,"Oprawa wyposażona w przewód typu H05RN-F 3G1 Do podłączenia w odpowiednio dobranej puszce elektroinstalacyjnej.","7152XX0009.png","7152XX0009.ldt",1,null,1,64]
["7153","7153XX0009","VARBERG LED T4-B 3000K DALI2","Varberg","Ground,Ground/Wall","Aluminium","Malowane",null,"PRO","LED zintegrowane","AC","DALI2",null,"7,8W",null,"742lm",null,null,"65","IK08","Class I",3000,"szerokie góra",null,null,null,"CE",null,"DALI","> 109 000h",50,"Oprawa typu naświetlacz","Soczewka firmy Ledil typu T4-B (IESNA typ IV).","T4-B","Luminaire for illuminating facades, gardens, private areas and other architectural concepts. Possibility to adjust the direction of light also in the vertical plane.",null,null,null,"Profil aluminiowy wyciskany, malowany proszkowo.",null,"Soczewka hermetyczna zewnętrzna- tworzywo sztuczne PC przeźroczyste.",null,"Dławnica mosiężna niklowana.",null,null,"Oprawa ściemnialna fazowo TRAILING EDGE (TE)","Moduł LED","Cree DK200402 V1 XTE-HE 3K","Osram OTi DALI 15/220…240/1A0 LT2 NFC",100000,null,null,80,"E",null,"Oprawa wyposażona w przewód typu H05RN-F 3G1 Do podłączenia w odpowiednio dobranej puszce elektroinstalacyjnej.","7153XX0009.png","7153XX0009.ldt",3,null,1,64]
["7154","7154XX0009","VARBERG LED T4-B 4000K DIM. TRIAC","Varberg","Ground,Ground/Wall","Aluminium","Malowane",null,"PRO","LED zintegrowane","AC","DIM. TRIAC",null,"7,7W",null,"759lm",null,null,"65","IK08","Class I",4000,"szerokie góra",null,null,null,"CE",null,null,"> 109 000h",50,"Oprawa typu naświetlacz","Soczewka firmy Ledil typu T4-B (IESNA typ IV).","T4-B","Luminaire for illuminating facades, gardens, private areas and other architectural concepts. Possibility to adjust the direction of light also in the vertical plane.",null,null,null,"Profil aluminiowy wyciskany, malowany proszkowo.",null,"Soczewka hermetyczna zewnętrzna- tworzywo sztuczne PC przeźroczyste.",null,"Dławnica mosiężna niklowana.",null,null,"Oprawa ściemnialna fazowo TRAILING EDGE (TE)","Moduł LED","Cree DK200402 V1 XTE-HE 3V 4K.","Philips Xitanium 10W 0,5A 20V TE SC 230V",0,null,null,80,"E",null,"Oprawa wyposażona w przewód typu H05RN-F 3G1 Do podłączenia w odpowiednio dobranej puszce elektroinstalacyjnej.","7154XX0009.png","7154XX0009.ldt",1,null,1,64]
["7155","7155XX0009","VARBERG LED T4-B 4000K DALI2","Varberg","Ground,Ground/Wall","Aluminium","Malowane",null,"PRO","LED zintegrowane","AC","DALI2",null,"7,8W",null,"760lm",null,null,"65","IK08","Class I",4000,"szerokie góra",null,null,null,"CE",null,"DALI","> 109 000h",50,"Oprawa typu naświetlacz","Soczewka firmy Ledil typu T4-B (IESNA typ IV).","T4-B","Luminaire for illuminating facades, gardens, private areas and other architectural concepts. Possibility to adjust the direction of light also in the vertical plane.",null,null,null,"Profil aluminiowy wyciskany, malowany proszkowo.",null,"Soczewka hermetyczna zewnętrzna- tworzywo sztuczne PC przeźroczyste.",null,"Dławnica mosiężna niklowana.",null,null,"Oprawa ściemnialna fazowo TRAILING EDGE (TE)","Moduł LED","Cree DK200402 V1 XTE-HE 3V 4K.","Osram OTi DALI 15/220…240/1A0 LT2 NFC",100000,null,null,80,"E",null,"Oprawa wyposażona w przewód typu H05RN-F 3G1 Do podłączenia w odpowiednio dobranej puszce elektroinstalacyjnej.","7155XX0009.png","7155XX0009.ldt",3,null,1,64]
["718","718XX0015","NORDLAND CEILING/WALL LED 911LM 3000K DIM.","Nordland","Wall,Ceiling","Aluminium",null,null,null,"LED zintegrowane","AC","DIM.","10W","10W","911lm","574lm",null,null,"65","IK10","Class I",3000,null,0.28000000000000003,0.28000000000000003,0.1,"CE",null,null,"50 000h",7,"Oprawa sufitowo-ścienna.","Światło rozproszone.",null,"A ceiling-type luminaire with a modern design For lighting private areas and other architectural concepts",null,null,null,"Odlew aluminiowy malowany proszkowo.",null,"Klosz- poliwęglan mleczny, stabilizowany UV.","Uszczelka silikonowa.","Dławnica EPDM.","NIE",null,"Oprawa ściemnialna fazowo TRAILING EDGE (TE) - LEADING EDGE (LE)","Moduł LED","Lumens DLM 100C 10W 830 230V F201 V0,5 3K",null,0,"Ściemnianie fazowe Lumens LED AC",null,80,"F",null,"Zaciski podłączeniowe: max 3x2,5mm², możliwość podłączenia oprawy w pętle max 3x2,5mm². Przewód w oponie okrągłej o średnicy ø7...10,5mm.","718XX0015.jpg","718XX0015.ldt",1,null,1,7]
["724","724XX0010","KOSTER WALL E27","Koster","Wall","Aluminium",null,null,null,"Wymienne","E27",null,"LED max 9W","LED max 9W",null,null,null,null,"54","IK10","Class I",null,null,null,null,null,"CE",null,null,null,12,"Oprawa ścienna.","Światło jednostronne: symetryczne, ukierunkowane w dół.",null,"Modern design wall-mounted luminaire. Possibility to install on corners of architectural objects.",null,null,"Oprawa na wymienne źródło światła typu: lampa LED, świetlówka TC-SE, tradycyjna żarówka (halogenowa) o trzonku E27. Źródło światła należy dokupić oddzielnie.","Odlew aluminiowy malowany proszkowo.",null,"Klosz- poliwęglan przeźroczysty ze strukturą, stabilizowany UV.","Uszczelka silikonowa.","Dławnica EPDM.",null,null,null,"Lampa E27","LED A55..60",null,0,null,0,80,null,"158XX0009","Zaciski podłączeniowe: max 3x2,5mm², możliwość podłączenia oprawy w pętle max 3x1,5mm². Przewód w oponie okrągłej o średnicy ø7...10,5mm.","724XX0010.jpg","724XX0010.ldt",4,"E27",1,27]
["725","725XX0012","KOSTER WALL LED 1080LM 3000K ON/OFF","Koster","Wall","Aluminium",null,null,null,"LED zintegrowane","AC","ON/OFF","9,5W","9,5W","1080lm","872lm",null,null,"54",null,"Class I",3000,null,null,null,null,"CE",null,null,"50000",12,"Oprawa ścienna.","Światło jednostronne: symetryczne, ukierunkowane w dół.",null,"Modern design wall-mounted luminaire. Possibility to install on corners of architectural objects.",null,null,"Oprawa wyposażona w wymienne źródło światła typu moduł LED, który zapewnia trwałość i optymalny rozsył światła, przy zachowaniu stosunkowo niskiego zużycia energii.","Odlew aluminiowy malowany proszkowo.",null,"Klosz- poliwęglan przeźroczysty ze strukturą, stabilizowany UV.",null,"Dławnica EPDM.",null,"Ramię proste","Oprawa nieściemnialna","Moduł LED","Philips Fortimo DLM ES 1100/8xx G2 3K",null,null,null,0,80,"E","158XX0009","Zaciski podłączeniowe: max 3x2,5mm², możliwość podłączenia oprawy w pętle max 3x1,5mm². Przewód w oponie okrągłej o średnicy ø7...10,5mm.","725XX0012.jpg","725XX0012.ldt",4,null,1,27]
["750","750XX0010","TORINO WALL E27","Torino","Wall","Aluminium",null,null,null,"Wymienne","E27",null,"LED max 9W","LED max 9W",null,null,null,null,"54",null,"Class II",null,null,0.38,0.28000000000000003,0.34,"CE",null,null,null,12,"Oprawa ścienna.","Światło odkryte.",null,"Classic design wall-mounted luminaire. For lighting gardens, terraces and other architectural concepts.",null,null,"Oprawa na wymienne źródło światła typu: lampa LED, świetlówka TC-SE, tradycyjna żarówka (halogenowa) o trzonku E27. Źródło światła należy dokupić oddzielnie.","Odlew aluminiowy malowany proszkowo.",null,"Klosz- poliwęglan przeźroczysty, stabilizowany UV.",null,"Dławnica EPDM.",null,null,null,"Lampa E27","A55..60",null,0,null,null,80,null,null,"Zaciski podłączeniowe: max 2x2,5mm², Przewód w oponie okrągłej o średnicy ø7...10,5mm.","750XX0010.jpg","750XX0010.ldt",4,"E27",1,9]
["777","777XX0017","NICE POLE-TOP LED 5127LM 3000K ON/OFF","Nice","Post,Head","Aluminium",null,null,null,"LED zintegrowane","AC","ON/OFF","33,9W","38W","5127lm","3029lm",null,null,"65",null,"Class I",3000,null,0.7,0.55000000000000004,0.55000000000000004,"CE",null,null,"> 110 000h",2,"Oprawa słupowa (nasadzana).","Światło symetryczne pośrednie.",null,"Top-mounted luminaire designed for mounting on a lighting pole with a Ø60mm mounting shaft",null,null,null,"Odlew aluminiowy malowany proszkowo.",null,"Klosz- szkło bezpieczne, przeźroczyste.","Uszczelka silikonowa.",null,null,null,"Oprawa nieściemnialna","Moduł LED","Philips Fortimo SLM C 1211 L19 2828 G7 3K","Philips Xitanium 36W/m 929001486006",0,null,6.8400000000000002E-2,80,"D","154XX0009, 3005XX0009, 7662ZX0009, 7664ZX0009, 7665XX0009","Przewód H05VV-F 3G1 o długości 4,5m do podłączenia wewnątrz słupa oświetleniowego (w odpowiednio dobranej puszce elektroinstalacyjnej).","777XX0017.jpg","777XX0017.ldt",4,null,1,21]
["796","796XX0011","SANDVIK CEILING LED GU10 265LM DOWN 25D 2700K DIM.","Sandvik","Ceiling","Aluminium",null,null,null,"Wymienne","GU10",null,"3,9W","3,9W","~265lm","210lm",null,null,"54","IK08","Class I",2700,null,0,0,0,"CE",null,null,"40000",6,"Oprawa sufitowa.","Światło jednostronne: ukierunkowane w dół o kącie 25D","Down 25D","Classic design ceiling luminaire. For lighting private areas and public spaces.",null,null,"Oprawa wyposażona w wymienne źródło światła typu lampa LED o trzonku Gu10, która zapewnia trwałość i optymalny rozsył światła, przy zachowaniu stosunkowo małego zużycia energii.","Odlew aluminiowy malowany proszkowo.",null,"Klosz- szkło bezpieczne, satynowane.","Uszczelka silikonowa.","Dławnica EPDM.",null,null,"Oprawa ściemnialna fazowo TRAILING EDGE (TE) - LEADING EDGE (LE)","Lampa LED GU10","Philips MASTER LED ExpertColor 3.9-35W GU10 927 25D",null,0,"Ściemnianie fazowe LED GU10 E27",null,90,"G",null,"Zaciski podłączeniowe: max 3x2,5mm², możliwość podłączenia oprawy w pętle max 3x1,5mm². Przewód w oponie okrągłej o średnicy ø7...10,5mm.","796XX0011.jpg","796XX0011.ldt",1,"GU10",1,74]
["800","800XX0012","FIRENZE WALL E27","Florence","Wall","Aluminium",null,null,null,"Wymienne","E27",null,"LED max 9W","LED max 9W",null,null,null,null,"54",null,"Class II",null,null,null,null,null,"CE",null,null,null,12,"Oprawa ścienna.","Światło odkryte.",null,"Classic type wall-mounted luminaire. Possibility to install on corners of architectural objects.",null,null,null,"Odlew aluminiowy malowany proszkowo.",null,"Klosz- poliwęglan przeźroczysty, stabilizowany UV.",null,"Dławnica EPDM.",null,"Ramię na pałąku",null,"Lampa E27","LED A55...60",null,0,null,null,80,null,"152XX0009, 46999021","Zaciski podłączeniowe, max 2x2,5mm². Przewód w oponie okrągłej o średnicy ø7...10,5mm.","800XX0012.jpg","800XX0012.ldt",4,"E27",1,9]
["800A","800XX0110","FIRENZE CEILING-CHAIN E27","Florence","Ceiling","Aluminium",null,null,null,"Wymienne","E27",null,"LED max 9W","LED max 9W",null,null,null,null,"54",null,"Class II",null,null,0,0,0,"CE",null,null,null,16,"Oprawa wisząca.","Światło odkryte.",null,"Classic design luminaire with chain suspension. For lighting gardens, terraces and other architectural concepts.",null,null,"Oprawa na wymienne źródło światła typu: lampa LED, świetlówka TC-SE, tradycyjna żarówka (halogenowa) o trzonku E27. Źródło światła należy dokupić oddzielnie.","Odlew aluminiowy malowany proszkowo.","Łańcuch stalowy malowany proszkowo.","Klosz- poliwęglan przeźroczysty, stabilizowany UV.",null,null,null,null,null,"Lampa E27","LED A55..60",null,0,null,null,80,null,null,"Zaciski podłączeniowe, max 2x2,5mm². Przewód w oponie okrągłej o średnicy ø7...10,5mm.","800XX0110.jpg","800XX0110.ldt",4,"E27",1,9]
["805","805XX0011","FIRENZE BOLLARD E27","Florence","Bollard,Flower","Aluminium",null,null,null,"Wymienne","E27",null,"LED max 9W","LED max 9W",null,null,null,null,"54",null,"Class II",null,null,0,0,0,"CE",null,null,null,1,"Oprawa słupkowa.","Światło odkryte, częściowo przysłonięte od góry.",null,"Classic design luminaire. For lighting gardens, private areas and public spaces. Other accessories need to be purchased separately.",null,null,"Oprawa na wymienne źródło światła typu: lampa LED, tradycyjna żarówka (halogenowa) o trzonku E27. Źródło światła należy dokupić oddzielnie.","Odlew aluminiowy malowany proszkowo.",null,"Klosz- poliwęglan przeźroczysty, stabilizowany UV.",null,"Dławnica EPDM.",null,null,null,"Lampa E27","LED A55...60",null,0,null,null,80,null,"307ZX0009, 46999021","Zaciski podłączeniowe: max 2x2,5mm², możliwość podłączenia oprawy w pętle max 2x1,5mm². Przewód w oponie okrągłej o średnicy ø7...10,5mm.","805XX0011.jpg","805XX0011.ldt",4,"E27",1,23]
["810","810XX0309","FIRENZE POLE LUMINAIRE. E27","Florence","Post,Post complete","Aluminium",null,null,null,"Wymienne","E27",null,"LED max 9W","LED max 9W",null,null,null,null,"54",null,"Class II",null,null,null,null,null,"CE",null,null,null,23,"Oprawa słupowa.","Światło odkryte.",null,"Classic design luminaire, mounted on a telescopic lighting pole. Adjustable height 1930..2560mm. For lighting gardens, terraces and other architectural concepts.",null,null,"Oprawa na wymienne źródło światła typu: lampa LED, świetlówka TC-SE, tradycyjna żarówka (halogenowa) o trzonku E27. Źródło światła należy dokupić oddzielnie.","Odlew aluminiowy malowany proszkowo.",null,"Klosz- poliwęglan przeźroczysty, stabilizowany UV.","Uszczelka silikonowa.",null,"Pojedyncze",null,null,"Lampa E27","LED A55..60",null,0,null,null,80,null,"108GA0009, 305ZX0009, 306ZX0009, 46999021","Zaciski podłączeniowe: max 4x2,5mm², możliwość podłączenia oprawy w pętle max 4x2,5mm². Przewód w oponie okrągłej o średnicy ø6...12,5mm.","810XX0309.jpg","810XX0309.ldt",4,"E27",1,9]
["820","820XX0309","FIRENZE POLE LUMINAIRE. E27","Florence","Post,Post complete","Aluminium",null,null,null,"Wymienne","E27",null,"LED max 2x 9W","LED max 2x 9W",null,null,null,null,"54",null,"Class II",null,null,null,null,null,"CE",null,null,null,23,"Oprawa słupowa.","Światło odkryte.",null,"Classic design luminaire, mounted on a telescopic lighting pole. Adjustable height 1930..2560mm. For lighting gardens, terraces and other architectural concepts.",null,null,"Oprawa na wymienne źródło światła typu: lampa LED, świetlówka TC-SE, tradycyjna żarówka (halogenowa) o trzonku E27. Źródło światła należy dokupić oddzielnie.","Odlew aluminiowy malowany proszkowo.",null,"Klosz- poliwęglan przeźroczysty, stabilizowany UV.","Uszczelka silikonowa.",null,"Podwójne",null,null,"Lampa E27","LED A55..60",null,0,null,null,80,null,"108GA0009, 305ZX0009, 306ZX0009, 46999021","Zaciski podłączeniowe: max 4x2,5mm², możliwość podłączenia oprawy w pętle max 4x2,5mm². Przewód w oponie okrągłej o średnicy ø6...12,5mm.","820XX0309.jpg","820XX0309.ldt",4,"E27",1,9]
["830","830XX0309","FIRENZE POLE LUMINAIRE. E27","Florence","Post,Post complete","Aluminium",null,null,null,"Wymienne","E27",null,"LED max 3x 9W","LED max 3x 9W",null,null,null,null,"54",null,"Class II",null,null,null,null,null,"CE",null,null,null,23,"Oprawa słupowa.","Światło odkryte.",null,"Classic design luminaire, mounted on a telescopic lighting pole. Adjustable height 1930..2560mm. For lighting gardens, terraces and other architectural concepts.",null,null,"Oprawa na wymienne źródło światła typu: lampa LED, świetlówka TC-SE, tradycyjna żarówka (halogenowa) o trzonku E27. Źródło światła należy dokupić oddzielnie.","Odlew aluminiowy malowany proszkowo.",null,"Klosz- poliwęglan przeźroczysty, stabilizowany UV.","Uszczelka silikonowa.",null,"Potrójne",null,null,"Lampa E27","LED A55..60",null,0,null,null,80,null,"108GA0009, 305ZX0009, 306ZX0009, 46999021","Zaciski podłączeniowe: max 4x2,5mm², możliwość podłączenia oprawy w pętle max 4x2,5mm². Przewód w oponie okrągłej o średnicy ø6...12,5mm.","830XX0309.jpg","830XX0309.ldt",4,"E27",1,9]
["866","866XX0013","BODEN WALL LED 743LM 3000K DIM.","Boden","Wall","Stal",null,null,null,"LED zintegrowane","AC","DIM.","8W","8W","743lm","307lm",null,null,"54",null,"Class I",3000,null,0,0,0,"CE",null,null,"50 000h",12,"Oprawa ścienna.","Światło rozproszone.",null,"A ceiling-type luminaire with a contemporary design",null,null,null,null,"Front- stal cynkowana ogniowo lub odlew aluminiowy malowany proszkowo.","Klosz- poliwęglan mleczny, stabilizowany UV.","Uszczelka silikonowa.","Podstawa- odlew aluminiowy malowany proszkowo.",null,"mleczny","Oprawa ściemnialna fazowo TRAILING EDGE (TE) - LEADING EDGE (LE)","Moduł LED","Lumens EDC 57C 8W xxx 230V F201 3K",null,0,"Ściemnianie fazowe Lumens LED AC",null,80,"F",null,"Zaciski podłączeniowe: max 3x2,5mm², możliwość podłączenia oprawy w pętle max 3x1,5mm². Przewód w oponie okrągłej o średnicy ø7...10,5mm.","866XX0013.jpg","866XX0013.ldt",1,null,1,7]
["891","891XX0013","ARVIKA BOLLARD LED 1370LM 3000K ON/OFF","Arvika","Bollard","Stal",null,null,null,"LED zintegrowane","AC","ON/OFF","7,4W","8,8W","1370lm","543lm",null,null,"44",null,"Class I",3000,"szerokie dół",0.14000000000000001,0.14000000000000001,0.89,"CE",null,null,"> 102 000h",1,"Oprawa słupkowa.","Czterostronny wylot światła przysłonięty od góry.",null,"Bollard luminaire for lighting private areas, gardens and other architectural concepts",null,null,null,"Stal cynkowana ogniowo.","Stal cynkowana ogniowo i malowana proszkowo.","Klosz- poliwęglan przeźroczysty, stabilizowany UV.","Uszczelka silikonowa.",null,null,null,"Oprawa nieściemnialna","Moduł LED","Cree DK210704 V2 JB2835 3V 3K","OSRAM OT FIT 15/220-240/350 NFC 4052899617179",0,null,0,80,"C","207GA0010, 208ZX0009","Zaciski podłączeniowe: max 3x4mm², możliwość podłączenia oprawy w pętle max 3x4mm². Przewód w oponie okrągłej o średnicy: ø8...12mm lub ø10...13,6mm","891XX0013.jpg","891XX0013.ldt",4,null,1,16]
["893","893XX0013","ARVIKA BOLLARD-CONNECTORS LED 1370LM 3000K ON/OFF","Arvika","Bollard","Stal",null,null,null,"LED zintegrowane","AC","ON/OFF","7,4W","8,8W","1370lm","543lm",null,null,"44",null,"Class I",3000,null,0.14000000000000001,0.14000000000000001,0.89,"CE",null,null,"> 102 000h",8,"Oprawa słupkowa-dystrybutor energii.","Czterostronny wylot światła przysłonięty od góry.",null,"Bollard luminaire and electricity distributor 220...240V. For lighting private and public areas such as gardens, campsites, etc","Bollard luminaire and electricity distributor 220...240V. For lighting private and public areas such as gardens, campsites, etc. Luminaire equipped with: 1. A replaceable LED module-type light source, 2. Two F-type sockets (SHUKO), two MCB B 16A current fuses, RCCB 30mA residual current circuit breaker, 3. Lighting system equipped with an MCB B 6A current fuse.",null,null,"Stal cynkowana ogniowo.","Stal malowana proszkowo.","Klosz- poliwęglan przeźroczysty, stabilizowany UV.","Uszczelka silikonowa.",null,null,"F (SCHUKO)","Oprawa nieściemnialna","Moduł LED","Cree DK210704 V2 JB2835 3V 3K","OSRAM OT FIT 15/220-240/350 NFC 4052899617179",0,null,0,80,"C","207GA0010, 208ZX0009","Zaciski podłączeniowe: max 5x4mm², możliwość podłączenia oprawy w pętle max 5x4mm². Przewód w oponie okrągłej o średnicy max ø20mm.","893XX0013.jpg","893XX0013.ldt",4,null,1,16]
["901","901XX0009","ARVIKA BOLLARD - CONNECTORS E [UNI] 4XLED 1424LM 3000K ON/OFF","Arvika","Bollard","Stal",null,null,null,"LED zintegrowane","AC","ON/OFF","9,9W","8,8W","1424lm","543lm",null,null,"44",null,"Class I",3000,"szerokie dół",0.14000000000000001,0.14000000000000001,0.89,"CE",null,null,"> 72 000h",41,"Oprawa słupkowa - dystrybutor energii E [Uni].","Czterostronny wylot światła przysłonięty od góry.",null,"E [Uni] sockets","Bollard luminaire and 220...240V electricity distributor. For lighting private areas and other areas, such as gardens, campsites, etc. Luminaire equipped with: 1. A replaceable light source of the LED module type, 2. Two E (UNI) sockets, two current fuses, MCB B 16A type, residual current circuit breaker type RCCB 30mA, 3. The lighting system is equipped with an MCB B 6A fuse",null,null,"Stal cynkowana ogniowo.","Stal malowana proszkowo.","Klosz- poliwęglan przeźroczysty, stabilizowany UV.","Uszczelka silikonowa.",null,null,"E (UNI)","Oprawa nieściemnialna","4 Moduły LED","Cree DK180501 V3 JK3030 3V 3K","Osram OT FIT 15/220-240/500 LT2 S",0,null,0,80,"E","207GA0010, 208ZX0009","Zaciski podłączeniowe: max 5x4mm², możliwość podłączenia oprawy w pętle max 5x4mm². Przewód w oponie okrągłej o średnicy max ø20mm.","901XX0009.jpg","901XX0009.ldt",4,null,1,16]

{"sheet":"RÓŻNICE","index":9,"n_rows":3271,"n_cols":2,"rows_kept":3271,"cut":false,"hidden":false,"merged":[]}
["COŚ NOWEGO"]
["JEST W KP","JEST W IMPORCIE"]
[{"$f":"ID","v":"1000"},{"$f":"INDEX('Import data'!$A:$A,MATCH($A3,'Import data'!$A:$A,0),1)","v":"1000"}]
["1001",{"$f":"INDEX('Import data'!$A:$A,MATCH($A4,'Import data'!$A:$A,0),1)","v":"1001"}]
["1002",{"$f":"INDEX('Import data'!$A:$A,MATCH($A5,'Import data'!$A:$A,0),1)","v":"1002"}]
["1003",{"$f":"INDEX('Import data'!$A:$A,MATCH($A6,'Import data'!$A:$A,0),1)","v":"1003"}]
["1006",{"$f":"INDEX('Import data'!$A:$A,MATCH($A7,'Import data'!$A:$A,0),1)","v":"1006"}]
["1007",{"$f":"INDEX('Import data'!$A:$A,MATCH($A8,'Import data'!$A:$A,0),1)","v":"1007"}]
["1010",{"$f":"INDEX('Import data'!$A:$A,MATCH($A9,'Import data'!$A:$A,0),1)","v":"1010"}]
["1011",{"$f":"INDEX('Import data'!$A:$A,MATCH($A10,'Import data'!$A:$A,0),1)","v":"1011"}]
["1012",{"$f":"INDEX('Import data'!$A:$A,MATCH($A11,'Import data'!$A:$A,0),1)","v":"1012"}]
["1013",{"$f":"INDEX('Import data'!$A:$A,MATCH($A12,'Import data'!$A:$A,0),1)","v":"1013"}]
["1014",{"$f":"INDEX('Import data'!$A:$A,MATCH($A13,'Import data'!$A:$A,0),1)","v":{"$error":"#N/A"}}]
["1015",{"$f":"INDEX('Import data'!$A:$A,MATCH($A14,'Import data'!$A:$A,0),1)","v":{"$error":"#N/A"}}]
["1018",{"$f":"INDEX('Import data'!$A:$A,MATCH($A15,'Import data'!$A:$A,0),1)","v":{"$error":"#N/A"}}]
["1019",{"$f":"INDEX('Import data'!$A:$A,MATCH($A16,'Import data'!$A:$A,0),1)","v":{"$error":"#N/A"}}]
["1022",{"$f":"INDEX('Import data'!$A:$A,MATCH($A17,'Import data'!$A:$A,0),1)","v":{"$error":"#N/A"}}]
["1023",{"$f":"INDEX('Import data'!$A:$A,MATCH($A18,'Import data'!$A:$A,0),1)","v":{"$error":"#N/A"}}]
["1024",{"$f":"INDEX('Import data'!$A:$A,MATCH($A19,'Import data'!$A:$A,0),1)","v":"1024"}]
["1025",{"$f":"INDEX('Import data'!$A:$A,MATCH($A20,'Import data'!$A:$A,0),1)","v":"1025"}]
["1026",{"$f":"INDEX('Import data'!$A:$A,MATCH($A21,'Import data'!$A:$A,0),1)","v":{"$error":"#N/A"}}]
["1027",{"$f":"INDEX('Import data'!$A:$A,MATCH($A22,'Import data'!$A:$A,0),1)","v":{"$error":"#N/A"}}]
["1030",{"$f":"INDEX('Import data'!$A:$A,MATCH($A23,'Import data'!$A:$A,0),1)","v":{"$error":"#N/A"}}]
["1031",{"$f":"INDEX('Import data'!$A:$A,MATCH($A24,'Import data'!$A:$A,0),1)","v":{"$error":"#N/A"}}]
["1034",{"$f":"INDEX('Import data'!$A:$A,MATCH($A25,'Import data'!$A:$A,0),1)","v":{"$error":"#N/A"}}]
["1035",{"$f":"INDEX('Import data'!$A:$A,MATCH($A26,'Import data'!$A:$A,0),1)","v":{"$error":"#N/A"}}]
["1036",{"$f":"INDEX('Import data'!$A:$A,MATCH($A27,'Import data'!$A:$A,0),1)","v":"1036"}]
["1037",{"$f":"INDEX('Import data'!$A:$A,MATCH($A28,'Import data'!$A:$A,0),1)","v":"1037"}]
["1038",{"$f":"INDEX('Import data'!$A:$A,MATCH($A29,'Import data'!$A:$A,0),1)","v":"1038"}]
["1039",{"$f":"INDEX('Import data'!$A:$A,MATCH($A30,'Import data'!$A:$A,0),1)","v":"1039"}]
["1042",{"$f":"INDEX('Import data'!$A:$A,MATCH($A31,'Import data'!$A:$A,0),1)","v":"1042"}]
["1043",{"$f":"INDEX('Import data'!$A:$A,MATCH($A32,'Import data'!$A:$A,0),1)","v":"1043"}]
["1046",{"$f":"INDEX('Import data'!$A:$A,MATCH($A33,'Import data'!$A:$A,0),1)","v":"1046"}]
["1047",{"$f":"INDEX('Import data'!$A:$A,MATCH($A34,'Import data'!$A:$A,0),1)","v":"1047"}]
["1048",{"$f":"INDEX('Import data'!$A:$A,MATCH($A35,'Import data'!$A:$A,0),1)","v":"1048"}]
["1049",{"$f":"INDEX('Import data'!$A:$A,MATCH($A36,'Import data'!$A:$A,0),1)","v":"1049"}]
["1050",{"$f":"INDEX('Import data'!$A:$A,MATCH($A37,'Import data'!$A:$A,0),1)","v":{"$error":"#N/A"}}]
["1051",{"$f":"INDEX('Import data'!$A:$A,MATCH($A38,'Import data'!$A:$A,0),1)","v":{"$error":"#N/A"}}]
["1054",{"$f":"INDEX('Import data'!$A:$A,MATCH($A39,'Import data'!$A:$A,0),1)","v":"1054"}]
["1055",{"$f":"INDEX('Import data'!$A:$A,MATCH($A40,'Import data'!$A:$A,0),1)","v":"1055"}]
["1058",{"$f":"INDEX('Import data'!$A:$A,MATCH($A41,'Import data'!$A:$A,0),1)","v":"1058"}]
["1059",{"$f":"INDEX('Import data'!$A:$A,MATCH($A42,'Import data'!$A:$A,0),1)","v":"1059"}]
["1060",{"$f":"INDEX('Import data'!$A:$A,MATCH($A43,'Import data'!$A:$A,0),1)","v":"1060"}]
["1061",{"$f":"INDEX('Import data'!$A:$A,MATCH($A44,'Import data'!$A:$A,0),1)","v":"1061"}]
["1062",{"$f":"INDEX('Import data'!$A:$A,MATCH($A45,'Import data'!$A:$A,0),1)","v":{"$error":"#N/A"}}]
["1063",{"$f":"INDEX('Import data'!$A:$A,MATCH($A46,'Import data'!$A:$A,0),1)","v":{"$error":"#N/A"}}]
["1066",{"$f":"INDEX('Import data'!$A:$A,MATCH($A47,'Import data'!$A:$A,0),1)","v":{"$error":"#N/A"}}]
["1067",{"$f":"INDEX('Import data'!$A:$A,MATCH($A48,'Import data'!$A:$A,0),1)","v":{"$error":"#N/A"}}]
["1070",{"$f":"INDEX('Import data'!$A:$A,MATCH($A49,'Import data'!$A:$A,0),1)","v":{"$error":"#N/A"}}]
["1071",{"$f":"INDEX('Import data'!$A:$A,MATCH($A50,'Import data'!$A:$A,0),1)","v":{"$error":"#N/A"}}]
["1072",{"$f":"INDEX('Import data'!$A:$A,MATCH($A51,'Import data'!$A:$A,0),1)","v":"1072"}]
["1073",{"$f":"INDEX('Import data'!$A:$A,MATCH($A52,'Import data'!$A:$A,0),1)","v":"1073"}]
["1078",{"$f":"INDEX('Import data'!$A:$A,MATCH($A53,'Import data'!$A:$A,0),1)","v":{"$error":"#N/A"}}]
["1079",{"$f":"INDEX('Import data'!$A:$A,MATCH($A54,'Import data'!$A:$A,0),1)","v":{"$error":"#N/A"}}]
["1082",{"$f":"INDEX('Import data'!$A:$A,MATCH($A55,'Import data'!$A:$A,0),1)","v":{"$error":"#N/A"}}]
["1083",{"$f":"INDEX('Import data'!$A:$A,MATCH($A56,'Import data'!$A:$A,0),1)","v":{"$error":"#N/A"}}]
["1084",{"$f":"INDEX('Import data'!$A:$A,MATCH($A57,'Import data'!$A:$A,0),1)","v":"1084"}]
["1085",{"$f":"INDEX('Import data'!$A:$A,MATCH($A58,'Import data'!$A:$A,0),1)","v":"1085"}]
["1086",{"$f":"INDEX('Import data'!$A:$A,MATCH($A59,'Import data'!$A:$A,0),1)","v":{"$error":"#N/A"}}]
["1087",{"$f":"INDEX('Import data'!$A:$A,MATCH($A60,'Import data'!$A:$A,0),1)","v":{"$error":"#N/A"}}]
["1090",{"$f":"INDEX('Import data'!$A:$A,MATCH($A61,'Import data'!$A:$A,0),1)","v":"1090"}]
["1091",{"$f":"INDEX('Import data'!$A:$A,MATCH($A62,'Import data'!$A:$A,0),1)","v":"1091"}]
["1094",{"$f":"INDEX('Import data'!$A:$A,MATCH($A63,'Import data'!$A:$A,0),1)","v":"1094"}]
["1095",{"$f":"INDEX('Import data'!$A:$A,MATCH($A64,'Import data'!$A:$A,0),1)","v":"1095"}]
["1096",{"$f":"INDEX('Import data'!$A:$A,MATCH($A65,'Import data'!$A:$A,0),1)","v":"1096"}]
["1097",{"$f":"INDEX('Import data'!$A:$A,MATCH($A66,'Import data'!$A:$A,0),1)","v":"1097"}]
[{"$f":"ID","v":"1100"},{"$f":"INDEX('Import data'!$A:$A,MATCH($A67,'Import data'!$A:$A,0),1)","v":"1100"}]
["1101",{"$f":"INDEX('Import data'!$A:$A,MATCH($A68,'Import data'!$A:$A,0),1)","v":"1101"}]
["1102",{"$f":"INDEX('Import data'!$A:$A,MATCH($A69,'Import data'!$A:$A,0),1)","v":"1102"}]
["1103",{"$f":"INDEX('Import data'!$A:$A,MATCH($A70,'Import data'!$A:$A,0),1)","v":"1103"}]
["1104",{"$f":"INDEX('Import data'!$A:$A,MATCH($A71,'Import data'!$A:$A,0),1)","v":"1104"}]
["1105",{"$f":"INDEX('Import data'!$A:$A,MATCH($A72,'Import data'!$A:$A,0),1)","v":"1105"}]
["1106",{"$f":"INDEX('Import data'!$A:$A,MATCH($A73,'Import data'!$A:$A,0),1)","v":"1106"}]
["1107",{"$f":"INDEX('Import data'!$A:$A,MATCH($A74,'Import data'!$A:$A,0),1)","v":"1107"}]
["1108",{"$f":"INDEX('Import data'!$A:$A,MATCH($A75,'Import data'!$A:$A,0),1)","v":"1108"}]
["1109",{"$f":"INDEX('Import data'!$A:$A,MATCH($A76,'Import data'!$A:$A,0),1)","v":"1109"}]
["1157",{"$f":"INDEX('Import data'!$A:$A,MATCH($A77,'Import data'!$A:$A,0),1)","v":"1157"}]
["1159",{"$f":"INDEX('Import data'!$A:$A,MATCH($A78,'Import data'!$A:$A,0),1)","v":"1159"}]
["1165",{"$f":"INDEX('Import data'!$A:$A,MATCH($A79,'Import data'!$A:$A,0),1)","v":"1165"}]
["1167",{"$f":"INDEX('Import data'!$A:$A,MATCH($A80,'Import data'!$A:$A,0),1)","v":"1167"}]
["1173",{"$f":"INDEX('Import data'!$A:$A,MATCH($A81,'Import data'!$A:$A,0),1)","v":"1173"}]
["1175",{"$f":"INDEX('Import data'!$A:$A,MATCH($A82,'Import data'!$A:$A,0),1)","v":"1175"}]
["1179",{"$f":"INDEX('Import data'!$A:$A,MATCH($A83,'Import data'!$A:$A,0),1)","v":"1179"}]
["1181",{"$f":"INDEX('Import data'!$A:$A,MATCH($A84,'Import data'!$A:$A,0),1)","v":"1181"}]
["1187",{"$f":"INDEX('Import data'!$A:$A,MATCH($A85,'Import data'!$A:$A,0),1)","v":"1187"}]
["1189",{"$f":"INDEX('Import data'!$A:$A,MATCH($A86,'Import data'!$A:$A,0),1)","v":"1189"}]
["1195",{"$f":"INDEX('Import data'!$A:$A,MATCH($A87,'Import data'!$A:$A,0),1)","v":"1195"}]
["1197",{"$f":"INDEX('Import data'!$A:$A,MATCH($A88,'Import data'!$A:$A,0),1)","v":"1197"}]
["120",{"$f":"INDEX('Import data'!$A:$A,MATCH($A89,'Import data'!$A:$A,0),1)","v":"120"}]
["1240",{"$f":"INDEX('Import data'!$A:$A,MATCH($A90,'Import data'!$A:$A,0),1)","v":"1240"}]
["1244",{"$f":"INDEX('Import data'!$A:$A,MATCH($A91,'Import data'!$A:$A,0),1)","v":"1244"}]
["1247",{"$f":"INDEX('Import data'!$A:$A,MATCH($A92,'Import data'!$A:$A,0),1)","v":"1247"}]
["1260",{"$f":"INDEX('Import data'!$A:$A,MATCH($A93,'Import data'!$A:$A,0),1)","v":"1260"}]
["1261",{"$f":"INDEX('Import data'!$A:$A,MATCH($A94,'Import data'!$A:$A,0),1)","v":"1261"}]
["1262",{"$f":"INDEX('Import data'!$A:$A,MATCH($A95,'Import data'!$A:$A,0),1)","v":"1262"}]
["1263",{"$f":"INDEX('Import data'!$A:$A,MATCH($A96,'Import data'!$A:$A,0),1)","v":"1263"}]
["1264",{"$f":"INDEX('Import data'!$A:$A,MATCH($A97,'Import data'!$A:$A,0),1)","v":"1264"}]
["1265",{"$f":"INDEX('Import data'!$A:$A,MATCH($A98,'Import data'!$A:$A,0),1)","v":"1265"}]
["1268",{"$f":"INDEX('Import data'!$A:$A,MATCH($A99,'Import data'!$A:$A,0),1)","v":"1268"}]
["1269",{"$f":"INDEX('Import data'!$A:$A,MATCH($A100,'Import data'!$A:$A,0),1)","v":"1269"}]
["127",{"$f":"INDEX('Import data'!$A:$A,MATCH($A101,'Import data'!$A:$A,0),1)","v":"127"}]
["1280",{"$f":"INDEX('Import data'!$A:$A,MATCH($A102,'Import data'!$A:$A,0),1)","v":"1280"}]
["1281",{"$f":"INDEX('Import data'!$A:$A,MATCH($A103,'Import data'!$A:$A,0),1)","v":"1281"}]
["1282",{"$f":"INDEX('Import data'!$A:$A,MATCH($A104,'Import data'!$A:$A,0),1)","v":"1282"}]
["1283",{"$f":"INDEX('Import data'!$A:$A,MATCH($A105,'Import data'!$A:$A,0),1)","v":"1283"}]
["1284",{"$f":"INDEX('Import data'!$A:$A,MATCH($A106,'Import data'!$A:$A,0),1)","v":"1284"}]
["128",{"$f":"INDEX('Import data'!$A:$A,MATCH($A107,'Import data'!$A:$A,0),1)","v":"128"}]
["1290",{"$f":"INDEX('Import data'!$A:$A,MATCH($A108,'Import data'!$A:$A,0),1)","v":"1290"}]
["1291",{"$f":"INDEX('Import data'!$A:$A,MATCH($A109,'Import data'!$A:$A,0),1)","v":"1291"}]
["1300",{"$f":"INDEX('Import data'!$A:$A,MATCH($A110,'Import data'!$A:$A,0),1)","v":"1300"}]
["1302",{"$f":"INDEX('Import data'!$A:$A,MATCH($A111,'Import data'!$A:$A,0),1)","v":"1302"}]
["1303",{"$f":"INDEX('Import data'!$A:$A,MATCH($A112,'Import data'!$A:$A,0),1)","v":"1303"}]
["1305",{"$f":"INDEX('Import data'!$A:$A,MATCH($A113,'Import data'!$A:$A,0),1)","v":"1305"}]
["1306",{"$f":"INDEX('Import data'!$A:$A,MATCH($A114,'Import data'!$A:$A,0),1)","v":"1306"}]
["1308",{"$f":"INDEX('Import data'!$A:$A,MATCH($A115,'Import data'!$A:$A,0),1)","v":"1308"}]
["1310",{"$f":"INDEX('Import data'!$A:$A,MATCH($A116,'Import data'!$A:$A,0),1)","v":"1310"}]
["1311",{"$f":"INDEX('Import data'!$A:$A,MATCH($A117,'Import data'!$A:$A,0),1)","v":"1311"}]
["1312",{"$f":"INDEX('Import data'!$A:$A,MATCH($A118,'Import data'!$A:$A,0),1)","v":"1312"}]
["1314",{"$f":"INDEX('Import data'!$A:$A,MATCH($A119,'Import data'!$A:$A,0),1)","v":"1314"}]
["1315",{"$f":"INDEX('Import data'!$A:$A,MATCH($A120,'Import data'!$A:$A,0),1)","v":"1315"}]
["1316",{"$f":"INDEX('Import data'!$A:$A,MATCH($A121,'Import data'!$A:$A,0),1)","v":"1316"}]
["1317",{"$f":"INDEX('Import data'!$A:$A,MATCH($A122,'Import data'!$A:$A,0),1)","v":"1317"}]
["1318",{"$f":"INDEX('Import data'!$A:$A,MATCH($A123,'Import data'!$A:$A,0),1)","v":"1318"}]
["1319",{"$f":"INDEX('Import data'!$A:$A,MATCH($A124,'Import data'!$A:$A,0),1)","v":"1319"}]
["1320",{"$f":"INDEX('Import data'!$A:$A,MATCH($A125,'Import data'!$A:$A,0),1)","v":"1320"}]
["1321",{"$f":"INDEX('Import data'!$A:$A,MATCH($A126,'Import data'!$A:$A,0),1)","v":"1321"}]
["1322",{"$f":"INDEX('Import data'!$A:$A,MATCH($A127,'Import data'!$A:$A,0),1)","v":"1322"}]
["1324",{"$f":"INDEX('Import data'!$A:$A,MATCH($A128,'Import data'!$A:$A,0),1)","v":"1324"}]
["1330",{"$f":"INDEX('Import data'!$A:$A,MATCH($A129,'Import data'!$A:$A,0),1)","v":"1330"}]
["1331",{"$f":"INDEX('Import data'!$A:$A,MATCH($A130,'Import data'!$A:$A,0),1)","v":"1331"}]
[{"$f":"ID","v":"1336"},{"$f":"INDEX('Import data'!$A:$A,MATCH($A131,'Import data'!$A:$A,0),1)","v":"1336"}]
["1337",{"$f":"INDEX('Import data'!$A:$A,MATCH($A132,'Import data'!$A:$A,0),1)","v":"1337"}]
["1338",{"$f":"INDEX('Import data'!$A:$A,MATCH($A133,'Import data'!$A:$A,0),1)","v":"1338"}]
["1339",{"$f":"INDEX('Import data'!$A:$A,MATCH($A134,'Import data'!$A:$A,0),1)","v":"1339"}]
["1340",{"$f":"INDEX('Import data'!$A:$A,MATCH($A135,'Import data'!$A:$A,0),1)","v":"1340"}]
["1341",{"$f":"INDEX('Import data'!$A:$A,MATCH($A136,'Import data'!$A:$A,0),1)","v":"1341"}]
["1346",{"$f":"INDEX('Import data'!$A:$A,MATCH($A137,'Import data'!$A:$A,0),1)","v":"1346"}]
["1347",{"$f":"INDEX('Import data'!$A:$A,MATCH($A138,'Import data'!$A:$A,0),1)","v":"1347"}]
["1350",{"$f":"INDEX('Import data'!$A:$A,MATCH($A139,'Import data'!$A:$A,0),1)","v":"1350"}]
["1353",{"$f":"INDEX('Import data'!$A:$A,MATCH($A140,'Import data'!$A:$A,0),1)","v":"1353"}]
["1356",{"$f":"INDEX('Import data'!$A:$A,MATCH($A141,'Import data'!$A:$A,0),1)","v":"1356"}]
["1360",{"$f":"INDEX('Import data'!$A:$A,MATCH($A142,'Import data'!$A:$A,0),1)","v":"1360"}]
["1361",{"$f":"INDEX('Import data'!$A:$A,MATCH($A143,'Import data'!$A:$A,0),1)","v":"1361"}]
["1362",{"$f":"INDEX('Import data'!$A:$A,MATCH($A144,'Import data'!$A:$A,0),1)","v":"1362"}]
["1363",{"$f":"INDEX('Import data'!$A:$A,MATCH($A145,'Import data'!$A:$A,0),1)","v":"1363"}]
["1364",{"$f":"INDEX('Import data'!$A:$A,MATCH($A146,'Import data'!$A:$A,0),1)","v":"1364"}]
["1365",{"$f":"INDEX('Import data'!$A:$A,MATCH($A147,'Import data'!$A:$A,0),1)","v":"1365"}]
["1366",{"$f":"INDEX('Import data'!$A:$A,MATCH($A148,'Import data'!$A:$A,0),1)","v":"1366"}]
["1367",{"$f":"INDEX('Import data'!$A:$A,MATCH($A149,'Import data'!$A:$A,0),1)","v":"1367"}]
["1368",{"$f":"INDEX('Import data'!$A:$A,MATCH($A150,'Import data'!$A:$A,0),1)","v":"1368"}]
["1369",{"$f":"INDEX('Import data'!$A:$A,MATCH($A151,'Import data'!$A:$A,0),1)","v":"1369"}]
["1370",{"$f":"INDEX('Import data'!$A:$A,MATCH($A152,'Import data'!$A:$A,0),1)","v":"1370"}]
["1371",{"$f":"INDEX('Import data'!$A:$A,MATCH($A153,'Import data'!$A:$A,0),1)","v":"1371"}]
["1373",{"$f":"INDEX('Import data'!$A:$A,MATCH($A154,'Import data'!$A:$A,0),1)","v":"1373"}]
["1374",{"$f":"INDEX('Import data'!$A:$A,MATCH($A155,'Import data'!$A:$A,0),1)","v":"1374"}]
["1380",{"$f":"INDEX('Import data'!$A:$A,MATCH($A156,'Import data'!$A:$A,0),1)","v":"1380"}]
["1382",{"$f":"INDEX('Import data'!$A:$A,MATCH($A157,'Import data'!$A:$A,0),1)","v":"1382"}]
["1383",{"$f":"INDEX('Import data'!$A:$A,MATCH($A158,'Import data'!$A:$A,0),1)","v":"1383"}]
["1384",{"$f":"INDEX('Import data'!$A:$A,MATCH($A159,'Import data'!$A:$A,0),1)","v":"1384"}]
["1390",{"$f":"INDEX('Import data'!$A:$A,MATCH($A160,'Import data'!$A:$A,0),1)","v":"1390"}]
["1392",{"$f":"INDEX('Import data'!$A:$A,MATCH($A161,'Import data'!$A:$A,0),1)","v":"1392"}]
["1400",{"$f":"INDEX('Import data'!$A:$A,MATCH($A162,'Import data'!$A:$A,0),1)","v":"1400"}]
["1403",{"$f":"INDEX('Import data'!$A:$A,MATCH($A163,'Import data'!$A:$A,0),1)","v":"1403"}]
["1407",{"$f":"INDEX('Import data'!$A:$A,MATCH($A164,'Import data'!$A:$A,0),1)","v":"1407"}]
["1409",{"$f":"INDEX('Import data'!$A:$A,MATCH($A165,'Import data'!$A:$A,0),1)","v":"1409"}]
["1410",{"$f":"INDEX('Import data'!$A:$A,MATCH($A166,'Import data'!$A:$A,0),1)","v":"1410"}]
["1413",{"$f":"INDEX('Import data'!$A:$A,MATCH($A167,'Import data'!$A:$A,0),1)","v":"1413"}]
["1417",{"$f":"INDEX('Import data'!$A:$A,MATCH($A168,'Import data'!$A:$A,0),1)","v":"1417"}]
["1419",{"$f":"INDEX('Import data'!$A:$A,MATCH($A169,'Import data'!$A:$A,0),1)","v":"1419"}]
["1420",{"$f":"INDEX('Import data'!$A:$A,MATCH($A170,'Import data'!$A:$A,0),1)","v":"1420"}]
["1423",{"$f":"INDEX('Import data'!$A:$A,MATCH($A171,'Import data'!$A:$A,0),1)","v":"1423"}]
["1426",{"$f":"INDEX('Import data'!$A:$A,MATCH($A172,'Import data'!$A:$A,0),1)","v":"1426"}]
["1429",{"$f":"INDEX('Import data'!$A:$A,MATCH($A173,'Import data'!$A:$A,0),1)","v":"1429"}]
["1430",{"$f":"INDEX('Import data'!$A:$A,MATCH($A174,'Import data'!$A:$A,0),1)","v":"1430"}]
["1433",{"$f":"INDEX('Import data'!$A:$A,MATCH($A175,'Import data'!$A:$A,0),1)","v":"1433"}]
["1436",{"$f":"INDEX('Import data'!$A:$A,MATCH($A176,'Import data'!$A:$A,0),1)","v":"1436"}]
["1439",{"$f":"INDEX('Import data'!$A:$A,MATCH($A177,'Import data'!$A:$A,0),1)","v":"1439"}]
["1440",{"$f":"INDEX('Import data'!$A:$A,MATCH($A178,'Import data'!$A:$A,0),1)","v":"1440"}]
["1443",{"$f":"INDEX('Import data'!$A:$A,MATCH($A179,'Import data'!$A:$A,0),1)","v":"1443"}]
["1450",{"$f":"INDEX('Import data'!$A:$A,MATCH($A180,'Import data'!$A:$A,0),1)","v":"1450"}]
["1453",{"$f":"INDEX('Import data'!$A:$A,MATCH($A181,'Import data'!$A:$A,0),1)","v":"1453"}]
["1464",{"$f":"INDEX('Import data'!$A:$A,MATCH($A182,'Import data'!$A:$A,0),1)","v":"1464"}]
["1468",{"$f":"INDEX('Import data'!$A:$A,MATCH($A183,'Import data'!$A:$A,0),1)","v":"1468"}]
["1469",{"$f":"INDEX('Import data'!$A:$A,MATCH($A184,'Import data'!$A:$A,0),1)","v":"1469"}]
["1475",{"$f":"INDEX('Import data'!$A:$A,MATCH($A185,'Import data'!$A:$A,0),1)","v":"1475"}]
["1476",{"$f":"INDEX('Import data'!$A:$A,MATCH($A186,'Import data'!$A:$A,0),1)","v":"1476"}]
["1477",{"$f":"INDEX('Import data'!$A:$A,MATCH($A187,'Import data'!$A:$A,0),1)","v":"1477"}]
["1479",{"$f":"INDEX('Import data'!$A:$A,MATCH($A188,'Import data'!$A:$A,0),1)","v":"1479"}]
["1482",{"$f":"INDEX('Import data'!$A:$A,MATCH($A189,'Import data'!$A:$A,0),1)","v":"1482"}]
["1483",{"$f":"INDEX('Import data'!$A:$A,MATCH($A190,'Import data'!$A:$A,0),1)","v":"1483"}]
["1488",{"$f":"INDEX('Import data'!$A:$A,MATCH($A191,'Import data'!$A:$A,0),1)","v":"1488"}]
["1489",{"$f":"INDEX('Import data'!$A:$A,MATCH($A192,'Import data'!$A:$A,0),1)","v":"1489"}]
["1489",{"$f":"INDEX('Import data'!$A:$A,MATCH($A193,'Import data'!$A:$A,0),1)","v":"1489"}]
["1495",{"$f":"INDEX('Import data'!$A:$A,MATCH($A194,'Import data'!$A:$A,0),1)","v":"1495"}]
[{"$f":"ID","v":"1496"},{"$f":"INDEX('Import data'!$A:$A,MATCH($A195,'Import data'!$A:$A,0),1)","v":"1496"}]
["1510",{"$f":"INDEX('Import data'!$A:$A,MATCH($A196,'Import data'!$A:$A,0),1)","v":"1510"}]
["1511",{"$f":"INDEX('Import data'!$A:$A,MATCH($A197,'Import data'!$A:$A,0),1)","v":"1511"}]
["1513",{"$f":"INDEX('Import data'!$A:$A,MATCH($A198,'Import data'!$A:$A,0),1)","v":"1513"}]
["1514",{"$f":"INDEX('Import data'!$A:$A,MATCH($A199,'Import data'!$A:$A,0),1)","v":"1514"}]
["1544",{"$f":"INDEX('Import data'!$A:$A,MATCH($A200,'Import data'!$A:$A,0),1)","v":"1544"}]
["1545",{"$f":"INDEX('Import data'!$A:$A,MATCH($A201,'Import data'!$A:$A,0),1)","v":"1545"}]
["1550",{"$f":"INDEX('Import data'!$A:$A,MATCH($A202,'Import data'!$A:$A,0),1)","v":"1550"}]
["1551",{"$f":"INDEX('Import data'!$A:$A,MATCH($A203,'Import data'!$A:$A,0),1)","v":"1551"}]
["1552",{"$f":"INDEX('Import data'!$A:$A,MATCH($A204,'Import data'!$A:$A,0),1)","v":"1552"}]
["1553",{"$f":"INDEX('Import data'!$A:$A,MATCH($A205,'Import data'!$A:$A,0),1)","v":"1553"}]
["1554",{"$f":"INDEX('Import data'!$A:$A,MATCH($A206,'Import data'!$A:$A,0),1)","v":"1554"}]
["1555",{"$f":"INDEX('Import data'!$A:$A,MATCH($A207,'Import data'!$A:$A,0),1)","v":"1555"}]
["1556",{"$f":"INDEX('Import data'!$A:$A,MATCH($A208,'Import data'!$A:$A,0),1)","v":"1556"}]
["1557",{"$f":"INDEX('Import data'!$A:$A,MATCH($A209,'Import data'!$A:$A,0),1)","v":"1557"}]
["1561",{"$f":"INDEX('Import data'!$A:$A,MATCH($A210,'Import data'!$A:$A,0),1)","v":"1561"}]
["1562",{"$f":"INDEX('Import data'!$A:$A,MATCH($A211,'Import data'!$A:$A,0),1)","v":"1562"}]
["1566",{"$f":"INDEX('Import data'!$A:$A,MATCH($A212,'Import data'!$A:$A,0),1)","v":"1566"}]
["1567",{"$f":"INDEX('Import data'!$A:$A,MATCH($A213,'Import data'!$A:$A,0),1)","v":"1567"}]
["1580",{"$f":"INDEX('Import data'!$A:$A,MATCH($A214,'Import data'!$A:$A,0),1)","v":"1580"}]
["1581",{"$f":"INDEX('Import data'!$A:$A,MATCH($A215,'Import data'!$A:$A,0),1)","v":"1581"}]
["1582",{"$f":"INDEX('Import data'!$A:$A,MATCH($A216,'Import data'!$A:$A,0),1)","v":"1582"}]
["1583",{"$f":"INDEX('Import data'!$A:$A,MATCH($A217,'Import data'!$A:$A,0),1)","v":"1583"}]
["1584",{"$f":"INDEX('Import data'!$A:$A,MATCH($A218,'Import data'!$A:$A,0),1)","v":"1584"}]
["1585",{"$f":"INDEX('Import data'!$A:$A,MATCH($A219,'Import data'!$A:$A,0),1)","v":"1585"}]
["1586",{"$f":"INDEX('Import data'!$A:$A,MATCH($A220,'Import data'!$A:$A,0),1)","v":"1586"}]
["1587",{"$f":"INDEX('Import data'!$A:$A,MATCH($A221,'Import data'!$A:$A,0),1)","v":"1587"}]
["1588",{"$f":"INDEX('Import data'!$A:$A,MATCH($A222,'Import data'!$A:$A,0),1)","v":"1588"}]
["1592",{"$f":"INDEX('Import data'!$A:$A,MATCH($A223,'Import data'!$A:$A,0),1)","v":"1592"}]
["1593",{"$f":"INDEX('Import data'!$A:$A,MATCH($A224,'Import data'!$A:$A,0),1)","v":"1593"}]
["1594",{"$f":"INDEX('Import data'!$A:$A,MATCH($A225,'Import data'!$A:$A,0),1)","v":"1594"}]
["1598",{"$f":"INDEX('Import data'!$A:$A,MATCH($A226,'Import data'!$A:$A,0),1)","v":"1598"}]
["1600",{"$f":"INDEX('Import data'!$A:$A,MATCH($A227,'Import data'!$A:$A,0),1)","v":"1600"}]
["160",{"$f":"INDEX('Import data'!$A:$A,MATCH($A228,'Import data'!$A:$A,0),1)","v":"160"}]
["1620",{"$f":"INDEX('Import data'!$A:$A,MATCH($A229,'Import data'!$A:$A,0),1)","v":"1620"}]
["1630",{"$f":"INDEX('Import data'!$A:$A,MATCH($A230,'Import data'!$A:$A,0),1)","v":"1630"}]
["1631",{"$f":"INDEX('Import data'!$A:$A,MATCH($A231,'Import data'!$A:$A,0),1)","v":"1631"}]
["1632",{"$f":"INDEX('Import data'!$A:$A,MATCH($A232,'Import data'!$A:$A,0),1)","v":"1632"}]
["1633",{"$f":"INDEX('Import data'!$A:$A,MATCH($A233,'Import data'!$A:$A,0),1)","v":"1633"}]
["163",{"$f":"INDEX('Import data'!$A:$A,MATCH($A234,'Import data'!$A:$A,0),1)","v":"163"}]
["1640",{"$f":"INDEX('Import data'!$A:$A,MATCH($A235,'Import data'!$A:$A,0),1)","v":"1640"}]
["1641",{"$f":"INDEX('Import data'!$A:$A,MATCH($A236,'Import data'!$A:$A,0),1)","v":"1641"}]
["1642",{"$f":"INDEX('Import data'!$A:$A,MATCH($A237,'Import data'!$A:$A,0),1)","v":"1642"}]
["1643",{"$f":"INDEX('Import data'!$A:$A,MATCH($A238,'Import data'!$A:$A,0),1)","v":"1643"}]
["1644",{"$f":"INDEX('Import data'!$A:$A,MATCH($A239,'Import data'!$A:$A,0),1)","v":"1644"}]
["1645",{"$f":"INDEX('Import data'!$A:$A,MATCH($A240,'Import data'!$A:$A,0),1)","v":"1645"}]
["1646",{"$f":"INDEX('Import data'!$A:$A,MATCH($A241,'Import data'!$A:$A,0),1)","v":"1646"}]
["1647",{"$f":"INDEX('Import data'!$A:$A,MATCH($A242,'Import data'!$A:$A,0),1)","v":"1647"}]
["1650",{"$f":"INDEX('Import data'!$A:$A,MATCH($A243,'Import data'!$A:$A,0),1)","v":"1650"}]
["1651",{"$f":"INDEX('Import data'!$A:$A,MATCH($A244,'Import data'!$A:$A,0),1)","v":"1651"}]
["1652",{"$f":"INDEX('Import data'!$A:$A,MATCH($A245,'Import data'!$A:$A,0),1)","v":"1652"}]
["1653",{"$f":"INDEX('Import data'!$A:$A,MATCH($A246,'Import data'!$A:$A,0),1)","v":"1653"}]
["1700",{"$f":"INDEX('Import data'!$A:$A,MATCH($A247,'Import data'!$A:$A,0),1)","v":"1700"}]
["1702",{"$f":"INDEX('Import data'!$A:$A,MATCH($A248,'Import data'!$A:$A,0),1)","v":"1702"}]
["1705",{"$f":"INDEX('Import data'!$A:$A,MATCH($A249,'Import data'!$A:$A,0),1)","v":"1705"}]
["1707",{"$f":"INDEX('Import data'!$A:$A,MATCH($A250,'Import data'!$A:$A,0),1)","v":"1707"}]
["1710",{"$f":"INDEX('Import data'!$A:$A,MATCH($A251,'Import data'!$A:$A,0),1)","v":"1710"}]
["1712",{"$f":"INDEX('Import data'!$A:$A,MATCH($A252,'Import data'!$A:$A,0),1)","v":"1712"}]
["1715",{"$f":"INDEX('Import data'!$A:$A,MATCH($A253,'Import data'!$A:$A,0),1)","v":"1715"}]
["1717",{"$f":"INDEX('Import data'!$A:$A,MATCH($A254,'Import data'!$A:$A,0),1)","v":"1717"}]
["1720",{"$f":"INDEX('Import data'!$A:$A,MATCH($A255,'Import data'!$A:$A,0),1)","v":"1720"}]
["1726",{"$f":"INDEX('Import data'!$A:$A,MATCH($A256,'Import data'!$A:$A,0),1)","v":"1726"}]
["1727",{"$f":"INDEX('Import data'!$A:$A,MATCH($A257,'Import data'!$A:$A,0),1)","v":"1727"}]
["1730",{"$f":"INDEX('Import data'!$A:$A,MATCH($A258,'Import data'!$A:$A,0),1)","v":"1730"}]
[{"$f":"ID","v":"1731"},{"$f":"INDEX('Import data'!$A:$A,MATCH($A259,'Import data'!$A:$A,0),1)","v":"1731"}]
["1732",{"$f":"INDEX('Import data'!$A:$A,MATCH($A260,'Import data'!$A:$A,0),1)","v":"1732"}]
["1733",{"$f":"INDEX('Import data'!$A:$A,MATCH($A261,'Import data'!$A:$A,0),1)","v":"1733"}]
["1734",{"$f":"INDEX('Import data'!$A:$A,MATCH($A262,'Import data'!$A:$A,0),1)","v":"1734"}]
["1735",{"$f":"INDEX('Import data'!$A:$A,MATCH($A263,'Import data'!$A:$A,0),1)","v":"1735"}]
["1736",{"$f":"INDEX('Import data'!$A:$A,MATCH($A264,'Import data'!$A:$A,0),1)","v":"1736"}]
["1737",{"$f":"INDEX('Import data'!$A:$A,MATCH($A265,'Import data'!$A:$A,0),1)","v":"1737"}]
["1738",{"$f":"INDEX('Import data'!$A:$A,MATCH($A266,'Import data'!$A:$A,0),1)","v":"1738"}]
["1740",{"$f":"INDEX('Import data'!$A:$A,MATCH($A267,'Import data'!$A:$A,0),1)","v":"1740"}]
["1741",{"$f":"INDEX('Import data'!$A:$A,MATCH($A268,'Import data'!$A:$A,0),1)","v":"1741"}]
["1742",{"$f":"INDEX('Import data'!$A:$A,MATCH($A269,'Import data'!$A:$A,0),1)","v":"1742"}]
["1751",{"$f":"INDEX('Import data'!$A:$A,MATCH($A270,'Import data'!$A:$A,0),1)","v":"1751"}]
["1753",{"$f":"INDEX('Import data'!$A:$A,MATCH($A271,'Import data'!$A:$A,0),1)","v":"1753"}]
["1754",{"$f":"INDEX('Import data'!$A:$A,MATCH($A272,'Import data'!$A:$A,0),1)","v":"1754"}]
["1755",{"$f":"INDEX('Import data'!$A:$A,MATCH($A273,'Import data'!$A:$A,0),1)","v":"1755"}]
["1756",{"$f":"INDEX('Import data'!$A:$A,MATCH($A274,'Import data'!$A:$A,0),1)","v":"1756"}]
["1757",{"$f":"INDEX('Import data'!$A:$A,MATCH($A275,'Import data'!$A:$A,0),1)","v":"1757"}]
["1760",{"$f":"INDEX('Import data'!$A:$A,MATCH($A276,'Import data'!$A:$A,0),1)","v":"1760"}]
["1761",{"$f":"INDEX('Import data'!$A:$A,MATCH($A277,'Import data'!$A:$A,0),1)","v":"1761"}]
["1762",{"$f":"INDEX('Import data'!$A:$A,MATCH($A278,'Import data'!$A:$A,0),1)","v":"1762"}]
["1763",{"$f":"INDEX('Import data'!$A:$A,MATCH($A279,'Import data'!$A:$A,0),1)","v":"1763"}]
["1764",{"$f":"INDEX('Import data'!$A:$A,MATCH($A280,'Import data'!$A:$A,0),1)","v":"1764"}]
["1765",{"$f":"INDEX('Import data'!$A:$A,MATCH($A281,'Import data'!$A:$A,0),1)","v":"1765"}]
["1766",{"$f":"INDEX('Import data'!$A:$A,MATCH($A282,'Import data'!$A:$A,0),1)","v":"1766"}]
["1767",{"$f":"INDEX('Import data'!$A:$A,MATCH($A283,'Import data'!$A:$A,0),1)","v":"1767"}]
["1769",{"$f":"INDEX('Import data'!$A:$A,MATCH($A284,'Import data'!$A:$A,0),1)","v":"1769"}]
["1773",{"$f":"INDEX('Import data'!$A:$A,MATCH($A285,'Import data'!$A:$A,0),1)","v":"1773"}]
["1774",{"$f":"INDEX('Import data'!$A:$A,MATCH($A286,'Import data'!$A:$A,0),1)","v":"1774"}]
["1814",{"$f":"INDEX('Import data'!$A:$A,MATCH($A287,'Import data'!$A:$A,0),1)","v":"1814"}]
["1815",{"$f":"INDEX('Import data'!$A:$A,MATCH($A288,'Import data'!$A:$A,0),1)","v":"1815"}]
["1816",{"$f":"INDEX('Import data'!$A:$A,MATCH($A289,'Import data'!$A:$A,0),1)","v":"1816"}]
["1817",{"$f":"INDEX('Import data'!$A:$A,MATCH($A290,'Import data'!$A:$A,0),1)","v":"1817"}]
["1822",{"$f":"INDEX('Import data'!$A:$A,MATCH($A291,'Import data'!$A:$A,0),1)","v":"1822"}]
["1823",{"$f":"INDEX('Import data'!$A:$A,MATCH($A292,'Import data'!$A:$A,0),1)","v":"1823"}]
["1824",{"$f":"INDEX('Import data'!$A:$A,MATCH($A293,'Import data'!$A:$A,0),1)","v":"1824"}]
["1825",{"$f":"INDEX('Import data'!$A:$A,MATCH($A294,'Import data'!$A:$A,0),1)","v":"1825"}]
["1834",{"$f":"INDEX('Import data'!$A:$A,MATCH($A295,'Import data'!$A:$A,0),1)","v":"1834"}]
["1835",{"$f":"INDEX('Import data'!$A:$A,MATCH($A296,'Import data'!$A:$A,0),1)","v":"1835"}]
["1836",{"$f":"INDEX('Import data'!$A:$A,MATCH($A297,'Import data'!$A:$A,0),1)","v":"1836"}]
["1837",{"$f":"INDEX('Import data'!$A:$A,MATCH($A298,'Import data'!$A:$A,0),1)","v":"1837"}]
["1842",{"$f":"INDEX('Import data'!$A:$A,MATCH($A299,'Import data'!$A:$A,0),1)","v":"1842"}]
["1843",{"$f":"INDEX('Import data'!$A:$A,MATCH($A300,'Import data'!$A:$A,0),1)","v":"1843"}]
["1844",{"$f":"INDEX('Import data'!$A:$A,MATCH($A301,'Import data'!$A:$A,0),1)","v":"1844"}]
["1845",{"$f":"INDEX('Import data'!$A:$A,MATCH($A302,'Import data'!$A:$A,0),1)","v":"1845"}]
["1850",{"$f":"INDEX('Import data'!$A:$A,MATCH($A303,'Import data'!$A:$A,0),1)","v":"1850"}]
["1851",{"$f":"INDEX('Import data'!$A:$A,MATCH($A304,'Import data'!$A:$A,0),1)","v":"1851"}]
["1852",{"$f":"INDEX('Import data'!$A:$A,MATCH($A305,'Import data'!$A:$A,0),1)","v":"1852"}]
["1853",{"$f":"INDEX('Import data'!$A:$A,MATCH($A306,'Import data'!$A:$A,0),1)","v":"1853"}]
["1874",{"$f":"INDEX('Import data'!$A:$A,MATCH($A307,'Import data'!$A:$A,0),1)","v":"1874"}]
["1879",{"$f":"INDEX('Import data'!$A:$A,MATCH($A308,'Import data'!$A:$A,0),1)","v":"1879"}]
["1880",{"$f":"INDEX('Import data'!$A:$A,MATCH($A309,'Import data'!$A:$A,0),1)","v":"1880"}]
["1901",{"$f":"INDEX('Import data'!$A:$A,MATCH($A310,'Import data'!$A:$A,0),1)","v":"1901"}]
["1903",{"$f":"INDEX('Import data'!$A:$A,MATCH($A311,'Import data'!$A:$A,0),1)","v":"1903"}]
["1904",{"$f":"INDEX('Import data'!$A:$A,MATCH($A312,'Import data'!$A:$A,0),1)","v":"1904"}]
["1912",{"$f":"INDEX('Import data'!$A:$A,MATCH($A313,'Import data'!$A:$A,0),1)","v":"1912"}]
["1913",{"$f":"INDEX('Import data'!$A:$A,MATCH($A314,'Import data'!$A:$A,0),1)","v":"1913"}]
["1914",{"$f":"INDEX('Import data'!$A:$A,MATCH($A315,'Import data'!$A:$A,0),1)","v":"1914"}]
["1915",{"$f":"INDEX('Import data'!$A:$A,MATCH($A316,'Import data'!$A:$A,0),1)","v":"1915"}]
["1920",{"$f":"INDEX('Import data'!$A:$A,MATCH($A317,'Import data'!$A:$A,0),1)","v":"1920"}]
["1921",{"$f":"INDEX('Import data'!$A:$A,MATCH($A318,'Import data'!$A:$A,0),1)","v":"1921"}]
["1922",{"$f":"INDEX('Import data'!$A:$A,MATCH($A319,'Import data'!$A:$A,0),1)","v":"1922"}]
["1923",{"$f":"INDEX('Import data'!$A:$A,MATCH($A320,'Import data'!$A:$A,0),1)","v":"1923"}]
["1924",{"$f":"INDEX('Import data'!$A:$A,MATCH($A321,'Import data'!$A:$A,0),1)","v":"1924"}]
["1929",{"$f":"INDEX('Import data'!$A:$A,MATCH($A322,'Import data'!$A:$A,0),1)","v":"1929"}]
[{"$f":"ID","v":"1930"},{"$f":"INDEX('Import data'!$A:$A,MATCH($A323,'Import data'!$A:$A,0),1)","v":"1930"}]
["1931",{"$f":"INDEX('Import data'!$A:$A,MATCH($A324,'Import data'!$A:$A,0),1)","v":"1931"}]
["1932",{"$f":"INDEX('Import data'!$A:$A,MATCH($A325,'Import data'!$A:$A,0),1)","v":"1932"}]
["1933",{"$f":"INDEX('Import data'!$A:$A,MATCH($A326,'Import data'!$A:$A,0),1)","v":"1933"}]
["1950",{"$f":"INDEX('Import data'!$A:$A,MATCH($A327,'Import data'!$A:$A,0),1)","v":"1950"}]
["1954",{"$f":"INDEX('Import data'!$A:$A,MATCH($A328,'Import data'!$A:$A,0),1)","v":"1954"}]
["1955",{"$f":"INDEX('Import data'!$A:$A,MATCH($A329,'Import data'!$A:$A,0),1)","v":"1955"}]
["1960",{"$f":"INDEX('Import data'!$A:$A,MATCH($A330,'Import data'!$A:$A,0),1)","v":"1960"}]
["1963",{"$f":"INDEX('Import data'!$A:$A,MATCH($A331,'Import data'!$A:$A,0),1)","v":"1963"}]
["1970",{"$f":"INDEX('Import data'!$A:$A,MATCH($A332,'Import data'!$A:$A,0),1)","v":"1970"}]
["1971",{"$f":"INDEX('Import data'!$A:$A,MATCH($A333,'Import data'!$A:$A,0),1)","v":"1971"}]
["1972",{"$f":"INDEX('Import data'!$A:$A,MATCH($A334,'Import data'!$A:$A,0),1)","v":"1972"}]
["1973",{"$f":"INDEX('Import data'!$A:$A,MATCH($A335,'Import data'!$A:$A,0),1)","v":"1973"}]
["2018",{"$f":"INDEX('Import data'!$A:$A,MATCH($A336,'Import data'!$A:$A,0),1)","v":"2018"}]
["2026",{"$f":"INDEX('Import data'!$A:$A,MATCH($A337,'Import data'!$A:$A,0),1)","v":"2026"}]
["2027",{"$f":"INDEX('Import data'!$A:$A,MATCH($A338,'Import data'!$A:$A,0),1)","v":"2027"}]
["2028",{"$f":"INDEX('Import data'!$A:$A,MATCH($A339,'Import data'!$A:$A,0),1)","v":"2028"}]
["2029",{"$f":"INDEX('Import data'!$A:$A,MATCH($A340,'Import data'!$A:$A,0),1)","v":"2029"}]
["210",{"$f":"INDEX('Import data'!$A:$A,MATCH($A341,'Import data'!$A:$A,0),1)","v":"210"}]
["211",{"$f":"INDEX('Import data'!$A:$A,MATCH($A342,'Import data'!$A:$A,0),1)","v":"211"}]
["2120",{"$f":"INDEX('Import data'!$A:$A,MATCH($A343,'Import data'!$A:$A,0),1)","v":"2120"}]
["2121",{"$f":"INDEX('Import data'!$A:$A,MATCH($A344,'Import data'!$A:$A,0),1)","v":"2121"}]
["2122",{"$f":"INDEX('Import data'!$A:$A,MATCH($A345,'Import data'!$A:$A,0),1)","v":"2122"}]
["2123",{"$f":"INDEX('Import data'!$A:$A,MATCH($A346,'Import data'!$A:$A,0),1)","v":"2123"}]
["2124",{"$f":"INDEX('Import data'!$A:$A,MATCH($A347,'Import data'!$A:$A,0),1)","v":"2124"}]
["2125",{"$f":"INDEX('Import data'!$A:$A,MATCH($A348,'Import data'!$A:$A,0),1)","v":"2125"}]
["212",{"$f":"INDEX('Import data'!$A:$A,MATCH($A349,'Import data'!$A:$A,0),1)","v":"212"}]
["2240",{"$f":"INDEX('Import data'!$A:$A,MATCH($A350,'Import data'!$A:$A,0),1)","v":"2240"}]
["2241",{"$f":"INDEX('Import data'!$A:$A,MATCH($A351,'Import data'!$A:$A,0),1)","v":"2241"}]
["2244",{"$f":"INDEX('Import data'!$A:$A,MATCH($A352,'Import data'!$A:$A,0),1)","v":"2244"}]
["2245",{"$f":"INDEX('Import data'!$A:$A,MATCH($A353,'Import data'!$A:$A,0),1)","v":"2245"}]
["2248",{"$f":"INDEX('Import data'!$A:$A,MATCH($A354,'Import data'!$A:$A,0),1)","v":"2248"}]
["2249",{"$f":"INDEX('Import data'!$A:$A,MATCH($A355,'Import data'!$A:$A,0),1)","v":"2249"}]
["2304",{"$f":"INDEX('Import data'!$A:$A,MATCH($A356,'Import data'!$A:$A,0),1)","v":"2304"}]
["2305",{"$f":"INDEX('Import data'!$A:$A,MATCH($A357,'Import data'!$A:$A,0),1)","v":"2305"}]
["2308",{"$f":"INDEX('Import data'!$A:$A,MATCH($A358,'Import data'!$A:$A,0),1)","v":"2308"}]
["2309",{"$f":"INDEX('Import data'!$A:$A,MATCH($A359,'Import data'!$A:$A,0),1)","v":"2309"}]
["2317",{"$f":"INDEX('Import data'!$A:$A,MATCH($A360,'Import data'!$A:$A,0),1)","v":"2317"}]
["2320",{"$f":"INDEX('Import data'!$A:$A,MATCH($A361,'Import data'!$A:$A,0),1)","v":"2320"}]
["2321",{"$f":"INDEX('Import data'!$A:$A,MATCH($A362,'Import data'!$A:$A,0),1)","v":"2321"}]
["2330",{"$f":"INDEX('Import data'!$A:$A,MATCH($A363,'Import data'!$A:$A,0),1)","v":"2330"}]
["2331",{"$f":"INDEX('Import data'!$A:$A,MATCH($A364,'Import data'!$A:$A,0),1)","v":"2331"}]
["2334",{"$f":"INDEX('Import data'!$A:$A,MATCH($A365,'Import data'!$A:$A,0),1)","v":"2334"}]
["2335",{"$f":"INDEX('Import data'!$A:$A,MATCH($A366,'Import data'!$A:$A,0),1)","v":"2335"}]
["2338",{"$f":"INDEX('Import data'!$A:$A,MATCH($A367,'Import data'!$A:$A,0),1)","v":"2338"}]
["2339",{"$f":"INDEX('Import data'!$A:$A,MATCH($A368,'Import data'!$A:$A,0),1)","v":"2339"}]
["2342",{"$f":"INDEX('Import data'!$A:$A,MATCH($A369,'Import data'!$A:$A,0),1)","v":"2342"}]
["2343",{"$f":"INDEX('Import data'!$A:$A,MATCH($A370,'Import data'!$A:$A,0),1)","v":"2343"}]
["2346",{"$f":"INDEX('Import data'!$A:$A,MATCH($A371,'Import data'!$A:$A,0),1)","v":"2346"}]
["2347",{"$f":"INDEX('Import data'!$A:$A,MATCH($A372,'Import data'!$A:$A,0),1)","v":"2347"}]
["2350",{"$f":"INDEX('Import data'!$A:$A,MATCH($A373,'Import data'!$A:$A,0),1)","v":"2350"}]
["2351",{"$f":"INDEX('Import data'!$A:$A,MATCH($A374,'Import data'!$A:$A,0),1)","v":"2351"}]
["2360",{"$f":"INDEX('Import data'!$A:$A,MATCH($A375,'Import data'!$A:$A,0),1)","v":"2360"}]
["2361",{"$f":"INDEX('Import data'!$A:$A,MATCH($A376,'Import data'!$A:$A,0),1)","v":"2361"}]
["2364",{"$f":"INDEX('Import data'!$A:$A,MATCH($A377,'Import data'!$A:$A,0),1)","v":"2364"}]
["2365",{"$f":"INDEX('Import data'!$A:$A,MATCH($A378,'Import data'!$A:$A,0),1)","v":"2365"}]
["2400",{"$f":"INDEX('Import data'!$A:$A,MATCH($A379,'Import data'!$A:$A,0),1)","v":"2400"}]
["2401",{"$f":"INDEX('Import data'!$A:$A,MATCH($A380,'Import data'!$A:$A,0),1)","v":"2401"}]
["2402",{"$f":"INDEX('Import data'!$A:$A,MATCH($A381,'Import data'!$A:$A,0),1)","v":"2402"}]
["2403",{"$f":"INDEX('Import data'!$A:$A,MATCH($A382,'Import data'!$A:$A,0),1)","v":"2403"}]
["2404",{"$f":"INDEX('Import data'!$A:$A,MATCH($A383,'Import data'!$A:$A,0),1)","v":"2404"}]
["2405",{"$f":"INDEX('Import data'!$A:$A,MATCH($A384,'Import data'!$A:$A,0),1)","v":"2405"}]
["2406",{"$f":"INDEX('Import data'!$A:$A,MATCH($A385,'Import data'!$A:$A,0),1)","v":"2406"}]
["2407",{"$f":"INDEX('Import data'!$A:$A,MATCH($A386,'Import data'!$A:$A,0),1)","v":"2407"}]
[{"$f":"ID","v":"240A"},{"$f":"INDEX('Import data'!$A:$A,MATCH($A387,'Import data'!$A:$A,0),1)","v":"240A"}]
["2410",{"$f":"INDEX('Import data'!$A:$A,MATCH($A388,'Import data'!$A:$A,0),1)","v":"2410"}]
["2411",{"$f":"INDEX('Import data'!$A:$A,MATCH($A389,'Import data'!$A:$A,0),1)","v":"2411"}]
["2412",{"$f":"INDEX('Import data'!$A:$A,MATCH($A390,'Import data'!$A:$A,0),1)","v":"2412"}]
["2413",{"$f":"INDEX('Import data'!$A:$A,MATCH($A391,'Import data'!$A:$A,0),1)","v":"2413"}]
["2414",{"$f":"INDEX('Import data'!$A:$A,MATCH($A392,'Import data'!$A:$A,0),1)","v":"2414"}]
["2415",{"$f":"INDEX('Import data'!$A:$A,MATCH($A393,'Import data'!$A:$A,0),1)","v":"2415"}]
["2416",{"$f":"INDEX('Import data'!$A:$A,MATCH($A394,'Import data'!$A:$A,0),1)","v":"2416"}]
["2417",{"$f":"INDEX('Import data'!$A:$A,MATCH($A395,'Import data'!$A:$A,0),1)","v":"2417"}]
["242",{"$f":"INDEX('Import data'!$A:$A,MATCH($A396,'Import data'!$A:$A,0),1)","v":"242"}]
["245",{"$f":"INDEX('Import data'!$A:$A,MATCH($A397,'Import data'!$A:$A,0),1)","v":"245"}]
["280",{"$f":"INDEX('Import data'!$A:$A,MATCH($A398,'Import data'!$A:$A,0),1)","v":"280"}]
["281",{"$f":"INDEX('Import data'!$A:$A,MATCH($A399,'Import data'!$A:$A,0),1)","v":"281"}]
["283",{"$f":"INDEX('Import data'!$A:$A,MATCH($A400,'Import data'!$A:$A,0),1)","v":"283"}]
["284",{"$f":"INDEX('Import data'!$A:$A,MATCH($A401,'Import data'!$A:$A,0),1)","v":"284"}]
["285",{"$f":"INDEX('Import data'!$A:$A,MATCH($A402,'Import data'!$A:$A,0),1)","v":"285"}]
["286",{"$f":"INDEX('Import data'!$A:$A,MATCH($A403,'Import data'!$A:$A,0),1)","v":"286"}]
["287",{"$f":"INDEX('Import data'!$A:$A,MATCH($A404,'Import data'!$A:$A,0),1)","v":"287"}]
["288",{"$f":"INDEX('Import data'!$A:$A,MATCH($A405,'Import data'!$A:$A,0),1)","v":"288"}]
["289",{"$f":"INDEX('Import data'!$A:$A,MATCH($A406,'Import data'!$A:$A,0),1)","v":"289"}]
["291",{"$f":"INDEX('Import data'!$A:$A,MATCH($A407,'Import data'!$A:$A,0),1)","v":"291"}]
["2935",{"$f":"INDEX('Import data'!$A:$A,MATCH($A408,'Import data'!$A:$A,0),1)","v":"2935"}]
["2937",{"$f":"INDEX('Import data'!$A:$A,MATCH($A409,'Import data'!$A:$A,0),1)","v":"2937"}]
["2939",{"$f":"INDEX('Import data'!$A:$A,MATCH($A410,'Import data'!$A:$A,0),1)","v":"2939"}]
["293",{"$f":"INDEX('Import data'!$A:$A,MATCH($A411,'Import data'!$A:$A,0),1)","v":"293"}]
["2941",{"$f":"INDEX('Import data'!$A:$A,MATCH($A412,'Import data'!$A:$A,0),1)","v":"2941"}]
["2943",{"$f":"INDEX('Import data'!$A:$A,MATCH($A413,'Import data'!$A:$A,0),1)","v":"2943"}]
["2945",{"$f":"INDEX('Import data'!$A:$A,MATCH($A414,'Import data'!$A:$A,0),1)","v":"2945"}]
["2947",{"$f":"INDEX('Import data'!$A:$A,MATCH($A415,'Import data'!$A:$A,0),1)","v":"2947"}]
["2949",{"$f":"INDEX('Import data'!$A:$A,MATCH($A416,'Import data'!$A:$A,0),1)","v":"2949"}]
["295",{"$f":"INDEX('Import data'!$A:$A,MATCH($A417,'Import data'!$A:$A,0),1)","v":"295"}]
["296",{"$f":"INDEX('Import data'!$A:$A,MATCH($A418,'Import data'!$A:$A,0),1)","v":"296"}]
["297",{"$f":"INDEX('Import data'!$A:$A,MATCH($A419,'Import data'!$A:$A,0),1)","v":"297"}]
["298",{"$f":"INDEX('Import data'!$A:$A,MATCH($A420,'Import data'!$A:$A,0),1)","v":"298"}]
["299",{"$f":"INDEX('Import data'!$A:$A,MATCH($A421,'Import data'!$A:$A,0),1)","v":"299"}]
["370",{"$f":"INDEX('Import data'!$A:$A,MATCH($A422,'Import data'!$A:$A,0),1)","v":"370"}]
["371",{"$f":"INDEX('Import data'!$A:$A,MATCH($A423,'Import data'!$A:$A,0),1)","v":"371"}]
["372",{"$f":"INDEX('Import data'!$A:$A,MATCH($A424,'Import data'!$A:$A,0),1)","v":"372"}]
["373",{"$f":"INDEX('Import data'!$A:$A,MATCH($A425,'Import data'!$A:$A,0),1)","v":"373"}]
["375",{"$f":"INDEX('Import data'!$A:$A,MATCH($A426,'Import data'!$A:$A,0),1)","v":"375"}]
["4043",{"$f":"INDEX('Import data'!$A:$A,MATCH($A427,'Import data'!$A:$A,0),1)","v":"4043"}]
["4044",{"$f":"INDEX('Import data'!$A:$A,MATCH($A428,'Import data'!$A:$A,0),1)","v":"4044"}]
["4045",{"$f":"INDEX('Import data'!$A:$A,MATCH($A429,'Import data'!$A:$A,0),1)","v":"4045"}]
["4046",{"$f":"INDEX('Import data'!$A:$A,MATCH($A430,'Import data'!$A:$A,0),1)","v":"4046"}]
["4047",{"$f":"INDEX('Import data'!$A:$A,MATCH($A431,'Import data'!$A:$A,0),1)","v":"4047"}]
["4048",{"$f":"INDEX('Import data'!$A:$A,MATCH($A432,'Import data'!$A:$A,0),1)","v":"4048"}]
["4049",{"$f":"INDEX('Import data'!$A:$A,MATCH($A433,'Import data'!$A:$A,0),1)","v":"4049"}]
["4050",{"$f":"INDEX('Import data'!$A:$A,MATCH($A434,'Import data'!$A:$A,0),1)","v":"4050"}]
["4051",{"$f":"INDEX('Import data'!$A:$A,MATCH($A435,'Import data'!$A:$A,0),1)","v":"4051"}]
["4052",{"$f":"INDEX('Import data'!$A:$A,MATCH($A436,'Import data'!$A:$A,0),1)","v":"4052"}]
["4053",{"$f":"INDEX('Import data'!$A:$A,MATCH($A437,'Import data'!$A:$A,0),1)","v":"4053"}]
["4054",{"$f":"INDEX('Import data'!$A:$A,MATCH($A438,'Import data'!$A:$A,0),1)","v":"4054"}]
["4055",{"$f":"INDEX('Import data'!$A:$A,MATCH($A439,'Import data'!$A:$A,0),1)","v":"4055"}]
["4056",{"$f":"INDEX('Import data'!$A:$A,MATCH($A440,'Import data'!$A:$A,0),1)","v":"4056"}]
["4057",{"$f":"INDEX('Import data'!$A:$A,MATCH($A441,'Import data'!$A:$A,0),1)","v":"4057"}]
["4058",{"$f":"INDEX('Import data'!$A:$A,MATCH($A442,'Import data'!$A:$A,0),1)","v":"4058"}]
["4113",{"$f":"INDEX('Import data'!$A:$A,MATCH($A443,'Import data'!$A:$A,0),1)","v":"4113"}]
["4114",{"$f":"INDEX('Import data'!$A:$A,MATCH($A444,'Import data'!$A:$A,0),1)","v":"4114"}]
["4116",{"$f":"INDEX('Import data'!$A:$A,MATCH($A445,'Import data'!$A:$A,0),1)","v":"4116"}]
["4117",{"$f":"INDEX('Import data'!$A:$A,MATCH($A446,'Import data'!$A:$A,0),1)","v":"4117"}]
["4118",{"$f":"INDEX('Import data'!$A:$A,MATCH($A447,'Import data'!$A:$A,0),1)","v":"4118"}]
["4119",{"$f":"INDEX('Import data'!$A:$A,MATCH($A448,'Import data'!$A:$A,0),1)","v":"4119"}]
["4120",{"$f":"INDEX('Import data'!$A:$A,MATCH($A449,'Import data'!$A:$A,0),1)","v":"4120"}]
["4121",{"$f":"INDEX('Import data'!$A:$A,MATCH($A450,'Import data'!$A:$A,0),1)","v":"4121"}]
[{"$f":"ID","v":"4122"},{"$f":"INDEX('Import data'!$A:$A,MATCH($A451,'Import data'!$A:$A,0),1)","v":"4122"}]
["4126",{"$f":"INDEX('Import data'!$A:$A,MATCH($A452,'Import data'!$A:$A,0),1)","v":"4126"}]
["4136",{"$f":"INDEX('Import data'!$A:$A,MATCH($A453,'Import data'!$A:$A,0),1)","v":"4136"}]
["4140",{"$f":"INDEX('Import data'!$A:$A,MATCH($A454,'Import data'!$A:$A,0),1)","v":"4140"}]
["4300",{"$f":"INDEX('Import data'!$A:$A,MATCH($A455,'Import data'!$A:$A,0),1)","v":"4300"}]
["4301",{"$f":"INDEX('Import data'!$A:$A,MATCH($A456,'Import data'!$A:$A,0),1)","v":"4301"}]
["4302",{"$f":"INDEX('Import data'!$A:$A,MATCH($A457,'Import data'!$A:$A,0),1)","v":"4302"}]
["4303",{"$f":"INDEX('Import data'!$A:$A,MATCH($A458,'Import data'!$A:$A,0),1)","v":"4303"}]
["4310",{"$f":"INDEX('Import data'!$A:$A,MATCH($A459,'Import data'!$A:$A,0),1)","v":"4310"}]
["4311",{"$f":"INDEX('Import data'!$A:$A,MATCH($A460,'Import data'!$A:$A,0),1)","v":"4311"}]
["4312",{"$f":"INDEX('Import data'!$A:$A,MATCH($A461,'Import data'!$A:$A,0),1)","v":"4312"}]
["4313",{"$f":"INDEX('Import data'!$A:$A,MATCH($A462,'Import data'!$A:$A,0),1)","v":"4313"}]
["4322",{"$f":"INDEX('Import data'!$A:$A,MATCH($A463,'Import data'!$A:$A,0),1)","v":"4322"}]
["4323",{"$f":"INDEX('Import data'!$A:$A,MATCH($A464,'Import data'!$A:$A,0),1)","v":"4323"}]
["4332",{"$f":"INDEX('Import data'!$A:$A,MATCH($A465,'Import data'!$A:$A,0),1)","v":"4332"}]
["4333",{"$f":"INDEX('Import data'!$A:$A,MATCH($A466,'Import data'!$A:$A,0),1)","v":"4333"}]
["4362",{"$f":"INDEX('Import data'!$A:$A,MATCH($A467,'Import data'!$A:$A,0),1)","v":"4362"}]
["4363",{"$f":"INDEX('Import data'!$A:$A,MATCH($A468,'Import data'!$A:$A,0),1)","v":"4363"}]
["4372",{"$f":"INDEX('Import data'!$A:$A,MATCH($A469,'Import data'!$A:$A,0),1)","v":"4372"}]
["4373",{"$f":"INDEX('Import data'!$A:$A,MATCH($A470,'Import data'!$A:$A,0),1)","v":"4373"}]
["450",{"$f":"INDEX('Import data'!$A:$A,MATCH($A471,'Import data'!$A:$A,0),1)","v":"450"}]
["454",{"$f":"INDEX('Import data'!$A:$A,MATCH($A472,'Import data'!$A:$A,0),1)","v":"454"}]
["5001",{"$f":"INDEX('Import data'!$A:$A,MATCH($A473,'Import data'!$A:$A,0),1)","v":"5001"}]
["5002",{"$f":"INDEX('Import data'!$A:$A,MATCH($A474,'Import data'!$A:$A,0),1)","v":"5002"}]
["5003",{"$f":"INDEX('Import data'!$A:$A,MATCH($A475,'Import data'!$A:$A,0),1)","v":"5003"}]
["5004",{"$f":"INDEX('Import data'!$A:$A,MATCH($A476,'Import data'!$A:$A,0),1)","v":"5004"}]
["5006",{"$f":"INDEX('Import data'!$A:$A,MATCH($A477,'Import data'!$A:$A,0),1)","v":"5006"}]
["5007",{"$f":"INDEX('Import data'!$A:$A,MATCH($A478,'Import data'!$A:$A,0),1)","v":"5007"}]
["5008",{"$f":"INDEX('Import data'!$A:$A,MATCH($A479,'Import data'!$A:$A,0),1)","v":"5008"}]
["5009",{"$f":"INDEX('Import data'!$A:$A,MATCH($A480,'Import data'!$A:$A,0),1)","v":"5009"}]
["5010",{"$f":"INDEX('Import data'!$A:$A,MATCH($A481,'Import data'!$A:$A,0),1)","v":"5010"}]
["5011",{"$f":"INDEX('Import data'!$A:$A,MATCH($A482,'Import data'!$A:$A,0),1)","v":"5011"}]
["5012",{"$f":"INDEX('Import data'!$A:$A,MATCH($A483,'Import data'!$A:$A,0),1)","v":"5012"}]
["5013",{"$f":"INDEX('Import data'!$A:$A,MATCH($A484,'Import data'!$A:$A,0),1)","v":"5013"}]
["5014",{"$f":"INDEX('Import data'!$A:$A,MATCH($A485,'Import data'!$A:$A,0),1)","v":"5014"}]
["5015",{"$f":"INDEX('Import data'!$A:$A,MATCH($A486,'Import data'!$A:$A,0),1)","v":"5015"}]
["5016",{"$f":"INDEX('Import data'!$A:$A,MATCH($A487,'Import data'!$A:$A,0),1)","v":"5016"}]
["5018",{"$f":"INDEX('Import data'!$A:$A,MATCH($A488,'Import data'!$A:$A,0),1)","v":"5018"}]
["5019",{"$f":"INDEX('Import data'!$A:$A,MATCH($A489,'Import data'!$A:$A,0),1)","v":"5019"}]
["5020",{"$f":"INDEX('Import data'!$A:$A,MATCH($A490,'Import data'!$A:$A,0),1)","v":"5020"}]
["5021",{"$f":"INDEX('Import data'!$A:$A,MATCH($A491,'Import data'!$A:$A,0),1)","v":"5021"}]
["5022",{"$f":"INDEX('Import data'!$A:$A,MATCH($A492,'Import data'!$A:$A,0),1)","v":"5022"}]
["5023",{"$f":"INDEX('Import data'!$A:$A,MATCH($A493,'Import data'!$A:$A,0),1)","v":"5023"}]
["5024",{"$f":"INDEX('Import data'!$A:$A,MATCH($A494,'Import data'!$A:$A,0),1)","v":"5024"}]
["5028",{"$f":"INDEX('Import data'!$A:$A,MATCH($A495,'Import data'!$A:$A,0),1)","v":"5028"}]
["5029",{"$f":"INDEX('Import data'!$A:$A,MATCH($A496,'Import data'!$A:$A,0),1)","v":"5029"}]
["5030",{"$f":"INDEX('Import data'!$A:$A,MATCH($A497,'Import data'!$A:$A,0),1)","v":"5030"}]
["5031",{"$f":"INDEX('Import data'!$A:$A,MATCH($A498,'Import data'!$A:$A,0),1)","v":"5031"}]
["5032",{"$f":"INDEX('Import data'!$A:$A,MATCH($A499,'Import data'!$A:$A,0),1)","v":"5032"}]
["5033",{"$f":"INDEX('Import data'!$A:$A,MATCH($A500,'Import data'!$A:$A,0),1)","v":"5033"}]
["5038",{"$f":"INDEX('Import data'!$A:$A,MATCH($A501,'Import data'!$A:$A,0),1)","v":"5038"}]
["5039",{"$f":"INDEX('Import data'!$A:$A,MATCH($A502,'Import data'!$A:$A,0),1)","v":"5039"}]
["5045",{"$f":"INDEX('Import data'!$A:$A,MATCH($A503,'Import data'!$A:$A,0),1)","v":"5045"}]
["5046",{"$f":"INDEX('Import data'!$A:$A,MATCH($A504,'Import data'!$A:$A,0),1)","v":"5046"}]
["5047",{"$f":"INDEX('Import data'!$A:$A,MATCH($A505,'Import data'!$A:$A,0),1)","v":"5047"}]
["5060",{"$f":"INDEX('Import data'!$A:$A,MATCH($A506,'Import data'!$A:$A,0),1)","v":"5060"}]
["5061",{"$f":"INDEX('Import data'!$A:$A,MATCH($A507,'Import data'!$A:$A,0),1)","v":"5061"}]
["5062",{"$f":"INDEX('Import data'!$A:$A,MATCH($A508,'Import data'!$A:$A,0),1)","v":"5062"}]
["5063",{"$f":"INDEX('Import data'!$A:$A,MATCH($A509,'Import data'!$A:$A,0),1)","v":"5063"}]
["5065",{"$f":"INDEX('Import data'!$A:$A,MATCH($A510,'Import data'!$A:$A,0),1)","v":"5065"}]
["5066",{"$f":"INDEX('Import data'!$A:$A,MATCH($A511,'Import data'!$A:$A,0),1)","v":"5066"}]
["5068",{"$f":"INDEX('Import data'!$A:$A,MATCH($A512,'Import data'!$A:$A,0),1)","v":"5068"}]
["5069",{"$f":"INDEX('Import data'!$A:$A,MATCH($A513,'Import data'!$A:$A,0),1)","v":"5069"}]
["5070",{"$f":"INDEX('Import data'!$A:$A,MATCH($A514,'Import data'!$A:$A,0),1)","v":"5070"}]
[{"$f":"ID","v":"5080"},{"$f":"INDEX('Import data'!$A:$A,MATCH($A515,'Import data'!$A:$A,0),1)","v":"5080"}]
["5085",{"$f":"INDEX('Import data'!$A:$A,MATCH($A516,'Import data'!$A:$A,0),1)","v":"5085"}]
["5086",{"$f":"INDEX('Import data'!$A:$A,MATCH($A517,'Import data'!$A:$A,0),1)","v":"5086"}]
["5087",{"$f":"INDEX('Import data'!$A:$A,MATCH($A518,'Import data'!$A:$A,0),1)","v":"5087"}]
["5088",{"$f":"INDEX('Import data'!$A:$A,MATCH($A519,'Import data'!$A:$A,0),1)","v":"5088"}]
["5089",{"$f":"INDEX('Import data'!$A:$A,MATCH($A520,'Import data'!$A:$A,0),1)","v":"5089"}]
["5090",{"$f":"INDEX('Import data'!$A:$A,MATCH($A521,'Import data'!$A:$A,0),1)","v":"5090"}]
["5091",{"$f":"INDEX('Import data'!$A:$A,MATCH($A522,'Import data'!$A:$A,0),1)","v":"5091"}]
["5092",{"$f":"INDEX('Import data'!$A:$A,MATCH($A523,'Import data'!$A:$A,0),1)","v":"5092"}]
["5093",{"$f":"INDEX('Import data'!$A:$A,MATCH($A524,'Import data'!$A:$A,0),1)","v":"5093"}]
["5096",{"$f":"INDEX('Import data'!$A:$A,MATCH($A525,'Import data'!$A:$A,0),1)","v":"5096"}]
["5097",{"$f":"INDEX('Import data'!$A:$A,MATCH($A526,'Import data'!$A:$A,0),1)","v":"5097"}]
["5100",{"$f":"INDEX('Import data'!$A:$A,MATCH($A527,'Import data'!$A:$A,0),1)","v":"5100"}]
["5101",{"$f":"INDEX('Import data'!$A:$A,MATCH($A528,'Import data'!$A:$A,0),1)","v":"5101"}]
["5102",{"$f":"INDEX('Import data'!$A:$A,MATCH($A529,'Import data'!$A:$A,0),1)","v":"5102"}]
["5103",{"$f":"INDEX('Import data'!$A:$A,MATCH($A530,'Import data'!$A:$A,0),1)","v":"5103"}]
["5104",{"$f":"INDEX('Import data'!$A:$A,MATCH($A531,'Import data'!$A:$A,0),1)","v":"5104"}]
["5105",{"$f":"INDEX('Import data'!$A:$A,MATCH($A532,'Import data'!$A:$A,0),1)","v":"5105"}]
["5106",{"$f":"INDEX('Import data'!$A:$A,MATCH($A533,'Import data'!$A:$A,0),1)","v":"5106"}]
["5107",{"$f":"INDEX('Import data'!$A:$A,MATCH($A534,'Import data'!$A:$A,0),1)","v":"5107"}]
["510",{"$f":"INDEX('Import data'!$A:$A,MATCH($A535,'Import data'!$A:$A,0),1)","v":"510"}]
["5110",{"$f":"INDEX('Import data'!$A:$A,MATCH($A536,'Import data'!$A:$A,0),1)","v":"5110"}]
["5113",{"$f":"INDEX('Import data'!$A:$A,MATCH($A537,'Import data'!$A:$A,0),1)","v":"5113"}]
["5114",{"$f":"INDEX('Import data'!$A:$A,MATCH($A538,'Import data'!$A:$A,0),1)","v":"5114"}]
["5115",{"$f":"INDEX('Import data'!$A:$A,MATCH($A539,'Import data'!$A:$A,0),1)","v":"5115"}]
["5116",{"$f":"INDEX('Import data'!$A:$A,MATCH($A540,'Import data'!$A:$A,0),1)","v":"5116"}]
["5117",{"$f":"INDEX('Import data'!$A:$A,MATCH($A541,'Import data'!$A:$A,0),1)","v":"5117"}]
["5118",{"$f":"INDEX('Import data'!$A:$A,MATCH($A542,'Import data'!$A:$A,0),1)","v":"5118"}]
["5120",{"$f":"INDEX('Import data'!$A:$A,MATCH($A543,'Import data'!$A:$A,0),1)","v":"5120"}]
["5121",{"$f":"INDEX('Import data'!$A:$A,MATCH($A544,'Import data'!$A:$A,0),1)","v":"5121"}]
["5122",{"$f":"INDEX('Import data'!$A:$A,MATCH($A545,'Import data'!$A:$A,0),1)","v":"5122"}]
["5123",{"$f":"INDEX('Import data'!$A:$A,MATCH($A546,'Import data'!$A:$A,0),1)","v":"5123"}]
["5123",{"$f":"INDEX('Import data'!$A:$A,MATCH($A547,'Import data'!$A:$A,0),1)","v":"5123"}]
["5124",{"$f":"INDEX('Import data'!$A:$A,MATCH($A548,'Import data'!$A:$A,0),1)","v":"5124"}]
["5126",{"$f":"INDEX('Import data'!$A:$A,MATCH($A549,'Import data'!$A:$A,0),1)","v":"5126"}]
["5127",{"$f":"INDEX('Import data'!$A:$A,MATCH($A550,'Import data'!$A:$A,0),1)","v":"5127"}]
["5128",{"$f":"INDEX('Import data'!$A:$A,MATCH($A551,'Import data'!$A:$A,0),1)","v":"5128"}]
["5130",{"$f":"INDEX('Import data'!$A:$A,MATCH($A552,'Import data'!$A:$A,0),1)","v":"5130"}]
["5131",{"$f":"INDEX('Import data'!$A:$A,MATCH($A553,'Import data'!$A:$A,0),1)","v":"5131"}]
["5132",{"$f":"INDEX('Import data'!$A:$A,MATCH($A554,'Import data'!$A:$A,0),1)","v":"5132"}]
["5135",{"$f":"INDEX('Import data'!$A:$A,MATCH($A555,'Import data'!$A:$A,0),1)","v":"5135"}]
["5136",{"$f":"INDEX('Import data'!$A:$A,MATCH($A556,'Import data'!$A:$A,0),1)","v":"5136"}]
["5137",{"$f":"INDEX('Import data'!$A:$A,MATCH($A557,'Import data'!$A:$A,0),1)","v":"5137"}]
["5140",{"$f":"INDEX('Import data'!$A:$A,MATCH($A558,'Import data'!$A:$A,0),1)","v":"5140"}]
["5142",{"$f":"INDEX('Import data'!$A:$A,MATCH($A559,'Import data'!$A:$A,0),1)","v":"5142"}]
["5145",{"$f":"INDEX('Import data'!$A:$A,MATCH($A560,'Import data'!$A:$A,0),1)","v":"5145"}]
["5147",{"$f":"INDEX('Import data'!$A:$A,MATCH($A561,'Import data'!$A:$A,0),1)","v":"5147"}]
["5147",{"$f":"INDEX('Import data'!$A:$A,MATCH($A562,'Import data'!$A:$A,0),1)","v":"5147"}]
["5150",{"$f":"INDEX('Import data'!$A:$A,MATCH($A563,'Import data'!$A:$A,0),1)","v":"5150"}]
["5151",{"$f":"INDEX('Import data'!$A:$A,MATCH($A564,'Import data'!$A:$A,0),1)","v":"5151"}]
["5152",{"$f":"INDEX('Import data'!$A:$A,MATCH($A565,'Import data'!$A:$A,0),1)","v":"5152"}]
["5153",{"$f":"INDEX('Import data'!$A:$A,MATCH($A566,'Import data'!$A:$A,0),1)","v":"5153"}]
["5157",{"$f":"INDEX('Import data'!$A:$A,MATCH($A567,'Import data'!$A:$A,0),1)","v":"5157"}]
["515",{"$f":"INDEX('Import data'!$A:$A,MATCH($A568,'Import data'!$A:$A,0),1)","v":"515"}]
["5160",{"$f":"INDEX('Import data'!$A:$A,MATCH($A569,'Import data'!$A:$A,0),1)","v":"5160"}]
["5164",{"$f":"INDEX('Import data'!$A:$A,MATCH($A570,'Import data'!$A:$A,0),1)","v":"5164"}]
["5165",{"$f":"INDEX('Import data'!$A:$A,MATCH($A571,'Import data'!$A:$A,0),1)","v":"5165"}]
["5167",{"$f":"INDEX('Import data'!$A:$A,MATCH($A572,'Import data'!$A:$A,0),1)","v":"5167"}]
["5169",{"$f":"INDEX('Import data'!$A:$A,MATCH($A573,'Import data'!$A:$A,0),1)","v":"5169"}]
["5170",{"$f":"INDEX('Import data'!$A:$A,MATCH($A574,'Import data'!$A:$A,0),1)","v":"5170"}]
["517",{"$f":"INDEX('Import data'!$A:$A,MATCH($A575,'Import data'!$A:$A,0),1)","v":"517"}]
["5180",{"$f":"INDEX('Import data'!$A:$A,MATCH($A576,'Import data'!$A:$A,0),1)","v":"5180"}]
["5181",{"$f":"INDEX('Import data'!$A:$A,MATCH($A577,'Import data'!$A:$A,0),1)","v":"5181"}]
["5182",{"$f":"INDEX('Import data'!$A:$A,MATCH($A578,'Import data'!$A:$A,0),1)","v":"5182"}]
[{"$f":"ID","v":"5183"},{"$f":"INDEX('Import data'!$A:$A,MATCH($A579,'Import data'!$A:$A,0),1)","v":"5183"}]
["5184",{"$f":"INDEX('Import data'!$A:$A,MATCH($A580,'Import data'!$A:$A,0),1)","v":"5184"}]
["5185",{"$f":"INDEX('Import data'!$A:$A,MATCH($A581,'Import data'!$A:$A,0),1)","v":"5185"}]
["5187",{"$f":"INDEX('Import data'!$A:$A,MATCH($A582,'Import data'!$A:$A,0),1)","v":"5187"}]
["5190",{"$f":"INDEX('Import data'!$A:$A,MATCH($A583,'Import data'!$A:$A,0),1)","v":"5190"}]
["5191",{"$f":"INDEX('Import data'!$A:$A,MATCH($A584,'Import data'!$A:$A,0),1)","v":"5191"}]
["5192",{"$f":"INDEX('Import data'!$A:$A,MATCH($A585,'Import data'!$A:$A,0),1)","v":"5192"}]
["5193",{"$f":"INDEX('Import data'!$A:$A,MATCH($A586,'Import data'!$A:$A,0),1)","v":"5193"}]
["5194",{"$f":"INDEX('Import data'!$A:$A,MATCH($A587,'Import data'!$A:$A,0),1)","v":"5194"}]
["5195",{"$f":"INDEX('Import data'!$A:$A,MATCH($A588,'Import data'!$A:$A,0),1)","v":"5195"}]
["5196",{"$f":"INDEX('Import data'!$A:$A,MATCH($A589,'Import data'!$A:$A,0),1)","v":"5196"}]
["5197",{"$f":"INDEX('Import data'!$A:$A,MATCH($A590,'Import data'!$A:$A,0),1)","v":"5197"}]
["5200",{"$f":"INDEX('Import data'!$A:$A,MATCH($A591,'Import data'!$A:$A,0),1)","v":"5200"}]
["5201",{"$f":"INDEX('Import data'!$A:$A,MATCH($A592,'Import data'!$A:$A,0),1)","v":"5201"}]
["5202",{"$f":"INDEX('Import data'!$A:$A,MATCH($A593,'Import data'!$A:$A,0),1)","v":"5202"}]
["5203",{"$f":"INDEX('Import data'!$A:$A,MATCH($A594,'Import data'!$A:$A,0),1)","v":"5203"}]
["5204",{"$f":"INDEX('Import data'!$A:$A,MATCH($A595,'Import data'!$A:$A,0),1)","v":"5204"}]
["5205",{"$f":"INDEX('Import data'!$A:$A,MATCH($A596,'Import data'!$A:$A,0),1)","v":"5205"}]
["5206",{"$f":"INDEX('Import data'!$A:$A,MATCH($A597,'Import data'!$A:$A,0),1)","v":"5206"}]
["5207",{"$f":"INDEX('Import data'!$A:$A,MATCH($A598,'Import data'!$A:$A,0),1)","v":"5207"}]
["5210",{"$f":"INDEX('Import data'!$A:$A,MATCH($A599,'Import data'!$A:$A,0),1)","v":"5210"}]
["5211",{"$f":"INDEX('Import data'!$A:$A,MATCH($A600,'Import data'!$A:$A,0),1)","v":"5211"}]
["5212",{"$f":"INDEX('Import data'!$A:$A,MATCH($A601,'Import data'!$A:$A,0),1)","v":"5212"}]
["5213",{"$f":"INDEX('Import data'!$A:$A,MATCH($A602,'Import data'!$A:$A,0),1)","v":"5213"}]
["5214",{"$f":"INDEX('Import data'!$A:$A,MATCH($A603,'Import data'!$A:$A,0),1)","v":"5214"}]
["5215",{"$f":"INDEX('Import data'!$A:$A,MATCH($A604,'Import data'!$A:$A,0),1)","v":"5215"}]
["5216",{"$f":"INDEX('Import data'!$A:$A,MATCH($A605,'Import data'!$A:$A,0),1)","v":"5216"}]
["5217",{"$f":"INDEX('Import data'!$A:$A,MATCH($A606,'Import data'!$A:$A,0),1)","v":"5217"}]
["5218",{"$f":"INDEX('Import data'!$A:$A,MATCH($A607,'Import data'!$A:$A,0),1)","v":"5218"}]
["5222",{"$f":"INDEX('Import data'!$A:$A,MATCH($A608,'Import data'!$A:$A,0),1)","v":"5222"}]
["5223",{"$f":"INDEX('Import data'!$A:$A,MATCH($A609,'Import data'!$A:$A,0),1)","v":"5223"}]
["5224",{"$f":"INDEX('Import data'!$A:$A,MATCH($A610,'Import data'!$A:$A,0),1)","v":"5224"}]
["5225",{"$f":"INDEX('Import data'!$A:$A,MATCH($A611,'Import data'!$A:$A,0),1)","v":"5225"}]
["5226",{"$f":"INDEX('Import data'!$A:$A,MATCH($A612,'Import data'!$A:$A,0),1)","v":"5226"}]
["5227",{"$f":"INDEX('Import data'!$A:$A,MATCH($A613,'Import data'!$A:$A,0),1)","v":"5227"}]
["5228",{"$f":"INDEX('Import data'!$A:$A,MATCH($A614,'Import data'!$A:$A,0),1)","v":"5228"}]
["5229",{"$f":"INDEX('Import data'!$A:$A,MATCH($A615,'Import data'!$A:$A,0),1)","v":"5229"}]
["5253",{"$f":"INDEX('Import data'!$A:$A,MATCH($A616,'Import data'!$A:$A,0),1)","v":"5253"}]
["5255",{"$f":"INDEX('Import data'!$A:$A,MATCH($A617,'Import data'!$A:$A,0),1)","v":"5255"}]
["537",{"$f":"INDEX('Import data'!$A:$A,MATCH($A618,'Import data'!$A:$A,0),1)","v":"537"}]
["539",{"$f":"INDEX('Import data'!$A:$A,MATCH($A619,'Import data'!$A:$A,0),1)","v":"539"}]
["541",{"$f":"INDEX('Import data'!$A:$A,MATCH($A620,'Import data'!$A:$A,0),1)","v":"541"}]
["542",{"$f":"INDEX('Import data'!$A:$A,MATCH($A621,'Import data'!$A:$A,0),1)","v":"542"}]
["544",{"$f":"INDEX('Import data'!$A:$A,MATCH($A622,'Import data'!$A:$A,0),1)","v":"544"}]
["545",{"$f":"INDEX('Import data'!$A:$A,MATCH($A623,'Import data'!$A:$A,0),1)","v":"545"}]
["548",{"$f":"INDEX('Import data'!$A:$A,MATCH($A624,'Import data'!$A:$A,0),1)","v":"548"}]
["549",{"$f":"INDEX('Import data'!$A:$A,MATCH($A625,'Import data'!$A:$A,0),1)","v":"549"}]
["553",{"$f":"INDEX('Import data'!$A:$A,MATCH($A626,'Import data'!$A:$A,0),1)","v":"553"}]
["557",{"$f":"INDEX('Import data'!$A:$A,MATCH($A627,'Import data'!$A:$A,0),1)","v":"557"}]
["559",{"$f":"INDEX('Import data'!$A:$A,MATCH($A628,'Import data'!$A:$A,0),1)","v":"559"}]
["576",{"$f":"INDEX('Import data'!$A:$A,MATCH($A629,'Import data'!$A:$A,0),1)","v":"576"}]
["577",{"$f":"INDEX('Import data'!$A:$A,MATCH($A630,'Import data'!$A:$A,0),1)","v":"577"}]
["596",{"$f":"INDEX('Import data'!$A:$A,MATCH($A631,'Import data'!$A:$A,0),1)","v":"596"}]
["6031",{"$f":"INDEX('Import data'!$A:$A,MATCH($A632,'Import data'!$A:$A,0),1)","v":"6031"}]
["6032",{"$f":"INDEX('Import data'!$A:$A,MATCH($A633,'Import data'!$A:$A,0),1)","v":"6032"}]
["6033",{"$f":"INDEX('Import data'!$A:$A,MATCH($A634,'Import data'!$A:$A,0),1)","v":"6033"}]
["6034",{"$f":"INDEX('Import data'!$A:$A,MATCH($A635,'Import data'!$A:$A,0),1)","v":"6034"}]
["6035",{"$f":"INDEX('Import data'!$A:$A,MATCH($A636,'Import data'!$A:$A,0),1)","v":"6035"}]
["6036",{"$f":"INDEX('Import data'!$A:$A,MATCH($A637,'Import data'!$A:$A,0),1)","v":"6036"}]
["6081",{"$f":"INDEX('Import data'!$A:$A,MATCH($A638,'Import data'!$A:$A,0),1)","v":"6081"}]
["6082",{"$f":"INDEX('Import data'!$A:$A,MATCH($A639,'Import data'!$A:$A,0),1)","v":"6082"}]
["6083",{"$f":"INDEX('Import data'!$A:$A,MATCH($A640,'Import data'!$A:$A,0),1)","v":"6083"}]
["6090",{"$f":"INDEX('Import data'!$A:$A,MATCH($A641,'Import data'!$A:$A,0),1)","v":"6090"}]
["6091",{"$f":"INDEX('Import data'!$A:$A,MATCH($A642,'Import data'!$A:$A,0),1)","v":"6091"}]
[{"$f":"ID","v":"6092"},{"$f":"INDEX('Import data'!$A:$A,MATCH($A643,'Import data'!$A:$A,0),1)","v":"6092"}]
["6093",{"$f":"INDEX('Import data'!$A:$A,MATCH($A644,'Import data'!$A:$A,0),1)","v":"6093"}]
["6105",{"$f":"INDEX('Import data'!$A:$A,MATCH($A645,'Import data'!$A:$A,0),1)","v":"6105"}]
["6106",{"$f":"INDEX('Import data'!$A:$A,MATCH($A646,'Import data'!$A:$A,0),1)","v":"6106"}]
["6108",{"$f":"INDEX('Import data'!$A:$A,MATCH($A647,'Import data'!$A:$A,0),1)","v":"6108"}]
["610",{"$f":"INDEX('Import data'!$A:$A,MATCH($A648,'Import data'!$A:$A,0),1)","v":"610"}]
["6111",{"$f":"INDEX('Import data'!$A:$A,MATCH($A649,'Import data'!$A:$A,0),1)","v":"6111"}]
["6112",{"$f":"INDEX('Import data'!$A:$A,MATCH($A650,'Import data'!$A:$A,0),1)","v":"6112"}]
["6113",{"$f":"INDEX('Import data'!$A:$A,MATCH($A651,'Import data'!$A:$A,0),1)","v":"6113"}]
["6114",{"$f":"INDEX('Import data'!$A:$A,MATCH($A652,'Import data'!$A:$A,0),1)","v":"6114"}]
["6115",{"$f":"INDEX('Import data'!$A:$A,MATCH($A653,'Import data'!$A:$A,0),1)","v":"6115"}]
["6116",{"$f":"INDEX('Import data'!$A:$A,MATCH($A654,'Import data'!$A:$A,0),1)","v":"6116"}]
["6118",{"$f":"INDEX('Import data'!$A:$A,MATCH($A655,'Import data'!$A:$A,0),1)","v":"6118"}]
["611",{"$f":"INDEX('Import data'!$A:$A,MATCH($A656,'Import data'!$A:$A,0),1)","v":"611"}]
["6120",{"$f":"INDEX('Import data'!$A:$A,MATCH($A657,'Import data'!$A:$A,0),1)","v":"6120"}]
["6121",{"$f":"INDEX('Import data'!$A:$A,MATCH($A658,'Import data'!$A:$A,0),1)","v":"6121"}]
["6122",{"$f":"INDEX('Import data'!$A:$A,MATCH($A659,'Import data'!$A:$A,0),1)","v":"6122"}]
["6123",{"$f":"INDEX('Import data'!$A:$A,MATCH($A660,'Import data'!$A:$A,0),1)","v":"6123"}]
["6140",{"$f":"INDEX('Import data'!$A:$A,MATCH($A661,'Import data'!$A:$A,0),1)","v":"6140"}]
["6141",{"$f":"INDEX('Import data'!$A:$A,MATCH($A662,'Import data'!$A:$A,0),1)","v":"6141"}]
["6146",{"$f":"INDEX('Import data'!$A:$A,MATCH($A663,'Import data'!$A:$A,0),1)","v":"6146"}]
["6148",{"$f":"INDEX('Import data'!$A:$A,MATCH($A664,'Import data'!$A:$A,0),1)","v":"6148"}]
["6150",{"$f":"INDEX('Import data'!$A:$A,MATCH($A665,'Import data'!$A:$A,0),1)","v":"6150"}]
["6151",{"$f":"INDEX('Import data'!$A:$A,MATCH($A666,'Import data'!$A:$A,0),1)","v":"6151"}]
["6153",{"$f":"INDEX('Import data'!$A:$A,MATCH($A667,'Import data'!$A:$A,0),1)","v":"6153"}]
["6154",{"$f":"INDEX('Import data'!$A:$A,MATCH($A668,'Import data'!$A:$A,0),1)","v":"6154"}]
["6155",{"$f":"INDEX('Import data'!$A:$A,MATCH($A669,'Import data'!$A:$A,0),1)","v":"6155"}]
["6156",{"$f":"INDEX('Import data'!$A:$A,MATCH($A670,'Import data'!$A:$A,0),1)","v":"6156"}]
["615",{"$f":"INDEX('Import data'!$A:$A,MATCH($A671,'Import data'!$A:$A,0),1)","v":"615"}]
["6161",{"$f":"INDEX('Import data'!$A:$A,MATCH($A672,'Import data'!$A:$A,0),1)","v":"6161"}]
["6163",{"$f":"INDEX('Import data'!$A:$A,MATCH($A673,'Import data'!$A:$A,0),1)","v":"6163"}]
["6164",{"$f":"INDEX('Import data'!$A:$A,MATCH($A674,'Import data'!$A:$A,0),1)","v":"6164"}]
["6165",{"$f":"INDEX('Import data'!$A:$A,MATCH($A675,'Import data'!$A:$A,0),1)","v":"6165"}]
["6166",{"$f":"INDEX('Import data'!$A:$A,MATCH($A676,'Import data'!$A:$A,0),1)","v":"6166"}]
["6167.01",{"$f":"INDEX('Import data'!$A:$A,MATCH($A677,'Import data'!$A:$A,0),1)","v":{"$error":"#N/A"}}]
["6167",{"$f":"INDEX('Import data'!$A:$A,MATCH($A678,'Import data'!$A:$A,0),1)","v":"6167"}]
["6168",{"$f":"INDEX('Import data'!$A:$A,MATCH($A679,'Import data'!$A:$A,0),1)","v":"6168"}]
["6170",{"$f":"INDEX('Import data'!$A:$A,MATCH($A680,'Import data'!$A:$A,0),1)","v":"6170"}]
["6171",{"$f":"INDEX('Import data'!$A:$A,MATCH($A681,'Import data'!$A:$A,0),1)","v":"6171"}]
["6172",{"$f":"INDEX('Import data'!$A:$A,MATCH($A682,'Import data'!$A:$A,0),1)","v":"6172"}]
["6173",{"$f":"INDEX('Import data'!$A:$A,MATCH($A683,'Import data'!$A:$A,0),1)","v":"6173"}]
["617",{"$f":"INDEX('Import data'!$A:$A,MATCH($A684,'Import data'!$A:$A,0),1)","v":"617"}]
["6180",{"$f":"INDEX('Import data'!$A:$A,MATCH($A685,'Import data'!$A:$A,0),1)","v":"6180"}]
["6181",{"$f":"INDEX('Import data'!$A:$A,MATCH($A686,'Import data'!$A:$A,0),1)","v":"6181"}]
["6182",{"$f":"INDEX('Import data'!$A:$A,MATCH($A687,'Import data'!$A:$A,0),1)","v":"6182"}]
["6183",{"$f":"INDEX('Import data'!$A:$A,MATCH($A688,'Import data'!$A:$A,0),1)","v":"6183"}]
["6190",{"$f":"INDEX('Import data'!$A:$A,MATCH($A689,'Import data'!$A:$A,0),1)","v":"6190"}]
["6191",{"$f":"INDEX('Import data'!$A:$A,MATCH($A690,'Import data'!$A:$A,0),1)","v":"6191"}]
["6192",{"$f":"INDEX('Import data'!$A:$A,MATCH($A691,'Import data'!$A:$A,0),1)","v":"6192"}]
["6193",{"$f":"INDEX('Import data'!$A:$A,MATCH($A692,'Import data'!$A:$A,0),1)","v":"6193"}]
["630",{"$f":"INDEX('Import data'!$A:$A,MATCH($A693,'Import data'!$A:$A,0),1)","v":"630"}]
["631",{"$f":"INDEX('Import data'!$A:$A,MATCH($A694,'Import data'!$A:$A,0),1)","v":"631"}]
["6346",{"$f":"INDEX('Import data'!$A:$A,MATCH($A695,'Import data'!$A:$A,0),1)","v":"6346"}]
["6352",{"$f":"INDEX('Import data'!$A:$A,MATCH($A696,'Import data'!$A:$A,0),1)","v":"6352"}]
["6355",{"$f":"INDEX('Import data'!$A:$A,MATCH($A697,'Import data'!$A:$A,0),1)","v":"6355"}]
["6361",{"$f":"INDEX('Import data'!$A:$A,MATCH($A698,'Import data'!$A:$A,0),1)","v":"6361"}]
["6370",{"$f":"INDEX('Import data'!$A:$A,MATCH($A699,'Import data'!$A:$A,0),1)","v":"6370"}]
["6376",{"$f":"INDEX('Import data'!$A:$A,MATCH($A700,'Import data'!$A:$A,0),1)","v":"6376"}]
["6379",{"$f":"INDEX('Import data'!$A:$A,MATCH($A701,'Import data'!$A:$A,0),1)","v":"6379"}]
["637",{"$f":"INDEX('Import data'!$A:$A,MATCH($A702,'Import data'!$A:$A,0),1)","v":"637"}]
["6385",{"$f":"INDEX('Import data'!$A:$A,MATCH($A703,'Import data'!$A:$A,0),1)","v":"6385"}]
["638",{"$f":"INDEX('Import data'!$A:$A,MATCH($A704,'Import data'!$A:$A,0),1)","v":"638"}]
["6401",{"$f":"INDEX('Import data'!$A:$A,MATCH($A705,'Import data'!$A:$A,0),1)","v":"6401"}]
["6402",{"$f":"INDEX('Import data'!$A:$A,MATCH($A706,'Import data'!$A:$A,0),1)","v":"6402"}]
[{"$f":"ID","v":"6403"},{"$f":"INDEX('Import data'!$A:$A,MATCH($A707,'Import data'!$A:$A,0),1)","v":"6403"}]
["6404",{"$f":"INDEX('Import data'!$A:$A,MATCH($A708,'Import data'!$A:$A,0),1)","v":"6404"}]
["6405",{"$f":"INDEX('Import data'!$A:$A,MATCH($A709,'Import data'!$A:$A,0),1)","v":"6405"}]
["6406",{"$f":"INDEX('Import data'!$A:$A,MATCH($A710,'Import data'!$A:$A,0),1)","v":"6406"}]
["6407",{"$f":"INDEX('Import data'!$A:$A,MATCH($A711,'Import data'!$A:$A,0),1)","v":"6407"}]
["6408",{"$f":"INDEX('Import data'!$A:$A,MATCH($A712,'Import data'!$A:$A,0),1)","v":"6408"}]
["6421",{"$f":"INDEX('Import data'!$A:$A,MATCH($A713,'Import data'!$A:$A,0),1)","v":"6421"}]
["6422",{"$f":"INDEX('Import data'!$A:$A,MATCH($A714,'Import data'!$A:$A,0),1)","v":"6422"}]
["6423",{"$f":"INDEX('Import data'!$A:$A,MATCH($A715,'Import data'!$A:$A,0),1)","v":"6423"}]
["6424",{"$f":"INDEX('Import data'!$A:$A,MATCH($A716,'Import data'!$A:$A,0),1)","v":"6424"}]
["6425",{"$f":"INDEX('Import data'!$A:$A,MATCH($A717,'Import data'!$A:$A,0),1)","v":"6425"}]
["6426",{"$f":"INDEX('Import data'!$A:$A,MATCH($A718,'Import data'!$A:$A,0),1)","v":"6426"}]
["6427",{"$f":"INDEX('Import data'!$A:$A,MATCH($A719,'Import data'!$A:$A,0),1)","v":"6427"}]
["6428",{"$f":"INDEX('Import data'!$A:$A,MATCH($A720,'Import data'!$A:$A,0),1)","v":"6428"}]
["6460",{"$f":"INDEX('Import data'!$A:$A,MATCH($A721,'Import data'!$A:$A,0),1)","v":"6460"}]
["6461",{"$f":"INDEX('Import data'!$A:$A,MATCH($A722,'Import data'!$A:$A,0),1)","v":"6461"}]
["6466",{"$f":"INDEX('Import data'!$A:$A,MATCH($A723,'Import data'!$A:$A,0),1)","v":"6466"}]
["6467",{"$f":"INDEX('Import data'!$A:$A,MATCH($A724,'Import data'!$A:$A,0),1)","v":"6467"}]
["6471",{"$f":"INDEX('Import data'!$A:$A,MATCH($A725,'Import data'!$A:$A,0),1)","v":"6471"}]
["6473",{"$f":"INDEX('Import data'!$A:$A,MATCH($A726,'Import data'!$A:$A,0),1)","v":"6473"}]
["6483",{"$f":"INDEX('Import data'!$A:$A,MATCH($A727,'Import data'!$A:$A,0),1)","v":"6483"}]
["6485",{"$f":"INDEX('Import data'!$A:$A,MATCH($A728,'Import data'!$A:$A,0),1)","v":"6485"}]
["655",{"$f":"INDEX('Import data'!$A:$A,MATCH($A729,'Import data'!$A:$A,0),1)","v":"655"}]
["6600",{"$f":"INDEX('Import data'!$A:$A,MATCH($A730,'Import data'!$A:$A,0),1)","v":"6600"}]
["6601",{"$f":"INDEX('Import data'!$A:$A,MATCH($A731,'Import data'!$A:$A,0),1)","v":"6601"}]
["6602",{"$f":"INDEX('Import data'!$A:$A,MATCH($A732,'Import data'!$A:$A,0),1)","v":"6602"}]
["6603",{"$f":"INDEX('Import data'!$A:$A,MATCH($A733,'Import data'!$A:$A,0),1)","v":"6603"}]
["660",{"$f":"INDEX('Import data'!$A:$A,MATCH($A734,'Import data'!$A:$A,0),1)","v":"660"}]
["661",{"$f":"INDEX('Import data'!$A:$A,MATCH($A735,'Import data'!$A:$A,0),1)","v":"661"}]
["668",{"$f":"INDEX('Import data'!$A:$A,MATCH($A736,'Import data'!$A:$A,0),1)","v":"668"}]
["6702",{"$f":"INDEX('Import data'!$A:$A,MATCH($A737,'Import data'!$A:$A,0),1)","v":"6702"}]
["6706",{"$f":"INDEX('Import data'!$A:$A,MATCH($A738,'Import data'!$A:$A,0),1)","v":"6706"}]
["6732",{"$f":"INDEX('Import data'!$A:$A,MATCH($A739,'Import data'!$A:$A,0),1)","v":"6732"}]
["6735",{"$f":"INDEX('Import data'!$A:$A,MATCH($A740,'Import data'!$A:$A,0),1)","v":"6735"}]
["6738",{"$f":"INDEX('Import data'!$A:$A,MATCH($A741,'Import data'!$A:$A,0),1)","v":"6738"}]
["6750",{"$f":"INDEX('Import data'!$A:$A,MATCH($A742,'Import data'!$A:$A,0),1)","v":"6750"}]
["6753",{"$f":"INDEX('Import data'!$A:$A,MATCH($A743,'Import data'!$A:$A,0),1)","v":"6753"}]
["6756",{"$f":"INDEX('Import data'!$A:$A,MATCH($A744,'Import data'!$A:$A,0),1)","v":"6756"}]
["675",{"$f":"INDEX('Import data'!$A:$A,MATCH($A745,'Import data'!$A:$A,0),1)","v":"675"}]
["676",{"$f":"INDEX('Import data'!$A:$A,MATCH($A746,'Import data'!$A:$A,0),1)","v":"676"}]
["6772",{"$f":"INDEX('Import data'!$A:$A,MATCH($A747,'Import data'!$A:$A,0),1)","v":"6772"}]
["6778",{"$f":"INDEX('Import data'!$A:$A,MATCH($A748,'Import data'!$A:$A,0),1)","v":"6778"}]
["7120",{"$f":"INDEX('Import data'!$A:$A,MATCH($A749,'Import data'!$A:$A,0),1)","v":"7120"}]
["7150",{"$f":"INDEX('Import data'!$A:$A,MATCH($A750,'Import data'!$A:$A,0),1)","v":"7150"}]
["7151",{"$f":"INDEX('Import data'!$A:$A,MATCH($A751,'Import data'!$A:$A,0),1)","v":"7151"}]
["7152",{"$f":"INDEX('Import data'!$A:$A,MATCH($A752,'Import data'!$A:$A,0),1)","v":"7152"}]
["7153",{"$f":"INDEX('Import data'!$A:$A,MATCH($A753,'Import data'!$A:$A,0),1)","v":"7153"}]
["7154",{"$f":"INDEX('Import data'!$A:$A,MATCH($A754,'Import data'!$A:$A,0),1)","v":"7154"}]
["7155",{"$f":"INDEX('Import data'!$A:$A,MATCH($A755,'Import data'!$A:$A,0),1)","v":"7155"}]
["718",{"$f":"INDEX('Import data'!$A:$A,MATCH($A756,'Import data'!$A:$A,0),1)","v":"718"}]
["724",{"$f":"INDEX('Import data'!$A:$A,MATCH($A757,'Import data'!$A:$A,0),1)","v":"724"}]
["725",{"$f":"INDEX('Import data'!$A:$A,MATCH($A758,'Import data'!$A:$A,0),1)","v":"725"}]
["750",{"$f":"INDEX('Import data'!$A:$A,MATCH($A759,'Import data'!$A:$A,0),1)","v":"750"}]
["777",{"$f":"INDEX('Import data'!$A:$A,MATCH($A760,'Import data'!$A:$A,0),1)","v":"777"}]
["796",{"$f":"INDEX('Import data'!$A:$A,MATCH($A761,'Import data'!$A:$A,0),1)","v":"796"}]
["800",{"$f":"INDEX('Import data'!$A:$A,MATCH($A762,'Import data'!$A:$A,0),1)","v":"800"}]
["800A",{"$f":"INDEX('Import data'!$A:$A,MATCH($A763,'Import data'!$A:$A,0),1)","v":"800A"}]
["805",{"$f":"INDEX('Import data'!$A:$A,MATCH($A764,'Import data'!$A:$A,0),1)","v":"805"}]
["810",{"$f":"INDEX('Import data'!$A:$A,MATCH($A765,'Import data'!$A:$A,0),1)","v":"810"}]
["820",{"$f":"INDEX('Import data'!$A:$A,MATCH($A766,'Import data'!$A:$A,0),1)","v":"820"}]
["830",{"$f":"INDEX('Import data'!$A:$A,MATCH($A767,'Import data'!$A:$A,0),1)","v":"830"}]
["866",{"$f":"INDEX('Import data'!$A:$A,MATCH($A768,'Import data'!$A:$A,0),1)","v":"866"}]
["891",{"$f":"INDEX('Import data'!$A:$A,MATCH($A769,'Import data'!$A:$A,0),1)","v":"891"}]
["893",{"$f":"INDEX('Import data'!$A:$A,MATCH($A770,'Import data'!$A:$A,0),1)","v":"893"}]
[{"$f":"ID","v":"901"},{"$f":"INDEX('Import data'!$A:$A,MATCH($A771,'Import data'!$A:$A,0),1)","v":"901"}]
[0,{"$f":"INDEX('Import data'!$A:$A,MATCH($A772,'Import data'!$A:$A,0),1)","v":{"$error":"#N/A"}}]
[0,{"$f":"INDEX('Import data'!$A:$A,MATCH($A773,'Import data'!$A:$A,0),1)","v":{"$error":"#N/A"}}]
[0,{"$f":"INDEX('Import data'!$A:$A,MATCH($A774,'Import data'!$A:$A,0),1)","v":{"$error":"#N/A"}}]
[0,{"$f":"INDEX('Import data'!$A:$A,MATCH($A775,'Import data'!$A:$A,0),1)","v":{"$error":"#N/A"}}]
[0,{"$f":"INDEX('Import data'!$A:$A,MATCH($A776,'Import data'!$A:$A,0),1)","v":{"$error":"#N/A"}}]
[0,{"$f":"INDEX('Import data'!$A:$A,MATCH($A777,'Import data'!$A:$A,0),1)","v":{"$error":"#N/A"}}]
[0,{"$f":"INDEX('Import data'!$A:$A,MATCH($A778,'Import data'!$A:$A,0),1)","v":{"$error":"#N/A"}}]
[0,{"$f":"INDEX('Import data'!$A:$A,MATCH($A779,'Import data'!$A:$A,0),1)","v":{"$error":"#N/A"}}]
[0,{"$f":"INDEX('Import data'!$A:$A,MATCH($A780,'Import data'!$A:$A,0),1)","v":{"$error":"#N/A"}}]
[0,{"$f":"INDEX('Import data'!$A:$A,MATCH($A781,'Import data'!$A:$A,0),1)","v":{"$error":"#N/A"}}]
[0,{"$f":"INDEX('Import data'!$A:$A,MATCH($A782,'Import data'!$A:$A,0),1)","v":{"$error":"#N/A"}}]
[0,{"$f":"INDEX('Import data'!$A:$A,MATCH($A783,'Import data'!$A:$A,0),1)","v":{"$error":"#N/A"}}]
[0,{"$f":"INDEX('Import data'!$A:$A,MATCH($A784,'Import data'!$A:$A,0),1)","v":{"$error":"#N/A"}}]
[0,{"$f":"INDEX('Import data'!$A:$A,MATCH($A785,'Import data'!$A:$A,0),1)","v":{"$error":"#N/A"}}]
[0,{"$f":"INDEX('Import data'!$A:$A,MATCH($A786,'Import data'!$A:$A,0),1)","v":{"$error":"#N/A"}}]
[0,{"$f":"INDEX('Import data'!$A:$A,MATCH($A787,'Import data'!$A:$A,0),1)","v":{"$error":"#N/A"}}]
[0,{"$f":"INDEX('Import data'!$A:$A,MATCH($A788,'Import data'!$A:$A,0),1)","v":{"$error":"#N/A"}}]
[0,{"$f":"INDEX('Import data'!$A:$A,MATCH($A789,'Import data'!$A:$A,0),1)","v":{"$error":"#N/A"}}]
[0,{"$f":"INDEX('Import data'!$A:$A,MATCH($A790,'Import data'!$A:$A,0),1)","v":{"$error":"#N/A"}}]
[0,{"$f":"INDEX('Import data'!$A:$A,MATCH($A791,'Import data'!$A:$A,0),1)","v":{"$error":"#N/A"}}]
[0,{"$f":"INDEX('Import data'!$A:$A,MATCH($A792,'Import data'!$A:$A,0),1)","v":{"$error":"#N/A"}}]
[0,{"$f":"INDEX('Import data'!$A:$A,MATCH($A793,'Import data'!$A:$A,0),1)","v":{"$error":"#N/A"}}]
[0,{"$f":"INDEX('Import data'!$A:$A,MATCH($A794,'Import data'!$A:$A,0),1)","v":{"$error":"#N/A"}}]
[0,{"$f":"INDEX('Import data'!$A:$A,MATCH($A795,'Import data'!$A:$A,0),1)","v":{"$error":"#N/A"}}]
[0,{"$f":"INDEX('Import data'!$A:$A,MATCH($A796,'Import data'!$A:$A,0),1)","v":{"$error":"#N/A"}}]
[0,{"$f":"INDEX('Import data'!$A:$A,MATCH($A797,'Import data'!$A:$A,0),1)","v":{"$error":"#N/A"}}]
[0,{"$f":"INDEX('Import data'!$A:$A,MATCH($A798,'Import data'!$A:$A,0),1)","v":{"$error":"#N/A"}}]
[0,{"$f":"INDEX('Import data'!$A:$A,MATCH($A799,'Import data'!$A:$A,0),1)","v":{"$error":"#N/A"}}]
[0,{"$f":"INDEX('Import data'!$A:$A,MATCH($A800,'Import data'!$A:$A,0),1)","v":{"$error":"#N/A"}}]
[0,{"$f":"INDEX('Import data'!$A:$A,MATCH($A801,'Import data'!$A:$A,0),1)","v":{"$error":"#N/A"}}]
[0,{"$f":"INDEX('Import data'!$A:$A,MATCH($A802,'Import data'!$A:$A,0),1)","v":{"$error":"#N/A"}}]
[0,{"$f":"INDEX('Import data'!$A:$A,MATCH($A803,'Import data'!$A:$A,0),1)","v":{"$error":"#N/A"}}]
[0,{"$f":"INDEX('Import data'!$A:$A,MATCH($A804,'Import data'!$A:$A,0),1)","v":{"$error":"#N/A"}}]
[0,{"$f":"INDEX('Import data'!$A:$A,MATCH($A805,'Import data'!$A:$A,0),1)","v":{"$error":"#N/A"}}]
[0,{"$f":"INDEX('Import data'!$A:$A,MATCH($A806,'Import data'!$A:$A,0),1)","v":{"$error":"#N/A"}}]
[0,{"$f":"INDEX('Import data'!$A:$A,MATCH($A807,'Import data'!$A:$A,0),1)","v":{"$error":"#N/A"}}]
[0,{"$f":"INDEX('Import data'!$A:$A,MATCH($A808,'Import data'!$A:$A,0),1)","v":{"$error":"#N/A"}}]
[0,{"$f":"INDEX('Import data'!$A:$A,MATCH($A809,'Import data'!$A:$A,0),1)","v":{"$error":"#N/A"}}]
[0,{"$f":"INDEX('Import data'!$A:$A,MATCH($A810,'Import data'!$A:$A,0),1)","v":{"$error":"#N/A"}}]
[0,{"$f":"INDEX('Import data'!$A:$A,MATCH($A811,'Import data'!$A:$A,0),1)","v":{"$error":"#N/A"}}]
[0,{"$f":"INDEX('Import data'!$A:$A,MATCH($A812,'Import data'!$A:$A,0),1)","v":{"$error":"#N/A"}}]
[0,{"$f":"INDEX('Import data'!$A:$A,MATCH($A813,'Import data'!$A:$A,0),1)","v":{"$error":"#N/A"}}]
[0,{"$f":"INDEX('Import data'!$A:$A,MATCH($A814,'Import data'!$A:$A,0),1)","v":{"$error":"#N/A"}}]
[0,{"$f":"INDEX('Import data'!$A:$A,MATCH($A815,'Import data'!$A:$A,0),1)","v":{"$error":"#N/A"}}]
[0,{"$f":"INDEX('Import data'!$A:$A,MATCH($A816,'Import data'!$A:$A,0),1)","v":{"$error":"#N/A"}}]
[0,{"$f":"INDEX('Import data'!$A:$A,MATCH($A817,'Import data'!$A:$A,0),1)","v":{"$error":"#N/A"}}]
[0,{"$f":"INDEX('Import data'!$A:$A,MATCH($A818,'Import data'!$A:$A,0),1)","v":{"$error":"#N/A"}}]
[0,{"$f":"INDEX('Import data'!$A:$A,MATCH($A819,'Import data'!$A:$A,0),1)","v":{"$error":"#N/A"}}]
[0,{"$f":"INDEX('Import data'!$A:$A,MATCH($A820,'Import data'!$A:$A,0),1)","v":{"$error":"#N/A"}}]
[0,{"$f":"INDEX('Import data'!$A:$A,MATCH($A821,'Import data'!$A:$A,0),1)","v":{"$error":"#N/A"}}]
[0,{"$f":"INDEX('Import data'!$A:$A,MATCH($A822,'Import data'!$A:$A,0),1)","v":{"$error":"#N/A"}}]
[0,{"$f":"INDEX('Import data'!$A:$A,MATCH($A823,'Import data'!$A:$A,0),1)","v":{"$error":"#N/A"}}]
[0,{"$f":"INDEX('Import data'!$A:$A,MATCH($A824,'Import data'!$A:$A,0),1)","v":{"$error":"#N/A"}}]
[0,{"$f":"INDEX('Import data'!$A:$A,MATCH($A825,'Import data'!$A:$A,0),1)","v":{"$error":"#N/A"}}]
[0,{"$f":"INDEX('Import data'!$A:$A,MATCH($A826,'Import data'!$A:$A,0),1)","v":{"$error":"#N/A"}}]
[0,{"$f":"INDEX('Import data'!$A:$A,MATCH($A827,'Import data'!$A:$A,0),1)","v":{"$error":"#N/A"}}]
[0,{"$f":"INDEX('Import data'!$A:$A,MATCH($A828,'Import data'!$A:$A,0),1)","v":{"$error":"#N/A"}}]
[0,{"$f":"INDEX('Import data'!$A:$A,MATCH($A829,'Import data'!$A:$A,0),1)","v":{"$error":"#N/A"}}]
[0,{"$f":"INDEX('Import data'!$A:$A,MATCH($A830,'Import data'!$A:$A,0),1)","v":{"$error":"#N/A"}}]
[0,{"$f":"INDEX('Import data'!$A:$A,MATCH($A831,'Import data'!$A:$A,0),1)","v":{"$error":"#N/A"}}]
[0,{"$f":"INDEX('Import data'!$A:$A,MATCH($A832,'Import data'!$A:$A,0),1)","v":{"$error":"#N/A"}}]
[0,{"$f":"INDEX('Import data'!$A:$A,MATCH($A833,'Import data'!$A:$A,0),1)","v":{"$error":"#N/A"}}]
[0,{"$f":"INDEX('Import data'!$A:$A,MATCH($A834,'Import data'!$A:$A,0),1)","v":{"$error":"#N/A"}}]
[{"$f":"ID","v":0},{"$f":"INDEX('Import data'!$A:$A,MATCH($A835,'Import data'!$A:$A,0),1)","v":{"$error":"#N/A"}}]
[0,{"$f":"INDEX('Import data'!$A:$A,MATCH($A836,'Import data'!$A:$A,0),1)","v":{"$error":"#N/A"}}]
[0,{"$f":"INDEX('Import data'!$A:$A,MATCH($A837,'Import data'!$A:$A,0),1)","v":{"$error":"#N/A"}}]
[0,{"$f":"INDEX('Import data'!$A:$A,MATCH($A838,'Import data'!$A:$A,0),1)","v":{"$error":"#N/A"}}]
[0,{"$f":"INDEX('Import data'!$A:$A,MATCH($A839,'Import data'!$A:$A,0),1)","v":{"$error":"#N/A"}}]
[0,{"$f":"INDEX('Import data'!$A:$A,MATCH($A840,'Import data'!$A:$A,0),1)","v":{"$error":"#N/A"}}]
[0,{"$f":"INDEX('Import data'!$A:$A,MATCH($A841,'Import data'!$A:$A,0),1)","v":{"$error":"#N/A"}}]
[0,{"$f":"INDEX('Import data'!$A:$A,MATCH($A842,'Import data'!$A:$A,0),1)","v":{"$error":"#N/A"}}]
[0,{"$f":"INDEX('Import data'!$A:$A,MATCH($A843,'Import data'!$A:$A,0),1)","v":{"$error":"#N/A"}}]
[0,{"$f":"INDEX('Import data'!$A:$A,MATCH($A844,'Import data'!$A:$A,0),1)","v":{"$error":"#N/A"}}]
[0,{"$f":"INDEX('Import data'!$A:$A,MATCH($A845,'Import data'!$A:$A,0),1)","v":{"$error":"#N/A"}}]
[0,{"$f":"INDEX('Import data'!$A:$A,MATCH($A846,'Import data'!$A:$A,0),1)","v":{"$error":"#N/A"}}]
[0,{"$f":"INDEX('Import data'!$A:$A,MATCH($A847,'Import data'!$A:$A,0),1)","v":{"$error":"#N/A"}}]
[0,{"$f":"INDEX('Import data'!$A:$A,MATCH($A848,'Import data'!$A:$A,0),1)","v":{"$error":"#N/A"}}]
[0,{"$f":"INDEX('Import data'!$A:$A,MATCH($A849,'Import data'!$A:$A,0),1)","v":{"$error":"#N/A"}}]
[0,{"$f":"INDEX('Import data'!$A:$A,MATCH($A850,'Import data'!$A:$A,0),1)","v":{"$error":"#N/A"}}]
[0,{"$f":"INDEX('Import data'!$A:$A,MATCH($A851,'Import data'!$A:$A,0),1)","v":{"$error":"#N/A"}}]
[0,{"$f":"INDEX('Import data'!$A:$A,MATCH($A852,'Import data'!$A:$A,0),1)","v":{"$error":"#N/A"}}]
[0,{"$f":"INDEX('Import data'!$A:$A,MATCH($A853,'Import data'!$A:$A,0),1)","v":{"$error":"#N/A"}}]
[0,{"$f":"INDEX('Import data'!$A:$A,MATCH($A854,'Import data'!$A:$A,0),1)","v":{"$error":"#N/A"}}]
[0,{"$f":"INDEX('Import data'!$A:$A,MATCH($A855,'Import data'!$A:$A,0),1)","v":{"$error":"#N/A"}}]
[0,{"$f":"INDEX('Import data'!$A:$A,MATCH($A856,'Import data'!$A:$A,0),1)","v":{"$error":"#N/A"}}]
[0,{"$f":"INDEX('Import data'!$A:$A,MATCH($A857,'Import data'!$A:$A,0),1)","v":{"$error":"#N/A"}}]
[0,{"$f":"INDEX('Import data'!$A:$A,MATCH($A858,'Import data'!$A:$A,0),1)","v":{"$error":"#N/A"}}]
[0,{"$f":"INDEX('Import data'!$A:$A,MATCH($A859,'Import data'!$A:$A,0),1)","v":{"$error":"#N/A"}}]
[0,{"$f":"INDEX('Import data'!$A:$A,MATCH($A860,'Import data'!$A:$A,0),1)","v":{"$error":"#N/A"}}]
[0,{"$f":"INDEX('Import data'!$A:$A,MATCH($A861,'Import data'!$A:$A,0),1)","v":{"$error":"#N/A"}}]
[0,{"$f":"INDEX('Import data'!$A:$A,MATCH($A862,'Import data'!$A:$A,0),1)","v":{"$error":"#N/A"}}]
[0,{"$f":"INDEX('Import data'!$A:$A,MATCH($A863,'Import data'!$A:$A,0),1)","v":{"$error":"#N/A"}}]
[0,{"$f":"INDEX('Import data'!$A:$A,MATCH($A864,'Import data'!$A:$A,0),1)","v":{"$error":"#N/A"}}]
[0,{"$f":"INDEX('Import data'!$A:$A,MATCH($A865,'Import data'!$A:$A,0),1)","v":{"$error":"#N/A"}}]
[0,{"$f":"INDEX('Import data'!$A:$A,MATCH($A866,'Import data'!$A:$A,0),1)","v":{"$error":"#N/A"}}]
[0,{"$f":"INDEX('Import data'!$A:$A,MATCH($A867,'Import data'!$A:$A,0),1)","v":{"$error":"#N/A"}}]
[0,{"$f":"INDEX('Import data'!$A:$A,MATCH($A868,'Import data'!$A:$A,0),1)","v":{"$error":"#N/A"}}]
[0,{"$f":"INDEX('Import data'!$A:$A,MATCH($A869,'Import data'!$A:$A,0),1)","v":{"$error":"#N/A"}}]
[0,{"$f":"INDEX('Import data'!$A:$A,MATCH($A870,'Import data'!$A:$A,0),1)","v":{"$error":"#N/A"}}]
[0,{"$f":"INDEX('Import data'!$A:$A,MATCH($A871,'Import data'!$A:$A,0),1)","v":{"$error":"#N/A"}}]
[0,{"$f":"INDEX('Import data'!$A:$A,MATCH($A872,'Import data'!$A:$A,0),1)","v":{"$error":"#N/A"}}]
[0,{"$f":"INDEX('Import data'!$A:$A,MATCH($A873,'Import data'!$A:$A,0),1)","v":{"$error":"#N/A"}}]
[0,{"$f":"INDEX('Import data'!$A:$A,MATCH($A874,'Import data'!$A:$A,0),1)","v":{"$error":"#N/A"}}]
[0,{"$f":"INDEX('Import data'!$A:$A,MATCH($A875,'Import data'!$A:$A,0),1)","v":{"$error":"#N/A"}}]
[0,{"$f":"INDEX('Import data'!$A:$A,MATCH($A876,'Import data'!$A:$A,0),1)","v":{"$error":"#N/A"}}]
[0,{"$f":"INDEX('Import data'!$A:$A,MATCH($A877,'Import data'!$A:$A,0),1)","v":{"$error":"#N/A"}}]
[0,{"$f":"INDEX('Import data'!$A:$A,MATCH($A878,'Import data'!$A:$A,0),1)","v":{"$error":"#N/A"}}]
[0,{"$f":"INDEX('Import data'!$A:$A,MATCH($A879,'Import data'!$A:$A,0),1)","v":{"$error":"#N/A"}}]
[0,{"$f":"INDEX('Import data'!$A:$A,MATCH($A880,'Import data'!$A:$A,0),1)","v":{"$error":"#N/A"}}]
[0,{"$f":"INDEX('Import data'!$A:$A,MATCH($A881,'Import data'!$A:$A,0),1)","v":{"$error":"#N/A"}}]
[0,{"$f":"INDEX('Import data'!$A:$A,MATCH($A882,'Import data'!$A:$A,0),1)","v":{"$error":"#N/A"}}]
[0,{"$f":"INDEX('Import data'!$A:$A,MATCH($A883,'Import data'!$A:$A,0),1)","v":{"$error":"#N/A"}}]
[0,{"$f":"INDEX('Import data'!$A:$A,MATCH($A884,'Import data'!$A:$A,0),1)","v":{"$error":"#N/A"}}]
[0,{"$f":"INDEX('Import data'!$A:$A,MATCH($A885,'Import data'!$A:$A,0),1)","v":{"$error":"#N/A"}}]
[0,{"$f":"INDEX('Import data'!$A:$A,MATCH($A886,'Import data'!$A:$A,0),1)","v":{"$error":"#N/A"}}]
[0,{"$f":"INDEX('Import data'!$A:$A,MATCH($A887,'Import data'!$A:$A,0),1)","v":{"$error":"#N/A"}}]
[0,{"$f":"INDEX('Import data'!$A:$A,MATCH($A888,'Import data'!$A:$A,0),1)","v":{"$error":"#N/A"}}]
[0,{"$f":"INDEX('Import data'!$A:$A,MATCH($A889,'Import data'!$A:$A,0),1)","v":{"$error":"#N/A"}}]
[0,{"$f":"INDEX('Import data'!$A:$A,MATCH($A890,'Import data'!$A:$A,0),1)","v":{"$error":"#N/A"}}]
[0,{"$f":"INDEX('Import data'!$A:$A,MATCH($A891,'Import data'!$A:$A,0),1)","v":{"$error":"#N/A"}}]
[0,{"$f":"INDEX('Import data'!$A:$A,MATCH($A892,'Import data'!$A:$A,0),1)","v":{"$error":"#N/A"}}]
[0,{"$f":"INDEX('Import data'!$A:$A,MATCH($A893,'Import data'!$A:$A,0),1)","v":{"$error":"#N/A"}}]
[0,{"$f":"INDEX('Import data'!$A:$A,MATCH($A894,'Import data'!$A:$A,0),1)","v":{"$error":"#N/A"}}]
[0,{"$f":"INDEX('Import data'!$A:$A,MATCH($A895,'Import data'!$A:$A,0),1)","v":{"$error":"#N/A"}}]
[0,{"$f":"INDEX('Import data'!$A:$A,MATCH($A896,'Import data'!$A:$A,0),1)","v":{"$error":"#N/A"}}]
[0,{"$f":"INDEX('Import data'!$A:$A,MATCH($A897,'Import data'!$A:$A,0),1)","v":{"$error":"#N/A"}}]
[0,{"$f":"INDEX('Import data'!$A:$A,MATCH($A898,'Import data'!$A:$A,0),1)","v":{"$error":"#N/A"}}]
[{"$f":"ID","v":0},{"$f":"INDEX('Import data'!$A:$A,MATCH($A899,'Import data'!$A:$A,0),1)","v":{"$error":"#N/A"}}]
[0,{"$f":"INDEX('Import data'!$A:$A,MATCH($A900,'Import data'!$A:$A,0),1)","v":{"$error":"#N/A"}}]
[0,{"$f":"INDEX('Import data'!$A:$A,MATCH($A901,'Import data'!$A:$A,0),1)","v":{"$error":"#N/A"}}]
[0,{"$f":"INDEX('Import data'!$A:$A,MATCH($A902,'Import data'!$A:$A,0),1)","v":{"$error":"#N/A"}}]
[0,{"$f":"INDEX('Import data'!$A:$A,MATCH($A903,'Import data'!$A:$A,0),1)","v":{"$error":"#N/A"}}]
[0,{"$f":"INDEX('Import data'!$A:$A,MATCH($A904,'Import data'!$A:$A,0),1)","v":{"$error":"#N/A"}}]
[0,{"$f":"INDEX('Import data'!$A:$A,MATCH($A905,'Import data'!$A:$A,0),1)","v":{"$error":"#N/A"}}]
[0,{"$f":"INDEX('Import data'!$A:$A,MATCH($A906,'Import data'!$A:$A,0),1)","v":{"$error":"#N/A"}}]
[0,{"$f":"INDEX('Import data'!$A:$A,MATCH($A907,'Import data'!$A:$A,0),1)","v":{"$error":"#N/A"}}]
[0,{"$f":"INDEX('Import data'!$A:$A,MATCH($A908,'Import data'!$A:$A,0),1)","v":{"$error":"#N/A"}}]
[0,{"$f":"INDEX('Import data'!$A:$A,MATCH($A909,'Import data'!$A:$A,0),1)","v":{"$error":"#N/A"}}]
[0,{"$f":"INDEX('Import data'!$A:$A,MATCH($A910,'Import data'!$A:$A,0),1)","v":{"$error":"#N/A"}}]
[0,{"$f":"INDEX('Import data'!$A:$A,MATCH($A911,'Import data'!$A:$A,0),1)","v":{"$error":"#N/A"}}]
[0,{"$f":"INDEX('Import data'!$A:$A,MATCH($A912,'Import data'!$A:$A,0),1)","v":{"$error":"#N/A"}}]
[0,{"$f":"INDEX('Import data'!$A:$A,MATCH($A913,'Import data'!$A:$A,0),1)","v":{"$error":"#N/A"}}]
[0,{"$f":"INDEX('Import data'!$A:$A,MATCH($A914,'Import data'!$A:$A,0),1)","v":{"$error":"#N/A"}}]
[0,{"$f":"INDEX('Import data'!$A:$A,MATCH($A915,'Import data'!$A:$A,0),1)","v":{"$error":"#N/A"}}]
[0,{"$f":"INDEX('Import data'!$A:$A,MATCH($A916,'Import data'!$A:$A,0),1)","v":{"$error":"#N/A"}}]
[0,{"$f":"INDEX('Import data'!$A:$A,MATCH($A917,'Import data'!$A:$A,0),1)","v":{"$error":"#N/A"}}]
[0,{"$f":"INDEX('Import data'!$A:$A,MATCH($A918,'Import data'!$A:$A,0),1)","v":{"$error":"#N/A"}}]
[0,{"$f":"INDEX('Import data'!$A:$A,MATCH($A919,'Import data'!$A:$A,0),1)","v":{"$error":"#N/A"}}]
[0,{"$f":"INDEX('Import data'!$A:$A,MATCH($A920,'Import data'!$A:$A,0),1)","v":{"$error":"#N/A"}}]
[0,{"$f":"INDEX('Import data'!$A:$A,MATCH($A921,'Import data'!$A:$A,0),1)","v":{"$error":"#N/A"}}]
[0,{"$f":"INDEX('Import data'!$A:$A,MATCH($A922,'Import data'!$A:$A,0),1)","v":{"$error":"#N/A"}}]
[0,{"$f":"INDEX('Import data'!$A:$A,MATCH($A923,'Import data'!$A:$A,0),1)","v":{"$error":"#N/A"}}]
[0,{"$f":"INDEX('Import data'!$A:$A,MATCH($A924,'Import data'!$A:$A,0),1)","v":{"$error":"#N/A"}}]
[0,{"$f":"INDEX('Import data'!$A:$A,MATCH($A925,'Import data'!$A:$A,0),1)","v":{"$error":"#N/A"}}]
[0,{"$f":"INDEX('Import data'!$A:$A,MATCH($A926,'Import data'!$A:$A,0),1)","v":{"$error":"#N/A"}}]
[0,{"$f":"INDEX('Import data'!$A:$A,MATCH($A927,'Import data'!$A:$A,0),1)","v":{"$error":"#N/A"}}]
[0,{"$f":"INDEX('Import data'!$A:$A,MATCH($A928,'Import data'!$A:$A,0),1)","v":{"$error":"#N/A"}}]
[0,{"$f":"INDEX('Import data'!$A:$A,MATCH($A929,'Import data'!$A:$A,0),1)","v":{"$error":"#N/A"}}]
[0,{"$f":"INDEX('Import data'!$A:$A,MATCH($A930,'Import data'!$A:$A,0),1)","v":{"$error":"#N/A"}}]
[0,{"$f":"INDEX('Import data'!$A:$A,MATCH($A931,'Import data'!$A:$A,0),1)","v":{"$error":"#N/A"}}]
[0,{"$f":"INDEX('Import data'!$A:$A,MATCH($A932,'Import data'!$A:$A,0),1)","v":{"$error":"#N/A"}}]
[0,{"$f":"INDEX('Import data'!$A:$A,MATCH($A933,'Import data'!$A:$A,0),1)","v":{"$error":"#N/A"}}]
[0,{"$f":"INDEX('Import data'!$A:$A,MATCH($A934,'Import data'!$A:$A,0),1)","v":{"$error":"#N/A"}}]
[0,{"$f":"INDEX('Import data'!$A:$A,MATCH($A935,'Import data'!$A:$A,0),1)","v":{"$error":"#N/A"}}]
[0,{"$f":"INDEX('Import data'!$A:$A,MATCH($A936,'Import data'!$A:$A,0),1)","v":{"$error":"#N/A"}}]
[0,{"$f":"INDEX('Import data'!$A:$A,MATCH($A937,'Import data'!$A:$A,0),1)","v":{"$error":"#N/A"}}]
[0,{"$f":"INDEX('Import data'!$A:$A,MATCH($A938,'Import data'!$A:$A,0),1)","v":{"$error":"#N/A"}}]
[0,{"$f":"INDEX('Import data'!$A:$A,MATCH($A939,'Import data'!$A:$A,0),1)","v":{"$error":"#N/A"}}]
[0,{"$f":"INDEX('Import data'!$A:$A,MATCH($A940,'Import data'!$A:$A,0),1)","v":{"$error":"#N/A"}}]
[0,{"$f":"INDEX('Import data'!$A:$A,MATCH($A941,'Import data'!$A:$A,0),1)","v":{"$error":"#N/A"}}]
[0,{"$f":"INDEX('Import data'!$A:$A,MATCH($A942,'Import data'!$A:$A,0),1)","v":{"$error":"#N/A"}}]
[0,{"$f":"INDEX('Import data'!$A:$A,MATCH($A943,'Import data'!$A:$A,0),1)","v":{"$error":"#N/A"}}]
[0,{"$f":"INDEX('Import data'!$A:$A,MATCH($A944,'Import data'!$A:$A,0),1)","v":{"$error":"#N/A"}}]
[0,{"$f":"INDEX('Import data'!$A:$A,MATCH($A945,'Import data'!$A:$A,0),1)","v":{"$error":"#N/A"}}]
[0,{"$f":"INDEX('Import data'!$A:$A,MATCH($A946,'Import data'!$A:$A,0),1)","v":{"$error":"#N/A"}}]
[0,{"$f":"INDEX('Import data'!$A:$A,MATCH($A947,'Import data'!$A:$A,0),1)","v":{"$error":"#N/A"}}]
[0,{"$f":"INDEX('Import data'!$A:$A,MATCH($A948,'Import data'!$A:$A,0),1)","v":{"$error":"#N/A"}}]
[0,{"$f":"INDEX('Import data'!$A:$A,MATCH($A949,'Import data'!$A:$A,0),1)","v":{"$error":"#N/A"}}]
[0,{"$f":"INDEX('Import data'!$A:$A,MATCH($A950,'Import data'!$A:$A,0),1)","v":{"$error":"#N/A"}}]
[0,{"$f":"INDEX('Import data'!$A:$A,MATCH($A951,'Import data'!$A:$A,0),1)","v":{"$error":"#N/A"}}]
[0,{"$f":"INDEX('Import data'!$A:$A,MATCH($A952,'Import data'!$A:$A,0),1)","v":{"$error":"#N/A"}}]
[0,{"$f":"INDEX('Import data'!$A:$A,MATCH($A953,'Import data'!$A:$A,0),1)","v":{"$error":"#N/A"}}]
[0,{"$f":"INDEX('Import data'!$A:$A,MATCH($A954,'Import data'!$A:$A,0),1)","v":{"$error":"#N/A"}}]
[0,{"$f":"INDEX('Import data'!$A:$A,MATCH($A955,'Import data'!$A:$A,0),1)","v":{"$error":"#N/A"}}]
[0,{"$f":"INDEX('Import data'!$A:$A,MATCH($A956,'Import data'!$A:$A,0),1)","v":{"$error":"#N/A"}}]
[0,{"$f":"INDEX('Import data'!$A:$A,MATCH($A957,'Import data'!$A:$A,0),1)","v":{"$error":"#N/A"}}]
[0,{"$f":"INDEX('Import data'!$A:$A,MATCH($A958,'Import data'!$A:$A,0),1)","v":{"$error":"#N/A"}}]
[0,{"$f":"INDEX('Import data'!$A:$A,MATCH($A959,'Import data'!$A:$A,0),1)","v":{"$error":"#N/A"}}]
[0,{"$f":"INDEX('Import data'!$A:$A,MATCH($A960,'Import data'!$A:$A,0),1)","v":{"$error":"#N/A"}}]
[0,{"$f":"INDEX('Import data'!$A:$A,MATCH($A961,'Import data'!$A:$A,0),1)","v":{"$error":"#N/A"}}]
[0,{"$f":"INDEX('Import data'!$A:$A,MATCH($A962,'Import data'!$A:$A,0),1)","v":{"$error":"#N/A"}}]
[{"$f":"ID","v":0},{"$f":"INDEX('Import data'!$A:$A,MATCH($A963,'Import data'!$A:$A,0),1)","v":{"$error":"#N/A"}}]
[0,{"$f":"INDEX('Import data'!$A:$A,MATCH($A964,'Import data'!$A:$A,0),1)","v":{"$error":"#N/A"}}]
[0,{"$f":"INDEX('Import data'!$A:$A,MATCH($A965,'Import data'!$A:$A,0),1)","v":{"$error":"#N/A"}}]
[0,{"$f":"INDEX('Import data'!$A:$A,MATCH($A966,'Import data'!$A:$A,0),1)","v":{"$error":"#N/A"}}]
[0,{"$f":"INDEX('Import data'!$A:$A,MATCH($A967,'Import data'!$A:$A,0),1)","v":{"$error":"#N/A"}}]
[0,{"$f":"INDEX('Import data'!$A:$A,MATCH($A968,'Import data'!$A:$A,0),1)","v":{"$error":"#N/A"}}]
[0,{"$f":"INDEX('Import data'!$A:$A,MATCH($A969,'Import data'!$A:$A,0),1)","v":{"$error":"#N/A"}}]
[0,{"$f":"INDEX('Import data'!$A:$A,MATCH($A970,'Import data'!$A:$A,0),1)","v":{"$error":"#N/A"}}]
[0,{"$f":"INDEX('Import data'!$A:$A,MATCH($A971,'Import data'!$A:$A,0),1)","v":{"$error":"#N/A"}}]
[0,{"$f":"INDEX('Import data'!$A:$A,MATCH($A972,'Import data'!$A:$A,0),1)","v":{"$error":"#N/A"}}]
[0,{"$f":"INDEX('Import data'!$A:$A,MATCH($A973,'Import data'!$A:$A,0),1)","v":{"$error":"#N/A"}}]
[0,{"$f":"INDEX('Import data'!$A:$A,MATCH($A974,'Import data'!$A:$A,0),1)","v":{"$error":"#N/A"}}]
[0,{"$f":"INDEX('Import data'!$A:$A,MATCH($A975,'Import data'!$A:$A,0),1)","v":{"$error":"#N/A"}}]
[0,{"$f":"INDEX('Import data'!$A:$A,MATCH($A976,'Import data'!$A:$A,0),1)","v":{"$error":"#N/A"}}]
[0,{"$f":"INDEX('Import data'!$A:$A,MATCH($A977,'Import data'!$A:$A,0),1)","v":{"$error":"#N/A"}}]
[0,{"$f":"INDEX('Import data'!$A:$A,MATCH($A978,'Import data'!$A:$A,0),1)","v":{"$error":"#N/A"}}]
[0,{"$f":"INDEX('Import data'!$A:$A,MATCH($A979,'Import data'!$A:$A,0),1)","v":{"$error":"#N/A"}}]
[0,{"$f":"INDEX('Import data'!$A:$A,MATCH($A980,'Import data'!$A:$A,0),1)","v":{"$error":"#N/A"}}]
[0,{"$f":"INDEX('Import data'!$A:$A,MATCH($A981,'Import data'!$A:$A,0),1)","v":{"$error":"#N/A"}}]
[0,{"$f":"INDEX('Import data'!$A:$A,MATCH($A982,'Import data'!$A:$A,0),1)","v":{"$error":"#N/A"}}]
[0,{"$f":"INDEX('Import data'!$A:$A,MATCH($A983,'Import data'!$A:$A,0),1)","v":{"$error":"#N/A"}}]
[0,{"$f":"INDEX('Import data'!$A:$A,MATCH($A984,'Import data'!$A:$A,0),1)","v":{"$error":"#N/A"}}]
[0,{"$f":"INDEX('Import data'!$A:$A,MATCH($A985,'Import data'!$A:$A,0),1)","v":{"$error":"#N/A"}}]
[0,{"$f":"INDEX('Import data'!$A:$A,MATCH($A986,'Import data'!$A:$A,0),1)","v":{"$error":"#N/A"}}]
[0,{"$f":"INDEX('Import data'!$A:$A,MATCH($A987,'Import data'!$A:$A,0),1)","v":{"$error":"#N/A"}}]
[0,{"$f":"INDEX('Import data'!$A:$A,MATCH($A988,'Import data'!$A:$A,0),1)","v":{"$error":"#N/A"}}]
[0,{"$f":"INDEX('Import data'!$A:$A,MATCH($A989,'Import data'!$A:$A,0),1)","v":{"$error":"#N/A"}}]
[0,{"$f":"INDEX('Import data'!$A:$A,MATCH($A990,'Import data'!$A:$A,0),1)","v":{"$error":"#N/A"}}]
[0,{"$f":"INDEX('Import data'!$A:$A,MATCH($A991,'Import data'!$A:$A,0),1)","v":{"$error":"#N/A"}}]
[0,{"$f":"INDEX('Import data'!$A:$A,MATCH($A992,'Import data'!$A:$A,0),1)","v":{"$error":"#N/A"}}]
[0,{"$f":"INDEX('Import data'!$A:$A,MATCH($A993,'Import data'!$A:$A,0),1)","v":{"$error":"#N/A"}}]
[0,{"$f":"INDEX('Import data'!$A:$A,MATCH($A994,'Import data'!$A:$A,0),1)","v":{"$error":"#N/A"}}]
[0,{"$f":"INDEX('Import data'!$A:$A,MATCH($A995,'Import data'!$A:$A,0),1)","v":{"$error":"#N/A"}}]
[0,{"$f":"INDEX('Import data'!$A:$A,MATCH($A996,'Import data'!$A:$A,0),1)","v":{"$error":"#N/A"}}]
[0,{"$f":"INDEX('Import data'!$A:$A,MATCH($A997,'Import data'!$A:$A,0),1)","v":{"$error":"#N/A"}}]
[0,{"$f":"INDEX('Import data'!$A:$A,MATCH($A998,'Import data'!$A:$A,0),1)","v":{"$error":"#N/A"}}]
[0,{"$f":"INDEX('Import data'!$A:$A,MATCH($A999,'Import data'!$A:$A,0),1)","v":{"$error":"#N/A"}}]
[0,{"$f":"INDEX('Import data'!$A:$A,MATCH($A1000,'Import data'!$A:$A,0),1)","v":{"$error":"#N/A"}}]
[0,{"$f":"INDEX('Import data'!$A:$A,MATCH($A1001,'Import data'!$A:$A,0),1)","v":{"$error":"#N/A"}}]
[0,{"$f":"INDEX('Import data'!$A:$A,MATCH($A1002,'Import data'!$A:$A,0),1)","v":{"$error":"#N/A"}}]
[0,{"$f":"INDEX('Import data'!$A:$A,MATCH($A1003,'Import data'!$A:$A,0),1)","v":{"$error":"#N/A"}}]
[0,{"$f":"INDEX('Import data'!$A:$A,MATCH($A1004,'Import data'!$A:$A,0),1)","v":{"$error":"#N/A"}}]
[0,{"$f":"INDEX('Import data'!$A:$A,MATCH($A1005,'Import data'!$A:$A,0),1)","v":{"$error":"#N/A"}}]
[0,{"$f":"INDEX('Import data'!$A:$A,MATCH($A1006,'Import data'!$A:$A,0),1)","v":{"$error":"#N/A"}}]
[0,{"$f":"INDEX('Import data'!$A:$A,MATCH($A1007,'Import data'!$A:$A,0),1)","v":{"$error":"#N/A"}}]
[0,{"$f":"INDEX('Import data'!$A:$A,MATCH($A1008,'Import data'!$A:$A,0),1)","v":{"$error":"#N/A"}}]
[0,{"$f":"INDEX('Import data'!$A:$A,MATCH($A1009,'Import data'!$A:$A,0),1)","v":{"$error":"#N/A"}}]
[0,{"$f":"INDEX('Import data'!$A:$A,MATCH($A1010,'Import data'!$A:$A,0),1)","v":{"$error":"#N/A"}}]
[0,{"$f":"INDEX('Import data'!$A:$A,MATCH($A1011,'Import data'!$A:$A,0),1)","v":{"$error":"#N/A"}}]
[0,{"$f":"INDEX('Import data'!$A:$A,MATCH($A1012,'Import data'!$A:$A,0),1)","v":{"$error":"#N/A"}}]
[0,{"$f":"INDEX('Import data'!$A:$A,MATCH($A1013,'Import data'!$A:$A,0),1)","v":{"$error":"#N/A"}}]
[0,{"$f":"INDEX('Import data'!$A:$A,MATCH($A1014,'Import data'!$A:$A,0),1)","v":{"$error":"#N/A"}}]
[0,{"$f":"INDEX('Import data'!$A:$A,MATCH($A1015,'Import data'!$A:$A,0),1)","v":{"$error":"#N/A"}}]
[0,{"$f":"INDEX('Import data'!$A:$A,MATCH($A1016,'Import data'!$A:$A,0),1)","v":{"$error":"#N/A"}}]
[0,{"$f":"INDEX('Import data'!$A:$A,MATCH($A1017,'Import data'!$A:$A,0),1)","v":{"$error":"#N/A"}}]
[0,{"$f":"INDEX('Import data'!$A:$A,MATCH($A1018,'Import data'!$A:$A,0),1)","v":{"$error":"#N/A"}}]
[0,{"$f":"INDEX('Import data'!$A:$A,MATCH($A1019,'Import data'!$A:$A,0),1)","v":{"$error":"#N/A"}}]
[0,{"$f":"INDEX('Import data'!$A:$A,MATCH($A1020,'Import data'!$A:$A,0),1)","v":{"$error":"#N/A"}}]
[0,{"$f":"INDEX('Import data'!$A:$A,MATCH($A1021,'Import data'!$A:$A,0),1)","v":{"$error":"#N/A"}}]
[0,{"$f":"INDEX('Import data'!$A:$A,MATCH($A1022,'Import data'!$A:$A,0),1)","v":{"$error":"#N/A"}}]
[0,{"$f":"INDEX('Import data'!$A:$A,MATCH($A1023,'Import data'!$A:$A,0),1)","v":{"$error":"#N/A"}}]
[0,{"$f":"INDEX('Import data'!$A:$A,MATCH($A1024,'Import data'!$A:$A,0),1)","v":{"$error":"#N/A"}}]
[0,{"$f":"INDEX('Import data'!$A:$A,MATCH($A1025,'Import data'!$A:$A,0),1)","v":{"$error":"#N/A"}}]
[0,{"$f":"INDEX('Import data'!$A:$A,MATCH($A1026,'Import data'!$A:$A,0),1)","v":{"$error":"#N/A"}}]
[{"$f":"ID","v":0},{"$f":"INDEX('Import data'!$A:$A,MATCH($A1027,'Import data'!$A:$A,0),1)","v":{"$error":"#N/A"}}]
[0,{"$f":"INDEX('Import data'!$A:$A,MATCH($A1028,'Import data'!$A:$A,0),1)","v":{"$error":"#N/A"}}]
[0,{"$f":"INDEX('Import data'!$A:$A,MATCH($A1029,'Import data'!$A:$A,0),1)","v":{"$error":"#N/A"}}]
[0,{"$f":"INDEX('Import data'!$A:$A,MATCH($A1030,'Import data'!$A:$A,0),1)","v":{"$error":"#N/A"}}]
[0,{"$f":"INDEX('Import data'!$A:$A,MATCH($A1031,'Import data'!$A:$A,0),1)","v":{"$error":"#N/A"}}]
[0,{"$f":"INDEX('Import data'!$A:$A,MATCH($A1032,'Import data'!$A:$A,0),1)","v":{"$error":"#N/A"}}]
[0,{"$f":"INDEX('Import data'!$A:$A,MATCH($A1033,'Import data'!$A:$A,0),1)","v":{"$error":"#N/A"}}]
[0,{"$f":"INDEX('Import data'!$A:$A,MATCH($A1034,'Import data'!$A:$A,0),1)","v":{"$error":"#N/A"}}]
[0,{"$f":"INDEX('Import data'!$A:$A,MATCH($A1035,'Import data'!$A:$A,0),1)","v":{"$error":"#N/A"}}]
[0,{"$f":"INDEX('Import data'!$A:$A,MATCH($A1036,'Import data'!$A:$A,0),1)","v":{"$error":"#N/A"}}]
[0,{"$f":"INDEX('Import data'!$A:$A,MATCH($A1037,'Import data'!$A:$A,0),1)","v":{"$error":"#N/A"}}]
[0,{"$f":"INDEX('Import data'!$A:$A,MATCH($A1038,'Import data'!$A:$A,0),1)","v":{"$error":"#N/A"}}]
[0,{"$f":"INDEX('Import data'!$A:$A,MATCH($A1039,'Import data'!$A:$A,0),1)","v":{"$error":"#N/A"}}]
[0,{"$f":"INDEX('Import data'!$A:$A,MATCH($A1040,'Import data'!$A:$A,0),1)","v":{"$error":"#N/A"}}]
[0,{"$f":"INDEX('Import data'!$A:$A,MATCH($A1041,'Import data'!$A:$A,0),1)","v":{"$error":"#N/A"}}]
[0,{"$f":"INDEX('Import data'!$A:$A,MATCH($A1042,'Import data'!$A:$A,0),1)","v":{"$error":"#N/A"}}]
[0,{"$f":"INDEX('Import data'!$A:$A,MATCH($A1043,'Import data'!$A:$A,0),1)","v":{"$error":"#N/A"}}]
[0,{"$f":"INDEX('Import data'!$A:$A,MATCH($A1044,'Import data'!$A:$A,0),1)","v":{"$error":"#N/A"}}]
[0,{"$f":"INDEX('Import data'!$A:$A,MATCH($A1045,'Import data'!$A:$A,0),1)","v":{"$error":"#N/A"}}]
[0,{"$f":"INDEX('Import data'!$A:$A,MATCH($A1046,'Import data'!$A:$A,0),1)","v":{"$error":"#N/A"}}]
[0,{"$f":"INDEX('Import data'!$A:$A,MATCH($A1047,'Import data'!$A:$A,0),1)","v":{"$error":"#N/A"}}]
[0,{"$f":"INDEX('Import data'!$A:$A,MATCH($A1048,'Import data'!$A:$A,0),1)","v":{"$error":"#N/A"}}]
[0,{"$f":"INDEX('Import data'!$A:$A,MATCH($A1049,'Import data'!$A:$A,0),1)","v":{"$error":"#N/A"}}]
[0,{"$f":"INDEX('Import data'!$A:$A,MATCH($A1050,'Import data'!$A:$A,0),1)","v":{"$error":"#N/A"}}]
[0,{"$f":"INDEX('Import data'!$A:$A,MATCH($A1051,'Import data'!$A:$A,0),1)","v":{"$error":"#N/A"}}]
[0,{"$f":"INDEX('Import data'!$A:$A,MATCH($A1052,'Import data'!$A:$A,0),1)","v":{"$error":"#N/A"}}]
[0,{"$f":"INDEX('Import data'!$A:$A,MATCH($A1053,'Import data'!$A:$A,0),1)","v":{"$error":"#N/A"}}]
[0,{"$f":"INDEX('Import data'!$A:$A,MATCH($A1054,'Import data'!$A:$A,0),1)","v":{"$error":"#N/A"}}]
[0,{"$f":"INDEX('Import data'!$A:$A,MATCH($A1055,'Import data'!$A:$A,0),1)","v":{"$error":"#N/A"}}]
[0,{"$f":"INDEX('Import data'!$A:$A,MATCH($A1056,'Import data'!$A:$A,0),1)","v":{"$error":"#N/A"}}]
[0,{"$f":"INDEX('Import data'!$A:$A,MATCH($A1057,'Import data'!$A:$A,0),1)","v":{"$error":"#N/A"}}]
[0,{"$f":"INDEX('Import data'!$A:$A,MATCH($A1058,'Import data'!$A:$A,0),1)","v":{"$error":"#N/A"}}]
[0,{"$f":"INDEX('Import data'!$A:$A,MATCH($A1059,'Import data'!$A:$A,0),1)","v":{"$error":"#N/A"}}]
[0,{"$f":"INDEX('Import data'!$A:$A,MATCH($A1060,'Import data'!$A:$A,0),1)","v":{"$error":"#N/A"}}]
[0,{"$f":"INDEX('Import data'!$A:$A,MATCH($A1061,'Import data'!$A:$A,0),1)","v":{"$error":"#N/A"}}]
[0,{"$f":"INDEX('Import data'!$A:$A,MATCH($A1062,'Import data'!$A:$A,0),1)","v":{"$error":"#N/A"}}]
[0,{"$f":"INDEX('Import data'!$A:$A,MATCH($A1063,'Import data'!$A:$A,0),1)","v":{"$error":"#N/A"}}]
[0,{"$f":"INDEX('Import data'!$A:$A,MATCH($A1064,'Import data'!$A:$A,0),1)","v":{"$error":"#N/A"}}]
[0,{"$f":"INDEX('Import data'!$A:$A,MATCH($A1065,'Import data'!$A:$A,0),1)","v":{"$error":"#N/A"}}]
[0,{"$f":"INDEX('Import data'!$A:$A,MATCH($A1066,'Import data'!$A:$A,0),1)","v":{"$error":"#N/A"}}]
[0,{"$f":"INDEX('Import data'!$A:$A,MATCH($A1067,'Import data'!$A:$A,0),1)","v":{"$error":"#N/A"}}]
[0,{"$f":"INDEX('Import data'!$A:$A,MATCH($A1068,'Import data'!$A:$A,0),1)","v":{"$error":"#N/A"}}]
[0,{"$f":"INDEX('Import data'!$A:$A,MATCH($A1069,'Import data'!$A:$A,0),1)","v":{"$error":"#N/A"}}]
[0,{"$f":"INDEX('Import data'!$A:$A,MATCH($A1070,'Import data'!$A:$A,0),1)","v":{"$error":"#N/A"}}]
[0,{"$f":"INDEX('Import data'!$A:$A,MATCH($A1071,'Import data'!$A:$A,0),1)","v":{"$error":"#N/A"}}]
[0,{"$f":"INDEX('Import data'!$A:$A,MATCH($A1072,'Import data'!$A:$A,0),1)","v":{"$error":"#N/A"}}]
[0,{"$f":"INDEX('Import data'!$A:$A,MATCH($A1073,'Import data'!$A:$A,0),1)","v":{"$error":"#N/A"}}]
[0,{"$f":"INDEX('Import data'!$A:$A,MATCH($A1074,'Import data'!$A:$A,0),1)","v":{"$error":"#N/A"}}]
[0,{"$f":"INDEX('Import data'!$A:$A,MATCH($A1075,'Import data'!$A:$A,0),1)","v":{"$error":"#N/A"}}]
[0,{"$f":"INDEX('Import data'!$A:$A,MATCH($A1076,'Import data'!$A:$A,0),1)","v":{"$error":"#N/A"}}]
[0,{"$f":"INDEX('Import data'!$A:$A,MATCH($A1077,'Import data'!$A:$A,0),1)","v":{"$error":"#N/A"}}]
[0,{"$f":"INDEX('Import data'!$A:$A,MATCH($A1078,'Import data'!$A:$A,0),1)","v":{"$error":"#N/A"}}]
[0,{"$f":"INDEX('Import data'!$A:$A,MATCH($A1079,'Import data'!$A:$A,0),1)","v":{"$error":"#N/A"}}]
[0,{"$f":"INDEX('Import data'!$A:$A,MATCH($A1080,'Import data'!$A:$A,0),1)","v":{"$error":"#N/A"}}]
[0,{"$f":"INDEX('Import data'!$A:$A,MATCH($A1081,'Import data'!$A:$A,0),1)","v":{"$error":"#N/A"}}]
[0,{"$f":"INDEX('Import data'!$A:$A,MATCH($A1082,'Import data'!$A:$A,0),1)","v":{"$error":"#N/A"}}]
[0,{"$f":"INDEX('Import data'!$A:$A,MATCH($A1083,'Import data'!$A:$A,0),1)","v":{"$error":"#N/A"}}]
[0,{"$f":"INDEX('Import data'!$A:$A,MATCH($A1084,'Import data'!$A:$A,0),1)","v":{"$error":"#N/A"}}]
[0,{"$f":"INDEX('Import data'!$A:$A,MATCH($A1085,'Import data'!$A:$A,0),1)","v":{"$error":"#N/A"}}]
[0,{"$f":"INDEX('Import data'!$A:$A,MATCH($A1086,'Import data'!$A:$A,0),1)","v":{"$error":"#N/A"}}]
[0,{"$f":"INDEX('Import data'!$A:$A,MATCH($A1087,'Import data'!$A:$A,0),1)","v":{"$error":"#N/A"}}]
[0,{"$f":"INDEX('Import data'!$A:$A,MATCH($A1088,'Import data'!$A:$A,0),1)","v":{"$error":"#N/A"}}]
[0,{"$f":"INDEX('Import data'!$A:$A,MATCH($A1089,'Import data'!$A:$A,0),1)","v":{"$error":"#N/A"}}]
[0,{"$f":"INDEX('Import data'!$A:$A,MATCH($A1090,'Import data'!$A:$A,0),1)","v":{"$error":"#N/A"}}]
[{"$f":"ID","v":0},{"$f":"INDEX('Import data'!$A:$A,MATCH($A1091,'Import data'!$A:$A,0),1)","v":{"$error":"#N/A"}}]
[0,{"$f":"INDEX('Import data'!$A:$A,MATCH($A1092,'Import data'!$A:$A,0),1)","v":{"$error":"#N/A"}}]
[0,{"$f":"INDEX('Import data'!$A:$A,MATCH($A1093,'Import data'!$A:$A,0),1)","v":{"$error":"#N/A"}}]
[0,{"$f":"INDEX('Import data'!$A:$A,MATCH($A1094,'Import data'!$A:$A,0),1)","v":{"$error":"#N/A"}}]
[0,{"$f":"INDEX('Import data'!$A:$A,MATCH($A1095,'Import data'!$A:$A,0),1)","v":{"$error":"#N/A"}}]
[0,{"$f":"INDEX('Import data'!$A:$A,MATCH($A1096,'Import data'!$A:$A,0),1)","v":{"$error":"#N/A"}}]
[0,{"$f":"INDEX('Import data'!$A:$A,MATCH($A1097,'Import data'!$A:$A,0),1)","v":{"$error":"#N/A"}}]
[0,{"$f":"INDEX('Import data'!$A:$A,MATCH($A1098,'Import data'!$A:$A,0),1)","v":{"$error":"#N/A"}}]
[0,{"$f":"INDEX('Import data'!$A:$A,MATCH($A1099,'Import data'!$A:$A,0),1)","v":{"$error":"#N/A"}}]
[0,{"$f":"INDEX('Import data'!$A:$A,MATCH($A1100,'Import data'!$A:$A,0),1)","v":{"$error":"#N/A"}}]
[0,{"$f":"INDEX('Import data'!$A:$A,MATCH($A1101,'Import data'!$A:$A,0),1)","v":{"$error":"#N/A"}}]
[0,{"$f":"INDEX('Import data'!$A:$A,MATCH($A1102,'Import data'!$A:$A,0),1)","v":{"$error":"#N/A"}}]
[0,{"$f":"INDEX('Import data'!$A:$A,MATCH($A1103,'Import data'!$A:$A,0),1)","v":{"$error":"#N/A"}}]
[0,{"$f":"INDEX('Import data'!$A:$A,MATCH($A1104,'Import data'!$A:$A,0),1)","v":{"$error":"#N/A"}}]
[0,{"$f":"INDEX('Import data'!$A:$A,MATCH($A1105,'Import data'!$A:$A,0),1)","v":{"$error":"#N/A"}}]
[0,{"$f":"INDEX('Import data'!$A:$A,MATCH($A1106,'Import data'!$A:$A,0),1)","v":{"$error":"#N/A"}}]
[0,{"$f":"INDEX('Import data'!$A:$A,MATCH($A1107,'Import data'!$A:$A,0),1)","v":{"$error":"#N/A"}}]
[0,{"$f":"INDEX('Import data'!$A:$A,MATCH($A1108,'Import data'!$A:$A,0),1)","v":{"$error":"#N/A"}}]
[0,{"$f":"INDEX('Import data'!$A:$A,MATCH($A1109,'Import data'!$A:$A,0),1)","v":{"$error":"#N/A"}}]
[0,{"$f":"INDEX('Import data'!$A:$A,MATCH($A1110,'Import data'!$A:$A,0),1)","v":{"$error":"#N/A"}}]
[0,{"$f":"INDEX('Import data'!$A:$A,MATCH($A1111,'Import data'!$A:$A,0),1)","v":{"$error":"#N/A"}}]
[0,{"$f":"INDEX('Import data'!$A:$A,MATCH($A1112,'Import data'!$A:$A,0),1)","v":{"$error":"#N/A"}}]
[0,{"$f":"INDEX('Import data'!$A:$A,MATCH($A1113,'Import data'!$A:$A,0),1)","v":{"$error":"#N/A"}}]
[0,{"$f":"INDEX('Import data'!$A:$A,MATCH($A1114,'Import data'!$A:$A,0),1)","v":{"$error":"#N/A"}}]
[0,{"$f":"INDEX('Import data'!$A:$A,MATCH($A1115,'Import data'!$A:$A,0),1)","v":{"$error":"#N/A"}}]
[0,{"$f":"INDEX('Import data'!$A:$A,MATCH($A1116,'Import data'!$A:$A,0),1)","v":{"$error":"#N/A"}}]
[0,{"$f":"INDEX('Import data'!$A:$A,MATCH($A1117,'Import data'!$A:$A,0),1)","v":{"$error":"#N/A"}}]
[0,{"$f":"INDEX('Import data'!$A:$A,MATCH($A1118,'Import data'!$A:$A,0),1)","v":{"$error":"#N/A"}}]
[0,{"$f":"INDEX('Import data'!$A:$A,MATCH($A1119,'Import data'!$A:$A,0),1)","v":{"$error":"#N/A"}}]
[0,{"$f":"INDEX('Import data'!$A:$A,MATCH($A1120,'Import data'!$A:$A,0),1)","v":{"$error":"#N/A"}}]
[0,{"$f":"INDEX('Import data'!$A:$A,MATCH($A1121,'Import data'!$A:$A,0),1)","v":{"$error":"#N/A"}}]
[0,{"$f":"INDEX('Import data'!$A:$A,MATCH($A1122,'Import data'!$A:$A,0),1)","v":{"$error":"#N/A"}}]
[0,{"$f":"INDEX('Import data'!$A:$A,MATCH($A1123,'Import data'!$A:$A,0),1)","v":{"$error":"#N/A"}}]
[0,{"$f":"INDEX('Import data'!$A:$A,MATCH($A1124,'Import data'!$A:$A,0),1)","v":{"$error":"#N/A"}}]
[0,{"$f":"INDEX('Import data'!$A:$A,MATCH($A1125,'Import data'!$A:$A,0),1)","v":{"$error":"#N/A"}}]
[0,{"$f":"INDEX('Import data'!$A:$A,MATCH($A1126,'Import data'!$A:$A,0),1)","v":{"$error":"#N/A"}}]
[0,{"$f":"INDEX('Import data'!$A:$A,MATCH($A1127,'Import data'!$A:$A,0),1)","v":{"$error":"#N/A"}}]
[0,{"$f":"INDEX('Import data'!$A:$A,MATCH($A1128,'Import data'!$A:$A,0),1)","v":{"$error":"#N/A"}}]
[0,{"$f":"INDEX('Import data'!$A:$A,MATCH($A1129,'Import data'!$A:$A,0),1)","v":{"$error":"#N/A"}}]
[0,{"$f":"INDEX('Import data'!$A:$A,MATCH($A1130,'Import data'!$A:$A,0),1)","v":{"$error":"#N/A"}}]
[0,{"$f":"INDEX('Import data'!$A:$A,MATCH($A1131,'Import data'!$A:$A,0),1)","v":{"$error":"#N/A"}}]
[0,{"$f":"INDEX('Import data'!$A:$A,MATCH($A1132,'Import data'!$A:$A,0),1)","v":{"$error":"#N/A"}}]
[0,{"$f":"INDEX('Import data'!$A:$A,MATCH($A1133,'Import data'!$A:$A,0),1)","v":{"$error":"#N/A"}}]
[0,{"$f":"INDEX('Import data'!$A:$A,MATCH($A1134,'Import data'!$A:$A,0),1)","v":{"$error":"#N/A"}}]
[0,{"$f":"INDEX('Import data'!$A:$A,MATCH($A1135,'Import data'!$A:$A,0),1)","v":{"$error":"#N/A"}}]
[0,{"$f":"INDEX('Import data'!$A:$A,MATCH($A1136,'Import data'!$A:$A,0),1)","v":{"$error":"#N/A"}}]
[0,{"$f":"INDEX('Import data'!$A:$A,MATCH($A1137,'Import data'!$A:$A,0),1)","v":{"$error":"#N/A"}}]
[0,{"$f":"INDEX('Import data'!$A:$A,MATCH($A1138,'Import data'!$A:$A,0),1)","v":{"$error":"#N/A"}}]
[0,{"$f":"INDEX('Import data'!$A:$A,MATCH($A1139,'Import data'!$A:$A,0),1)","v":{"$error":"#N/A"}}]
[0,{"$f":"INDEX('Import data'!$A:$A,MATCH($A1140,'Import data'!$A:$A,0),1)","v":{"$error":"#N/A"}}]
[0,{"$f":"INDEX('Import data'!$A:$A,MATCH($A1141,'Import data'!$A:$A,0),1)","v":{"$error":"#N/A"}}]
[0,{"$f":"INDEX('Import data'!$A:$A,MATCH($A1142,'Import data'!$A:$A,0),1)","v":{"$error":"#N/A"}}]
[0,{"$f":"INDEX('Import data'!$A:$A,MATCH($A1143,'Import data'!$A:$A,0),1)","v":{"$error":"#N/A"}}]
[0,{"$f":"INDEX('Import data'!$A:$A,MATCH($A1144,'Import data'!$A:$A,0),1)","v":{"$error":"#N/A"}}]
[0,{"$f":"INDEX('Import data'!$A:$A,MATCH($A1145,'Import data'!$A:$A,0),1)","v":{"$error":"#N/A"}}]
[0,{"$f":"INDEX('Import data'!$A:$A,MATCH($A1146,'Import data'!$A:$A,0),1)","v":{"$error":"#N/A"}}]
[0,{"$f":"INDEX('Import data'!$A:$A,MATCH($A1147,'Import data'!$A:$A,0),1)","v":{"$error":"#N/A"}}]
[0,{"$f":"INDEX('Import data'!$A:$A,MATCH($A1148,'Import data'!$A:$A,0),1)","v":{"$error":"#N/A"}}]
[0,{"$f":"INDEX('Import data'!$A:$A,MATCH($A1149,'Import data'!$A:$A,0),1)","v":{"$error":"#N/A"}}]
[0,{"$f":"INDEX('Import data'!$A:$A,MATCH($A1150,'Import data'!$A:$A,0),1)","v":{"$error":"#N/A"}}]
[0,{"$f":"INDEX('Import data'!$A:$A,MATCH($A1151,'Import data'!$A:$A,0),1)","v":{"$error":"#N/A"}}]
[0,{"$f":"INDEX('Import data'!$A:$A,MATCH($A1152,'Import data'!$A:$A,0),1)","v":{"$error":"#N/A"}}]
[0,{"$f":"INDEX('Import data'!$A:$A,MATCH($A1153,'Import data'!$A:$A,0),1)","v":{"$error":"#N/A"}}]
[0,{"$f":"INDEX('Import data'!$A:$A,MATCH($A1154,'Import data'!$A:$A,0),1)","v":{"$error":"#N/A"}}]
[{"$f":"ID","v":0},{"$f":"INDEX('Import data'!$A:$A,MATCH($A1155,'Import data'!$A:$A,0),1)","v":{"$error":"#N/A"}}]
[0,{"$f":"INDEX('Import data'!$A:$A,MATCH($A1156,'Import data'!$A:$A,0),1)","v":{"$error":"#N/A"}}]
[0,{"$f":"INDEX('Import data'!$A:$A,MATCH($A1157,'Import data'!$A:$A,0),1)","v":{"$error":"#N/A"}}]
[0,{"$f":"INDEX('Import data'!$A:$A,MATCH($A1158,'Import data'!$A:$A,0),1)","v":{"$error":"#N/A"}}]
[0,{"$f":"INDEX('Import data'!$A:$A,MATCH($A1159,'Import data'!$A:$A,0),1)","v":{"$error":"#N/A"}}]
[0,{"$f":"INDEX('Import data'!$A:$A,MATCH($A1160,'Import data'!$A:$A,0),1)","v":{"$error":"#N/A"}}]
[0,{"$f":"INDEX('Import data'!$A:$A,MATCH($A1161,'Import data'!$A:$A,0),1)","v":{"$error":"#N/A"}}]
[0,{"$f":"INDEX('Import data'!$A:$A,MATCH($A1162,'Import data'!$A:$A,0),1)","v":{"$error":"#N/A"}}]
[0,{"$f":"INDEX('Import data'!$A:$A,MATCH($A1163,'Import data'!$A:$A,0),1)","v":{"$error":"#N/A"}}]
[0,{"$f":"INDEX('Import data'!$A:$A,MATCH($A1164,'Import data'!$A:$A,0),1)","v":{"$error":"#N/A"}}]
[0,{"$f":"INDEX('Import data'!$A:$A,MATCH($A1165,'Import data'!$A:$A,0),1)","v":{"$error":"#N/A"}}]
[0,{"$f":"INDEX('Import data'!$A:$A,MATCH($A1166,'Import data'!$A:$A,0),1)","v":{"$error":"#N/A"}}]
[0,{"$f":"INDEX('Import data'!$A:$A,MATCH($A1167,'Import data'!$A:$A,0),1)","v":{"$error":"#N/A"}}]
[0,{"$f":"INDEX('Import data'!$A:$A,MATCH($A1168,'Import data'!$A:$A,0),1)","v":{"$error":"#N/A"}}]
[0,{"$f":"INDEX('Import data'!$A:$A,MATCH($A1169,'Import data'!$A:$A,0),1)","v":{"$error":"#N/A"}}]
[0,{"$f":"INDEX('Import data'!$A:$A,MATCH($A1170,'Import data'!$A:$A,0),1)","v":{"$error":"#N/A"}}]
[0,{"$f":"INDEX('Import data'!$A:$A,MATCH($A1171,'Import data'!$A:$A,0),1)","v":{"$error":"#N/A"}}]
[0,{"$f":"INDEX('Import data'!$A:$A,MATCH($A1172,'Import data'!$A:$A,0),1)","v":{"$error":"#N/A"}}]
[0,{"$f":"INDEX('Import data'!$A:$A,MATCH($A1173,'Import data'!$A:$A,0),1)","v":{"$error":"#N/A"}}]
[0,{"$f":"INDEX('Import data'!$A:$A,MATCH($A1174,'Import data'!$A:$A,0),1)","v":{"$error":"#N/A"}}]
[0,{"$f":"INDEX('Import data'!$A:$A,MATCH($A1175,'Import data'!$A:$A,0),1)","v":{"$error":"#N/A"}}]
[0,{"$f":"INDEX('Import data'!$A:$A,MATCH($A1176,'Import data'!$A:$A,0),1)","v":{"$error":"#N/A"}}]
[0,{"$f":"INDEX('Import data'!$A:$A,MATCH($A1177,'Import data'!$A:$A,0),1)","v":{"$error":"#N/A"}}]
[0,{"$f":"INDEX('Import data'!$A:$A,MATCH($A1178,'Import data'!$A:$A,0),1)","v":{"$error":"#N/A"}}]
[0,{"$f":"INDEX('Import data'!$A:$A,MATCH($A1179,'Import data'!$A:$A,0),1)","v":{"$error":"#N/A"}}]
[0,{"$f":"INDEX('Import data'!$A:$A,MATCH($A1180,'Import data'!$A:$A,0),1)","v":{"$error":"#N/A"}}]
[0,{"$f":"INDEX('Import data'!$A:$A,MATCH($A1181,'Import data'!$A:$A,0),1)","v":{"$error":"#N/A"}}]
[0,{"$f":"INDEX('Import data'!$A:$A,MATCH($A1182,'Import data'!$A:$A,0),1)","v":{"$error":"#N/A"}}]
[0,{"$f":"INDEX('Import data'!$A:$A,MATCH($A1183,'Import data'!$A:$A,0),1)","v":{"$error":"#N/A"}}]
[0,{"$f":"INDEX('Import data'!$A:$A,MATCH($A1184,'Import data'!$A:$A,0),1)","v":{"$error":"#N/A"}}]
[0,{"$f":"INDEX('Import data'!$A:$A,MATCH($A1185,'Import data'!$A:$A,0),1)","v":{"$error":"#N/A"}}]
[0,{"$f":"INDEX('Import data'!$A:$A,MATCH($A1186,'Import data'!$A:$A,0),1)","v":{"$error":"#N/A"}}]
[0,{"$f":"INDEX('Import data'!$A:$A,MATCH($A1187,'Import data'!$A:$A,0),1)","v":{"$error":"#N/A"}}]
[0,{"$f":"INDEX('Import data'!$A:$A,MATCH($A1188,'Import data'!$A:$A,0),1)","v":{"$error":"#N/A"}}]
[0,{"$f":"INDEX('Import data'!$A:$A,MATCH($A1189,'Import data'!$A:$A,0),1)","v":{"$error":"#N/A"}}]
[0,{"$f":"INDEX('Import data'!$A:$A,MATCH($A1190,'Import data'!$A:$A,0),1)","v":{"$error":"#N/A"}}]
[0,{"$f":"INDEX('Import data'!$A:$A,MATCH($A1191,'Import data'!$A:$A,0),1)","v":{"$error":"#N/A"}}]
[0,{"$f":"INDEX('Import data'!$A:$A,MATCH($A1192,'Import data'!$A:$A,0),1)","v":{"$error":"#N/A"}}]
[0,{"$f":"INDEX('Import data'!$A:$A,MATCH($A1193,'Import data'!$A:$A,0),1)","v":{"$error":"#N/A"}}]
[0,{"$f":"INDEX('Import data'!$A:$A,MATCH($A1194,'Import data'!$A:$A,0),1)","v":{"$error":"#N/A"}}]
[0,{"$f":"INDEX('Import data'!$A:$A,MATCH($A1195,'Import data'!$A:$A,0),1)","v":{"$error":"#N/A"}}]
[0,{"$f":"INDEX('Import data'!$A:$A,MATCH($A1196,'Import data'!$A:$A,0),1)","v":{"$error":"#N/A"}}]
[0,{"$f":"INDEX('Import data'!$A:$A,MATCH($A1197,'Import data'!$A:$A,0),1)","v":{"$error":"#N/A"}}]
[0,{"$f":"INDEX('Import data'!$A:$A,MATCH($A1198,'Import data'!$A:$A,0),1)","v":{"$error":"#N/A"}}]
[0,{"$f":"INDEX('Import data'!$A:$A,MATCH($A1199,'Import data'!$A:$A,0),1)","v":{"$error":"#N/A"}}]
[0,{"$f":"INDEX('Import data'!$A:$A,MATCH($A1200,'Import data'!$A:$A,0),1)","v":{"$error":"#N/A"}}]
[0,{"$f":"INDEX('Import data'!$A:$A,MATCH($A1201,'Import data'!$A:$A,0),1)","v":{"$error":"#N/A"}}]
[0,{"$f":"INDEX('Import data'!$A:$A,MATCH($A1202,'Import data'!$A:$A,0),1)","v":{"$error":"#N/A"}}]
[0,{"$f":"INDEX('Import data'!$A:$A,MATCH($A1203,'Import data'!$A:$A,0),1)","v":{"$error":"#N/A"}}]
[0,{"$f":"INDEX('Import data'!$A:$A,MATCH($A1204,'Import data'!$A:$A,0),1)","v":{"$error":"#N/A"}}]
[0,{"$f":"INDEX('Import data'!$A:$A,MATCH($A1205,'Import data'!$A:$A,0),1)","v":{"$error":"#N/A"}}]
[0,{"$f":"INDEX('Import data'!$A:$A,MATCH($A1206,'Import data'!$A:$A,0),1)","v":{"$error":"#N/A"}}]
[0,{"$f":"INDEX('Import data'!$A:$A,MATCH($A1207,'Import data'!$A:$A,0),1)","v":{"$error":"#N/A"}}]
[0,{"$f":"INDEX('Import data'!$A:$A,MATCH($A1208,'Import data'!$A:$A,0),1)","v":{"$error":"#N/A"}}]
[0,{"$f":"INDEX('Import data'!$A:$A,MATCH($A1209,'Import data'!$A:$A,0),1)","v":{"$error":"#N/A"}}]
[0,{"$f":"INDEX('Import data'!$A:$A,MATCH($A1210,'Import data'!$A:$A,0),1)","v":{"$error":"#N/A"}}]
[0,{"$f":"INDEX('Import data'!$A:$A,MATCH($A1211,'Import data'!$A:$A,0),1)","v":{"$error":"#N/A"}}]
[0,{"$f":"INDEX('Import data'!$A:$A,MATCH($A1212,'Import data'!$A:$A,0),1)","v":{"$error":"#N/A"}}]
[0,{"$f":"INDEX('Import data'!$A:$A,MATCH($A1213,'Import data'!$A:$A,0),1)","v":{"$error":"#N/A"}}]
[0,{"$f":"INDEX('Import data'!$A:$A,MATCH($A1214,'Import data'!$A:$A,0),1)","v":{"$error":"#N/A"}}]
[0,{"$f":"INDEX('Import data'!$A:$A,MATCH($A1215,'Import data'!$A:$A,0),1)","v":{"$error":"#N/A"}}]
[0,{"$f":"INDEX('Import data'!$A:$A,MATCH($A1216,'Import data'!$A:$A,0),1)","v":{"$error":"#N/A"}}]
[0,{"$f":"INDEX('Import data'!$A:$A,MATCH($A1217,'Import data'!$A:$A,0),1)","v":{"$error":"#N/A"}}]
[0,{"$f":"INDEX('Import data'!$A:$A,MATCH($A1218,'Import data'!$A:$A,0),1)","v":{"$error":"#N/A"}}]
[{"$f":"ID","v":0},{"$f":"INDEX('Import data'!$A:$A,MATCH($A1219,'Import data'!$A:$A,0),1)","v":{"$error":"#N/A"}}]
[0,{"$f":"INDEX('Import data'!$A:$A,MATCH($A1220,'Import data'!$A:$A,0),1)","v":{"$error":"#N/A"}}]
[0,{"$f":"INDEX('Import data'!$A:$A,MATCH($A1221,'Import data'!$A:$A,0),1)","v":{"$error":"#N/A"}}]
[0,{"$f":"INDEX('Import data'!$A:$A,MATCH($A1222,'Import data'!$A:$A,0),1)","v":{"$error":"#N/A"}}]
[0,{"$f":"INDEX('Import data'!$A:$A,MATCH($A1223,'Import data'!$A:$A,0),1)","v":{"$error":"#N/A"}}]
[0,{"$f":"INDEX('Import data'!$A:$A,MATCH($A1224,'Import data'!$A:$A,0),1)","v":{"$error":"#N/A"}}]
[0,{"$f":"INDEX('Import data'!$A:$A,MATCH($A1225,'Import data'!$A:$A,0),1)","v":{"$error":"#N/A"}}]
[0,{"$f":"INDEX('Import data'!$A:$A,MATCH($A1226,'Import data'!$A:$A,0),1)","v":{"$error":"#N/A"}}]
[0,{"$f":"INDEX('Import data'!$A:$A,MATCH($A1227,'Import data'!$A:$A,0),1)","v":{"$error":"#N/A"}}]
[0,{"$f":"INDEX('Import data'!$A:$A,MATCH($A1228,'Import data'!$A:$A,0),1)","v":{"$error":"#N/A"}}]
[0,{"$f":"INDEX('Import data'!$A:$A,MATCH($A1229,'Import data'!$A:$A,0),1)","v":{"$error":"#N/A"}}]
[0,{"$f":"INDEX('Import data'!$A:$A,MATCH($A1230,'Import data'!$A:$A,0),1)","v":{"$error":"#N/A"}}]
[0,{"$f":"INDEX('Import data'!$A:$A,MATCH($A1231,'Import data'!$A:$A,0),1)","v":{"$error":"#N/A"}}]
[0,{"$f":"INDEX('Import data'!$A:$A,MATCH($A1232,'Import data'!$A:$A,0),1)","v":{"$error":"#N/A"}}]
[0,{"$f":"INDEX('Import data'!$A:$A,MATCH($A1233,'Import data'!$A:$A,0),1)","v":{"$error":"#N/A"}}]
[0,{"$f":"INDEX('Import data'!$A:$A,MATCH($A1234,'Import data'!$A:$A,0),1)","v":{"$error":"#N/A"}}]
[0,{"$f":"INDEX('Import data'!$A:$A,MATCH($A1235,'Import data'!$A:$A,0),1)","v":{"$error":"#N/A"}}]
[0,{"$f":"INDEX('Import data'!$A:$A,MATCH($A1236,'Import data'!$A:$A,0),1)","v":{"$error":"#N/A"}}]
[0,{"$f":"INDEX('Import data'!$A:$A,MATCH($A1237,'Import data'!$A:$A,0),1)","v":{"$error":"#N/A"}}]
[0,{"$f":"INDEX('Import data'!$A:$A,MATCH($A1238,'Import data'!$A:$A,0),1)","v":{"$error":"#N/A"}}]
[0,{"$f":"INDEX('Import data'!$A:$A,MATCH($A1239,'Import data'!$A:$A,0),1)","v":{"$error":"#N/A"}}]
[0,{"$f":"INDEX('Import data'!$A:$A,MATCH($A1240,'Import data'!$A:$A,0),1)","v":{"$error":"#N/A"}}]
[0,{"$f":"INDEX('Import data'!$A:$A,MATCH($A1241,'Import data'!$A:$A,0),1)","v":{"$error":"#N/A"}}]
[0,{"$f":"INDEX('Import data'!$A:$A,MATCH($A1242,'Import data'!$A:$A,0),1)","v":{"$error":"#N/A"}}]
[0,{"$f":"INDEX('Import data'!$A:$A,MATCH($A1243,'Import data'!$A:$A,0),1)","v":{"$error":"#N/A"}}]
[0,{"$f":"INDEX('Import data'!$A:$A,MATCH($A1244,'Import data'!$A:$A,0),1)","v":{"$error":"#N/A"}}]
[0,{"$f":"INDEX('Import data'!$A:$A,MATCH($A1245,'Import data'!$A:$A,0),1)","v":{"$error":"#N/A"}}]
[0,{"$f":"INDEX('Import data'!$A:$A,MATCH($A1246,'Import data'!$A:$A,0),1)","v":{"$error":"#N/A"}}]
[0,{"$f":"INDEX('Import data'!$A:$A,MATCH($A1247,'Import data'!$A:$A,0),1)","v":{"$error":"#N/A"}}]
[0,{"$f":"INDEX('Import data'!$A:$A,MATCH($A1248,'Import data'!$A:$A,0),1)","v":{"$error":"#N/A"}}]
[0,{"$f":"INDEX('Import data'!$A:$A,MATCH($A1249,'Import data'!$A:$A,0),1)","v":{"$error":"#N/A"}}]
[0,{"$f":"INDEX('Import data'!$A:$A,MATCH($A1250,'Import data'!$A:$A,0),1)","v":{"$error":"#N/A"}}]
[0,{"$f":"INDEX('Import data'!$A:$A,MATCH($A1251,'Import data'!$A:$A,0),1)","v":{"$error":"#N/A"}}]
[0,{"$f":"INDEX('Import data'!$A:$A,MATCH($A1252,'Import data'!$A:$A,0),1)","v":{"$error":"#N/A"}}]
[0,{"$f":"INDEX('Import data'!$A:$A,MATCH($A1253,'Import data'!$A:$A,0),1)","v":{"$error":"#N/A"}}]
[0,{"$f":"INDEX('Import data'!$A:$A,MATCH($A1254,'Import data'!$A:$A,0),1)","v":{"$error":"#N/A"}}]
[0,{"$f":"INDEX('Import data'!$A:$A,MATCH($A1255,'Import data'!$A:$A,0),1)","v":{"$error":"#N/A"}}]
[0,{"$f":"INDEX('Import data'!$A:$A,MATCH($A1256,'Import data'!$A:$A,0),1)","v":{"$error":"#N/A"}}]
[0,{"$f":"INDEX('Import data'!$A:$A,MATCH($A1257,'Import data'!$A:$A,0),1)","v":{"$error":"#N/A"}}]
[0,{"$f":"INDEX('Import data'!$A:$A,MATCH($A1258,'Import data'!$A:$A,0),1)","v":{"$error":"#N/A"}}]
[0,{"$f":"INDEX('Import data'!$A:$A,MATCH($A1259,'Import data'!$A:$A,0),1)","v":{"$error":"#N/A"}}]
[0,{"$f":"INDEX('Import data'!$A:$A,MATCH($A1260,'Import data'!$A:$A,0),1)","v":{"$error":"#N/A"}}]
[0,{"$f":"INDEX('Import data'!$A:$A,MATCH($A1261,'Import data'!$A:$A,0),1)","v":{"$error":"#N/A"}}]
[0,{"$f":"INDEX('Import data'!$A:$A,MATCH($A1262,'Import data'!$A:$A,0),1)","v":{"$error":"#N/A"}}]
[0,{"$f":"INDEX('Import data'!$A:$A,MATCH($A1263,'Import data'!$A:$A,0),1)","v":{"$error":"#N/A"}}]
[0,{"$f":"INDEX('Import data'!$A:$A,MATCH($A1264,'Import data'!$A:$A,0),1)","v":{"$error":"#N/A"}}]
[0,{"$f":"INDEX('Import data'!$A:$A,MATCH($A1265,'Import data'!$A:$A,0),1)","v":{"$error":"#N/A"}}]
[0,{"$f":"INDEX('Import data'!$A:$A,MATCH($A1266,'Import data'!$A:$A,0),1)","v":{"$error":"#N/A"}}]
[0,{"$f":"INDEX('Import data'!$A:$A,MATCH($A1267,'Import data'!$A:$A,0),1)","v":{"$error":"#N/A"}}]
[0,{"$f":"INDEX('Import data'!$A:$A,MATCH($A1268,'Import data'!$A:$A,0),1)","v":{"$error":"#N/A"}}]
[0,{"$f":"INDEX('Import data'!$A:$A,MATCH($A1269,'Import data'!$A:$A,0),1)","v":{"$error":"#N/A"}}]
[0,{"$f":"INDEX('Import data'!$A:$A,MATCH($A1270,'Import data'!$A:$A,0),1)","v":{"$error":"#N/A"}}]
[0,{"$f":"INDEX('Import data'!$A:$A,MATCH($A1271,'Import data'!$A:$A,0),1)","v":{"$error":"#N/A"}}]
[0,{"$f":"INDEX('Import data'!$A:$A,MATCH($A1272,'Import data'!$A:$A,0),1)","v":{"$error":"#N/A"}}]
[0,{"$f":"INDEX('Import data'!$A:$A,MATCH($A1273,'Import data'!$A:$A,0),1)","v":{"$error":"#N/A"}}]
[0,{"$f":"INDEX('Import data'!$A:$A,MATCH($A1274,'Import data'!$A:$A,0),1)","v":{"$error":"#N/A"}}]
[0,{"$f":"INDEX('Import data'!$A:$A,MATCH($A1275,'Import data'!$A:$A,0),1)","v":{"$error":"#N/A"}}]
[0,{"$f":"INDEX('Import data'!$A:$A,MATCH($A1276,'Import data'!$A:$A,0),1)","v":{"$error":"#N/A"}}]
[0,{"$f":"INDEX('Import data'!$A:$A,MATCH($A1277,'Import data'!$A:$A,0),1)","v":{"$error":"#N/A"}}]
[0,{"$f":"INDEX('Import data'!$A:$A,MATCH($A1278,'Import data'!$A:$A,0),1)","v":{"$error":"#N/A"}}]
[0,{"$f":"INDEX('Import data'!$A:$A,MATCH($A1279,'Import data'!$A:$A,0),1)","v":{"$error":"#N/A"}}]
[0,{"$f":"INDEX('Import data'!$A:$A,MATCH($A1280,'Import data'!$A:$A,0),1)","v":{"$error":"#N/A"}}]
[0,{"$f":"INDEX('Import data'!$A:$A,MATCH($A1281,'Import data'!$A:$A,0),1)","v":{"$error":"#N/A"}}]
[0,{"$f":"INDEX('Import data'!$A:$A,MATCH($A1282,'Import data'!$A:$A,0),1)","v":{"$error":"#N/A"}}]
[{"$f":"ID","v":0},{"$f":"INDEX('Import data'!$A:$A,MATCH($A1283,'Import data'!$A:$A,0),1)","v":{"$error":"#N/A"}}]
[0,{"$f":"INDEX('Import data'!$A:$A,MATCH($A1284,'Import data'!$A:$A,0),1)","v":{"$error":"#N/A"}}]
[0,{"$f":"INDEX('Import data'!$A:$A,MATCH($A1285,'Import data'!$A:$A,0),1)","v":{"$error":"#N/A"}}]
[0,{"$f":"INDEX('Import data'!$A:$A,MATCH($A1286,'Import data'!$A:$A,0),1)","v":{"$error":"#N/A"}}]
[0,{"$f":"INDEX('Import data'!$A:$A,MATCH($A1287,'Import data'!$A:$A,0),1)","v":{"$error":"#N/A"}}]
[0,{"$f":"INDEX('Import data'!$A:$A,MATCH($A1288,'Import data'!$A:$A,0),1)","v":{"$error":"#N/A"}}]
[0,{"$f":"INDEX('Import data'!$A:$A,MATCH($A1289,'Import data'!$A:$A,0),1)","v":{"$error":"#N/A"}}]
[0,{"$f":"INDEX('Import data'!$A:$A,MATCH($A1290,'Import data'!$A:$A,0),1)","v":{"$error":"#N/A"}}]
[0,{"$f":"INDEX('Import data'!$A:$A,MATCH($A1291,'Import data'!$A:$A,0),1)","v":{"$error":"#N/A"}}]
[0,{"$f":"INDEX('Import data'!$A:$A,MATCH($A1292,'Import data'!$A:$A,0),1)","v":{"$error":"#N/A"}}]
[0,{"$f":"INDEX('Import data'!$A:$A,MATCH($A1293,'Import data'!$A:$A,0),1)","v":{"$error":"#N/A"}}]
[0,{"$f":"INDEX('Import data'!$A:$A,MATCH($A1294,'Import data'!$A:$A,0),1)","v":{"$error":"#N/A"}}]
[0,{"$f":"INDEX('Import data'!$A:$A,MATCH($A1295,'Import data'!$A:$A,0),1)","v":{"$error":"#N/A"}}]
[0,{"$f":"INDEX('Import data'!$A:$A,MATCH($A1296,'Import data'!$A:$A,0),1)","v":{"$error":"#N/A"}}]
[0,{"$f":"INDEX('Import data'!$A:$A,MATCH($A1297,'Import data'!$A:$A,0),1)","v":{"$error":"#N/A"}}]
[0,{"$f":"INDEX('Import data'!$A:$A,MATCH($A1298,'Import data'!$A:$A,0),1)","v":{"$error":"#N/A"}}]
[0,{"$f":"INDEX('Import data'!$A:$A,MATCH($A1299,'Import data'!$A:$A,0),1)","v":{"$error":"#N/A"}}]
[0,{"$f":"INDEX('Import data'!$A:$A,MATCH($A1300,'Import data'!$A:$A,0),1)","v":{"$error":"#N/A"}}]
[0,{"$f":"INDEX('Import data'!$A:$A,MATCH($A1301,'Import data'!$A:$A,0),1)","v":{"$error":"#N/A"}}]
[0,{"$f":"INDEX('Import data'!$A:$A,MATCH($A1302,'Import data'!$A:$A,0),1)","v":{"$error":"#N/A"}}]
[0,{"$f":"INDEX('Import data'!$A:$A,MATCH($A1303,'Import data'!$A:$A,0),1)","v":{"$error":"#N/A"}}]
[0,{"$f":"INDEX('Import data'!$A:$A,MATCH($A1304,'Import data'!$A:$A,0),1)","v":{"$error":"#N/A"}}]
[0,{"$f":"INDEX('Import data'!$A:$A,MATCH($A1305,'Import data'!$A:$A,0),1)","v":{"$error":"#N/A"}}]
[0,{"$f":"INDEX('Import data'!$A:$A,MATCH($A1306,'Import data'!$A:$A,0),1)","v":{"$error":"#N/A"}}]
[0,{"$f":"INDEX('Import data'!$A:$A,MATCH($A1307,'Import data'!$A:$A,0),1)","v":{"$error":"#N/A"}}]
[0,{"$f":"INDEX('Import data'!$A:$A,MATCH($A1308,'Import data'!$A:$A,0),1)","v":{"$error":"#N/A"}}]
[0,{"$f":"INDEX('Import data'!$A:$A,MATCH($A1309,'Import data'!$A:$A,0),1)","v":{"$error":"#N/A"}}]
[0,{"$f":"INDEX('Import data'!$A:$A,MATCH($A1310,'Import data'!$A:$A,0),1)","v":{"$error":"#N/A"}}]
[0,{"$f":"INDEX('Import data'!$A:$A,MATCH($A1311,'Import data'!$A:$A,0),1)","v":{"$error":"#N/A"}}]
[0,{"$f":"INDEX('Import data'!$A:$A,MATCH($A1312,'Import data'!$A:$A,0),1)","v":{"$error":"#N/A"}}]
[0,{"$f":"INDEX('Import data'!$A:$A,MATCH($A1313,'Import data'!$A:$A,0),1)","v":{"$error":"#N/A"}}]
[0,{"$f":"INDEX('Import data'!$A:$A,MATCH($A1314,'Import data'!$A:$A,0),1)","v":{"$error":"#N/A"}}]
[0,{"$f":"INDEX('Import data'!$A:$A,MATCH($A1315,'Import data'!$A:$A,0),1)","v":{"$error":"#N/A"}}]
[0,{"$f":"INDEX('Import data'!$A:$A,MATCH($A1316,'Import data'!$A:$A,0),1)","v":{"$error":"#N/A"}}]
[0,{"$f":"INDEX('Import data'!$A:$A,MATCH($A1317,'Import data'!$A:$A,0),1)","v":{"$error":"#N/A"}}]
[0,{"$f":"INDEX('Import data'!$A:$A,MATCH($A1318,'Import data'!$A:$A,0),1)","v":{"$error":"#N/A"}}]
[0,{"$f":"INDEX('Import data'!$A:$A,MATCH($A1319,'Import data'!$A:$A,0),1)","v":{"$error":"#N/A"}}]
[0,{"$f":"INDEX('Import data'!$A:$A,MATCH($A1320,'Import data'!$A:$A,0),1)","v":{"$error":"#N/A"}}]
[0,{"$f":"INDEX('Import data'!$A:$A,MATCH($A1321,'Import data'!$A:$A,0),1)","v":{"$error":"#N/A"}}]
[0,{"$f":"INDEX('Import data'!$A:$A,MATCH($A1322,'Import data'!$A:$A,0),1)","v":{"$error":"#N/A"}}]
[0,{"$f":"INDEX('Import data'!$A:$A,MATCH($A1323,'Import data'!$A:$A,0),1)","v":{"$error":"#N/A"}}]
[0,{"$f":"INDEX('Import data'!$A:$A,MATCH($A1324,'Import data'!$A:$A,0),1)","v":{"$error":"#N/A"}}]
[0,{"$f":"INDEX('Import data'!$A:$A,MATCH($A1325,'Import data'!$A:$A,0),1)","v":{"$error":"#N/A"}}]
[0,{"$f":"INDEX('Import data'!$A:$A,MATCH($A1326,'Import data'!$A:$A,0),1)","v":{"$error":"#N/A"}}]
[0,{"$f":"INDEX('Import data'!$A:$A,MATCH($A1327,'Import data'!$A:$A,0),1)","v":{"$error":"#N/A"}}]
[0,{"$f":"INDEX('Import data'!$A:$A,MATCH($A1328,'Import data'!$A:$A,0),1)","v":{"$error":"#N/A"}}]
[0,{"$f":"INDEX('Import data'!$A:$A,MATCH($A1329,'Import data'!$A:$A,0),1)","v":{"$error":"#N/A"}}]
[0,{"$f":"INDEX('Import data'!$A:$A,MATCH($A1330,'Import data'!$A:$A,0),1)","v":{"$error":"#N/A"}}]
[0,{"$f":"INDEX('Import data'!$A:$A,MATCH($A1331,'Import data'!$A:$A,0),1)","v":{"$error":"#N/A"}}]
[0,{"$f":"INDEX('Import data'!$A:$A,MATCH($A1332,'Import data'!$A:$A,0),1)","v":{"$error":"#N/A"}}]
[0,{"$f":"INDEX('Import data'!$A:$A,MATCH($A1333,'Import data'!$A:$A,0),1)","v":{"$error":"#N/A"}}]
[0,{"$f":"INDEX('Import data'!$A:$A,MATCH($A1334,'Import data'!$A:$A,0),1)","v":{"$error":"#N/A"}}]
[0,{"$f":"INDEX('Import data'!$A:$A,MATCH($A1335,'Import data'!$A:$A,0),1)","v":{"$error":"#N/A"}}]
[0,{"$f":"INDEX('Import data'!$A:$A,MATCH($A1336,'Import data'!$A:$A,0),1)","v":{"$error":"#N/A"}}]
[0,{"$f":"INDEX('Import data'!$A:$A,MATCH($A1337,'Import data'!$A:$A,0),1)","v":{"$error":"#N/A"}}]
[0,{"$f":"INDEX('Import data'!$A:$A,MATCH($A1338,'Import data'!$A:$A,0),1)","v":{"$error":"#N/A"}}]
[0,{"$f":"INDEX('Import data'!$A:$A,MATCH($A1339,'Import data'!$A:$A,0),1)","v":{"$error":"#N/A"}}]
[0,{"$f":"INDEX('Import data'!$A:$A,MATCH($A1340,'Import data'!$A:$A,0),1)","v":{"$error":"#N/A"}}]
[0,{"$f":"INDEX('Import data'!$A:$A,MATCH($A1341,'Import data'!$A:$A,0),1)","v":{"$error":"#N/A"}}]
[0,{"$f":"INDEX('Import data'!$A:$A,MATCH($A1342,'Import data'!$A:$A,0),1)","v":{"$error":"#N/A"}}]
[0,{"$f":"INDEX('Import data'!$A:$A,MATCH($A1343,'Import data'!$A:$A,0),1)","v":{"$error":"#N/A"}}]
[0,{"$f":"INDEX('Import data'!$A:$A,MATCH($A1344,'Import data'!$A:$A,0),1)","v":{"$error":"#N/A"}}]
[0,{"$f":"INDEX('Import data'!$A:$A,MATCH($A1345,'Import data'!$A:$A,0),1)","v":{"$error":"#N/A"}}]
[0,{"$f":"INDEX('Import data'!$A:$A,MATCH($A1346,'Import data'!$A:$A,0),1)","v":{"$error":"#N/A"}}]
[{"$f":"ID","v":0},{"$f":"INDEX('Import data'!$A:$A,MATCH($A1347,'Import data'!$A:$A,0),1)","v":{"$error":"#N/A"}}]
[0,{"$f":"INDEX('Import data'!$A:$A,MATCH($A1348,'Import data'!$A:$A,0),1)","v":{"$error":"#N/A"}}]
[0,{"$f":"INDEX('Import data'!$A:$A,MATCH($A1349,'Import data'!$A:$A,0),1)","v":{"$error":"#N/A"}}]
[0,{"$f":"INDEX('Import data'!$A:$A,MATCH($A1350,'Import data'!$A:$A,0),1)","v":{"$error":"#N/A"}}]
[0,{"$f":"INDEX('Import data'!$A:$A,MATCH($A1351,'Import data'!$A:$A,0),1)","v":{"$error":"#N/A"}}]
[0,{"$f":"INDEX('Import data'!$A:$A,MATCH($A1352,'Import data'!$A:$A,0),1)","v":{"$error":"#N/A"}}]
[0,{"$f":"INDEX('Import data'!$A:$A,MATCH($A1353,'Import data'!$A:$A,0),1)","v":{"$error":"#N/A"}}]
[0,{"$f":"INDEX('Import data'!$A:$A,MATCH($A1354,'Import data'!$A:$A,0),1)","v":{"$error":"#N/A"}}]
[0,{"$f":"INDEX('Import data'!$A:$A,MATCH($A1355,'Import data'!$A:$A,0),1)","v":{"$error":"#N/A"}}]
[0,{"$f":"INDEX('Import data'!$A:$A,MATCH($A1356,'Import data'!$A:$A,0),1)","v":{"$error":"#N/A"}}]
[0,{"$f":"INDEX('Import data'!$A:$A,MATCH($A1357,'Import data'!$A:$A,0),1)","v":{"$error":"#N/A"}}]
[0,{"$f":"INDEX('Import data'!$A:$A,MATCH($A1358,'Import data'!$A:$A,0),1)","v":{"$error":"#N/A"}}]
[0,{"$f":"INDEX('Import data'!$A:$A,MATCH($A1359,'Import data'!$A:$A,0),1)","v":{"$error":"#N/A"}}]
[0,{"$f":"INDEX('Import data'!$A:$A,MATCH($A1360,'Import data'!$A:$A,0),1)","v":{"$error":"#N/A"}}]
[0,{"$f":"INDEX('Import data'!$A:$A,MATCH($A1361,'Import data'!$A:$A,0),1)","v":{"$error":"#N/A"}}]
[0,{"$f":"INDEX('Import data'!$A:$A,MATCH($A1362,'Import data'!$A:$A,0),1)","v":{"$error":"#N/A"}}]
[0,{"$f":"INDEX('Import data'!$A:$A,MATCH($A1363,'Import data'!$A:$A,0),1)","v":{"$error":"#N/A"}}]
[0,{"$f":"INDEX('Import data'!$A:$A,MATCH($A1364,'Import data'!$A:$A,0),1)","v":{"$error":"#N/A"}}]
[0,{"$f":"INDEX('Import data'!$A:$A,MATCH($A1365,'Import data'!$A:$A,0),1)","v":{"$error":"#N/A"}}]
[0,{"$f":"INDEX('Import data'!$A:$A,MATCH($A1366,'Import data'!$A:$A,0),1)","v":{"$error":"#N/A"}}]
[0,{"$f":"INDEX('Import data'!$A:$A,MATCH($A1367,'Import data'!$A:$A,0),1)","v":{"$error":"#N/A"}}]
[0,{"$f":"INDEX('Import data'!$A:$A,MATCH($A1368,'Import data'!$A:$A,0),1)","v":{"$error":"#N/A"}}]
[0,{"$f":"INDEX('Import data'!$A:$A,MATCH($A1369,'Import data'!$A:$A,0),1)","v":{"$error":"#N/A"}}]
[0,{"$f":"INDEX('Import data'!$A:$A,MATCH($A1370,'Import data'!$A:$A,0),1)","v":{"$error":"#N/A"}}]
[0,{"$f":"INDEX('Import data'!$A:$A,MATCH($A1371,'Import data'!$A:$A,0),1)","v":{"$error":"#N/A"}}]
[0,{"$f":"INDEX('Import data'!$A:$A,MATCH($A1372,'Import data'!$A:$A,0),1)","v":{"$error":"#N/A"}}]
[0,{"$f":"INDEX('Import data'!$A:$A,MATCH($A1373,'Import data'!$A:$A,0),1)","v":{"$error":"#N/A"}}]
[0,{"$f":"INDEX('Import data'!$A:$A,MATCH($A1374,'Import data'!$A:$A,0),1)","v":{"$error":"#N/A"}}]
[0,{"$f":"INDEX('Import data'!$A:$A,MATCH($A1375,'Import data'!$A:$A,0),1)","v":{"$error":"#N/A"}}]
[0,{"$f":"INDEX('Import data'!$A:$A,MATCH($A1376,'Import data'!$A:$A,0),1)","v":{"$error":"#N/A"}}]
[0,{"$f":"INDEX('Import data'!$A:$A,MATCH($A1377,'Import data'!$A:$A,0),1)","v":{"$error":"#N/A"}}]
[0,{"$f":"INDEX('Import data'!$A:$A,MATCH($A1378,'Import data'!$A:$A,0),1)","v":{"$error":"#N/A"}}]
[0,{"$f":"INDEX('Import data'!$A:$A,MATCH($A1379,'Import data'!$A:$A,0),1)","v":{"$error":"#N/A"}}]
[0,{"$f":"INDEX('Import data'!$A:$A,MATCH($A1380,'Import data'!$A:$A,0),1)","v":{"$error":"#N/A"}}]
[0,{"$f":"INDEX('Import data'!$A:$A,MATCH($A1381,'Import data'!$A:$A,0),1)","v":{"$error":"#N/A"}}]
[0,{"$f":"INDEX('Import data'!$A:$A,MATCH($A1382,'Import data'!$A:$A,0),1)","v":{"$error":"#N/A"}}]
[0,{"$f":"INDEX('Import data'!$A:$A,MATCH($A1383,'Import data'!$A:$A,0),1)","v":{"$error":"#N/A"}}]
[0,{"$f":"INDEX('Import data'!$A:$A,MATCH($A1384,'Import data'!$A:$A,0),1)","v":{"$error":"#N/A"}}]
[0,{"$f":"INDEX('Import data'!$A:$A,MATCH($A1385,'Import data'!$A:$A,0),1)","v":{"$error":"#N/A"}}]
[0,{"$f":"INDEX('Import data'!$A:$A,MATCH($A1386,'Import data'!$A:$A,0),1)","v":{"$error":"#N/A"}}]
[0,{"$f":"INDEX('Import data'!$A:$A,MATCH($A1387,'Import data'!$A:$A,0),1)","v":{"$error":"#N/A"}}]
[0,{"$f":"INDEX('Import data'!$A:$A,MATCH($A1388,'Import data'!$A:$A,0),1)","v":{"$error":"#N/A"}}]
[0,{"$f":"INDEX('Import data'!$A:$A,MATCH($A1389,'Import data'!$A:$A,0),1)","v":{"$error":"#N/A"}}]
[0,{"$f":"INDEX('Import data'!$A:$A,MATCH($A1390,'Import data'!$A:$A,0),1)","v":{"$error":"#N/A"}}]
[0,{"$f":"INDEX('Import data'!$A:$A,MATCH($A1391,'Import data'!$A:$A,0),1)","v":{"$error":"#N/A"}}]
[0,{"$f":"INDEX('Import data'!$A:$A,MATCH($A1392,'Import data'!$A:$A,0),1)","v":{"$error":"#N/A"}}]
[0,{"$f":"INDEX('Import data'!$A:$A,MATCH($A1393,'Import data'!$A:$A,0),1)","v":{"$error":"#N/A"}}]
[0,{"$f":"INDEX('Import data'!$A:$A,MATCH($A1394,'Import data'!$A:$A,0),1)","v":{"$error":"#N/A"}}]
[0,{"$f":"INDEX('Import data'!$A:$A,MATCH($A1395,'Import data'!$A:$A,0),1)","v":{"$error":"#N/A"}}]
[0,{"$f":"INDEX('Import data'!$A:$A,MATCH($A1396,'Import data'!$A:$A,0),1)","v":{"$error":"#N/A"}}]
[0,{"$f":"INDEX('Import data'!$A:$A,MATCH($A1397,'Import data'!$A:$A,0),1)","v":{"$error":"#N/A"}}]
[0,{"$f":"INDEX('Import data'!$A:$A,MATCH($A1398,'Import data'!$A:$A,0),1)","v":{"$error":"#N/A"}}]
[0,{"$f":"INDEX('Import data'!$A:$A,MATCH($A1399,'Import data'!$A:$A,0),1)","v":{"$error":"#N/A"}}]
[0,{"$f":"INDEX('Import data'!$A:$A,MATCH($A1400,'Import data'!$A:$A,0),1)","v":{"$error":"#N/A"}}]
[0,{"$f":"INDEX('Import data'!$A:$A,MATCH($A1401,'Import data'!$A:$A,0),1)","v":{"$error":"#N/A"}}]
[0,{"$f":"INDEX('Import data'!$A:$A,MATCH($A1402,'Import data'!$A:$A,0),1)","v":{"$error":"#N/A"}}]
[0,{"$f":"INDEX('Import data'!$A:$A,MATCH($A1403,'Import data'!$A:$A,0),1)","v":{"$error":"#N/A"}}]
[0,{"$f":"INDEX('Import data'!$A:$A,MATCH($A1404,'Import data'!$A:$A,0),1)","v":{"$error":"#N/A"}}]
[0,{"$f":"INDEX('Import data'!$A:$A,MATCH($A1405,'Import data'!$A:$A,0),1)","v":{"$error":"#N/A"}}]
[0,{"$f":"INDEX('Import data'!$A:$A,MATCH($A1406,'Import data'!$A:$A,0),1)","v":{"$error":"#N/A"}}]
[0,{"$f":"INDEX('Import data'!$A:$A,MATCH($A1407,'Import data'!$A:$A,0),1)","v":{"$error":"#N/A"}}]
[0,{"$f":"INDEX('Import data'!$A:$A,MATCH($A1408,'Import data'!$A:$A,0),1)","v":{"$error":"#N/A"}}]
[0,{"$f":"INDEX('Import data'!$A:$A,MATCH($A1409,'Import data'!$A:$A,0),1)","v":{"$error":"#N/A"}}]
[0,{"$f":"INDEX('Import data'!$A:$A,MATCH($A1410,'Import data'!$A:$A,0),1)","v":{"$error":"#N/A"}}]
[{"$f":"ID","v":0},{"$f":"INDEX('Import data'!$A:$A,MATCH($A1411,'Import data'!$A:$A,0),1)","v":{"$error":"#N/A"}}]
[0,{"$f":"INDEX('Import data'!$A:$A,MATCH($A1412,'Import data'!$A:$A,0),1)","v":{"$error":"#N/A"}}]
[0,{"$f":"INDEX('Import data'!$A:$A,MATCH($A1413,'Import data'!$A:$A,0),1)","v":{"$error":"#N/A"}}]
[0,{"$f":"INDEX('Import data'!$A:$A,MATCH($A1414,'Import data'!$A:$A,0),1)","v":{"$error":"#N/A"}}]
[0,{"$f":"INDEX('Import data'!$A:$A,MATCH($A1415,'Import data'!$A:$A,0),1)","v":{"$error":"#N/A"}}]
[0,{"$f":"INDEX('Import data'!$A:$A,MATCH($A1416,'Import data'!$A:$A,0),1)","v":{"$error":"#N/A"}}]
[0,{"$f":"INDEX('Import data'!$A:$A,MATCH($A1417,'Import data'!$A:$A,0),1)","v":{"$error":"#N/A"}}]
[0,{"$f":"INDEX('Import data'!$A:$A,MATCH($A1418,'Import data'!$A:$A,0),1)","v":{"$error":"#N/A"}}]
[0,{"$f":"INDEX('Import data'!$A:$A,MATCH($A1419,'Import data'!$A:$A,0),1)","v":{"$error":"#N/A"}}]
[0,{"$f":"INDEX('Import data'!$A:$A,MATCH($A1420,'Import data'!$A:$A,0),1)","v":{"$error":"#N/A"}}]
[0,{"$f":"INDEX('Import data'!$A:$A,MATCH($A1421,'Import data'!$A:$A,0),1)","v":{"$error":"#N/A"}}]
[0,{"$f":"INDEX('Import data'!$A:$A,MATCH($A1422,'Import data'!$A:$A,0),1)","v":{"$error":"#N/A"}}]
[0,{"$f":"INDEX('Import data'!$A:$A,MATCH($A1423,'Import data'!$A:$A,0),1)","v":{"$error":"#N/A"}}]
[0,{"$f":"INDEX('Import data'!$A:$A,MATCH($A1424,'Import data'!$A:$A,0),1)","v":{"$error":"#N/A"}}]
[0,{"$f":"INDEX('Import data'!$A:$A,MATCH($A1425,'Import data'!$A:$A,0),1)","v":{"$error":"#N/A"}}]
[0,{"$f":"INDEX('Import data'!$A:$A,MATCH($A1426,'Import data'!$A:$A,0),1)","v":{"$error":"#N/A"}}]
[0,{"$f":"INDEX('Import data'!$A:$A,MATCH($A1427,'Import data'!$A:$A,0),1)","v":{"$error":"#N/A"}}]
[0,{"$f":"INDEX('Import data'!$A:$A,MATCH($A1428,'Import data'!$A:$A,0),1)","v":{"$error":"#N/A"}}]
[0,{"$f":"INDEX('Import data'!$A:$A,MATCH($A1429,'Import data'!$A:$A,0),1)","v":{"$error":"#N/A"}}]
[0,{"$f":"INDEX('Import data'!$A:$A,MATCH($A1430,'Import data'!$A:$A,0),1)","v":{"$error":"#N/A"}}]
[0,{"$f":"INDEX('Import data'!$A:$A,MATCH($A1431,'Import data'!$A:$A,0),1)","v":{"$error":"#N/A"}}]
[0,{"$f":"INDEX('Import data'!$A:$A,MATCH($A1432,'Import data'!$A:$A,0),1)","v":{"$error":"#N/A"}}]
[0,{"$f":"INDEX('Import data'!$A:$A,MATCH($A1433,'Import data'!$A:$A,0),1)","v":{"$error":"#N/A"}}]
[0,{"$f":"INDEX('Import data'!$A:$A,MATCH($A1434,'Import data'!$A:$A,0),1)","v":{"$error":"#N/A"}}]
[0,{"$f":"INDEX('Import data'!$A:$A,MATCH($A1435,'Import data'!$A:$A,0),1)","v":{"$error":"#N/A"}}]
[0,{"$f":"INDEX('Import data'!$A:$A,MATCH($A1436,'Import data'!$A:$A,0),1)","v":{"$error":"#N/A"}}]
[0,{"$f":"INDEX('Import data'!$A:$A,MATCH($A1437,'Import data'!$A:$A,0),1)","v":{"$error":"#N/A"}}]
[0,{"$f":"INDEX('Import data'!$A:$A,MATCH($A1438,'Import data'!$A:$A,0),1)","v":{"$error":"#N/A"}}]
[0,{"$f":"INDEX('Import data'!$A:$A,MATCH($A1439,'Import data'!$A:$A,0),1)","v":{"$error":"#N/A"}}]
[0,{"$f":"INDEX('Import data'!$A:$A,MATCH($A1440,'Import data'!$A:$A,0),1)","v":{"$error":"#N/A"}}]
[0,{"$f":"INDEX('Import data'!$A:$A,MATCH($A1441,'Import data'!$A:$A,0),1)","v":{"$error":"#N/A"}}]
[0,{"$f":"INDEX('Import data'!$A:$A,MATCH($A1442,'Import data'!$A:$A,0),1)","v":{"$error":"#N/A"}}]
[0,{"$f":"INDEX('Import data'!$A:$A,MATCH($A1443,'Import data'!$A:$A,0),1)","v":{"$error":"#N/A"}}]
[0,{"$f":"INDEX('Import data'!$A:$A,MATCH($A1444,'Import data'!$A:$A,0),1)","v":{"$error":"#N/A"}}]
[0,{"$f":"INDEX('Import data'!$A:$A,MATCH($A1445,'Import data'!$A:$A,0),1)","v":{"$error":"#N/A"}}]
[0,{"$f":"INDEX('Import data'!$A:$A,MATCH($A1446,'Import data'!$A:$A,0),1)","v":{"$error":"#N/A"}}]
[0,{"$f":"INDEX('Import data'!$A:$A,MATCH($A1447,'Import data'!$A:$A,0),1)","v":{"$error":"#N/A"}}]
[0,{"$f":"INDEX('Import data'!$A:$A,MATCH($A1448,'Import data'!$A:$A,0),1)","v":{"$error":"#N/A"}}]
[0,{"$f":"INDEX('Import data'!$A:$A,MATCH($A1449,'Import data'!$A:$A,0),1)","v":{"$error":"#N/A"}}]
[0,{"$f":"INDEX('Import data'!$A:$A,MATCH($A1450,'Import data'!$A:$A,0),1)","v":{"$error":"#N/A"}}]
[0,{"$f":"INDEX('Import data'!$A:$A,MATCH($A1451,'Import data'!$A:$A,0),1)","v":{"$error":"#N/A"}}]
[0,{"$f":"INDEX('Import data'!$A:$A,MATCH($A1452,'Import data'!$A:$A,0),1)","v":{"$error":"#N/A"}}]
[0,{"$f":"INDEX('Import data'!$A:$A,MATCH($A1453,'Import data'!$A:$A,0),1)","v":{"$error":"#N/A"}}]
[0,{"$f":"INDEX('Import data'!$A:$A,MATCH($A1454,'Import data'!$A:$A,0),1)","v":{"$error":"#N/A"}}]
[0,{"$f":"INDEX('Import data'!$A:$A,MATCH($A1455,'Import data'!$A:$A,0),1)","v":{"$error":"#N/A"}}]
[0,{"$f":"INDEX('Import data'!$A:$A,MATCH($A1456,'Import data'!$A:$A,0),1)","v":{"$error":"#N/A"}}]
[0,{"$f":"INDEX('Import data'!$A:$A,MATCH($A1457,'Import data'!$A:$A,0),1)","v":{"$error":"#N/A"}}]
[0,{"$f":"INDEX('Import data'!$A:$A,MATCH($A1458,'Import data'!$A:$A,0),1)","v":{"$error":"#N/A"}}]
[0,{"$f":"INDEX('Import data'!$A:$A,MATCH($A1459,'Import data'!$A:$A,0),1)","v":{"$error":"#N/A"}}]
[0,{"$f":"INDEX('Import data'!$A:$A,MATCH($A1460,'Import data'!$A:$A,0),1)","v":{"$error":"#N/A"}}]
[0,{"$f":"INDEX('Import data'!$A:$A,MATCH($A1461,'Import data'!$A:$A,0),1)","v":{"$error":"#N/A"}}]
[0,{"$f":"INDEX('Import data'!$A:$A,MATCH($A1462,'Import data'!$A:$A,0),1)","v":{"$error":"#N/A"}}]
[0,{"$f":"INDEX('Import data'!$A:$A,MATCH($A1463,'Import data'!$A:$A,0),1)","v":{"$error":"#N/A"}}]
[0,{"$f":"INDEX('Import data'!$A:$A,MATCH($A1464,'Import data'!$A:$A,0),1)","v":{"$error":"#N/A"}}]
[0,{"$f":"INDEX('Import data'!$A:$A,MATCH($A1465,'Import data'!$A:$A,0),1)","v":{"$error":"#N/A"}}]
[0,{"$f":"INDEX('Import data'!$A:$A,MATCH($A1466,'Import data'!$A:$A,0),1)","v":{"$error":"#N/A"}}]
[0,{"$f":"INDEX('Import data'!$A:$A,MATCH($A1467,'Import data'!$A:$A,0),1)","v":{"$error":"#N/A"}}]
[0,{"$f":"INDEX('Import data'!$A:$A,MATCH($A1468,'Import data'!$A:$A,0),1)","v":{"$error":"#N/A"}}]
[0,{"$f":"INDEX('Import data'!$A:$A,MATCH($A1469,'Import data'!$A:$A,0),1)","v":{"$error":"#N/A"}}]
[0,{"$f":"INDEX('Import data'!$A:$A,MATCH($A1470,'Import data'!$A:$A,0),1)","v":{"$error":"#N/A"}}]
[0,{"$f":"INDEX('Import data'!$A:$A,MATCH($A1471,'Import data'!$A:$A,0),1)","v":{"$error":"#N/A"}}]
[0,{"$f":"INDEX('Import data'!$A:$A,MATCH($A1472,'Import data'!$A:$A,0),1)","v":{"$error":"#N/A"}}]
[0,{"$f":"INDEX('Import data'!$A:$A,MATCH($A1473,'Import data'!$A:$A,0),1)","v":{"$error":"#N/A"}}]
[0,{"$f":"INDEX('Import data'!$A:$A,MATCH($A1474,'Import data'!$A:$A,0),1)","v":{"$error":"#N/A"}}]
[{"$f":"ID","v":0},{"$f":"INDEX('Import data'!$A:$A,MATCH($A1475,'Import data'!$A:$A,0),1)","v":{"$error":"#N/A"}}]
[0,{"$f":"INDEX('Import data'!$A:$A,MATCH($A1476,'Import data'!$A:$A,0),1)","v":{"$error":"#N/A"}}]
[0,{"$f":"INDEX('Import data'!$A:$A,MATCH($A1477,'Import data'!$A:$A,0),1)","v":{"$error":"#N/A"}}]
[0,{"$f":"INDEX('Import data'!$A:$A,MATCH($A1478,'Import data'!$A:$A,0),1)","v":{"$error":"#N/A"}}]
[0,{"$f":"INDEX('Import data'!$A:$A,MATCH($A1479,'Import data'!$A:$A,0),1)","v":{"$error":"#N/A"}}]
[0,{"$f":"INDEX('Import data'!$A:$A,MATCH($A1480,'Import data'!$A:$A,0),1)","v":{"$error":"#N/A"}}]
[0,{"$f":"INDEX('Import data'!$A:$A,MATCH($A1481,'Import data'!$A:$A,0),1)","v":{"$error":"#N/A"}}]
[0,{"$f":"INDEX('Import data'!$A:$A,MATCH($A1482,'Import data'!$A:$A,0),1)","v":{"$error":"#N/A"}}]
[0,{"$f":"INDEX('Import data'!$A:$A,MATCH($A1483,'Import data'!$A:$A,0),1)","v":{"$error":"#N/A"}}]
[0,{"$f":"INDEX('Import data'!$A:$A,MATCH($A1484,'Import data'!$A:$A,0),1)","v":{"$error":"#N/A"}}]
[0,{"$f":"INDEX('Import data'!$A:$A,MATCH($A1485,'Import data'!$A:$A,0),1)","v":{"$error":"#N/A"}}]
[0,{"$f":"INDEX('Import data'!$A:$A,MATCH($A1486,'Import data'!$A:$A,0),1)","v":{"$error":"#N/A"}}]
[0,{"$f":"INDEX('Import data'!$A:$A,MATCH($A1487,'Import data'!$A:$A,0),1)","v":{"$error":"#N/A"}}]
[0,{"$f":"INDEX('Import data'!$A:$A,MATCH($A1488,'Import data'!$A:$A,0),1)","v":{"$error":"#N/A"}}]
[0,{"$f":"INDEX('Import data'!$A:$A,MATCH($A1489,'Import data'!$A:$A,0),1)","v":{"$error":"#N/A"}}]
[0,{"$f":"INDEX('Import data'!$A:$A,MATCH($A1490,'Import data'!$A:$A,0),1)","v":{"$error":"#N/A"}}]
[0,{"$f":"INDEX('Import data'!$A:$A,MATCH($A1491,'Import data'!$A:$A,0),1)","v":{"$error":"#N/A"}}]
[0,{"$f":"INDEX('Import data'!$A:$A,MATCH($A1492,'Import data'!$A:$A,0),1)","v":{"$error":"#N/A"}}]
[0,{"$f":"INDEX('Import data'!$A:$A,MATCH($A1493,'Import data'!$A:$A,0),1)","v":{"$error":"#N/A"}}]
[0,{"$f":"INDEX('Import data'!$A:$A,MATCH($A1494,'Import data'!$A:$A,0),1)","v":{"$error":"#N/A"}}]
[0,{"$f":"INDEX('Import data'!$A:$A,MATCH($A1495,'Import data'!$A:$A,0),1)","v":{"$error":"#N/A"}}]
[0,{"$f":"INDEX('Import data'!$A:$A,MATCH($A1496,'Import data'!$A:$A,0),1)","v":{"$error":"#N/A"}}]
[0,{"$f":"INDEX('Import data'!$A:$A,MATCH($A1497,'Import data'!$A:$A,0),1)","v":{"$error":"#N/A"}}]
[0,{"$f":"INDEX('Import data'!$A:$A,MATCH($A1498,'Import data'!$A:$A,0),1)","v":{"$error":"#N/A"}}]
[0,{"$f":"INDEX('Import data'!$A:$A,MATCH($A1499,'Import data'!$A:$A,0),1)","v":{"$error":"#N/A"}}]
[0,{"$f":"INDEX('Import data'!$A:$A,MATCH($A1500,'Import data'!$A:$A,0),1)","v":{"$error":"#N/A"}}]
[0,{"$f":"INDEX('Import data'!$A:$A,MATCH($A1501,'Import data'!$A:$A,0),1)","v":{"$error":"#N/A"}}]
[0,{"$f":"INDEX('Import data'!$A:$A,MATCH($A1502,'Import data'!$A:$A,0),1)","v":{"$error":"#N/A"}}]
[0,{"$f":"INDEX('Import data'!$A:$A,MATCH($A1503,'Import data'!$A:$A,0),1)","v":{"$error":"#N/A"}}]
[0,{"$f":"INDEX('Import data'!$A:$A,MATCH($A1504,'Import data'!$A:$A,0),1)","v":{"$error":"#N/A"}}]
[0,{"$f":"INDEX('Import data'!$A:$A,MATCH($A1505,'Import data'!$A:$A,0),1)","v":{"$error":"#N/A"}}]
[0,{"$f":"INDEX('Import data'!$A:$A,MATCH($A1506,'Import data'!$A:$A,0),1)","v":{"$error":"#N/A"}}]
[0,{"$f":"INDEX('Import data'!$A:$A,MATCH($A1507,'Import data'!$A:$A,0),1)","v":{"$error":"#N/A"}}]
[0,{"$f":"INDEX('Import data'!$A:$A,MATCH($A1508,'Import data'!$A:$A,0),1)","v":{"$error":"#N/A"}}]
[0,{"$f":"INDEX('Import data'!$A:$A,MATCH($A1509,'Import data'!$A:$A,0),1)","v":{"$error":"#N/A"}}]
[0,{"$f":"INDEX('Import data'!$A:$A,MATCH($A1510,'Import data'!$A:$A,0),1)","v":{"$error":"#N/A"}}]
[0,{"$f":"INDEX('Import data'!$A:$A,MATCH($A1511,'Import data'!$A:$A,0),1)","v":{"$error":"#N/A"}}]
[0,{"$f":"INDEX('Import data'!$A:$A,MATCH($A1512,'Import data'!$A:$A,0),1)","v":{"$error":"#N/A"}}]
[0,{"$f":"INDEX('Import data'!$A:$A,MATCH($A1513,'Import data'!$A:$A,0),1)","v":{"$error":"#N/A"}}]
[0,{"$f":"INDEX('Import data'!$A:$A,MATCH($A1514,'Import data'!$A:$A,0),1)","v":{"$error":"#N/A"}}]
[0,{"$f":"INDEX('Import data'!$A:$A,MATCH($A1515,'Import data'!$A:$A,0),1)","v":{"$error":"#N/A"}}]
[0,{"$f":"INDEX('Import data'!$A:$A,MATCH($A1516,'Import data'!$A:$A,0),1)","v":{"$error":"#N/A"}}]
[0,{"$f":"INDEX('Import data'!$A:$A,MATCH($A1517,'Import data'!$A:$A,0),1)","v":{"$error":"#N/A"}}]
[0,{"$f":"INDEX('Import data'!$A:$A,MATCH($A1518,'Import data'!$A:$A,0),1)","v":{"$error":"#N/A"}}]
[0,{"$f":"INDEX('Import data'!$A:$A,MATCH($A1519,'Import data'!$A:$A,0),1)","v":{"$error":"#N/A"}}]
[0,{"$f":"INDEX('Import data'!$A:$A,MATCH($A1520,'Import data'!$A:$A,0),1)","v":{"$error":"#N/A"}}]
[0,{"$f":"INDEX('Import data'!$A:$A,MATCH($A1521,'Import data'!$A:$A,0),1)","v":{"$error":"#N/A"}}]
[0,{"$f":"INDEX('Import data'!$A:$A,MATCH($A1522,'Import data'!$A:$A,0),1)","v":{"$error":"#N/A"}}]
[0,{"$f":"INDEX('Import data'!$A:$A,MATCH($A1523,'Import data'!$A:$A,0),1)","v":{"$error":"#N/A"}}]
[0,{"$f":"INDEX('Import data'!$A:$A,MATCH($A1524,'Import data'!$A:$A,0),1)","v":{"$error":"#N/A"}}]
[0,{"$f":"INDEX('Import data'!$A:$A,MATCH($A1525,'Import data'!$A:$A,0),1)","v":{"$error":"#N/A"}}]
[0,{"$f":"INDEX('Import data'!$A:$A,MATCH($A1526,'Import data'!$A:$A,0),1)","v":{"$error":"#N/A"}}]
[0,{"$f":"INDEX('Import data'!$A:$A,MATCH($A1527,'Import data'!$A:$A,0),1)","v":{"$error":"#N/A"}}]
[0,{"$f":"INDEX('Import data'!$A:$A,MATCH($A1528,'Import data'!$A:$A,0),1)","v":{"$error":"#N/A"}}]
[0,{"$f":"INDEX('Import data'!$A:$A,MATCH($A1529,'Import data'!$A:$A,0),1)","v":{"$error":"#N/A"}}]
[0,{"$f":"INDEX('Import data'!$A:$A,MATCH($A1530,'Import data'!$A:$A,0),1)","v":{"$error":"#N/A"}}]
[0,{"$f":"INDEX('Import data'!$A:$A,MATCH($A1531,'Import data'!$A:$A,0),1)","v":{"$error":"#N/A"}}]
[0,{"$f":"INDEX('Import data'!$A:$A,MATCH($A1532,'Import data'!$A:$A,0),1)","v":{"$error":"#N/A"}}]
[0,{"$f":"INDEX('Import data'!$A:$A,MATCH($A1533,'Import data'!$A:$A,0),1)","v":{"$error":"#N/A"}}]
[0,{"$f":"INDEX('Import data'!$A:$A,MATCH($A1534,'Import data'!$A:$A,0),1)","v":{"$error":"#N/A"}}]
[0,{"$f":"INDEX('Import data'!$A:$A,MATCH($A1535,'Import data'!$A:$A,0),1)","v":{"$error":"#N/A"}}]
[0,{"$f":"INDEX('Import data'!$A:$A,MATCH($A1536,'Import data'!$A:$A,0),1)","v":{"$error":"#N/A"}}]
[0,{"$f":"INDEX('Import data'!$A:$A,MATCH($A1537,'Import data'!$A:$A,0),1)","v":{"$error":"#N/A"}}]
[0,{"$f":"INDEX('Import data'!$A:$A,MATCH($A1538,'Import data'!$A:$A,0),1)","v":{"$error":"#N/A"}}]
[{"$f":"ID","v":0},{"$f":"INDEX('Import data'!$A:$A,MATCH($A1539,'Import data'!$A:$A,0),1)","v":{"$error":"#N/A"}}]
[0,{"$f":"INDEX('Import data'!$A:$A,MATCH($A1540,'Import data'!$A:$A,0),1)","v":{"$error":"#N/A"}}]
[0,{"$f":"INDEX('Import data'!$A:$A,MATCH($A1541,'Import data'!$A:$A,0),1)","v":{"$error":"#N/A"}}]
[0,{"$f":"INDEX('Import data'!$A:$A,MATCH($A1542,'Import data'!$A:$A,0),1)","v":{"$error":"#N/A"}}]
[0,{"$f":"INDEX('Import data'!$A:$A,MATCH($A1543,'Import data'!$A:$A,0),1)","v":{"$error":"#N/A"}}]
[0,{"$f":"INDEX('Import data'!$A:$A,MATCH($A1544,'Import data'!$A:$A,0),1)","v":{"$error":"#N/A"}}]
[0,{"$f":"INDEX('Import data'!$A:$A,MATCH($A1545,'Import data'!$A:$A,0),1)","v":{"$error":"#N/A"}}]
[0,{"$f":"INDEX('Import data'!$A:$A,MATCH($A1546,'Import data'!$A:$A,0),1)","v":{"$error":"#N/A"}}]
[0,{"$f":"INDEX('Import data'!$A:$A,MATCH($A1547,'Import data'!$A:$A,0),1)","v":{"$error":"#N/A"}}]
[0,{"$f":"INDEX('Import data'!$A:$A,MATCH($A1548,'Import data'!$A:$A,0),1)","v":{"$error":"#N/A"}}]
[0,{"$f":"INDEX('Import data'!$A:$A,MATCH($A1549,'Import data'!$A:$A,0),1)","v":{"$error":"#N/A"}}]
[0,{"$f":"INDEX('Import data'!$A:$A,MATCH($A1550,'Import data'!$A:$A,0),1)","v":{"$error":"#N/A"}}]
[0,{"$f":"INDEX('Import data'!$A:$A,MATCH($A1551,'Import data'!$A:$A,0),1)","v":{"$error":"#N/A"}}]
[0,{"$f":"INDEX('Import data'!$A:$A,MATCH($A1552,'Import data'!$A:$A,0),1)","v":{"$error":"#N/A"}}]
[0,{"$f":"INDEX('Import data'!$A:$A,MATCH($A1553,'Import data'!$A:$A,0),1)","v":{"$error":"#N/A"}}]
[0,{"$f":"INDEX('Import data'!$A:$A,MATCH($A1554,'Import data'!$A:$A,0),1)","v":{"$error":"#N/A"}}]
[0,{"$f":"INDEX('Import data'!$A:$A,MATCH($A1555,'Import data'!$A:$A,0),1)","v":{"$error":"#N/A"}}]
[0,{"$f":"INDEX('Import data'!$A:$A,MATCH($A1556,'Import data'!$A:$A,0),1)","v":{"$error":"#N/A"}}]
[0,{"$f":"INDEX('Import data'!$A:$A,MATCH($A1557,'Import data'!$A:$A,0),1)","v":{"$error":"#N/A"}}]
[0,{"$f":"INDEX('Import data'!$A:$A,MATCH($A1558,'Import data'!$A:$A,0),1)","v":{"$error":"#N/A"}}]
[0,{"$f":"INDEX('Import data'!$A:$A,MATCH($A1559,'Import data'!$A:$A,0),1)","v":{"$error":"#N/A"}}]
[0,{"$f":"INDEX('Import data'!$A:$A,MATCH($A1560,'Import data'!$A:$A,0),1)","v":{"$error":"#N/A"}}]
[0,{"$f":"INDEX('Import data'!$A:$A,MATCH($A1561,'Import data'!$A:$A,0),1)","v":{"$error":"#N/A"}}]
[0,{"$f":"INDEX('Import data'!$A:$A,MATCH($A1562,'Import data'!$A:$A,0),1)","v":{"$error":"#N/A"}}]
[0,{"$f":"INDEX('Import data'!$A:$A,MATCH($A1563,'Import data'!$A:$A,0),1)","v":{"$error":"#N/A"}}]
[0,{"$f":"INDEX('Import data'!$A:$A,MATCH($A1564,'Import data'!$A:$A,0),1)","v":{"$error":"#N/A"}}]
[0,{"$f":"INDEX('Import data'!$A:$A,MATCH($A1565,'Import data'!$A:$A,0),1)","v":{"$error":"#N/A"}}]
[0,{"$f":"INDEX('Import data'!$A:$A,MATCH($A1566,'Import data'!$A:$A,0),1)","v":{"$error":"#N/A"}}]
[0,{"$f":"INDEX('Import data'!$A:$A,MATCH($A1567,'Import data'!$A:$A,0),1)","v":{"$error":"#N/A"}}]
[0,{"$f":"INDEX('Import data'!$A:$A,MATCH($A1568,'Import data'!$A:$A,0),1)","v":{"$error":"#N/A"}}]
[0,{"$f":"INDEX('Import data'!$A:$A,MATCH($A1569,'Import data'!$A:$A,0),1)","v":{"$error":"#N/A"}}]
[0,{"$f":"INDEX('Import data'!$A:$A,MATCH($A1570,'Import data'!$A:$A,0),1)","v":{"$error":"#N/A"}}]
[0,{"$f":"INDEX('Import data'!$A:$A,MATCH($A1571,'Import data'!$A:$A,0),1)","v":{"$error":"#N/A"}}]
[0,{"$f":"INDEX('Import data'!$A:$A,MATCH($A1572,'Import data'!$A:$A,0),1)","v":{"$error":"#N/A"}}]
[0,{"$f":"INDEX('Import data'!$A:$A,MATCH($A1573,'Import data'!$A:$A,0),1)","v":{"$error":"#N/A"}}]
[0,{"$f":"INDEX('Import data'!$A:$A,MATCH($A1574,'Import data'!$A:$A,0),1)","v":{"$error":"#N/A"}}]
[0,{"$f":"INDEX('Import data'!$A:$A,MATCH($A1575,'Import data'!$A:$A,0),1)","v":{"$error":"#N/A"}}]
[0,{"$f":"INDEX('Import data'!$A:$A,MATCH($A1576,'Import data'!$A:$A,0),1)","v":{"$error":"#N/A"}}]
[0,{"$f":"INDEX('Import data'!$A:$A,MATCH($A1577,'Import data'!$A:$A,0),1)","v":{"$error":"#N/A"}}]
[0,{"$f":"INDEX('Import data'!$A:$A,MATCH($A1578,'Import data'!$A:$A,0),1)","v":{"$error":"#N/A"}}]
[0,{"$f":"INDEX('Import data'!$A:$A,MATCH($A1579,'Import data'!$A:$A,0),1)","v":{"$error":"#N/A"}}]
[0,{"$f":"INDEX('Import data'!$A:$A,MATCH($A1580,'Import data'!$A:$A,0),1)","v":{"$error":"#N/A"}}]
[0,{"$f":"INDEX('Import data'!$A:$A,MATCH($A1581,'Import data'!$A:$A,0),1)","v":{"$error":"#N/A"}}]
[0,{"$f":"INDEX('Import data'!$A:$A,MATCH($A1582,'Import data'!$A:$A,0),1)","v":{"$error":"#N/A"}}]
[0,{"$f":"INDEX('Import data'!$A:$A,MATCH($A1583,'Import data'!$A:$A,0),1)","v":{"$error":"#N/A"}}]
[0,{"$f":"INDEX('Import data'!$A:$A,MATCH($A1584,'Import data'!$A:$A,0),1)","v":{"$error":"#N/A"}}]
[0,{"$f":"INDEX('Import data'!$A:$A,MATCH($A1585,'Import data'!$A:$A,0),1)","v":{"$error":"#N/A"}}]
[0,{"$f":"INDEX('Import data'!$A:$A,MATCH($A1586,'Import data'!$A:$A,0),1)","v":{"$error":"#N/A"}}]
[0,{"$f":"INDEX('Import data'!$A:$A,MATCH($A1587,'Import data'!$A:$A,0),1)","v":{"$error":"#N/A"}}]
[0,{"$f":"INDEX('Import data'!$A:$A,MATCH($A1588,'Import data'!$A:$A,0),1)","v":{"$error":"#N/A"}}]
[0,{"$f":"INDEX('Import data'!$A:$A,MATCH($A1589,'Import data'!$A:$A,0),1)","v":{"$error":"#N/A"}}]
[0,{"$f":"INDEX('Import data'!$A:$A,MATCH($A1590,'Import data'!$A:$A,0),1)","v":{"$error":"#N/A"}}]
[0,{"$f":"INDEX('Import data'!$A:$A,MATCH($A1591,'Import data'!$A:$A,0),1)","v":{"$error":"#N/A"}}]
[0,{"$f":"INDEX('Import data'!$A:$A,MATCH($A1592,'Import data'!$A:$A,0),1)","v":{"$error":"#N/A"}}]
[0,{"$f":"INDEX('Import data'!$A:$A,MATCH($A1593,'Import data'!$A:$A,0),1)","v":{"$error":"#N/A"}}]
[0,{"$f":"INDEX('Import data'!$A:$A,MATCH($A1594,'Import data'!$A:$A,0),1)","v":{"$error":"#N/A"}}]
[0,{"$f":"INDEX('Import data'!$A:$A,MATCH($A1595,'Import data'!$A:$A,0),1)","v":{"$error":"#N/A"}}]
[0,{"$f":"INDEX('Import data'!$A:$A,MATCH($A1596,'Import data'!$A:$A,0),1)","v":{"$error":"#N/A"}}]
[0,{"$f":"INDEX('Import data'!$A:$A,MATCH($A1597,'Import data'!$A:$A,0),1)","v":{"$error":"#N/A"}}]
[0,{"$f":"INDEX('Import data'!$A:$A,MATCH($A1598,'Import data'!$A:$A,0),1)","v":{"$error":"#N/A"}}]
[0,{"$f":"INDEX('Import data'!$A:$A,MATCH($A1599,'Import data'!$A:$A,0),1)","v":{"$error":"#N/A"}}]
[0,{"$f":"INDEX('Import data'!$A:$A,MATCH($A1600,'Import data'!$A:$A,0),1)","v":{"$error":"#N/A"}}]
[0,{"$f":"INDEX('Import data'!$A:$A,MATCH($A1601,'Import data'!$A:$A,0),1)","v":{"$error":"#N/A"}}]
[0,{"$f":"INDEX('Import data'!$A:$A,MATCH($A1602,'Import data'!$A:$A,0),1)","v":{"$error":"#N/A"}}]
[{"$f":"ID","v":0},{"$f":"INDEX('Import data'!$A:$A,MATCH($A1603,'Import data'!$A:$A,0),1)","v":{"$error":"#N/A"}}]
[0,{"$f":"INDEX('Import data'!$A:$A,MATCH($A1604,'Import data'!$A:$A,0),1)","v":{"$error":"#N/A"}}]
[0,{"$f":"INDEX('Import data'!$A:$A,MATCH($A1605,'Import data'!$A:$A,0),1)","v":{"$error":"#N/A"}}]
[0,{"$f":"INDEX('Import data'!$A:$A,MATCH($A1606,'Import data'!$A:$A,0),1)","v":{"$error":"#N/A"}}]
[0,{"$f":"INDEX('Import data'!$A:$A,MATCH($A1607,'Import data'!$A:$A,0),1)","v":{"$error":"#N/A"}}]
[0,{"$f":"INDEX('Import data'!$A:$A,MATCH($A1608,'Import data'!$A:$A,0),1)","v":{"$error":"#N/A"}}]
[0,{"$f":"INDEX('Import data'!$A:$A,MATCH($A1609,'Import data'!$A:$A,0),1)","v":{"$error":"#N/A"}}]
[0,{"$f":"INDEX('Import data'!$A:$A,MATCH($A1610,'Import data'!$A:$A,0),1)","v":{"$error":"#N/A"}}]
[0,{"$f":"INDEX('Import data'!$A:$A,MATCH($A1611,'Import data'!$A:$A,0),1)","v":{"$error":"#N/A"}}]
[0,{"$f":"INDEX('Import data'!$A:$A,MATCH($A1612,'Import data'!$A:$A,0),1)","v":{"$error":"#N/A"}}]
[0,{"$f":"INDEX('Import data'!$A:$A,MATCH($A1613,'Import data'!$A:$A,0),1)","v":{"$error":"#N/A"}}]
[0,{"$f":"INDEX('Import data'!$A:$A,MATCH($A1614,'Import data'!$A:$A,0),1)","v":{"$error":"#N/A"}}]
[0,{"$f":"INDEX('Import data'!$A:$A,MATCH($A1615,'Import data'!$A:$A,0),1)","v":{"$error":"#N/A"}}]
[0,{"$f":"INDEX('Import data'!$A:$A,MATCH($A1616,'Import data'!$A:$A,0),1)","v":{"$error":"#N/A"}}]
[0,{"$f":"INDEX('Import data'!$A:$A,MATCH($A1617,'Import data'!$A:$A,0),1)","v":{"$error":"#N/A"}}]
[0,{"$f":"INDEX('Import data'!$A:$A,MATCH($A1618,'Import data'!$A:$A,0),1)","v":{"$error":"#N/A"}}]
[0,{"$f":"INDEX('Import data'!$A:$A,MATCH($A1619,'Import data'!$A:$A,0),1)","v":{"$error":"#N/A"}}]
[0,{"$f":"INDEX('Import data'!$A:$A,MATCH($A1620,'Import data'!$A:$A,0),1)","v":{"$error":"#N/A"}}]
[0,{"$f":"INDEX('Import data'!$A:$A,MATCH($A1621,'Import data'!$A:$A,0),1)","v":{"$error":"#N/A"}}]
[0,{"$f":"INDEX('Import data'!$A:$A,MATCH($A1622,'Import data'!$A:$A,0),1)","v":{"$error":"#N/A"}}]
[0,{"$f":"INDEX('Import data'!$A:$A,MATCH($A1623,'Import data'!$A:$A,0),1)","v":{"$error":"#N/A"}}]
[0,{"$f":"INDEX('Import data'!$A:$A,MATCH($A1624,'Import data'!$A:$A,0),1)","v":{"$error":"#N/A"}}]
[0,{"$f":"INDEX('Import data'!$A:$A,MATCH($A1625,'Import data'!$A:$A,0),1)","v":{"$error":"#N/A"}}]
[0,{"$f":"INDEX('Import data'!$A:$A,MATCH($A1626,'Import data'!$A:$A,0),1)","v":{"$error":"#N/A"}}]
[0,{"$f":"INDEX('Import data'!$A:$A,MATCH($A1627,'Import data'!$A:$A,0),1)","v":{"$error":"#N/A"}}]
[0,{"$f":"INDEX('Import data'!$A:$A,MATCH($A1628,'Import data'!$A:$A,0),1)","v":{"$error":"#N/A"}}]
[0,{"$f":"INDEX('Import data'!$A:$A,MATCH($A1629,'Import data'!$A:$A,0),1)","v":{"$error":"#N/A"}}]
[0,{"$f":"INDEX('Import data'!$A:$A,MATCH($A1630,'Import data'!$A:$A,0),1)","v":{"$error":"#N/A"}}]
[0,{"$f":"INDEX('Import data'!$A:$A,MATCH($A1631,'Import data'!$A:$A,0),1)","v":{"$error":"#N/A"}}]
[0,{"$f":"INDEX('Import data'!$A:$A,MATCH($A1632,'Import data'!$A:$A,0),1)","v":{"$error":"#N/A"}}]
[0,{"$f":"INDEX('Import data'!$A:$A,MATCH($A1633,'Import data'!$A:$A,0),1)","v":{"$error":"#N/A"}}]
[0,{"$f":"INDEX('Import data'!$A:$A,MATCH($A1634,'Import data'!$A:$A,0),1)","v":{"$error":"#N/A"}}]
[0,{"$f":"INDEX('Import data'!$A:$A,MATCH($A1635,'Import data'!$A:$A,0),1)","v":{"$error":"#N/A"}}]
[0,{"$f":"INDEX('Import data'!$A:$A,MATCH($A1636,'Import data'!$A:$A,0),1)","v":{"$error":"#N/A"}}]
[0,{"$f":"INDEX('Import data'!$A:$A,MATCH($A1637,'Import data'!$A:$A,0),1)","v":{"$error":"#N/A"}}]
[0,{"$f":"INDEX('Import data'!$A:$A,MATCH($A1638,'Import data'!$A:$A,0),1)","v":{"$error":"#N/A"}}]
[0,{"$f":"INDEX('Import data'!$A:$A,MATCH($A1639,'Import data'!$A:$A,0),1)","v":{"$error":"#N/A"}}]
[0,{"$f":"INDEX('Import data'!$A:$A,MATCH($A1640,'Import data'!$A:$A,0),1)","v":{"$error":"#N/A"}}]
[0,{"$f":"INDEX('Import data'!$A:$A,MATCH($A1641,'Import data'!$A:$A,0),1)","v":{"$error":"#N/A"}}]
[0,{"$f":"INDEX('Import data'!$A:$A,MATCH($A1642,'Import data'!$A:$A,0),1)","v":{"$error":"#N/A"}}]
[0,{"$f":"INDEX('Import data'!$A:$A,MATCH($A1643,'Import data'!$A:$A,0),1)","v":{"$error":"#N/A"}}]
[0,{"$f":"INDEX('Import data'!$A:$A,MATCH($A1644,'Import data'!$A:$A,0),1)","v":{"$error":"#N/A"}}]
[0,{"$f":"INDEX('Import data'!$A:$A,MATCH($A1645,'Import data'!$A:$A,0),1)","v":{"$error":"#N/A"}}]
[0,{"$f":"INDEX('Import data'!$A:$A,MATCH($A1646,'Import data'!$A:$A,0),1)","v":{"$error":"#N/A"}}]
[0,{"$f":"INDEX('Import data'!$A:$A,MATCH($A1647,'Import data'!$A:$A,0),1)","v":{"$error":"#N/A"}}]
[0,{"$f":"INDEX('Import data'!$A:$A,MATCH($A1648,'Import data'!$A:$A,0),1)","v":{"$error":"#N/A"}}]
[0,{"$f":"INDEX('Import data'!$A:$A,MATCH($A1649,'Import data'!$A:$A,0),1)","v":{"$error":"#N/A"}}]
[0,{"$f":"INDEX('Import data'!$A:$A,MATCH($A1650,'Import data'!$A:$A,0),1)","v":{"$error":"#N/A"}}]
[0,{"$f":"INDEX('Import data'!$A:$A,MATCH($A1651,'Import data'!$A:$A,0),1)","v":{"$error":"#N/A"}}]
[0,{"$f":"INDEX('Import data'!$A:$A,MATCH($A1652,'Import data'!$A:$A,0),1)","v":{"$error":"#N/A"}}]
[0,{"$f":"INDEX('Import data'!$A:$A,MATCH($A1653,'Import data'!$A:$A,0),1)","v":{"$error":"#N/A"}}]
[0,{"$f":"INDEX('Import data'!$A:$A,MATCH($A1654,'Import data'!$A:$A,0),1)","v":{"$error":"#N/A"}}]
[0,{"$f":"INDEX('Import data'!$A:$A,MATCH($A1655,'Import data'!$A:$A,0),1)","v":{"$error":"#N/A"}}]
[0,{"$f":"INDEX('Import data'!$A:$A,MATCH($A1656,'Import data'!$A:$A,0),1)","v":{"$error":"#N/A"}}]
[0,{"$f":"INDEX('Import data'!$A:$A,MATCH($A1657,'Import data'!$A:$A,0),1)","v":{"$error":"#N/A"}}]
[0,{"$f":"INDEX('Import data'!$A:$A,MATCH($A1658,'Import data'!$A:$A,0),1)","v":{"$error":"#N/A"}}]
[0,{"$f":"INDEX('Import data'!$A:$A,MATCH($A1659,'Import data'!$A:$A,0),1)","v":{"$error":"#N/A"}}]
[0,{"$f":"INDEX('Import data'!$A:$A,MATCH($A1660,'Import data'!$A:$A,0),1)","v":{"$error":"#N/A"}}]
[0,{"$f":"INDEX('Import data'!$A:$A,MATCH($A1661,'Import data'!$A:$A,0),1)","v":{"$error":"#N/A"}}]
[0,{"$f":"INDEX('Import data'!$A:$A,MATCH($A1662,'Import data'!$A:$A,0),1)","v":{"$error":"#N/A"}}]
[0,{"$f":"INDEX('Import data'!$A:$A,MATCH($A1663,'Import data'!$A:$A,0),1)","v":{"$error":"#N/A"}}]
[0,{"$f":"INDEX('Import data'!$A:$A,MATCH($A1664,'Import data'!$A:$A,0),1)","v":{"$error":"#N/A"}}]
[0,{"$f":"INDEX('Import data'!$A:$A,MATCH($A1665,'Import data'!$A:$A,0),1)","v":{"$error":"#N/A"}}]
[0,{"$f":"INDEX('Import data'!$A:$A,MATCH($A1666,'Import data'!$A:$A,0),1)","v":{"$error":"#N/A"}}]
[{"$f":"ID","v":0},{"$f":"INDEX('Import data'!$A:$A,MATCH($A1667,'Import data'!$A:$A,0),1)","v":{"$error":"#N/A"}}]
[0,{"$f":"INDEX('Import data'!$A:$A,MATCH($A1668,'Import data'!$A:$A,0),1)","v":{"$error":"#N/A"}}]
[0,{"$f":"INDEX('Import data'!$A:$A,MATCH($A1669,'Import data'!$A:$A,0),1)","v":{"$error":"#N/A"}}]
[0,{"$f":"INDEX('Import data'!$A:$A,MATCH($A1670,'Import data'!$A:$A,0),1)","v":{"$error":"#N/A"}}]
[0,{"$f":"INDEX('Import data'!$A:$A,MATCH($A1671,'Import data'!$A:$A,0),1)","v":{"$error":"#N/A"}}]
[0,{"$f":"INDEX('Import data'!$A:$A,MATCH($A1672,'Import data'!$A:$A,0),1)","v":{"$error":"#N/A"}}]
[0,{"$f":"INDEX('Import data'!$A:$A,MATCH($A1673,'Import data'!$A:$A,0),1)","v":{"$error":"#N/A"}}]
[0,{"$f":"INDEX('Import data'!$A:$A,MATCH($A1674,'Import data'!$A:$A,0),1)","v":{"$error":"#N/A"}}]
[0,{"$f":"INDEX('Import data'!$A:$A,MATCH($A1675,'Import data'!$A:$A,0),1)","v":{"$error":"#N/A"}}]
[0,{"$f":"INDEX('Import data'!$A:$A,MATCH($A1676,'Import data'!$A:$A,0),1)","v":{"$error":"#N/A"}}]
[0,{"$f":"INDEX('Import data'!$A:$A,MATCH($A1677,'Import data'!$A:$A,0),1)","v":{"$error":"#N/A"}}]
[0,{"$f":"INDEX('Import data'!$A:$A,MATCH($A1678,'Import data'!$A:$A,0),1)","v":{"$error":"#N/A"}}]
[0,{"$f":"INDEX('Import data'!$A:$A,MATCH($A1679,'Import data'!$A:$A,0),1)","v":{"$error":"#N/A"}}]
[0,{"$f":"INDEX('Import data'!$A:$A,MATCH($A1680,'Import data'!$A:$A,0),1)","v":{"$error":"#N/A"}}]
[0,{"$f":"INDEX('Import data'!$A:$A,MATCH($A1681,'Import data'!$A:$A,0),1)","v":{"$error":"#N/A"}}]
[0,{"$f":"INDEX('Import data'!$A:$A,MATCH($A1682,'Import data'!$A:$A,0),1)","v":{"$error":"#N/A"}}]
[0,{"$f":"INDEX('Import data'!$A:$A,MATCH($A1683,'Import data'!$A:$A,0),1)","v":{"$error":"#N/A"}}]
[0,{"$f":"INDEX('Import data'!$A:$A,MATCH($A1684,'Import data'!$A:$A,0),1)","v":{"$error":"#N/A"}}]
[0,{"$f":"INDEX('Import data'!$A:$A,MATCH($A1685,'Import data'!$A:$A,0),1)","v":{"$error":"#N/A"}}]
[0,{"$f":"INDEX('Import data'!$A:$A,MATCH($A1686,'Import data'!$A:$A,0),1)","v":{"$error":"#N/A"}}]
[0,{"$f":"INDEX('Import data'!$A:$A,MATCH($A1687,'Import data'!$A:$A,0),1)","v":{"$error":"#N/A"}}]
[0,{"$f":"INDEX('Import data'!$A:$A,MATCH($A1688,'Import data'!$A:$A,0),1)","v":{"$error":"#N/A"}}]
[0,{"$f":"INDEX('Import data'!$A:$A,MATCH($A1689,'Import data'!$A:$A,0),1)","v":{"$error":"#N/A"}}]
[0,{"$f":"INDEX('Import data'!$A:$A,MATCH($A1690,'Import data'!$A:$A,0),1)","v":{"$error":"#N/A"}}]
[0,{"$f":"INDEX('Import data'!$A:$A,MATCH($A1691,'Import data'!$A:$A,0),1)","v":{"$error":"#N/A"}}]
[0,{"$f":"INDEX('Import data'!$A:$A,MATCH($A1692,'Import data'!$A:$A,0),1)","v":{"$error":"#N/A"}}]
[0,{"$f":"INDEX('Import data'!$A:$A,MATCH($A1693,'Import data'!$A:$A,0),1)","v":{"$error":"#N/A"}}]
[0,{"$f":"INDEX('Import data'!$A:$A,MATCH($A1694,'Import data'!$A:$A,0),1)","v":{"$error":"#N/A"}}]
[0,{"$f":"INDEX('Import data'!$A:$A,MATCH($A1695,'Import data'!$A:$A,0),1)","v":{"$error":"#N/A"}}]
[0,{"$f":"INDEX('Import data'!$A:$A,MATCH($A1696,'Import data'!$A:$A,0),1)","v":{"$error":"#N/A"}}]
[0,{"$f":"INDEX('Import data'!$A:$A,MATCH($A1697,'Import data'!$A:$A,0),1)","v":{"$error":"#N/A"}}]
[0,{"$f":"INDEX('Import data'!$A:$A,MATCH($A1698,'Import data'!$A:$A,0),1)","v":{"$error":"#N/A"}}]
[0,{"$f":"INDEX('Import data'!$A:$A,MATCH($A1699,'Import data'!$A:$A,0),1)","v":{"$error":"#N/A"}}]
[0,{"$f":"INDEX('Import data'!$A:$A,MATCH($A1700,'Import data'!$A:$A,0),1)","v":{"$error":"#N/A"}}]
[0,{"$f":"INDEX('Import data'!$A:$A,MATCH($A1701,'Import data'!$A:$A,0),1)","v":{"$error":"#N/A"}}]
[0,{"$f":"INDEX('Import data'!$A:$A,MATCH($A1702,'Import data'!$A:$A,0),1)","v":{"$error":"#N/A"}}]
[0,{"$f":"INDEX('Import data'!$A:$A,MATCH($A1703,'Import data'!$A:$A,0),1)","v":{"$error":"#N/A"}}]
[0,{"$f":"INDEX('Import data'!$A:$A,MATCH($A1704,'Import data'!$A:$A,0),1)","v":{"$error":"#N/A"}}]
[0,{"$f":"INDEX('Import data'!$A:$A,MATCH($A1705,'Import data'!$A:$A,0),1)","v":{"$error":"#N/A"}}]
[0,{"$f":"INDEX('Import data'!$A:$A,MATCH($A1706,'Import data'!$A:$A,0),1)","v":{"$error":"#N/A"}}]
[0,{"$f":"INDEX('Import data'!$A:$A,MATCH($A1707,'Import data'!$A:$A,0),1)","v":{"$error":"#N/A"}}]
[0,{"$f":"INDEX('Import data'!$A:$A,MATCH($A1708,'Import data'!$A:$A,0),1)","v":{"$error":"#N/A"}}]
[0,{"$f":"INDEX('Import data'!$A:$A,MATCH($A1709,'Import data'!$A:$A,0),1)","v":{"$error":"#N/A"}}]
[0,{"$f":"INDEX('Import data'!$A:$A,MATCH($A1710,'Import data'!$A:$A,0),1)","v":{"$error":"#N/A"}}]
[0,{"$f":"INDEX('Import data'!$A:$A,MATCH($A1711,'Import data'!$A:$A,0),1)","v":{"$error":"#N/A"}}]
[0,{"$f":"INDEX('Import data'!$A:$A,MATCH($A1712,'Import data'!$A:$A,0),1)","v":{"$error":"#N/A"}}]
[0,{"$f":"INDEX('Import data'!$A:$A,MATCH($A1713,'Import data'!$A:$A,0),1)","v":{"$error":"#N/A"}}]
[0,{"$f":"INDEX('Import data'!$A:$A,MATCH($A1714,'Import data'!$A:$A,0),1)","v":{"$error":"#N/A"}}]
[0,{"$f":"INDEX('Import data'!$A:$A,MATCH($A1715,'Import data'!$A:$A,0),1)","v":{"$error":"#N/A"}}]
[0,{"$f":"INDEX('Import data'!$A:$A,MATCH($A1716,'Import data'!$A:$A,0),1)","v":{"$error":"#N/A"}}]
[0,{"$f":"INDEX('Import data'!$A:$A,MATCH($A1717,'Import data'!$A:$A,0),1)","v":{"$error":"#N/A"}}]
[0,{"$f":"INDEX('Import data'!$A:$A,MATCH($A1718,'Import data'!$A:$A,0),1)","v":{"$error":"#N/A"}}]
[0,{"$f":"INDEX('Import data'!$A:$A,MATCH($A1719,'Import data'!$A:$A,0),1)","v":{"$error":"#N/A"}}]
[0,{"$f":"INDEX('Import data'!$A:$A,MATCH($A1720,'Import data'!$A:$A,0),1)","v":{"$error":"#N/A"}}]
[0,{"$f":"INDEX('Import data'!$A:$A,MATCH($A1721,'Import data'!$A:$A,0),1)","v":{"$error":"#N/A"}}]
[0,{"$f":"INDEX('Import data'!$A:$A,MATCH($A1722,'Import data'!$A:$A,0),1)","v":{"$error":"#N/A"}}]
[0,{"$f":"INDEX('Import data'!$A:$A,MATCH($A1723,'Import data'!$A:$A,0),1)","v":{"$error":"#N/A"}}]
[0,{"$f":"INDEX('Import data'!$A:$A,MATCH($A1724,'Import data'!$A:$A,0),1)","v":{"$error":"#N/A"}}]
[0,{"$f":"INDEX('Import data'!$A:$A,MATCH($A1725,'Import data'!$A:$A,0),1)","v":{"$error":"#N/A"}}]
[0,{"$f":"INDEX('Import data'!$A:$A,MATCH($A1726,'Import data'!$A:$A,0),1)","v":{"$error":"#N/A"}}]
[0,{"$f":"INDEX('Import data'!$A:$A,MATCH($A1727,'Import data'!$A:$A,0),1)","v":{"$error":"#N/A"}}]
[0,{"$f":"INDEX('Import data'!$A:$A,MATCH($A1728,'Import data'!$A:$A,0),1)","v":{"$error":"#N/A"}}]
[0,{"$f":"INDEX('Import data'!$A:$A,MATCH($A1729,'Import data'!$A:$A,0),1)","v":{"$error":"#N/A"}}]
[0,{"$f":"INDEX('Import data'!$A:$A,MATCH($A1730,'Import data'!$A:$A,0),1)","v":{"$error":"#N/A"}}]
[{"$f":"ID","v":0},{"$f":"INDEX('Import data'!$A:$A,MATCH($A1731,'Import data'!$A:$A,0),1)","v":{"$error":"#N/A"}}]
[0,{"$f":"INDEX('Import data'!$A:$A,MATCH($A1732,'Import data'!$A:$A,0),1)","v":{"$error":"#N/A"}}]
[0,{"$f":"INDEX('Import data'!$A:$A,MATCH($A1733,'Import data'!$A:$A,0),1)","v":{"$error":"#N/A"}}]
[0,{"$f":"INDEX('Import data'!$A:$A,MATCH($A1734,'Import data'!$A:$A,0),1)","v":{"$error":"#N/A"}}]
[0,{"$f":"INDEX('Import data'!$A:$A,MATCH($A1735,'Import data'!$A:$A,0),1)","v":{"$error":"#N/A"}}]
[0,{"$f":"INDEX('Import data'!$A:$A,MATCH($A1736,'Import data'!$A:$A,0),1)","v":{"$error":"#N/A"}}]
[0,{"$f":"INDEX('Import data'!$A:$A,MATCH($A1737,'Import data'!$A:$A,0),1)","v":{"$error":"#N/A"}}]
[0,{"$f":"INDEX('Import data'!$A:$A,MATCH($A1738,'Import data'!$A:$A,0),1)","v":{"$error":"#N/A"}}]
[0,{"$f":"INDEX('Import data'!$A:$A,MATCH($A1739,'Import data'!$A:$A,0),1)","v":{"$error":"#N/A"}}]
[0,{"$f":"INDEX('Import data'!$A:$A,MATCH($A1740,'Import data'!$A:$A,0),1)","v":{"$error":"#N/A"}}]
[0,{"$f":"INDEX('Import data'!$A:$A,MATCH($A1741,'Import data'!$A:$A,0),1)","v":{"$error":"#N/A"}}]
[0,{"$f":"INDEX('Import data'!$A:$A,MATCH($A1742,'Import data'!$A:$A,0),1)","v":{"$error":"#N/A"}}]
[0,{"$f":"INDEX('Import data'!$A:$A,MATCH($A1743,'Import data'!$A:$A,0),1)","v":{"$error":"#N/A"}}]
[0,{"$f":"INDEX('Import data'!$A:$A,MATCH($A1744,'Import data'!$A:$A,0),1)","v":{"$error":"#N/A"}}]
[0,{"$f":"INDEX('Import data'!$A:$A,MATCH($A1745,'Import data'!$A:$A,0),1)","v":{"$error":"#N/A"}}]
[0,{"$f":"INDEX('Import data'!$A:$A,MATCH($A1746,'Import data'!$A:$A,0),1)","v":{"$error":"#N/A"}}]
[0,{"$f":"INDEX('Import data'!$A:$A,MATCH($A1747,'Import data'!$A:$A,0),1)","v":{"$error":"#N/A"}}]
[0,{"$f":"INDEX('Import data'!$A:$A,MATCH($A1748,'Import data'!$A:$A,0),1)","v":{"$error":"#N/A"}}]
[0,{"$f":"INDEX('Import data'!$A:$A,MATCH($A1749,'Import data'!$A:$A,0),1)","v":{"$error":"#N/A"}}]
[0,{"$f":"INDEX('Import data'!$A:$A,MATCH($A1750,'Import data'!$A:$A,0),1)","v":{"$error":"#N/A"}}]
[0,{"$f":"INDEX('Import data'!$A:$A,MATCH($A1751,'Import data'!$A:$A,0),1)","v":{"$error":"#N/A"}}]
[0,{"$f":"INDEX('Import data'!$A:$A,MATCH($A1752,'Import data'!$A:$A,0),1)","v":{"$error":"#N/A"}}]
[0,{"$f":"INDEX('Import data'!$A:$A,MATCH($A1753,'Import data'!$A:$A,0),1)","v":{"$error":"#N/A"}}]
[0,{"$f":"INDEX('Import data'!$A:$A,MATCH($A1754,'Import data'!$A:$A,0),1)","v":{"$error":"#N/A"}}]
[0,{"$f":"INDEX('Import data'!$A:$A,MATCH($A1755,'Import data'!$A:$A,0),1)","v":{"$error":"#N/A"}}]
[0,{"$f":"INDEX('Import data'!$A:$A,MATCH($A1756,'Import data'!$A:$A,0),1)","v":{"$error":"#N/A"}}]
[0,{"$f":"INDEX('Import data'!$A:$A,MATCH($A1757,'Import data'!$A:$A,0),1)","v":{"$error":"#N/A"}}]
[0,{"$f":"INDEX('Import data'!$A:$A,MATCH($A1758,'Import data'!$A:$A,0),1)","v":{"$error":"#N/A"}}]
[0,{"$f":"INDEX('Import data'!$A:$A,MATCH($A1759,'Import data'!$A:$A,0),1)","v":{"$error":"#N/A"}}]
[0,{"$f":"INDEX('Import data'!$A:$A,MATCH($A1760,'Import data'!$A:$A,0),1)","v":{"$error":"#N/A"}}]
[0,{"$f":"INDEX('Import data'!$A:$A,MATCH($A1761,'Import data'!$A:$A,0),1)","v":{"$error":"#N/A"}}]
[0,{"$f":"INDEX('Import data'!$A:$A,MATCH($A1762,'Import data'!$A:$A,0),1)","v":{"$error":"#N/A"}}]
[0,{"$f":"INDEX('Import data'!$A:$A,MATCH($A1763,'Import data'!$A:$A,0),1)","v":{"$error":"#N/A"}}]
[0,{"$f":"INDEX('Import data'!$A:$A,MATCH($A1764,'Import data'!$A:$A,0),1)","v":{"$error":"#N/A"}}]
[0,{"$f":"INDEX('Import data'!$A:$A,MATCH($A1765,'Import data'!$A:$A,0),1)","v":{"$error":"#N/A"}}]
[0,{"$f":"INDEX('Import data'!$A:$A,MATCH($A1766,'Import data'!$A:$A,0),1)","v":{"$error":"#N/A"}}]
[0,{"$f":"INDEX('Import data'!$A:$A,MATCH($A1767,'Import data'!$A:$A,0),1)","v":{"$error":"#N/A"}}]
[0,{"$f":"INDEX('Import data'!$A:$A,MATCH($A1768,'Import data'!$A:$A,0),1)","v":{"$error":"#N/A"}}]
[0,{"$f":"INDEX('Import data'!$A:$A,MATCH($A1769,'Import data'!$A:$A,0),1)","v":{"$error":"#N/A"}}]
[0,{"$f":"INDEX('Import data'!$A:$A,MATCH($A1770,'Import data'!$A:$A,0),1)","v":{"$error":"#N/A"}}]
[0,{"$f":"INDEX('Import data'!$A:$A,MATCH($A1771,'Import data'!$A:$A,0),1)","v":{"$error":"#N/A"}}]
[0,{"$f":"INDEX('Import data'!$A:$A,MATCH($A1772,'Import data'!$A:$A,0),1)","v":{"$error":"#N/A"}}]
[0,{"$f":"INDEX('Import data'!$A:$A,MATCH($A1773,'Import data'!$A:$A,0),1)","v":{"$error":"#N/A"}}]
[0,{"$f":"INDEX('Import data'!$A:$A,MATCH($A1774,'Import data'!$A:$A,0),1)","v":{"$error":"#N/A"}}]
[0,{"$f":"INDEX('Import data'!$A:$A,MATCH($A1775,'Import data'!$A:$A,0),1)","v":{"$error":"#N/A"}}]
[0,{"$f":"INDEX('Import data'!$A:$A,MATCH($A1776,'Import data'!$A:$A,0),1)","v":{"$error":"#N/A"}}]
[0,{"$f":"INDEX('Import data'!$A:$A,MATCH($A1777,'Import data'!$A:$A,0),1)","v":{"$error":"#N/A"}}]
[0,{"$f":"INDEX('Import data'!$A:$A,MATCH($A1778,'Import data'!$A:$A,0),1)","v":{"$error":"#N/A"}}]
[0,{"$f":"INDEX('Import data'!$A:$A,MATCH($A1779,'Import data'!$A:$A,0),1)","v":{"$error":"#N/A"}}]
[0,{"$f":"INDEX('Import data'!$A:$A,MATCH($A1780,'Import data'!$A:$A,0),1)","v":{"$error":"#N/A"}}]
[0,{"$f":"INDEX('Import data'!$A:$A,MATCH($A1781,'Import data'!$A:$A,0),1)","v":{"$error":"#N/A"}}]
[0,{"$f":"INDEX('Import data'!$A:$A,MATCH($A1782,'Import data'!$A:$A,0),1)","v":{"$error":"#N/A"}}]
[0,{"$f":"INDEX('Import data'!$A:$A,MATCH($A1783,'Import data'!$A:$A,0),1)","v":{"$error":"#N/A"}}]
[0,{"$f":"INDEX('Import data'!$A:$A,MATCH($A1784,'Import data'!$A:$A,0),1)","v":{"$error":"#N/A"}}]
[0,{"$f":"INDEX('Import data'!$A:$A,MATCH($A1785,'Import data'!$A:$A,0),1)","v":{"$error":"#N/A"}}]
[0,{"$f":"INDEX('Import data'!$A:$A,MATCH($A1786,'Import data'!$A:$A,0),1)","v":{"$error":"#N/A"}}]
[0,{"$f":"INDEX('Import data'!$A:$A,MATCH($A1787,'Import data'!$A:$A,0),1)","v":{"$error":"#N/A"}}]
[0,{"$f":"INDEX('Import data'!$A:$A,MATCH($A1788,'Import data'!$A:$A,0),1)","v":{"$error":"#N/A"}}]
[0,{"$f":"INDEX('Import data'!$A:$A,MATCH($A1789,'Import data'!$A:$A,0),1)","v":{"$error":"#N/A"}}]
[0,{"$f":"INDEX('Import data'!$A:$A,MATCH($A1790,'Import data'!$A:$A,0),1)","v":{"$error":"#N/A"}}]
[0,{"$f":"INDEX('Import data'!$A:$A,MATCH($A1791,'Import data'!$A:$A,0),1)","v":{"$error":"#N/A"}}]
[0,{"$f":"INDEX('Import data'!$A:$A,MATCH($A1792,'Import data'!$A:$A,0),1)","v":{"$error":"#N/A"}}]
[0,{"$f":"INDEX('Import data'!$A:$A,MATCH($A1793,'Import data'!$A:$A,0),1)","v":{"$error":"#N/A"}}]
[0,{"$f":"INDEX('Import data'!$A:$A,MATCH($A1794,'Import data'!$A:$A,0),1)","v":{"$error":"#N/A"}}]
[{"$f":"ID","v":0},{"$f":"INDEX('Import data'!$A:$A,MATCH($A1795,'Import data'!$A:$A,0),1)","v":{"$error":"#N/A"}}]
[0,{"$f":"INDEX('Import data'!$A:$A,MATCH($A1796,'Import data'!$A:$A,0),1)","v":{"$error":"#N/A"}}]
[0,{"$f":"INDEX('Import data'!$A:$A,MATCH($A1797,'Import data'!$A:$A,0),1)","v":{"$error":"#N/A"}}]
[0,{"$f":"INDEX('Import data'!$A:$A,MATCH($A1798,'Import data'!$A:$A,0),1)","v":{"$error":"#N/A"}}]
[0,{"$f":"INDEX('Import data'!$A:$A,MATCH($A1799,'Import data'!$A:$A,0),1)","v":{"$error":"#N/A"}}]
[0,{"$f":"INDEX('Import data'!$A:$A,MATCH($A1800,'Import data'!$A:$A,0),1)","v":{"$error":"#N/A"}}]
[0,{"$f":"INDEX('Import data'!$A:$A,MATCH($A1801,'Import data'!$A:$A,0),1)","v":{"$error":"#N/A"}}]
[0,{"$f":"INDEX('Import data'!$A:$A,MATCH($A1802,'Import data'!$A:$A,0),1)","v":{"$error":"#N/A"}}]
[0,{"$f":"INDEX('Import data'!$A:$A,MATCH($A1803,'Import data'!$A:$A,0),1)","v":{"$error":"#N/A"}}]
[0,{"$f":"INDEX('Import data'!$A:$A,MATCH($A1804,'Import data'!$A:$A,0),1)","v":{"$error":"#N/A"}}]
[0,{"$f":"INDEX('Import data'!$A:$A,MATCH($A1805,'Import data'!$A:$A,0),1)","v":{"$error":"#N/A"}}]
[0,{"$f":"INDEX('Import data'!$A:$A,MATCH($A1806,'Import data'!$A:$A,0),1)","v":{"$error":"#N/A"}}]
[0,{"$f":"INDEX('Import data'!$A:$A,MATCH($A1807,'Import data'!$A:$A,0),1)","v":{"$error":"#N/A"}}]
[0,{"$f":"INDEX('Import data'!$A:$A,MATCH($A1808,'Import data'!$A:$A,0),1)","v":{"$error":"#N/A"}}]
[0,{"$f":"INDEX('Import data'!$A:$A,MATCH($A1809,'Import data'!$A:$A,0),1)","v":{"$error":"#N/A"}}]
[0,{"$f":"INDEX('Import data'!$A:$A,MATCH($A1810,'Import data'!$A:$A,0),1)","v":{"$error":"#N/A"}}]
[0,{"$f":"INDEX('Import data'!$A:$A,MATCH($A1811,'Import data'!$A:$A,0),1)","v":{"$error":"#N/A"}}]
[0,{"$f":"INDEX('Import data'!$A:$A,MATCH($A1812,'Import data'!$A:$A,0),1)","v":{"$error":"#N/A"}}]
[0,{"$f":"INDEX('Import data'!$A:$A,MATCH($A1813,'Import data'!$A:$A,0),1)","v":{"$error":"#N/A"}}]
[0,{"$f":"INDEX('Import data'!$A:$A,MATCH($A1814,'Import data'!$A:$A,0),1)","v":{"$error":"#N/A"}}]
[0,{"$f":"INDEX('Import data'!$A:$A,MATCH($A1815,'Import data'!$A:$A,0),1)","v":{"$error":"#N/A"}}]
[0,{"$f":"INDEX('Import data'!$A:$A,MATCH($A1816,'Import data'!$A:$A,0),1)","v":{"$error":"#N/A"}}]
[0,{"$f":"INDEX('Import data'!$A:$A,MATCH($A1817,'Import data'!$A:$A,0),1)","v":{"$error":"#N/A"}}]
[0,{"$f":"INDEX('Import data'!$A:$A,MATCH($A1818,'Import data'!$A:$A,0),1)","v":{"$error":"#N/A"}}]
[0,{"$f":"INDEX('Import data'!$A:$A,MATCH($A1819,'Import data'!$A:$A,0),1)","v":{"$error":"#N/A"}}]
[0,{"$f":"INDEX('Import data'!$A:$A,MATCH($A1820,'Import data'!$A:$A,0),1)","v":{"$error":"#N/A"}}]
[0,{"$f":"INDEX('Import data'!$A:$A,MATCH($A1821,'Import data'!$A:$A,0),1)","v":{"$error":"#N/A"}}]
[0,{"$f":"INDEX('Import data'!$A:$A,MATCH($A1822,'Import data'!$A:$A,0),1)","v":{"$error":"#N/A"}}]
[0,{"$f":"INDEX('Import data'!$A:$A,MATCH($A1823,'Import data'!$A:$A,0),1)","v":{"$error":"#N/A"}}]
[0,{"$f":"INDEX('Import data'!$A:$A,MATCH($A1824,'Import data'!$A:$A,0),1)","v":{"$error":"#N/A"}}]
[0,{"$f":"INDEX('Import data'!$A:$A,MATCH($A1825,'Import data'!$A:$A,0),1)","v":{"$error":"#N/A"}}]
[0,{"$f":"INDEX('Import data'!$A:$A,MATCH($A1826,'Import data'!$A:$A,0),1)","v":{"$error":"#N/A"}}]
[0,{"$f":"INDEX('Import data'!$A:$A,MATCH($A1827,'Import data'!$A:$A,0),1)","v":{"$error":"#N/A"}}]
[0,{"$f":"INDEX('Import data'!$A:$A,MATCH($A1828,'Import data'!$A:$A,0),1)","v":{"$error":"#N/A"}}]
[0,{"$f":"INDEX('Import data'!$A:$A,MATCH($A1829,'Import data'!$A:$A,0),1)","v":{"$error":"#N/A"}}]
[0,{"$f":"INDEX('Import data'!$A:$A,MATCH($A1830,'Import data'!$A:$A,0),1)","v":{"$error":"#N/A"}}]
[0,{"$f":"INDEX('Import data'!$A:$A,MATCH($A1831,'Import data'!$A:$A,0),1)","v":{"$error":"#N/A"}}]
[0,{"$f":"INDEX('Import data'!$A:$A,MATCH($A1832,'Import data'!$A:$A,0),1)","v":{"$error":"#N/A"}}]
[0,{"$f":"INDEX('Import data'!$A:$A,MATCH($A1833,'Import data'!$A:$A,0),1)","v":{"$error":"#N/A"}}]
[0,{"$f":"INDEX('Import data'!$A:$A,MATCH($A1834,'Import data'!$A:$A,0),1)","v":{"$error":"#N/A"}}]
[0,{"$f":"INDEX('Import data'!$A:$A,MATCH($A1835,'Import data'!$A:$A,0),1)","v":{"$error":"#N/A"}}]
[0,{"$f":"INDEX('Import data'!$A:$A,MATCH($A1836,'Import data'!$A:$A,0),1)","v":{"$error":"#N/A"}}]
[0,{"$f":"INDEX('Import data'!$A:$A,MATCH($A1837,'Import data'!$A:$A,0),1)","v":{"$error":"#N/A"}}]
[0,{"$f":"INDEX('Import data'!$A:$A,MATCH($A1838,'Import data'!$A:$A,0),1)","v":{"$error":"#N/A"}}]
[0,{"$f":"INDEX('Import data'!$A:$A,MATCH($A1839,'Import data'!$A:$A,0),1)","v":{"$error":"#N/A"}}]
[0,{"$f":"INDEX('Import data'!$A:$A,MATCH($A1840,'Import data'!$A:$A,0),1)","v":{"$error":"#N/A"}}]
[0,{"$f":"INDEX('Import data'!$A:$A,MATCH($A1841,'Import data'!$A:$A,0),1)","v":{"$error":"#N/A"}}]
[0,{"$f":"INDEX('Import data'!$A:$A,MATCH($A1842,'Import data'!$A:$A,0),1)","v":{"$error":"#N/A"}}]
[0,{"$f":"INDEX('Import data'!$A:$A,MATCH($A1843,'Import data'!$A:$A,0),1)","v":{"$error":"#N/A"}}]
[0,{"$f":"INDEX('Import data'!$A:$A,MATCH($A1844,'Import data'!$A:$A,0),1)","v":{"$error":"#N/A"}}]
[0,{"$f":"INDEX('Import data'!$A:$A,MATCH($A1845,'Import data'!$A:$A,0),1)","v":{"$error":"#N/A"}}]
[0,{"$f":"INDEX('Import data'!$A:$A,MATCH($A1846,'Import data'!$A:$A,0),1)","v":{"$error":"#N/A"}}]
[0,{"$f":"INDEX('Import data'!$A:$A,MATCH($A1847,'Import data'!$A:$A,0),1)","v":{"$error":"#N/A"}}]
[0,{"$f":"INDEX('Import data'!$A:$A,MATCH($A1848,'Import data'!$A:$A,0),1)","v":{"$error":"#N/A"}}]
[0,{"$f":"INDEX('Import data'!$A:$A,MATCH($A1849,'Import data'!$A:$A,0),1)","v":{"$error":"#N/A"}}]
[0,{"$f":"INDEX('Import data'!$A:$A,MATCH($A1850,'Import data'!$A:$A,0),1)","v":{"$error":"#N/A"}}]
[0,{"$f":"INDEX('Import data'!$A:$A,MATCH($A1851,'Import data'!$A:$A,0),1)","v":{"$error":"#N/A"}}]
[0,{"$f":"INDEX('Import data'!$A:$A,MATCH($A1852,'Import data'!$A:$A,0),1)","v":{"$error":"#N/A"}}]
[0,{"$f":"INDEX('Import data'!$A:$A,MATCH($A1853,'Import data'!$A:$A,0),1)","v":{"$error":"#N/A"}}]
[0,{"$f":"INDEX('Import data'!$A:$A,MATCH($A1854,'Import data'!$A:$A,0),1)","v":{"$error":"#N/A"}}]
[0,{"$f":"INDEX('Import data'!$A:$A,MATCH($A1855,'Import data'!$A:$A,0),1)","v":{"$error":"#N/A"}}]
[0,{"$f":"INDEX('Import data'!$A:$A,MATCH($A1856,'Import data'!$A:$A,0),1)","v":{"$error":"#N/A"}}]
[0,{"$f":"INDEX('Import data'!$A:$A,MATCH($A1857,'Import data'!$A:$A,0),1)","v":{"$error":"#N/A"}}]
[0,{"$f":"INDEX('Import data'!$A:$A,MATCH($A1858,'Import data'!$A:$A,0),1)","v":{"$error":"#N/A"}}]
[{"$f":"ID","v":0},{"$f":"INDEX('Import data'!$A:$A,MATCH($A1859,'Import data'!$A:$A,0),1)","v":{"$error":"#N/A"}}]
[0,{"$f":"INDEX('Import data'!$A:$A,MATCH($A1860,'Import data'!$A:$A,0),1)","v":{"$error":"#N/A"}}]
[0,{"$f":"INDEX('Import data'!$A:$A,MATCH($A1861,'Import data'!$A:$A,0),1)","v":{"$error":"#N/A"}}]
[0,{"$f":"INDEX('Import data'!$A:$A,MATCH($A1862,'Import data'!$A:$A,0),1)","v":{"$error":"#N/A"}}]
[0,{"$f":"INDEX('Import data'!$A:$A,MATCH($A1863,'Import data'!$A:$A,0),1)","v":{"$error":"#N/A"}}]
[0,{"$f":"INDEX('Import data'!$A:$A,MATCH($A1864,'Import data'!$A:$A,0),1)","v":{"$error":"#N/A"}}]
[0,{"$f":"INDEX('Import data'!$A:$A,MATCH($A1865,'Import data'!$A:$A,0),1)","v":{"$error":"#N/A"}}]
[0,{"$f":"INDEX('Import data'!$A:$A,MATCH($A1866,'Import data'!$A:$A,0),1)","v":{"$error":"#N/A"}}]
[0,{"$f":"INDEX('Import data'!$A:$A,MATCH($A1867,'Import data'!$A:$A,0),1)","v":{"$error":"#N/A"}}]
[0,{"$f":"INDEX('Import data'!$A:$A,MATCH($A1868,'Import data'!$A:$A,0),1)","v":{"$error":"#N/A"}}]
[0,{"$f":"INDEX('Import data'!$A:$A,MATCH($A1869,'Import data'!$A:$A,0),1)","v":{"$error":"#N/A"}}]
[0,{"$f":"INDEX('Import data'!$A:$A,MATCH($A1870,'Import data'!$A:$A,0),1)","v":{"$error":"#N/A"}}]
[0,{"$f":"INDEX('Import data'!$A:$A,MATCH($A1871,'Import data'!$A:$A,0),1)","v":{"$error":"#N/A"}}]
[0,{"$f":"INDEX('Import data'!$A:$A,MATCH($A1872,'Import data'!$A:$A,0),1)","v":{"$error":"#N/A"}}]
[0,{"$f":"INDEX('Import data'!$A:$A,MATCH($A1873,'Import data'!$A:$A,0),1)","v":{"$error":"#N/A"}}]
[0,{"$f":"INDEX('Import data'!$A:$A,MATCH($A1874,'Import data'!$A:$A,0),1)","v":{"$error":"#N/A"}}]
[0,{"$f":"INDEX('Import data'!$A:$A,MATCH($A1875,'Import data'!$A:$A,0),1)","v":{"$error":"#N/A"}}]
[0,{"$f":"INDEX('Import data'!$A:$A,MATCH($A1876,'Import data'!$A:$A,0),1)","v":{"$error":"#N/A"}}]
[0,{"$f":"INDEX('Import data'!$A:$A,MATCH($A1877,'Import data'!$A:$A,0),1)","v":{"$error":"#N/A"}}]
[0,{"$f":"INDEX('Import data'!$A:$A,MATCH($A1878,'Import data'!$A:$A,0),1)","v":{"$error":"#N/A"}}]
[0,{"$f":"INDEX('Import data'!$A:$A,MATCH($A1879,'Import data'!$A:$A,0),1)","v":{"$error":"#N/A"}}]
[0,{"$f":"INDEX('Import data'!$A:$A,MATCH($A1880,'Import data'!$A:$A,0),1)","v":{"$error":"#N/A"}}]
[0,{"$f":"INDEX('Import data'!$A:$A,MATCH($A1881,'Import data'!$A:$A,0),1)","v":{"$error":"#N/A"}}]
[0,{"$f":"INDEX('Import data'!$A:$A,MATCH($A1882,'Import data'!$A:$A,0),1)","v":{"$error":"#N/A"}}]
[0,{"$f":"INDEX('Import data'!$A:$A,MATCH($A1883,'Import data'!$A:$A,0),1)","v":{"$error":"#N/A"}}]
[0,{"$f":"INDEX('Import data'!$A:$A,MATCH($A1884,'Import data'!$A:$A,0),1)","v":{"$error":"#N/A"}}]
[0,{"$f":"INDEX('Import data'!$A:$A,MATCH($A1885,'Import data'!$A:$A,0),1)","v":{"$error":"#N/A"}}]
[0,{"$f":"INDEX('Import data'!$A:$A,MATCH($A1886,'Import data'!$A:$A,0),1)","v":{"$error":"#N/A"}}]
[0,{"$f":"INDEX('Import data'!$A:$A,MATCH($A1887,'Import data'!$A:$A,0),1)","v":{"$error":"#N/A"}}]
[0,{"$f":"INDEX('Import data'!$A:$A,MATCH($A1888,'Import data'!$A:$A,0),1)","v":{"$error":"#N/A"}}]
[0,{"$f":"INDEX('Import data'!$A:$A,MATCH($A1889,'Import data'!$A:$A,0),1)","v":{"$error":"#N/A"}}]
[0,{"$f":"INDEX('Import data'!$A:$A,MATCH($A1890,'Import data'!$A:$A,0),1)","v":{"$error":"#N/A"}}]
[0,{"$f":"INDEX('Import data'!$A:$A,MATCH($A1891,'Import data'!$A:$A,0),1)","v":{"$error":"#N/A"}}]
[0,{"$f":"INDEX('Import data'!$A:$A,MATCH($A1892,'Import data'!$A:$A,0),1)","v":{"$error":"#N/A"}}]
[0,{"$f":"INDEX('Import data'!$A:$A,MATCH($A1893,'Import data'!$A:$A,0),1)","v":{"$error":"#N/A"}}]
[0,{"$f":"INDEX('Import data'!$A:$A,MATCH($A1894,'Import data'!$A:$A,0),1)","v":{"$error":"#N/A"}}]
[0,{"$f":"INDEX('Import data'!$A:$A,MATCH($A1895,'Import data'!$A:$A,0),1)","v":{"$error":"#N/A"}}]
[0,{"$f":"INDEX('Import data'!$A:$A,MATCH($A1896,'Import data'!$A:$A,0),1)","v":{"$error":"#N/A"}}]
[0,{"$f":"INDEX('Import data'!$A:$A,MATCH($A1897,'Import data'!$A:$A,0),1)","v":{"$error":"#N/A"}}]
[0,{"$f":"INDEX('Import data'!$A:$A,MATCH($A1898,'Import data'!$A:$A,0),1)","v":{"$error":"#N/A"}}]
[0,{"$f":"INDEX('Import data'!$A:$A,MATCH($A1899,'Import data'!$A:$A,0),1)","v":{"$error":"#N/A"}}]
[0,{"$f":"INDEX('Import data'!$A:$A,MATCH($A1900,'Import data'!$A:$A,0),1)","v":{"$error":"#N/A"}}]
[0,{"$f":"INDEX('Import data'!$A:$A,MATCH($A1901,'Import data'!$A:$A,0),1)","v":{"$error":"#N/A"}}]
[0,{"$f":"INDEX('Import data'!$A:$A,MATCH($A1902,'Import data'!$A:$A,0),1)","v":{"$error":"#N/A"}}]
[0,{"$f":"INDEX('Import data'!$A:$A,MATCH($A1903,'Import data'!$A:$A,0),1)","v":{"$error":"#N/A"}}]
[0,{"$f":"INDEX('Import data'!$A:$A,MATCH($A1904,'Import data'!$A:$A,0),1)","v":{"$error":"#N/A"}}]
[0,{"$f":"INDEX('Import data'!$A:$A,MATCH($A1905,'Import data'!$A:$A,0),1)","v":{"$error":"#N/A"}}]
[0,{"$f":"INDEX('Import data'!$A:$A,MATCH($A1906,'Import data'!$A:$A,0),1)","v":{"$error":"#N/A"}}]
[0,{"$f":"INDEX('Import data'!$A:$A,MATCH($A1907,'Import data'!$A:$A,0),1)","v":{"$error":"#N/A"}}]
[0,{"$f":"INDEX('Import data'!$A:$A,MATCH($A1908,'Import data'!$A:$A,0),1)","v":{"$error":"#N/A"}}]
[0,{"$f":"INDEX('Import data'!$A:$A,MATCH($A1909,'Import data'!$A:$A,0),1)","v":{"$error":"#N/A"}}]
[0,{"$f":"INDEX('Import data'!$A:$A,MATCH($A1910,'Import data'!$A:$A,0),1)","v":{"$error":"#N/A"}}]
[0,{"$f":"INDEX('Import data'!$A:$A,MATCH($A1911,'Import data'!$A:$A,0),1)","v":{"$error":"#N/A"}}]
[0,{"$f":"INDEX('Import data'!$A:$A,MATCH($A1912,'Import data'!$A:$A,0),1)","v":{"$error":"#N/A"}}]
[0,{"$f":"INDEX('Import data'!$A:$A,MATCH($A1913,'Import data'!$A:$A,0),1)","v":{"$error":"#N/A"}}]
[0,{"$f":"INDEX('Import data'!$A:$A,MATCH($A1914,'Import data'!$A:$A,0),1)","v":{"$error":"#N/A"}}]
[0,{"$f":"INDEX('Import data'!$A:$A,MATCH($A1915,'Import data'!$A:$A,0),1)","v":{"$error":"#N/A"}}]
[0,{"$f":"INDEX('Import data'!$A:$A,MATCH($A1916,'Import data'!$A:$A,0),1)","v":{"$error":"#N/A"}}]
[0,{"$f":"INDEX('Import data'!$A:$A,MATCH($A1917,'Import data'!$A:$A,0),1)","v":{"$error":"#N/A"}}]
[0,{"$f":"INDEX('Import data'!$A:$A,MATCH($A1918,'Import data'!$A:$A,0),1)","v":{"$error":"#N/A"}}]
[0,{"$f":"INDEX('Import data'!$A:$A,MATCH($A1919,'Import data'!$A:$A,0),1)","v":{"$error":"#N/A"}}]
[0,{"$f":"INDEX('Import data'!$A:$A,MATCH($A1920,'Import data'!$A:$A,0),1)","v":{"$error":"#N/A"}}]
[0,{"$f":"INDEX('Import data'!$A:$A,MATCH($A1921,'Import data'!$A:$A,0),1)","v":{"$error":"#N/A"}}]
[0,{"$f":"INDEX('Import data'!$A:$A,MATCH($A1922,'Import data'!$A:$A,0),1)","v":{"$error":"#N/A"}}]
[{"$f":"ID","v":0},{"$f":"INDEX('Import data'!$A:$A,MATCH($A1923,'Import data'!$A:$A,0),1)","v":{"$error":"#N/A"}}]
[0,{"$f":"INDEX('Import data'!$A:$A,MATCH($A1924,'Import data'!$A:$A,0),1)","v":{"$error":"#N/A"}}]
[0,{"$f":"INDEX('Import data'!$A:$A,MATCH($A1925,'Import data'!$A:$A,0),1)","v":{"$error":"#N/A"}}]
[0,{"$f":"INDEX('Import data'!$A:$A,MATCH($A1926,'Import data'!$A:$A,0),1)","v":{"$error":"#N/A"}}]
[0,{"$f":"INDEX('Import data'!$A:$A,MATCH($A1927,'Import data'!$A:$A,0),1)","v":{"$error":"#N/A"}}]
[0,{"$f":"INDEX('Import data'!$A:$A,MATCH($A1928,'Import data'!$A:$A,0),1)","v":{"$error":"#N/A"}}]
[0,{"$f":"INDEX('Import data'!$A:$A,MATCH($A1929,'Import data'!$A:$A,0),1)","v":{"$error":"#N/A"}}]
[0,{"$f":"INDEX('Import data'!$A:$A,MATCH($A1930,'Import data'!$A:$A,0),1)","v":{"$error":"#N/A"}}]
[0,{"$f":"INDEX('Import data'!$A:$A,MATCH($A1931,'Import data'!$A:$A,0),1)","v":{"$error":"#N/A"}}]
[0,{"$f":"INDEX('Import data'!$A:$A,MATCH($A1932,'Import data'!$A:$A,0),1)","v":{"$error":"#N/A"}}]
[0,{"$f":"INDEX('Import data'!$A:$A,MATCH($A1933,'Import data'!$A:$A,0),1)","v":{"$error":"#N/A"}}]
[0,{"$f":"INDEX('Import data'!$A:$A,MATCH($A1934,'Import data'!$A:$A,0),1)","v":{"$error":"#N/A"}}]
[0,{"$f":"INDEX('Import data'!$A:$A,MATCH($A1935,'Import data'!$A:$A,0),1)","v":{"$error":"#N/A"}}]
[0,{"$f":"INDEX('Import data'!$A:$A,MATCH($A1936,'Import data'!$A:$A,0),1)","v":{"$error":"#N/A"}}]
[0,{"$f":"INDEX('Import data'!$A:$A,MATCH($A1937,'Import data'!$A:$A,0),1)","v":{"$error":"#N/A"}}]
[0,{"$f":"INDEX('Import data'!$A:$A,MATCH($A1938,'Import data'!$A:$A,0),1)","v":{"$error":"#N/A"}}]
[0,{"$f":"INDEX('Import data'!$A:$A,MATCH($A1939,'Import data'!$A:$A,0),1)","v":{"$error":"#N/A"}}]
[0,{"$f":"INDEX('Import data'!$A:$A,MATCH($A1940,'Import data'!$A:$A,0),1)","v":{"$error":"#N/A"}}]
[0,{"$f":"INDEX('Import data'!$A:$A,MATCH($A1941,'Import data'!$A:$A,0),1)","v":{"$error":"#N/A"}}]
[0,{"$f":"INDEX('Import data'!$A:$A,MATCH($A1942,'Import data'!$A:$A,0),1)","v":{"$error":"#N/A"}}]
[0,{"$f":"INDEX('Import data'!$A:$A,MATCH($A1943,'Import data'!$A:$A,0),1)","v":{"$error":"#N/A"}}]
[0,{"$f":"INDEX('Import data'!$A:$A,MATCH($A1944,'Import data'!$A:$A,0),1)","v":{"$error":"#N/A"}}]
[0,{"$f":"INDEX('Import data'!$A:$A,MATCH($A1945,'Import data'!$A:$A,0),1)","v":{"$error":"#N/A"}}]
[0,{"$f":"INDEX('Import data'!$A:$A,MATCH($A1946,'Import data'!$A:$A,0),1)","v":{"$error":"#N/A"}}]
[0,{"$f":"INDEX('Import data'!$A:$A,MATCH($A1947,'Import data'!$A:$A,0),1)","v":{"$error":"#N/A"}}]
[0,{"$f":"INDEX('Import data'!$A:$A,MATCH($A1948,'Import data'!$A:$A,0),1)","v":{"$error":"#N/A"}}]
[0,{"$f":"INDEX('Import data'!$A:$A,MATCH($A1949,'Import data'!$A:$A,0),1)","v":{"$error":"#N/A"}}]
[0,{"$f":"INDEX('Import data'!$A:$A,MATCH($A1950,'Import data'!$A:$A,0),1)","v":{"$error":"#N/A"}}]
[0,{"$f":"INDEX('Import data'!$A:$A,MATCH($A1951,'Import data'!$A:$A,0),1)","v":{"$error":"#N/A"}}]
[0,{"$f":"INDEX('Import data'!$A:$A,MATCH($A1952,'Import data'!$A:$A,0),1)","v":{"$error":"#N/A"}}]
[0,{"$f":"INDEX('Import data'!$A:$A,MATCH($A1953,'Import data'!$A:$A,0),1)","v":{"$error":"#N/A"}}]
[0,{"$f":"INDEX('Import data'!$A:$A,MATCH($A1954,'Import data'!$A:$A,0),1)","v":{"$error":"#N/A"}}]
[0,{"$f":"INDEX('Import data'!$A:$A,MATCH($A1955,'Import data'!$A:$A,0),1)","v":{"$error":"#N/A"}}]
[0,{"$f":"INDEX('Import data'!$A:$A,MATCH($A1956,'Import data'!$A:$A,0),1)","v":{"$error":"#N/A"}}]
[0,{"$f":"INDEX('Import data'!$A:$A,MATCH($A1957,'Import data'!$A:$A,0),1)","v":{"$error":"#N/A"}}]
[0,{"$f":"INDEX('Import data'!$A:$A,MATCH($A1958,'Import data'!$A:$A,0),1)","v":{"$error":"#N/A"}}]
[0,{"$f":"INDEX('Import data'!$A:$A,MATCH($A1959,'Import data'!$A:$A,0),1)","v":{"$error":"#N/A"}}]
[0,{"$f":"INDEX('Import data'!$A:$A,MATCH($A1960,'Import data'!$A:$A,0),1)","v":{"$error":"#N/A"}}]
[0,{"$f":"INDEX('Import data'!$A:$A,MATCH($A1961,'Import data'!$A:$A,0),1)","v":{"$error":"#N/A"}}]
[0,{"$f":"INDEX('Import data'!$A:$A,MATCH($A1962,'Import data'!$A:$A,0),1)","v":{"$error":"#N/A"}}]
[0,{"$f":"INDEX('Import data'!$A:$A,MATCH($A1963,'Import data'!$A:$A,0),1)","v":{"$error":"#N/A"}}]
[0,{"$f":"INDEX('Import data'!$A:$A,MATCH($A1964,'Import data'!$A:$A,0),1)","v":{"$error":"#N/A"}}]
[0,{"$f":"INDEX('Import data'!$A:$A,MATCH($A1965,'Import data'!$A:$A,0),1)","v":{"$error":"#N/A"}}]
[0,{"$f":"INDEX('Import data'!$A:$A,MATCH($A1966,'Import data'!$A:$A,0),1)","v":{"$error":"#N/A"}}]
[0,{"$f":"INDEX('Import data'!$A:$A,MATCH($A1967,'Import data'!$A:$A,0),1)","v":{"$error":"#N/A"}}]
[0,{"$f":"INDEX('Import data'!$A:$A,MATCH($A1968,'Import data'!$A:$A,0),1)","v":{"$error":"#N/A"}}]
[0,{"$f":"INDEX('Import data'!$A:$A,MATCH($A1969,'Import data'!$A:$A,0),1)","v":{"$error":"#N/A"}}]
[0,{"$f":"INDEX('Import data'!$A:$A,MATCH($A1970,'Import data'!$A:$A,0),1)","v":{"$error":"#N/A"}}]
[0,{"$f":"INDEX('Import data'!$A:$A,MATCH($A1971,'Import data'!$A:$A,0),1)","v":{"$error":"#N/A"}}]
[0,{"$f":"INDEX('Import data'!$A:$A,MATCH($A1972,'Import data'!$A:$A,0),1)","v":{"$error":"#N/A"}}]
[0,{"$f":"INDEX('Import data'!$A:$A,MATCH($A1973,'Import data'!$A:$A,0),1)","v":{"$error":"#N/A"}}]
[0,{"$f":"INDEX('Import data'!$A:$A,MATCH($A1974,'Import data'!$A:$A,0),1)","v":{"$error":"#N/A"}}]
[0,{"$f":"INDEX('Import data'!$A:$A,MATCH($A1975,'Import data'!$A:$A,0),1)","v":{"$error":"#N/A"}}]
[0,{"$f":"INDEX('Import data'!$A:$A,MATCH($A1976,'Import data'!$A:$A,0),1)","v":{"$error":"#N/A"}}]
[0,{"$f":"INDEX('Import data'!$A:$A,MATCH($A1977,'Import data'!$A:$A,0),1)","v":{"$error":"#N/A"}}]
[0,{"$f":"INDEX('Import data'!$A:$A,MATCH($A1978,'Import data'!$A:$A,0),1)","v":{"$error":"#N/A"}}]
[0,{"$f":"INDEX('Import data'!$A:$A,MATCH($A1979,'Import data'!$A:$A,0),1)","v":{"$error":"#N/A"}}]
[0,{"$f":"INDEX('Import data'!$A:$A,MATCH($A1980,'Import data'!$A:$A,0),1)","v":{"$error":"#N/A"}}]
[0,{"$f":"INDEX('Import data'!$A:$A,MATCH($A1981,'Import data'!$A:$A,0),1)","v":{"$error":"#N/A"}}]
[0,{"$f":"INDEX('Import data'!$A:$A,MATCH($A1982,'Import data'!$A:$A,0),1)","v":{"$error":"#N/A"}}]
[0,{"$f":"INDEX('Import data'!$A:$A,MATCH($A1983,'Import data'!$A:$A,0),1)","v":{"$error":"#N/A"}}]
[0,{"$f":"INDEX('Import data'!$A:$A,MATCH($A1984,'Import data'!$A:$A,0),1)","v":{"$error":"#N/A"}}]
[0,{"$f":"INDEX('Import data'!$A:$A,MATCH($A1985,'Import data'!$A:$A,0),1)","v":{"$error":"#N/A"}}]
[0,{"$f":"INDEX('Import data'!$A:$A,MATCH($A1986,'Import data'!$A:$A,0),1)","v":{"$error":"#N/A"}}]
[{"$f":"ID","v":0},{"$f":"INDEX('Import data'!$A:$A,MATCH($A1987,'Import data'!$A:$A,0),1)","v":{"$error":"#N/A"}}]
[0,{"$f":"INDEX('Import data'!$A:$A,MATCH($A1988,'Import data'!$A:$A,0),1)","v":{"$error":"#N/A"}}]
[0,{"$f":"INDEX('Import data'!$A:$A,MATCH($A1989,'Import data'!$A:$A,0),1)","v":{"$error":"#N/A"}}]
[0,{"$f":"INDEX('Import data'!$A:$A,MATCH($A1990,'Import data'!$A:$A,0),1)","v":{"$error":"#N/A"}}]
[0,{"$f":"INDEX('Import data'!$A:$A,MATCH($A1991,'Import data'!$A:$A,0),1)","v":{"$error":"#N/A"}}]
[0,{"$f":"INDEX('Import data'!$A:$A,MATCH($A1992,'Import data'!$A:$A,0),1)","v":{"$error":"#N/A"}}]
[0,{"$f":"INDEX('Import data'!$A:$A,MATCH($A1993,'Import data'!$A:$A,0),1)","v":{"$error":"#N/A"}}]
[0,{"$f":"INDEX('Import data'!$A:$A,MATCH($A1994,'Import data'!$A:$A,0),1)","v":{"$error":"#N/A"}}]
[0,{"$f":"INDEX('Import data'!$A:$A,MATCH($A1995,'Import data'!$A:$A,0),1)","v":{"$error":"#N/A"}}]
[0,{"$f":"INDEX('Import data'!$A:$A,MATCH($A1996,'Import data'!$A:$A,0),1)","v":{"$error":"#N/A"}}]
[0,{"$f":"INDEX('Import data'!$A:$A,MATCH($A1997,'Import data'!$A:$A,0),1)","v":{"$error":"#N/A"}}]
[0,{"$f":"INDEX('Import data'!$A:$A,MATCH($A1998,'Import data'!$A:$A,0),1)","v":{"$error":"#N/A"}}]
[0,{"$f":"INDEX('Import data'!$A:$A,MATCH($A1999,'Import data'!$A:$A,0),1)","v":{"$error":"#N/A"}}]
[0,{"$f":"INDEX('Import data'!$A:$A,MATCH($A2000,'Import data'!$A:$A,0),1)","v":{"$error":"#N/A"}}]
[0,{"$f":"INDEX('Import data'!$A:$A,MATCH($A2001,'Import data'!$A:$A,0),1)","v":{"$error":"#N/A"}}]
[0,{"$f":"INDEX('Import data'!$A:$A,MATCH($A2002,'Import data'!$A:$A,0),1)","v":{"$error":"#N/A"}}]
[0,{"$f":"INDEX('Import data'!$A:$A,MATCH($A2003,'Import data'!$A:$A,0),1)","v":{"$error":"#N/A"}}]
[0,{"$f":"INDEX('Import data'!$A:$A,MATCH($A2004,'Import data'!$A:$A,0),1)","v":{"$error":"#N/A"}}]
[0,{"$f":"INDEX('Import data'!$A:$A,MATCH($A2005,'Import data'!$A:$A,0),1)","v":{"$error":"#N/A"}}]
[0,{"$f":"INDEX('Import data'!$A:$A,MATCH($A2006,'Import data'!$A:$A,0),1)","v":{"$error":"#N/A"}}]
[0,{"$f":"INDEX('Import data'!$A:$A,MATCH($A2007,'Import data'!$A:$A,0),1)","v":{"$error":"#N/A"}}]
[0,{"$f":"INDEX('Import data'!$A:$A,MATCH($A2008,'Import data'!$A:$A,0),1)","v":{"$error":"#N/A"}}]
[0,{"$f":"INDEX('Import data'!$A:$A,MATCH($A2009,'Import data'!$A:$A,0),1)","v":{"$error":"#N/A"}}]
[0,{"$f":"INDEX('Import data'!$A:$A,MATCH($A2010,'Import data'!$A:$A,0),1)","v":{"$error":"#N/A"}}]
[0,{"$f":"INDEX('Import data'!$A:$A,MATCH($A2011,'Import data'!$A:$A,0),1)","v":{"$error":"#N/A"}}]
[0,{"$f":"INDEX('Import data'!$A:$A,MATCH($A2012,'Import data'!$A:$A,0),1)","v":{"$error":"#N/A"}}]
[0,{"$f":"INDEX('Import data'!$A:$A,MATCH($A2013,'Import data'!$A:$A,0),1)","v":{"$error":"#N/A"}}]
[0,{"$f":"INDEX('Import data'!$A:$A,MATCH($A2014,'Import data'!$A:$A,0),1)","v":{"$error":"#N/A"}}]
[0,{"$f":"INDEX('Import data'!$A:$A,MATCH($A2015,'Import data'!$A:$A,0),1)","v":{"$error":"#N/A"}}]
[0,{"$f":"INDEX('Import data'!$A:$A,MATCH($A2016,'Import data'!$A:$A,0),1)","v":{"$error":"#N/A"}}]
[0,{"$f":"INDEX('Import data'!$A:$A,MATCH($A2017,'Import data'!$A:$A,0),1)","v":{"$error":"#N/A"}}]
[0,{"$f":"INDEX('Import data'!$A:$A,MATCH($A2018,'Import data'!$A:$A,0),1)","v":{"$error":"#N/A"}}]
[0,{"$f":"INDEX('Import data'!$A:$A,MATCH($A2019,'Import data'!$A:$A,0),1)","v":{"$error":"#N/A"}}]
[0,{"$f":"INDEX('Import data'!$A:$A,MATCH($A2020,'Import data'!$A:$A,0),1)","v":{"$error":"#N/A"}}]
[0,{"$f":"INDEX('Import data'!$A:$A,MATCH($A2021,'Import data'!$A:$A,0),1)","v":{"$error":"#N/A"}}]
[0,{"$f":"INDEX('Import data'!$A:$A,MATCH($A2022,'Import data'!$A:$A,0),1)","v":{"$error":"#N/A"}}]
[0,{"$f":"INDEX('Import data'!$A:$A,MATCH($A2023,'Import data'!$A:$A,0),1)","v":{"$error":"#N/A"}}]
[0,{"$f":"INDEX('Import data'!$A:$A,MATCH($A2024,'Import data'!$A:$A,0),1)","v":{"$error":"#N/A"}}]
[0,{"$f":"INDEX('Import data'!$A:$A,MATCH($A2025,'Import data'!$A:$A,0),1)","v":{"$error":"#N/A"}}]
[0,{"$f":"INDEX('Import data'!$A:$A,MATCH($A2026,'Import data'!$A:$A,0),1)","v":{"$error":"#N/A"}}]
[0,{"$f":"INDEX('Import data'!$A:$A,MATCH($A2027,'Import data'!$A:$A,0),1)","v":{"$error":"#N/A"}}]
[0,{"$f":"INDEX('Import data'!$A:$A,MATCH($A2028,'Import data'!$A:$A,0),1)","v":{"$error":"#N/A"}}]
[0,{"$f":"INDEX('Import data'!$A:$A,MATCH($A2029,'Import data'!$A:$A,0),1)","v":{"$error":"#N/A"}}]
[0,{"$f":"INDEX('Import data'!$A:$A,MATCH($A2030,'Import data'!$A:$A,0),1)","v":{"$error":"#N/A"}}]
[0,{"$f":"INDEX('Import data'!$A:$A,MATCH($A2031,'Import data'!$A:$A,0),1)","v":{"$error":"#N/A"}}]
[0,{"$f":"INDEX('Import data'!$A:$A,MATCH($A2032,'Import data'!$A:$A,0),1)","v":{"$error":"#N/A"}}]
[0,{"$f":"INDEX('Import data'!$A:$A,MATCH($A2033,'Import data'!$A:$A,0),1)","v":{"$error":"#N/A"}}]
[0,{"$f":"INDEX('Import data'!$A:$A,MATCH($A2034,'Import data'!$A:$A,0),1)","v":{"$error":"#N/A"}}]
[0,{"$f":"INDEX('Import data'!$A:$A,MATCH($A2035,'Import data'!$A:$A,0),1)","v":{"$error":"#N/A"}}]
[0,{"$f":"INDEX('Import data'!$A:$A,MATCH($A2036,'Import data'!$A:$A,0),1)","v":{"$error":"#N/A"}}]
[0,{"$f":"INDEX('Import data'!$A:$A,MATCH($A2037,'Import data'!$A:$A,0),1)","v":{"$error":"#N/A"}}]
[0,{"$f":"INDEX('Import data'!$A:$A,MATCH($A2038,'Import data'!$A:$A,0),1)","v":{"$error":"#N/A"}}]
[0,{"$f":"INDEX('Import data'!$A:$A,MATCH($A2039,'Import data'!$A:$A,0),1)","v":{"$error":"#N/A"}}]
[0,{"$f":"INDEX('Import data'!$A:$A,MATCH($A2040,'Import data'!$A:$A,0),1)","v":{"$error":"#N/A"}}]
[0,{"$f":"INDEX('Import data'!$A:$A,MATCH($A2041,'Import data'!$A:$A,0),1)","v":{"$error":"#N/A"}}]
[0,{"$f":"INDEX('Import data'!$A:$A,MATCH($A2042,'Import data'!$A:$A,0),1)","v":{"$error":"#N/A"}}]
[0,{"$f":"INDEX('Import data'!$A:$A,MATCH($A2043,'Import data'!$A:$A,0),1)","v":{"$error":"#N/A"}}]
[0,{"$f":"INDEX('Import data'!$A:$A,MATCH($A2044,'Import data'!$A:$A,0),1)","v":{"$error":"#N/A"}}]
[0,{"$f":"INDEX('Import data'!$A:$A,MATCH($A2045,'Import data'!$A:$A,0),1)","v":{"$error":"#N/A"}}]
[0,{"$f":"INDEX('Import data'!$A:$A,MATCH($A2046,'Import data'!$A:$A,0),1)","v":{"$error":"#N/A"}}]
[0,{"$f":"INDEX('Import data'!$A:$A,MATCH($A2047,'Import data'!$A:$A,0),1)","v":{"$error":"#N/A"}}]
[0,{"$f":"INDEX('Import data'!$A:$A,MATCH($A2048,'Import data'!$A:$A,0),1)","v":{"$error":"#N/A"}}]
[0,{"$f":"INDEX('Import data'!$A:$A,MATCH($A2049,'Import data'!$A:$A,0),1)","v":{"$error":"#N/A"}}]
[0,{"$f":"INDEX('Import data'!$A:$A,MATCH($A2050,'Import data'!$A:$A,0),1)","v":{"$error":"#N/A"}}]
[{"$f":"ID","v":0},{"$f":"INDEX('Import data'!$A:$A,MATCH($A2051,'Import data'!$A:$A,0),1)","v":{"$error":"#N/A"}}]
[0,{"$f":"INDEX('Import data'!$A:$A,MATCH($A2052,'Import data'!$A:$A,0),1)","v":{"$error":"#N/A"}}]
[0,{"$f":"INDEX('Import data'!$A:$A,MATCH($A2053,'Import data'!$A:$A,0),1)","v":{"$error":"#N/A"}}]
[0,{"$f":"INDEX('Import data'!$A:$A,MATCH($A2054,'Import data'!$A:$A,0),1)","v":{"$error":"#N/A"}}]
[0,{"$f":"INDEX('Import data'!$A:$A,MATCH($A2055,'Import data'!$A:$A,0),1)","v":{"$error":"#N/A"}}]
[0,{"$f":"INDEX('Import data'!$A:$A,MATCH($A2056,'Import data'!$A:$A,0),1)","v":{"$error":"#N/A"}}]
[0,{"$f":"INDEX('Import data'!$A:$A,MATCH($A2057,'Import data'!$A:$A,0),1)","v":{"$error":"#N/A"}}]
[0,{"$f":"INDEX('Import data'!$A:$A,MATCH($A2058,'Import data'!$A:$A,0),1)","v":{"$error":"#N/A"}}]
[0,{"$f":"INDEX('Import data'!$A:$A,MATCH($A2059,'Import data'!$A:$A,0),1)","v":{"$error":"#N/A"}}]
[0,{"$f":"INDEX('Import data'!$A:$A,MATCH($A2060,'Import data'!$A:$A,0),1)","v":{"$error":"#N/A"}}]
[0,{"$f":"INDEX('Import data'!$A:$A,MATCH($A2061,'Import data'!$A:$A,0),1)","v":{"$error":"#N/A"}}]
[0,{"$f":"INDEX('Import data'!$A:$A,MATCH($A2062,'Import data'!$A:$A,0),1)","v":{"$error":"#N/A"}}]
[0,{"$f":"INDEX('Import data'!$A:$A,MATCH($A2063,'Import data'!$A:$A,0),1)","v":{"$error":"#N/A"}}]
[0,{"$f":"INDEX('Import data'!$A:$A,MATCH($A2064,'Import data'!$A:$A,0),1)","v":{"$error":"#N/A"}}]
[0,{"$f":"INDEX('Import data'!$A:$A,MATCH($A2065,'Import data'!$A:$A,0),1)","v":{"$error":"#N/A"}}]
[0,{"$f":"INDEX('Import data'!$A:$A,MATCH($A2066,'Import data'!$A:$A,0),1)","v":{"$error":"#N/A"}}]
[0,{"$f":"INDEX('Import data'!$A:$A,MATCH($A2067,'Import data'!$A:$A,0),1)","v":{"$error":"#N/A"}}]
[0,{"$f":"INDEX('Import data'!$A:$A,MATCH($A2068,'Import data'!$A:$A,0),1)","v":{"$error":"#N/A"}}]
[0,{"$f":"INDEX('Import data'!$A:$A,MATCH($A2069,'Import data'!$A:$A,0),1)","v":{"$error":"#N/A"}}]
[0,{"$f":"INDEX('Import data'!$A:$A,MATCH($A2070,'Import data'!$A:$A,0),1)","v":{"$error":"#N/A"}}]
[0,{"$f":"INDEX('Import data'!$A:$A,MATCH($A2071,'Import data'!$A:$A,0),1)","v":{"$error":"#N/A"}}]
[0,{"$f":"INDEX('Import data'!$A:$A,MATCH($A2072,'Import data'!$A:$A,0),1)","v":{"$error":"#N/A"}}]
[0,{"$f":"INDEX('Import data'!$A:$A,MATCH($A2073,'Import data'!$A:$A,0),1)","v":{"$error":"#N/A"}}]
[0,{"$f":"INDEX('Import data'!$A:$A,MATCH($A2074,'Import data'!$A:$A,0),1)","v":{"$error":"#N/A"}}]
[0,{"$f":"INDEX('Import data'!$A:$A,MATCH($A2075,'Import data'!$A:$A,0),1)","v":{"$error":"#N/A"}}]
[0,{"$f":"INDEX('Import data'!$A:$A,MATCH($A2076,'Import data'!$A:$A,0),1)","v":{"$error":"#N/A"}}]
[0,{"$f":"INDEX('Import data'!$A:$A,MATCH($A2077,'Import data'!$A:$A,0),1)","v":{"$error":"#N/A"}}]
[0,{"$f":"INDEX('Import data'!$A:$A,MATCH($A2078,'Import data'!$A:$A,0),1)","v":{"$error":"#N/A"}}]
[0,{"$f":"INDEX('Import data'!$A:$A,MATCH($A2079,'Import data'!$A:$A,0),1)","v":{"$error":"#N/A"}}]
[0,{"$f":"INDEX('Import data'!$A:$A,MATCH($A2080,'Import data'!$A:$A,0),1)","v":{"$error":"#N/A"}}]
[0,{"$f":"INDEX('Import data'!$A:$A,MATCH($A2081,'Import data'!$A:$A,0),1)","v":{"$error":"#N/A"}}]
[0,{"$f":"INDEX('Import data'!$A:$A,MATCH($A2082,'Import data'!$A:$A,0),1)","v":{"$error":"#N/A"}}]
[0,{"$f":"INDEX('Import data'!$A:$A,MATCH($A2083,'Import data'!$A:$A,0),1)","v":{"$error":"#N/A"}}]
[0,{"$f":"INDEX('Import data'!$A:$A,MATCH($A2084,'Import data'!$A:$A,0),1)","v":{"$error":"#N/A"}}]
[0,{"$f":"INDEX('Import data'!$A:$A,MATCH($A2085,'Import data'!$A:$A,0),1)","v":{"$error":"#N/A"}}]
[0,{"$f":"INDEX('Import data'!$A:$A,MATCH($A2086,'Import data'!$A:$A,0),1)","v":{"$error":"#N/A"}}]
[0,{"$f":"INDEX('Import data'!$A:$A,MATCH($A2087,'Import data'!$A:$A,0),1)","v":{"$error":"#N/A"}}]
[0,{"$f":"INDEX('Import data'!$A:$A,MATCH($A2088,'Import data'!$A:$A,0),1)","v":{"$error":"#N/A"}}]
[0,{"$f":"INDEX('Import data'!$A:$A,MATCH($A2089,'Import data'!$A:$A,0),1)","v":{"$error":"#N/A"}}]
[0,{"$f":"INDEX('Import data'!$A:$A,MATCH($A2090,'Import data'!$A:$A,0),1)","v":{"$error":"#N/A"}}]
[0,{"$f":"INDEX('Import data'!$A:$A,MATCH($A2091,'Import data'!$A:$A,0),1)","v":{"$error":"#N/A"}}]
[0,{"$f":"INDEX('Import data'!$A:$A,MATCH($A2092,'Import data'!$A:$A,0),1)","v":{"$error":"#N/A"}}]
[0,{"$f":"INDEX('Import data'!$A:$A,MATCH($A2093,'Import data'!$A:$A,0),1)","v":{"$error":"#N/A"}}]
[0,{"$f":"INDEX('Import data'!$A:$A,MATCH($A2094,'Import data'!$A:$A,0),1)","v":{"$error":"#N/A"}}]
[0,{"$f":"INDEX('Import data'!$A:$A,MATCH($A2095,'Import data'!$A:$A,0),1)","v":{"$error":"#N/A"}}]
[0,{"$f":"INDEX('Import data'!$A:$A,MATCH($A2096,'Import data'!$A:$A,0),1)","v":{"$error":"#N/A"}}]
[0,{"$f":"INDEX('Import data'!$A:$A,MATCH($A2097,'Import data'!$A:$A,0),1)","v":{"$error":"#N/A"}}]
[0,{"$f":"INDEX('Import data'!$A:$A,MATCH($A2098,'Import data'!$A:$A,0),1)","v":{"$error":"#N/A"}}]
[0,{"$f":"INDEX('Import data'!$A:$A,MATCH($A2099,'Import data'!$A:$A,0),1)","v":{"$error":"#N/A"}}]
[0,{"$f":"INDEX('Import data'!$A:$A,MATCH($A2100,'Import data'!$A:$A,0),1)","v":{"$error":"#N/A"}}]
[0,{"$f":"INDEX('Import data'!$A:$A,MATCH($A2101,'Import data'!$A:$A,0),1)","v":{"$error":"#N/A"}}]
[0,{"$f":"INDEX('Import data'!$A:$A,MATCH($A2102,'Import data'!$A:$A,0),1)","v":{"$error":"#N/A"}}]
[0,{"$f":"INDEX('Import data'!$A:$A,MATCH($A2103,'Import data'!$A:$A,0),1)","v":{"$error":"#N/A"}}]
[0,{"$f":"INDEX('Import data'!$A:$A,MATCH($A2104,'Import data'!$A:$A,0),1)","v":{"$error":"#N/A"}}]
[0,{"$f":"INDEX('Import data'!$A:$A,MATCH($A2105,'Import data'!$A:$A,0),1)","v":{"$error":"#N/A"}}]
[0,{"$f":"INDEX('Import data'!$A:$A,MATCH($A2106,'Import data'!$A:$A,0),1)","v":{"$error":"#N/A"}}]
[0,{"$f":"INDEX('Import data'!$A:$A,MATCH($A2107,'Import data'!$A:$A,0),1)","v":{"$error":"#N/A"}}]
[0,{"$f":"INDEX('Import data'!$A:$A,MATCH($A2108,'Import data'!$A:$A,0),1)","v":{"$error":"#N/A"}}]
[0,{"$f":"INDEX('Import data'!$A:$A,MATCH($A2109,'Import data'!$A:$A,0),1)","v":{"$error":"#N/A"}}]
[0,{"$f":"INDEX('Import data'!$A:$A,MATCH($A2110,'Import data'!$A:$A,0),1)","v":{"$error":"#N/A"}}]
[0,{"$f":"INDEX('Import data'!$A:$A,MATCH($A2111,'Import data'!$A:$A,0),1)","v":{"$error":"#N/A"}}]
[0,{"$f":"INDEX('Import data'!$A:$A,MATCH($A2112,'Import data'!$A:$A,0),1)","v":{"$error":"#N/A"}}]
[0,{"$f":"INDEX('Import data'!$A:$A,MATCH($A2113,'Import data'!$A:$A,0),1)","v":{"$error":"#N/A"}}]
[0,{"$f":"INDEX('Import data'!$A:$A,MATCH($A2114,'Import data'!$A:$A,0),1)","v":{"$error":"#N/A"}}]
[{"$f":"ID","v":0},{"$f":"INDEX('Import data'!$A:$A,MATCH($A2115,'Import data'!$A:$A,0),1)","v":{"$error":"#N/A"}}]
[0,{"$f":"INDEX('Import data'!$A:$A,MATCH($A2116,'Import data'!$A:$A,0),1)","v":{"$error":"#N/A"}}]
[0,{"$f":"INDEX('Import data'!$A:$A,MATCH($A2117,'Import data'!$A:$A,0),1)","v":{"$error":"#N/A"}}]
[0,{"$f":"INDEX('Import data'!$A:$A,MATCH($A2118,'Import data'!$A:$A,0),1)","v":{"$error":"#N/A"}}]
[0,{"$f":"INDEX('Import data'!$A:$A,MATCH($A2119,'Import data'!$A:$A,0),1)","v":{"$error":"#N/A"}}]
[0,{"$f":"INDEX('Import data'!$A:$A,MATCH($A2120,'Import data'!$A:$A,0),1)","v":{"$error":"#N/A"}}]
[0,{"$f":"INDEX('Import data'!$A:$A,MATCH($A2121,'Import data'!$A:$A,0),1)","v":{"$error":"#N/A"}}]
[0,{"$f":"INDEX('Import data'!$A:$A,MATCH($A2122,'Import data'!$A:$A,0),1)","v":{"$error":"#N/A"}}]
[0,{"$f":"INDEX('Import data'!$A:$A,MATCH($A2123,'Import data'!$A:$A,0),1)","v":{"$error":"#N/A"}}]
[0,{"$f":"INDEX('Import data'!$A:$A,MATCH($A2124,'Import data'!$A:$A,0),1)","v":{"$error":"#N/A"}}]
[0,{"$f":"INDEX('Import data'!$A:$A,MATCH($A2125,'Import data'!$A:$A,0),1)","v":{"$error":"#N/A"}}]
[0,{"$f":"INDEX('Import data'!$A:$A,MATCH($A2126,'Import data'!$A:$A,0),1)","v":{"$error":"#N/A"}}]
[0,{"$f":"INDEX('Import data'!$A:$A,MATCH($A2127,'Import data'!$A:$A,0),1)","v":{"$error":"#N/A"}}]
[0,{"$f":"INDEX('Import data'!$A:$A,MATCH($A2128,'Import data'!$A:$A,0),1)","v":{"$error":"#N/A"}}]
[0,{"$f":"INDEX('Import data'!$A:$A,MATCH($A2129,'Import data'!$A:$A,0),1)","v":{"$error":"#N/A"}}]
[0,{"$f":"INDEX('Import data'!$A:$A,MATCH($A2130,'Import data'!$A:$A,0),1)","v":{"$error":"#N/A"}}]
[0,{"$f":"INDEX('Import data'!$A:$A,MATCH($A2131,'Import data'!$A:$A,0),1)","v":{"$error":"#N/A"}}]
[0,{"$f":"INDEX('Import data'!$A:$A,MATCH($A2132,'Import data'!$A:$A,0),1)","v":{"$error":"#N/A"}}]
[0,{"$f":"INDEX('Import data'!$A:$A,MATCH($A2133,'Import data'!$A:$A,0),1)","v":{"$error":"#N/A"}}]
[0,{"$f":"INDEX('Import data'!$A:$A,MATCH($A2134,'Import data'!$A:$A,0),1)","v":{"$error":"#N/A"}}]
[0,{"$f":"INDEX('Import data'!$A:$A,MATCH($A2135,'Import data'!$A:$A,0),1)","v":{"$error":"#N/A"}}]
[0,{"$f":"INDEX('Import data'!$A:$A,MATCH($A2136,'Import data'!$A:$A,0),1)","v":{"$error":"#N/A"}}]
[0,{"$f":"INDEX('Import data'!$A:$A,MATCH($A2137,'Import data'!$A:$A,0),1)","v":{"$error":"#N/A"}}]
[0,{"$f":"INDEX('Import data'!$A:$A,MATCH($A2138,'Import data'!$A:$A,0),1)","v":{"$error":"#N/A"}}]
[0,{"$f":"INDEX('Import data'!$A:$A,MATCH($A2139,'Import data'!$A:$A,0),1)","v":{"$error":"#N/A"}}]
[0,{"$f":"INDEX('Import data'!$A:$A,MATCH($A2140,'Import data'!$A:$A,0),1)","v":{"$error":"#N/A"}}]
[0,{"$f":"INDEX('Import data'!$A:$A,MATCH($A2141,'Import data'!$A:$A,0),1)","v":{"$error":"#N/A"}}]
[0,{"$f":"INDEX('Import data'!$A:$A,MATCH($A2142,'Import data'!$A:$A,0),1)","v":{"$error":"#N/A"}}]
[0,{"$f":"INDEX('Import data'!$A:$A,MATCH($A2143,'Import data'!$A:$A,0),1)","v":{"$error":"#N/A"}}]
[0,{"$f":"INDEX('Import data'!$A:$A,MATCH($A2144,'Import data'!$A:$A,0),1)","v":{"$error":"#N/A"}}]
[0,{"$f":"INDEX('Import data'!$A:$A,MATCH($A2145,'Import data'!$A:$A,0),1)","v":{"$error":"#N/A"}}]
[0,{"$f":"INDEX('Import data'!$A:$A,MATCH($A2146,'Import data'!$A:$A,0),1)","v":{"$error":"#N/A"}}]
[0,{"$f":"INDEX('Import data'!$A:$A,MATCH($A2147,'Import data'!$A:$A,0),1)","v":{"$error":"#N/A"}}]
[0,{"$f":"INDEX('Import data'!$A:$A,MATCH($A2148,'Import data'!$A:$A,0),1)","v":{"$error":"#N/A"}}]
[0,{"$f":"INDEX('Import data'!$A:$A,MATCH($A2149,'Import data'!$A:$A,0),1)","v":{"$error":"#N/A"}}]
[0,{"$f":"INDEX('Import data'!$A:$A,MATCH($A2150,'Import data'!$A:$A,0),1)","v":{"$error":"#N/A"}}]
[0,{"$f":"INDEX('Import data'!$A:$A,MATCH($A2151,'Import data'!$A:$A,0),1)","v":{"$error":"#N/A"}}]
[0,{"$f":"INDEX('Import data'!$A:$A,MATCH($A2152,'Import data'!$A:$A,0),1)","v":{"$error":"#N/A"}}]
[0,{"$f":"INDEX('Import data'!$A:$A,MATCH($A2153,'Import data'!$A:$A,0),1)","v":{"$error":"#N/A"}}]
[0,{"$f":"INDEX('Import data'!$A:$A,MATCH($A2154,'Import data'!$A:$A,0),1)","v":{"$error":"#N/A"}}]
[0,{"$f":"INDEX('Import data'!$A:$A,MATCH($A2155,'Import data'!$A:$A,0),1)","v":{"$error":"#N/A"}}]
[0,{"$f":"INDEX('Import data'!$A:$A,MATCH($A2156,'Import data'!$A:$A,0),1)","v":{"$error":"#N/A"}}]
[0,{"$f":"INDEX('Import data'!$A:$A,MATCH($A2157,'Import data'!$A:$A,0),1)","v":{"$error":"#N/A"}}]
[0,{"$f":"INDEX('Import data'!$A:$A,MATCH($A2158,'Import data'!$A:$A,0),1)","v":{"$error":"#N/A"}}]
[0,{"$f":"INDEX('Import data'!$A:$A,MATCH($A2159,'Import data'!$A:$A,0),1)","v":{"$error":"#N/A"}}]
[0,{"$f":"INDEX('Import data'!$A:$A,MATCH($A2160,'Import data'!$A:$A,0),1)","v":{"$error":"#N/A"}}]
[0,{"$f":"INDEX('Import data'!$A:$A,MATCH($A2161,'Import data'!$A:$A,0),1)","v":{"$error":"#N/A"}}]
[0,{"$f":"INDEX('Import data'!$A:$A,MATCH($A2162,'Import data'!$A:$A,0),1)","v":{"$error":"#N/A"}}]
[0,{"$f":"INDEX('Import data'!$A:$A,MATCH($A2163,'Import data'!$A:$A,0),1)","v":{"$error":"#N/A"}}]
[0,{"$f":"INDEX('Import data'!$A:$A,MATCH($A2164,'Import data'!$A:$A,0),1)","v":{"$error":"#N/A"}}]
[0,{"$f":"INDEX('Import data'!$A:$A,MATCH($A2165,'Import data'!$A:$A,0),1)","v":{"$error":"#N/A"}}]
[0,{"$f":"INDEX('Import data'!$A:$A,MATCH($A2166,'Import data'!$A:$A,0),1)","v":{"$error":"#N/A"}}]
[0,{"$f":"INDEX('Import data'!$A:$A,MATCH($A2167,'Import data'!$A:$A,0),1)","v":{"$error":"#N/A"}}]
[0,{"$f":"INDEX('Import data'!$A:$A,MATCH($A2168,'Import data'!$A:$A,0),1)","v":{"$error":"#N/A"}}]
[0,{"$f":"INDEX('Import data'!$A:$A,MATCH($A2169,'Import data'!$A:$A,0),1)","v":{"$error":"#N/A"}}]
[0,{"$f":"INDEX('Import data'!$A:$A,MATCH($A2170,'Import data'!$A:$A,0),1)","v":{"$error":"#N/A"}}]
[0,{"$f":"INDEX('Import data'!$A:$A,MATCH($A2171,'Import data'!$A:$A,0),1)","v":{"$error":"#N/A"}}]
[0,{"$f":"INDEX('Import data'!$A:$A,MATCH($A2172,'Import data'!$A:$A,0),1)","v":{"$error":"#N/A"}}]
[0,{"$f":"INDEX('Import data'!$A:$A,MATCH($A2173,'Import data'!$A:$A,0),1)","v":{"$error":"#N/A"}}]
[0,{"$f":"INDEX('Import data'!$A:$A,MATCH($A2174,'Import data'!$A:$A,0),1)","v":{"$error":"#N/A"}}]
[0,{"$f":"INDEX('Import data'!$A:$A,MATCH($A2175,'Import data'!$A:$A,0),1)","v":{"$error":"#N/A"}}]
[0,{"$f":"INDEX('Import data'!$A:$A,MATCH($A2176,'Import data'!$A:$A,0),1)","v":{"$error":"#N/A"}}]
[0,{"$f":"INDEX('Import data'!$A:$A,MATCH($A2177,'Import data'!$A:$A,0),1)","v":{"$error":"#N/A"}}]
[0,{"$f":"INDEX('Import data'!$A:$A,MATCH($A2178,'Import data'!$A:$A,0),1)","v":{"$error":"#N/A"}}]
[{"$f":"ID","v":0},{"$f":"INDEX('Import data'!$A:$A,MATCH($A2179,'Import data'!$A:$A,0),1)","v":{"$error":"#N/A"}}]
[0,{"$f":"INDEX('Import data'!$A:$A,MATCH($A2180,'Import data'!$A:$A,0),1)","v":{"$error":"#N/A"}}]
[0,{"$f":"INDEX('Import data'!$A:$A,MATCH($A2181,'Import data'!$A:$A,0),1)","v":{"$error":"#N/A"}}]
[0,{"$f":"INDEX('Import data'!$A:$A,MATCH($A2182,'Import data'!$A:$A,0),1)","v":{"$error":"#N/A"}}]
[0,{"$f":"INDEX('Import data'!$A:$A,MATCH($A2183,'Import data'!$A:$A,0),1)","v":{"$error":"#N/A"}}]
[0,{"$f":"INDEX('Import data'!$A:$A,MATCH($A2184,'Import data'!$A:$A,0),1)","v":{"$error":"#N/A"}}]
[0,{"$f":"INDEX('Import data'!$A:$A,MATCH($A2185,'Import data'!$A:$A,0),1)","v":{"$error":"#N/A"}}]
[0,{"$f":"INDEX('Import data'!$A:$A,MATCH($A2186,'Import data'!$A:$A,0),1)","v":{"$error":"#N/A"}}]
[0,{"$f":"INDEX('Import data'!$A:$A,MATCH($A2187,'Import data'!$A:$A,0),1)","v":{"$error":"#N/A"}}]
[0,{"$f":"INDEX('Import data'!$A:$A,MATCH($A2188,'Import data'!$A:$A,0),1)","v":{"$error":"#N/A"}}]
[0,{"$f":"INDEX('Import data'!$A:$A,MATCH($A2189,'Import data'!$A:$A,0),1)","v":{"$error":"#N/A"}}]
[0,{"$f":"INDEX('Import data'!$A:$A,MATCH($A2190,'Import data'!$A:$A,0),1)","v":{"$error":"#N/A"}}]
[0,{"$f":"INDEX('Import data'!$A:$A,MATCH($A2191,'Import data'!$A:$A,0),1)","v":{"$error":"#N/A"}}]
[0,{"$f":"INDEX('Import data'!$A:$A,MATCH($A2192,'Import data'!$A:$A,0),1)","v":{"$error":"#N/A"}}]
[0,{"$f":"INDEX('Import data'!$A:$A,MATCH($A2193,'Import data'!$A:$A,0),1)","v":{"$error":"#N/A"}}]
[0,{"$f":"INDEX('Import data'!$A:$A,MATCH($A2194,'Import data'!$A:$A,0),1)","v":{"$error":"#N/A"}}]
[0,{"$f":"INDEX('Import data'!$A:$A,MATCH($A2195,'Import data'!$A:$A,0),1)","v":{"$error":"#N/A"}}]
[0,{"$f":"INDEX('Import data'!$A:$A,MATCH($A2196,'Import data'!$A:$A,0),1)","v":{"$error":"#N/A"}}]
[0,{"$f":"INDEX('Import data'!$A:$A,MATCH($A2197,'Import data'!$A:$A,0),1)","v":{"$error":"#N/A"}}]
[0,{"$f":"INDEX('Import data'!$A:$A,MATCH($A2198,'Import data'!$A:$A,0),1)","v":{"$error":"#N/A"}}]
[0,{"$f":"INDEX('Import data'!$A:$A,MATCH($A2199,'Import data'!$A:$A,0),1)","v":{"$error":"#N/A"}}]
[0,{"$f":"INDEX('Import data'!$A:$A,MATCH($A2200,'Import data'!$A:$A,0),1)","v":{"$error":"#N/A"}}]
[0,{"$f":"INDEX('Import data'!$A:$A,MATCH($A2201,'Import data'!$A:$A,0),1)","v":{"$error":"#N/A"}}]
[0,{"$f":"INDEX('Import data'!$A:$A,MATCH($A2202,'Import data'!$A:$A,0),1)","v":{"$error":"#N/A"}}]
[0,{"$f":"INDEX('Import data'!$A:$A,MATCH($A2203,'Import data'!$A:$A,0),1)","v":{"$error":"#N/A"}}]
[0,{"$f":"INDEX('Import data'!$A:$A,MATCH($A2204,'Import data'!$A:$A,0),1)","v":{"$error":"#N/A"}}]
[0,{"$f":"INDEX('Import data'!$A:$A,MATCH($A2205,'Import data'!$A:$A,0),1)","v":{"$error":"#N/A"}}]
[0,{"$f":"INDEX('Import data'!$A:$A,MATCH($A2206,'Import data'!$A:$A,0),1)","v":{"$error":"#N/A"}}]
[0,{"$f":"INDEX('Import data'!$A:$A,MATCH($A2207,'Import data'!$A:$A,0),1)","v":{"$error":"#N/A"}}]
[0,{"$f":"INDEX('Import data'!$A:$A,MATCH($A2208,'Import data'!$A:$A,0),1)","v":{"$error":"#N/A"}}]
[0,{"$f":"INDEX('Import data'!$A:$A,MATCH($A2209,'Import data'!$A:$A,0),1)","v":{"$error":"#N/A"}}]
[0,{"$f":"INDEX('Import data'!$A:$A,MATCH($A2210,'Import data'!$A:$A,0),1)","v":{"$error":"#N/A"}}]
[0,{"$f":"INDEX('Import data'!$A:$A,MATCH($A2211,'Import data'!$A:$A,0),1)","v":{"$error":"#N/A"}}]
[0,{"$f":"INDEX('Import data'!$A:$A,MATCH($A2212,'Import data'!$A:$A,0),1)","v":{"$error":"#N/A"}}]
[0,{"$f":"INDEX('Import data'!$A:$A,MATCH($A2213,'Import data'!$A:$A,0),1)","v":{"$error":"#N/A"}}]
[0,{"$f":"INDEX('Import data'!$A:$A,MATCH($A2214,'Import data'!$A:$A,0),1)","v":{"$error":"#N/A"}}]
[0,{"$f":"INDEX('Import data'!$A:$A,MATCH($A2215,'Import data'!$A:$A,0),1)","v":{"$error":"#N/A"}}]
[0,{"$f":"INDEX('Import data'!$A:$A,MATCH($A2216,'Import data'!$A:$A,0),1)","v":{"$error":"#N/A"}}]
[0,{"$f":"INDEX('Import data'!$A:$A,MATCH($A2217,'Import data'!$A:$A,0),1)","v":{"$error":"#N/A"}}]
[0,{"$f":"INDEX('Import data'!$A:$A,MATCH($A2218,'Import data'!$A:$A,0),1)","v":{"$error":"#N/A"}}]
[0,{"$f":"INDEX('Import data'!$A:$A,MATCH($A2219,'Import data'!$A:$A,0),1)","v":{"$error":"#N/A"}}]
[0,{"$f":"INDEX('Import data'!$A:$A,MATCH($A2220,'Import data'!$A:$A,0),1)","v":{"$error":"#N/A"}}]
[0,{"$f":"INDEX('Import data'!$A:$A,MATCH($A2221,'Import data'!$A:$A,0),1)","v":{"$error":"#N/A"}}]
[0,{"$f":"INDEX('Import data'!$A:$A,MATCH($A2222,'Import data'!$A:$A,0),1)","v":{"$error":"#N/A"}}]
[0,{"$f":"INDEX('Import data'!$A:$A,MATCH($A2223,'Import data'!$A:$A,0),1)","v":{"$error":"#N/A"}}]
[0,{"$f":"INDEX('Import data'!$A:$A,MATCH($A2224,'Import data'!$A:$A,0),1)","v":{"$error":"#N/A"}}]
[0,{"$f":"INDEX('Import data'!$A:$A,MATCH($A2225,'Import data'!$A:$A,0),1)","v":{"$error":"#N/A"}}]
[0,{"$f":"INDEX('Import data'!$A:$A,MATCH($A2226,'Import data'!$A:$A,0),1)","v":{"$error":"#N/A"}}]
[0,{"$f":"INDEX('Import data'!$A:$A,MATCH($A2227,'Import data'!$A:$A,0),1)","v":{"$error":"#N/A"}}]
[0,{"$f":"INDEX('Import data'!$A:$A,MATCH($A2228,'Import data'!$A:$A,0),1)","v":{"$error":"#N/A"}}]
[0,{"$f":"INDEX('Import data'!$A:$A,MATCH($A2229,'Import data'!$A:$A,0),1)","v":{"$error":"#N/A"}}]
[0,{"$f":"INDEX('Import data'!$A:$A,MATCH($A2230,'Import data'!$A:$A,0),1)","v":{"$error":"#N/A"}}]
[0,{"$f":"INDEX('Import data'!$A:$A,MATCH($A2231,'Import data'!$A:$A,0),1)","v":{"$error":"#N/A"}}]
[0,{"$f":"INDEX('Import data'!$A:$A,MATCH($A2232,'Import data'!$A:$A,0),1)","v":{"$error":"#N/A"}}]
[0,{"$f":"INDEX('Import data'!$A:$A,MATCH($A2233,'Import data'!$A:$A,0),1)","v":{"$error":"#N/A"}}]
[0,{"$f":"INDEX('Import data'!$A:$A,MATCH($A2234,'Import data'!$A:$A,0),1)","v":{"$error":"#N/A"}}]
[0,{"$f":"INDEX('Import data'!$A:$A,MATCH($A2235,'Import data'!$A:$A,0),1)","v":{"$error":"#N/A"}}]
[0,{"$f":"INDEX('Import data'!$A:$A,MATCH($A2236,'Import data'!$A:$A,0),1)","v":{"$error":"#N/A"}}]
[0,{"$f":"INDEX('Import data'!$A:$A,MATCH($A2237,'Import data'!$A:$A,0),1)","v":{"$error":"#N/A"}}]
[0,{"$f":"INDEX('Import data'!$A:$A,MATCH($A2238,'Import data'!$A:$A,0),1)","v":{"$error":"#N/A"}}]
[0,{"$f":"INDEX('Import data'!$A:$A,MATCH($A2239,'Import data'!$A:$A,0),1)","v":{"$error":"#N/A"}}]
[0,{"$f":"INDEX('Import data'!$A:$A,MATCH($A2240,'Import data'!$A:$A,0),1)","v":{"$error":"#N/A"}}]
[0,{"$f":"INDEX('Import data'!$A:$A,MATCH($A2241,'Import data'!$A:$A,0),1)","v":{"$error":"#N/A"}}]
[0,{"$f":"INDEX('Import data'!$A:$A,MATCH($A2242,'Import data'!$A:$A,0),1)","v":{"$error":"#N/A"}}]
[{"$f":"ID","v":0},{"$f":"INDEX('Import data'!$A:$A,MATCH($A2243,'Import data'!$A:$A,0),1)","v":{"$error":"#N/A"}}]
[0,{"$f":"INDEX('Import data'!$A:$A,MATCH($A2244,'Import data'!$A:$A,0),1)","v":{"$error":"#N/A"}}]
[0,{"$f":"INDEX('Import data'!$A:$A,MATCH($A2245,'Import data'!$A:$A,0),1)","v":{"$error":"#N/A"}}]
[0,{"$f":"INDEX('Import data'!$A:$A,MATCH($A2246,'Import data'!$A:$A,0),1)","v":{"$error":"#N/A"}}]
[0,{"$f":"INDEX('Import data'!$A:$A,MATCH($A2247,'Import data'!$A:$A,0),1)","v":{"$error":"#N/A"}}]
[0,{"$f":"INDEX('Import data'!$A:$A,MATCH($A2248,'Import data'!$A:$A,0),1)","v":{"$error":"#N/A"}}]
[0,{"$f":"INDEX('Import data'!$A:$A,MATCH($A2249,'Import data'!$A:$A,0),1)","v":{"$error":"#N/A"}}]
[0,{"$f":"INDEX('Import data'!$A:$A,MATCH($A2250,'Import data'!$A:$A,0),1)","v":{"$error":"#N/A"}}]
[0,{"$f":"INDEX('Import data'!$A:$A,MATCH($A2251,'Import data'!$A:$A,0),1)","v":{"$error":"#N/A"}}]
[0,{"$f":"INDEX('Import data'!$A:$A,MATCH($A2252,'Import data'!$A:$A,0),1)","v":{"$error":"#N/A"}}]
[0,{"$f":"INDEX('Import data'!$A:$A,MATCH($A2253,'Import data'!$A:$A,0),1)","v":{"$error":"#N/A"}}]
[0,{"$f":"INDEX('Import data'!$A:$A,MATCH($A2254,'Import data'!$A:$A,0),1)","v":{"$error":"#N/A"}}]
[0,{"$f":"INDEX('Import data'!$A:$A,MATCH($A2255,'Import data'!$A:$A,0),1)","v":{"$error":"#N/A"}}]
[0,{"$f":"INDEX('Import data'!$A:$A,MATCH($A2256,'Import data'!$A:$A,0),1)","v":{"$error":"#N/A"}}]
[0,{"$f":"INDEX('Import data'!$A:$A,MATCH($A2257,'Import data'!$A:$A,0),1)","v":{"$error":"#N/A"}}]
[0,{"$f":"INDEX('Import data'!$A:$A,MATCH($A2258,'Import data'!$A:$A,0),1)","v":{"$error":"#N/A"}}]
[0,{"$f":"INDEX('Import data'!$A:$A,MATCH($A2259,'Import data'!$A:$A,0),1)","v":{"$error":"#N/A"}}]
[0,{"$f":"INDEX('Import data'!$A:$A,MATCH($A2260,'Import data'!$A:$A,0),1)","v":{"$error":"#N/A"}}]
[0,{"$f":"INDEX('Import data'!$A:$A,MATCH($A2261,'Import data'!$A:$A,0),1)","v":{"$error":"#N/A"}}]
[0,{"$f":"INDEX('Import data'!$A:$A,MATCH($A2262,'Import data'!$A:$A,0),1)","v":{"$error":"#N/A"}}]
[0,{"$f":"INDEX('Import data'!$A:$A,MATCH($A2263,'Import data'!$A:$A,0),1)","v":{"$error":"#N/A"}}]
[0,{"$f":"INDEX('Import data'!$A:$A,MATCH($A2264,'Import data'!$A:$A,0),1)","v":{"$error":"#N/A"}}]
[0,{"$f":"INDEX('Import data'!$A:$A,MATCH($A2265,'Import data'!$A:$A,0),1)","v":{"$error":"#N/A"}}]
[0,{"$f":"INDEX('Import data'!$A:$A,MATCH($A2266,'Import data'!$A:$A,0),1)","v":{"$error":"#N/A"}}]
[0,{"$f":"INDEX('Import data'!$A:$A,MATCH($A2267,'Import data'!$A:$A,0),1)","v":{"$error":"#N/A"}}]
[0,{"$f":"INDEX('Import data'!$A:$A,MATCH($A2268,'Import data'!$A:$A,0),1)","v":{"$error":"#N/A"}}]
[0,{"$f":"INDEX('Import data'!$A:$A,MATCH($A2269,'Import data'!$A:$A,0),1)","v":{"$error":"#N/A"}}]
[0,{"$f":"INDEX('Import data'!$A:$A,MATCH($A2270,'Import data'!$A:$A,0),1)","v":{"$error":"#N/A"}}]
[0,{"$f":"INDEX('Import data'!$A:$A,MATCH($A2271,'Import data'!$A:$A,0),1)","v":{"$error":"#N/A"}}]
[0,{"$f":"INDEX('Import data'!$A:$A,MATCH($A2272,'Import data'!$A:$A,0),1)","v":{"$error":"#N/A"}}]
[0,{"$f":"INDEX('Import data'!$A:$A,MATCH($A2273,'Import data'!$A:$A,0),1)","v":{"$error":"#N/A"}}]
[0,{"$f":"INDEX('Import data'!$A:$A,MATCH($A2274,'Import data'!$A:$A,0),1)","v":{"$error":"#N/A"}}]
[0,{"$f":"INDEX('Import data'!$A:$A,MATCH($A2275,'Import data'!$A:$A,0),1)","v":{"$error":"#N/A"}}]
[0,{"$f":"INDEX('Import data'!$A:$A,MATCH($A2276,'Import data'!$A:$A,0),1)","v":{"$error":"#N/A"}}]
[0,{"$f":"INDEX('Import data'!$A:$A,MATCH($A2277,'Import data'!$A:$A,0),1)","v":{"$error":"#N/A"}}]
[0,{"$f":"INDEX('Import data'!$A:$A,MATCH($A2278,'Import data'!$A:$A,0),1)","v":{"$error":"#N/A"}}]
[0,{"$f":"INDEX('Import data'!$A:$A,MATCH($A2279,'Import data'!$A:$A,0),1)","v":{"$error":"#N/A"}}]
[0,{"$f":"INDEX('Import data'!$A:$A,MATCH($A2280,'Import data'!$A:$A,0),1)","v":{"$error":"#N/A"}}]
[0,{"$f":"INDEX('Import data'!$A:$A,MATCH($A2281,'Import data'!$A:$A,0),1)","v":{"$error":"#N/A"}}]
[0,{"$f":"INDEX('Import data'!$A:$A,MATCH($A2282,'Import data'!$A:$A,0),1)","v":{"$error":"#N/A"}}]
[0,{"$f":"INDEX('Import data'!$A:$A,MATCH($A2283,'Import data'!$A:$A,0),1)","v":{"$error":"#N/A"}}]
[0,{"$f":"INDEX('Import data'!$A:$A,MATCH($A2284,'Import data'!$A:$A,0),1)","v":{"$error":"#N/A"}}]
[0,{"$f":"INDEX('Import data'!$A:$A,MATCH($A2285,'Import data'!$A:$A,0),1)","v":{"$error":"#N/A"}}]
[0,{"$f":"INDEX('Import data'!$A:$A,MATCH($A2286,'Import data'!$A:$A,0),1)","v":{"$error":"#N/A"}}]
[0,{"$f":"INDEX('Import data'!$A:$A,MATCH($A2287,'Import data'!$A:$A,0),1)","v":{"$error":"#N/A"}}]
[0,{"$f":"INDEX('Import data'!$A:$A,MATCH($A2288,'Import data'!$A:$A,0),1)","v":{"$error":"#N/A"}}]
[0,{"$f":"INDEX('Import data'!$A:$A,MATCH($A2289,'Import data'!$A:$A,0),1)","v":{"$error":"#N/A"}}]
[0,{"$f":"INDEX('Import data'!$A:$A,MATCH($A2290,'Import data'!$A:$A,0),1)","v":{"$error":"#N/A"}}]
[0,{"$f":"INDEX('Import data'!$A:$A,MATCH($A2291,'Import data'!$A:$A,0),1)","v":{"$error":"#N/A"}}]
[0,{"$f":"INDEX('Import data'!$A:$A,MATCH($A2292,'Import data'!$A:$A,0),1)","v":{"$error":"#N/A"}}]
[0,{"$f":"INDEX('Import data'!$A:$A,MATCH($A2293,'Import data'!$A:$A,0),1)","v":{"$error":"#N/A"}}]
[0,{"$f":"INDEX('Import data'!$A:$A,MATCH($A2294,'Import data'!$A:$A,0),1)","v":{"$error":"#N/A"}}]
[0,{"$f":"INDEX('Import data'!$A:$A,MATCH($A2295,'Import data'!$A:$A,0),1)","v":{"$error":"#N/A"}}]
[0,{"$f":"INDEX('Import data'!$A:$A,MATCH($A2296,'Import data'!$A:$A,0),1)","v":{"$error":"#N/A"}}]
[0,{"$f":"INDEX('Import data'!$A:$A,MATCH($A2297,'Import data'!$A:$A,0),1)","v":{"$error":"#N/A"}}]
[0,{"$f":"INDEX('Import data'!$A:$A,MATCH($A2298,'Import data'!$A:$A,0),1)","v":{"$error":"#N/A"}}]
[0,{"$f":"INDEX('Import data'!$A:$A,MATCH($A2299,'Import data'!$A:$A,0),1)","v":{"$error":"#N/A"}}]
[0,{"$f":"INDEX('Import data'!$A:$A,MATCH($A2300,'Import data'!$A:$A,0),1)","v":{"$error":"#N/A"}}]
[0,{"$f":"INDEX('Import data'!$A:$A,MATCH($A2301,'Import data'!$A:$A,0),1)","v":{"$error":"#N/A"}}]
[0,{"$f":"INDEX('Import data'!$A:$A,MATCH($A2302,'Import data'!$A:$A,0),1)","v":{"$error":"#N/A"}}]
[0,{"$f":"INDEX('Import data'!$A:$A,MATCH($A2303,'Import data'!$A:$A,0),1)","v":{"$error":"#N/A"}}]
[0,{"$f":"INDEX('Import data'!$A:$A,MATCH($A2304,'Import data'!$A:$A,0),1)","v":{"$error":"#N/A"}}]
[0,{"$f":"INDEX('Import data'!$A:$A,MATCH($A2305,'Import data'!$A:$A,0),1)","v":{"$error":"#N/A"}}]
[0,{"$f":"INDEX('Import data'!$A:$A,MATCH($A2306,'Import data'!$A:$A,0),1)","v":{"$error":"#N/A"}}]
[{"$f":"ID","v":0},{"$f":"INDEX('Import data'!$A:$A,MATCH($A2307,'Import data'!$A:$A,0),1)","v":{"$error":"#N/A"}}]
[0,{"$f":"INDEX('Import data'!$A:$A,MATCH($A2308,'Import data'!$A:$A,0),1)","v":{"$error":"#N/A"}}]
[0,{"$f":"INDEX('Import data'!$A:$A,MATCH($A2309,'Import data'!$A:$A,0),1)","v":{"$error":"#N/A"}}]
[0,{"$f":"INDEX('Import data'!$A:$A,MATCH($A2310,'Import data'!$A:$A,0),1)","v":{"$error":"#N/A"}}]
[0,{"$f":"INDEX('Import data'!$A:$A,MATCH($A2311,'Import data'!$A:$A,0),1)","v":{"$error":"#N/A"}}]
[0,{"$f":"INDEX('Import data'!$A:$A,MATCH($A2312,'Import data'!$A:$A,0),1)","v":{"$error":"#N/A"}}]
[0,{"$f":"INDEX('Import data'!$A:$A,MATCH($A2313,'Import data'!$A:$A,0),1)","v":{"$error":"#N/A"}}]
[0,{"$f":"INDEX('Import data'!$A:$A,MATCH($A2314,'Import data'!$A:$A,0),1)","v":{"$error":"#N/A"}}]
[0,{"$f":"INDEX('Import data'!$A:$A,MATCH($A2315,'Import data'!$A:$A,0),1)","v":{"$error":"#N/A"}}]
[0,{"$f":"INDEX('Import data'!$A:$A,MATCH($A2316,'Import data'!$A:$A,0),1)","v":{"$error":"#N/A"}}]
[0,{"$f":"INDEX('Import data'!$A:$A,MATCH($A2317,'Import data'!$A:$A,0),1)","v":{"$error":"#N/A"}}]
[0,{"$f":"INDEX('Import data'!$A:$A,MATCH($A2318,'Import data'!$A:$A,0),1)","v":{"$error":"#N/A"}}]
[0,{"$f":"INDEX('Import data'!$A:$A,MATCH($A2319,'Import data'!$A:$A,0),1)","v":{"$error":"#N/A"}}]
[0,{"$f":"INDEX('Import data'!$A:$A,MATCH($A2320,'Import data'!$A:$A,0),1)","v":{"$error":"#N/A"}}]
[0,{"$f":"INDEX('Import data'!$A:$A,MATCH($A2321,'Import data'!$A:$A,0),1)","v":{"$error":"#N/A"}}]
[0,{"$f":"INDEX('Import data'!$A:$A,MATCH($A2322,'Import data'!$A:$A,0),1)","v":{"$error":"#N/A"}}]
[0,{"$f":"INDEX('Import data'!$A:$A,MATCH($A2323,'Import data'!$A:$A,0),1)","v":{"$error":"#N/A"}}]
[0,{"$f":"INDEX('Import data'!$A:$A,MATCH($A2324,'Import data'!$A:$A,0),1)","v":{"$error":"#N/A"}}]
[0,{"$f":"INDEX('Import data'!$A:$A,MATCH($A2325,'Import data'!$A:$A,0),1)","v":{"$error":"#N/A"}}]
[0,{"$f":"INDEX('Import data'!$A:$A,MATCH($A2326,'Import data'!$A:$A,0),1)","v":{"$error":"#N/A"}}]
[0,{"$f":"INDEX('Import data'!$A:$A,MATCH($A2327,'Import data'!$A:$A,0),1)","v":{"$error":"#N/A"}}]
[0,{"$f":"INDEX('Import data'!$A:$A,MATCH($A2328,'Import data'!$A:$A,0),1)","v":{"$error":"#N/A"}}]
[0,{"$f":"INDEX('Import data'!$A:$A,MATCH($A2329,'Import data'!$A:$A,0),1)","v":{"$error":"#N/A"}}]
[0,{"$f":"INDEX('Import data'!$A:$A,MATCH($A2330,'Import data'!$A:$A,0),1)","v":{"$error":"#N/A"}}]
[0,{"$f":"INDEX('Import data'!$A:$A,MATCH($A2331,'Import data'!$A:$A,0),1)","v":{"$error":"#N/A"}}]
[0,{"$f":"INDEX('Import data'!$A:$A,MATCH($A2332,'Import data'!$A:$A,0),1)","v":{"$error":"#N/A"}}]
[0,{"$f":"INDEX('Import data'!$A:$A,MATCH($A2333,'Import data'!$A:$A,0),1)","v":{"$error":"#N/A"}}]
[0,{"$f":"INDEX('Import data'!$A:$A,MATCH($A2334,'Import data'!$A:$A,0),1)","v":{"$error":"#N/A"}}]
[0,{"$f":"INDEX('Import data'!$A:$A,MATCH($A2335,'Import data'!$A:$A,0),1)","v":{"$error":"#N/A"}}]
[0,{"$f":"INDEX('Import data'!$A:$A,MATCH($A2336,'Import data'!$A:$A,0),1)","v":{"$error":"#N/A"}}]
[0,{"$f":"INDEX('Import data'!$A:$A,MATCH($A2337,'Import data'!$A:$A,0),1)","v":{"$error":"#N/A"}}]
[0,{"$f":"INDEX('Import data'!$A:$A,MATCH($A2338,'Import data'!$A:$A,0),1)","v":{"$error":"#N/A"}}]
[0,{"$f":"INDEX('Import data'!$A:$A,MATCH($A2339,'Import data'!$A:$A,0),1)","v":{"$error":"#N/A"}}]
[0,{"$f":"INDEX('Import data'!$A:$A,MATCH($A2340,'Import data'!$A:$A,0),1)","v":{"$error":"#N/A"}}]
[0,{"$f":"INDEX('Import data'!$A:$A,MATCH($A2341,'Import data'!$A:$A,0),1)","v":{"$error":"#N/A"}}]
[0,{"$f":"INDEX('Import data'!$A:$A,MATCH($A2342,'Import data'!$A:$A,0),1)","v":{"$error":"#N/A"}}]
[0,{"$f":"INDEX('Import data'!$A:$A,MATCH($A2343,'Import data'!$A:$A,0),1)","v":{"$error":"#N/A"}}]
[0,{"$f":"INDEX('Import data'!$A:$A,MATCH($A2344,'Import data'!$A:$A,0),1)","v":{"$error":"#N/A"}}]
[0,{"$f":"INDEX('Import data'!$A:$A,MATCH($A2345,'Import data'!$A:$A,0),1)","v":{"$error":"#N/A"}}]
[0,{"$f":"INDEX('Import data'!$A:$A,MATCH($A2346,'Import data'!$A:$A,0),1)","v":{"$error":"#N/A"}}]
[0,{"$f":"INDEX('Import data'!$A:$A,MATCH($A2347,'Import data'!$A:$A,0),1)","v":{"$error":"#N/A"}}]
[0,{"$f":"INDEX('Import data'!$A:$A,MATCH($A2348,'Import data'!$A:$A,0),1)","v":{"$error":"#N/A"}}]
[0,{"$f":"INDEX('Import data'!$A:$A,MATCH($A2349,'Import data'!$A:$A,0),1)","v":{"$error":"#N/A"}}]
[0,{"$f":"INDEX('Import data'!$A:$A,MATCH($A2350,'Import data'!$A:$A,0),1)","v":{"$error":"#N/A"}}]
[0,{"$f":"INDEX('Import data'!$A:$A,MATCH($A2351,'Import data'!$A:$A,0),1)","v":{"$error":"#N/A"}}]
[0,{"$f":"INDEX('Import data'!$A:$A,MATCH($A2352,'Import data'!$A:$A,0),1)","v":{"$error":"#N/A"}}]
[0,{"$f":"INDEX('Import data'!$A:$A,MATCH($A2353,'Import data'!$A:$A,0),1)","v":{"$error":"#N/A"}}]
[0,{"$f":"INDEX('Import data'!$A:$A,MATCH($A2354,'Import data'!$A:$A,0),1)","v":{"$error":"#N/A"}}]
[0,{"$f":"INDEX('Import data'!$A:$A,MATCH($A2355,'Import data'!$A:$A,0),1)","v":{"$error":"#N/A"}}]
[0,{"$f":"INDEX('Import data'!$A:$A,MATCH($A2356,'Import data'!$A:$A,0),1)","v":{"$error":"#N/A"}}]
[0,{"$f":"INDEX('Import data'!$A:$A,MATCH($A2357,'Import data'!$A:$A,0),1)","v":{"$error":"#N/A"}}]
[0,{"$f":"INDEX('Import data'!$A:$A,MATCH($A2358,'Import data'!$A:$A,0),1)","v":{"$error":"#N/A"}}]
[0,{"$f":"INDEX('Import data'!$A:$A,MATCH($A2359,'Import data'!$A:$A,0),1)","v":{"$error":"#N/A"}}]
[0,{"$f":"INDEX('Import data'!$A:$A,MATCH($A2360,'Import data'!$A:$A,0),1)","v":{"$error":"#N/A"}}]
[0,{"$f":"INDEX('Import data'!$A:$A,MATCH($A2361,'Import data'!$A:$A,0),1)","v":{"$error":"#N/A"}}]
[0,{"$f":"INDEX('Import data'!$A:$A,MATCH($A2362,'Import data'!$A:$A,0),1)","v":{"$error":"#N/A"}}]
[0,{"$f":"INDEX('Import data'!$A:$A,MATCH($A2363,'Import data'!$A:$A,0),1)","v":{"$error":"#N/A"}}]
[0,{"$f":"INDEX('Import data'!$A:$A,MATCH($A2364,'Import data'!$A:$A,0),1)","v":{"$error":"#N/A"}}]
[0,{"$f":"INDEX('Import data'!$A:$A,MATCH($A2365,'Import data'!$A:$A,0),1)","v":{"$error":"#N/A"}}]
[0,{"$f":"INDEX('Import data'!$A:$A,MATCH($A2366,'Import data'!$A:$A,0),1)","v":{"$error":"#N/A"}}]
[0,{"$f":"INDEX('Import data'!$A:$A,MATCH($A2367,'Import data'!$A:$A,0),1)","v":{"$error":"#N/A"}}]
[0,{"$f":"INDEX('Import data'!$A:$A,MATCH($A2368,'Import data'!$A:$A,0),1)","v":{"$error":"#N/A"}}]
[0,{"$f":"INDEX('Import data'!$A:$A,MATCH($A2369,'Import data'!$A:$A,0),1)","v":{"$error":"#N/A"}}]
[0,{"$f":"INDEX('Import data'!$A:$A,MATCH($A2370,'Import data'!$A:$A,0),1)","v":{"$error":"#N/A"}}]
[{"$f":"ID","v":0},{"$f":"INDEX('Import data'!$A:$A,MATCH($A2371,'Import data'!$A:$A,0),1)","v":{"$error":"#N/A"}}]
[0,{"$f":"INDEX('Import data'!$A:$A,MATCH($A2372,'Import data'!$A:$A,0),1)","v":{"$error":"#N/A"}}]
[0,{"$f":"INDEX('Import data'!$A:$A,MATCH($A2373,'Import data'!$A:$A,0),1)","v":{"$error":"#N/A"}}]
[0,{"$f":"INDEX('Import data'!$A:$A,MATCH($A2374,'Import data'!$A:$A,0),1)","v":{"$error":"#N/A"}}]
[0,{"$f":"INDEX('Import data'!$A:$A,MATCH($A2375,'Import data'!$A:$A,0),1)","v":{"$error":"#N/A"}}]
[0,{"$f":"INDEX('Import data'!$A:$A,MATCH($A2376,'Import data'!$A:$A,0),1)","v":{"$error":"#N/A"}}]
[0,{"$f":"INDEX('Import data'!$A:$A,MATCH($A2377,'Import data'!$A:$A,0),1)","v":{"$error":"#N/A"}}]
[0,{"$f":"INDEX('Import data'!$A:$A,MATCH($A2378,'Import data'!$A:$A,0),1)","v":{"$error":"#N/A"}}]
[0,{"$f":"INDEX('Import data'!$A:$A,MATCH($A2379,'Import data'!$A:$A,0),1)","v":{"$error":"#N/A"}}]
[0,{"$f":"INDEX('Import data'!$A:$A,MATCH($A2380,'Import data'!$A:$A,0),1)","v":{"$error":"#N/A"}}]
[0,{"$f":"INDEX('Import data'!$A:$A,MATCH($A2381,'Import data'!$A:$A,0),1)","v":{"$error":"#N/A"}}]
[0,{"$f":"INDEX('Import data'!$A:$A,MATCH($A2382,'Import data'!$A:$A,0),1)","v":{"$error":"#N/A"}}]
[0,{"$f":"INDEX('Import data'!$A:$A,MATCH($A2383,'Import data'!$A:$A,0),1)","v":{"$error":"#N/A"}}]
[0,{"$f":"INDEX('Import data'!$A:$A,MATCH($A2384,'Import data'!$A:$A,0),1)","v":{"$error":"#N/A"}}]
[0,{"$f":"INDEX('Import data'!$A:$A,MATCH($A2385,'Import data'!$A:$A,0),1)","v":{"$error":"#N/A"}}]
[0,{"$f":"INDEX('Import data'!$A:$A,MATCH($A2386,'Import data'!$A:$A,0),1)","v":{"$error":"#N/A"}}]
[0,{"$f":"INDEX('Import data'!$A:$A,MATCH($A2387,'Import data'!$A:$A,0),1)","v":{"$error":"#N/A"}}]
[0,{"$f":"INDEX('Import data'!$A:$A,MATCH($A2388,'Import data'!$A:$A,0),1)","v":{"$error":"#N/A"}}]
[0,{"$f":"INDEX('Import data'!$A:$A,MATCH($A2389,'Import data'!$A:$A,0),1)","v":{"$error":"#N/A"}}]
[0,{"$f":"INDEX('Import data'!$A:$A,MATCH($A2390,'Import data'!$A:$A,0),1)","v":{"$error":"#N/A"}}]
[0,{"$f":"INDEX('Import data'!$A:$A,MATCH($A2391,'Import data'!$A:$A,0),1)","v":{"$error":"#N/A"}}]
[0,{"$f":"INDEX('Import data'!$A:$A,MATCH($A2392,'Import data'!$A:$A,0),1)","v":{"$error":"#N/A"}}]
[0,{"$f":"INDEX('Import data'!$A:$A,MATCH($A2393,'Import data'!$A:$A,0),1)","v":{"$error":"#N/A"}}]
[0,{"$f":"INDEX('Import data'!$A:$A,MATCH($A2394,'Import data'!$A:$A,0),1)","v":{"$error":"#N/A"}}]
[0,{"$f":"INDEX('Import data'!$A:$A,MATCH($A2395,'Import data'!$A:$A,0),1)","v":{"$error":"#N/A"}}]
[0,{"$f":"INDEX('Import data'!$A:$A,MATCH($A2396,'Import data'!$A:$A,0),1)","v":{"$error":"#N/A"}}]
[0,{"$f":"INDEX('Import data'!$A:$A,MATCH($A2397,'Import data'!$A:$A,0),1)","v":{"$error":"#N/A"}}]
[0,{"$f":"INDEX('Import data'!$A:$A,MATCH($A2398,'Import data'!$A:$A,0),1)","v":{"$error":"#N/A"}}]
[0,{"$f":"INDEX('Import data'!$A:$A,MATCH($A2399,'Import data'!$A:$A,0),1)","v":{"$error":"#N/A"}}]
[0,{"$f":"INDEX('Import data'!$A:$A,MATCH($A2400,'Import data'!$A:$A,0),1)","v":{"$error":"#N/A"}}]
[0,{"$f":"INDEX('Import data'!$A:$A,MATCH($A2401,'Import data'!$A:$A,0),1)","v":{"$error":"#N/A"}}]
[0,{"$f":"INDEX('Import data'!$A:$A,MATCH($A2402,'Import data'!$A:$A,0),1)","v":{"$error":"#N/A"}}]
[0,{"$f":"INDEX('Import data'!$A:$A,MATCH($A2403,'Import data'!$A:$A,0),1)","v":{"$error":"#N/A"}}]
[0,{"$f":"INDEX('Import data'!$A:$A,MATCH($A2404,'Import data'!$A:$A,0),1)","v":{"$error":"#N/A"}}]
[0,{"$f":"INDEX('Import data'!$A:$A,MATCH($A2405,'Import data'!$A:$A,0),1)","v":{"$error":"#N/A"}}]
[0,{"$f":"INDEX('Import data'!$A:$A,MATCH($A2406,'Import data'!$A:$A,0),1)","v":{"$error":"#N/A"}}]
[0,{"$f":"INDEX('Import data'!$A:$A,MATCH($A2407,'Import data'!$A:$A,0),1)","v":{"$error":"#N/A"}}]
[0,{"$f":"INDEX('Import data'!$A:$A,MATCH($A2408,'Import data'!$A:$A,0),1)","v":{"$error":"#N/A"}}]
[0,{"$f":"INDEX('Import data'!$A:$A,MATCH($A2409,'Import data'!$A:$A,0),1)","v":{"$error":"#N/A"}}]
[0,{"$f":"INDEX('Import data'!$A:$A,MATCH($A2410,'Import data'!$A:$A,0),1)","v":{"$error":"#N/A"}}]
[0,{"$f":"INDEX('Import data'!$A:$A,MATCH($A2411,'Import data'!$A:$A,0),1)","v":{"$error":"#N/A"}}]
[0,{"$f":"INDEX('Import data'!$A:$A,MATCH($A2412,'Import data'!$A:$A,0),1)","v":{"$error":"#N/A"}}]
[0,{"$f":"INDEX('Import data'!$A:$A,MATCH($A2413,'Import data'!$A:$A,0),1)","v":{"$error":"#N/A"}}]
[0,{"$f":"INDEX('Import data'!$A:$A,MATCH($A2414,'Import data'!$A:$A,0),1)","v":{"$error":"#N/A"}}]
[0,{"$f":"INDEX('Import data'!$A:$A,MATCH($A2415,'Import data'!$A:$A,0),1)","v":{"$error":"#N/A"}}]
[0,{"$f":"INDEX('Import data'!$A:$A,MATCH($A2416,'Import data'!$A:$A,0),1)","v":{"$error":"#N/A"}}]
[0,{"$f":"INDEX('Import data'!$A:$A,MATCH($A2417,'Import data'!$A:$A,0),1)","v":{"$error":"#N/A"}}]
[0,{"$f":"INDEX('Import data'!$A:$A,MATCH($A2418,'Import data'!$A:$A,0),1)","v":{"$error":"#N/A"}}]
[0,{"$f":"INDEX('Import data'!$A:$A,MATCH($A2419,'Import data'!$A:$A,0),1)","v":{"$error":"#N/A"}}]
[0,{"$f":"INDEX('Import data'!$A:$A,MATCH($A2420,'Import data'!$A:$A,0),1)","v":{"$error":"#N/A"}}]
[0,{"$f":"INDEX('Import data'!$A:$A,MATCH($A2421,'Import data'!$A:$A,0),1)","v":{"$error":"#N/A"}}]
[0,{"$f":"INDEX('Import data'!$A:$A,MATCH($A2422,'Import data'!$A:$A,0),1)","v":{"$error":"#N/A"}}]
[0,{"$f":"INDEX('Import data'!$A:$A,MATCH($A2423,'Import data'!$A:$A,0),1)","v":{"$error":"#N/A"}}]
[0,{"$f":"INDEX('Import data'!$A:$A,MATCH($A2424,'Import data'!$A:$A,0),1)","v":{"$error":"#N/A"}}]
[0,{"$f":"INDEX('Import data'!$A:$A,MATCH($A2425,'Import data'!$A:$A,0),1)","v":{"$error":"#N/A"}}]
[0,{"$f":"INDEX('Import data'!$A:$A,MATCH($A2426,'Import data'!$A:$A,0),1)","v":{"$error":"#N/A"}}]
[0,{"$f":"INDEX('Import data'!$A:$A,MATCH($A2427,'Import data'!$A:$A,0),1)","v":{"$error":"#N/A"}}]
[0,{"$f":"INDEX('Import data'!$A:$A,MATCH($A2428,'Import data'!$A:$A,0),1)","v":{"$error":"#N/A"}}]
[0,{"$f":"INDEX('Import data'!$A:$A,MATCH($A2429,'Import data'!$A:$A,0),1)","v":{"$error":"#N/A"}}]
[0,{"$f":"INDEX('Import data'!$A:$A,MATCH($A2430,'Import data'!$A:$A,0),1)","v":{"$error":"#N/A"}}]
[0,{"$f":"INDEX('Import data'!$A:$A,MATCH($A2431,'Import data'!$A:$A,0),1)","v":{"$error":"#N/A"}}]
[0,{"$f":"INDEX('Import data'!$A:$A,MATCH($A2432,'Import data'!$A:$A,0),1)","v":{"$error":"#N/A"}}]
[0,{"$f":"INDEX('Import data'!$A:$A,MATCH($A2433,'Import data'!$A:$A,0),1)","v":{"$error":"#N/A"}}]
[0,{"$f":"INDEX('Import data'!$A:$A,MATCH($A2434,'Import data'!$A:$A,0),1)","v":{"$error":"#N/A"}}]
[{"$f":"ID","v":0},{"$f":"INDEX('Import data'!$A:$A,MATCH($A2435,'Import data'!$A:$A,0),1)","v":{"$error":"#N/A"}}]
[0,{"$f":"INDEX('Import data'!$A:$A,MATCH($A2436,'Import data'!$A:$A,0),1)","v":{"$error":"#N/A"}}]
[0,{"$f":"INDEX('Import data'!$A:$A,MATCH($A2437,'Import data'!$A:$A,0),1)","v":{"$error":"#N/A"}}]
[0,{"$f":"INDEX('Import data'!$A:$A,MATCH($A2438,'Import data'!$A:$A,0),1)","v":{"$error":"#N/A"}}]
[0,{"$f":"INDEX('Import data'!$A:$A,MATCH($A2439,'Import data'!$A:$A,0),1)","v":{"$error":"#N/A"}}]
[0,{"$f":"INDEX('Import data'!$A:$A,MATCH($A2440,'Import data'!$A:$A,0),1)","v":{"$error":"#N/A"}}]
[0,{"$f":"INDEX('Import data'!$A:$A,MATCH($A2441,'Import data'!$A:$A,0),1)","v":{"$error":"#N/A"}}]
[0,{"$f":"INDEX('Import data'!$A:$A,MATCH($A2442,'Import data'!$A:$A,0),1)","v":{"$error":"#N/A"}}]
[0,{"$f":"INDEX('Import data'!$A:$A,MATCH($A2443,'Import data'!$A:$A,0),1)","v":{"$error":"#N/A"}}]
[0,{"$f":"INDEX('Import data'!$A:$A,MATCH($A2444,'Import data'!$A:$A,0),1)","v":{"$error":"#N/A"}}]
[0,{"$f":"INDEX('Import data'!$A:$A,MATCH($A2445,'Import data'!$A:$A,0),1)","v":{"$error":"#N/A"}}]
[0,{"$f":"INDEX('Import data'!$A:$A,MATCH($A2446,'Import data'!$A:$A,0),1)","v":{"$error":"#N/A"}}]
[0,{"$f":"INDEX('Import data'!$A:$A,MATCH($A2447,'Import data'!$A:$A,0),1)","v":{"$error":"#N/A"}}]
[0,{"$f":"INDEX('Import data'!$A:$A,MATCH($A2448,'Import data'!$A:$A,0),1)","v":{"$error":"#N/A"}}]
[0,{"$f":"INDEX('Import data'!$A:$A,MATCH($A2449,'Import data'!$A:$A,0),1)","v":{"$error":"#N/A"}}]
[0,{"$f":"INDEX('Import data'!$A:$A,MATCH($A2450,'Import data'!$A:$A,0),1)","v":{"$error":"#N/A"}}]
[0,{"$f":"INDEX('Import data'!$A:$A,MATCH($A2451,'Import data'!$A:$A,0),1)","v":{"$error":"#N/A"}}]
[0,{"$f":"INDEX('Import data'!$A:$A,MATCH($A2452,'Import data'!$A:$A,0),1)","v":{"$error":"#N/A"}}]
[0,{"$f":"INDEX('Import data'!$A:$A,MATCH($A2453,'Import data'!$A:$A,0),1)","v":{"$error":"#N/A"}}]
[0,{"$f":"INDEX('Import data'!$A:$A,MATCH($A2454,'Import data'!$A:$A,0),1)","v":{"$error":"#N/A"}}]
[0,{"$f":"INDEX('Import data'!$A:$A,MATCH($A2455,'Import data'!$A:$A,0),1)","v":{"$error":"#N/A"}}]
[0,{"$f":"INDEX('Import data'!$A:$A,MATCH($A2456,'Import data'!$A:$A,0),1)","v":{"$error":"#N/A"}}]
[0,{"$f":"INDEX('Import data'!$A:$A,MATCH($A2457,'Import data'!$A:$A,0),1)","v":{"$error":"#N/A"}}]
[0,{"$f":"INDEX('Import data'!$A:$A,MATCH($A2458,'Import data'!$A:$A,0),1)","v":{"$error":"#N/A"}}]
[0,{"$f":"INDEX('Import data'!$A:$A,MATCH($A2459,'Import data'!$A:$A,0),1)","v":{"$error":"#N/A"}}]
[0,{"$f":"INDEX('Import data'!$A:$A,MATCH($A2460,'Import data'!$A:$A,0),1)","v":{"$error":"#N/A"}}]
[0,{"$f":"INDEX('Import data'!$A:$A,MATCH($A2461,'Import data'!$A:$A,0),1)","v":{"$error":"#N/A"}}]
[0,{"$f":"INDEX('Import data'!$A:$A,MATCH($A2462,'Import data'!$A:$A,0),1)","v":{"$error":"#N/A"}}]
[0,{"$f":"INDEX('Import data'!$A:$A,MATCH($A2463,'Import data'!$A:$A,0),1)","v":{"$error":"#N/A"}}]
[0,{"$f":"INDEX('Import data'!$A:$A,MATCH($A2464,'Import data'!$A:$A,0),1)","v":{"$error":"#N/A"}}]
[0,{"$f":"INDEX('Import data'!$A:$A,MATCH($A2465,'Import data'!$A:$A,0),1)","v":{"$error":"#N/A"}}]
[0,{"$f":"INDEX('Import data'!$A:$A,MATCH($A2466,'Import data'!$A:$A,0),1)","v":{"$error":"#N/A"}}]
[0,{"$f":"INDEX('Import data'!$A:$A,MATCH($A2467,'Import data'!$A:$A,0),1)","v":{"$error":"#N/A"}}]
[0,{"$f":"INDEX('Import data'!$A:$A,MATCH($A2468,'Import data'!$A:$A,0),1)","v":{"$error":"#N/A"}}]
[0,{"$f":"INDEX('Import data'!$A:$A,MATCH($A2469,'Import data'!$A:$A,0),1)","v":{"$error":"#N/A"}}]
[0,{"$f":"INDEX('Import data'!$A:$A,MATCH($A2470,'Import data'!$A:$A,0),1)","v":{"$error":"#N/A"}}]
[0,{"$f":"INDEX('Import data'!$A:$A,MATCH($A2471,'Import data'!$A:$A,0),1)","v":{"$error":"#N/A"}}]
[0,{"$f":"INDEX('Import data'!$A:$A,MATCH($A2472,'Import data'!$A:$A,0),1)","v":{"$error":"#N/A"}}]
[0,{"$f":"INDEX('Import data'!$A:$A,MATCH($A2473,'Import data'!$A:$A,0),1)","v":{"$error":"#N/A"}}]
[0,{"$f":"INDEX('Import data'!$A:$A,MATCH($A2474,'Import data'!$A:$A,0),1)","v":{"$error":"#N/A"}}]
[0,{"$f":"INDEX('Import data'!$A:$A,MATCH($A2475,'Import data'!$A:$A,0),1)","v":{"$error":"#N/A"}}]
[0,{"$f":"INDEX('Import data'!$A:$A,MATCH($A2476,'Import data'!$A:$A,0),1)","v":{"$error":"#N/A"}}]
[0,{"$f":"INDEX('Import data'!$A:$A,MATCH($A2477,'Import data'!$A:$A,0),1)","v":{"$error":"#N/A"}}]
[0,{"$f":"INDEX('Import data'!$A:$A,MATCH($A2478,'Import data'!$A:$A,0),1)","v":{"$error":"#N/A"}}]
[0,{"$f":"INDEX('Import data'!$A:$A,MATCH($A2479,'Import data'!$A:$A,0),1)","v":{"$error":"#N/A"}}]
[0,{"$f":"INDEX('Import data'!$A:$A,MATCH($A2480,'Import data'!$A:$A,0),1)","v":{"$error":"#N/A"}}]
[0,{"$f":"INDEX('Import data'!$A:$A,MATCH($A2481,'Import data'!$A:$A,0),1)","v":{"$error":"#N/A"}}]
[0,{"$f":"INDEX('Import data'!$A:$A,MATCH($A2482,'Import data'!$A:$A,0),1)","v":{"$error":"#N/A"}}]
[0,{"$f":"INDEX('Import data'!$A:$A,MATCH($A2483,'Import data'!$A:$A,0),1)","v":{"$error":"#N/A"}}]
[0,{"$f":"INDEX('Import data'!$A:$A,MATCH($A2484,'Import data'!$A:$A,0),1)","v":{"$error":"#N/A"}}]
[0,{"$f":"INDEX('Import data'!$A:$A,MATCH($A2485,'Import data'!$A:$A,0),1)","v":{"$error":"#N/A"}}]
[0,{"$f":"INDEX('Import data'!$A:$A,MATCH($A2486,'Import data'!$A:$A,0),1)","v":{"$error":"#N/A"}}]
[0,{"$f":"INDEX('Import data'!$A:$A,MATCH($A2487,'Import data'!$A:$A,0),1)","v":{"$error":"#N/A"}}]
[0,{"$f":"INDEX('Import data'!$A:$A,MATCH($A2488,'Import data'!$A:$A,0),1)","v":{"$error":"#N/A"}}]
[0,{"$f":"INDEX('Import data'!$A:$A,MATCH($A2489,'Import data'!$A:$A,0),1)","v":{"$error":"#N/A"}}]
[0,{"$f":"INDEX('Import data'!$A:$A,MATCH($A2490,'Import data'!$A:$A,0),1)","v":{"$error":"#N/A"}}]
[0,{"$f":"INDEX('Import data'!$A:$A,MATCH($A2491,'Import data'!$A:$A,0),1)","v":{"$error":"#N/A"}}]
[0,{"$f":"INDEX('Import data'!$A:$A,MATCH($A2492,'Import data'!$A:$A,0),1)","v":{"$error":"#N/A"}}]
[0,{"$f":"INDEX('Import data'!$A:$A,MATCH($A2493,'Import data'!$A:$A,0),1)","v":{"$error":"#N/A"}}]
[0,{"$f":"INDEX('Import data'!$A:$A,MATCH($A2494,'Import data'!$A:$A,0),1)","v":{"$error":"#N/A"}}]
[0,{"$f":"INDEX('Import data'!$A:$A,MATCH($A2495,'Import data'!$A:$A,0),1)","v":{"$error":"#N/A"}}]
[0,{"$f":"INDEX('Import data'!$A:$A,MATCH($A2496,'Import data'!$A:$A,0),1)","v":{"$error":"#N/A"}}]
[0,{"$f":"INDEX('Import data'!$A:$A,MATCH($A2497,'Import data'!$A:$A,0),1)","v":{"$error":"#N/A"}}]
[0,{"$f":"INDEX('Import data'!$A:$A,MATCH($A2498,'Import data'!$A:$A,0),1)","v":{"$error":"#N/A"}}]
[{"$f":"ID","v":0},{"$f":"INDEX('Import data'!$A:$A,MATCH($A2499,'Import data'!$A:$A,0),1)","v":{"$error":"#N/A"}}]
[0,{"$f":"INDEX('Import data'!$A:$A,MATCH($A2500,'Import data'!$A:$A,0),1)","v":{"$error":"#N/A"}}]
[0,{"$f":"INDEX('Import data'!$A:$A,MATCH($A2501,'Import data'!$A:$A,0),1)","v":{"$error":"#N/A"}}]
[0,{"$f":"INDEX('Import data'!$A:$A,MATCH($A2502,'Import data'!$A:$A,0),1)","v":{"$error":"#N/A"}}]
[0,{"$f":"INDEX('Import data'!$A:$A,MATCH($A2503,'Import data'!$A:$A,0),1)","v":{"$error":"#N/A"}}]
[0,{"$f":"INDEX('Import data'!$A:$A,MATCH($A2504,'Import data'!$A:$A,0),1)","v":{"$error":"#N/A"}}]
[0,{"$f":"INDEX('Import data'!$A:$A,MATCH($A2505,'Import data'!$A:$A,0),1)","v":{"$error":"#N/A"}}]
[0,{"$f":"INDEX('Import data'!$A:$A,MATCH($A2506,'Import data'!$A:$A,0),1)","v":{"$error":"#N/A"}}]
[0,{"$f":"INDEX('Import data'!$A:$A,MATCH($A2507,'Import data'!$A:$A,0),1)","v":{"$error":"#N/A"}}]
[0,{"$f":"INDEX('Import data'!$A:$A,MATCH($A2508,'Import data'!$A:$A,0),1)","v":{"$error":"#N/A"}}]
[0,{"$f":"INDEX('Import data'!$A:$A,MATCH($A2509,'Import data'!$A:$A,0),1)","v":{"$error":"#N/A"}}]
[0,{"$f":"INDEX('Import data'!$A:$A,MATCH($A2510,'Import data'!$A:$A,0),1)","v":{"$error":"#N/A"}}]
[0,{"$f":"INDEX('Import data'!$A:$A,MATCH($A2511,'Import data'!$A:$A,0),1)","v":{"$error":"#N/A"}}]
[0,{"$f":"INDEX('Import data'!$A:$A,MATCH($A2512,'Import data'!$A:$A,0),1)","v":{"$error":"#N/A"}}]
[0,{"$f":"INDEX('Import data'!$A:$A,MATCH($A2513,'Import data'!$A:$A,0),1)","v":{"$error":"#N/A"}}]
[0,{"$f":"INDEX('Import data'!$A:$A,MATCH($A2514,'Import data'!$A:$A,0),1)","v":{"$error":"#N/A"}}]
[0,{"$f":"INDEX('Import data'!$A:$A,MATCH($A2515,'Import data'!$A:$A,0),1)","v":{"$error":"#N/A"}}]
[0,{"$f":"INDEX('Import data'!$A:$A,MATCH($A2516,'Import data'!$A:$A,0),1)","v":{"$error":"#N/A"}}]
[0,{"$f":"INDEX('Import data'!$A:$A,MATCH($A2517,'Import data'!$A:$A,0),1)","v":{"$error":"#N/A"}}]
[0,{"$f":"INDEX('Import data'!$A:$A,MATCH($A2518,'Import data'!$A:$A,0),1)","v":{"$error":"#N/A"}}]
[0,{"$f":"INDEX('Import data'!$A:$A,MATCH($A2519,'Import data'!$A:$A,0),1)","v":{"$error":"#N/A"}}]
[0,{"$f":"INDEX('Import data'!$A:$A,MATCH($A2520,'Import data'!$A:$A,0),1)","v":{"$error":"#N/A"}}]
[0,{"$f":"INDEX('Import data'!$A:$A,MATCH($A2521,'Import data'!$A:$A,0),1)","v":{"$error":"#N/A"}}]
[0,{"$f":"INDEX('Import data'!$A:$A,MATCH($A2522,'Import data'!$A:$A,0),1)","v":{"$error":"#N/A"}}]
[0,{"$f":"INDEX('Import data'!$A:$A,MATCH($A2523,'Import data'!$A:$A,0),1)","v":{"$error":"#N/A"}}]
[0,{"$f":"INDEX('Import data'!$A:$A,MATCH($A2524,'Import data'!$A:$A,0),1)","v":{"$error":"#N/A"}}]
[0,{"$f":"INDEX('Import data'!$A:$A,MATCH($A2525,'Import data'!$A:$A,0),1)","v":{"$error":"#N/A"}}]
[0,{"$f":"INDEX('Import data'!$A:$A,MATCH($A2526,'Import data'!$A:$A,0),1)","v":{"$error":"#N/A"}}]
[0,{"$f":"INDEX('Import data'!$A:$A,MATCH($A2527,'Import data'!$A:$A,0),1)","v":{"$error":"#N/A"}}]
[0,{"$f":"INDEX('Import data'!$A:$A,MATCH($A2528,'Import data'!$A:$A,0),1)","v":{"$error":"#N/A"}}]
[0,{"$f":"INDEX('Import data'!$A:$A,MATCH($A2529,'Import data'!$A:$A,0),1)","v":{"$error":"#N/A"}}]
[0,{"$f":"INDEX('Import data'!$A:$A,MATCH($A2530,'Import data'!$A:$A,0),1)","v":{"$error":"#N/A"}}]
[0,{"$f":"INDEX('Import data'!$A:$A,MATCH($A2531,'Import data'!$A:$A,0),1)","v":{"$error":"#N/A"}}]
[0,{"$f":"INDEX('Import data'!$A:$A,MATCH($A2532,'Import data'!$A:$A,0),1)","v":{"$error":"#N/A"}}]
[0,{"$f":"INDEX('Import data'!$A:$A,MATCH($A2533,'Import data'!$A:$A,0),1)","v":{"$error":"#N/A"}}]
[0,{"$f":"INDEX('Import data'!$A:$A,MATCH($A2534,'Import data'!$A:$A,0),1)","v":{"$error":"#N/A"}}]
[0,{"$f":"INDEX('Import data'!$A:$A,MATCH($A2535,'Import data'!$A:$A,0),1)","v":{"$error":"#N/A"}}]
[0,{"$f":"INDEX('Import data'!$A:$A,MATCH($A2536,'Import data'!$A:$A,0),1)","v":{"$error":"#N/A"}}]
[0,{"$f":"INDEX('Import data'!$A:$A,MATCH($A2537,'Import data'!$A:$A,0),1)","v":{"$error":"#N/A"}}]
[0,{"$f":"INDEX('Import data'!$A:$A,MATCH($A2538,'Import data'!$A:$A,0),1)","v":{"$error":"#N/A"}}]
[0,{"$f":"INDEX('Import data'!$A:$A,MATCH($A2539,'Import data'!$A:$A,0),1)","v":{"$error":"#N/A"}}]
[0,{"$f":"INDEX('Import data'!$A:$A,MATCH($A2540,'Import data'!$A:$A,0),1)","v":{"$error":"#N/A"}}]
[0,{"$f":"INDEX('Import data'!$A:$A,MATCH($A2541,'Import data'!$A:$A,0),1)","v":{"$error":"#N/A"}}]
[0,{"$f":"INDEX('Import data'!$A:$A,MATCH($A2542,'Import data'!$A:$A,0),1)","v":{"$error":"#N/A"}}]
[0,{"$f":"INDEX('Import data'!$A:$A,MATCH($A2543,'Import data'!$A:$A,0),1)","v":{"$error":"#N/A"}}]
[0,{"$f":"INDEX('Import data'!$A:$A,MATCH($A2544,'Import data'!$A:$A,0),1)","v":{"$error":"#N/A"}}]
[0,{"$f":"INDEX('Import data'!$A:$A,MATCH($A2545,'Import data'!$A:$A,0),1)","v":{"$error":"#N/A"}}]
[0,{"$f":"INDEX('Import data'!$A:$A,MATCH($A2546,'Import data'!$A:$A,0),1)","v":{"$error":"#N/A"}}]
[0,{"$f":"INDEX('Import data'!$A:$A,MATCH($A2547,'Import data'!$A:$A,0),1)","v":{"$error":"#N/A"}}]
[0,{"$f":"INDEX('Import data'!$A:$A,MATCH($A2548,'Import data'!$A:$A,0),1)","v":{"$error":"#N/A"}}]
[0,{"$f":"INDEX('Import data'!$A:$A,MATCH($A2549,'Import data'!$A:$A,0),1)","v":{"$error":"#N/A"}}]
[0,{"$f":"INDEX('Import data'!$A:$A,MATCH($A2550,'Import data'!$A:$A,0),1)","v":{"$error":"#N/A"}}]
[0,{"$f":"INDEX('Import data'!$A:$A,MATCH($A2551,'Import data'!$A:$A,0),1)","v":{"$error":"#N/A"}}]
[0,{"$f":"INDEX('Import data'!$A:$A,MATCH($A2552,'Import data'!$A:$A,0),1)","v":{"$error":"#N/A"}}]
[0,{"$f":"INDEX('Import data'!$A:$A,MATCH($A2553,'Import data'!$A:$A,0),1)","v":{"$error":"#N/A"}}]
[0,{"$f":"INDEX('Import data'!$A:$A,MATCH($A2554,'Import data'!$A:$A,0),1)","v":{"$error":"#N/A"}}]
[0,{"$f":"INDEX('Import data'!$A:$A,MATCH($A2555,'Import data'!$A:$A,0),1)","v":{"$error":"#N/A"}}]
[0,{"$f":"INDEX('Import data'!$A:$A,MATCH($A2556,'Import data'!$A:$A,0),1)","v":{"$error":"#N/A"}}]
[0,{"$f":"INDEX('Import data'!$A:$A,MATCH($A2557,'Import data'!$A:$A,0),1)","v":{"$error":"#N/A"}}]
[0,{"$f":"INDEX('Import data'!$A:$A,MATCH($A2558,'Import data'!$A:$A,0),1)","v":{"$error":"#N/A"}}]
[0,{"$f":"INDEX('Import data'!$A:$A,MATCH($A2559,'Import data'!$A:$A,0),1)","v":{"$error":"#N/A"}}]
[0,{"$f":"INDEX('Import data'!$A:$A,MATCH($A2560,'Import data'!$A:$A,0),1)","v":{"$error":"#N/A"}}]
[0,{"$f":"INDEX('Import data'!$A:$A,MATCH($A2561,'Import data'!$A:$A,0),1)","v":{"$error":"#N/A"}}]
[0,{"$f":"INDEX('Import data'!$A:$A,MATCH($A2562,'Import data'!$A:$A,0),1)","v":{"$error":"#N/A"}}]
[{"$f":"ID","v":0},{"$f":"INDEX('Import data'!$A:$A,MATCH($A2563,'Import data'!$A:$A,0),1)","v":{"$error":"#N/A"}}]
[0,{"$f":"INDEX('Import data'!$A:$A,MATCH($A2564,'Import data'!$A:$A,0),1)","v":{"$error":"#N/A"}}]
[0,{"$f":"INDEX('Import data'!$A:$A,MATCH($A2565,'Import data'!$A:$A,0),1)","v":{"$error":"#N/A"}}]
[0,{"$f":"INDEX('Import data'!$A:$A,MATCH($A2566,'Import data'!$A:$A,0),1)","v":{"$error":"#N/A"}}]
[0,{"$f":"INDEX('Import data'!$A:$A,MATCH($A2567,'Import data'!$A:$A,0),1)","v":{"$error":"#N/A"}}]
[0,{"$f":"INDEX('Import data'!$A:$A,MATCH($A2568,'Import data'!$A:$A,0),1)","v":{"$error":"#N/A"}}]
[0,{"$f":"INDEX('Import data'!$A:$A,MATCH($A2569,'Import data'!$A:$A,0),1)","v":{"$error":"#N/A"}}]
[0,{"$f":"INDEX('Import data'!$A:$A,MATCH($A2570,'Import data'!$A:$A,0),1)","v":{"$error":"#N/A"}}]
[0,{"$f":"INDEX('Import data'!$A:$A,MATCH($A2571,'Import data'!$A:$A,0),1)","v":{"$error":"#N/A"}}]
[0,{"$f":"INDEX('Import data'!$A:$A,MATCH($A2572,'Import data'!$A:$A,0),1)","v":{"$error":"#N/A"}}]
[0,{"$f":"INDEX('Import data'!$A:$A,MATCH($A2573,'Import data'!$A:$A,0),1)","v":{"$error":"#N/A"}}]
[0,{"$f":"INDEX('Import data'!$A:$A,MATCH($A2574,'Import data'!$A:$A,0),1)","v":{"$error":"#N/A"}}]
[0,{"$f":"INDEX('Import data'!$A:$A,MATCH($A2575,'Import data'!$A:$A,0),1)","v":{"$error":"#N/A"}}]
[0,{"$f":"INDEX('Import data'!$A:$A,MATCH($A2576,'Import data'!$A:$A,0),1)","v":{"$error":"#N/A"}}]
[0,{"$f":"INDEX('Import data'!$A:$A,MATCH($A2577,'Import data'!$A:$A,0),1)","v":{"$error":"#N/A"}}]
[0,{"$f":"INDEX('Import data'!$A:$A,MATCH($A2578,'Import data'!$A:$A,0),1)","v":{"$error":"#N/A"}}]
[0,{"$f":"INDEX('Import data'!$A:$A,MATCH($A2579,'Import data'!$A:$A,0),1)","v":{"$error":"#N/A"}}]
[0,{"$f":"INDEX('Import data'!$A:$A,MATCH($A2580,'Import data'!$A:$A,0),1)","v":{"$error":"#N/A"}}]
[0,{"$f":"INDEX('Import data'!$A:$A,MATCH($A2581,'Import data'!$A:$A,0),1)","v":{"$error":"#N/A"}}]
[0,{"$f":"INDEX('Import data'!$A:$A,MATCH($A2582,'Import data'!$A:$A,0),1)","v":{"$error":"#N/A"}}]
[0,{"$f":"INDEX('Import data'!$A:$A,MATCH($A2583,'Import data'!$A:$A,0),1)","v":{"$error":"#N/A"}}]
[0,{"$f":"INDEX('Import data'!$A:$A,MATCH($A2584,'Import data'!$A:$A,0),1)","v":{"$error":"#N/A"}}]
[0,{"$f":"INDEX('Import data'!$A:$A,MATCH($A2585,'Import data'!$A:$A,0),1)","v":{"$error":"#N/A"}}]
[0,{"$f":"INDEX('Import data'!$A:$A,MATCH($A2586,'Import data'!$A:$A,0),1)","v":{"$error":"#N/A"}}]
[0,{"$f":"INDEX('Import data'!$A:$A,MATCH($A2587,'Import data'!$A:$A,0),1)","v":{"$error":"#N/A"}}]
[0,{"$f":"INDEX('Import data'!$A:$A,MATCH($A2588,'Import data'!$A:$A,0),1)","v":{"$error":"#N/A"}}]
[0,{"$f":"INDEX('Import data'!$A:$A,MATCH($A2589,'Import data'!$A:$A,0),1)","v":{"$error":"#N/A"}}]
[0,{"$f":"INDEX('Import data'!$A:$A,MATCH($A2590,'Import data'!$A:$A,0),1)","v":{"$error":"#N/A"}}]
[0,{"$f":"INDEX('Import data'!$A:$A,MATCH($A2591,'Import data'!$A:$A,0),1)","v":{"$error":"#N/A"}}]
[0,{"$f":"INDEX('Import data'!$A:$A,MATCH($A2592,'Import data'!$A:$A,0),1)","v":{"$error":"#N/A"}}]
[0,{"$f":"INDEX('Import data'!$A:$A,MATCH($A2593,'Import data'!$A:$A,0),1)","v":{"$error":"#N/A"}}]
[0,{"$f":"INDEX('Import data'!$A:$A,MATCH($A2594,'Import data'!$A:$A,0),1)","v":{"$error":"#N/A"}}]
[0,{"$f":"INDEX('Import data'!$A:$A,MATCH($A2595,'Import data'!$A:$A,0),1)","v":{"$error":"#N/A"}}]
[0,{"$f":"INDEX('Import data'!$A:$A,MATCH($A2596,'Import data'!$A:$A,0),1)","v":{"$error":"#N/A"}}]
[0,{"$f":"INDEX('Import data'!$A:$A,MATCH($A2597,'Import data'!$A:$A,0),1)","v":{"$error":"#N/A"}}]
[0,{"$f":"INDEX('Import data'!$A:$A,MATCH($A2598,'Import data'!$A:$A,0),1)","v":{"$error":"#N/A"}}]
[0,{"$f":"INDEX('Import data'!$A:$A,MATCH($A2599,'Import data'!$A:$A,0),1)","v":{"$error":"#N/A"}}]
[0,{"$f":"INDEX('Import data'!$A:$A,MATCH($A2600,'Import data'!$A:$A,0),1)","v":{"$error":"#N/A"}}]
[0,{"$f":"INDEX('Import data'!$A:$A,MATCH($A2601,'Import data'!$A:$A,0),1)","v":{"$error":"#N/A"}}]
[0,{"$f":"INDEX('Import data'!$A:$A,MATCH($A2602,'Import data'!$A:$A,0),1)","v":{"$error":"#N/A"}}]
[0,{"$f":"INDEX('Import data'!$A:$A,MATCH($A2603,'Import data'!$A:$A,0),1)","v":{"$error":"#N/A"}}]
[0,{"$f":"INDEX('Import data'!$A:$A,MATCH($A2604,'Import data'!$A:$A,0),1)","v":{"$error":"#N/A"}}]
[0,{"$f":"INDEX('Import data'!$A:$A,MATCH($A2605,'Import data'!$A:$A,0),1)","v":{"$error":"#N/A"}}]
[0,{"$f":"INDEX('Import data'!$A:$A,MATCH($A2606,'Import data'!$A:$A,0),1)","v":{"$error":"#N/A"}}]
[0,{"$f":"INDEX('Import data'!$A:$A,MATCH($A2607,'Import data'!$A:$A,0),1)","v":{"$error":"#N/A"}}]
[0,{"$f":"INDEX('Import data'!$A:$A,MATCH($A2608,'Import data'!$A:$A,0),1)","v":{"$error":"#N/A"}}]
[0,{"$f":"INDEX('Import data'!$A:$A,MATCH($A2609,'Import data'!$A:$A,0),1)","v":{"$error":"#N/A"}}]
[0,{"$f":"INDEX('Import data'!$A:$A,MATCH($A2610,'Import data'!$A:$A,0),1)","v":{"$error":"#N/A"}}]
[0,{"$f":"INDEX('Import data'!$A:$A,MATCH($A2611,'Import data'!$A:$A,0),1)","v":{"$error":"#N/A"}}]
[0,{"$f":"INDEX('Import data'!$A:$A,MATCH($A2612,'Import data'!$A:$A,0),1)","v":{"$error":"#N/A"}}]
[0,{"$f":"INDEX('Import data'!$A:$A,MATCH($A2613,'Import data'!$A:$A,0),1)","v":{"$error":"#N/A"}}]
[0,{"$f":"INDEX('Import data'!$A:$A,MATCH($A2614,'Import data'!$A:$A,0),1)","v":{"$error":"#N/A"}}]
[0,{"$f":"INDEX('Import data'!$A:$A,MATCH($A2615,'Import data'!$A:$A,0),1)","v":{"$error":"#N/A"}}]
[0,{"$f":"INDEX('Import data'!$A:$A,MATCH($A2616,'Import data'!$A:$A,0),1)","v":{"$error":"#N/A"}}]
[0,{"$f":"INDEX('Import data'!$A:$A,MATCH($A2617,'Import data'!$A:$A,0),1)","v":{"$error":"#N/A"}}]
[0,{"$f":"INDEX('Import data'!$A:$A,MATCH($A2618,'Import data'!$A:$A,0),1)","v":{"$error":"#N/A"}}]
[0,{"$f":"INDEX('Import data'!$A:$A,MATCH($A2619,'Import data'!$A:$A,0),1)","v":{"$error":"#N/A"}}]
[0,{"$f":"INDEX('Import data'!$A:$A,MATCH($A2620,'Import data'!$A:$A,0),1)","v":{"$error":"#N/A"}}]
[0,{"$f":"INDEX('Import data'!$A:$A,MATCH($A2621,'Import data'!$A:$A,0),1)","v":{"$error":"#N/A"}}]
[0,{"$f":"INDEX('Import data'!$A:$A,MATCH($A2622,'Import data'!$A:$A,0),1)","v":{"$error":"#N/A"}}]
[0,{"$f":"INDEX('Import data'!$A:$A,MATCH($A2623,'Import data'!$A:$A,0),1)","v":{"$error":"#N/A"}}]
[0,{"$f":"INDEX('Import data'!$A:$A,MATCH($A2624,'Import data'!$A:$A,0),1)","v":{"$error":"#N/A"}}]
[0,{"$f":"INDEX('Import data'!$A:$A,MATCH($A2625,'Import data'!$A:$A,0),1)","v":{"$error":"#N/A"}}]
[0,{"$f":"INDEX('Import data'!$A:$A,MATCH($A2626,'Import data'!$A:$A,0),1)","v":{"$error":"#N/A"}}]
[{"$f":"ID","v":0},{"$f":"INDEX('Import data'!$A:$A,MATCH($A2627,'Import data'!$A:$A,0),1)","v":{"$error":"#N/A"}}]
[0,{"$f":"INDEX('Import data'!$A:$A,MATCH($A2628,'Import data'!$A:$A,0),1)","v":{"$error":"#N/A"}}]
[0,{"$f":"INDEX('Import data'!$A:$A,MATCH($A2629,'Import data'!$A:$A,0),1)","v":{"$error":"#N/A"}}]
[0,{"$f":"INDEX('Import data'!$A:$A,MATCH($A2630,'Import data'!$A:$A,0),1)","v":{"$error":"#N/A"}}]
[0,{"$f":"INDEX('Import data'!$A:$A,MATCH($A2631,'Import data'!$A:$A,0),1)","v":{"$error":"#N/A"}}]
[0,{"$f":"INDEX('Import data'!$A:$A,MATCH($A2632,'Import data'!$A:$A,0),1)","v":{"$error":"#N/A"}}]
[0,{"$f":"INDEX('Import data'!$A:$A,MATCH($A2633,'Import data'!$A:$A,0),1)","v":{"$error":"#N/A"}}]
[0,{"$f":"INDEX('Import data'!$A:$A,MATCH($A2634,'Import data'!$A:$A,0),1)","v":{"$error":"#N/A"}}]
[0,{"$f":"INDEX('Import data'!$A:$A,MATCH($A2635,'Import data'!$A:$A,0),1)","v":{"$error":"#N/A"}}]
[0,{"$f":"INDEX('Import data'!$A:$A,MATCH($A2636,'Import data'!$A:$A,0),1)","v":{"$error":"#N/A"}}]
[0,{"$f":"INDEX('Import data'!$A:$A,MATCH($A2637,'Import data'!$A:$A,0),1)","v":{"$error":"#N/A"}}]
[0,{"$f":"INDEX('Import data'!$A:$A,MATCH($A2638,'Import data'!$A:$A,0),1)","v":{"$error":"#N/A"}}]
[0,{"$f":"INDEX('Import data'!$A:$A,MATCH($A2639,'Import data'!$A:$A,0),1)","v":{"$error":"#N/A"}}]
[0,{"$f":"INDEX('Import data'!$A:$A,MATCH($A2640,'Import data'!$A:$A,0),1)","v":{"$error":"#N/A"}}]
[0,{"$f":"INDEX('Import data'!$A:$A,MATCH($A2641,'Import data'!$A:$A,0),1)","v":{"$error":"#N/A"}}]
[0,{"$f":"INDEX('Import data'!$A:$A,MATCH($A2642,'Import data'!$A:$A,0),1)","v":{"$error":"#N/A"}}]
[0,{"$f":"INDEX('Import data'!$A:$A,MATCH($A2643,'Import data'!$A:$A,0),1)","v":{"$error":"#N/A"}}]
[0,{"$f":"INDEX('Import data'!$A:$A,MATCH($A2644,'Import data'!$A:$A,0),1)","v":{"$error":"#N/A"}}]
[0,{"$f":"INDEX('Import data'!$A:$A,MATCH($A2645,'Import data'!$A:$A,0),1)","v":{"$error":"#N/A"}}]
[0,{"$f":"INDEX('Import data'!$A:$A,MATCH($A2646,'Import data'!$A:$A,0),1)","v":{"$error":"#N/A"}}]
[0,{"$f":"INDEX('Import data'!$A:$A,MATCH($A2647,'Import data'!$A:$A,0),1)","v":{"$error":"#N/A"}}]
[0,{"$f":"INDEX('Import data'!$A:$A,MATCH($A2648,'Import data'!$A:$A,0),1)","v":{"$error":"#N/A"}}]
[0,{"$f":"INDEX('Import data'!$A:$A,MATCH($A2649,'Import data'!$A:$A,0),1)","v":{"$error":"#N/A"}}]
[0,{"$f":"INDEX('Import data'!$A:$A,MATCH($A2650,'Import data'!$A:$A,0),1)","v":{"$error":"#N/A"}}]
[0,{"$f":"INDEX('Import data'!$A:$A,MATCH($A2651,'Import data'!$A:$A,0),1)","v":{"$error":"#N/A"}}]
[0,{"$f":"INDEX('Import data'!$A:$A,MATCH($A2652,'Import data'!$A:$A,0),1)","v":{"$error":"#N/A"}}]
[0,{"$f":"INDEX('Import data'!$A:$A,MATCH($A2653,'Import data'!$A:$A,0),1)","v":{"$error":"#N/A"}}]
[0,{"$f":"INDEX('Import data'!$A:$A,MATCH($A2654,'Import data'!$A:$A,0),1)","v":{"$error":"#N/A"}}]
[0,{"$f":"INDEX('Import data'!$A:$A,MATCH($A2655,'Import data'!$A:$A,0),1)","v":{"$error":"#N/A"}}]
[0,{"$f":"INDEX('Import data'!$A:$A,MATCH($A2656,'Import data'!$A:$A,0),1)","v":{"$error":"#N/A"}}]
[0,{"$f":"INDEX('Import data'!$A:$A,MATCH($A2657,'Import data'!$A:$A,0),1)","v":{"$error":"#N/A"}}]
[0,{"$f":"INDEX('Import data'!$A:$A,MATCH($A2658,'Import data'!$A:$A,0),1)","v":{"$error":"#N/A"}}]
[0,{"$f":"INDEX('Import data'!$A:$A,MATCH($A2659,'Import data'!$A:$A,0),1)","v":{"$error":"#N/A"}}]
[0,{"$f":"INDEX('Import data'!$A:$A,MATCH($A2660,'Import data'!$A:$A,0),1)","v":{"$error":"#N/A"}}]
[0,{"$f":"INDEX('Import data'!$A:$A,MATCH($A2661,'Import data'!$A:$A,0),1)","v":{"$error":"#N/A"}}]
[0,{"$f":"INDEX('Import data'!$A:$A,MATCH($A2662,'Import data'!$A:$A,0),1)","v":{"$error":"#N/A"}}]
[0,{"$f":"INDEX('Import data'!$A:$A,MATCH($A2663,'Import data'!$A:$A,0),1)","v":{"$error":"#N/A"}}]
[0,{"$f":"INDEX('Import data'!$A:$A,MATCH($A2664,'Import data'!$A:$A,0),1)","v":{"$error":"#N/A"}}]
[0,{"$f":"INDEX('Import data'!$A:$A,MATCH($A2665,'Import data'!$A:$A,0),1)","v":{"$error":"#N/A"}}]
[0,{"$f":"INDEX('Import data'!$A:$A,MATCH($A2666,'Import data'!$A:$A,0),1)","v":{"$error":"#N/A"}}]
[0,{"$f":"INDEX('Import data'!$A:$A,MATCH($A2667,'Import data'!$A:$A,0),1)","v":{"$error":"#N/A"}}]
[0,{"$f":"INDEX('Import data'!$A:$A,MATCH($A2668,'Import data'!$A:$A,0),1)","v":{"$error":"#N/A"}}]
[0,{"$f":"INDEX('Import data'!$A:$A,MATCH($A2669,'Import data'!$A:$A,0),1)","v":{"$error":"#N/A"}}]
[0,{"$f":"INDEX('Import data'!$A:$A,MATCH($A2670,'Import data'!$A:$A,0),1)","v":{"$error":"#N/A"}}]
[0,{"$f":"INDEX('Import data'!$A:$A,MATCH($A2671,'Import data'!$A:$A,0),1)","v":{"$error":"#N/A"}}]
[0,{"$f":"INDEX('Import data'!$A:$A,MATCH($A2672,'Import data'!$A:$A,0),1)","v":{"$error":"#N/A"}}]
[0,{"$f":"INDEX('Import data'!$A:$A,MATCH($A2673,'Import data'!$A:$A,0),1)","v":{"$error":"#N/A"}}]
[0,{"$f":"INDEX('Import data'!$A:$A,MATCH($A2674,'Import data'!$A:$A,0),1)","v":{"$error":"#N/A"}}]
[0,{"$f":"INDEX('Import data'!$A:$A,MATCH($A2675,'Import data'!$A:$A,0),1)","v":{"$error":"#N/A"}}]
[0,{"$f":"INDEX('Import data'!$A:$A,MATCH($A2676,'Import data'!$A:$A,0),1)","v":{"$error":"#N/A"}}]
[0,{"$f":"INDEX('Import data'!$A:$A,MATCH($A2677,'Import data'!$A:$A,0),1)","v":{"$error":"#N/A"}}]
[0,{"$f":"INDEX('Import data'!$A:$A,MATCH($A2678,'Import data'!$A:$A,0),1)","v":{"$error":"#N/A"}}]
[0,{"$f":"INDEX('Import data'!$A:$A,MATCH($A2679,'Import data'!$A:$A,0),1)","v":{"$error":"#N/A"}}]
[0,{"$f":"INDEX('Import data'!$A:$A,MATCH($A2680,'Import data'!$A:$A,0),1)","v":{"$error":"#N/A"}}]
[0,{"$f":"INDEX('Import data'!$A:$A,MATCH($A2681,'Import data'!$A:$A,0),1)","v":{"$error":"#N/A"}}]
[0,{"$f":"INDEX('Import data'!$A:$A,MATCH($A2682,'Import data'!$A:$A,0),1)","v":{"$error":"#N/A"}}]
[0,{"$f":"INDEX('Import data'!$A:$A,MATCH($A2683,'Import data'!$A:$A,0),1)","v":{"$error":"#N/A"}}]
[0,{"$f":"INDEX('Import data'!$A:$A,MATCH($A2684,'Import data'!$A:$A,0),1)","v":{"$error":"#N/A"}}]
[0,{"$f":"INDEX('Import data'!$A:$A,MATCH($A2685,'Import data'!$A:$A,0),1)","v":{"$error":"#N/A"}}]
[0,{"$f":"INDEX('Import data'!$A:$A,MATCH($A2686,'Import data'!$A:$A,0),1)","v":{"$error":"#N/A"}}]
[0,{"$f":"INDEX('Import data'!$A:$A,MATCH($A2687,'Import data'!$A:$A,0),1)","v":{"$error":"#N/A"}}]
[0,{"$f":"INDEX('Import data'!$A:$A,MATCH($A2688,'Import data'!$A:$A,0),1)","v":{"$error":"#N/A"}}]
[0,{"$f":"INDEX('Import data'!$A:$A,MATCH($A2689,'Import data'!$A:$A,0),1)","v":{"$error":"#N/A"}}]
[0,{"$f":"INDEX('Import data'!$A:$A,MATCH($A2690,'Import data'!$A:$A,0),1)","v":{"$error":"#N/A"}}]
[{"$f":"ID","v":0},{"$f":"INDEX('Import data'!$A:$A,MATCH($A2691,'Import data'!$A:$A,0),1)","v":{"$error":"#N/A"}}]
[0,{"$f":"INDEX('Import data'!$A:$A,MATCH($A2692,'Import data'!$A:$A,0),1)","v":{"$error":"#N/A"}}]
[0,{"$f":"INDEX('Import data'!$A:$A,MATCH($A2693,'Import data'!$A:$A,0),1)","v":{"$error":"#N/A"}}]
[0,{"$f":"INDEX('Import data'!$A:$A,MATCH($A2694,'Import data'!$A:$A,0),1)","v":{"$error":"#N/A"}}]
[0,{"$f":"INDEX('Import data'!$A:$A,MATCH($A2695,'Import data'!$A:$A,0),1)","v":{"$error":"#N/A"}}]
[0,{"$f":"INDEX('Import data'!$A:$A,MATCH($A2696,'Import data'!$A:$A,0),1)","v":{"$error":"#N/A"}}]
[0,{"$f":"INDEX('Import data'!$A:$A,MATCH($A2697,'Import data'!$A:$A,0),1)","v":{"$error":"#N/A"}}]
[0,{"$f":"INDEX('Import data'!$A:$A,MATCH($A2698,'Import data'!$A:$A,0),1)","v":{"$error":"#N/A"}}]
[0,{"$f":"INDEX('Import data'!$A:$A,MATCH($A2699,'Import data'!$A:$A,0),1)","v":{"$error":"#N/A"}}]
[0,{"$f":"INDEX('Import data'!$A:$A,MATCH($A2700,'Import data'!$A:$A,0),1)","v":{"$error":"#N/A"}}]
[0,{"$f":"INDEX('Import data'!$A:$A,MATCH($A2701,'Import data'!$A:$A,0),1)","v":{"$error":"#N/A"}}]
[0,{"$f":"INDEX('Import data'!$A:$A,MATCH($A2702,'Import data'!$A:$A,0),1)","v":{"$error":"#N/A"}}]
[0,{"$f":"INDEX('Import data'!$A:$A,MATCH($A2703,'Import data'!$A:$A,0),1)","v":{"$error":"#N/A"}}]
[0,{"$f":"INDEX('Import data'!$A:$A,MATCH($A2704,'Import data'!$A:$A,0),1)","v":{"$error":"#N/A"}}]
[0,{"$f":"INDEX('Import data'!$A:$A,MATCH($A2705,'Import data'!$A:$A,0),1)","v":{"$error":"#N/A"}}]
[0,{"$f":"INDEX('Import data'!$A:$A,MATCH($A2706,'Import data'!$A:$A,0),1)","v":{"$error":"#N/A"}}]
[0,{"$f":"INDEX('Import data'!$A:$A,MATCH($A2707,'Import data'!$A:$A,0),1)","v":{"$error":"#N/A"}}]
[0,{"$f":"INDEX('Import data'!$A:$A,MATCH($A2708,'Import data'!$A:$A,0),1)","v":{"$error":"#N/A"}}]
[0,{"$f":"INDEX('Import data'!$A:$A,MATCH($A2709,'Import data'!$A:$A,0),1)","v":{"$error":"#N/A"}}]
[0,{"$f":"INDEX('Import data'!$A:$A,MATCH($A2710,'Import data'!$A:$A,0),1)","v":{"$error":"#N/A"}}]
[0,{"$f":"INDEX('Import data'!$A:$A,MATCH($A2711,'Import data'!$A:$A,0),1)","v":{"$error":"#N/A"}}]
[0,{"$f":"INDEX('Import data'!$A:$A,MATCH($A2712,'Import data'!$A:$A,0),1)","v":{"$error":"#N/A"}}]
[0,{"$f":"INDEX('Import data'!$A:$A,MATCH($A2713,'Import data'!$A:$A,0),1)","v":{"$error":"#N/A"}}]
[0,{"$f":"INDEX('Import data'!$A:$A,MATCH($A2714,'Import data'!$A:$A,0),1)","v":{"$error":"#N/A"}}]
[0,{"$f":"INDEX('Import data'!$A:$A,MATCH($A2715,'Import data'!$A:$A,0),1)","v":{"$error":"#N/A"}}]
[0,{"$f":"INDEX('Import data'!$A:$A,MATCH($A2716,'Import data'!$A:$A,0),1)","v":{"$error":"#N/A"}}]
[0,{"$f":"INDEX('Import data'!$A:$A,MATCH($A2717,'Import data'!$A:$A,0),1)","v":{"$error":"#N/A"}}]
[0,{"$f":"INDEX('Import data'!$A:$A,MATCH($A2718,'Import data'!$A:$A,0),1)","v":{"$error":"#N/A"}}]
[0,{"$f":"INDEX('Import data'!$A:$A,MATCH($A2719,'Import data'!$A:$A,0),1)","v":{"$error":"#N/A"}}]
[0,{"$f":"INDEX('Import data'!$A:$A,MATCH($A2720,'Import data'!$A:$A,0),1)","v":{"$error":"#N/A"}}]
[0,{"$f":"INDEX('Import data'!$A:$A,MATCH($A2721,'Import data'!$A:$A,0),1)","v":{"$error":"#N/A"}}]
[0,{"$f":"INDEX('Import data'!$A:$A,MATCH($A2722,'Import data'!$A:$A,0),1)","v":{"$error":"#N/A"}}]
[0,{"$f":"INDEX('Import data'!$A:$A,MATCH($A2723,'Import data'!$A:$A,0),1)","v":{"$error":"#N/A"}}]
[0,{"$f":"INDEX('Import data'!$A:$A,MATCH($A2724,'Import data'!$A:$A,0),1)","v":{"$error":"#N/A"}}]
[0,{"$f":"INDEX('Import data'!$A:$A,MATCH($A2725,'Import data'!$A:$A,0),1)","v":{"$error":"#N/A"}}]
[0,{"$f":"INDEX('Import data'!$A:$A,MATCH($A2726,'Import data'!$A:$A,0),1)","v":{"$error":"#N/A"}}]
[0,{"$f":"INDEX('Import data'!$A:$A,MATCH($A2727,'Import data'!$A:$A,0),1)","v":{"$error":"#N/A"}}]
[0,{"$f":"INDEX('Import data'!$A:$A,MATCH($A2728,'Import data'!$A:$A,0),1)","v":{"$error":"#N/A"}}]
[0,{"$f":"INDEX('Import data'!$A:$A,MATCH($A2729,'Import data'!$A:$A,0),1)","v":{"$error":"#N/A"}}]
[0,{"$f":"INDEX('Import data'!$A:$A,MATCH($A2730,'Import data'!$A:$A,0),1)","v":{"$error":"#N/A"}}]
[0,{"$f":"INDEX('Import data'!$A:$A,MATCH($A2731,'Import data'!$A:$A,0),1)","v":{"$error":"#N/A"}}]
[0,{"$f":"INDEX('Import data'!$A:$A,MATCH($A2732,'Import data'!$A:$A,0),1)","v":{"$error":"#N/A"}}]
[0,{"$f":"INDEX('Import data'!$A:$A,MATCH($A2733,'Import data'!$A:$A,0),1)","v":{"$error":"#N/A"}}]
[0,{"$f":"INDEX('Import data'!$A:$A,MATCH($A2734,'Import data'!$A:$A,0),1)","v":{"$error":"#N/A"}}]
[0,{"$f":"INDEX('Import data'!$A:$A,MATCH($A2735,'Import data'!$A:$A,0),1)","v":{"$error":"#N/A"}}]
[0,{"$f":"INDEX('Import data'!$A:$A,MATCH($A2736,'Import data'!$A:$A,0),1)","v":{"$error":"#N/A"}}]
[0,{"$f":"INDEX('Import data'!$A:$A,MATCH($A2737,'Import data'!$A:$A,0),1)","v":{"$error":"#N/A"}}]
[0,{"$f":"INDEX('Import data'!$A:$A,MATCH($A2738,'Import data'!$A:$A,0),1)","v":{"$error":"#N/A"}}]
[0,{"$f":"INDEX('Import data'!$A:$A,MATCH($A2739,'Import data'!$A:$A,0),1)","v":{"$error":"#N/A"}}]
[0,{"$f":"INDEX('Import data'!$A:$A,MATCH($A2740,'Import data'!$A:$A,0),1)","v":{"$error":"#N/A"}}]
[0,{"$f":"INDEX('Import data'!$A:$A,MATCH($A2741,'Import data'!$A:$A,0),1)","v":{"$error":"#N/A"}}]
[0,{"$f":"INDEX('Import data'!$A:$A,MATCH($A2742,'Import data'!$A:$A,0),1)","v":{"$error":"#N/A"}}]
[0,{"$f":"INDEX('Import data'!$A:$A,MATCH($A2743,'Import data'!$A:$A,0),1)","v":{"$error":"#N/A"}}]
[0,{"$f":"INDEX('Import data'!$A:$A,MATCH($A2744,'Import data'!$A:$A,0),1)","v":{"$error":"#N/A"}}]
[0,{"$f":"INDEX('Import data'!$A:$A,MATCH($A2745,'Import data'!$A:$A,0),1)","v":{"$error":"#N/A"}}]
[0,{"$f":"INDEX('Import data'!$A:$A,MATCH($A2746,'Import data'!$A:$A,0),1)","v":{"$error":"#N/A"}}]
[0,{"$f":"INDEX('Import data'!$A:$A,MATCH($A2747,'Import data'!$A:$A,0),1)","v":{"$error":"#N/A"}}]
[0,{"$f":"INDEX('Import data'!$A:$A,MATCH($A2748,'Import data'!$A:$A,0),1)","v":{"$error":"#N/A"}}]
[0,{"$f":"INDEX('Import data'!$A:$A,MATCH($A2749,'Import data'!$A:$A,0),1)","v":{"$error":"#N/A"}}]
[0,{"$f":"INDEX('Import data'!$A:$A,MATCH($A2750,'Import data'!$A:$A,0),1)","v":{"$error":"#N/A"}}]
[0,{"$f":"INDEX('Import data'!$A:$A,MATCH($A2751,'Import data'!$A:$A,0),1)","v":{"$error":"#N/A"}}]
[0,{"$f":"INDEX('Import data'!$A:$A,MATCH($A2752,'Import data'!$A:$A,0),1)","v":{"$error":"#N/A"}}]
[0,{"$f":"INDEX('Import data'!$A:$A,MATCH($A2753,'Import data'!$A:$A,0),1)","v":{"$error":"#N/A"}}]
[0,{"$f":"INDEX('Import data'!$A:$A,MATCH($A2754,'Import data'!$A:$A,0),1)","v":{"$error":"#N/A"}}]
[{"$f":"ID","v":0},{"$f":"INDEX('Import data'!$A:$A,MATCH($A2755,'Import data'!$A:$A,0),1)","v":{"$error":"#N/A"}}]
[0,{"$f":"INDEX('Import data'!$A:$A,MATCH($A2756,'Import data'!$A:$A,0),1)","v":{"$error":"#N/A"}}]
[0,{"$f":"INDEX('Import data'!$A:$A,MATCH($A2757,'Import data'!$A:$A,0),1)","v":{"$error":"#N/A"}}]
[0,{"$f":"INDEX('Import data'!$A:$A,MATCH($A2758,'Import data'!$A:$A,0),1)","v":{"$error":"#N/A"}}]
[0,{"$f":"INDEX('Import data'!$A:$A,MATCH($A2759,'Import data'!$A:$A,0),1)","v":{"$error":"#N/A"}}]
[0,{"$f":"INDEX('Import data'!$A:$A,MATCH($A2760,'Import data'!$A:$A,0),1)","v":{"$error":"#N/A"}}]
[0,{"$f":"INDEX('Import data'!$A:$A,MATCH($A2761,'Import data'!$A:$A,0),1)","v":{"$error":"#N/A"}}]
[0,{"$f":"INDEX('Import data'!$A:$A,MATCH($A2762,'Import data'!$A:$A,0),1)","v":{"$error":"#N/A"}}]
[0,{"$f":"INDEX('Import data'!$A:$A,MATCH($A2763,'Import data'!$A:$A,0),1)","v":{"$error":"#N/A"}}]
[0,{"$f":"INDEX('Import data'!$A:$A,MATCH($A2764,'Import data'!$A:$A,0),1)","v":{"$error":"#N/A"}}]
[0,{"$f":"INDEX('Import data'!$A:$A,MATCH($A2765,'Import data'!$A:$A,0),1)","v":{"$error":"#N/A"}}]
[0,{"$f":"INDEX('Import data'!$A:$A,MATCH($A2766,'Import data'!$A:$A,0),1)","v":{"$error":"#N/A"}}]
[0,{"$f":"INDEX('Import data'!$A:$A,MATCH($A2767,'Import data'!$A:$A,0),1)","v":{"$error":"#N/A"}}]
[0,{"$f":"INDEX('Import data'!$A:$A,MATCH($A2768,'Import data'!$A:$A,0),1)","v":{"$error":"#N/A"}}]
[0,{"$f":"INDEX('Import data'!$A:$A,MATCH($A2769,'Import data'!$A:$A,0),1)","v":{"$error":"#N/A"}}]
[0,{"$f":"INDEX('Import data'!$A:$A,MATCH($A2770,'Import data'!$A:$A,0),1)","v":{"$error":"#N/A"}}]
[0,{"$f":"INDEX('Import data'!$A:$A,MATCH($A2771,'Import data'!$A:$A,0),1)","v":{"$error":"#N/A"}}]
[0,{"$f":"INDEX('Import data'!$A:$A,MATCH($A2772,'Import data'!$A:$A,0),1)","v":{"$error":"#N/A"}}]
[0,{"$f":"INDEX('Import data'!$A:$A,MATCH($A2773,'Import data'!$A:$A,0),1)","v":{"$error":"#N/A"}}]
[0,{"$f":"INDEX('Import data'!$A:$A,MATCH($A2774,'Import data'!$A:$A,0),1)","v":{"$error":"#N/A"}}]
[0,{"$f":"INDEX('Import data'!$A:$A,MATCH($A2775,'Import data'!$A:$A,0),1)","v":{"$error":"#N/A"}}]
[0,{"$f":"INDEX('Import data'!$A:$A,MATCH($A2776,'Import data'!$A:$A,0),1)","v":{"$error":"#N/A"}}]
[0,{"$f":"INDEX('Import data'!$A:$A,MATCH($A2777,'Import data'!$A:$A,0),1)","v":{"$error":"#N/A"}}]
[0,{"$f":"INDEX('Import data'!$A:$A,MATCH($A2778,'Import data'!$A:$A,0),1)","v":{"$error":"#N/A"}}]
[0,{"$f":"INDEX('Import data'!$A:$A,MATCH($A2779,'Import data'!$A:$A,0),1)","v":{"$error":"#N/A"}}]
[0,{"$f":"INDEX('Import data'!$A:$A,MATCH($A2780,'Import data'!$A:$A,0),1)","v":{"$error":"#N/A"}}]
[0,{"$f":"INDEX('Import data'!$A:$A,MATCH($A2781,'Import data'!$A:$A,0),1)","v":{"$error":"#N/A"}}]
[0,{"$f":"INDEX('Import data'!$A:$A,MATCH($A2782,'Import data'!$A:$A,0),1)","v":{"$error":"#N/A"}}]
[0,{"$f":"INDEX('Import data'!$A:$A,MATCH($A2783,'Import data'!$A:$A,0),1)","v":{"$error":"#N/A"}}]
[0,{"$f":"INDEX('Import data'!$A:$A,MATCH($A2784,'Import data'!$A:$A,0),1)","v":{"$error":"#N/A"}}]
[0,{"$f":"INDEX('Import data'!$A:$A,MATCH($A2785,'Import data'!$A:$A,0),1)","v":{"$error":"#N/A"}}]
[0,{"$f":"INDEX('Import data'!$A:$A,MATCH($A2786,'Import data'!$A:$A,0),1)","v":{"$error":"#N/A"}}]
[0,{"$f":"INDEX('Import data'!$A:$A,MATCH($A2787,'Import data'!$A:$A,0),1)","v":{"$error":"#N/A"}}]
[0,{"$f":"INDEX('Import data'!$A:$A,MATCH($A2788,'Import data'!$A:$A,0),1)","v":{"$error":"#N/A"}}]
[0,{"$f":"INDEX('Import data'!$A:$A,MATCH($A2789,'Import data'!$A:$A,0),1)","v":{"$error":"#N/A"}}]
[0,{"$f":"INDEX('Import data'!$A:$A,MATCH($A2790,'Import data'!$A:$A,0),1)","v":{"$error":"#N/A"}}]
[0,{"$f":"INDEX('Import data'!$A:$A,MATCH($A2791,'Import data'!$A:$A,0),1)","v":{"$error":"#N/A"}}]
[0,{"$f":"INDEX('Import data'!$A:$A,MATCH($A2792,'Import data'!$A:$A,0),1)","v":{"$error":"#N/A"}}]
[0,{"$f":"INDEX('Import data'!$A:$A,MATCH($A2793,'Import data'!$A:$A,0),1)","v":{"$error":"#N/A"}}]
[0,{"$f":"INDEX('Import data'!$A:$A,MATCH($A2794,'Import data'!$A:$A,0),1)","v":{"$error":"#N/A"}}]
[0,{"$f":"INDEX('Import data'!$A:$A,MATCH($A2795,'Import data'!$A:$A,0),1)","v":{"$error":"#N/A"}}]
[0,{"$f":"INDEX('Import data'!$A:$A,MATCH($A2796,'Import data'!$A:$A,0),1)","v":{"$error":"#N/A"}}]
[0,{"$f":"INDEX('Import data'!$A:$A,MATCH($A2797,'Import data'!$A:$A,0),1)","v":{"$error":"#N/A"}}]
[0,{"$f":"INDEX('Import data'!$A:$A,MATCH($A2798,'Import data'!$A:$A,0),1)","v":{"$error":"#N/A"}}]
[0,{"$f":"INDEX('Import data'!$A:$A,MATCH($A2799,'Import data'!$A:$A,0),1)","v":{"$error":"#N/A"}}]
[0,{"$f":"INDEX('Import data'!$A:$A,MATCH($A2800,'Import data'!$A:$A,0),1)","v":{"$error":"#N/A"}}]
[0,{"$f":"INDEX('Import data'!$A:$A,MATCH($A2801,'Import data'!$A:$A,0),1)","v":{"$error":"#N/A"}}]
[0,{"$f":"INDEX('Import data'!$A:$A,MATCH($A2802,'Import data'!$A:$A,0),1)","v":{"$error":"#N/A"}}]
[0,{"$f":"INDEX('Import data'!$A:$A,MATCH($A2803,'Import data'!$A:$A,0),1)","v":{"$error":"#N/A"}}]
[0,{"$f":"INDEX('Import data'!$A:$A,MATCH($A2804,'Import data'!$A:$A,0),1)","v":{"$error":"#N/A"}}]
[0,{"$f":"INDEX('Import data'!$A:$A,MATCH($A2805,'Import data'!$A:$A,0),1)","v":{"$error":"#N/A"}}]
[0,{"$f":"INDEX('Import data'!$A:$A,MATCH($A2806,'Import data'!$A:$A,0),1)","v":{"$error":"#N/A"}}]
[0,{"$f":"INDEX('Import data'!$A:$A,MATCH($A2807,'Import data'!$A:$A,0),1)","v":{"$error":"#N/A"}}]
[0,{"$f":"INDEX('Import data'!$A:$A,MATCH($A2808,'Import data'!$A:$A,0),1)","v":{"$error":"#N/A"}}]
[0,{"$f":"INDEX('Import data'!$A:$A,MATCH($A2809,'Import data'!$A:$A,0),1)","v":{"$error":"#N/A"}}]
[0,{"$f":"INDEX('Import data'!$A:$A,MATCH($A2810,'Import data'!$A:$A,0),1)","v":{"$error":"#N/A"}}]
[0,{"$f":"INDEX('Import data'!$A:$A,MATCH($A2811,'Import data'!$A:$A,0),1)","v":{"$error":"#N/A"}}]
[0,{"$f":"INDEX('Import data'!$A:$A,MATCH($A2812,'Import data'!$A:$A,0),1)","v":{"$error":"#N/A"}}]
[0,{"$f":"INDEX('Import data'!$A:$A,MATCH($A2813,'Import data'!$A:$A,0),1)","v":{"$error":"#N/A"}}]
[0,{"$f":"INDEX('Import data'!$A:$A,MATCH($A2814,'Import data'!$A:$A,0),1)","v":{"$error":"#N/A"}}]
[0,{"$f":"INDEX('Import data'!$A:$A,MATCH($A2815,'Import data'!$A:$A,0),1)","v":{"$error":"#N/A"}}]
[0,{"$f":"INDEX('Import data'!$A:$A,MATCH($A2816,'Import data'!$A:$A,0),1)","v":{"$error":"#N/A"}}]
[0,{"$f":"INDEX('Import data'!$A:$A,MATCH($A2817,'Import data'!$A:$A,0),1)","v":{"$error":"#N/A"}}]
[0,{"$f":"INDEX('Import data'!$A:$A,MATCH($A2818,'Import data'!$A:$A,0),1)","v":{"$error":"#N/A"}}]
[{"$f":"ID","v":0},{"$f":"INDEX('Import data'!$A:$A,MATCH($A2819,'Import data'!$A:$A,0),1)","v":{"$error":"#N/A"}}]
[0,{"$f":"INDEX('Import data'!$A:$A,MATCH($A2820,'Import data'!$A:$A,0),1)","v":{"$error":"#N/A"}}]
[0,{"$f":"INDEX('Import data'!$A:$A,MATCH($A2821,'Import data'!$A:$A,0),1)","v":{"$error":"#N/A"}}]
[0,{"$f":"INDEX('Import data'!$A:$A,MATCH($A2822,'Import data'!$A:$A,0),1)","v":{"$error":"#N/A"}}]
[0,{"$f":"INDEX('Import data'!$A:$A,MATCH($A2823,'Import data'!$A:$A,0),1)","v":{"$error":"#N/A"}}]
[0,{"$f":"INDEX('Import data'!$A:$A,MATCH($A2824,'Import data'!$A:$A,0),1)","v":{"$error":"#N/A"}}]
[0,{"$f":"INDEX('Import data'!$A:$A,MATCH($A2825,'Import data'!$A:$A,0),1)","v":{"$error":"#N/A"}}]
[0,{"$f":"INDEX('Import data'!$A:$A,MATCH($A2826,'Import data'!$A:$A,0),1)","v":{"$error":"#N/A"}}]
[0,{"$f":"INDEX('Import data'!$A:$A,MATCH($A2827,'Import data'!$A:$A,0),1)","v":{"$error":"#N/A"}}]
[0,{"$f":"INDEX('Import data'!$A:$A,MATCH($A2828,'Import data'!$A:$A,0),1)","v":{"$error":"#N/A"}}]
[0,{"$f":"INDEX('Import data'!$A:$A,MATCH($A2829,'Import data'!$A:$A,0),1)","v":{"$error":"#N/A"}}]
[0,{"$f":"INDEX('Import data'!$A:$A,MATCH($A2830,'Import data'!$A:$A,0),1)","v":{"$error":"#N/A"}}]
[0,{"$f":"INDEX('Import data'!$A:$A,MATCH($A2831,'Import data'!$A:$A,0),1)","v":{"$error":"#N/A"}}]
[0,{"$f":"INDEX('Import data'!$A:$A,MATCH($A2832,'Import data'!$A:$A,0),1)","v":{"$error":"#N/A"}}]
[0,{"$f":"INDEX('Import data'!$A:$A,MATCH($A2833,'Import data'!$A:$A,0),1)","v":{"$error":"#N/A"}}]
[0,{"$f":"INDEX('Import data'!$A:$A,MATCH($A2834,'Import data'!$A:$A,0),1)","v":{"$error":"#N/A"}}]
[0,{"$f":"INDEX('Import data'!$A:$A,MATCH($A2835,'Import data'!$A:$A,0),1)","v":{"$error":"#N/A"}}]
[0,{"$f":"INDEX('Import data'!$A:$A,MATCH($A2836,'Import data'!$A:$A,0),1)","v":{"$error":"#N/A"}}]
[0,{"$f":"INDEX('Import data'!$A:$A,MATCH($A2837,'Import data'!$A:$A,0),1)","v":{"$error":"#N/A"}}]
[0,{"$f":"INDEX('Import data'!$A:$A,MATCH($A2838,'Import data'!$A:$A,0),1)","v":{"$error":"#N/A"}}]
[0,{"$f":"INDEX('Import data'!$A:$A,MATCH($A2839,'Import data'!$A:$A,0),1)","v":{"$error":"#N/A"}}]
[0,{"$f":"INDEX('Import data'!$A:$A,MATCH($A2840,'Import data'!$A:$A,0),1)","v":{"$error":"#N/A"}}]
[0,{"$f":"INDEX('Import data'!$A:$A,MATCH($A2841,'Import data'!$A:$A,0),1)","v":{"$error":"#N/A"}}]
[0,{"$f":"INDEX('Import data'!$A:$A,MATCH($A2842,'Import data'!$A:$A,0),1)","v":{"$error":"#N/A"}}]
[0,{"$f":"INDEX('Import data'!$A:$A,MATCH($A2843,'Import data'!$A:$A,0),1)","v":{"$error":"#N/A"}}]
[0,{"$f":"INDEX('Import data'!$A:$A,MATCH($A2844,'Import data'!$A:$A,0),1)","v":{"$error":"#N/A"}}]
[0,{"$f":"INDEX('Import data'!$A:$A,MATCH($A2845,'Import data'!$A:$A,0),1)","v":{"$error":"#N/A"}}]
[0,{"$f":"INDEX('Import data'!$A:$A,MATCH($A2846,'Import data'!$A:$A,0),1)","v":{"$error":"#N/A"}}]
[0,{"$f":"INDEX('Import data'!$A:$A,MATCH($A2847,'Import data'!$A:$A,0),1)","v":{"$error":"#N/A"}}]
[0,{"$f":"INDEX('Import data'!$A:$A,MATCH($A2848,'Import data'!$A:$A,0),1)","v":{"$error":"#N/A"}}]
[0,{"$f":"INDEX('Import data'!$A:$A,MATCH($A2849,'Import data'!$A:$A,0),1)","v":{"$error":"#N/A"}}]
[0,{"$f":"INDEX('Import data'!$A:$A,MATCH($A2850,'Import data'!$A:$A,0),1)","v":{"$error":"#N/A"}}]
[0,{"$f":"INDEX('Import data'!$A:$A,MATCH($A2851,'Import data'!$A:$A,0),1)","v":{"$error":"#N/A"}}]
[0,{"$f":"INDEX('Import data'!$A:$A,MATCH($A2852,'Import data'!$A:$A,0),1)","v":{"$error":"#N/A"}}]
[0,{"$f":"INDEX('Import data'!$A:$A,MATCH($A2853,'Import data'!$A:$A,0),1)","v":{"$error":"#N/A"}}]
[0,{"$f":"INDEX('Import data'!$A:$A,MATCH($A2854,'Import data'!$A:$A,0),1)","v":{"$error":"#N/A"}}]
[0,{"$f":"INDEX('Import data'!$A:$A,MATCH($A2855,'Import data'!$A:$A,0),1)","v":{"$error":"#N/A"}}]
[0,{"$f":"INDEX('Import data'!$A:$A,MATCH($A2856,'Import data'!$A:$A,0),1)","v":{"$error":"#N/A"}}]
[0,{"$f":"INDEX('Import data'!$A:$A,MATCH($A2857,'Import data'!$A:$A,0),1)","v":{"$error":"#N/A"}}]
[0,{"$f":"INDEX('Import data'!$A:$A,MATCH($A2858,'Import data'!$A:$A,0),1)","v":{"$error":"#N/A"}}]
[0,{"$f":"INDEX('Import data'!$A:$A,MATCH($A2859,'Import data'!$A:$A,0),1)","v":{"$error":"#N/A"}}]
[0,{"$f":"INDEX('Import data'!$A:$A,MATCH($A2860,'Import data'!$A:$A,0),1)","v":{"$error":"#N/A"}}]
[0,{"$f":"INDEX('Import data'!$A:$A,MATCH($A2861,'Import data'!$A:$A,0),1)","v":{"$error":"#N/A"}}]
[0,{"$f":"INDEX('Import data'!$A:$A,MATCH($A2862,'Import data'!$A:$A,0),1)","v":{"$error":"#N/A"}}]
[0,{"$f":"INDEX('Import data'!$A:$A,MATCH($A2863,'Import data'!$A:$A,0),1)","v":{"$error":"#N/A"}}]
[0,{"$f":"INDEX('Import data'!$A:$A,MATCH($A2864,'Import data'!$A:$A,0),1)","v":{"$error":"#N/A"}}]
[0,{"$f":"INDEX('Import data'!$A:$A,MATCH($A2865,'Import data'!$A:$A,0),1)","v":{"$error":"#N/A"}}]
[0,{"$f":"INDEX('Import data'!$A:$A,MATCH($A2866,'Import data'!$A:$A,0),1)","v":{"$error":"#N/A"}}]
[0,{"$f":"INDEX('Import data'!$A:$A,MATCH($A2867,'Import data'!$A:$A,0),1)","v":{"$error":"#N/A"}}]
[0,{"$f":"INDEX('Import data'!$A:$A,MATCH($A2868,'Import data'!$A:$A,0),1)","v":{"$error":"#N/A"}}]
[0,{"$f":"INDEX('Import data'!$A:$A,MATCH($A2869,'Import data'!$A:$A,0),1)","v":{"$error":"#N/A"}}]
[0,{"$f":"INDEX('Import data'!$A:$A,MATCH($A2870,'Import data'!$A:$A,0),1)","v":{"$error":"#N/A"}}]
[0,{"$f":"INDEX('Import data'!$A:$A,MATCH($A2871,'Import data'!$A:$A,0),1)","v":{"$error":"#N/A"}}]
[0,{"$f":"INDEX('Import data'!$A:$A,MATCH($A2872,'Import data'!$A:$A,0),1)","v":{"$error":"#N/A"}}]
[0,{"$f":"INDEX('Import data'!$A:$A,MATCH($A2873,'Import data'!$A:$A,0),1)","v":{"$error":"#N/A"}}]
[0,{"$f":"INDEX('Import data'!$A:$A,MATCH($A2874,'Import data'!$A:$A,0),1)","v":{"$error":"#N/A"}}]
[0,{"$f":"INDEX('Import data'!$A:$A,MATCH($A2875,'Import data'!$A:$A,0),1)","v":{"$error":"#N/A"}}]
[0,{"$f":"INDEX('Import data'!$A:$A,MATCH($A2876,'Import data'!$A:$A,0),1)","v":{"$error":"#N/A"}}]
[0,{"$f":"INDEX('Import data'!$A:$A,MATCH($A2877,'Import data'!$A:$A,0),1)","v":{"$error":"#N/A"}}]
[0,{"$f":"INDEX('Import data'!$A:$A,MATCH($A2878,'Import data'!$A:$A,0),1)","v":{"$error":"#N/A"}}]
[0,{"$f":"INDEX('Import data'!$A:$A,MATCH($A2879,'Import data'!$A:$A,0),1)","v":{"$error":"#N/A"}}]
[0,{"$f":"INDEX('Import data'!$A:$A,MATCH($A2880,'Import data'!$A:$A,0),1)","v":{"$error":"#N/A"}}]
[0,{"$f":"INDEX('Import data'!$A:$A,MATCH($A2881,'Import data'!$A:$A,0),1)","v":{"$error":"#N/A"}}]
[0,{"$f":"INDEX('Import data'!$A:$A,MATCH($A2882,'Import data'!$A:$A,0),1)","v":{"$error":"#N/A"}}]
[{"$f":"ID","v":0},{"$f":"INDEX('Import data'!$A:$A,MATCH($A2883,'Import data'!$A:$A,0),1)","v":{"$error":"#N/A"}}]
[0,{"$f":"INDEX('Import data'!$A:$A,MATCH($A2884,'Import data'!$A:$A,0),1)","v":{"$error":"#N/A"}}]
[0,{"$f":"INDEX('Import data'!$A:$A,MATCH($A2885,'Import data'!$A:$A,0),1)","v":{"$error":"#N/A"}}]
[0,{"$f":"INDEX('Import data'!$A:$A,MATCH($A2886,'Import data'!$A:$A,0),1)","v":{"$error":"#N/A"}}]
[0,{"$f":"INDEX('Import data'!$A:$A,MATCH($A2887,'Import data'!$A:$A,0),1)","v":{"$error":"#N/A"}}]
[0,{"$f":"INDEX('Import data'!$A:$A,MATCH($A2888,'Import data'!$A:$A,0),1)","v":{"$error":"#N/A"}}]
[0,{"$f":"INDEX('Import data'!$A:$A,MATCH($A2889,'Import data'!$A:$A,0),1)","v":{"$error":"#N/A"}}]
[0,{"$f":"INDEX('Import data'!$A:$A,MATCH($A2890,'Import data'!$A:$A,0),1)","v":{"$error":"#N/A"}}]
[0,{"$f":"INDEX('Import data'!$A:$A,MATCH($A2891,'Import data'!$A:$A,0),1)","v":{"$error":"#N/A"}}]
[0,{"$f":"INDEX('Import data'!$A:$A,MATCH($A2892,'Import data'!$A:$A,0),1)","v":{"$error":"#N/A"}}]
[0,{"$f":"INDEX('Import data'!$A:$A,MATCH($A2893,'Import data'!$A:$A,0),1)","v":{"$error":"#N/A"}}]
[0,{"$f":"INDEX('Import data'!$A:$A,MATCH($A2894,'Import data'!$A:$A,0),1)","v":{"$error":"#N/A"}}]
[0,{"$f":"INDEX('Import data'!$A:$A,MATCH($A2895,'Import data'!$A:$A,0),1)","v":{"$error":"#N/A"}}]
[0,{"$f":"INDEX('Import data'!$A:$A,MATCH($A2896,'Import data'!$A:$A,0),1)","v":{"$error":"#N/A"}}]
[0,{"$f":"INDEX('Import data'!$A:$A,MATCH($A2897,'Import data'!$A:$A,0),1)","v":{"$error":"#N/A"}}]
[0,{"$f":"INDEX('Import data'!$A:$A,MATCH($A2898,'Import data'!$A:$A,0),1)","v":{"$error":"#N/A"}}]
[0,{"$f":"INDEX('Import data'!$A:$A,MATCH($A2899,'Import data'!$A:$A,0),1)","v":{"$error":"#N/A"}}]
[0,{"$f":"INDEX('Import data'!$A:$A,MATCH($A2900,'Import data'!$A:$A,0),1)","v":{"$error":"#N/A"}}]
[0,{"$f":"INDEX('Import data'!$A:$A,MATCH($A2901,'Import data'!$A:$A,0),1)","v":{"$error":"#N/A"}}]
[0,{"$f":"INDEX('Import data'!$A:$A,MATCH($A2902,'Import data'!$A:$A,0),1)","v":{"$error":"#N/A"}}]
[0,{"$f":"INDEX('Import data'!$A:$A,MATCH($A2903,'Import data'!$A:$A,0),1)","v":{"$error":"#N/A"}}]
[0,{"$f":"INDEX('Import data'!$A:$A,MATCH($A2904,'Import data'!$A:$A,0),1)","v":{"$error":"#N/A"}}]
[0,{"$f":"INDEX('Import data'!$A:$A,MATCH($A2905,'Import data'!$A:$A,0),1)","v":{"$error":"#N/A"}}]
[0,{"$f":"INDEX('Import data'!$A:$A,MATCH($A2906,'Import data'!$A:$A,0),1)","v":{"$error":"#N/A"}}]
[0,{"$f":"INDEX('Import data'!$A:$A,MATCH($A2907,'Import data'!$A:$A,0),1)","v":{"$error":"#N/A"}}]
[0,{"$f":"INDEX('Import data'!$A:$A,MATCH($A2908,'Import data'!$A:$A,0),1)","v":{"$error":"#N/A"}}]
[0,{"$f":"INDEX('Import data'!$A:$A,MATCH($A2909,'Import data'!$A:$A,0),1)","v":{"$error":"#N/A"}}]
[0,{"$f":"INDEX('Import data'!$A:$A,MATCH($A2910,'Import data'!$A:$A,0),1)","v":{"$error":"#N/A"}}]
[0,{"$f":"INDEX('Import data'!$A:$A,MATCH($A2911,'Import data'!$A:$A,0),1)","v":{"$error":"#N/A"}}]
[0,{"$f":"INDEX('Import data'!$A:$A,MATCH($A2912,'Import data'!$A:$A,0),1)","v":{"$error":"#N/A"}}]
[0,{"$f":"INDEX('Import data'!$A:$A,MATCH($A2913,'Import data'!$A:$A,0),1)","v":{"$error":"#N/A"}}]
[0,{"$f":"INDEX('Import data'!$A:$A,MATCH($A2914,'Import data'!$A:$A,0),1)","v":{"$error":"#N/A"}}]
[0,{"$f":"INDEX('Import data'!$A:$A,MATCH($A2915,'Import data'!$A:$A,0),1)","v":{"$error":"#N/A"}}]
[0,{"$f":"INDEX('Import data'!$A:$A,MATCH($A2916,'Import data'!$A:$A,0),1)","v":{"$error":"#N/A"}}]
[0,{"$f":"INDEX('Import data'!$A:$A,MATCH($A2917,'Import data'!$A:$A,0),1)","v":{"$error":"#N/A"}}]
[0,{"$f":"INDEX('Import data'!$A:$A,MATCH($A2918,'Import data'!$A:$A,0),1)","v":{"$error":"#N/A"}}]
[0,{"$f":"INDEX('Import data'!$A:$A,MATCH($A2919,'Import data'!$A:$A,0),1)","v":{"$error":"#N/A"}}]
[0,{"$f":"INDEX('Import data'!$A:$A,MATCH($A2920,'Import data'!$A:$A,0),1)","v":{"$error":"#N/A"}}]
[0,{"$f":"INDEX('Import data'!$A:$A,MATCH($A2921,'Import data'!$A:$A,0),1)","v":{"$error":"#N/A"}}]
[0,{"$f":"INDEX('Import data'!$A:$A,MATCH($A2922,'Import data'!$A:$A,0),1)","v":{"$error":"#N/A"}}]
[0,{"$f":"INDEX('Import data'!$A:$A,MATCH($A2923,'Import data'!$A:$A,0),1)","v":{"$error":"#N/A"}}]
[0,{"$f":"INDEX('Import data'!$A:$A,MATCH($A2924,'Import data'!$A:$A,0),1)","v":{"$error":"#N/A"}}]
[0,{"$f":"INDEX('Import data'!$A:$A,MATCH($A2925,'Import data'!$A:$A,0),1)","v":{"$error":"#N/A"}}]
[0,{"$f":"INDEX('Import data'!$A:$A,MATCH($A2926,'Import data'!$A:$A,0),1)","v":{"$error":"#N/A"}}]
[0,{"$f":"INDEX('Import data'!$A:$A,MATCH($A2927,'Import data'!$A:$A,0),1)","v":{"$error":"#N/A"}}]
[0,{"$f":"INDEX('Import data'!$A:$A,MATCH($A2928,'Import data'!$A:$A,0),1)","v":{"$error":"#N/A"}}]
[0,{"$f":"INDEX('Import data'!$A:$A,MATCH($A2929,'Import data'!$A:$A,0),1)","v":{"$error":"#N/A"}}]
[0,{"$f":"INDEX('Import data'!$A:$A,MATCH($A2930,'Import data'!$A:$A,0),1)","v":{"$error":"#N/A"}}]
[0,{"$f":"INDEX('Import data'!$A:$A,MATCH($A2931,'Import data'!$A:$A,0),1)","v":{"$error":"#N/A"}}]
[0,{"$f":"INDEX('Import data'!$A:$A,MATCH($A2932,'Import data'!$A:$A,0),1)","v":{"$error":"#N/A"}}]
[0,{"$f":"INDEX('Import data'!$A:$A,MATCH($A2933,'Import data'!$A:$A,0),1)","v":{"$error":"#N/A"}}]
[0,{"$f":"INDEX('Import data'!$A:$A,MATCH($A2934,'Import data'!$A:$A,0),1)","v":{"$error":"#N/A"}}]
[0,{"$f":"INDEX('Import data'!$A:$A,MATCH($A2935,'Import data'!$A:$A,0),1)","v":{"$error":"#N/A"}}]
[0,{"$f":"INDEX('Import data'!$A:$A,MATCH($A2936,'Import data'!$A:$A,0),1)","v":{"$error":"#N/A"}}]
[0,{"$f":"INDEX('Import data'!$A:$A,MATCH($A2937,'Import data'!$A:$A,0),1)","v":{"$error":"#N/A"}}]
[0,{"$f":"INDEX('Import data'!$A:$A,MATCH($A2938,'Import data'!$A:$A,0),1)","v":{"$error":"#N/A"}}]
[0,{"$f":"INDEX('Import data'!$A:$A,MATCH($A2939,'Import data'!$A:$A,0),1)","v":{"$error":"#N/A"}}]
[0,{"$f":"INDEX('Import data'!$A:$A,MATCH($A2940,'Import data'!$A:$A,0),1)","v":{"$error":"#N/A"}}]
[0,{"$f":"INDEX('Import data'!$A:$A,MATCH($A2941,'Import data'!$A:$A,0),1)","v":{"$error":"#N/A"}}]
[0,{"$f":"INDEX('Import data'!$A:$A,MATCH($A2942,'Import data'!$A:$A,0),1)","v":{"$error":"#N/A"}}]
[0,{"$f":"INDEX('Import data'!$A:$A,MATCH($A2943,'Import data'!$A:$A,0),1)","v":{"$error":"#N/A"}}]
[0,{"$f":"INDEX('Import data'!$A:$A,MATCH($A2944,'Import data'!$A:$A,0),1)","v":{"$error":"#N/A"}}]
[0,{"$f":"INDEX('Import data'!$A:$A,MATCH($A2945,'Import data'!$A:$A,0),1)","v":{"$error":"#N/A"}}]
[0,{"$f":"INDEX('Import data'!$A:$A,MATCH($A2946,'Import data'!$A:$A,0),1)","v":{"$error":"#N/A"}}]
[{"$f":"ID","v":0},{"$f":"INDEX('Import data'!$A:$A,MATCH($A2947,'Import data'!$A:$A,0),1)","v":{"$error":"#N/A"}}]
[0,{"$f":"INDEX('Import data'!$A:$A,MATCH($A2948,'Import data'!$A:$A,0),1)","v":{"$error":"#N/A"}}]
[0,{"$f":"INDEX('Import data'!$A:$A,MATCH($A2949,'Import data'!$A:$A,0),1)","v":{"$error":"#N/A"}}]
[0,{"$f":"INDEX('Import data'!$A:$A,MATCH($A2950,'Import data'!$A:$A,0),1)","v":{"$error":"#N/A"}}]
[0,{"$f":"INDEX('Import data'!$A:$A,MATCH($A2951,'Import data'!$A:$A,0),1)","v":{"$error":"#N/A"}}]
[0,{"$f":"INDEX('Import data'!$A:$A,MATCH($A2952,'Import data'!$A:$A,0),1)","v":{"$error":"#N/A"}}]
[0,{"$f":"INDEX('Import data'!$A:$A,MATCH($A2953,'Import data'!$A:$A,0),1)","v":{"$error":"#N/A"}}]
[0,{"$f":"INDEX('Import data'!$A:$A,MATCH($A2954,'Import data'!$A:$A,0),1)","v":{"$error":"#N/A"}}]
[0,{"$f":"INDEX('Import data'!$A:$A,MATCH($A2955,'Import data'!$A:$A,0),1)","v":{"$error":"#N/A"}}]
[0,{"$f":"INDEX('Import data'!$A:$A,MATCH($A2956,'Import data'!$A:$A,0),1)","v":{"$error":"#N/A"}}]
[0,{"$f":"INDEX('Import data'!$A:$A,MATCH($A2957,'Import data'!$A:$A,0),1)","v":{"$error":"#N/A"}}]
[0,{"$f":"INDEX('Import data'!$A:$A,MATCH($A2958,'Import data'!$A:$A,0),1)","v":{"$error":"#N/A"}}]
[0,{"$f":"INDEX('Import data'!$A:$A,MATCH($A2959,'Import data'!$A:$A,0),1)","v":{"$error":"#N/A"}}]
[0,{"$f":"INDEX('Import data'!$A:$A,MATCH($A2960,'Import data'!$A:$A,0),1)","v":{"$error":"#N/A"}}]
[0,{"$f":"INDEX('Import data'!$A:$A,MATCH($A2961,'Import data'!$A:$A,0),1)","v":{"$error":"#N/A"}}]
[0,{"$f":"INDEX('Import data'!$A:$A,MATCH($A2962,'Import data'!$A:$A,0),1)","v":{"$error":"#N/A"}}]
[0,{"$f":"INDEX('Import data'!$A:$A,MATCH($A2963,'Import data'!$A:$A,0),1)","v":{"$error":"#N/A"}}]
[0,{"$f":"INDEX('Import data'!$A:$A,MATCH($A2964,'Import data'!$A:$A,0),1)","v":{"$error":"#N/A"}}]
[0,{"$f":"INDEX('Import data'!$A:$A,MATCH($A2965,'Import data'!$A:$A,0),1)","v":{"$error":"#N/A"}}]
[0,{"$f":"INDEX('Import data'!$A:$A,MATCH($A2966,'Import data'!$A:$A,0),1)","v":{"$error":"#N/A"}}]
[0,{"$f":"INDEX('Import data'!$A:$A,MATCH($A2967,'Import data'!$A:$A,0),1)","v":{"$error":"#N/A"}}]
[0,{"$f":"INDEX('Import data'!$A:$A,MATCH($A2968,'Import data'!$A:$A,0),1)","v":{"$error":"#N/A"}}]
[0,{"$f":"INDEX('Import data'!$A:$A,MATCH($A2969,'Import data'!$A:$A,0),1)","v":{"$error":"#N/A"}}]
[0,{"$f":"INDEX('Import data'!$A:$A,MATCH($A2970,'Import data'!$A:$A,0),1)","v":{"$error":"#N/A"}}]
[0,{"$f":"INDEX('Import data'!$A:$A,MATCH($A2971,'Import data'!$A:$A,0),1)","v":{"$error":"#N/A"}}]
[0,{"$f":"INDEX('Import data'!$A:$A,MATCH($A2972,'Import data'!$A:$A,0),1)","v":{"$error":"#N/A"}}]
[0,{"$f":"INDEX('Import data'!$A:$A,MATCH($A2973,'Import data'!$A:$A,0),1)","v":{"$error":"#N/A"}}]
[0,{"$f":"INDEX('Import data'!$A:$A,MATCH($A2974,'Import data'!$A:$A,0),1)","v":{"$error":"#N/A"}}]
[0,{"$f":"INDEX('Import data'!$A:$A,MATCH($A2975,'Import data'!$A:$A,0),1)","v":{"$error":"#N/A"}}]
[0,{"$f":"INDEX('Import data'!$A:$A,MATCH($A2976,'Import data'!$A:$A,0),1)","v":{"$error":"#N/A"}}]
[0,{"$f":"INDEX('Import data'!$A:$A,MATCH($A2977,'Import data'!$A:$A,0),1)","v":{"$error":"#N/A"}}]
[0,{"$f":"INDEX('Import data'!$A:$A,MATCH($A2978,'Import data'!$A:$A,0),1)","v":{"$error":"#N/A"}}]
[0,{"$f":"INDEX('Import data'!$A:$A,MATCH($A2979,'Import data'!$A:$A,0),1)","v":{"$error":"#N/A"}}]
[0,{"$f":"INDEX('Import data'!$A:$A,MATCH($A2980,'Import data'!$A:$A,0),1)","v":{"$error":"#N/A"}}]
[0,{"$f":"INDEX('Import data'!$A:$A,MATCH($A2981,'Import data'!$A:$A,0),1)","v":{"$error":"#N/A"}}]
[0,{"$f":"INDEX('Import data'!$A:$A,MATCH($A2982,'Import data'!$A:$A,0),1)","v":{"$error":"#N/A"}}]
[0,{"$f":"INDEX('Import data'!$A:$A,MATCH($A2983,'Import data'!$A:$A,0),1)","v":{"$error":"#N/A"}}]
[0,{"$f":"INDEX('Import data'!$A:$A,MATCH($A2984,'Import data'!$A:$A,0),1)","v":{"$error":"#N/A"}}]
[0,{"$f":"INDEX('Import data'!$A:$A,MATCH($A2985,'Import data'!$A:$A,0),1)","v":{"$error":"#N/A"}}]
[0,{"$f":"INDEX('Import data'!$A:$A,MATCH($A2986,'Import data'!$A:$A,0),1)","v":{"$error":"#N/A"}}]
[0,{"$f":"INDEX('Import data'!$A:$A,MATCH($A2987,'Import data'!$A:$A,0),1)","v":{"$error":"#N/A"}}]
[0,{"$f":"INDEX('Import data'!$A:$A,MATCH($A2988,'Import data'!$A:$A,0),1)","v":{"$error":"#N/A"}}]
[0,{"$f":"INDEX('Import data'!$A:$A,MATCH($A2989,'Import data'!$A:$A,0),1)","v":{"$error":"#N/A"}}]
[0,{"$f":"INDEX('Import data'!$A:$A,MATCH($A2990,'Import data'!$A:$A,0),1)","v":{"$error":"#N/A"}}]
[0,{"$f":"INDEX('Import data'!$A:$A,MATCH($A2991,'Import data'!$A:$A,0),1)","v":{"$error":"#N/A"}}]
[0,{"$f":"INDEX('Import data'!$A:$A,MATCH($A2992,'Import data'!$A:$A,0),1)","v":{"$error":"#N/A"}}]
[0,{"$f":"INDEX('Import data'!$A:$A,MATCH($A2993,'Import data'!$A:$A,0),1)","v":{"$error":"#N/A"}}]
[0,{"$f":"INDEX('Import data'!$A:$A,MATCH($A2994,'Import data'!$A:$A,0),1)","v":{"$error":"#N/A"}}]
[0,{"$f":"INDEX('Import data'!$A:$A,MATCH($A2995,'Import data'!$A:$A,0),1)","v":{"$error":"#N/A"}}]
[0,{"$f":"INDEX('Import data'!$A:$A,MATCH($A2996,'Import data'!$A:$A,0),1)","v":{"$error":"#N/A"}}]
[0,{"$f":"INDEX('Import data'!$A:$A,MATCH($A2997,'Import data'!$A:$A,0),1)","v":{"$error":"#N/A"}}]
[0,{"$f":"INDEX('Import data'!$A:$A,MATCH($A2998,'Import data'!$A:$A,0),1)","v":{"$error":"#N/A"}}]
[0,{"$f":"INDEX('Import data'!$A:$A,MATCH($A2999,'Import data'!$A:$A,0),1)","v":{"$error":"#N/A"}}]
[0,{"$f":"INDEX('Import data'!$A:$A,MATCH($A3000,'Import data'!$A:$A,0),1)","v":{"$error":"#N/A"}}]
[0,{"$f":"INDEX('Import data'!$A:$A,MATCH($A3001,'Import data'!$A:$A,0),1)","v":{"$error":"#N/A"}}]
[0,{"$f":"INDEX('Import data'!$A:$A,MATCH($A3002,'Import data'!$A:$A,0),1)","v":{"$error":"#N/A"}}]
[0,{"$f":"INDEX('Import data'!$A:$A,MATCH($A3003,'Import data'!$A:$A,0),1)","v":{"$error":"#N/A"}}]
[0,{"$f":"INDEX('Import data'!$A:$A,MATCH($A3004,'Import data'!$A:$A,0),1)","v":{"$error":"#N/A"}}]
[0,{"$f":"INDEX('Import data'!$A:$A,MATCH($A3005,'Import data'!$A:$A,0),1)","v":{"$error":"#N/A"}}]
[0,{"$f":"INDEX('Import data'!$A:$A,MATCH($A3006,'Import data'!$A:$A,0),1)","v":{"$error":"#N/A"}}]
[0,{"$f":"INDEX('Import data'!$A:$A,MATCH($A3007,'Import data'!$A:$A,0),1)","v":{"$error":"#N/A"}}]
[0,{"$f":"INDEX('Import data'!$A:$A,MATCH($A3008,'Import data'!$A:$A,0),1)","v":{"$error":"#N/A"}}]
[0,{"$f":"INDEX('Import data'!$A:$A,MATCH($A3009,'Import data'!$A:$A,0),1)","v":{"$error":"#N/A"}}]
[0,{"$f":"INDEX('Import data'!$A:$A,MATCH($A3010,'Import data'!$A:$A,0),1)","v":{"$error":"#N/A"}}]
[{"$f":"ID","v":0},{"$f":"INDEX('Import data'!$A:$A,MATCH($A3011,'Import data'!$A:$A,0),1)","v":{"$error":"#N/A"}}]
[0,{"$f":"INDEX('Import data'!$A:$A,MATCH($A3012,'Import data'!$A:$A,0),1)","v":{"$error":"#N/A"}}]
[0,{"$f":"INDEX('Import data'!$A:$A,MATCH($A3013,'Import data'!$A:$A,0),1)","v":{"$error":"#N/A"}}]
[0,{"$f":"INDEX('Import data'!$A:$A,MATCH($A3014,'Import data'!$A:$A,0),1)","v":{"$error":"#N/A"}}]
[0,{"$f":"INDEX('Import data'!$A:$A,MATCH($A3015,'Import data'!$A:$A,0),1)","v":{"$error":"#N/A"}}]
[0,{"$f":"INDEX('Import data'!$A:$A,MATCH($A3016,'Import data'!$A:$A,0),1)","v":{"$error":"#N/A"}}]
[0,{"$f":"INDEX('Import data'!$A:$A,MATCH($A3017,'Import data'!$A:$A,0),1)","v":{"$error":"#N/A"}}]
[0,{"$f":"INDEX('Import data'!$A:$A,MATCH($A3018,'Import data'!$A:$A,0),1)","v":{"$error":"#N/A"}}]
[0,{"$f":"INDEX('Import data'!$A:$A,MATCH($A3019,'Import data'!$A:$A,0),1)","v":{"$error":"#N/A"}}]
[0,{"$f":"INDEX('Import data'!$A:$A,MATCH($A3020,'Import data'!$A:$A,0),1)","v":{"$error":"#N/A"}}]
[0,{"$f":"INDEX('Import data'!$A:$A,MATCH($A3021,'Import data'!$A:$A,0),1)","v":{"$error":"#N/A"}}]
[0,{"$f":"INDEX('Import data'!$A:$A,MATCH($A3022,'Import data'!$A:$A,0),1)","v":{"$error":"#N/A"}}]
[0,{"$f":"INDEX('Import data'!$A:$A,MATCH($A3023,'Import data'!$A:$A,0),1)","v":{"$error":"#N/A"}}]
[0,{"$f":"INDEX('Import data'!$A:$A,MATCH($A3024,'Import data'!$A:$A,0),1)","v":{"$error":"#N/A"}}]
[0,{"$f":"INDEX('Import data'!$A:$A,MATCH($A3025,'Import data'!$A:$A,0),1)","v":{"$error":"#N/A"}}]
[0,{"$f":"INDEX('Import data'!$A:$A,MATCH($A3026,'Import data'!$A:$A,0),1)","v":{"$error":"#N/A"}}]
[0,{"$f":"INDEX('Import data'!$A:$A,MATCH($A3027,'Import data'!$A:$A,0),1)","v":{"$error":"#N/A"}}]
[0,{"$f":"INDEX('Import data'!$A:$A,MATCH($A3028,'Import data'!$A:$A,0),1)","v":{"$error":"#N/A"}}]
[0,{"$f":"INDEX('Import data'!$A:$A,MATCH($A3029,'Import data'!$A:$A,0),1)","v":{"$error":"#N/A"}}]
[0,{"$f":"INDEX('Import data'!$A:$A,MATCH($A3030,'Import data'!$A:$A,0),1)","v":{"$error":"#N/A"}}]
[0,{"$f":"INDEX('Import data'!$A:$A,MATCH($A3031,'Import data'!$A:$A,0),1)","v":{"$error":"#N/A"}}]
[0,{"$f":"INDEX('Import data'!$A:$A,MATCH($A3032,'Import data'!$A:$A,0),1)","v":{"$error":"#N/A"}}]
[0,{"$f":"INDEX('Import data'!$A:$A,MATCH($A3033,'Import data'!$A:$A,0),1)","v":{"$error":"#N/A"}}]
[0,{"$f":"INDEX('Import data'!$A:$A,MATCH($A3034,'Import data'!$A:$A,0),1)","v":{"$error":"#N/A"}}]
[0,{"$f":"INDEX('Import data'!$A:$A,MATCH($A3035,'Import data'!$A:$A,0),1)","v":{"$error":"#N/A"}}]
[0,{"$f":"INDEX('Import data'!$A:$A,MATCH($A3036,'Import data'!$A:$A,0),1)","v":{"$error":"#N/A"}}]
[0,{"$f":"INDEX('Import data'!$A:$A,MATCH($A3037,'Import data'!$A:$A,0),1)","v":{"$error":"#N/A"}}]
[0,{"$f":"INDEX('Import data'!$A:$A,MATCH($A3038,'Import data'!$A:$A,0),1)","v":{"$error":"#N/A"}}]
[0,{"$f":"INDEX('Import data'!$A:$A,MATCH($A3039,'Import data'!$A:$A,0),1)","v":{"$error":"#N/A"}}]
[0,{"$f":"INDEX('Import data'!$A:$A,MATCH($A3040,'Import data'!$A:$A,0),1)","v":{"$error":"#N/A"}}]
[0,{"$f":"INDEX('Import data'!$A:$A,MATCH($A3041,'Import data'!$A:$A,0),1)","v":{"$error":"#N/A"}}]
[0,{"$f":"INDEX('Import data'!$A:$A,MATCH($A3042,'Import data'!$A:$A,0),1)","v":{"$error":"#N/A"}}]
[0,{"$f":"INDEX('Import data'!$A:$A,MATCH($A3043,'Import data'!$A:$A,0),1)","v":{"$error":"#N/A"}}]
[0,{"$f":"INDEX('Import data'!$A:$A,MATCH($A3044,'Import data'!$A:$A,0),1)","v":{"$error":"#N/A"}}]
[0,{"$f":"INDEX('Import data'!$A:$A,MATCH($A3045,'Import data'!$A:$A,0),1)","v":{"$error":"#N/A"}}]
[0,{"$f":"INDEX('Import data'!$A:$A,MATCH($A3046,'Import data'!$A:$A,0),1)","v":{"$error":"#N/A"}}]
[0,{"$f":"INDEX('Import data'!$A:$A,MATCH($A3047,'Import data'!$A:$A,0),1)","v":{"$error":"#N/A"}}]
[0,{"$f":"INDEX('Import data'!$A:$A,MATCH($A3048,'Import data'!$A:$A,0),1)","v":{"$error":"#N/A"}}]
[0,{"$f":"INDEX('Import data'!$A:$A,MATCH($A3049,'Import data'!$A:$A,0),1)","v":{"$error":"#N/A"}}]
[0,{"$f":"INDEX('Import data'!$A:$A,MATCH($A3050,'Import data'!$A:$A,0),1)","v":{"$error":"#N/A"}}]
[0,{"$f":"INDEX('Import data'!$A:$A,MATCH($A3051,'Import data'!$A:$A,0),1)","v":{"$error":"#N/A"}}]
[0,{"$f":"INDEX('Import data'!$A:$A,MATCH($A3052,'Import data'!$A:$A,0),1)","v":{"$error":"#N/A"}}]
[0,{"$f":"INDEX('Import data'!$A:$A,MATCH($A3053,'Import data'!$A:$A,0),1)","v":{"$error":"#N/A"}}]
[0,{"$f":"INDEX('Import data'!$A:$A,MATCH($A3054,'Import data'!$A:$A,0),1)","v":{"$error":"#N/A"}}]
[0,{"$f":"INDEX('Import data'!$A:$A,MATCH($A3055,'Import data'!$A:$A,0),1)","v":{"$error":"#N/A"}}]
[0,{"$f":"INDEX('Import data'!$A:$A,MATCH($A3056,'Import data'!$A:$A,0),1)","v":{"$error":"#N/A"}}]
[0,{"$f":"INDEX('Import data'!$A:$A,MATCH($A3057,'Import data'!$A:$A,0),1)","v":{"$error":"#N/A"}}]
[0,{"$f":"INDEX('Import data'!$A:$A,MATCH($A3058,'Import data'!$A:$A,0),1)","v":{"$error":"#N/A"}}]
[0,{"$f":"INDEX('Import data'!$A:$A,MATCH($A3059,'Import data'!$A:$A,0),1)","v":{"$error":"#N/A"}}]
[0,{"$f":"INDEX('Import data'!$A:$A,MATCH($A3060,'Import data'!$A:$A,0),1)","v":{"$error":"#N/A"}}]
[0,{"$f":"INDEX('Import data'!$A:$A,MATCH($A3061,'Import data'!$A:$A,0),1)","v":{"$error":"#N/A"}}]
[0,{"$f":"INDEX('Import data'!$A:$A,MATCH($A3062,'Import data'!$A:$A,0),1)","v":{"$error":"#N/A"}}]
[0,{"$f":"INDEX('Import data'!$A:$A,MATCH($A3063,'Import data'!$A:$A,0),1)","v":{"$error":"#N/A"}}]
[0,{"$f":"INDEX('Import data'!$A:$A,MATCH($A3064,'Import data'!$A:$A,0),1)","v":{"$error":"#N/A"}}]
[0,{"$f":"INDEX('Import data'!$A:$A,MATCH($A3065,'Import data'!$A:$A,0),1)","v":{"$error":"#N/A"}}]
[0,{"$f":"INDEX('Import data'!$A:$A,MATCH($A3066,'Import data'!$A:$A,0),1)","v":{"$error":"#N/A"}}]
[0,{"$f":"INDEX('Import data'!$A:$A,MATCH($A3067,'Import data'!$A:$A,0),1)","v":{"$error":"#N/A"}}]
[0,{"$f":"INDEX('Import data'!$A:$A,MATCH($A3068,'Import data'!$A:$A,0),1)","v":{"$error":"#N/A"}}]
[0,{"$f":"INDEX('Import data'!$A:$A,MATCH($A3069,'Import data'!$A:$A,0),1)","v":{"$error":"#N/A"}}]
[0,{"$f":"INDEX('Import data'!$A:$A,MATCH($A3070,'Import data'!$A:$A,0),1)","v":{"$error":"#N/A"}}]
[0,{"$f":"INDEX('Import data'!$A:$A,MATCH($A3071,'Import data'!$A:$A,0),1)","v":{"$error":"#N/A"}}]
[0,{"$f":"INDEX('Import data'!$A:$A,MATCH($A3072,'Import data'!$A:$A,0),1)","v":{"$error":"#N/A"}}]
[0,{"$f":"INDEX('Import data'!$A:$A,MATCH($A3073,'Import data'!$A:$A,0),1)","v":{"$error":"#N/A"}}]
[0,{"$f":"INDEX('Import data'!$A:$A,MATCH($A3074,'Import data'!$A:$A,0),1)","v":{"$error":"#N/A"}}]
[{"$f":"ID","v":0},{"$f":"INDEX('Import data'!$A:$A,MATCH($A3075,'Import data'!$A:$A,0),1)","v":{"$error":"#N/A"}}]
[0,{"$f":"INDEX('Import data'!$A:$A,MATCH($A3076,'Import data'!$A:$A,0),1)","v":{"$error":"#N/A"}}]
[0,{"$f":"INDEX('Import data'!$A:$A,MATCH($A3077,'Import data'!$A:$A,0),1)","v":{"$error":"#N/A"}}]
[0,{"$f":"INDEX('Import data'!$A:$A,MATCH($A3078,'Import data'!$A:$A,0),1)","v":{"$error":"#N/A"}}]
[0,{"$f":"INDEX('Import data'!$A:$A,MATCH($A3079,'Import data'!$A:$A,0),1)","v":{"$error":"#N/A"}}]
[0,{"$f":"INDEX('Import data'!$A:$A,MATCH($A3080,'Import data'!$A:$A,0),1)","v":{"$error":"#N/A"}}]
[0,{"$f":"INDEX('Import data'!$A:$A,MATCH($A3081,'Import data'!$A:$A,0),1)","v":{"$error":"#N/A"}}]
[0,{"$f":"INDEX('Import data'!$A:$A,MATCH($A3082,'Import data'!$A:$A,0),1)","v":{"$error":"#N/A"}}]
[0,{"$f":"INDEX('Import data'!$A:$A,MATCH($A3083,'Import data'!$A:$A,0),1)","v":{"$error":"#N/A"}}]
[0,{"$f":"INDEX('Import data'!$A:$A,MATCH($A3084,'Import data'!$A:$A,0),1)","v":{"$error":"#N/A"}}]
[0,{"$f":"INDEX('Import data'!$A:$A,MATCH($A3085,'Import data'!$A:$A,0),1)","v":{"$error":"#N/A"}}]
[0,{"$f":"INDEX('Import data'!$A:$A,MATCH($A3086,'Import data'!$A:$A,0),1)","v":{"$error":"#N/A"}}]
[0,{"$f":"INDEX('Import data'!$A:$A,MATCH($A3087,'Import data'!$A:$A,0),1)","v":{"$error":"#N/A"}}]
[0,{"$f":"INDEX('Import data'!$A:$A,MATCH($A3088,'Import data'!$A:$A,0),1)","v":{"$error":"#N/A"}}]
[0,{"$f":"INDEX('Import data'!$A:$A,MATCH($A3089,'Import data'!$A:$A,0),1)","v":{"$error":"#N/A"}}]
[0,{"$f":"INDEX('Import data'!$A:$A,MATCH($A3090,'Import data'!$A:$A,0),1)","v":{"$error":"#N/A"}}]
[0,{"$f":"INDEX('Import data'!$A:$A,MATCH($A3091,'Import data'!$A:$A,0),1)","v":{"$error":"#N/A"}}]
[0,{"$f":"INDEX('Import data'!$A:$A,MATCH($A3092,'Import data'!$A:$A,0),1)","v":{"$error":"#N/A"}}]
[0,{"$f":"INDEX('Import data'!$A:$A,MATCH($A3093,'Import data'!$A:$A,0),1)","v":{"$error":"#N/A"}}]
[0,{"$f":"INDEX('Import data'!$A:$A,MATCH($A3094,'Import data'!$A:$A,0),1)","v":{"$error":"#N/A"}}]
[0,{"$f":"INDEX('Import data'!$A:$A,MATCH($A3095,'Import data'!$A:$A,0),1)","v":{"$error":"#N/A"}}]
[0,{"$f":"INDEX('Import data'!$A:$A,MATCH($A3096,'Import data'!$A:$A,0),1)","v":{"$error":"#N/A"}}]
[0,{"$f":"INDEX('Import data'!$A:$A,MATCH($A3097,'Import data'!$A:$A,0),1)","v":{"$error":"#N/A"}}]
[0,{"$f":"INDEX('Import data'!$A:$A,MATCH($A3098,'Import data'!$A:$A,0),1)","v":{"$error":"#N/A"}}]
[0,{"$f":"INDEX('Import data'!$A:$A,MATCH($A3099,'Import data'!$A:$A,0),1)","v":{"$error":"#N/A"}}]
[0,{"$f":"INDEX('Import data'!$A:$A,MATCH($A3100,'Import data'!$A:$A,0),1)","v":{"$error":"#N/A"}}]
[0,{"$f":"INDEX('Import data'!$A:$A,MATCH($A3101,'Import data'!$A:$A,0),1)","v":{"$error":"#N/A"}}]
[0,{"$f":"INDEX('Import data'!$A:$A,MATCH($A3102,'Import data'!$A:$A,0),1)","v":{"$error":"#N/A"}}]
[0,{"$f":"INDEX('Import data'!$A:$A,MATCH($A3103,'Import data'!$A:$A,0),1)","v":{"$error":"#N/A"}}]
[0,{"$f":"INDEX('Import data'!$A:$A,MATCH($A3104,'Import data'!$A:$A,0),1)","v":{"$error":"#N/A"}}]
[0,{"$f":"INDEX('Import data'!$A:$A,MATCH($A3105,'Import data'!$A:$A,0),1)","v":{"$error":"#N/A"}}]
[0,{"$f":"INDEX('Import data'!$A:$A,MATCH($A3106,'Import data'!$A:$A,0),1)","v":{"$error":"#N/A"}}]
[0,{"$f":"INDEX('Import data'!$A:$A,MATCH($A3107,'Import data'!$A:$A,0),1)","v":{"$error":"#N/A"}}]
[0,{"$f":"INDEX('Import data'!$A:$A,MATCH($A3108,'Import data'!$A:$A,0),1)","v":{"$error":"#N/A"}}]
[0,{"$f":"INDEX('Import data'!$A:$A,MATCH($A3109,'Import data'!$A:$A,0),1)","v":{"$error":"#N/A"}}]
[0,{"$f":"INDEX('Import data'!$A:$A,MATCH($A3110,'Import data'!$A:$A,0),1)","v":{"$error":"#N/A"}}]
[0,{"$f":"INDEX('Import data'!$A:$A,MATCH($A3111,'Import data'!$A:$A,0),1)","v":{"$error":"#N/A"}}]
[0,{"$f":"INDEX('Import data'!$A:$A,MATCH($A3112,'Import data'!$A:$A,0),1)","v":{"$error":"#N/A"}}]
[0,{"$f":"INDEX('Import data'!$A:$A,MATCH($A3113,'Import data'!$A:$A,0),1)","v":{"$error":"#N/A"}}]
[0,{"$f":"INDEX('Import data'!$A:$A,MATCH($A3114,'Import data'!$A:$A,0),1)","v":{"$error":"#N/A"}}]
[0,{"$f":"INDEX('Import data'!$A:$A,MATCH($A3115,'Import data'!$A:$A,0),1)","v":{"$error":"#N/A"}}]
[0,{"$f":"INDEX('Import data'!$A:$A,MATCH($A3116,'Import data'!$A:$A,0),1)","v":{"$error":"#N/A"}}]
[0,{"$f":"INDEX('Import data'!$A:$A,MATCH($A3117,'Import data'!$A:$A,0),1)","v":{"$error":"#N/A"}}]
[0,{"$f":"INDEX('Import data'!$A:$A,MATCH($A3118,'Import data'!$A:$A,0),1)","v":{"$error":"#N/A"}}]
[0,{"$f":"INDEX('Import data'!$A:$A,MATCH($A3119,'Import data'!$A:$A,0),1)","v":{"$error":"#N/A"}}]
[0,{"$f":"INDEX('Import data'!$A:$A,MATCH($A3120,'Import data'!$A:$A,0),1)","v":{"$error":"#N/A"}}]
[0,{"$f":"INDEX('Import data'!$A:$A,MATCH($A3121,'Import data'!$A:$A,0),1)","v":{"$error":"#N/A"}}]
[0,{"$f":"INDEX('Import data'!$A:$A,MATCH($A3122,'Import data'!$A:$A,0),1)","v":{"$error":"#N/A"}}]
[0,{"$f":"INDEX('Import data'!$A:$A,MATCH($A3123,'Import data'!$A:$A,0),1)","v":{"$error":"#N/A"}}]
[0,{"$f":"INDEX('Import data'!$A:$A,MATCH($A3124,'Import data'!$A:$A,0),1)","v":{"$error":"#N/A"}}]
[0,{"$f":"INDEX('Import data'!$A:$A,MATCH($A3125,'Import data'!$A:$A,0),1)","v":{"$error":"#N/A"}}]
[0,{"$f":"INDEX('Import data'!$A:$A,MATCH($A3126,'Import data'!$A:$A,0),1)","v":{"$error":"#N/A"}}]
[0,{"$f":"INDEX('Import data'!$A:$A,MATCH($A3127,'Import data'!$A:$A,0),1)","v":{"$error":"#N/A"}}]
[0,{"$f":"INDEX('Import data'!$A:$A,MATCH($A3128,'Import data'!$A:$A,0),1)","v":{"$error":"#N/A"}}]
[0,{"$f":"INDEX('Import data'!$A:$A,MATCH($A3129,'Import data'!$A:$A,0),1)","v":{"$error":"#N/A"}}]
[0,{"$f":"INDEX('Import data'!$A:$A,MATCH($A3130,'Import data'!$A:$A,0),1)","v":{"$error":"#N/A"}}]
[0,{"$f":"INDEX('Import data'!$A:$A,MATCH($A3131,'Import data'!$A:$A,0),1)","v":{"$error":"#N/A"}}]
[0,{"$f":"INDEX('Import data'!$A:$A,MATCH($A3132,'Import data'!$A:$A,0),1)","v":{"$error":"#N/A"}}]
[0,{"$f":"INDEX('Import data'!$A:$A,MATCH($A3133,'Import data'!$A:$A,0),1)","v":{"$error":"#N/A"}}]
[0,{"$f":"INDEX('Import data'!$A:$A,MATCH($A3134,'Import data'!$A:$A,0),1)","v":{"$error":"#N/A"}}]
[0,{"$f":"INDEX('Import data'!$A:$A,MATCH($A3135,'Import data'!$A:$A,0),1)","v":{"$error":"#N/A"}}]
[0,{"$f":"INDEX('Import data'!$A:$A,MATCH($A3136,'Import data'!$A:$A,0),1)","v":{"$error":"#N/A"}}]
[0,{"$f":"INDEX('Import data'!$A:$A,MATCH($A3137,'Import data'!$A:$A,0),1)","v":{"$error":"#N/A"}}]
[0,{"$f":"INDEX('Import data'!$A:$A,MATCH($A3138,'Import data'!$A:$A,0),1)","v":{"$error":"#N/A"}}]
[{"$f":"ID","v":0},{"$f":"INDEX('Import data'!$A:$A,MATCH($A3139,'Import data'!$A:$A,0),1)","v":{"$error":"#N/A"}}]
[0,{"$f":"INDEX('Import data'!$A:$A,MATCH($A3140,'Import data'!$A:$A,0),1)","v":{"$error":"#N/A"}}]
[0,{"$f":"INDEX('Import data'!$A:$A,MATCH($A3141,'Import data'!$A:$A,0),1)","v":{"$error":"#N/A"}}]
[0,{"$f":"INDEX('Import data'!$A:$A,MATCH($A3142,'Import data'!$A:$A,0),1)","v":{"$error":"#N/A"}}]
[0,{"$f":"INDEX('Import data'!$A:$A,MATCH($A3143,'Import data'!$A:$A,0),1)","v":{"$error":"#N/A"}}]
[0,{"$f":"INDEX('Import data'!$A:$A,MATCH($A3144,'Import data'!$A:$A,0),1)","v":{"$error":"#N/A"}}]
[0,{"$f":"INDEX('Import data'!$A:$A,MATCH($A3145,'Import data'!$A:$A,0),1)","v":{"$error":"#N/A"}}]
[0,{"$f":"INDEX('Import data'!$A:$A,MATCH($A3146,'Import data'!$A:$A,0),1)","v":{"$error":"#N/A"}}]
[0,{"$f":"INDEX('Import data'!$A:$A,MATCH($A3147,'Import data'!$A:$A,0),1)","v":{"$error":"#N/A"}}]
[0,{"$f":"INDEX('Import data'!$A:$A,MATCH($A3148,'Import data'!$A:$A,0),1)","v":{"$error":"#N/A"}}]
[0,{"$f":"INDEX('Import data'!$A:$A,MATCH($A3149,'Import data'!$A:$A,0),1)","v":{"$error":"#N/A"}}]
[0,{"$f":"INDEX('Import data'!$A:$A,MATCH($A3150,'Import data'!$A:$A,0),1)","v":{"$error":"#N/A"}}]
[0,{"$f":"INDEX('Import data'!$A:$A,MATCH($A3151,'Import data'!$A:$A,0),1)","v":{"$error":"#N/A"}}]
[0,{"$f":"INDEX('Import data'!$A:$A,MATCH($A3152,'Import data'!$A:$A,0),1)","v":{"$error":"#N/A"}}]
[0,{"$f":"INDEX('Import data'!$A:$A,MATCH($A3153,'Import data'!$A:$A,0),1)","v":{"$error":"#N/A"}}]
[0,{"$f":"INDEX('Import data'!$A:$A,MATCH($A3154,'Import data'!$A:$A,0),1)","v":{"$error":"#N/A"}}]
[0,{"$f":"INDEX('Import data'!$A:$A,MATCH($A3155,'Import data'!$A:$A,0),1)","v":{"$error":"#N/A"}}]
[0,{"$f":"INDEX('Import data'!$A:$A,MATCH($A3156,'Import data'!$A:$A,0),1)","v":{"$error":"#N/A"}}]
[0,{"$f":"INDEX('Import data'!$A:$A,MATCH($A3157,'Import data'!$A:$A,0),1)","v":{"$error":"#N/A"}}]
[0,{"$f":"INDEX('Import data'!$A:$A,MATCH($A3158,'Import data'!$A:$A,0),1)","v":{"$error":"#N/A"}}]
[0,{"$f":"INDEX('Import data'!$A:$A,MATCH($A3159,'Import data'!$A:$A,0),1)","v":{"$error":"#N/A"}}]
[0,{"$f":"INDEX('Import data'!$A:$A,MATCH($A3160,'Import data'!$A:$A,0),1)","v":{"$error":"#N/A"}}]
[0,{"$f":"INDEX('Import data'!$A:$A,MATCH($A3161,'Import data'!$A:$A,0),1)","v":{"$error":"#N/A"}}]
[0,{"$f":"INDEX('Import data'!$A:$A,MATCH($A3162,'Import data'!$A:$A,0),1)","v":{"$error":"#N/A"}}]
[0,{"$f":"INDEX('Import data'!$A:$A,MATCH($A3163,'Import data'!$A:$A,0),1)","v":{"$error":"#N/A"}}]
[0,{"$f":"INDEX('Import data'!$A:$A,MATCH($A3164,'Import data'!$A:$A,0),1)","v":{"$error":"#N/A"}}]
[0,{"$f":"INDEX('Import data'!$A:$A,MATCH($A3165,'Import data'!$A:$A,0),1)","v":{"$error":"#N/A"}}]
[0,{"$f":"INDEX('Import data'!$A:$A,MATCH($A3166,'Import data'!$A:$A,0),1)","v":{"$error":"#N/A"}}]
[0,{"$f":"INDEX('Import data'!$A:$A,MATCH($A3167,'Import data'!$A:$A,0),1)","v":{"$error":"#N/A"}}]
[0,{"$f":"INDEX('Import data'!$A:$A,MATCH($A3168,'Import data'!$A:$A,0),1)","v":{"$error":"#N/A"}}]
[0,{"$f":"INDEX('Import data'!$A:$A,MATCH($A3169,'Import data'!$A:$A,0),1)","v":{"$error":"#N/A"}}]
[0,{"$f":"INDEX('Import data'!$A:$A,MATCH($A3170,'Import data'!$A:$A,0),1)","v":{"$error":"#N/A"}}]
[0,{"$f":"INDEX('Import data'!$A:$A,MATCH($A3171,'Import data'!$A:$A,0),1)","v":{"$error":"#N/A"}}]
[0,{"$f":"INDEX('Import data'!$A:$A,MATCH($A3172,'Import data'!$A:$A,0),1)","v":{"$error":"#N/A"}}]
[0,{"$f":"INDEX('Import data'!$A:$A,MATCH($A3173,'Import data'!$A:$A,0),1)","v":{"$error":"#N/A"}}]
[0,{"$f":"INDEX('Import data'!$A:$A,MATCH($A3174,'Import data'!$A:$A,0),1)","v":{"$error":"#N/A"}}]
[0,{"$f":"INDEX('Import data'!$A:$A,MATCH($A3175,'Import data'!$A:$A,0),1)","v":{"$error":"#N/A"}}]
[0,{"$f":"INDEX('Import data'!$A:$A,MATCH($A3176,'Import data'!$A:$A,0),1)","v":{"$error":"#N/A"}}]
[0,{"$f":"INDEX('Import data'!$A:$A,MATCH($A3177,'Import data'!$A:$A,0),1)","v":{"$error":"#N/A"}}]
[0,{"$f":"INDEX('Import data'!$A:$A,MATCH($A3178,'Import data'!$A:$A,0),1)","v":{"$error":"#N/A"}}]
[0,{"$f":"INDEX('Import data'!$A:$A,MATCH($A3179,'Import data'!$A:$A,0),1)","v":{"$error":"#N/A"}}]
[0,{"$f":"INDEX('Import data'!$A:$A,MATCH($A3180,'Import data'!$A:$A,0),1)","v":{"$error":"#N/A"}}]
[0,{"$f":"INDEX('Import data'!$A:$A,MATCH($A3181,'Import data'!$A:$A,0),1)","v":{"$error":"#N/A"}}]
[0,{"$f":"INDEX('Import data'!$A:$A,MATCH($A3182,'Import data'!$A:$A,0),1)","v":{"$error":"#N/A"}}]
[0,{"$f":"INDEX('Import data'!$A:$A,MATCH($A3183,'Import data'!$A:$A,0),1)","v":{"$error":"#N/A"}}]
[0,{"$f":"INDEX('Import data'!$A:$A,MATCH($A3184,'Import data'!$A:$A,0),1)","v":{"$error":"#N/A"}}]
[0,{"$f":"INDEX('Import data'!$A:$A,MATCH($A3185,'Import data'!$A:$A,0),1)","v":{"$error":"#N/A"}}]
[0,{"$f":"INDEX('Import data'!$A:$A,MATCH($A3186,'Import data'!$A:$A,0),1)","v":{"$error":"#N/A"}}]
[0,{"$f":"INDEX('Import data'!$A:$A,MATCH($A3187,'Import data'!$A:$A,0),1)","v":{"$error":"#N/A"}}]
[0,{"$f":"INDEX('Import data'!$A:$A,MATCH($A3188,'Import data'!$A:$A,0),1)","v":{"$error":"#N/A"}}]
[0,{"$f":"INDEX('Import data'!$A:$A,MATCH($A3189,'Import data'!$A:$A,0),1)","v":{"$error":"#N/A"}}]
[0,{"$f":"INDEX('Import data'!$A:$A,MATCH($A3190,'Import data'!$A:$A,0),1)","v":{"$error":"#N/A"}}]
[0,{"$f":"INDEX('Import data'!$A:$A,MATCH($A3191,'Import data'!$A:$A,0),1)","v":{"$error":"#N/A"}}]
[0,{"$f":"INDEX('Import data'!$A:$A,MATCH($A3192,'Import data'!$A:$A,0),1)","v":{"$error":"#N/A"}}]
[0,{"$f":"INDEX('Import data'!$A:$A,MATCH($A3193,'Import data'!$A:$A,0),1)","v":{"$error":"#N/A"}}]
[0,{"$f":"INDEX('Import data'!$A:$A,MATCH($A3194,'Import data'!$A:$A,0),1)","v":{"$error":"#N/A"}}]
[0,{"$f":"INDEX('Import data'!$A:$A,MATCH($A3195,'Import data'!$A:$A,0),1)","v":{"$error":"#N/A"}}]
[0,{"$f":"INDEX('Import data'!$A:$A,MATCH($A3196,'Import data'!$A:$A,0),1)","v":{"$error":"#N/A"}}]
[0,{"$f":"INDEX('Import data'!$A:$A,MATCH($A3197,'Import data'!$A:$A,0),1)","v":{"$error":"#N/A"}}]
[0,{"$f":"INDEX('Import data'!$A:$A,MATCH($A3198,'Import data'!$A:$A,0),1)","v":{"$error":"#N/A"}}]
[0,{"$f":"INDEX('Import data'!$A:$A,MATCH($A3199,'Import data'!$A:$A,0),1)","v":{"$error":"#N/A"}}]
[0,{"$f":"INDEX('Import data'!$A:$A,MATCH($A3200,'Import data'!$A:$A,0),1)","v":{"$error":"#N/A"}}]
[0,{"$f":"INDEX('Import data'!$A:$A,MATCH($A3201,'Import data'!$A:$A,0),1)","v":{"$error":"#N/A"}}]
[0,{"$f":"INDEX('Import data'!$A:$A,MATCH($A3202,'Import data'!$A:$A,0),1)","v":{"$error":"#N/A"}}]
[{"$f":"ID","v":0},{"$f":"INDEX('Import data'!$A:$A,MATCH($A3203,'Import data'!$A:$A,0),1)","v":{"$error":"#N/A"}}]
[0,{"$f":"INDEX('Import data'!$A:$A,MATCH($A3204,'Import data'!$A:$A,0),1)","v":{"$error":"#N/A"}}]
[0,{"$f":"INDEX('Import data'!$A:$A,MATCH($A3205,'Import data'!$A:$A,0),1)","v":{"$error":"#N/A"}}]
[0,{"$f":"INDEX('Import data'!$A:$A,MATCH($A3206,'Import data'!$A:$A,0),1)","v":{"$error":"#N/A"}}]
[0,{"$f":"INDEX('Import data'!$A:$A,MATCH($A3207,'Import data'!$A:$A,0),1)","v":{"$error":"#N/A"}}]
[0,{"$f":"INDEX('Import data'!$A:$A,MATCH($A3208,'Import data'!$A:$A,0),1)","v":{"$error":"#N/A"}}]
[0,{"$f":"INDEX('Import data'!$A:$A,MATCH($A3209,'Import data'!$A:$A,0),1)","v":{"$error":"#N/A"}}]
[0,{"$f":"INDEX('Import data'!$A:$A,MATCH($A3210,'Import data'!$A:$A,0),1)","v":{"$error":"#N/A"}}]
[0,{"$f":"INDEX('Import data'!$A:$A,MATCH($A3211,'Import data'!$A:$A,0),1)","v":{"$error":"#N/A"}}]
[0,{"$f":"INDEX('Import data'!$A:$A,MATCH($A3212,'Import data'!$A:$A,0),1)","v":{"$error":"#N/A"}}]
[0,{"$f":"INDEX('Import data'!$A:$A,MATCH($A3213,'Import data'!$A:$A,0),1)","v":{"$error":"#N/A"}}]
[0,{"$f":"INDEX('Import data'!$A:$A,MATCH($A3214,'Import data'!$A:$A,0),1)","v":{"$error":"#N/A"}}]
[0,{"$f":"INDEX('Import data'!$A:$A,MATCH($A3215,'Import data'!$A:$A,0),1)","v":{"$error":"#N/A"}}]
[0,{"$f":"INDEX('Import data'!$A:$A,MATCH($A3216,'Import data'!$A:$A,0),1)","v":{"$error":"#N/A"}}]
[0,{"$f":"INDEX('Import data'!$A:$A,MATCH($A3217,'Import data'!$A:$A,0),1)","v":{"$error":"#N/A"}}]
[0,{"$f":"INDEX('Import data'!$A:$A,MATCH($A3218,'Import data'!$A:$A,0),1)","v":{"$error":"#N/A"}}]
[0,{"$f":"INDEX('Import data'!$A:$A,MATCH($A3219,'Import data'!$A:$A,0),1)","v":{"$error":"#N/A"}}]
[0,{"$f":"INDEX('Import data'!$A:$A,MATCH($A3220,'Import data'!$A:$A,0),1)","v":{"$error":"#N/A"}}]
[0,{"$f":"INDEX('Import data'!$A:$A,MATCH($A3221,'Import data'!$A:$A,0),1)","v":{"$error":"#N/A"}}]
[0,{"$f":"INDEX('Import data'!$A:$A,MATCH($A3222,'Import data'!$A:$A,0),1)","v":{"$error":"#N/A"}}]
[0,{"$f":"INDEX('Import data'!$A:$A,MATCH($A3223,'Import data'!$A:$A,0),1)","v":{"$error":"#N/A"}}]
[0,{"$f":"INDEX('Import data'!$A:$A,MATCH($A3224,'Import data'!$A:$A,0),1)","v":{"$error":"#N/A"}}]
[0,{"$f":"INDEX('Import data'!$A:$A,MATCH($A3225,'Import data'!$A:$A,0),1)","v":{"$error":"#N/A"}}]
[0,{"$f":"INDEX('Import data'!$A:$A,MATCH($A3226,'Import data'!$A:$A,0),1)","v":{"$error":"#N/A"}}]
[0,{"$f":"INDEX('Import data'!$A:$A,MATCH($A3227,'Import data'!$A:$A,0),1)","v":{"$error":"#N/A"}}]
[0,{"$f":"INDEX('Import data'!$A:$A,MATCH($A3228,'Import data'!$A:$A,0),1)","v":{"$error":"#N/A"}}]
[0,{"$f":"INDEX('Import data'!$A:$A,MATCH($A3229,'Import data'!$A:$A,0),1)","v":{"$error":"#N/A"}}]
[0,{"$f":"INDEX('Import data'!$A:$A,MATCH($A3230,'Import data'!$A:$A,0),1)","v":{"$error":"#N/A"}}]
[0,{"$f":"INDEX('Import data'!$A:$A,MATCH($A3231,'Import data'!$A:$A,0),1)","v":{"$error":"#N/A"}}]
[0,{"$f":"INDEX('Import data'!$A:$A,MATCH($A3232,'Import data'!$A:$A,0),1)","v":{"$error":"#N/A"}}]
[0,{"$f":"INDEX('Import data'!$A:$A,MATCH($A3233,'Import data'!$A:$A,0),1)","v":{"$error":"#N/A"}}]
[0,{"$f":"INDEX('Import data'!$A:$A,MATCH($A3234,'Import data'!$A:$A,0),1)","v":{"$error":"#N/A"}}]
[0,{"$f":"INDEX('Import data'!$A:$A,MATCH($A3235,'Import data'!$A:$A,0),1)","v":{"$error":"#N/A"}}]
[0,{"$f":"INDEX('Import data'!$A:$A,MATCH($A3236,'Import data'!$A:$A,0),1)","v":{"$error":"#N/A"}}]
[0,{"$f":"INDEX('Import data'!$A:$A,MATCH($A3237,'Import data'!$A:$A,0),1)","v":{"$error":"#N/A"}}]
[0,{"$f":"INDEX('Import data'!$A:$A,MATCH($A3238,'Import data'!$A:$A,0),1)","v":{"$error":"#N/A"}}]
[0,{"$f":"INDEX('Import data'!$A:$A,MATCH($A3239,'Import data'!$A:$A,0),1)","v":{"$error":"#N/A"}}]
[0,{"$f":"INDEX('Import data'!$A:$A,MATCH($A3240,'Import data'!$A:$A,0),1)","v":{"$error":"#N/A"}}]
[0,{"$f":"INDEX('Import data'!$A:$A,MATCH($A3241,'Import data'!$A:$A,0),1)","v":{"$error":"#N/A"}}]
[0,{"$f":"INDEX('Import data'!$A:$A,MATCH($A3242,'Import data'!$A:$A,0),1)","v":{"$error":"#N/A"}}]
[0,{"$f":"INDEX('Import data'!$A:$A,MATCH($A3243,'Import data'!$A:$A,0),1)","v":{"$error":"#N/A"}}]
[0,{"$f":"INDEX('Import data'!$A:$A,MATCH($A3244,'Import data'!$A:$A,0),1)","v":{"$error":"#N/A"}}]
[0,{"$f":"INDEX('Import data'!$A:$A,MATCH($A3245,'Import data'!$A:$A,0),1)","v":{"$error":"#N/A"}}]
[0,{"$f":"INDEX('Import data'!$A:$A,MATCH($A3246,'Import data'!$A:$A,0),1)","v":{"$error":"#N/A"}}]
[0,{"$f":"INDEX('Import data'!$A:$A,MATCH($A3247,'Import data'!$A:$A,0),1)","v":{"$error":"#N/A"}}]
[0,{"$f":"INDEX('Import data'!$A:$A,MATCH($A3248,'Import data'!$A:$A,0),1)","v":{"$error":"#N/A"}}]
[0,{"$f":"INDEX('Import data'!$A:$A,MATCH($A3249,'Import data'!$A:$A,0),1)","v":{"$error":"#N/A"}}]
[0,{"$f":"INDEX('Import data'!$A:$A,MATCH($A3250,'Import data'!$A:$A,0),1)","v":{"$error":"#N/A"}}]
[0,{"$f":"INDEX('Import data'!$A:$A,MATCH($A3251,'Import data'!$A:$A,0),1)","v":{"$error":"#N/A"}}]
[0,{"$f":"INDEX('Import data'!$A:$A,MATCH($A3252,'Import data'!$A:$A,0),1)","v":{"$error":"#N/A"}}]
[0,{"$f":"INDEX('Import data'!$A:$A,MATCH($A3253,'Import data'!$A:$A,0),1)","v":{"$error":"#N/A"}}]
[0,{"$f":"INDEX('Import data'!$A:$A,MATCH($A3254,'Import data'!$A:$A,0),1)","v":{"$error":"#N/A"}}]
[0,{"$f":"INDEX('Import data'!$A:$A,MATCH($A3255,'Import data'!$A:$A,0),1)","v":{"$error":"#N/A"}}]
[0,{"$f":"INDEX('Import data'!$A:$A,MATCH($A3256,'Import data'!$A:$A,0),1)","v":{"$error":"#N/A"}}]
[0,{"$f":"INDEX('Import data'!$A:$A,MATCH($A3257,'Import data'!$A:$A,0),1)","v":{"$error":"#N/A"}}]
[0,{"$f":"INDEX('Import data'!$A:$A,MATCH($A3258,'Import data'!$A:$A,0),1)","v":{"$error":"#N/A"}}]
[0,{"$f":"INDEX('Import data'!$A:$A,MATCH($A3259,'Import data'!$A:$A,0),1)","v":{"$error":"#N/A"}}]
[0,{"$f":"INDEX('Import data'!$A:$A,MATCH($A3260,'Import data'!$A:$A,0),1)","v":{"$error":"#N/A"}}]
[0,{"$f":"INDEX('Import data'!$A:$A,MATCH($A3261,'Import data'!$A:$A,0),1)","v":{"$error":"#N/A"}}]
[0,{"$f":"INDEX('Import data'!$A:$A,MATCH($A3262,'Import data'!$A:$A,0),1)","v":{"$error":"#N/A"}}]
[0,{"$f":"INDEX('Import data'!$A:$A,MATCH($A3263,'Import data'!$A:$A,0),1)","v":{"$error":"#N/A"}}]
[0,{"$f":"INDEX('Import data'!$A:$A,MATCH($A3264,'Import data'!$A:$A,0),1)","v":{"$error":"#N/A"}}]
[0,{"$f":"INDEX('Import data'!$A:$A,MATCH($A3265,'Import data'!$A:$A,0),1)","v":{"$error":"#N/A"}}]
[0,{"$f":"INDEX('Import data'!$A:$A,MATCH($A3266,'Import data'!$A:$A,0),1)","v":{"$error":"#N/A"}}]
[0,{"$f":"INDEX('Import data'!$A:$A,MATCH($A3267,'Import data'!$A:$A,0),1)","v":{"$error":"#N/A"}}]
[0,{"$f":"INDEX('Import data'!$A:$A,MATCH($A3268,'Import data'!$A:$A,0),1)","v":{"$error":"#N/A"}}]
[0,{"$f":"INDEX('Import data'!$A:$A,MATCH($A3269,'Import data'!$A:$A,0),1)","v":{"$error":"#N/A"}}]
[0,{"$f":"INDEX('Import data'!$A:$A,MATCH($A3270,'Import data'!$A:$A,0),1)","v":{"$error":"#N/A"}}]
[0,{"$f":"INDEX('Import data'!$A:$A,MATCH($A3271,'Import data'!$A:$A,0),1)","v":{"$error":"#N/A"}}]

{"sheet":"BRYŁY FOTO","index":10,"n_rows":78,"n_cols":7,"rows_kept":78,"cut":false,"hidden":false,"merged":[]}
["id_brylafoto_slo","id_brylafoto","brylafoto","brylafoto_skrot","LumDistTypeID","DcLightDistributionId","Komentarz"]
[1,1,"Światło obrotowo symetryczne przysłonięte od góry.",null,1,7.3]
[2,2,"Światło obrotowo-symetryczne pośrednie.",null,2,9]
[3,3,"Światło przysłonięte od góry.",null,1,""]
[4,4,"Światło dwustronne: ukierunkowane do góry i w dół.","Up-Down",1,8,"Askery ściana Genewa Vasa"]
[5,5,"Światło jednostronne: ukierunkowane do góry lub w dół.",null,1,""]
[6,6,"Światło jednostronne: ukierunkowane w dół.","Down",1,7,"Światło rozproszone półsferyczne ukierunkowane w dół"]
[7,7,"Światło rozproszone.",null,1,8]
[8,8,"Światło rozproszone półsferyczne ukierunkowane w dół 1",null,1,7,"Światło rozproszone półsferyczne ukierunkowane w dół"]
[9,9,"Światło odkryte.",null,1,9]
[10,10,"Światło przysłonięte ukierunkowane ku dołowi.",null,1,7,"Światło rozproszone półsferyczne ukierunkowane w dół"]
[12,12,"Światło jednostronne: o kącie 60º do góry lub w dół.",null,1,10,"Lillehammer"]
[13,13,"Światło dwustronne: o kącie 60º do góry i w dół.","Up60º & Down60º",1,10,"Lillehammer Fysfjord"]
[14,14,"Światło dwustronne: o kącie 4º do góry i w dół.","Up4º & Down4º",1,10,"Lillehammery; Lysfjord VOSS"]
[15,15,"Światło jednostronne: o kącie 4º do góry lub w dół.",null,1,10,"lillehammer"]
[16,16,"Czterostronny wylot światła przysłonięty od góry.",null,1,4]
[17,17,"Światło obrotowo-symetryczne.",null,1,3]
[18,18,"Światło obrotowo - symetryczne pośrednie ukierunkowane w dół.",null,2,9]
[19,19,"Światło asymetryczne rozproszone ukierunkowane w dół.",null,1,6]
[20,20,"Światło symetryczne (kombinacja pośrednie/bezpośrednie).",null,1,9]
[21,21,"Światło symetryczne pośrednie.",null,2,9]
[22,22,"Światło dwustronne: o kącie 4º do góry i kącie 60º w dół, lub odwrotnie.","Up & Down 4º/60º",1,10,"Lillehammery"]
[23,23,"Światło odkryte, częściowo przysłonięte od góry.",null,1,7]
[24,24,"Światło odkryte, rozproszone z obrotowo- symetrycznym rozsyłem światła.",null,1,7]
[25,25,"Światło rozproszone przysłonięte od góry.",null,1,7.9]
[26,26,"Światło odkryte z obrotowo-symetrycznym rozsyłem światła.",null,1,9]
[27,27,"Światło jednostronne: symetryczne, ukierunkowane w dół.",null,1,3]
[28,28,"Do zastosowania w oprawach słupowych typu: Koster, Nicea, Visby oraz innych opraw nasadzanych.",null,1,""]
[29,29,"Światło symetryczne o kącie 40D","40D",1,2]
[30,30,"Światło obrotowo- symetryczne (kombinacja pośrednie/bezpośrednie).",null,4,9]
[31,31,"Światło dwustronne: o kącie 4º do góry i kącie 62º w dół.",null,1,10,"VOSS"]
[32,32,"Światło jednostronne: o kącie 62º w dół.",null,1,10,"VOSS"]
[64,33,"Światło pośrednie, obrotowo- symetryczne, ukierunkowane w dół.",null,1,9]
[66,34,"Światło symetryczne ukierunkowane w dół.",null,1,3]
[67,35,"Światło symetryczne o kącie 36 stopni.","36º",1,2]
[70,36,"Światło dwustronne: o kącie 62º do góry i w dół.",null,1,10,"VOSS"]
[72,37,"Do zastosowania w oprawach słupkowych",null,1]
[73,38,"Światło jednostronne: o kącie 60º w dół.","Down60º",1,10,"Lillehammery; Lysfjord "]
[79,39,"Światło jednostronne: o kącie 4º do góry.","Up 4º",1,10,"Lillehammery; Lysfjord VOSS"]
[148,40,"Światło jednostronne: o kącie 4º w dół.","Down 4º",1,10,"Lillehammery; Lysfjord VOSS"]
[149,41,"Światło dwustronne: o kącie 36º do góry i w dół.","Up - Down 36D",1,2]
[150,42,"Światło dwustronne: o kącie 4º do góry i kącie 60º w dół.","Up4º & Down60º",1,10,"Lillehammery; Lysfjord"]
[151,43,"Światło jednostronne: ukierunkowane w dół o kącie 36 stopni.","Down 36º",1,2]
[152,44,"Światło jednostronne: ukierunkowane w dół (bryła fotometryczna typu DWC-B).","DWC-B",1,6]
[153,45,"Światło ukierunkowane w dół.",null,1,7]
[154,46,"Soczewka firmy Ledil typu SCL (IESNA typ II / III).","SCL",1,6]
[155,47,"Soczewka firmy Ledil typu VSM (IESNA typ V).","VSM",1,4]
[156,48,"Soczewka firmy Ledil typu T2-L (IESNA typ III).","T2-L",1,6]
[157,49,"Światło jednostronne: ukierunkowane w dół o kącie 25 stopni.","Down 25º",1,2]
[158,50,"Światło jednostronne rozproszone.","180D",1,9]
[160,51,"Światło dwustronne rozproszone.",null,1,8,"KISA"]
[161,52,"Światło jednostronne: o kącie 10º do góry lub w dół.",null,1,10,"lillehammer specjal"]
[162,53,"Światło jednostronne: o kącie 10º do góry.",null,1]
[163,54,"Światło jednostronne: o kącie 24º w dół.","Down 24º",1,2]
[164,55,"Światło dwustronne: o kącie 45º do góry i kącie 45º w dół.","Up45º & Down45º",1]
[165,56,"Światło jednostronne: o kącie 62º w górę.","Up62º",1,10,"VOSS"]
[166,57,"Światło symetryczne o kącie 24 stopni.","24º",1,2]
[167,58,"Światło symetryczne o kącie 15 stopni.","15º",1,1]
[170,59,"Światło dwustronne: o kącie 60º do góry i kącie 4º w dół.","Up60º & Down4º",1,10,"Lysfjord"]
[171,60,"Soczewki firmy Ledil typu V/C (bardzo szeroki rozsył światła).","V/C",1,6]
[178,61,"Światło jednostronne: ukierunkowane w górę o kącie 25 stopni.","Up 25º",1,2]
[179,62,"Światło jednostronne: ukierunkowane w górę.","Up",1,7,"Światło rozproszone półsferyczne ukierunkowane w górę"]
[180,63,"Światło jednostronne: ukierunkowane w górę o kącie 36 stopni.","Up 36º",1,2]
[181,64,"Soczewka firmy Ledil typu T4-B (IESNA typ IV).","T4-B",1,5]
[211,65,"Światło jednostronne: o kącie 60º w górę.","Up60º",1,10,"Lillehammery; Lysfjord "]
[212,66,"Światło symetryczne o kącie 15D","15D",1,1]
[220,67,"Światło symetryczne o kącie 24D","24D",1,2]
[228,68,"Światło symetryczne o kącie 36D","36D",1,2]
[236,69,"Światło jednostronne: o kącie 24D w dół.","Down 24D",1,2]
[244,70,"Światło dwustronne: o kącie 36D do góry i w dół.","Up36D&Down36D",1,2]
[252,71,"Światło jednostronne: ukierunkowane w dół o kącie 36D.","Down 36D",1,2]
[260,72,"Światło jednostronne: ukierunkowane w górę o kącie 36D","Up 36D",1,2]
[268,73,"Światło dwustronne: o kącie 25D do góry i w dół.","Up25D & Down25D",1,2]
[276,74,"Światło jednostronne: ukierunkowane w dół o kącie 25D","Down 25D",1,2]
[284,75,"Światło jednostronne: ukierunkowane w górę o kącie 25D","Up 25D",1,2]
[382,76,"Światło rozproszone półsferyczne ukierunkowane w dół",null,null,7]
[383,77,"Światło symetryczne o kącie 30D","30D",null,2]
[392,78,"Światło rozproszone półsferyczne ukierunkowane w górę",null,null,7]

{"sheet":"Zmiany Dawid Głód","index":11,"n_rows":209,"n_cols":3,"rows_kept":209,"cut":false,"hidden":false,"merged":[]}
["Zmiana wymiarów w Edytorze","Zmiana wymiarów w kliku LDT","Zmiana w ImportSchema"]
[1300,1000,655]
[1302,1001,675]
[1303,1330,676]
[1305,1331,866]
[1306,1356,544]
[1308,160,5121]
[1710,163,5122]
[1712,5170,542]
[1715,6154,545]
[1717,2240,630]
[5018,2241,631]
[5104,2244,637]
[1510,2245,638]
[1511,2248,1338]
[1513,2249,1339]
[1514,5008,1350]
[1700,5009,1407]
[1702,5010,1409]
[1705,5060,1417]
[1707,5061,1419]
[5100,5062,1483]
[5101,5063,1488]
[5102,5065,5022]
[5103,1420]
[120,1423]
[127,1430]
[128,1433]
[450,1436]
[454,1439]
[5019,1464]
[5092,1469]
[5093,288]
[5020,296]
[5096,5140]
[5097,5132]
[510,6146]
[515,6148]
[517,6140]
[1874,5001]
[1879,5088]
[1880,5089]
[1580,777]
[1581,1592]
[1582,1593]
[1583,1594]
[1584,1598]
[1585,2120]
[1586,2121]
[1587,2122]
[1588,2123]
[5028,2124]
[5029,2125]
[5030,2411]
[5031,2410]
[1370,2400]
[1371,2407]
[1373,291]
[1374,1443]
[1340,1450]
[1341,1453]
[1921,1475]
[1922,1477]
[1923,293]
[1924,5021]
[1931]
[1932]
[5012]
[5013]
[6033]
[6035]
[6034]
[6036]
[1929]
[1930]
[5011]
[6031]
[6032]
[1933]
[5116]
[1730]
[1731]
[1732]
[1740]
[1741]
[1742]
[5152]
[5153]
[796]
[1390]
[1392]
[5113]
[5039]
[1495]
[1496]
[5038]
[1960]
[1963]
[660]
[661]
[668]
[4116]
[4136]
[4113]
[4114]
[4117]
[370]
[280]
[286]
[1600]
[610]
[611]
[615]
[617]
[1912]
[5039]
[2935]
[2939]
[2937]
[2941]
[2943]
[2945]
[2947]
[2949]
[7150]
[7151]
[7152]
[7153]
[7154]
[7155]
[5024]
[5090]
[1901]
[1903]
[1904]
[1970]
[1972]
[1973]
[2026]
[2027]
[2028]
[2029]
[1544]
[1545]
[1261]
[1262]
[1263]
[1264]
[1281]
[1282]
[1283]
[1283]
[371]
[372]
[373]
[800]
["800A"]
[810]
[820]
[830]
[1814]
[1822]
[1834]
[1842]
[1815]
[1816]
[1817]
[1823]
[1824]
[1825]
[1835]
[1836]
[1837]
[1843]
[1844]
[1845]
[6402]
[6401]
[6403]
[6404]
[6405]
[6406]
[6407]
[6408]
[6421]
[6422]
[6423]
[6424]
[6425]
[6426]
[6427]
[6408]
[5016]
[5046]
[5045]
[5047]
[5253]
[5255]
[7120]
[718]
[539]
[537]
[549]
[548]
[1954]
[1955]
[5032]
[5033]
[5128]